**3GPP TSG-S4 Meeting #132*****S4-250969***

**Fukuoka, Japan, 19th–23rd May 2025** Revision of S4-250698

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **26.512** | **CR** | **0087** | **rev** | **2** | **Current version:** | **18.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** |  | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Adding OpenAPI code based on endorsed CR (26512-CR0087rev1) during SA4-131-bis-e meeting | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | OpenAPI changes are proposed based on agreements during SA4-131-bis-e on topic of WT3b: Multi-access media delivery.  Changes 1-9 were endorsed in previous SA4 meeting. Change 10 includes the proposed OpenAPI updates. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Multi-access media delivery feature is incomplete | | | | | | | | |
| ***Q*** | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.6.1, 4.9, 4.9.3 (new), 5.1, 12.4, 13.2.4, 13.2.5, 13.2.6 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | |  | | |
| ***affected:*** | |  | **X** | Test specifications | | | |  | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | S4-250505: Version implementing normative recommendations documented in clause 7.3.3 on topic of multi-access media delivery  S4-250698: Corrections based on feedback received during presentation of S4-250505 in SA4#131-bis-e.  S4-250698: Corrections during SA4#131-bis-e  S4-250969: OpenAPI changes based on CR agreements from S4-250698 | | | | | | | | |

CHANGE 1 (endorsed in sa4-131-bis-e)

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 26.501: "5G Media Streaming (5GMS); General description and architecture".

[3] DASH Industry Forum, "Specification of Live Media Ingest",   
<https://dashif-documents.azurewebsites.net/Ingest/master/DASH-IF-Ingest.pdf>

[4] 3GPP TS 26.247: "Transparent end-to-end Packet-switched Streaming Service (PSS); Progressive Download and Dynamic Adaptive Streaming over HTTP (3GP-DASH)".

[5] Standard ECMA-262, 5.1 Edition: "ECMAScript Language Specification", June 2011.

[6] IETF RFC 6234: "US Secure Hash Algorithms (SHA and SHA-based HMAC and HKDF)".

[7] 3GPP TS 23.003: "Numbering, addressing and identification".

[8] ITU-T Recommendation X.509 (2005) | ISO/IEC 9594-8:2005: "Information Technology – Open Systems Interconnection – The Directory: Public-key and attribute certificate frameworks".

[9] Void

[10] IETF RFC 4648: "The Base16, Base32, and Base64 Data Encodings".

[11] IEEE Standard 1003.1™, Issue 7: "The Open Group Base Specifications", 2018.  
<https://pubs.opengroup.org/onlinepubs/9699919799/>

[12] 3GPP TS 29.571: "Common Data Types for Service Based Interfaces; Stage 3".

[13] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification".

[14] 3GPP TS 36.321: "Evolved Universal Terrestrial Radio Access (E-UTRA); Medium Access Control (MAC) protocol specification".

[15] 3GPP TS 27.007: "AT Command set for User Equipment (UE)".

[16] Void[17] IETF RFC 7468: "Textual Encodings of PKIX, PKCS, and CMS Structures", April 2015.

[18] ISO 3166‑1: "Codes for the representation of names of countries and their subdivisions — Part 1: Country codes".

[19] ISO 3166‑2: "Codes for the representation of names of countries and their subdivisions — Part 2: Country subdivision code".

[20] IETF RFC 5280: "Internet X.509 Public Key Infrastructure Certificate and Certificate Revocation List (CRL) Profile", May 2008.

[21] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[22] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[23] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[24] IETF RFC 9112: "HTTP/1.1", June 2022.

[25] IETF RFC 9110: "HTTP Semantics", June 2022.

[26] Void

[27] Void

[28] IETF RFC 9111: "HTTP Caching", June 2022.

[29] Void

[30] IETF RFC 8446: "The Transport Layer Security (TLS) Protocol Version 1.3", August 2018.

[31] IETF RFC 9113: "HTTP/2", June 2022.

[32] ISO/IEC 23009-1: "Information technology; Dynamic adaptive streaming over HTTP (DASH) — Part 1: Media presentation description and segment formats".

[33] 3GPP TS 23.503: "Policy and charging control framework for the 5G System (5GS); Stage 2".

[34] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[35] 3GPP TS 26.511: "5G Media Streaming (5GMS); Profiles, codecs and formats".

[36] Void.

[37] 3GPP TS 26.244: "Transparent end-to-end packet switched streaming service (PSS); 3GPP file format (3GP)".

[38] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format", December 2017.

[39] ISO 14496-12: "Information technology – Coding of audio-visual objects – Part 12: ISO base media file format".

[40] ISO 23000-19: "Information technology – Coding of audio-visual objects – Part 19: Common media application format (CMAF) for segmented media".

[41] IETF RFC 3986: "URI Generic Syntax".

[42] 3GPP TS 26.118: "Virtual Reality (VR) profiles for streaming applications".

[43] 3GPP TS 24.558: "Enabling Edge Applications; Protocol specification".

[44] 3GPP TS 29.558: "Enabling Edge Applications; Application Programming Interface (API) specification; Stage 3".

[45] 3GPP TS 23.502: "Procedures for the 5G System (5GS); Stage 2".

[46] 3GPP TS 29.517: "5G System; Application Function Event Exposure Service; Stage 3".

[47] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services".

[48] 3GPP TS 26.531: "Data Collection and Reporting; General Description and Architecture".

[49] 3GPP TS 26.532: "Data Collection and Reporting; Protocols and Formats".

[50] 3GPP TS 29.522: "5G System. Network Exposure Function Northbound APIs; Stage 3".

[51] 3GPP TS 26.346: "Multimedia Broadcast/Multicast Service (MBMS); Protocols and codecs".

[52] 3GPP TS 26.347: "Multimedia Broadcast/Multicast Service (MBMS); Application Programming Interface and URL".

[53] IETF draft-bhutton-json-schema-validation: "JSON Schema Validation: A Vocabulary for Structural Validation of JSON", June 2022.

[54] IETF RFC 3339: "Date and Time on the Internet: Timestamps", July 2002.

[55] 3GPP 29.591: "Network Exposure Function Southbound Services; Stage 3".

[56] 3GPP TS 26.510: "Media delivery; interactions and APIs for provisioning and media session handling".

[57] IETF RFC 2045: "Multipurpose Internet Mail Extensions (MIME) Part One: Format of Internet Message Bodies".

[58] IETF RFC 9000: "QUIC: A UDP-Based Multiplexed and Secure Transport", May 2021.

[59] IETF RFC 9001: "Using TLS to Secure QUIC", May 2021.

[60] IETF RFC 9114: "HTTP/3", June 2022.

[61] IETF RFC 8673: "HTTP Random Access and Live Content", November 2019.

[62] Consumer Technology Association CTA-5005-A: "Web Application Video Ecosystem – DASH-HLS Interoperability Specification".

[63] DASH-IF Guidelines: "Low-latency Modes for DASH", available here:  
<https://dash-industry-forum.github.io/docs/CR-Low-Latency-Live-r8.pdf>

[64] 3GPP TS 26.517: "5G Multicast-Broadcast User Services; Protocols and Formats".

[65] Consumer Technology Association CTA‑5004: "Web Application Video Ecosystem – Common Media Client Data", September 2020,  
https://cdn.cta.tech/cta/media/media/resources/standards/pdfs/cta-5004-final.pdf.

[66] IETF RFC 4122: "A Universally Unique IDentifier (UUID) URN Namespace", July 2005.

[MPTCP] IETF RFC 8684: "TCP Extensions for Multipath Operation with Multiple Addresses".

[MPQUIC] IETF Draft: "Multipath Extension for QUIC", draft-ietf-quic-multipath-10, July 2024

change 2 - Media streaming procedures (M4d) (endorsed in sa4-131-bis-e)

### 4.6.1 Procedures for DASH Session

This procedure is used by a 5GMSd Client to establish a DASH session via the M4d interface. In order to establish such a session, the 5GMSd AS shall host an MPD as defined in ISO/IEC 23009-1 [32] or TS 26.247 [4] and the MPD URL is known to the 5GMSd Client typically using M8d.

The Media Player receives an MPD URL from the 5GMSd-Aware Application through M7d by methods defined in clause 13. The Media Player shall send an HTTP GET message to the 5GMSd AS including the URL of the MPD resource. On success, the 5GMSd AS shall respond with a 200 (OK) message that includes the requested MPD resource.

Additional procedures for reactions to different HTTP status codes are provided in TS 26.247 [4], clause A.7 and ISO/IEC 23009-1 [32] clause A.7.

Additional procedures for handling partial file responses are provided in TS 26.247 [4], clause A.9.

This information is provided through M7d to the application for selection. In addition, the currently used service description parameters are provided as status information through M7d in order for the Media Session Handler to make use of this information, for example for Dynamic Policy and Network Assistance.

The detailed handling of service description information is documented in clause 13.2 of the present document.

The Media Player may use multiple access networks available on the UE to connect to a service location on the 5GMSd AS via reference point M4d.

change 3 - Media Player Client API procedures (M7d/M11d) (endorsed in sa4-131-bis-e)

## 4.9 Procedures of the M7d/M11d (UE Media Player) interface

CHANGE 4 - (endorsed in sa4-131-bis-e)

### 4.9.3 Multi-access media delivery procedures

To facilitate multi-access media delivery at reference point M4d (see clause 4.6.1), the 5GMS-Aware Application and the Media Session Handler may configure multi-access delivery parameters at the Media Player via reference points M7 and M11 respectively. The multi-access media delivery parameters are described in clause 13.2.4.

The Media Player may inform the 5GMS-Aware Application and the Media Session Handler via reference points M7 and M11 respectively about the status of the multi-access delivery connection over reference point M4 as described in clauses 13.2.5 and 13.2.6. The 5GMS-Aware Application and the Media Session Handler may make use of this information, for example to re-configure multi-access media delivery connection properties, or to disable multi-access media delivery altogether, using the configuration and settings API specified in clause 13.2.4.

change 5 - PRocedurEs for Uplink Media Streaming(endorsed in sa4-131-bis-e)

## 5.1 General

Uplink media streaming functional entities in the 5GMS System include the 5GMSu Application Provider, 5GMSu AF, 5GMSu AS and the UE. To make use of these other entities, the UE includes a 5GMSu-Aware Application that is provided by the 5GMSu Application Provider and a 5GMSu Client comprising the Media Session Handler and the Media Streamer.

The M1 Provisioning API enables the 5GMSu Application Provider to establish and manage the uplink media session handling and streaming options of the 5GMSu System.

The content egest interface at reference point M2u enables uplink media streaming content that has been sent by the 5GMSu Client to the 5GMSu AS at reference point M4u to be subsequently delivered to the 5GMSu Application Provider. Uplink media streaming media transfer from the 5GMSu AS to the 5GMSu Application Provider may be either pull-based and initiated by the 5GMSu Application Provider using the HTTP GET method, or push-based and initiated by the 5GMSu AS using the HTTP PUT method. The 5GMSu Application Provider's target endpoint for push-based streaming content delivery at reference point M2u is provided to the 5GMSu AF as part of the M1 Provisioning Session and this is passed to the 5GMSu AS as part of the M3u configuration procedures.

The 5GMSu AF, having been successfully provisioned at reference point M1u, sets up corresponding resources at a reference point M5u endpoint from which Service Access Information for uplink media streaming session management, metrics reporting, network assistance and request for policy and/or charging treatment may be retrieved using its provisioned external application identifier. Certain types of configuration and policy information accessed over reference point M5u by the Media Session Handler, such as uplink metrics reporting, QoS policy, or support for AF-based network assistance are further passed to the Media Streamer via the M7u API.

The 5GMSu-Aware Application initiates a new uplink media streaming session by launching the Media Stream Handler at reference point M6u using a 3GPP Service URL for 5GMS (see clause 4.8.3). The 3GPP Service URL indicates the external application identifier. This may be used to retrieve Service Access Information from the 5GMSu AF at reference point M5. Alternatively, if the 5GMSu-Aware Application has already acquired all necessary Service Access Information via private means at reference point M8, this may be supplied directly to the Media Session Handler at reference point M6u as additional parameters.

Based on a request from the 5GMSu-Aware Application or from the Media Streamer received over the M6u API, and based on the Service Access Information acquired from the 5GMSu AF via reference point M5u, the Media Session Handler sets up an uplink media streaming session with a unique media delivery session identifier. Upon successful session establishment, the Media Session Handler triggers the Media Streamer to begin uplink media streaming of media content to the 5GMSu AS over reference point M4u. The Media Streamer may use multiple access networks available on the UE to connect to a service location on the 5GMSu AS via a reference point M4u.

Subscription to status and other event notification services is offered by the Media Session Handler to the 5GMSu-Aware Application and to the Media Streamer via the UE media session handling APIs exposed by the Media Session Handler at reference point M6u.

Subscription to status and other event notification services is also offered by the Media Streamer to the 5GMSu-Aware Application and to the Media Session Handler via the UE media stream handling APIs exposed by the Media Player at reference point M11u.

CHANGE 6 -(endorsed in sa4-131-bis-e)

## 12.4 3GPP Service URL for 5G Media Streaming

The 3GPP Service URL for 5G Media Streaming is based on the generic 3GPP Service URL defined in clause 6 of TS 26.510 [56].

If the service type discriminator service in the URL indicates ms, then the target service is a 5G Media Streaming service.

The parameters of the 3GPP Service URL for 5G Media Streaming are defined in table 12.4-1.

Table 12.4-1: 3GPP Service URL parameters for 5G Media Streaming

|  |  |  |
| --- | --- | --- |
| Path element | Cardinality | Description |
| service\_id | 1 | An External Service Identifier that resolves to a Provisioning Session in the 5GMS System. |
| Query parameter | Cardinality | Description |
| af-host-address | 0..\* | The Fully Qualified Domain Name and optional port number of a 5GMS AF endpoint to be used by the Media Session Handler at reference point M5 with the format hostname[:port].  More than one occurrence of this parameter may be present in the Service URL to indicate alternative host endpoint addresses. Any of these may be used by the Media Session Handler at reference point M5.  Supplied by the invoking 5GMS-Aware Application when the 5GMS AF is deployed in an External DN. The endpoint address(es) may, for example, have been passed to the 5GMS-Aware Application via reference point M8.  If omitted, the Media Session Handler assumes the default 5GMS AF host endpoint address ms.af.3gppservices.org:443 is to be used at reference point M5. |
| access-token | 0..1 | A token that is presented by the Media Session Handler to the 5GMS AF at reference point M5 that asserts its right to invoke the media session handling operations exposed by the 5GMS AF. |
| service-operation-point | 0..1 | A reference to the target Service Operation Point of the 5G Media Streaming session.  Overrides any default Service Operation Point signalled in the resource pointed to by media-entry-point. |
| estimated-volume | 0..1 | An estimate of the volume of media data to be transferred between the 5GMS Client and the 5GMS AS at reference point M4 during the 5G Media Streaming session.  Required if service-operation-point or media-entry-point refers to a Policy Template with an associated Background Data Transfer policy. |
| media-entry-point | 0..1 | A Media Entry Point reference expressed as a fully qualified URL per RFC 3986 [41], suitable for presentation to a 5GMS AS at reference point M4.  If supplied, used by the Media Session Handler to launch the Media Stream Handler (Media Player or Media Streamer) after successfully initiating media session handling. |
| multipath-protocol | 0..\* | The multipath transport protocol to be used for multi-access media delivery at reference point M4.  - The value MPTCP indicates the use of the protocol specified in RFC 8684[MPTCPMPTCP].  - The value MPQUIC indicates the use of the protocol specified in [MPQUIC]. |
| min-paths | 0..1 | The minimum number of subflows/paths to be used for multi-access media delivery at reference point M4.  Default value is 1 if omitted. |
| max-paths | 0..1 | The maximum number of subflows/paths to be used for multi-access media delivery at reference point M4.  Default value is 1 if omitted. |
| content-type | 0..\* | A MIME content type string conforming to section 5 of RFC 2045 [57] identifying a type of Media Entry Point that is acceptable to the Media Stream Handler (Media Player or Media Streamer).  More than one occurrence of this parameter may be present in the Service URL to indicate that more than one type of Media Entry Point is acceptable.  Used by the Media Session Handler to eliminate unacceptable Media Entry Points from those listed in the Service Access Information.  It is an error to supply this parameter if an explicit Media Entry Point is specified using media-entry-point. |
| profile | 0..\* | A fully-qualified term identifier from a controlled vocabulary specified outside the scope of the present document identifying a profile of Media Entry Point that is acceptable to the Media Stream Handler (Media Player or Media Streamer). The term identifier shall be formatted as a URI according to RFC 3986 [41].  More than one occurrence of this parameter may be present in the Service URL to indicate that more than one type of Media Entry Point is acceptable.  Used by the Media Session Handler to eliminate unacceptable Media Entry Points from those listed in the Service Access Information.  It is an error to supply this parameter if an explicit Media Entry Point is specified using media-entry-point. |

The service\_id path element, and the af-host-address and access-token query parameters correspond to the baseline Service Access Information for downlink media streaming specified in clause 4.2.3 of TS 26.501 [2] and the baseline parameters of the 3GPP Service URL for 5G Media Streaming defined in clause 4.10.2 of [2]. Together, they enable a full set of Service Access Information to be retrieved by the Media Session Handler from the 5GMS AF using the Service Access Information API at reference point M5 specified in clause 11.2 of the present document.

The service-operation-point parameter is used to support the procedure where the desired Service Operation Point is known *a priori* to the invoker and/or is not encoded in the Media Entry Point.

The estimated-volume parameter is used to support the procedure where the invoker intends the launched 5G Media Streaming session to be used for the purpose of Background Data Transfer.

The media-entry-point query parameter is used to support the procedure where the Media Session Handler launches media playback in the Media Stream Handler (Media Player or Media Streamer) after successfully retrieving a full set of Service Access Information via reference point M5 (if needed) and after successfully initiating media session handling.

The multipath-protocol parameter is used to support the use of multipath transport protocols for multi-access media delivery, as specified in clauses 4.6.1 and 4.9.3. When multiple instances of this parameter exist in the URL, the Media Stream Handler (Media Player/Streamer) shall sequentially attempt each specified protocol in their URL appearance order until establishing a successful multipath connection. . If all multipath connection attempts fail, , the Media Stream Handler (Media Player or Media Streamer) shall fall back to a single path transport connection. The min-paths and max-paths specify the permissible range of subflows/paths for all multipath transport protocols listed in the URL.

The remaining query parameters are used for client-side filtering of Media Entry Point information provided in the Service Access Information and selection of one Media Entry Point by the Media Session Handler. (They are mutually exclusive with the media-entry-point parameter.) In this case, media playback by the Media Stream Handler (Media Player or Media Streamer) is launched by the Media Session Handler with its chosen Media Entry Point.

If the 5GMS-Aware Application prefers to launch media streaming itself (rather than have the Media Session Handler launch media streaming on its behalf), the media-entry-point query parameter and all client-side filtering parameters shall be omitted from the 3GPP Service URL. In this case, the Media Session Handler initiates only media session handling for the 5GMS Provisioning Session identified by the External Service Identifier.

CHANGE 7 -(endorsed in sa4-131-bis-e)

### 13.2.4 Configurations and settings API

DASH streaming for a particular downlink media delivery session may be configured by the 5GMSd-Aware Application at reference point M7d or by the Media Session Handler at reference point M11d with the parameters provided in table 13.2.4-1. Note that these parameters may be set and they may also be observed.

Table 13.2.4-1: Media Player Configuration API

|  |  |  |  |
| --- | --- | --- | --- |
| Status | | Type | Definition |
| sessionId | | string | A media delivery session identifier for the downlink media streaming session that has been initialised using the method specified in clause 13.2.3.2. |
| source | | Object | Provides the MPD and all contained information. |
| consumptionMode | | Enum | Defines two modes:  live: in this case the target latency is maintained, if specified in the service description, according to the parameters  vod: in this case the latency is set by the application and the latency settings are ignored. |
| maxBufferTime | | Integer | Maximum buffer time in milliseconds for the service. |
| serviceDescriptionId | | id | Selects a service description by selecting an identifier. |
| serviceDescriptions[] | | Service description parameters | Configures a service description as defined in annex K of ISO/IEC 23009-1 [32]. This allows the application to define additional service descriptions beyond those defined in the MPD. |
|  | id | id | Sets a service description identifier different from the ones available in the service descriptions in the MPD or modifies existing service descriptions. |
|  | serviceLatency | Object | Sets service description parameters for the service latency, as defined in table K.1 of ISO/IEC 23009-1 [32]. |
|  | playBackRate | Object | Sets service description parameters for the playback rate, as defined in table K.2 of ISO/IEC 23009-1 [32] when the service is consumed in live mode. |
|  | operatingQuality | Object | Sets service description parameters for the operating quality, as defined in table K.3 of ISO/IEC 23009-1 [32]. |
|  | operatingBandwidth | Object | Sets service description parameters for the operating bandwidth, as defined in table K.4 of ISO/IEC 23009-1 [32]. |
| mediaSettings[] | | Media type audio, video, subtitle | Sets the selected Adaptation Set based on the available Adaptation Sets for each media type. |
| metricsConfiguration[ ] | | Object | Zero or more sets of settings for collecting metrics in relation to the downlink media streaming session. |
| multiAccessConfiguration | | Object | Configuration of multi-access media delivery at reference point M4d. If omitted, multi-access delivery is disabled. |
|  | transportProtocols | array(Enumeration) | A non-empty array of enumerated values from table 13.2.4‑2 to be used by the Media Player for multi-access media delivery at reference point M4d. |
|  | minPaths | Integer | Minimum number of subflows/paths used by the Media Player for multi-access media delivery at reference point M4d. |
|  | maxPaths | Integer | Maximum number of subflows/paths used by the Media Player for multi-access media delivery at reference point M4d. |

Table 13.2.4-2: Transport Protocols for multi-access media delivery

|  |  |
| --- | --- |
| Value | Description |
| MPTCP | Multipath TCP protocol specified in [MPTCP] |
| MPQUIC | Multipath QUIC protocol specified in [MPQUIC] |

CHANGE 8 -(endorsed in sa4-131-bis-e)

### 13.2.5 Notifications and error events

Table 13.2.5-1 provides a list of notification events that are provided by the Media Player to 5GMSd-Aware Applications at reference point M7d and to the Media Session Handler at reference point M11d. Every notification and error event is disambiguated by a media delivery session identifier.

Table 13.2.5-1: Media Player Notification events

|  |  |  |
| --- | --- | --- |
| Status | Definition | Payload |
| AST\_IN\_FUTURE | Triggered when playback will not start yet as the MPD's availabilityStartTime is in the future. | Media delivery session identifier, Time before playback will start. |
| AVAILABLE\_MEDIA\_CHANGED | The list of available media has changed. | Media delivery session identifier, Media type:  - video  - audio  - subtitle  - all |
| BUFFER\_EMPTY | Triggered when the media playback platform's buffer state changes to stalled. | Media delivery session identifier, Media Type |
| BUFFER\_LOADED | Triggered when the media playback platform's buffer state changes to loaded. | Media delivery session identifier, Media Type |
| CAN\_PLAY | Sent when enough data is available that the media can be played. | Media delivery session identifier |
| MANIFEST\_LOADED | Triggered when the manifest load is complete | Media delivery session identifier |
| METRIC\_ADDED | Triggered every time a new metric is added. | Media delivery session identifier |
| METRIC\_CHANGED | Triggered every time a metric value changes. | Media delivery session identifier,  Metric identifier |
| METRIC\_UPDATED | Triggered when the configuration of a metric is updated. | Media delivery session identifier,  Metric identifier |
| METRICS\_CHANGED | Triggered whenever there is a change to the overall metrics. | Media delivery session identifier |
| OPERATION\_POINT\_CHANGED | Triggered whenever there is a change of a Service Operation Point parameter. | Media delivery session identifier,  External reference identifier of currently selected Service Operation Point. |
| PLAYBACK\_ENDED | Sent when media playback completes normally. | Media delivery session identifier |
| PLAYBACK\_ERROR | Sent when an error occurs during media playback. The element's error attribute contains more information. | Media delivery session identifier,  Error reason (see table 13.2.5‑2). |
| PLAYBACK\_PAUSED | Sent when media playback is paused. | Media delivery session identifier |
| PLAYBACK\_PLAYING | Sent when the media begins to play (either for the first time, after having been paused, or after ending and then restarting). | Media delivery session identifier |
| PLAYBACK\_SEEKED | Sent when a media playback seek operation completes. | Media delivery session identifier |
| PLAYBACK\_SEEKING | Sent when a media playback seek operation begins. | Media delivery session identifier |
| PLAYBACK\_STALLED | Sent when the media playback platform reports stalled. | Media delivery session identifier |
| PLAYBACK\_STARTED | Sent when playback of the media starts after having been paused; that is, when playback is resumed after a prior pause event. | Media delivery session identifier |
| PLAYBACK\_WAITING | Sent when the media playback has stopped because of a temporary lack of data. | Media delivery session identifier |
| SERVICE\_DESCRIPTION\_SELECTED | sent when the DASH client has selected a service description. | Media delivery session identifier |
| SERVICE\_DESCRIPTION\_CHANGED | Sent when the DASH client has changed a service description. | Media delivery session identifier |
| SERVICE\_DESCRIPTION\_VIOLATED | Provides notification that the service description parameters are currently not met. | Media delivery session identifier,  Parameters of service description that are not met |
| SOURCE\_INITIALIZED | Triggered when the source is set up and ready. | Media delivery session identifier |
| DOWNLOAD\_STARTED | Sent when a non-real-time content download begins. | Media delivery session identifier |
| DOWNLOAD\_COMPLETED | Sent when a non-real-time content download is complete. | Media delivery session identifier |
| DOWNLOAD\_ERROR | Send when an error occurs during non-real-time content download | Media delivery session identifier,  Error reason (see table 13.2.5‑2). |
| MULTI-ACCESS\_DELIVERY\_ESTABLISHED | Triggered when the multi-access media delivery connection is set up and ready | Media delivery session identifier,  Multi-access connection status |
| MULTI-ACCESS\_DELIVERY\_CHANGED | Triggered when the multi-access media delivery connection status changes. | Media delivery session identifier, Multi-access connection status |

Table 13.2.5-2 provides a list of error reasons that are indicated for notifications of type PLAYBACK\_ERROR and DOWNLOAD\_ERROR.

Table 13.2.5-2: Media Player Error reasons

|  |  |
| --- | --- |
| Error reason | Definition |
| ERROR\_MEDIA\_ENTRY\_NOT\_FOUND | The Media Entry Point resource requested by the Media Player could not be located. |
| ERROR\_CONTENT\_NOT\_FOUND | Other content requested by the Media Player could not be located. |
| ERROR\_MEDIA\_PLAYBACK | There is an error from the media playback platform buffer. |
| ERROR\_INVALID\_MEDIA\_ENTRY | The Media Entry Point resource supplied is not syntactically valid. |
| ERROR\_INACCESSIBLE\_MEDIA\_TIME | The media time requested in a seek operation is not accessible in the current media presentation. |
| ERROR\_UNSUPPORTED\_PROFILE | The profile of the media presentation described by the Media Entry Point resource is not supported by the media playback platform. |
| ERROR\_DOWNLOAD\_DEADLINE\_MISSED | The download of content did not complete before the requested deadline and the incomplete download has been discarded. |
| ERROR\_MULTI-ACCESS\_DELIVERY\_UNAVAILABLE | The configured multi-access media delivery (see clause 13.2.4) is not supported by the Media Player or 5GMS AS. |

CHANGE 9 -(endorsed in sa4-131-bis-e)

### 13.2.6 Dynamic Status Information

Table 13.2.6-1 provides a list of dynamically changing status information that can be obtained from the Media Player via reference point M7d or M11d. A separate set of Dynamic Status Information is provided for each active downlink media streaming session, indexed by its media delivery session identifier initialised per clause 13.2.3.2.

Table 13.2.6-1: Media Player Dynamic Status information

|  |  |  |  |
| --- | --- | --- | --- |
| Status | Type | Parameter | Definition |
| state | Enumeration |  | An enumerated value from table 13.2.2‑1 indicating the current state of the Media Player. |
| averageThroughput | float | none | Current average throughput computed in the ABR logic in bit/s. |
| bufferLength | float | MediaType  "video", "audio" and "subtitle" | Current length of the buffer for a given media type, in seconds. If no type is passed in, then the minimum of video, audio and subtitle buffer length is returned. NaN is returned if an invalid type is requested, the presentation does not contain that type, or if no arguments are passed and the presentation does not include any adaption sets of valid media type. |
| liveLatency | float | none | Current live stream latency in seconds based on the latency measurement. |
| mediaSetting[ ] | MPDAdaptationSet | MediaType  "video", "audio" and "subtitle" | Current media settings for each media type based on the CMAF Header and the MPD information based on the selected Adaptation Set for this media type. |
| mediaTime | float | None | Current media playback time from media playback platform. The media time is in seconds and is relative to the start of the playback and provides the media that is actually rendered. |
| playbackRate | float | None | The current rate of playback. For a video that is playing twice as fast as the default playback, the playbackRate value should be 2.00. |
| availableServiceDescriptions[ ] | Array of service descriptions |  | Provides the list of available selectable service descriptions with an id to select from. Those are either configured ones or the ones in the MPD. |
| availableMediaOptions[ ] | List of Adaptation Set or Preselection ids | MediaType  "video", "audio" "subtitle" "all" | Provides the list of available media options that can be selected by the application based on the capability discovery and the subset information. |
| service‌Operation‌Points | array(Service‌Operation‌Point) |  | The set of Service Operation Points declared in the presentation manifest (e.g. DASH MPD) of the current media presentation. See table 13.2.6-2. |
| operative‌Service‌Operation‌Point | integer |  | A zero-based index into the service‌Operation‌Points array indicating the Service Operation Point currently operative in the playback session.  Set to -1 if the array is empty. |
| metrics[ ][ ] | Metrics |  | A data blob of metrics for each configured metrics collecting scheme. |
| multiAccessConnectionStatus | Multi‌Access‌Connection‌Status |  | Status information about multi-access media delivery connection(s). See table 13.2.6-3. |

Table 13.2.6-2 provides a list of configured operation point information that can be obtained from the client. Any change to a parameter below shall be announced with a notification OPERATION\_POINT\_CHANGED as specified in table 13.2.5‑1.

Table 13.2.6-2: Media Player Service Operation Point Information

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | | Type | Definition |
| ServiceOperationPoint | | | Object | The currently configured Service Operation Point parameters according to which the DASH client is operating. |
|  | externalIdentifier | | String | The external identifier uniquely identifying this Service Operation Point in the presentation manifest (e.g. DASH MPD). |
|  | mode | | Enum | The following operation modes are defined:  live: The DASH client operates to maintain configured target latencies using playback rate adjustments and possibly resync.  vod: The DASH client operates without latency requirements and rebuffering may result in additional latencies |
|  | maxBufferTime | | Integer | maximum buffer time in milliseconds for the service. |
|  | switchBufferTime | | Integer | buffer time threshold below which the DASH clients attempt to switch Representations. |
|  | latency | | Object | Defines the latency parameters used by the DASH client when operating in live mode. |
|  |  | target | Integer | The target latency for the service in milliseconds. |
|  |  | max | Integer | The maximum latency for the service in milliseconds. |
|  |  | min | Integer | The maximum latency for the service in milliseconds. |
|  | playbackRate | | MediaType  audio, video, all | Defines the playback rate parameters used by the DASH client for catchup mode and deceleration to avoid buffer underruns and maintaining target latencies. |
|  |  | max | Real | The maximum playback rate for the purposes of automatically adjusting playback latency and buffer occupancy during normal playback, where 1.0 is normal playback speed. |
|  |  | min | Real | The minimum playback rate for the purposes of automatically adjusting playback latency and buffer occupancy during normal playback, where 1.0 is normal playback speed. |
|  | bitRate | |  | Defines the operating bit rate parameters used by the DASH client used for a specific media type or aggregated. The values are on IP level. |
|  |  | target | Integer | The target bit rate for the service in bit/s that the client is configured to consume. |
|  |  | max | Integer | The maximum bit rate for the service in bit/s that the client is configured to consume. |
|  |  | min | Integer | The minimum bit rate for the service in bit/s that the client is configured to consume. |
|  | playerSpecificParameters | |  | Player-specific parameters may be provided, for example about the used algorithm, etc. |

Table 13.2.6-3 specifies the multi-access connection status parameters. Any change to a parameter below shall be announced with a notification MULTI-ACCES\_DELIVERY\_CHANGED as specified in table 13.2.5‑1.

Table 13.2.6-3: Multi-access connection status information

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Parameter | | Type | Parameter | Definition |
| MultiAccessConnectionStatus | | Object |  | Status information of multi-access media delivery connection |
|  | status | boolean |  | Indicates status of multi-access media delivery connection. |
|  | transportProtocol | Enumeration |  | An enumerated value from table 13.2.4-2 indicating the transport protocols used for multi-access media delivery. |
|  | numberOfPaths | Integer |  | The current number of active subflows/paths at reference point M4d. |

change 10 – OPENAPI changes

# Code changes

The code changes associated with this Change Request are available for review at the following URL on 3GPP Forge:

https://forge.3gpp.org/rep/sa4/amd-pro-med/-/merge\_requests/3

The proposed changes are reproduced below for posterity.

|  |
| --- |
| ---a/TS26512\_CommonData.yaml +++b/TS26512\_CommonData.yaml  @@ -142,6 +142,97 @@ components:  142 142 minimumBitRate:  143 143 $ref: 'TS29571\_CommonData.yaml#/components/schemas/BitRate'  144 144  145 + ServiceDescription:  146 + description: Service description as defined in annex K of ISO/IEC 23009-1. This allows the application to define additional service descriptions beyond those defined in a media description document such as MPD.  147 + type: object  148 + properties:  149 + id:  150 + type: string  151 + description: Service description identifier.  152 + serviceLatency:  153 + type: object  154 + description: Service description parameters for the service latency, as defined in table K.1 of ISO/IEC 23009-1.  155 + playBackRate:  156 + type: object  157 + description: Service description parameters for the playback rate, as defined in table K.2 of ISO/IEC 23009-1 when the service is consumed in live mode.  158 + operatingQuality:  159 + type: object  160 + description: Service description parameters for the operating quality, as defined in table K.3 of ISO/IEC 23009-1.  161 + operatingBandwidth:  162 + type: object  163 + description: Service description parameters for the operating bandwidth, as defined in table K.4 of ISO/IEC 23009-1.  164 +  165 + ServiceOperationPoint:  166 + description: Service Operation Point parameters according to which the DASH client is operating.  167 + type: object  168 + properties:  169 + externalIdentifier:  170 + type: string  171 + description: Identifier uniquely identifying Service Operation Point in the presentation manifest (e.g. DASH MPD).  172 + mode:  173 + $ref: '#/components/schemas/MediaOperationMode'  174 + description: >  175 + In case of live operation mode, the DASH client operates to maintain configured target latencies using playback rate adjustments and possibly resync.  176 + In case of vod operation mode, the DASH client operates without latency requirements and rebuffering may result in additional latencies.  177 + maxBufferTime:  178 + type: integer  179 + description: Maximum buffer time in milliseconds for the service.  180 + switchBufferTime:  181 + type: integer  182 + description: Buffer time threshold below which the DASH clients attempt to switch Representations.  183 + latency:  184 + type: object  185 + description: Defines the latency parameters used by the DASH client when operating in live mode.  186 + properties:  187 + target:  188 + type: integer  189 + description: The target latency for the service in milliseconds.  190 + max:  191 + type: integer  192 + description: The maximum latency for the service in milliseconds.  193 + min:  194 + type: integer  195 + description: The minimum latency for the service in milliseconds.  196 + playbackRate:  197 + type: object  198 + description: Defines the playback rate parameters used by the DASH client for catchup mode and deceleration to avoid buffer underruns and maintaining target latencies.  199 + properties:  200 + max:  201 + $ref: 'TS29571\_CommonData.yaml#/components/schemas/Double'  202 + description: Maximum playback rate for the purposes of automatically adjusting playback latency and buffer occupancy during normal playback, where 1.0 is normal playback speed.  203 + min:  204 + $ref: 'TS29571\_CommonData.yaml#/components/schemas/Double'  205 + description: Minimum playback rate for the purposes of automatically adjusting playback latency and buffer occupancy during normal playback, where 1.0 is normal playback speed.  206 + bitRate:  207 + type: object  208 + description: Defines the operating bit rate parameters used by the DASH client used for a specific media type or aggregated. The values are on IP level.  209 + properties:  210 + target:  211 + type: integer  212 + description: The target bit rate for the service in bit/s that the client is configured to consume.  213 + max:  214 + type: integer  215 + description: The maximum bit rate for the service in bit/s that the client is configured to consume.  216 + min:  217 + type: integer  218 + description: The minimum bit rate for the service in bit/s that the client is configured to consume.  219 + playerSpecificParameters:  220 + type: object  221 + description: Player-specific parameters may be provided, for example about the used algorithm, etc..  222 +  223 + MultiAccessConnectionStatus:  224 + description: Multi-access delivery connection status information.  225 + properties:  226 + status:  227 + type: boolean  228 + description: Indicates status of multi-access delivery connection.  229 + transportProtocol:  230 + $ref: '#/components/schemas/MultiAccessTransportProtocolType'  231 + description: An enumerated value indicating the multi-access transport protocol.  232 + numberOfPaths:  233 + type: integer  234 + description: The current number of active subflows or paths at reference point M4d.  235 +  145 236 #####################################  146 237 # Clause 6.4.4: Enumerated data types  147 238 #####################################  @@ -156,4 +247,92 @@ components:  156 247 description: >  157 248 This string provides forward-compatibility with future  158 249 extensions to the enumeration but is not used to encode  159 - content defined in the present version of this API.  No newline at end of file  250 + content defined in the present version of this API.  251 +  252 + MultiAccessTransportProtocolType:  253 + anyOf:  254 + - type: string  255 + enum:  256 + - MPTCP  257 + - MPQUIC  258 + - type: string  259 + description: >  260 + Represents type of multipath protocol for multi-access delivery introduced in TS 23.501  261 +  262 + MediaOperationMode:  263 + anyOf:  264 + - type: string  265 + enum:  266 + - live  267 + - vod  268 + - type: string  269 + description: >  270 + Two operation modes of 5GMS media delivery session.  271 +  272 + MediaPlayerNotificationEvent:  273 + description: 'Enumeration of media player notifications.'  274 + anyOf:  275 + - type: string  276 + enum:  277 + - NOTIFICATION\_AST\_IN\_FUTURE  278 + - NOTIFICATION\_AVAILABLE\_MEDIA\_CHANGED  279 + - NOTIFICATION\_BUFFER\_EMPTY  280 + - NOTIFICATION\_BUFFER\_LOADED  281 + - NOTIFICATION\_CAN\_PLAY  282 + - NOTIFICATION\_MANIFEST\_LOADED  283 + - NOTIFICATION\_METRIC\_ADDED  284 + - NOTIFICATION\_METRIC\_CHANGED  285 + - NOTIFICATION\_METRIC\_UPDATED  286 + - NOTIFICATION\_METRICS\_CHANGED  287 + - NOTIFICATION\_OPERATION\_POINT\_CHANGED  288 + - NOTIFICATION\_PLAYBACK\_ENDED  289 + - NOTIFICATION\_PLAYBACK\_ERROR  290 + - NOTIFICATION\_PLAYBACK\_PAUSED  291 + - NOTIFICATION\_PLAYBACK\_PLAYING  292 + - NOTIFICATION\_PLAYBACK\_SEEKED  293 + - NOTIFICATION\_PLAYBACK\_SEEKING  294 + - NOTIFICATION\_PLAYBACK\_STALLED  295 + - NOTIFICATION\_PLAYBACK\_STARTED  296 + - NOTIFICATION\_PLAYBACK\_WAITING  297 + - NOTIFICATION\_SERVICE\_DESCRIPTION\_SELECTED  298 + - NOTIFICATION\_SERVICE\_DESCRIPTION\_CHANGED  299 + - NOTIFICATION\_SERVICE\_DESCRIPTION\_VIOLATED  300 + - NOTIFICATION\_SOURCE\_INITIALIZED  301 + - NOTIFICATION\_DOWNLOAD\_STARTED  302 + - NOTIFICATION\_DOWNLOAD\_COMPLETED  303 + - NOTIFICATION\_DOWNLOAD\_ERROR  304 + - NOTIFICATION\_MULTI-ACCESS\_DELIVERY\_ESTABLISHED  305 + - NOTIFICATION\_MILTI-ACCESS\_DELIVERY\_CHANGED  306 + - type: object  307 + description: Notification payload.  308 +  309 + MediaPlayerErrorReason:  310 + description: 'Enumeration of media player errors.'  311 + anyOf:  312 + - type: string  313 + enum:  314 + - ERROR\_MEDIA\_ENTRY\_NOT\_FOUND  315 + - ERROR\_CONTENT\_NOT\_FOUND  316 + - ERROR\_MEDIA\_PLAYBACK  317 + - ERROR\_INVALID\_MEDIA\_ENTRY  318 + - ERROR\_INACCESSIBLE\_MEDIA\_TIME  319 + - ERROR\_UNSUPPORTED\_PROFILE  320 + - ERROR\_DOWNLOAD\_DEADLINE\_MISSED  321 + - ERROR\_MULTI-ACCESS\_DELIVERY\_UNAVAILABLE  322 + - type: object  323 + description: Error reason.  324 +  325 + MediaPlayerState:  326 + description: 'Enumeration of media player states.'  327 + anyOf:  328 + - type: string  329 + enum:  330 + - STATE\_INITIALIZED  331 + - STATE\_READY  332 + - STATE\_PRELOADED  333 + - STATE\_PLAYING  334 + - STATE\_PAUSED  335 + - STATE\_DOWNLOADING  336 + - STATE\_IDLE  337 + - type: object  338 + description: Media Player state.  No newline at end of file  ---/dev/null +++b/TS26512\_M6\_MediaSessionHandling.yaml  @@ -0,0 +1,73 @@  1 + openapi: 3.0.0  2 +  3 + info:  4 + title: 5GMS UE Media Session Handling  5 + version: 1.1.0  6 + description: |  7 + 5GMS UE Media Session Handling syntax  8 + © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  9 + All rights reserved.  10 +  11 + tags:  12 + - name: 5GMS UE Media Session Handling  13 + description: '5G Media Streaming: Media Session Handling'  14 +  15 + externalDocs:  16 + description: 'TS 26.512 V18.5.0; 5G Media Streaming (5GMS); Protocols'  17 + url: 'https://www.3gpp.org/ftp/Specs/archive/26\_series/26.512/'  18 +  19 + paths: {}  20 +  21 + components:  22 + schemas:  23 + 3GPPServiceURLParameters:  24 + type: object  25 + description: Parameters of the 3GPP Service URL for 5G Media Streaming  26 + required:  27 + - serviceId  28 + properties:  29 + serviceId:  30 + type: string  31 + description: An External Service Identifier that resolves to a Provisioning Session in the 5GMS System.  32 + afHostAddress:  33 + type: array  34 + minItems: 0  35 + items:  36 + $ref: 'TS26510\_CommonData.yaml#/components/schemas/EndpointAddressWithOptionalPort'  37 + description: The Fully Qualified Domain Name and optional port number of a 5GMS AF endpoint to be used by the Media Session Handler at reference point M5 with the format hostname[:port].  38 + accessToken:  39 + type: string  40 + description: A token that is presented by the Media Session Handler to the 5GMS AF at reference point M5 that asserts its right to invoke the media session handling operations exposed by the 5GMS AF.  41 + serviceOperationPoint:  42 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/ServiceOperationPoint'  43 + description: A reference to the target Service Operation Point of the 5G Media Streaming session.  44 + estimatedVolume:  45 + $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'  46 + description: A reference to the target Service Operation Point of the 5G Media Streaming sessionAn estimate of the volume of media data to be transferred between the 5GMS Client and the 5GMS AS at reference point M4 during the 5G Media Streaming session.  47 + mediaEntryPoint:  48 + $ref: 'TS26510\_CommonData.yaml#/components/schemas/Url'  49 + description: A Media Entry Point reference expressed as a fully qualified URL.  50 + multipathProtocol:  51 + type: array  52 + minItems: 0  53 + items:  54 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/MultiAccessTransportProtocolType'  55 + description: A multipath transport protocol to be used for multi-access media delivery at reference point M4.  56 + minPaths:  57 + type: integer  58 + description: The minimum number of subflows or paths to be used for multi-access media delivery at reference point M4.  59 + maxPaths:  60 + type: integer  61 + description: The maximum number of subflows or paths to be used for multi-access media delivery at reference point M4.  62 + contentType:  63 + type: array  64 + minItems: 0  65 + items:  66 + type: string  67 + description: An array of content type strings conforming to section 5 of RFC 2045 [57] identifying type of Media Entry Points that are acceptable to the Media Stream Handler (Media Player or Media Streamer).  68 + profile:  69 + type: array  70 + minItems: 0  71 + items:  72 + type: string  73 + description: Fully-qualified term identifiers from a controlled vocabulary specified outside the scope of the present document identifying profiles of Media Entry Points that are acceptable to the Media Stream Handler (Media Player or Media Streamer). The term identifier shall be formatted as a URI according to RFC 3986.  No newline at end of file  ---/dev/null +++b/TS26512\_M7\_M11\_MediaStreamHandling.yaml  @@ -0,0 +1,128 @@  1 + openapi: 3.0.0  2 +  3 + info:  4 + title: 5GMS UE Media Stream Handling  5 + version: 1.1.0  6 + description: |  7 + 5GMS UE Media Stream Handling syntax  8 + © 2024, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  9 + All rights reserved.  10 +  11 + tags:  12 + - name: 5GMS UE Media Stream Handling  13 + description: '5G Media Streaming: Media Stream Handling'  14 +  15 + externalDocs:  16 + description: 'TS 26.512 V18.5.0; 5G Media Streaming (5GMS); Protocols'  17 + url: 'https://www.3gpp.org/ftp/Specs/archive/26\_series/26.512/'  18 +  19 + paths: {}  20 +  21 + components:  22 + schemas:  23 + MediaPlayerConfiguration:  24 + type: object  25 + description: Configuration of 5GMS media delivery session by 5GMS-Aware Application at reference point M7 or by the Media Session Handler at reference point M11.  26 + properties:  27 + sessionId:  28 + type: string  29 + description: A media delivery session identifier for the downlink media streaming session.  30 + source:  31 + type: object  32 + description: Provides the MPD and all contained information.  33 + consumptionMode:  34 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/MediaOperationMode'  35 + description: >  36 + In case of live consumption mode, the target latency is maintained, if specified in the service description.  37 + In case of vod consumption mode, the latency is set by the application and the latency settings are ignored.  38 + maxBufferTime:  39 + type: integer  40 + description: Maximum buffer time in milliseconds for the service.  41 + serviceDescriptionId:  42 + type: string  43 + description: Selects a service description by selecting an identifier.  44 + serviceDescriptions:  45 + type: array  46 + items:  47 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/ServiceDescription'  48 + description: Service description parameters as defined in annex K of ISO/IEC 23009-1. This allows the application to define additional service descriptions beyond those defined in the MPD.  49 + mediaSettings:  50 + type: array  51 + items:  52 + $ref: 'TS29514\_Npcf\_PolicyAuthorization.yaml#/components/schemas/MediaType'  53 + description: Sets the selected Adaptation Set based on the available Adaptation Sets for each media type.  54 + metricsConfiguration:  55 + type: array  56 + items:  57 + type: object  58 + description: Zero or more sets of settings for collecting metrics in relation to the downlink media streaming session.  59 + multiAccessConfiguration:  60 + type: object  61 + description: Configuration of multi-access media delivery at reference point M4d. If omitted, multi-access delivery is disabled.  62 + properties:  63 + transportProtocols:  64 + type: array  65 + minItems: 1  66 + items:  67 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/MultiAccessTransportProtocolType'  68 + description: A non-empty array of enumerated values to be used by the Media Player for multi-access media delivery at reference point M4d.  69 + minPaths:  70 + type: integer  71 + description: Minimum number of subflows or paths used by the Media Player for multi-access delivery at reference point M4d.  72 + maxPaths:  73 + type: integer  74 + description: Maximum number of subflows or paths used by the Media Player for multi-access delivery at reference point M4d.  75 +  76 + MediaPlayerDynamicStatus:  77 + type: object  78 + description: Dynamically changing status information that can be obtained from the Media Player via reference point M7d or M11d.  79 + properties:  80 + state:  81 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/MediaPlayerState'  82 + description: Enumerated value from list of media player states.  83 + averageThroughput:  84 + $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'  85 + description: Current average throughput computed in the ABR logic in bit/s.  86 + bufferLength:  87 + $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'  88 + description: Current length of the buffer for a given media type, in seconds.  89 + liveLatency:  90 + $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'  91 + description: Current live stream latency in seconds based on the latency measurement.  92 + mediaSettings:  93 + type: array  94 + items:  95 + type: object  96 + description: Current media settings for each media type based on the CMAF Header and the MPD information based on the selected Adaptation Set for this media type.  97 + mediaTime:  98 + $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'  99 + description: Current media playback time from media playback platform.  100 + playbackRate:  101 + $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'  102 + description: The current rate of playback.  103 + availableServiceDescriptions:  104 + type: array  105 + items:  106 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/ServiceDescription'  107 + description: List of available selectable service descriptions with an id to select from.  108 + availableMediaOptions:  109 + type: array  110 + items:  111 + type: object  112 + description: List of available media options that can be selected by the application based on the capability discovery and the subset information.  113 + serviceOperationPoints:  114 + type: array  115 + items:  116 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/ServiceOperationPoint'  117 + description: Set of Service Operation Points declared in the presentation manifest (e.g. DASH MPD) of the current media presentation.  118 + operativeServiceOperationPoint:  119 + type: integer  120 + description: A zero-based index into the serviceOperationPoints array indicating the Service Operation Point currently operative in the playback session.  121 + metrics:  122 + type: array  123 + description: Data blob of metrics for each configured metrics collecting scheme.  124 + items:  125 + type: object  126 + multiAccessConnectionStatus:  127 + $ref: 'TS26512\_CommonData.yaml#/components/schemas/MultiAccessConnectionStatus'  128 + description: Status information of multi-access delivery connection instance.  No newline at end of file |

end CHANGEs