**3GPP TSG SA WG5 Meeting #162 S5-253657**

**Goteborg, SWEDEN 25 - 29 August 2025**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **32.291** | **CR** | **0629** | **rev** | **1** | **Current version:** | **19.3.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Rel-19 CR 32.291 Correction on the UPF ID |
|  |  |
| ***Source to WG:*** | China Mobile Com. Corporation |
| ***Source to TSG:*** | SA5 |
|  |  |
| ***Work item code:*** | 5GS\_Ph1-DCH |  | ***Date:*** | 2025-08-15 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | Since the billing side needs to regularly conduct data consistency checks with the network side to avoid CDR loss during transmission, and the data provided by the network side during these checks includes the UPF ID.However,the CDRs transmitted to the billing side do not carry the UPF ID in some cases.  |
|  |  |
| ***Summary of change:*** | The UPF ID field will be made mandatory. |
|  |  |
| ***Consequences if not approved:*** | This will lead to mismatch between the two sides' data and make it difficult to locate the root cause of the inconsistency. |
|  |  |
| ***Clauses affected:*** | 6.1.6.2.2.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** | **X** |  |  O&M Specifications | TS 32.255 CR 0600 |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Revision of S5-253319 |

|  |
| --- |
| **First Change** |

###### 6.1.6.2.2.4 Type MultipleUnitInformation

This clause is additional attributes of the type MultipleUnitInformationdefined in clause 6.1.6.2.1.8 for 5G data connectivity charging described in 3GPP TS 32.255[30].

Table 6.1.6.2.2.4-1: 5G Data Connectivity Specified attribute of type MultipleUnitInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| uPFID | NfInstanceId | OM | 0..1 | UPF id |  |

|  |
| --- |
| **End of Change** |