**3GPP TSG-SA WG6 Meeting #68 S6-253410**

**Gothenburg, Sweden 25th – 29th August 2025 (revision of S6-253024)**

**Source: Netherlands Police**

**Title: Pseudo-CR on Scenario for Discreet monitoring of one to one MCVideo push**

**Spec: 3GPP TR 23700-37-020**

**Agenda item: 9.1**

**Document for: Approval**

**Contact: keesdotverweijatpolitiedotnl**

**1. Introduction**

A scenario detailing one to one MCVideo push is added to clarify the usecase and identify technical impact. The text originates from TR 23.784, but has been enhanced as required.

**2. Reason for Change**

Scenario for one to one MCVideo push is missing.

**4. Proposal**

It is proposed to agree the following changes to 3GPP TR 23700-37-020 v 0.2.0.

\* \* \* First Change \* \* \* \*

## 4.5 Scenario 4: Discreet monitoring of one to one MCVideo push

This scenario describes the case where authorized MC user A requests discreet monitoring for MC user B where MC user B is within the authority of authorized MC user A, and authorized MC user A receives MCVideo streams initiated or received by target MC user B. As a one to one MCVideo push is procedurally identical to an MCVideo private call, the scenarios are the same as those described within the present document in subclause 4.2 for MCVideo private call.

\* \* \* End of Changes \* \* \* \*