**3GPP TSG-SA WG6 Meeting #68 S6-253414**

**Gothenburg, Sweden 25th – 29th August 2025 (revision of S6-253028)**

**Source: Netherlands Police**

**Title: Pseudo-CR on Scenario for Discreet monitoring of** **one from server MCVideo pull**

**Spec: 3GPP TR 23700-37-020**

**Agenda item: 9.1**

**Document for: Approval**

**Contact: keesdotverweijatpolitiedotnl**

**1. Introduction**

A scenario detailing one from server MCVideo pull is added to clarify the usecase and identify technical impact. The text originates from TR 23.784, but has been enhanced as required.

**2. Reason for Change**

Scenario for one from server MCVideo pull is missing.

**3. Proposal**

It is proposed to agree the following changes to 3GPP TR 23700-37-020 v 0.2.0.

\* \* \* First Change \* \* \* \*

## 4.9 Scenario 8: Discreet monitoring of one from server MCVideo pull

This scenario describes the case where authorized MC user A requests discreet monitoring for MC user B where MC user B is within the authority of authorized MC user A, and where authorized MC user A receives MCVideo pulls from the MC system initiated by target MC user B. In figure 4.9-1 below, MC user A and target MC user B have the same primary MC system, MC system A.



Figure 4.9-1: Discreet monitoring of MCVideo pull from server

The scenario consists of the following aspects:

- Authorized MC user A identifies MC user B as the target for discreet monitoring. MC system A verifies that MC user A is authorized to perform discreet monitoring on MC user B. This aspect takes place before any communications involving MC user B can be subject to discreet monitoring.

- Target MC user B initiates an MCVideo pull from the MCVideo server.

- MC system A provides MC service client A with information concerning the initiation of the MCVideo pull, and provides the MCVideo media sent from the MCVideo server to target MC user B.

\* \* \* End of Changes \* \* \* \*