**3GPP TSG-SA WG6 Meeting #68 S6-253436**

**Gothenburg, Sweden 25th – 29th August 2025 (was S6-253403)**

**(was S6-253013)**

**Source: Motorola Solutions**

**Title: Scenarios for Non session-based Recording support for MCPTT, MCVIDEO messages.**

**Spec: 3GPP TR 23.700-39 V0.2.0**

**Agenda item: 9.2**

**Document for: Approval**

**Contact: Adinarayana Setty (**[**Adinarayana.setty@motorolasolutions.com**](mailto:Adinarayana.setty@motorolasolutions.com)**)**

**Harish N (**[**harish.negalaguli@motorolasolutions.com**](mailto:harish.negalaguli@motorolasolutions.com)**)**

**1. Introduction**

This contribution proposes scenarios for supporting Non session based recording support for MCPTT, MCVideo messages.

**2. Reason for Change**

**3. Proposal**

It is proposed to agree the following changes to 3GPP TR 23.700-39 V0.2.0.

\* \* \* First Change \* \* \* \*

### 4.1.x Scenario X1: Recording support for Non communication based MCPTT messages.



Figure 4.1.x-1: Functional entities for supporting recording of Non communication based MCPTT messages.

This scenario describes the recording support for Non communication based MCPTT service between MC users.

* MC user A, MC user B (MCPTT ID A, MCPTT ID B) has/have been set as the target for the recording by a Recording admin user.
* Target MC users can be part of Non communication based MCPTT Services such as, MC user authentication and authorization for MCPTT services, Affiliation and De-affiliation to/from MCPTT Groups, Subscription and for functional alias etc.
* When the recording target MC users participate in any Non communication based MCPTT service activity, such MCPTT service activity needs to be recorded.

NOTE 1: Above provided Non communication based MCPTT service features are not an exhaustive list, but it should be noted that, this scenario is applicable for all Non communication based MCPTT service feature recording.

### 4.1.y Scenario X2: Recording support for Non communication based MCVideo messages.



Figure 4.1.y-1: Functional entities for supporting recording of Non communication based MCVideo messages.

This scenario describes the recording support for Non communication based MCVideo service messages between MC users.

* MC user A, MC user B (MCVideo ID A, MCVideo ID B) has/have been set as the target for recording by a Recording admin user.
* Target MC users can be part of Non communication based MCVideo services such as Affiliation and de-affiliation to/from MCVideo group(s), Functional alias management, User authentication and authorization for MCVideo service, Location information (on-network) etc.
* When the recording target MC users participate in any Non communication based MCVideo service activity, such MCVideo service activity needs to be recorded.

NOTE 2: Above provided Non communication based MCVideo service features are not an exhaustive list, but it should be noted that, this scenario is applicable for all Non communication based MCVideo service features recording.

\* \* \* End of Changes \* \* \* \*