**3GPP TSG-SA WG6 Meeting #68 S6-253407**

**Gothenburg, Sweden 25th – 29th August 2025 (revision of S6-253021)**

**Source: Netherlands Police**

**Title: Pseudo-CR on Scenario for Discreet** **monitoring of MCPTT and MCVideo private calls**

**Spec: 3GPP TR 23700-37-020**

**Agenda item: 9.1**

**Document for: Approval**

**Contact: keesdotverweijatpolitiedotnl**

**1. Introduction**

A scenario detailing MCPTT and MCVideo private calls is added to clarify the usecase and identify technical impact. The text originates from TR 23.784, but has been enhanced as required.

**2. Reason for Change**

Scenario for MCPTT and MCVideo private calls is missing.

**3. Proposal**

It is proposed to agree the following changes to 3GPP TR 23700-37-020 v 0.2.0.

\* \* \* First Change \* \* \* \*

## 4.2 Scenario 1: Discreet monitoring of MCPTT and MCVideo private calls

This scenario describes the case where authorized MC user A requests discreet monitoring for communications involving target MC user B where MC user A and MC user B are served by the same MC system, MC system A and target MC service user B is within the authority of authorized MC user A. The scenario is illustrated in figure 4.2-1 below.



Figure 4.2-1: Discreet monitoring of MCPTT or MCVideo private call in single MC system

The scenario consists of the following aspects:

- Authorized MC user A identifies MC user B as the target for discreet monitoring. MC system A verifies that MC user A is authorized to perform discreet monitoring on MC user B. This aspect takes place before any communications involving MC user B can be subject to discreet monitoring.

- Target MC user B places or receives an MCPTT or MCVideo private call to or from MC user C.

- MC system A provides MC service client A with information concerning the initiation of the call, including the identity of MC user C.

- MC system A provides the media exchanged between the target MC user B and MC user C in the private call.

- When the private call completes, the call completion is conveyed to MC service client A.

NOTE 1: The scenario also applies to emergency private calls.

NOTE 2: The scenario also applies to first-to-answer call.

NOTE 3: The scenario also applies to ambient listening call.

NOTE 4: The scenario also applies to forwarded private calls.

NOTE 5: The scenario also applies to transferred private calls.

\* \* \* End of Change \* \* \* \*