**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Nnef\_VFLTraining OpenAPI |
|  |  |
| ***Source to WG:*** | , vivo |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | AIML\_CN |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | 23.288 clause 12.2 defines the Nnef\_VFLTraining API, which enables an Untrusted AF acting as a VFL server to request from an NWDAF to act as a VFL client, as described in detail in 23.288 clause 6.2H. |
|  |  |
| ***Summary of change:*** | Defined the OpenAPI for the Nnef\_VFLTraining API. |
|  |  |
| ***Consequences if not approved:*** | Not fulfilled stage 2 requirements and non workable end-to-end VFL procedures. |
|  |  |
| ***Clauses affected:*** | 5.1, A.44 (new) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | This CR introduces a new OpenAPI:TS29522\_VFLTraining.yaml |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* First Change \*\*\*

5.1 Introduction

The NEF Northbound APIs are a set of APIs defining the related procedures and resources for the interaction between the NEF and the AF.

Tables 5.1-1 summarizes the APIs defined in this specification.

**Table 5.1-1: API Descriptions**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Service Name** | **Clause defined** | **Description** | **OpenAPI Specification File** | **API Name** | **Annex** |
| TrafficInfluence | 5.4 | Traffic Influence API | TS29522\_TrafficInfluence.yaml | 3gpp-traffic-influence | A.2 |
| NiddConfigurationTrigger | 5.5 | NIDD (Non-IP Data Delivery) Configuration Trigger API | TS29522\_NiddConfigurationTrigger.yaml | 3gpp-nidd-configuration-trigger | A.3 |
| AnalyticsExposure | 5.6 | Analytics Exposure API | TS29522\_AnalyticsExposure.yaml | 3gpp-analyticsexposure | A.4 |
| 5GLANParameterProvision | 5.7 | 5G LAN Parameter Provision API | TS29522\_5GLANParameterProvision.yaml | 3gpp-5glan-pp | A.5 |
| ApplyingBdtPolicy | 5.8 | Applying BDT Policy API | TS29522\_ApplyingBdtPolicy.yaml | 3gpp-applying-bdt-policy | A.6 |
| IPTVConfiguration | 5.9 | IPTV Configuration API | TS29522\_IPTVConfiguration.yaml | 3gpp-iptvconfiguration | A.7 |
| LpiParameterProvision | 5.10 | LPI (Location Privacy Indicator) Parameter Provision API | TS29522\_LpiParameterProvision.yaml | 3gpp-lpi-pp | A.8 |
| ServiceParameter | 5.11 | Service Parameter API | TS29522\_ServiceParameter.yaml | 3gpp-service-parameter | A.9 |
| ACSParameterProvision | 5.12 | ACS Parameter Provision API | TS29522\_ACSParameterProvision.yaml | 3gpp-acs-pp | A.10 |
| MoLcsNotify | 5.13 | MO LCS Notify API | TS29522\_MoLcsNotify.yaml | 3gpp-mo-lcs-notify | A.11 |
| AKMA | 5.14 | AKMA API | TS29522\_AKMA.yaml | 3gpp-akma | A.12 |
| TimeSyncExposure | 5.15 | Time Sync Exposure API | TS29522\_TimeSyncExposure.yaml | 3gpp-time-sync | A.13 |
| EcsAddressProvision | 5.16 | ECS Address Provision API | TS29522\_EcsAddressProvision.yaml | 3gpp-ecs-address-provision | A.14 |
| AMPolicyAuthorization | 5.17 | AM Policy Authorization API | TS29522\_AMPolicyAuthorization.yaml | 3gpp-am-policyauthorization | A.15 |
| AMInfluence | 5.18 | AM Influence API | TS29522\_AMInfluence.yaml | 3gpp-am-influence | A.16 |
| MBSTMGI | 5.19 | MBS TMGI API | TS29522\_MBSTMGI.yaml | 3gpp-mbs-tmgi | A.17 |
| MBSSession | 5.20 | MBS Session API | TS29522\_MBSSession.yaml | 3gpp-mbs-session | A.18 |
| EASDeployment | 5.21 | EAS Deployment API | TS29522\_EASDeployment.yaml | 3gpp-eas-deployment | A.19 |
| ASTI | 5.22 | ASTI API | TS29522\_ASTI.yaml | 3gpp-asti | A.20 |
| DataReporting | 5.23 | DataReporting API | TS29522\_DataReporting.yaml | 3gpp-data-reporting | A.21 |
| DataReportingProvisioning | 5.24 | DataReportingProvisioning API | TS29522\_DataReportingProvisioning.yaml | 3gpp-data-reporting-provisioning | A.22 |
| UEId | 5.25 | UE ID API | TS29522\_UEId.yaml | 3gpp-ueid | A.23 |
| MBSUserService | 5.26 | MBSUserService API | TS29522\_MBSUserService.yaml | 3gpp-mb-us | A.24 |
| MBSUserDataIngestSession | 5.27 | MBSUserDataIngestSession API | TS29522\_MBSUserDataIngestSession.yaml | 3gpp-mb-ud-ingest | A.25 |
| MSEventExposure | 5.28 | MSEventExposure API | TS29522\_MSEventExposure.yaml | 3gpp-ms-event-exposure | A.26 |
| MBSGroupMsgDelivery | 5.29 | MBSGroupMsgDelivery API | TS29522\_MBSGroupMsgDelivery.yaml | 3gpp-mbs-group-msg | A.27 |
| DNAIMapping | 5.30 | DNAIMapping API | TS29522\_DNAIMapping.yaml | 3gpp-dnai-mapping | A.28 |
| PDTQPolicyNegotiation | 5.31 | PDTQPolicyNegotiation API | TS29522\_PDTQPolicyNegotiation.yaml | 3gpp-pdtq-policy-negotiation | A.29 |
| MemberUESelectionAssistance | 5.32 | MemberUESelectionAssistance API | TS29522\_MemberUESelectionAssistance.yaml | 3gpp-musa | A.30 |
| GroupParametersProvisioning | 5.33 | Group Parameters Provisioning API | TS29522\_GroupParametersProvisioning.yaml | 3gpp-grp-pp | A.31 |
| SliceParamProvision | 5.34 | Network Slice Parameters Provisioning API | TS29522\_SliceParamProvision.yaml | 3gpp-slice-pp | A.32 |
| UEAddress | 5.35 | UE Address API | TS29522\_UEAddress.yaml | 3gpp-ue-address | A.33 |
| ECSAddress | 5.36 | ECS Address Configuration Information API | TS29522\_ECSAddress.yaml | 3gpp-ecs-address | A.34 |
| RSLPPIParametersProvisioning | 5.37 | RSLPPI Parameters Provisioning API | TS29522\_RSLPPIParametersProvisioning.yaml | 3gpp-rslppi-pp | A.35 |
| AddressingParamProvision | 5.38 | Addressing Parameters Provisioning API | TS29522\_AddressingParamProvision.yaml | 3gpp-addr-pp | A.36 |
| UAVFlightAssistance | 5.39 | UAV Flight Assistance API | TS29522\_UAVFlightAssistance.yaml | 3gpp-uav-fa | A.37 |
| CagInfoParamProvision | 5.40 | CAG Information Parameters Provisioning API | TS29522\_CagInfoParamProvision.yaml | 3gpp-caginfo-pp | A.38 |
| ImsSessionManagement | 5.42 | ImsSessionMangement API | TS29522\_ImsSessionManagement.yaml | 3gpp-ims-sm | A.40 |
| ImsEventExposure | 5.43 | ImsEventExposure API | TS29522\_ImsEventExposure.yaml | 3gpp-ims-ee | A.41 |
| ImsParamProvision | 5.44 | ImsParamProvision API | TS29522\_ImsParamProvision.yaml | 3gpp-ims-pp | A.42 |
| AIoT | 5.45 | AIoT API | TS29522\_AIoT.yaml | 3gpp-aiot | A.43 |
| VFLTraining | 5.46 | VFLTraining API | TS29522\_VFLTraining.yaml | 3gpp-vfl-training | A.44 |
| VFLNFDiscovery | 5.48 | VFLNFDiscovery API | TS29522\_VFLNFDiscovery.yaml | 3gpp-vfl-nf-discovery | A.46 |

\*\*\* Next Change \*\*\*

A.44 VFLTraining API

openapi: 3.0.0

info:

 title: 3gpp-vfl-training

 version: 1.0.0-alpha.1

 description: |

 API for VFL Training.

 © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 29.522 V19.4.0; 5G System; Network Exposure Function Northbound APIs.

 url: 'https://www.3gpp.org/ftp/Specs/archive/29\_series/29.522/'

servers:

 - url: '{apiRoot}/3gpp-vfl-training/v1'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in clause 5.2.4 of 3GPP TS 29.122.

security:

 - {}

 - oAuth2ClientCredentials: []

paths:

 /{afId}/subscriptions:

 parameters:

 - name: afId

 in: path

 description: Represents the identifier of the AF

 required: true

 schema:

 type: string

 get:

 summary: Retrieve all the active VFL Training Subscriptions.

 operationId: GetVFLTrainingSubscriptions

 tags:

 - VFL Training Subscriptions (Collection)

 responses:

 '200':

 description: >

 OK. All the Individual VFL Training Subscription resource(s) managed

 by the NEF are returned.

 If there are no active Individual VFL Training Subscription resources

 at the NEF, an empty array is returned.

 content:

 application/json:

 schema:

 type: array

 items:

 $ref: '#/components/schemas/VflTrainingSubs'

 minItems: 0

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 post:

 summary: Create a new Individual VFL Training Subscription.

 operationId: CreateVFLTrainingSubscription

 tags:

 - VFL Training Subscriptions (Collection)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VflTrainingSubs'

 responses:

 '201':

 description: >

 Created. A representation of the created Individual VFL Training Subscription

 resource is returned in the response body.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VflTrainingSubs'

 headers:

 Location:

 description: >

 Contains the URI of the newly created resource.

 required: true

 schema:

 type: string

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 callbacks:

 VFLTrainingNotification:

 '{$request.body#/notifUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: 'TS29520\_Nnwdaf\_VFLTraining.yaml#/components/schemas/VflTrainingNotify'

 responses:

 '204':

 description: >

 No Content. The notification is successfully received and acknowledged.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 /{afId}/subscriptions/{subId}:

 parameters:

 - name: afId

 in: path

 description: Represents the identifier of the AF.

 required: true

 schema:

 type: string

 - name: subId

 in: path

 description: Represents the identifier of the Individual VFL Training Subscription resource.

 required: true

 schema:

 type: string

 get:

 summary: Retrieve an existing Individual VFL Training Subscription resource.

 operationId: GetVFLTrainingSubscription

 tags:

 - Individual VFL Training Subscription (Document)

 responses:

 '200':

 description: >

 OK. The requested Individual VFL Training Subscription resource is

 successfully returned in the response body.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VflTrainingSubs'

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '406':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/406'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 put:

 summary: Request the update of an existing Individual VFL Training Subscription resource.

 operationId: UpdateVFLTrainingSubscription

 tags:

 - Individual VFL Training Subscription (Document)

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VflTrainingSubs'

 responses:

 '200':

 description: >

 OK. The Individual VFL Training Subscription resource is successfully updated

 and a representation of the updated resource is returned in the response body.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VflTrainingSubs'

 '204':

 description: >

 No Content. The Individual VFL Training Subscription resource is successfully

 updated and no content is returned in the response body.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 patch:

 summary: Request modification of an existing Individual VFL Training Subscription resource.

 operationId: ModifyVFLTrainingSubscription

 tags:

 - Individual VFL Training Subscription (Document)

 requestBody:

 required: true

 content:

 application/merge-patch+json:

 schema:

 $ref: '#/components/schemas/VflTrainingSubsPatch'

 responses:

 '200':

 description: >

 OK. The Individual VFL Training Subscription resource is successfully modified

 and a representation of the updated resource is returned in the response body.

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/VflTrainingSubs'

 '204':

 description: >

 No Content. The Individual VFL Training Subscription resource is successfully

 modified and no content is returned in the response body.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '411':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/413'

 '415':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/415'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

 delete:

 summary: Request deletion of an existing Individual VFL Training Subscription resource.

 operationId: DeleteVFLTrainingSubscription

 tags:

 - Individual VFL Training Subscription (Document)

 responses:

 '204':

 description: >

 No Content. The Individual VFL Training Subscription resource is

 successfully deleted.

 '307':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/307'

 '308':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/308'

 '400':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/400'

 '401':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/401'

 '403':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/403'

 '404':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/404'

 '429':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/429'

 '500':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29122\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29122\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{tokenUrl}'

 scopes: {}

 schemas:

 VflTrainingSubs:

 description: Represents VFL Training subscription.

 type: object

 properties:

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 notifCorrId:

 type: string

 description: Notification correlation identifier.

 vflTrainSubs:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_VFLTraining.yaml#/components/schemas/VflTrainingSub'

 minItems: 1

 extNwdafId:

 type: string

 description: >

 Contains the external identifier of the NWDAF that is being requested to act

 as VFL client.

 reportingReqs:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

 suppFeat:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 required:

 - notifUri

 - notifCorrId

 - vflTrainSubs

 - extNwdafId

 VflTrainingSubsPatch:

 description: Represents contents for modifying a VFL Training subscription.

 type: object

 properties:

 vflTrainSubs:

 type: array

 items:

 $ref: 'TS29520\_Nnwdaf\_VFLTraining.yaml#/components/schemas/VflTrainingSub'

 minItems: 1

 notifUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 notifCorrId:

 type: string

 description: Notification correlation identifier.

 reportingReqs:

 $ref: 'TS29523\_Npcf\_EventExposure.yaml#/components/schemas/ReportingInformation'

\*\*\* End of Changes \*\*\*