**3GPP TSG CT WG3 Meeting #142 *C3-253xxx***

**Goteborg, SE, 25th – 29th August, 2025 was C3-253428**

|  |
| --- |
| *CR-Form-v12.3* |
| **CHANGE REQUEST** |
|  |
|  | **29.548** | **CR** | **0056** | **rev** | **1** | **Current version:** | **19.3.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Complete the definition of the UE-to-UE policy of the Multi-modal SEALDD policy |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | CT3 |
|  |  |
| ***Work item code:*** | XRM\_Ph2\_App |  | ***Date:*** | 2025-08-29 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | The definition of the UEToUEPolicy data structure needs to be completed by completing the definition of the encoding of the ProximityThresholds data structure so that the related Editor's Note can be resolved.The current definition of the ProximityThresholds data structure is correct and aligned with the related stage 2 requirements. |
|  |  |
| ***Summary of change:*** | This CR proposes to:* Address the above-detailed necessary updates/corrections to complete the definition of the UE-to-UE Policy.
 |
|  |  |
| ***Consequences if not approved:*** | * The above-detailed necessary updates/corrections are not addressed and the UE-to-UE Policy definition is not complete in stage 3.
 |
|  |  |
| ***Clauses affected:*** | 6.5.6.2.17 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ... |
|  |  |
| ***Other comments:*** | This CR does not impact the OpenAPI descriptions of the APIs. |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* Start of changes \* \* \* \*

##### 6.6.6.2.17 Type: ProximityThresholds

Table 6.4.6.2.17-1: Definition of type ProximityThresholds

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| minUeToUedist | number | C | 0..1 | Contains the threshold minimum linear distance between the UEs, expressed in units of meters.(NOTE) |  |
| avgUeToUedist | number | C | 0..1 | Contains the threshold average linear distance between the UEs, expressed in units of meters.(NOTE) |  |
| maxUeToUedist | number | C | 0..1 | Contains the threshold maximum linear distance between the UEs, expressed in units of meters.(NOTE) |  |
| NOTE: At least one of these attributes shall be present. |

\* \* \* \* End of changes \* \* \* \*