* **The 6G RAN shall support Multi-RAT Spectrum Sharing between 6GR and NR.**
* **6G RAT shall support Spectrum Aggregation (e.g. Carrier Aggregation) for both uplink and downlink, and for both co-located and non-co-located TRPs**
* **6G RAN architecture shall support enhanced service awareness in RAN**