**3GPP TSG-WG SA2 Meeting #170S2-2506831r02**

**25 - 29 August 2025, Goteborg, Sweden (revision of S2-250xxxx)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **23.501** | **CR** |  | **rev** |  | **Current version:** | **19.4.0** |  |
|  | | | | | | | | |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm" \l "_blank)*** *on using this form: comprehensive instructions can be found at  <http://www.3gpp.org/Change-Requests>.* | | | | | | | | |
|  | | | | | | | | |

X

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Support for Dynamic Network Identity | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | China Mobile, MediaTek Inc | | | | | | | | | |
| ***Source to TSG:*** | SA2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | DNI | | | | |  | ***Date:*** | | | 2025-05-09 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | ***B*** |  | | | | | ***Release:*** | | | *Rel-20* |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Network Identity has long been introduced in stage 1, for the purpose of presenting the PLMN name of the service network, and is allowed to be changed at any time as defined in TS 22.042.  While in existing stage 2 specifications, how the network identity can be changed is not defined, which may further prevent the flexibility of network identity such as transferring updated information via dynamically assigned network identity to the end user behind the UE, e.g., specific tariff plan or relationship plan of the UE, thus the user can be aware of these service related inforamtion which is currently invisible to the user.  Considering the requirements above and potential extensions on the dynamic information presentation, it would be beneficial for both the Operator and the end user to enhance the dynamically assigned Network Identity as bridge of mutual awareness. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * Description for Network Identity is complemented based on existing capabilities. * The AMF is enhanced with receiving authorized Network Identity from the PCF for decision of Network Identity in use. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Dynamic change of network identity would remain unsupported in stage 2, and it is still not possible to present specific information to the end users. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 3.2, 5.X | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Start of Changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 22.261: "Service requirements for next generation new services and markets; Stage 1".

[3] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[4] 3GPP TS 23.203: "Policies and Charging control architecture; Stage 2".

[5] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS); Stage 2".

[6] 3GPP TS 24.011: "Point-to-Point (PP) Short Message Service (SMS) support on mobile radio interface: Stage 3".

[7] IETF RFC 7157: "IPv6 Multihoming without Network Address Translation".

[8] IETF RFC 4191: "Default Router Preferences and More-Specific Routes".

[9] IETF RFC 2131: "Dynamic Host Configuration Protocol".

[10] IETF RFC 4862: "IPv6 Stateless Address Autoconfiguration".

[11] ITU‑T Recommendation I.130: "Method for the characterization of telecommunication services supported by an ISDN and network capabilities of an ISDN".

[12] ITU‑T Recommendation Q.65: "The unified functional methodology for the characterization of services and network capabilities".

[13] 3GPP TS 24.301: "Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS): Stage 3".

[14] Void.

[15] 3GPP TS 23.228: "IP Multimedia Subsystem (IMS); Stage 2".

[16] 3GPP TS 22.173: "IMS Multimedia Telephony Service and supplementary services; Stage 1".

[17] 3GPP TS 23.122: "Non-Access-Stratum (NAS) functions related to Mobile Station in idle mode".

[18] 3GPP TS 23.167: "3rd Generation Partnership Project; Technical Specification Group Services and Systems Aspects; IP Multimedia Subsystem (IMS) emergency sessions".

[19] 3GPP TS 23.003: "Numbering, Addressing and Identification".

[20] IETF RFC 7542: "The Network Access Identifier".

[21] 3GPP TS 23.002: "Network Architecture".

[22] 3GPP TS 23.335: "User Data Convergence (UDC); Technical realization and information flows; Stage 2".

[23] 3GPP TS 23.221: "Architectural requirements".

[24] 3GPP TS 22.153: "Multimedia priority service".

[25] 3GPP TS 22.011: "Service Accessibility".

[26] 3GPP TS 23.401: "General Packet Radio Service (GPRS) enhancements for Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access".

[27] 3GPP TS 38.300: "NR; NR and NG-RAN Overall Description".

[28] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol Specification".

[29] 3GPP TS 33.501: "Security architecture and procedures for 5G system".

[30] 3GPP TS 36.300: "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Universal Terrestrial Radio Access Network (E-UTRAN); Overall description; Stage 2".

[31] 3GPP TS 37.340: "Evolved Universal Terrestrial Radio Access (E-UTRA) and NR; Multi-connectivity; Stage 2".

[32] 3GPP TS 23.214: "Architecture enhancements for control and user plane separation of EPC nodes; Stage 2".

[33] 3GPP TS 22.101: "3rd Generation Partnership Project; Technical Specification Group Services and Systems Aspects; Service aspects; Service principles".

[34] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[35] 3GPP TS 33.126: "Lawful Interception Requirements".

[36] 3GPP TS 23.682: "Architecture enhancements to facilitate communications with packet data networks and applications".

[37] 3GPP TS 22.280: "Mission Critical Services Common Requirements (MCCoRe); Stage 1".

[38] 3GPP TS 23.379: "Functional architecture and information flows to support Mission Critical Push To Talk (MCPTT); Stage 2".

[39] 3GPP TS 23.281: "Functional architecture and information flows to support Mission Critical Video (MCVideo); Stage 2".

[40] 3GPP TS 23.282: "Functional architecture and information flows to support Mission Critical Data (MCData); Stage 2".

[41] 3GPP TS 32.240: "Charging management; Charging architecture and principles".

[42] 3GPP TS 38.401: "NG-RAN Architecture description".

[43] 3GPP TS 23.402: "Architecture enhancements for non-3GPP accesses".

[44] IETF RFC 4960: "Stream Control Transmission Protocol".

[45] 3GPP TS 23.503: "Policy and Charging Control Framework for the 5G System".

[46] 3GPP TS 23.041: "Public Warning System".

[47] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS); Stage 3".

[48] 3GPP TS 24.502: "Access to the 5G System (5GS) via non-3GPP access networks; Stage 3".

[49] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[50] 3GPP TS 38.304: "NR; User Equipment (UE) procedures in idle mode".

[51] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol specification".

[52] 3GPP TS 36.304: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) procedures in idle mode".

[53] Void.

[54] IETF RFC 4861: "Neighbor Discovery for IP version 6 (IPv6)".

[55] 3GPP TS 23.271: "Functional stage 2 description of Location Services (LCS)".

[56] 3GPP TS 23.060: "General Packet Radio Service (GPRS); Service description; Stage 2".

[57] IETF RFC 4555: "IKEv2 Mobility and Multihoming Protocol (MOBIKE)".

[58] 3GPP TS 29.510: "5G System: Network function repository services; Stage 3".

[59] 3GPP TS 29.502: "5G System: Session Management Services: Stage 3".

[60] IETF RFC 7296: "Internet Key Exchange Protocol Version 2 (IKEv2) ".

[61] 3GPP TS 23.380: "IMS Restoration Procedures".

[62] 3GPP TS 24.229: "IP multimedia call control protocol based on Session Initiation Protocol (SIP) and Session Description Protocol (SDP); Stage 3".

[63] 3GPP TS 23.292: "IP Multimedia Subsystem (IMS) centralized services; Stage 2".

[64] 3GPP TS 23.222: "Functional architecture and information flows to support Common API Framework for 3GPP Northbound APIs".

[65] 3GPP TS 29.244: "Interface between the Control Plane and the User Plane Nodes; Stage 3".

[66] 3GPP TS 32.421: "Telecommunication management; Subscriber and equipment trace; Trace concepts and requirements".

[67] 3GPP TS 32.290: "5G system; Services, operations and procedures of charging using Service Based Interface (SBI)".

[68] 3GPP TS 32.255: "5G Data connectivity domain charging; Stage 2".

[69] 3GPP TS 38.306: "NR; User Equipment -UE) radio access capabilities".

[70] 3GPP TS 36.306: "Evolved Universal Terrestrial Radio Access -E-UTRA); User Equipment -UE) radio access capabilities".

[71] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[72] Void.

[73] IETF RFC 2865: "Remote Authentication Dial In User Service (RADIUS)".

[74] IETF RFC 3162: "RADIUS and IPv6".

[75] 3GPP TS 29.281: "General Packet Radio System (GPRS) Tunnelling Protocol User Plane (GTPv1-U)".

[76] 3GPP TS 26.238: "Uplink streaming".

[77] 3GPP TR 26.939: "Guidelines on the Framework for Live Uplink Streaming (FLUS)".

[78] International Telecommunication Union (ITU), Standardization Bureau (TSB): "Operational Bulletin No. 1156"; http://handle.itu.int/11.1002/pub/810cad63-en (retrieved October 5, 2018).

[79] 3GPP TS 28.533: "Management and orchestration; Architecture framework".

[80] 3GPP TS 24.250: "Protocol for Reliable Data Service; Stage 3".

[81] IETF RFC 8684: "TCP Extensions for Multipath Operation with Multiple Addresses".

[82] IETF RFC 8803: "0-RTT TCP Convert Protocol".

[83] IEEE Std 802.1CB-2017: "IEEE Standard for Local and metropolitan area networks-Frame Replication and Elimination for Reliability".

[84] 3GPP TS 23.316: "Wireless and wireline convergence access support for the 5G System (5GS)".

[85] WiFi Alliance Technical Committee, Hotspot 2.0 Technical Task Group: "Hotspot 2.0 (Release 2) Technical Specification".

[86] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services".

[87] 3GPP TS 23.273: "5G System (5GS) Location Services (LCS); Stage 2".

[88] 3GPP TS 23.216: "Single Radio Voice Call Continuity (SRVCC); Stage 2".

[89] CableLabs DOCSIS MULPI: "Data-Over-Cable Service Interface Specifications DOCSIS 3.1, MAC and Upper Layer Protocols Interface Specification".

[90] BBF TR-124 issue 5: "Functional Requirements for Broadband Residential Gateway Devices".

[91] BBF TR-101 issue 2: "Migration to Ethernet-Based Broadband Aggregation".

[92] BBF TR-178 issue 1: "Multi-service Broadband Network Architecture and Nodal Requirements".

[93] BBF TR-456 issue 2: "AGF Functional Requirements".

[94] BBF WT-457: "FMIF Functional Requirements".

Editor's note: The reference to BBF WT-457 will be revised when finalized by BBF.

[95] Void.

[96] Void.

[97] IEEE Std 802.1AB-2016: "IEEE Standard for Local and metropolitan area networks -- Station and Media Access Control Connectivity Discovery".

[98] IEEE Std 802.1Q-2022: "IEEE Standard for Local and metropolitan area networks--Bridges and Bridged Networks".

[99] 3GPP TS 38.423: "NG-RAN; Xn Application Protocol (XnAP)".

[100] 3GPP TS 36.413: "Evolved Universal Terrestrial Radio Access Network (E-UTRAN); S1 Application Protocol (S1AP)".

[101] 3GPP TS 29.274: "Evolved General Packet Radio Service (GPRS) Tunnelling Protocol for Control plane (GTPv2-C); Stage 3".

[102] 3GPP TS 23.632: "User Data Interworking, Coexistence and Migration; stage 2".

[103] 3GPP TS 29.563: "5G System (5GS); HSS services for interworking with UDM; Stage 3".

[104] IEEE Std 802.1AS-2020: "IEEE Standard for Local and metropolitan area networks--Timing and Synchronization for Time-Sensitive Applications".

[105] 3GPP TS 22.104: "Service requirements for cyber-physical control applications in vertical domains".

[106] IEEE Std 802.11-2012: "IEEE Standard for Information technology - Telecommunications and information exchange between systems - Local and metropolitan area networks - Specific requirements - Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications".

[107] IEEE Std 1588-2008: "IEEE Standard for a Precision Clock Synchronization Protocol for Networked Measurement and Control Systems".

[108] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements".

[109] 3GPP TS 24.193: "Access Traffic Steering, Switching and Splitting; Stage 3".

[110] 3GPP TS 24.526: "User Equipment (UE) policies for 5G System (5GS); Stage 3".

[111] 3GPP TS 22.186: "Enhancement of 3GPP support for V2X scenarios; Stage 1".

[112] 3GPP TR 38.824: "Study on physical layer enhancements for NR ultra-reliable and low latency case (URLLC)".

[113] IEEE: "Guidelines for Use of Extended Unique Identifier (EUI), Organizationally Unique Identifier (OUI) and Company ID (CID)", https://standards.ieee.org/content/dam/ieee-standards/standards/web/documents/tutorials/eui.pdf.

[114] 3GPP TS 32.256: "Charging Management; 5G connection and mobility domain charging; Stage 2".

[115] 3GPP TS 33.210: "Network Domain Security (NDS); IP network layer security".

[116] 3GPP TS 38.415: "PDU Session User Plane Protocol".

[117] 3GPP TS 24.535: "Device-side Time-Sensitive Networking (TSN) Translator (DS-TT) to network-side TSN Translator (NW-TT) protocol aspects; Stage 3".

[118] 3GPP TS 32.274: "Charging Management; Short Message Service (SMS) charging".

[119] 3GPP TS 23.008: "Organization of subscriber data".

[120] 3GPP TS 38.314: "NR; Layer 2 measurements".

[121] 3GPP TS 23.287: "Architecture enhancements for 5G System (5GS) to support Vehicle-to-Everything (V2X) services".

[122] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[123] 3GPP TS 32.254: "Charging management; Exposure function Northbound Application Program Interfaces (APIs) charging".

[124] 3GPP TS 33.535: "Authentication and Key Management for Applications based on 3GPP credentials in the 5G System (5GS)".

[125] 3GPP TS 38.410: "NG-RAN; NG general aspects and principles".

[126] IEEE Std 1588: "IEEE Standard for a Precision Clock Synchronization Protocol for Networked Measurement and Control Systems", Edition 2019.

[127] ST 2059-2:2015: "SMPTE Standard - SMPTE Profile for Use of IEEE-1588 Precision Time Protocol in Professional Broadcast Applications".

[128] 3GPP TS 23.304: "Proximity based Services (ProSe) in the 5G System (5GS)".

[129] 3GPP TS 23.247: "Architectural enhancements for 5G multicast-broadcast services".

[130] 3GPP TS 23.548: "5G System Enhancements for Edge Computing; Stage 2".

[131] IEEE Std 802.3: "Ethernet".

[132] 3GPP TS 29.561: "5G System; Interworking between 5G Network and external Data Networks; Stage 3".

[133] 3GPP TS 29.513: "Policy and Charging Control signalling flows and QoS parameter mapping; Stage 3".

[134] 3GPP TS 23.558: "Architecture for enabling Edge Applications (EA)".

[135] 3GPP TS 26.501: "5G Media Streaming (5GMS); General description and architecture".

[136] 3GPP TS 23.256: "Support of Uncrewed Aerial Systems (UAS) connectivity, identification and tracking; Stage 2".

[137] GSMA NG.116: "Generic Network Slice Template".

[138] IETF RFC 3948: "UDP Encapsulation of IPsec ESP Packets".

[139] 3GPP TS 24.539: "5G System (5GS); Network to TSN translator (TT) protocol aspects; Stage 3".

[140] 3GPP TS 33.220: "Generic Authentication Architecture (GAA); Generic bootstrapping architecture".

[141] 3GPP TS 33.223: "Generic Authentication Architecture (GAA); Generic Bootstrapping Architecture (GBA) Push function".

[142] 3GPP TS 23.540: "Technical realization of Service Based Short Message Service; Stage 2".

[143] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification".

[144] 3GPP TS 29.525: "5G System; UE Policy Control Service; Stage 3".

[145] 3GPP TS 29.505: "5G System; Usage of the Unified Data Repository Services for Subscription Data; Stage 3".

[146] IEEE Std 802.1Qdj-2024: "IEEE Draft Standard for Local and metropolitan area networks - Bridges and Bridged Networks - Amendment XX: Configuration Enhancements for Time-Sensitive Networking".

[147] Void.

[148] 3GPP TS 28.557: "Management and orchestration; Management of Non-Public Networks (NPN)".

[149] 3GPP TS 28.541: "Management and orchestration; 5G Network Resource Model (NRM)".

[150] IETF RFC 8655: "Deterministic Networking Architecture".

[151] IETF RFC 8343: "A YANG Data Model for Interface Management".

[152] IETF RFC 8344: "A YANG Data Model for IP Management".

[153] IETF RFC 7224: " IANA Interface Type YANG Module".

[154] IETF RFC 9633: "Deterministic Networking (DetNet) YANG Model".

[155] IETF RFC 6241: "Network Configuration Protocol (NETCONF)".

[156] IETF RFC 8040: "RESTCONF Protocol".

[157] IETF RFC 8939: "Deterministic Networking (DetNet) Data Plane: IP".

[158] IETF RFC 5279: "A Uniform Resource Name (URN) Namespace for the 3rd Generation Partnership Project (3GPP)".

[159] IETF RFC 9330:"Low Latency, Low Loss, Scalable Throughput (L4S) Internet Service: Architecture".

[160] IETF RFC 9331: "Explicit Congestion Notification (ECN) Protocol for Very Low Queuing Delay (L4S)".

[161] IETF RFC 9332: "Dual-Queue Coupled Active Queue Management (AQM) for Low Latency, Low Loss and Scalable Throughput (L4S)".

[162] IETF RFC 6603: "Prefix Exclude Option for DHCPv6-based Prefix Delegation".

[163] IETF RFC 8415: "Dynamic Host Configuration Protocol for IPv6 (DHCPv6)".

[164] ITU‑T Recommendation G.810: "Definitions and terminology for synchronization networks".

[165] 3GPP TS 38.470: "NG-RAN; F1 general aspects and principles".

[166] IETF RFC 9000: "QUIC: A UDP-Based Multiplexed and Secure Transport".

[167] IETF RFC 9001: "Using TLS to Secure QUIC".

[168] IETF RFC 9002: "QUIC Loss Detection and Congestion Control".

[169] IETF RFC 9221: "An Unreliable Datagram Extension to QUIC".

[170] IETF RFC 9298: "Proxying UDP in HTTP".

[171] IETF RFC 9114: "Hypertext Transfer Protocol Version 3 (HTTP/3)".

[172] IETF RFC 9297: "HTTP Datagrams and the Capsule Protocol".

[173] IETF RFC 9220: "Bootstrapping WebSockets with HTTP/3".

[174] draft-ietf-quic-multipath: "Multipath Extension for QUIC".

Editor's note: The above document cannot be formally referenced until it is published as an RFC.

[175] 3GPP TS 28.530: "Management and orchestration; Concepts, use cases and requirements".

[176] 3GPP TS 28.531: "Management and orchestration; Provisioning".

[177] 3GPP TS 23.434: "Service Enabler Architecture Layer for Verticals (SEAL); Functional architecture and information flows".

[178] IEEE Std 802.1CBdb-2021: "Amendment 2: Extend Stream Identification Functions".

[179] 3GPP TS 26.522: "5G Real-time Media Transport Protocol Configurations".

[180] 3GPP TS 23.586: "Architectural Enhancements to support Ranging based services and Sidelink Positioning".

[181] 3GPP TS 23.542: "Application layer support for Personal IoT Network".

[182] IETF RFC 8415: "Dynamic Host Configuration Protocol for IPv6 (DHCPv6)".

[183] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[184] 3GPP TS 23.289: "Mission Critical services over 5G System; Stage 2".

[185] IETF RFC 3550: "RTP: A Transport Protocol for Real-Time Applications".

[186] IETF RFC 3711: "The Secure Real-time Transport Protocol (SRTP)".

[187] IETF RFC 6184: "RTP Payload Format for H.264 Video".

[188] IETF RFC 7798: "RTP Payload Format for High Efficiency Video Coding (HEVC) ".

[189] IETF RFC 8285: "A General Mechanism for RTP Header Extensions".

[190] 3GPP TS 28.405: "Quality of Experience (QoE) measurement collection; Control and configuration".

[191] 3GPP TS 37.355: " LTE Positioning Protocol (LPP)".

[192] 3GPP TS 32.422: "Telecommunication management; Subscriber and equipment trace; Trace control and configuration management".

[193] IETF RFC 3168: "The Addition of Explicit Congestion Notification (ECN) to IP".

[194] 3GPP TS 33.503: "Security Aspects of Proximity based Services (ProSe) in the 5G System (5GS)".

[195] 3GPP TS 38.414: "NG-RAN; NG data transport".

[196] Void.

[197] 3GPP TS 28.310: "Management and orchestration; Energy efficiency of 5G".

[198] IETF RFC 6040: "Tunnelling of Explicit Congestion Notification".

[199] IETF RFC 9599: "Guidelines for Adding Congestion Notification to Protocols that Encapsulate IP".

[200] IETF draft-ietf-masque-quic-proxy: " QUIC-Aware Proxying Using HTTP".

Editor's note: The above reference will be revised to RFC when finalized by IETF.

[201] IETF draft-ietf-moq-transport: "Media over QUIC Transport".

Editor's note: The above reference will be revised to RFC when finalized by IETF.

[202] IETF draft-ietf-tsvwg-udp-options: "Transport Options for UDP".

Editor's note: The above reference will be revised to RFC when finalized by IETF.

[203] IETF RFC 5761: "Multiplexing RTP Data and Control Packets on a Single Port".

[204] IETF RFC 5764: "Datagram Transport Layer Security (DTLS) Extension to Establish Keys for the Secure Real-time Transport Protocol (SRTP)".

[205] IETF RFC 7983: "Multiplexing Scheme Updates for Secure Real-time Transport Protocol (SRTP) Extension for Datagram Transport Layer Security (DTLS)".

[206] IETF RFC 8872: "Guidelines for Using the Multiplexing Features of RTP to Support Multiple Media Streams".

[207] IETF RFC 9143: "Negotiating Media Multiplexing Using the Session Description Protocol (SDP)".

[208] IETF RFC 9443: "Multiplexing Scheme Updates for QUIC".

[209] 3GPP TS 28.554: "Management and orchestration; 5G end to end Key Performance Indicators (KPI)".

[210] 3GPP TS 23.527: "5G System; Restoration Procedures".

[211] IETF RFC 5357: "A Two-Way Active Measurement Protocol (TWAMP)".

[212] IETF  RFC 4656: "A One-way Active Measurement Protocol (OWAMP)".

[213] IETF RFC 8762: "Simple Two-Way Active Measurement Protocol".

[214] IETF RFC 9484: "Proxying IP in HTTP".

[215] IETF draft-ietf-masque-connect-ethernet: " Proxying Ethernet in HTTP".

Editor's note: The above document cannot be formally referenced until it is published as an RFC.

[216] IEC/IEEE 60802: "Time-Sensitive Networking Profile for Industrial Automation".

[217] 3GPP TS 38.424: "NG-RAN; Xn data transport".

[218] 3GPP TS 28.622: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Information Service (IS)".

[219] 3GPP TS 28.532: "Management and orchestration; Generic management services".

[XX] 3GPP TS 22.042: "Network Identity and Time Zone, Service Description, Stage 1".

[YY] 3GPP TS 31.102: "Characteristics of the USIM Application".

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Next Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

5GC 5G Core Network

5G DDNMF 5G Direct Discovery Name Management Function

5G LAN 5G Local Area Network

5GS 5G System

5G-AN 5G Access Network

5G-AN PDB 5G Access Network Packet Delay Budget

5G-EIR 5G-Equipment Identity Register

5G-GUTI 5G Globally Unique Temporary Identifier

5G-BRG 5G Broadband Residential Gateway

5G-CRG 5G Cable Residential Gateway

5G GM 5G Grand Master

5G NSWO 5G Non-Seamless WLAN offload

5G-RG 5G Residential Gateway

5G-S-TMSI 5G S-Temporary Mobile Subscription Identifier

5G VN 5G Virtual Network

5QI 5G QoS Identifier

ADRF Analytics Data Repository Function

AF Application Function

AI/ML Artificial Intelligence/Machine Learning

AKMA Authentication and Key Management for Applications

AnLF Analytics Logical Function

AMF Access and Mobility Management Function

AoI Area of Interest

AS Access Stratum

ATSSS Access Traffic Steering, Switching, Splitting

ATSSS-LL ATSSS Low-Layer

AUSF Authentication Server Function

BMCA Best Master Clock Algorithm

BSF Binding Support Function

CAG Closed Access Group

CAPIF Common API Framework for 3GPP northbound APIs

CH Credentials Holder

CHF Charging Function

CN PDB Core Network Packet Delay Budget

CP Control Plane

CQRCI Clock Quality Reporting Control Information

DAPS Dual Active Protocol Stacks

DCCF Data Collection Coordination Function

DCS Default Credentials Server

DetNet Deterministic Networking

DL Downlink

DN Data Network

DNAI DN Access Identifier

DNN Data Network Name

DRX Discontinuous Reception

DS-TT Device-side TSN translator

EAC Early Admission Control

EIF Energy Information Function

ePDG evolved Packet Data Gateway

EBI EPS Bearer Identity

EUI Extended Unique Identifier

FAR Forwarding Action Rule

FL Federated Learning

FN-BRG Fixed Network Broadband RG

FN-CRG Fixed Network Cable RG

FN-RG Fixed Network RG

FQDN Fully Qualified Domain Name

GBA Generic Bootstrapping Architecture

GBRSS Guaranteed Bit Rate Streaming Service

GEO Geostationary Orbit

GFBR Guaranteed Flow Bit Rate

GIN Group ID for Network Selection

GMLC Gateway Mobile Location Centre

GPSI Generic Public Subscription Identifier

GUAMI Globally Unique AMF Identifier

HMTC High-Performance Machine-Type Communications

HR Home Routed (roaming)

IAB Integrated access and backhaul

IMEI/TAC IMEI Type Allocation Code

IPUPS Inter PLMN UP Security

I-SMF Intermediate SMF

I-UPF Intermediate UPF

LADN Local Area Data Network

LBO Local Break Out (roaming)

LEO Low Earth Orbit

LMF Location Management Function

LoA Level of Automation

LPP LTE Positioning Protocol

LRF Location Retrieval Function

L4S Low Latency, Low Loss and Scalable Throughput

MBS Multicast/Broadcast Service

MBSF Multicast/Broadcast Service Function

MBSR Mobile Base Station Relay

MBSTF Multicast/Broadcast Service Transport Function

MB-SMF Multicast/Broadcast Session Management Function

MB-UPF Multicast/Broadcast User Plane Function

MEO Medium Earth Orbit

MFAF Messaging Framework Adaptor Function

MCX Mission Critical Service

MDBV Maximum Data Burst Volume

MFBR Maximum Flow Bit Rate

MICO Mobile Initiated Connection Only

MINT Minimization of Service Interruption

ML Machine Learning

MPQUIC Multi-Path QUIC

MPS Multimedia Priority Service

MPTCP Multi-Path TCP Protocol

MTLF Model Training Logical Function

MWAB Mobile gNB with wireless access backhauling

N3IWF Non-3GPP InterWorking Function

N3QAI Non-3GPP QoS Assistance Information

N5CW Non-5G-Capable over WLAN

NAI Network Access Identifier

NAT Network Address Translation

NCR Network Controlled Repeater

NCR-MT NCR Mobile Termination

NEF Network Exposure Function

NF Network Function

NGAP Next Generation Application Protocol

NID Network identifier

NITZ Network Identity and Time Zone

NPN Non-Public Network

NR New Radio

NRF Network Repository Function

NS-AoS Network Slice Area of Service

NSAC Network Slice Admission Control

NSACF Network Slice Admission Control Function

NSAG Network Slice AS Group

NSI ID Network Slice Instance Identifier

NSSAA Network Slice-Specific Authentication and Authorization

NSSAAF Network Slice-specific and SNPN Authentication and Authorization Function

NSSAI Network Slice Selection Assistance Information

NSSF Network Slice Selection Function

NSSP Network Slice Selection Policy

NSSRG Network Slice Simultaneous Registration Group

NSWO Non-Seamless WLAN offload

NSWOF Non-Seamless WLAN offload Function

NW-TT Network-side TSN translator

NWDAF Network Data Analytics Function

ONN Onboarding Network

ON-SNPN Onboarding Standalone Non-Public Network

PCF Policy Control Function

PDB Packet Delay Budget

PDR Packet Detection Rule

PDU Protocol Data Unit

PDV Packet Delay Variation

PEGC PIN Element with Gateway Capability

PEI Permanent Equipment Identifier

PEMC PIN Element with Management Capability

PER Packet Error Rate

PFD Packet Flow Description

PIN Personal IoT Network

PINE PIN Element

PLR Packet Loss Rate

PNI-NPN Public Network Integrated Non-Public Network

PPD Paging Policy Differentiation

PPF Paging Proceed Flag

PPI Paging Policy Indicator

PSA PDU Session Anchor

PSDB PDU Set Delay Budget

PSER PDU Set Error Rate

PSIHI PDU Set Integrated Handling Information

PTP Precision Time Protocol

PVS Provisioning Server

QFI QoS Flow Identifier

QMC QoE Measurement Collection

QoE Quality of Experience

RACS Radio Capabilities Signalling optimisation

(R)AN (Radio) Access Network

RG Residential Gateway

RIM Remote Interference Management

RQA Reflective QoS Attribute

RQI Reflective QoS Indication

RSN Redundancy Sequence Number

RTT Round Trip Time

SA NR Standalone New Radio

SBA Service Based Architecture

SBI Service Based Interface

SCP Service Communication Proxy

SD Slice Differentiator

SEAF Security Anchor Functionality

SEPP Security Edge Protection Proxy

SF Service Function

SFC Service Function Chain

SMF Session Management Function

SMSF Short Message Service Function

SN Sequence Number

SNPN Stand-alone Non-Public Network

S-NSSAI Single Network Slice Selection Assistance Information

SO-SNPN Subscription Owner Standalone Non-Public Network

SSC Session and Service Continuity

SSCMSP Session and Service Continuity Mode Selection Policy

SST Slice/Service Type

SUCI Subscription Concealed Identifier

SUPI Subscription Permanent Identifier

SV Software Version

TA Tracking Area

TAI Tracking Area Identity

TNAN Trusted Non-3GPP Access Network

TNAP Trusted Non-3GPP Access Point

TNGF Trusted Non-3GPP Gateway Function

TNL Transport Network Layer

TNLA Transport Network Layer Association

TSC Time Sensitive Communication

TSCAC TSC Assistance Container

TSCAI Traffic Assistance Information

TSCTSF Time Sensitive Communication and Time Synchronization Function

TSN Time Sensitive Networking

TSN GM TSN Grand Master

TSP Traffic Steering Policy

TSS Timing Synchronization Status

TT TSN Translator

TWIF Trusted WLAN Interworking Function

UAS NF Uncrewed Aerial System Network Function

UCMF UE radio Capability Management Function

UDM Unified Data Management

UDR Unified Data Repository

UDSF Unstructured Data Storage Function

UL Uplink

UL CL Uplink Classifier

UPF User Plane Function

URLLC Ultra Reliable Low Latency Communication

URRP-AMF UE Reachability Request Parameter for AMF

URSP UE Route Selection Policy

VID VLAN Identifier

VLAN Virtual Local Area Network

W-5GAN Wireline 5G Access Network

W-5GBAN Wireline BBF Access Network

W-5GCAN Wireline 5G Cable Access Network

W-AGF Wireline Access Gateway Function

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Next Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

## 5.X Support for Dynamic Network Identity

### 5.X.1 Overview

To support dynamic Network Identity display in the UE, the AMF provides the parameter 'Network Identity' as part of Network Identity and Time Zone (NITZ) as defined in TS 22.042 [XX] to the UE, via UE Configuration Update procedure as defined in clause 4.2.4.2 of TS 23.502 [3]. The Network Identity parameter is applied by the UE as described in clause A.3 of TS 22.101 [33].

NOTE X: A network identity stored in the USIM can supersede the network identity stored in the UE as described in clause A.3 of TS 22.101 [33].

The serving AMF may set the Network Identity in use for the UE based on operator’s policies, and/or authorized Network Identity received from the PCF in combination with an applicability condition (target area) during AM Policy Association Establishment procedure or AM Policy Association Modification procedure. The authorized Network Identity received from the PCF takes precedence over the locally configured Network Identity.

NOTE Y: Authorized Network Identity is not supported in the roaming scenarios in this release.

The AMF stores the Network Identity in use. When the Network Identity is changed, the AMF provides the updated Network Identity to the UE via UE Configuration Update procedure. During inter-AMF mobility procedures, the source AMF forwards the Network Identityin use and applicability condition (target area) to the target AMF. The target AMF may replace the received Network Identity with a new Network Identity in use based on operator’s policies .

NOTE Z: To avoid the display of invalid PLMN name resulted from last received network identity, all the CN nodes in HPLMN that provide the network identity, e.g. AMF, or MME in case of EPC, are required to enable again the configuration of the default network identity. There may be a risk that a wrong network identity is displayed after a UE is handed over to EPC.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Changes \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*