|  |  |
| --- | --- |
| 3GPP TS 38.101-3 V16.14.0 (2022-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 3: Range 1 and Range 2 Interworking operation with other radios  (Release 16) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 12

1 Scope 14

2 References 14

3 Definitions, symbols and abbreviations 15

3.1 Definitions 15

3.2 Symbols 15

3.3 Abbreviations 15

4 General 16

4.1 Relationship between minimum requirements and test requirements 16

4.2 Applicability of minimum requirements 17

4.3 Specification suffix information 17

5 Operating bands and channel arrangement 18

5.1 General 18

5.2 Operating bands 18

5.2A Operating bands for CA 18

5.2A.1 Inter-band CA between FR1 and FR2 18

5.2B Operating bands for DC 20

5.2B.1 General 20

5.2B.2 Void 20

5.2B.3 Void 20

5.2B.4 Void 20

5.2B.5 Void 20

5.2B.6 Void 20

5.2B.7 Void 20

5.2E Operating bands for V2X 20

5.2E.1 Intra-band V2X bands 20

5.2E.2 Inter-band V2X bands 20

5.3 UE Channel bandwidth 21

5.3A UE Channel bandwidth for CA 21

5.3A.1 Inter-band CA between FR1 and FR2 21

5.3B UE Channel bandwidth for EN-DC 21

5.3B.0 General 21

5.3B.1 Intra-band EN-DC in FR1 22

5.3B.1.1 General 22

5.3B.1.2 BCS for Intra-band contiguous EN-DC 22

5.3B.1.3 BCS for Intra-band non-contiguous EN-DC 25

5.3C Void 28

5.3D Void 28

5.3E UE Channel bandwidth for V2X 28

5.3E.0 General 28

5.3E.1 Intra-band contiguous V2X in FR1 28

5.3E.2 Intra-band non-contiguous V2X in FR1 29

5.3E.3 Inter-band V2X in FR1 29

5.4 Void 29

5.4A Channel arrangement for CA 29

5.4B Channel arrangement for DC 29

5.4B.0 General 29

5.4B.1 Channel spacing for intra-band EN-DC carriers 30

5.5 Configuration 31

5.5A Configuration for CA 31

5.5A.1 Inter-band CA configurations between FR1 and FR2 31

5.5B Configuration for DC 70

5.5B.1 General 70

5.5B.2 Intra-band contiguous EN-DC 71

5.5B.3 Intra-band non-contiguous EN-DC 71

5.5B.4 Inter-band EN-DC within FR1 73

5.5B.4.1 Inter-band EN-DC configurations within FR1 (two bands) 73

5.5B.4.2 Inter-band EN-DC configurations within FR1 (three bands) 81

5.5B.4.3 Inter-band EN-DC configurations within FR1 (four bands) 102

5.5B.4.4 Inter-band EN-DC configurations within FR1 (five bands) 122

5.5B.4.5 Inter-band EN-DC configurations within FR1 (six bands) 130

5.5B.4a Inter-band NE-DC within FR1 131

5.5B.4a.1 Inter-band NE-DC configurations within FR1 (two bands) 131

5.5B.5 Inter-band EN-DC including FR2 132

5.5B.5.1 Inter-band EN-DC configurations including FR2 (two bands) 132

5.5B.5.2 Inter-band EN-DC configurations including FR2 (three bands) 152

5.5B.5.3 Inter-band EN-DC configurations including FR2 (four bands) 175

5.5B.5.4 Inter-band EN-DC configurations including FR2 (five bands) 193

5.5B.5.5 Void 200

5.5B.6 Inter-band EN-DC including FR1 and FR2 200

5.5B.6.1 Void 200

5.5B.6.2 Inter-band EN-DC configurations including FR1 and FR2 (three bands) 200

5.5B.6.3 Inter-band EN-DC configurations including FR1 and FR2 (four bands) 209

5.5B.6.4 Inter-band EN-DC configurations including FR1 and FR2 (five bands) 227

5.5B.6.5 Inter-band EN-DC configurations including FR1 and FR2 (six bands) 241

5.5B.7 Inter-band NR-DC between FR1 and FR2 244

5.5B.7.0 General 244

5.5B.7.1 Inter-band NR-DC configurations between FR1 and FR2 (two bands) 246

5.5B.7.2 Inter-band NR-DC configurations between FR1 and FR2 (three bands) 249

5.5C Void 250

5.5D Void 250

5.5E Configuration for V2X operation 250

5.5E.1 General 250

5.5E.2 Intra-band contiguous V2X operation in FR1 250

5.5E.3 Intra-band non-contiguous V2X operation in FR1 250

5.5E.4 Inter-band V2X operation in FR1 250

5.5E.4.1 Inter-band V2X configurations within FR1 (two bands) 250

6 Transmitter characteristics 251

6.1 General 251

6.2 Void 251

6.2A Transmitter power for CA 251

6.2A.1 UE maximum output power for CA 251

6.2A.1.1 Inter-band CA between FR1 and FR2 251

6.2A.2 UE maximum output power reduction for CA 251

6.2A.2.1 Inter-band CA between FR1 and FR2 251

6.2A.3 UE additional maximum output power reduction for CA 251

6.2A.4 Configured output power for CA 251

6.2A.4.1 Configured output power level 251

6.2A.4.2 ΔTIB,c for CA 252

6.2A.4.2.1 ΔTIB,c for Inter-band CA between FR1 and FR2 252

6.2B Transmitter power for DC 252

6.2B.1 UE maximum output power for DC 252

6.2B.1.1 Intra-band contiguous EN-DC 252

6.2B.1.2 Intra-band non-contiguous EN-DC 254

6.2B.1.3 Inter-band EN-DC within FR1 255

6.2B.1.3a Inter-band NE-DC within FR1 261

6.2B.1.4 Inter-band EN-DC including FR2 262

6.2B.1.5 Inter-band EN-DC including both FR1 and FR2 262

6.2B.2 UE maximum output power reduction for DC 262

6.2B.2.0 General 262

6.2B.2.1 Intra-band contiguous EN-DC 262

6.2B.2.1.1 General 262

6.2B.2.1.2 MPR for power class 3 and power class 2 263

6.2B.2.2 Intra-band non-contiguous EN-DC 263

6.2B.2.2.1 General 263

6.2B.2.2.2 MPR for power class 3 and power class 2 264

6.2B.2.3 Inter-band EN-DC within FR1 265

6.2B.2.3a Inter-band NE-DC within FR1 265

6.2B.2.4 Inter-band EN-DC including FR2 265

6.2B.2.5 Inter-band EN-DC including both FR1 and FR2 265

6.2B.3 UE additional maximum output power reduction for EN-DC 265

6.2B.3.1 Intra-band contiguous EN-DC 265

6.2B.3.1.0 General 265

6.2B.3.1.1 A-MPR for DC\_(n)71AA 265

6.2B.3.1.2 A-MPR for NS\_04 267

6.2B.3.2 Intra-band non-contiguous EN-DC 269

6.2B.3.2.0 General 269

6.2B.3.2.1 A-MPR for NS\_04 270

6.2B.3.3 Inter-band EN-DC within FR1 271

6.2B.3.3A Inter-band NE-DC within FR1 274

6.2B.3.4 Inter-band EN-DC including FR2 275

6.2B.3.5 Inter-band EN-DC including both FR1 and FR2 275

6.2B.4 Configured output power for DC 275

6.2B.4.1 Configured output power level 275

6.2B.4.1.1 Intra-band contiguous EN-DC 275

6.2B.4.1.2 Intra-band non-contiguous EN-DC 279

6.2B.4.1.3a Inter-band NE-DC within FR1 284

6.2B.4.1.4 Inter-band EN-DC including FR2 287

6.2B.4.1.5 Inter-band EN-DC including both FR1 and FR2 288

6.2B.4.2 ΔTIB,c for DC 288

6.2B.4.2.0 General 288

6.2B.4.2.1 Intra-band contiguous EN-DC 288

6.2B.4.2.2 Intra-band non-contiguous EN-DC 288

6.2B.4.2.3 Inter-band EN-DC within FR1 289

6.2B.4.2.3.1 ΔTIB,c for EN-DC two bands 289

6.2B.4.2.3.2 ΔTIB,c for EN-DC three bands 296

6.2B.4.2.3.3 ΔTIB,c for EN-DC four bands 315

6.2B.4.2.3.4 ΔTIB,c for EN-DC five bands 333

6.2B.4.2.3.5 ΔTIB,c for EN-DC six bands 339

6.2B.4.2.3a Inter-band NE-DC within FR1 340

6.2B.4.2.4 Inter-band EN-DC including FR2 340

6.2B.4.2.4.1 ΔTIB,c for EN-DC two bands 340

6.2B.4.2.4.2 ΔTIB,c for EN-DC three bands 340

6.2B.4.2.4.3 ΔTIB,c for EN-DC four bands 340

6.2B.4.2.4.4 ΔTIB,c for EN-DC five bands 340

6.2B.4.2.4.5 Void 340

6.2B.4.2.5 Inter-band EN-DC including both FR1 and FR2 340

6.2B.4.2.5.1 ΔTIB,c for EN-DC three bands 340

6.2B.4.2.5.2 ΔTIB,c for EN-DC four bands 340

6.2B.4.2.5.3 ΔTIB,c for EN-DC five bands 341

6.2B.4.2.5.4 ΔTIB,c for EN-DC six bands 341

6.2B.5 Configured output power for NR-DC 341

6.2B.5.1 Configured output power level 341

6.2B.5.1.1 Inter-band NR-DC between FR1 and FR2 341

6.2E Transmitter power for V2X in FR1 341

6.2E.1 UE maximum output power for V2X 341

6.2E.1.1 UE maximum output power for Intra-band contiguous V2X 341

6.2E.1.2 UE maximum output power for Intra-band non-contiguous V2X 341

6.2E.1.3 UE maximum output power for Inter-band V2X 342

6.2E.2 UE maximum output power reduction for V2X 342

6.2E.2.1 UE maximum output power reduction for Intra-band V2X 342

6.2E.2.2 UE maximum output power reduction for Inter-band V2X 342

6.2E.3 UE additional maximum output power reduction for V2X 342

6.2E.3.1 UE additional maximum output power reduction for Intra-band V2X 342

6.2E.3.2 UE additional maximum output power reduction for Inter-band V2X 342

6.2E.4 Configured output power for V2X 342

6.2E.4.1 UE configured output power for Intra-band V2X 342

6.2E.4.2 UE configured output power for Inter-band V2X 343

6.3 Output power dynamics 343

6.3A Output power dynamics for CA 344

6.3B Output power dynamics for DC 344

6.3B.0 General 344

6.3B.1 Output power dynamics for EN-DC with UL sharing from UE perspective 344

6.3B.1.1 E-UTRA and NR switching time mask for TDM based UL sharing from UE perspective 344

6.3B.1a Output power dynamics for NE-DC with UL sharing from UE perspective 345

6.3B.2 Output power dynamics for intra-band EN-DC without dual PA capability 345

6.3B.3 Output power dynamics for intra-band EN-DC with dual PA capability 346

6.3B.4 Output power dynamics for switching between two uplink carriers 347

6.3B.4.1 E-UTRA and NR switching time mask between two uplink carriers 347

6.3B.5 Output power dynamics for inter-band EN-DC 347

6.3E Output power dynamics for V2X 348

6.3E.1 General 348

6.3E.2 Output power dynamics for intra-band V2X operation 348

6.3E.3 Output power dynamics for inter-band V2X con-current operation 349

6.4 Void 349

6.4A Transmit signal quality for CA 349

6.4A.1 Frequency error for CA 349

6.4A.2 Transmit modulation quality for CA 349

6.4B Transmit signal quality for DC 349

6.4B.2 Transmit modulation quality for DC 350

6.4B.2.1 Transmit modulation quality for Intra-band contiguous EN-DC 350

6.4B.2.1.1 Error Vector Magnitude 350

6.4B.2.1.2 Carrier leakage 350

6.4B.2.1.3 In-band emissions 350

6.4B.2.2 Transmit modulation quality for Intra-band non-contiguous EN-DC 350

6.4B.2.2.1 Error Vector Magnitude 350

6.4B.2.2.2 Carrier leakage 350

6.4B.2.2.3 In-band emissions 351

6.4B.2.3a Transmit modulation quality for Inter-band NE-DC within FR1 351

6.4B.2.4 Transmit modulation quality for Inter-band EN-DC including FR2 351

6.4B.2.5 Transmit modulation quality for inter-band EN-DC including both FR1 and FR2 351

6.4E Transmit signal quality for V2X operation in FR1 351

6.4E.1 Frequency error for V2X 351

6.4E.2 Transmit modulation quality for V2X 352

6.4E.2.1 Transmit modulation quality for Intra-band V2X 352

6.4E.2.2.1 Error Vector Magnitude 352

6.4E.2.2.2 Carrier leakage 352

6.4E.2.2.3 In-band emissions 352

6.4E.2.2 Transmit modulation quality for Inter-band V2X 352

6.5 Void 352

6.5A Output RF spectrum emissions for CA 352

6.5A.1 Occupied bandwidth for CA 352

6.5A.2 Out-of-band emissions for CA 352

6.5A.3 Spurious emissions for CA 352

6.5A.3.1 Inter-band CA between FR1 and FR2 352

6.5A.4 Transmit intermodulation for CA 353

6.5B Output RF spectrum emissions for DC 353

6.5B.1 Occupied bandwidth for EN-DC 353

6.5B.1.4 Inter-band EN-DC including FR2 353

6.5B.1.5 Inter-band EN-DC including both FR1 and FR2 353

6.5B.2 Out-of-band emissions for DC 353

6.5B.2.1 Intra-band contiguous EN-DC 353

6.5B.2.1.1 Spectrum emissions mask 353

6.5B.2.1.2 Additional spectrum emissions mask 354

6.5B.2.1.2.1 Requirements for network signalled value "NS\_35" 354

6.5B.2.1.2.2 Requirements for network signalled value "NS\_04" 354

6.5B.2.1.3 Adjacent channel leakage ratio 355

6.5B.2.2 Intra-band non-contiguous EN-DC 355

6.5B.2.2.1 Spectrum emissions mask 355

6.5B.2.2.2 Additional spectrum emissions mask 355

6.5B.2.2.3 Adjacent channel leakage ratio 355

6.5B.2.3 Inter-band EN-DC within FR1 356

6.5B.2.3a Inter-band NE-DC within FR1 356

6.5B.2.4 Inter-band EN-DC including FR2 356

6.5B.2.5 Inter-band EN-DC including both FR1 and FR2 356

6.5B.3 Spurious emissions for DC 356

6.5B.3.1 Intra-band contiguous EN-DC 356

6.5B.3.1.1 General spurious emissions 356

6.5B.3.1.2 Spurious emission band UE co-existence 356

6.5B.3.2 Intra-band non-contiguous EN-DC 357

6.5B.3.2.1 General spurious emissions 357

6.5B.3.2.2 Spurious emission band UE co-existence 357

6.5B.3.3 Inter-band EN-DC within FR1 358

6.5B.3.3.2 Spurious emission band UE co-existence 359

6.5B.3.3a Inter-band NE-DC within FR1 385

6.5B.3.3a.1 General spurious emissions 385

6.5B.3.3a.2 Spurious emission band UE co-existence 385

6.5B.3.4 Inter-band EN-DC including FR2 385

6.5B.3.4.0 General spurious emission 385

6.5B.3.4.1 Spurious emission band UE co-existence 385

6.5B.3.5 Inter-band EN-DC including both FR1 and FR2 385

6.5B.3.5.0 General spurious emission 385

6.5B.3.5.1 Spurious emission band UE co-existence 385

6.5B.4 Additional spurious emissions 386

6.5B.4.1 General 386

6.5B.4.1.1 Void 386

6.5B.4.2 Intra-band contiguous EN-DC 386

6.5B.4.2.1 Minimum requirement (network signalled value "NS\_04") 386

6.5B.4.3 Intra-band non-contiguous EN-DC 386

6.5B.4.3.1 Minimum requirement (network signalled value "NS\_04") 386

6.5B.4.4 Inter-band EN-DC within FR1 387

6.5B.4.4a Inter-band NE-DC within FR1 387

6.5B.4.5 Inter-band EN-DC including FR2 387

6.5B.4.6 Inter-band EN-DC including both FR1 and FR2 387

6.5B.5 Transmit intermodulation for DC 387

6.5B.5.1 Intra-band contiguous EN-DC 387

6.5B.5.2 Intra-band non-contiguous EN-DC 387

6.5B.5.3 Inter-band EN-DC within FR1 387

6.5B.5.3a Inter-band NE-DC within FR1 387

6.5B.5.4 Inter-band EN-DC including FR2 387

6.5B.5.5 Inter-band EN-DC including both FR1 and FR2 387

6.5E Output RF spectrum emissions for V2X operation in FR1 388

6.5E.1 Occupied bandwidth 388

6.5E.1.1 Intra-band V2X 388

6.5E.1.2 inter-band V2X con-current operation 388

6.5E.2 Out-of-band emissions 388

6.5E.2.1 Intra-band V2X 388

6.5E.2.2 Inter-band V2X con-current operation 388

6.5E.3 Spurious emissions 388

6.5E.3.1 Intra-band V2X 388

6.5E.3.1.1 General spurious emissions 388

6.5E.3.1.2 Spurious emission band UE co-existence 388

6.5E.3.2 Inter-band V2X con-current operation 388

6.5E.3.2.1 General spurious emissions 388

6.5E.3.2.2 Spurious emission band UE co-existence 389

6.5E.4 Transmit intermodulation 389

6.5E.4.1 Intra-band V2X 389

6.5E.4.2 Inter-band V2X con-current operation 389

6.6B Beam correspondence for DC 390

6.6B.1 Void 390

6.6B.2 Void 390

6.6B.3 Void 390

6.6B.4 Inter-band EN-DC including FR2 390

6.6B.5 Inter-band EN-DC including both FR1 and FR2 390

7 Receiver characteristics 390

7.1 General 390

7.2 Void 391

7.3 Void 391

7.3A Reference sensitivity for CA 391

7.3A.1 General 391

7.3A.2 Reference sensitivity power level for CA 391

7.3A.3 ΔRIB,c for CA 391

7.3A.3.1 ΔRIB,c for Inter-band CA between FR1 and FR2 392

7.3A.4 Void 392

7.3B Reference sensitivity level for DC 392

7.3B.1 General 392

7.3B.2 Reference sensitivity for DC 393

7.3B.2.1 Intra-band contiguous EN-DC 393

7.3B.2.2 Intra-band non-contiguous EN-DC 394

7.3B.2.3 Inter-band EN-DC within FR1 395

7.3B.2.3.0 General 395

7.3B.2.3.1 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1 395

7.3B.2.3.2 Reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1 402

7.3B.2.3.3 Void 404

7.3B.2.3.4 Reference sensitivity exceptions due to cross band isolation for EN-DC in NR FR1 404

7.3B.2.3.5 MSD for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 412

7.3B.2.3.5.1 MSD test points for intermodulation interference due to dual uplink operation for PC3 EN-DC in NR FR1 involving two bands 413

7.3B.2.3.5.2 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving three bands 418

7.3B.2.3.5.3 Void 442

7.3B.2.3.5.4 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving four bands 442

7.3B.2.3.6 Reference sensitivity exceptions due to Tx non-linearity interference in 1st or 2nd adjacent channel of UL band for EN-DC in NR FR1 442

7.3B.2.3a Inter-band NE-DC within FR1 443

7.3B.2.3a.0 General 443

7.3B.2.3a.1 Reference sensitivity exceptions due to UL harmonic interference for NE-DC in NR FR1 443

7.3B.2.4 Inter-band EN-DC including FR2 443

7.3B.2.4.1 Void 443

7.3B.2.5 Inter-band EN-DC including both FR1 and FR2 443

7.3B.2.5.1 Reference sensitivity exceptions due to UL harmonic interference for EN-DC including both FR1 and FR2 443

7.3B.3 ΔRIB,c, ΔRIBNC for DC 443

7.3B.3.0 General 443

7.3B.3.1 Intra-band contiguous EN-DC 445

7.3B.3.2 Intra-band non-contiguous EN-DC 445

7.3B.3.3 Inter-band EN-DC within FR1 450

7.3B.3.3.1 ΔRIB,c for EN-DC in two bands 450

7.3B.3.3.2 ΔRIB,c for EN-DC three bands 454

7.3B.3.3.3 ΔRIB,c for EN-DC four bands 465

7.3B.3.3.4 ΔRIB,c for EN-DC five bands 478

7.3B.3.3.5 ΔRIB,c for EN-DC six bands 483

7.3B.3.3a Inter-band NE-DC within FR1 483

7.3B.3.4 Inter-band EN-DC including FR2 483

7.3B.3.4.1 ΔRIB,c for EN-DC in two bands 483

7.3B.3.4.2 ΔRIB,c for EN-DC three bands 484

7.3B.3.4.3 ΔRIB,c for EN-DC four bands 484

7.3B.3.4.4 ΔRIB,c for EN-DC five bands 484

7.3B.3.4.5 Void 484

7.3B.3.5 Inter-band EN-DC including both FR1 and FR2 484

7.3B.3.5.2 ΔRIB,c for EN-DC three bands 484

7.3B.3.5.3 ΔRIB,c for EN-DC four bands 484

7.3B.3.5.4 ΔRIB,c for EN-DC five bands 484

7.3B.3.5.5 ΔRIB,c for EN-DC six bands 484

7.3E Reference sensitivity for V2X operation in FR1 485

7.3E.1 General 485

7.3E.2 Reference sensitivity for V2X 485

7.3E.2.1 Intra-band contiguous V2X 485

7.3E.2.2 Intra-band non-contiguous V2X 485

7.3E.2.3 Inter-band V2X con-current operation 485

7.3E.2.3.0 General 485

7.3E.2.3.1 Reference sensitivity exception due to UL harmonic problem 486

7.4 Void 487

7.4A Maximum input level for CA 487

7.4B Maximum input level for DC in FR1 487

7.4B.1 Intra-band contiguous EN-DC in FR1 487

7.4B.2 Intra-band non-contiguous EN-DC in FR1 487

7.4B.3 Inter-band EN-DC within FR1 487

7.4E Maximum input level for V2X operation in FR1 488

7.5 Void 488

7.5A Adjacent channel selectivity for CA 488

7.5B Adjacent channel selectivity for DC in FR1 488

7.5B.1 Intra-band contiguous EN-DC in FR1 488

7.5B.2 Intra-band non-contiguous EN-DC in FR1 489

7.5B.3 Inter-band EN-DC within FR1 489

7.5E Adjacent channel selectivity for V2X operation in FR1 490

7.6 Void 490

7.6A Blocking characteristics for CA 490

7.6B Blocking characteristics for DC in FR1 490

7.6B.1 General 490

7.6B.2 In-band blocking for DC in FR1 490

7.6B.2.1 Intra-band contiguous EN-DC in FR1 490

7.6B.2.2 Intra-band non-contiguous EN-DC in FR1 490

7.6B.2.3 Inter-band EN-DC within FR1 491

7.6B.2.3a Inter-band NE-DC within FR1 491

7.6B.2.4 Inter-band EN-DC including FR2 491

7.6B.2.5 Inter-band EN-DC including both FR1 and FR2 491

7.6B.2.6 Power imbalance for type 2 UE of inter-band EN-DC with overlapping DL bands 491

7.6B.3 Out-of-band blocking for DC in FR1 492

7.6B.3.1 Intra-band contiguous EN-DC in FR1 492

7.6B.3.2 Intra-band non-contiguous EN-DC in FR1 492

7.6B.3.3 Inter-band EN-DC within FR1 492

7.6B.4 Narrow band blocking for DC in FR1 494

7.6B.4.1 Intra-band contiguous EN-DC in FR1 494

7.6B.4.2 Intra-band non-contiguous EN-DC in FR1 494

7.6B.4.3 Inter-band EN-DC within FR1 494

7.6E Blocking characteristics for V2X in FR1 495

7.7 Void 495

7.7A Spurious response for CA 495

7.7B Spurious response for DC in FR1 495

7.7B.1 Intra-band contiguous EN-DC in FR1 495

7.7B.2 Intra-band non-contiguous EN-DC in FR1 495

7.7B.3 Inter-band EN-DC within FR1 496

7.7E Spurious response for V2X in FR1 496

7.8 Void 496

7.8A Intermodulation characteristics for CA 496

7.8B Intermodulation characteristics for DC in FR1 497

7.8B.1 General 497

7.8B.2 Wide band Intermodulation 497

7.8B.2.1 Intra-band contiguous EN-DC in FR1 497

7.8B.2.2 Intra-band non-contiguous EN-DC in FR1 497

7.8B.2.3 Inter-band EN-DC within FR1 497

7.8E Intermodulation characteristics for V2X operation in FR1 498

7.9 Void 498

7.9A Spurious emissions for CA 498

7.9B Spurious emissions for DC in FR1 498

7.9B.1 Intra-band contiguous EN-DC in FR1 498

7.9B.2 Intra-band non-contiguous EN-DC in FR1 498

7.9B.3 Inter-band EN-DC within FR1 498

Annex A (normative): Measurement channels 507

A.1 General 507

A.2 UL reference measurement channels for E-UTRA TDD Config 2 507

A.2.1 General 507

A.2.2 Reference measurement channels for E-UTRA 508

A.2.2.1 Full RB allocation 508

A.2.2.1.1 QPSK 508

A.2.2.1.2 16-QAM 509

A.2.2.1.3 64-QAM 510

A.2.2.1.4 256 QAM 511

A.2.2.2 Partial RB allocation 512

A.2.2.2.1 QPSK 512

A.2.2.2.2 16-QAM 515

A.2.2.2.3 64-QAM 518

A.2.2.2.4 256 QAM 521

A.3 DL reference measurement channels for E-UTRA 524

A.3.1 General 524

A.3.1.1 QPSK 525

A.3.1.2 64-QAM 526

A.3.1.3 256-QAM 527

Annex B: Void 527

Annex C: Void 527

Annex D: Void 527

Annex E: Void 528

Annex F: Void 528

Annex G: Void 528

Annex H (normative): Modified MPR behavior 528

Annex I (normative): Dual uplink interferer 529

Annex J: Void 529

Annex K: Void 529

Annex L (informative): Change history 530