|  |  |
| --- | --- |
| 3GPP TS 38.101-1 V16.14.0 (2022-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 1: Range 1 Standalone  (Release 16) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 16

1 Scope 18

2 References 18

3 Definitions, symbols and abbreviations 18

3.1 Definitions 18

3.2 Symbols 19

3.3 Abbreviations 21

4 General 23

4.1 Relationship between minimum requirements and test requirements 23

4.2 Applicability of minimum requirements 23

4.3 Specification suffix information 23

5 Operating bands and channel arrangement 24

5.1 General 24

5.2 Operating bands 24

5.2A Operating bands for CA 26

5.2A.0 General 26

5.2A.1 Intra-band CA 26

5.2A.2 Inter-band CA 27

5.2A.2.1 Inter-band CA (two bands) 27

5.2A.2.2 Inter-band CA (three bands) 31

5.2A.2.3 Inter-band CA (four bands) 32

5.2B Operating bands for DC 32

5.2C Operating band combination for SUL 32

5.2D Operating bands for UL MIMO 33

5.2E Operating band for V2X 33

5.2E.1 V2X operating bands 33

5.2E.2 V2X operating bands for con-current operation 34

5.3 UE channel bandwidth 34

5.3.1 General 34

5.3.2 Maximum transmission bandwidth configuration 35

5.3.3 Minimum guardband and transmission bandwidth configuration 35

5.3.4 RB alignment 37

5.3.5 UE channel bandwidth per operating band 37

5.3.6 Asymmetric channel bandwidths 40

5.3A UE channel bandwidth for CA 41

5.3A.1 General 41

5.3A.2 Maximum transmission bandwidth configuration for CA 41

5.3A.3 Minimum guardband and transmission bandwidth configuration for CA 41

5.3A.4 Void 43

5.3A.5 UE channel bandwidth per operating band for CA 43

5.3E Channel bandwidth for V2X 44

5.3E.1 General 44

5.3E.2 Channel bandwidth for V2X concurrent operation 45

5.4 Channel arrangement 45

5.4.1 Channel spacing 45

5.4.1.1 Channel spacing for adjacent NR carriers 45

5.4.2 Channel raster 45

5.4.2.1 NR-ARFCN and channel raster 45

5.4.2.2 Channel raster to resource element mapping 46

5.4.2.3 Channel raster entries for each operating band 46

5.4.3 Synchronization raster 49

5.4.3.1 Synchronization raster and numbering 49

5.4.3.3 Synchronization raster entries for each operating band 50

5.4.4 TX–RX frequency separation 53

5.4A Channel arrangement for CA 53

5.4A.1 Channel spacing for CA 53

5.4A.2 Channel raster for CA 54

5.4A.3 Synchronization raster for CA 54

5.4A.4 Tx-Rx frequency separation for CA 54

5.4B Reserved 54

5.4C Reserved 54

5.4D Reserved 54

5.4E Channel arrangement for V2X 54

5.4E.1 Channel spacing 54

5.4E.2 Channel raster 55

5.4E.2.1 NR-ARFCN and channel raster 55

5.4E.2.2 Channel raster to resource element mapping 55

5.4E.2.3 Channel raster entries for each operating band 55

5.4E.3 Synchronization raster for V2X 55

5.5 Void 55

5.5A Configurations for CA 55

5.5A.0 General 55

5.5A.1 Configurations for intra-band contiguous CA 57

5.5A.2 Configurations for intra-band non-contiguous CA 60

5.5A.3 Configurations for inter-band CA 60

5.5A.3.1 Configurations for inter-band CA (two bands) 60

5.5A.3.2 Configurations for inter-band CA (three bands) 72

5.5A.3.3 Configurations for inter-band CA (four bands) 80

5.5B Configurations for DC 83

5.5C Configurations for SUL 84

6 Transmitter characteristics 84

6.1 General 84

6.1A General 84

6.1F General 84

6.2 Transmitter power 84

6.2.1 UE maximum output power 84

6.2.2 UE maximum output power reduction 86

6.2.3 UE additional maximum output power reduction 89

6.2.3.1 General 89

6.2.3.2 A-MPR for NS\_04 94

6.2.3.3 A-MPR for NS\_10 95

6.2.3.4 A-MPR for NS\_05 and NS\_05U 95

6.2.3.5 A-MPR for NS\_40 98

6.2.3.6 A-MPR for NS\_43 and NS\_43U 98

6.2.3.7 A-MPR for NS\_03 and NS\_03U 99

6.2.3.8 A-MPR for NS\_37 100

6.2.3.9 A-MPR for NS\_38 101

6.2.3.10 A-MPR for NS\_39 101

6.2.3.11 A-MPR for NS\_41 101

6.2.3.12 A-MPR for NS\_42 102

6.2.3.13 A-MPR for NS\_18 102

6.2.3.14 A-MPR for NS\_21 103

6.2.3.15 A-MPR for NS\_24 103

6.2.3.16 A-MPR for NS\_27 104

6.2.3.17 A-MPR for NS\_46 105

6.2.3.18 A-MPR for NS\_47 106

6.2.3.19 A-MPR for NS\_50 107

6.2.3.20 A-MPR for NS\_44 107

6.2.3.21 A-MPR for NS\_12 108

6.2.3.22 A-MPR for NS\_13 108

6.2.3.23 A-MPR for NS\_14 109

6.2.3.24 A-MPR for NS\_15 110

6.2.3.25 A-MPR for NS\_45 110

6.2.3.26 A-MPR for NS\_48 111

6.2.3.27 A-MPR for NS\_49 111

6.2.3.28 A-MPR for NS\_51 112

6.2.4 Configured transmitted power 113

6.2A Transmitter power for CA 115

6.2A.1 UE maximum output power for CA 115

6.2A.1.1 UE maximum output power for Intra-band contiguous CA 115

6.2A.1.2 UE maximum output power for Intra-band non-contiguous CA 115

6.2A.1.3 UE maximum output power for Inter-band CA 116

6.2A.1.4 Void 119

6.2A.1.5 Void 119

6.2A.2 UE maximum output power reduction for CA 119

6.2A.2.1 UE maximum output power reduction for Intra-band contiguous CA 119

6.2A.2.2 UE maximum output power reduction for Intra-band non-contiguous CA 121

6.2A.2.2.0 General 121

6.2A.2.2.1 MPR to meet -30dBm/MHz 121

6.2A.2.2.2 MPR to meet -13dBm/MHz 122

6.2A.2.3 UE maximum output power reduction for Inter-band CA 122

6.2A.2.4 Void 122

6.2A.3 UE additional maximum output power reduction for CA 122

6.2A.3.1.1 UE additional maximum output power reduction for Intra-band contiguous CA 122

6.2A.3.1.1.1 A-MPR for CA\_NS\_04 123

6.2A.3.1.2 UE additional maximum output power reduction for Intra-band non-contiguous CA 129

6.2A.3.1.3 UE additional maximum output power reduction for Inter-band CA 131

6.2A.4 Configured output power for CA 134

6.2A.4.1 Configured transmitted power level 134

6.2A.4.1.1 Configured transmitted power for Intra-band contiguous CA 134

6.2A.4.1.2 Configured transmitted power for Intra-band non-contiguous CA 136

6.2A.4.1.3 Configured transmitted power for Inter-band CA 138

6.2A.4.1.4 Void 140

6.2A.4.2 ΔTIB,c for CA 140

6.2A.4.2.1 Void 140

6.2A.4.2.2 Void 140

6.2A.4.2.3 ΔTIB,c for Inter-band CA (two bands) 140

6.2A.4.2.4 ΔTIB,c for Inter-band CA (three bands) 145

6.2A.4.2.5 ΔTIB,c for Inter-band CA (four bands) 148

6.2B Transmitter power for NR-DC 148

6.2B.0 General 148

6.2B.1 UE maximum output power for NR-DC 148

6.2B.2 UE maximum output power reduction for NR-DC 149

6.2B.3 UE additional maximum output power reduction for NR-DC 149

6.2B.4 Configured output power for NR-DC 149

6.2B.4.1 Configured transmitted power level for NR-DC 149

6.2B.4.2 ΔTIB,c for NR-DC 152

6.2C Transmitter power for SUL 152

6.2C.1 Configured transmitted power for SUL 152

6.2C.2 ΔTIB,c 152

6.2D Transmitter power for UL MIMO 153

6.2D.1 UE maximum output power for UL MIMO 153

6.2D.2 UE maximum output power reduction for UL MIMO 154

6.2D.3 UE additional maximum output power reduction for UL MIMO 155

6.2D.4 Configured transmitted power for UL MIMO 155

6.2E Transmitter power for V2X 156

6.2E.1 UE maximum output power for V2X 156

6.2E.1.1 General 156

6.2E.1.2 UE maximum output power for V2X con-current operation 157

6.2E.2 UE maximum output power reduction for V2X 157

6.2E.2.1 General 157

6.2E.2.2 MPR for Power class 3 V2X UE 157

6.2E.2.3 MPR for Power class 3 V2X con-current operation 158

6.2E.3 UE additional maximum output power reduction for V2X 158

6.2E.3.1 General 158

6.2E.3.2 A-MPR for Power class 3 V2X UE by NS\_33 159

6.2E.3.3 A-MPR for Power class 3 V2X UE by NS\_52 161

6.2E.3.4 A-MPR for power class 3 V2X con-current operation 162

6.2E.4 Configured transmitted power for V2X 162

6.2E.4.1 General 162

6.2E.4.2 Configured transmitted power for V2X con-current operation 163

6.2F Transmitter power for shared spectrum channel access 164

6.2F.1 UE maximum output power 164

6.2F.1A UE maximum output power for CA 165

6.2F.1A.1 UE maximum output power for inter-band CA 165

6.2F.2 UE maximum output power reduction 165

6.2F.2A UE maximum output power reduction for CA 166

6.2F.2A.1 UE maximum output power reduction for inter-band CA 166

6.2F.3 UE additional maximum output power reduction 166

6.2F.3.1 General 166

6.2F.3.2 A-MPR for NS\_28 167

6.2F.3.3 A-MPR for NS\_29 168

6.2F.3.4 A-MPR for NS\_30 168

6.2F.3.5 A-MPR for NS\_31 169

6.2F.3.6 A-MPR for NS\_53 169

6.2F.3.7 A-MPR for NS\_54 170

6.2F.3A UE additional maximum output power reduction for CA 170

6.2F.3A.1 UE additional maximum output power reduction for inter-band CA 170

6.2F.4 Configured transmitted power 171

6.3 Output power dynamics 171

6.3.1 Minimum output power 171

6.3.2 Transmit OFF power 171

6.3.3 Transmit ON/OFF time mask 172

6.3.3.1 General 172

6.3.3.2 General ON/OFF time mask 172

6.3.3.3 Transmit power time mask for slot and short or long subslot boundaries 172

6.3.3.4 PRACH time mask 173

6.3.3.5 Void 174

6.3.3.6 SRS time mask 174

6.3.3.7 PUSCH-PUCCH and PUSCH-SRS time masks 175

6.3.3.8 Transmit power time mask for consecutive slot or long subslot transmission and short subslot transmission boundaries 177

6.3.3.9 Transmit power time mask for consecutive short subslot transmissions boundaries 177

6.3.4 Power control 178

6.3.4.1 General 178

6.3.4.2 Absolute power tolerance 178

6.3.4.3 Relative power tolerance 179

6.3.4.4 Aggregate power tolerance 179

6.3A Output power dynamics for CA 179

6.3A.1 Minimum output power for CA 179

6.3A.1.1 Minimum output power for intra-band contiguous CA 179

6.3A.1.2 Minimum output power for intra-band non-contiguous CA 180

6.3A.1.3 Minimum output power for inter-band CA 180

6.3A.1.4 Void 180

6.3A.2 Transmit OFF power for CA 180

6.3A.2.1 Transmit OFF power for intra-band contiguous CA 180

6.3A.2.2 Transmit OFF power for intra-band non-contiguous CA 180

6.3A.2.3 Transmit OFF power for inter-band CA 180

6.3A.2.4 Void 180

6.3A.3 Transmit ON/OFF time mask for CA 180

6.3A.3.1 Transmit ON/OFF time mask for intra-band contiguous CA 180

6.3A.3.2 Transmit ON/OFF time mask for intra-band non-contiguous CA 181

6.3A.3.3 Transmit ON/OFF time mask for inter-band CA 181

6.3A.3.3.1 General 181

6.3A.3.3.2 Time mask for switching between two uplink carriers 181

6.3A.3.4 Void 182

6.3A.4 Power control for CA 182

6.3A.4.1 Power control for intra-band contiguous CA 182

6.3A.4.1.1 Absolute power tolerance 182

6.3A.4.1.2 Relative power tolerance 182

6.3A.4.1.3 Aggregate power control tolerance 183

6.3A.4.2 Power control for intra-band non-contiguous CA 183

6.3A.4.2.1 Absolute power tolerance 183

6.3A.4.2.1.1 Minimum requirements 183

6.3A.4.2.2 Relative power tolerance 183

6.3A.4.2.2.1 Minimum requirements 183

6.3A.4.2.3 Aggregate power control tolerance 183

6.3A.4.3 Power control for inter-band CA 183

6.3A.4.4 Void 183

6.3B Output power dynamics for NR-DC 183

6.3C Output power dynamics for SUL 184

6.3C.1 Void 184

6.3C.2 Void 184

6.3C.3 Transmit ON/OFF time mask for SUL 184

6.3C.3.1 Time mask for switching between two uplink carriers 184

6.3D Output power dynamics for UL MIMO 185

6.3D.1 Minimum output power for UL MIMO 185

6.3D.2 Transmit OFF power for UL MIMO 185

6.3D.3 Transmit ON/OFF time mask for UL MIMO 185

6.3D.4 Power control for UL MIMO 185

6.3E Output power dynamics for V2X 185

6.3E.1 Minimum output power for V2X 185

6.3E.1.1 General 185

6.3E.1.2 Minimum output power for V2X con-current operation 186

6.3E.2 Transmit OFF power for V2X 186

6.3E.2.1 General 186

6.3E.2.2 Transmit OFF power for V2X con-current operation 186

6.3E.3 Transmit ON/OFF time mask for V2X 186

6.3E.3.1 General 186

6.3E.3.2 General time mask 187

6.3E.3.3 S-SSB time mask 187

6.3E.3.4 Transmit ON/OFF time mask for V2X con-current operation 188

6.3E.4 Power control for V2X 188

6.3E.4.1 General 188

6.3E.4.2 Absolute power tolerance 188

6.3E.4.3 Power control for V2X con-current operation 188

6.3F Output power dynamics for shared spectrum channel access 188

6.3F.1 Minimum output power 188

6.3F.2 Transmit OFF power 188

6.3F.3 Transmit ON/OFF time mask 188

6.3F.3.1 General 188

6.3F.3.2 General ON/OFF time mask 188

6.3F.3A General ON/OFF mask for CA 189

6.3F.3A.1 General ON/OFF mask for inter-band CA 189

6.3F.4 Power control 189

6.3F.4.1 General 189

6.3F.4.2 Absolute power tolerance 189

6.3F.4.3 Relative power tolerance 189

6.3F.4.4 Aggregate power tolerance 189

6.4 Transmit signal quality 190

6.4.1 Frequency error 190

6.4.2 Transmit modulation quality 190

6.4.2.0 General 190

6.4.2.1 Error Vector Magnitude 190

6.4.2.1a Error Vector Magnitude including symbols with transient period 191

6.4.2.2 Carrier leakage 192

6.4.2.3 In-band emissions 192

6.4.2.4 EVM equalizer spectrum flatness 193

6.4.2.4.1 Requirements for Pi/2 BPSK modulation 194

6.4A Transmit signal quality for CA 195

6.4A.1 Frequency error for CA 195

6.4A.1.1 Frequency error for intra-band contiguous CA 195

6.4A.1.2 Frequency error for intra-band non-contiguous CA 195

6.4A.1.3 Frequency error for inter-band CA 195

6.4A.1.4 Void 196

6.4A.2 Transmit modulation quality for CA 196

6.4A.2.1 Transmit modulation quality for intra-band contiguous CA 196

6.4A.2.1.0 General 196

6.4A.2.1.1 Error Vector Magnitude 196

6.4A.2.1.2 In-band emissions 196

6.4A.2.1.3 Carrier leakage 199

6.4A.2.2 Transmit modulation quality for intra-band non-contiguous CA 199

6.4A.2.2.0 General 199

6.4A.2.2.1 Error Vector Magnitude 199

6.4A.2.2.2 In-band emissions 200

6.4A.2.2.3 Carrier leakage 200

6.4A.2.3 Transmit modulation quality for inter-band CA 200

6.4A.2.4 Void 200

6.4B Transmit signal quality for NR-DC 200

6.4D Transmit signal quality for UL MIMO 200

6.4D.0 General 200

6.4D.1 Frequency error for UL MIMO 201

6.4D.2 Transmit modulation quality for UL MIMO 201

6.4D.2.0 General 201

6.4D.2.1 Error Vector Magnitude 201

6.4D.2.2 Carrier leakage 201

6.4D.2.3 In-band emissions 201

6.4D.2.4 EVM equalizer spectrum flatness for UL MIMO 201

6.4D.3 Time alignment error for UL MIMO 202

6.4D.4 Requirements for coherent UL MIMO 202

6.4E Transmit signal quality for V2X 202

6.4E.1 Frequency error for V2X 202

6.4E.1.1 General 202

6.4E.1.2 Frequency error for V2X con-current operation 203

6.4E.2 Transmit modulation quality for V2X 203

6.4E.2.1 General 203

6.4E.2.2 Error Vector Magnitude for V2X 203

6.4E.2.3 Carrier leakage for V2X 203

6.4E.2.4 In-band emissions for V2X 203

6.4E.2.5 EVM equalizer spectrum flatness for V2X 203

6.4E.2.6 Transmit modulation quality for V2X con-current operation 203

6.4F Transmit signal quality for shared spectrum channel access 204

6.4F.1 Frequency error 204

6.4F.2 Transmit modulation quality 204

6.4F.2.0 General 204

6.4F.2.1 Error Vector Magnitude 204

6.4F.2.2 Carrier leakage 204

6.4F.2.3 In-band emissions 204

6.4F.2.4 EVM equalizer spectrum flatness 205

6.4F.2A Transmit modulation quality for CA 205

6.4F.2A.1 Transmit modulation quality for inter-band CA 205

6.5 Output RF spectrum emissions 206

6.5.1 Occupied bandwidth 206

6.5.2 Out of band emission 206

6.5.2.1 General 206

6.5.2.2 Spectrum emission mask 206

6.5.2.3 Additional spectrum emission mask 207

6.5.2.3.1 Requirements for network signalling value "NS\_35" 207

6.5.2.3.2 Requirements for network signalling value "NS\_04" 208

6.5.2.3.3 Requirements for network signalling values "NS\_03", “NS\_03U”, and "NS\_21" 208

6.5.2.3.4 Requirements for network signalling value "NS\_06" 209

6.5.2.3.5 Void 210

6.5.2.3.6 Void 210

6.5.2.3.7 Void 210

6.5.2.3.8 Requirements for network signalling value "NS\_27" 210

6.5.2.4 Adjacent channel leakage ratio 210

6.5.2.4.1 NR ACLR 210

6.5.2.4.2 UTRA ACLR 211

6.5.3 Spurious emissions 211

6.5.3.0 General 211

6.5.3.1 General spurious emissions 212

6.5.3.2 Spurious emissions for UE co-existence 212

6.5.3.3 Additional spurious emissions 220

6.5.3.3.1 Requirement for network signalling value "NS\_04" 220

6.5.3.3.2 Requirement for network signalling value "NS\_17" 221

6.5.3.3.3 Requirement for network signalling value "NS\_18" 221

6.5.3.3.4 Requirement for network signalling values "NS\_05" and “NS\_05U” 221

6.5.3.3.5 Requirement for network signalling values "NS\_43" and “NS\_43U” 221

6.5.3.3.6 Requirement for network signalling value "NS\_37" 222

6.5.3.3.7 Requirement for network signalling value "NS\_38" 222

6.5.3.3.8 Requirement for network signalling value "NS\_39" 222

6.5.3.3.9 Requirement for network signalling value "NS\_40" 222

6.5.3.3.10 Requirement for network signalling value "NS\_41" 223

6.5.3.3.11 Requirement for network signalling value "NS\_42" 223

6.5.3.3.12 Requirement for network signalling value "NS\_21" 223

6.5.3.3.13 Requirement for network signalling value "NS\_24" 223

6.5.3.3.14 Requirement for network signalling value "NS\_27" 224

6.5.3.3.15 Requirement for network signalling value "NS\_47" 224

6.5.3.3.16 Requirement for network signalling value "NS\_50" 224

6.5.3.3.17 Requirement for network signalling value "NS\_12" 225

6.5.3.3.18 Requirement for network signalling value "NS\_13" 225

6.5.3.3.19 Requirement for network signalling value "NS\_14" 225

6.5.3.3.20 Requirement for network signalling value "NS\_15" 225

6.5.3.3.21 Requirement for network signalling value "NS\_45" 226

6.5.3.3.22 Requirement for network signalling values "NS\_48" and "NS\_51" 226

6.5.3.3.23 Requirement for network signalling value "NS\_49" 226

6.5.3.3.24 Requirement for network signalling value "NS\_44" 227

6.5.3.3.25 Requirement for network signalling value "NS\_46" 227

6.5.4 Transmit intermodulation 227

6.5A Output RF spectrum emissions for CA 228

6.5A.0 General 228

6.5A.1 Occupied bandwidth for CA 228

6.5A.1.1 Void 228

6.5A.1.1a Occupied bandwidth for Intra-band contiguous CA 228

6.5A.1.2 Occupied bandwidth for Intra-band non-contiguous CA 228

6.5A.1.3 Occupied bandwidth for Inter-band CA 228

6.5A.2 Out of band emission for CA 228

6.5A.2.1 General 228

6.5A.2.2 Spectrum emission mask 229

6.5A.2.2.1 Spectrum emission mask for intra-band contiguous CA 229

6.5A.2.2.2 Spectrum emission mask for intra-band non-contiguous CA 229

6.5A.2.2.3 Spectrum emission mask for Inter-band CA 229

6.5.A.2.2.4 Void 229

6.5A.2.3 Additional spectrum emission mask for CA 229

6.5A.2.3.1 Additional spectrum emission mask for intra-band contiguous CA 229

6.5A.2.3.1 Void 230

6.5A.2.3.2 Additional spectrum emission mask for Intra-band non-contiguous CA 230

6.5A.2.3.2.1 Minimum requirement (network signalling value “CA\_NC\_NS\_04”) 230

6.5A.2.3.3 Additional spectrum emission mask for Inter-band CA 230

6.5A.2.4 Adjacent channel leakage ratio 230

6.5A.2.4.1 NR ACLR 230

6.5A.2.4.2 UTRA ACLR 232

6.5A.3 Spurious emission for CA 232

6.5A.3.1 General spurious emissions 232

6.5A.3.2 Spurious emissions for UE co-existence 233

6.5A.3.2.1 Spurious emissions for UE co-existence for intra-band contiguous CA 233

6.5A.3.2.2 Spurious emissions for UE co-existence for intra-band non-contiguous CA 234

6.5A.3.2.3 Spurious emissions for UE co-existence for Inter-band CA 234

6.5A.3.2.4 Void 244

6.5A.3.2.5 Void 244

6.5A.3.2.6 Void 244

6.5A.3.3 Additional spurious emissions for CA 244

6.5A.3.3.1 Additional spurious emissions for intra-band contiguous CA 244

6.5A.3.3.2 Additional spurious emissions for intra-band non-contiguous CA 245

6.5A.4 Transmit intermodulation for CA 245

6.5A.4.2.1 Transmit intermodulation for intra-band contiguous CA 245

6.5A.4.2.2 Void 245

6.5B Output RF spectrum emissions for NR-DC 245

6.5D Output RF spectrum emissions for UL MIMO 246

6.5D.1 Occupied bandwidth for UL MIMO 246

6.5D.2 Out of band emission for UL MIMO 246

6.5D.3 Spurious emission for UL MIMO 246

6.5D.4 Transmit intermodulation for UL MIMO 246

6.5E Output RF spectrum emissions for V2X 247

6.5E.1 Occupied bandwidth for V2X 247

6.5E.1.1 General 247

6.5E.1.2 Occupied bandwidth for V2X con-current operation 247

6.5E.2 Out of band emission for V2X 247

6.5E.2.1 General 247

6.5E.2.2 Spectrum emission mask 247

6.5E.2.2.1 General 247

6.5E.2.2.2 Spectrum emission mask for V2X con-current operation 247

6.5E.2.3 Additional Spectrum emission mask 247

6.5E.2.3.1 Requirements for network signalling value "NS\_33" 247

6.5E.2.3.2 Requirements for network signalling value "NS\_52" 248

6.5E.2.4 Adjacent channel leakage ratio 248

6.5E.2.4.1 General 248

6.5E.2.4.2 ACLR for V2X con-current operation 249

6.5E.3 Spurious emissions for V2X 249

6.5E.3.1 General spurious emissions 249

6.5E.3.2 Spurious emissions for UE co-existence 249

6.5E.3.3 Spurious emissions for UE co-existence for V2X con-current operation 249

6.5E.3.4 Additional spurious emissions requirements for V2X 250

6.5E.3.4.1 General 250

6.5E.3.4.2 Requirements for network signalling value "NS\_33" 250

6.5E.3.4.3 Void 251

6.5E.4 Transmit intermodulation 251

6.5E.4.1 General 251

6.5E.4.2 Transmit intermodulation for V2X con-current operation 251

6.5F Output RF spectrum emissions 251

6.5F.1 Occupied bandwidth 251

6.5F.2 Out of band emission 251

6.5F.2.1 General 251

6.5F.2.2 Spectrum emission mask for operation with shared spectrum channel access 251

6.5F.2.2.0 General 251

6.5F.2.2.1 Spectrum emission mask for non-transmitted channels 252

6.5F.2.3 Additional spectrum emission mask 252

6.5F.2.4 Adjacent channel leakage ratio 252

6.5F.2.4.0 General 252

6.5F.2.4.1 Shared spectrum channel access ACLR 253

6.5F.2.4.2 Additional requirement for network signaled value "NS\_29" 253

6.5F.3 Spurious emissions 253

6.5F.3.0 General 253

6.5F.3.1 General spurious emissions 253

6.5F.3.2 Spurious emissions for UE co-existence 253

6.5F.3.3 Additional spurious emissions 254

6.5F.3.3.0 General 254

6.5F.3.3.1 Requirement for network signalling value "NS\_28" 254

6.5F.3.3.2 Requirement for network signalling value "NS\_29" 254

6.5F.3.3.3 Requirement for network signalling value "NS\_30" 256

6.5F.3.3.4 Requirement for network signalling value "NS\_31" 257

6.5F.3.3.5 Requirements for network signalling value "NS\_53" or "NS\_54" 258

6.5F.4 Transmit intermodulation 258

6.6 Void 258

6.6E Time alignment error 258

7 Receiver characteristics 259

7.1 General 259

7.1A General 259

7.1F General 260

7.2 Diversity characteristics 260

7.3 Reference sensitivity 260

7.3.1 General 260

7.3.2 Reference sensitivity power level 260

7.3.3 ΔRIB,c 268

7.3A Reference sensitivity for CA 269

7.3A.1 General 269

7.3A.2 Reference sensitivity power level for CA 269

7.3A.2.1 Reference sensitivity power level for Intra-band contiguous CA 269

7.3A.2.2 Reference sensitivity power level for Intra-band non-contiguous CA 269

7.3A.2.3 Reference sensitivity power level for Inter-band CA 270

7.3A.2.4 Void 270

7.3A.3 ΔRIB,c for CA 270

7.3A.3.1 General 270

7.3A.3.2 ΔRIB,c for Inter-band CA 270

7.3A.3.2.1 ΔRIB,c for two bands 272

7.3A.3.2.2 Void 275

7.3A.3.2.3 ΔRIB,c for three bands 275

7.3A.3.2.4 ΔRIB,c for four bands 278

7.3A.4 Reference sensitivity exceptions due to UL harmonic interference for CA 278

7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 283

7.3A.6 Reference sensitivity exceptions due to cross band isolation for CA 289

7.3B Reference sensitivity for NR-DC 290

7.3C Reference sensitivity for SUL 290

7.3C.1 General 290

7.3C.2 Reference sensitivity power level for SUL 290

7.3C.3 ΔRIB,c for SUL 293

7.3C.3.1 General 293

7.3C.3.2 SUL band combination 293

7.3C.3.2.1 ΔRIB,c for two bands 294

7.3D Reference sensitivity for UL MIMO 294

7.3E Reference sensitivity for V2X 294

7.3E.1 General 294

7.3E.2 Minimum requirements 294

7.3F Reference sensitivity for shared spectrum channel access 296

7.3F.1 General 296

7.3F.2 Reference sensitivity power level 296

7.3F.3 ΔRIB,c 297

7.3F.4 Intra-band contiguous shared spectrum channel access CA 298

7.3F.5 Inter-band CA with shared spectrum channel access 298

7.3F.5.1 Reference sensitivity exceptions due to UL harmonic interference 298

7.3F.5.2 Reference sensitivity exceptions due to receiver harmonic mixing 298

7.3F.5.3 Reference sensitivity exceptions due to cross band isolation 299

7.4 Maximum input level 299

7.4A Maximum input level for CA 300

7.4A.1 Maximum input level for Intra-band contiguous CA 300

7.4A.2 Maximum input level for Intra-band non-contiguous CA 300

7.4A.3 Maximum input level for Inter-band CA 300

7.4B Maximum input level for NR-DC 301

7.4D Maximum input level for UL MIMO 301

7.4E Maximum input level for V2X 301

7.4E.1 General 301

7.4E.2 Maximum input level for V2X con-current operation 301

7.5 Adjacent channel selectivity 301

7.5A Adjacent channel selectivity for CA 306

7.5A.1 Adjacent channel selectivity for Intra-band contiguous CA 306

7.5A.2 Adjacent channel selectivity Intra-band non-contiguous CA 308

7.5A.3 Adjacent channel selectivity Inter-band CA 309

7.5B Adjacent channel selectivity for NR-DC 309

7.5D Adjacent channel selectivity for UL MIMO 309

7.5E Adjacent channel selectivity for V2X 309

7.5E.1 General 309

7.5E.2 Adjacent channel selectivity for V2X con-current operation 310

7.5F Adjacent channel selectivity 310

7.5F.1 General 310

7.5F.2 Intra-band contiguous shared spectrum channel access CA 311

7.6 Blocking characteristics 312

7.6.1 General 312

7.6.2 In-band blocking 312

7.6.3 Out-of-band blocking 316

7.6.4 Narrow band blocking 319

7.6A Blocking characteristics for CA 320

7.6A.1 General 320

7.6A.2 In-band blocking for CA 320

7.6A.2.1 In-band blocking for Intra-band contiguous CA 320

7.6A.2.2 In-band blocking for Intra-band non-contiguous CA 321

7.6A.2.3 In-band blocking for Inter-band CA 321

7.6A.3 Out-of-band blocking for CA 322

7.6A.3.1 Out-of-band blocking for Intra-band contiguous CA 322

7.6A.3.2 Out-of-band blocking for Intra-band non-contiguous CA 323

7.6A.3.3 Out-of-band blocking for Inter-band CA 324

7.6A.4 Narrow band blocking for CA 325

7.6A.4.1 Narrow band blocking for Intra-band contiguous CA 325

7.6A.4.2 Narrow band blocking for Intra-band non-contiguous CA 325

7.6A.4.3 Narrow band blocking for Inter-band CA 326

7.6B Blocking characteristics for NR-DC 326

7.6C Blocking characteristics for SUL 326

7.6C.1 General 326

7.6C.2 In-band blocking for SUL 326

7.6C.3 Out-of-band blocking for SUL 326

7.6C.4 Narrow band blocking for SUL 327

7.6D Blocking characteristics for UL MIMO 327

7.6E Blocking characteristics for V2X 327

7.6E.1 General 327

7.6E.2 In-band blocking 327

7.6E.2.1 General 327

7.6E.2.2 In-band blocking for V2X con-current operation 328

7.6E.3 Out-of-band blocking 328

7.6E.3.1 General 328

7.6E.3.2 Out-of-band blocking for V2X con-current operation 329

7.6F Blocking characteristics 329

7.6F.1 General 329

7.6F.2 In-band blocking 329

7.6F.2.1 General 329

7.6F.2.2 Intra-band contiguous shared spectrum channel access CA 330

7.6F.3 Out-of-band blocking 331

7.6F.3.1 General 331

7.6F.3.2 Intra-band contiguous shared spectrum channel access CA 332

7.7 Spurious response 332

7.7A Spurious response for CA 334

7.7A.1 Spurious response for Intra-band contiguous CA 334

7.7A.2 Spurious response for Intra-band non-contiguous CA 334

7.7A.3 Spurious response for Inter-band CA 334

7.7B Spurious response for NR-DC 334

7.7D Spurious response for UL MIMO 335

7.7E Spurious response for V2X 335

7.7E.1 General 335

7.7E.2 Spurious response for V2X con-current operation 335

7.7F Spurious response for shared spectrum channel access 335

7.7F.1 General 335

7.7F.2 Intra-band contiguous shared spectrum channel access CA 336

7.8 Intermodulation characteristics 336

7.8.1 General 336

7.8.2 Wide band Intermodulation 336

7.8A Intermodulation characteristics for CA 339

7.8A.1 General 339

7.8A.2 Wide band intermodulation for CA 339

7.8A.2.1 Wide band intermodulation for Intra-band contiguous CA 339

7.8A.2.2 Wide band intermodulation for Intra-band non-contiguous CA 340

7.8A.2.3 Wide band intermodulation for Inter-band CA 340

7.8B Intermodulation characteristics for NR-DC 340

7.8D Intermodulation characteristics for UL MIMO 341

7.8E Intermodulation characteristics for V2X 341

7.8E.1 General 341

7.8E.2 Wide band Intermodulation 341

7.8E.2.1 General 341

7.8E.2.2 Wide band Intermodulation for V2X con-current operation 341

7.8F Intermodulation characteristics for shared spectrum channel access 341

7.8F.1 General 341

7.8F.2 Wide band Intermodulation 342

7.9 Spurious emissions 342

7.9A Spurious emissions for CA 343

7.9A.1 Void 343

7.9A.2 Void 343

7.9A.3 Spurious emissions for Inter-band CA 343

7.9B Spurious emissions for NR-DC 343

Annex A (normative): Measurement channels 341

A.1 General 341

A.2 UL reference measurement channels 341

A.2.1 General 341

A.2.2 Reference measurement channels 342

A.2.2.1 DFT-s-OFDM Pi/2-BPSK 342

A.2.2.2 DFT-s-OFDM QPSK 343

A.2.2.3 DFT-s-OFDM 16QAM 344

A.2.2.4 DFT-s-OFDM 64QAM 345

A.2.2.5 DFT-s-OFDM 256QAM 346

A.2.2.6 CP-OFDM QPSK 347

A.2.2.7 CP-OFDM 16QAM 349

A.2.2.8 CP-OFDM 64QAM 351

A.2.2.9 CP-OFDM 256QAM 353

A.2.3 Reference measurement channels for TDD 355

A.2.3.1 DFT-s-OFDM Pi/2-BPSK 355

A.2.3.2 DFT-s-OFDM QPSK 355

A.2.3.3 DFT-s-OFDM 16QAM 355

A.2.3.4 DFT-s-OFDM 64QAM 355

A.2.3.5 DFT-s-OFDM 256QAM 356

A.2.3.6 CP-OFDM QPSK 356

A.2.3.7 CP-OFDM 16QAM 356

A.2.3.8 CP-OFDM 64QAM 356

A.2.3.9 CP-OFDM 256QAM 357

A.3 DL reference measurement channels 358

A.3.1 General 358

A.3.2 DL reference measurement channels for FDD 359

A.3.2.1 General 359

A.3.2.2 FRC for receiver requirements for QPSK 359

A.3.2.3 FRC for maximum input level for 64QAM 361

A.3.2.4 FRC for maximum input level for 256 QAM 364

A.3.3 DL reference measurement channels for TDD 367

A.3.3.1 General 367

A.3.3.2 FRC for receiver requirements for QPSK 368

A.3.3.3 FRC for maximum input level for 64QAM 371

A.3.3.4 FRC for maximum input level for 256 QAM 374

A.4 CSI reference measurement channels 377

A.5 OFDMA Channel Noise Generator (OCNG) 377

A.5.1 OCNG Patterns for FDD 377

A.5.1.1 OCNG FDD pattern 1: Generic OCNG FDD Pattern for all unused REs 377

A.5.2 OCNG Patterns for TDD 377

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 377

A.6 Void 378

A.7 V2X reference measurement channels 378

A.7.1 General 378

A.7.2 FRC for V2X receiver requirements for QPSK 378

A.7.3 FRC for maximum input level for 64QAM 380

A.7.4 FRC for maximum input level for 256QAM 381

Annex B (informative): Void 383

Annex C (informative): Downlink physical channels 384

C.1 General 384

C.2 Setup 384

C.3 Connection 384

C.3.1 Measurement of Receiver Characteristics 384

Annex D (normative): Characteristics of the interfering signal 385

D.1 General 385

D.2 Interference signals 385

Annex E (normative): Environmental conditions 386

E.1 General 386

E.2 Environmental 386

E.2.1 Temperature 386

E.2.2 Voltage 387

E.2.3 Vibration 387

Annex F (normative): Transmit modulation 388

F.0 General 388

F.1 Measurement Point 388

F.2 Basic Error Vector Magnitude measurement 388

F.3 Basic in-band emissions measurement 389

F.4 Modified signal under test 390

F.5 Window length 392

F.5.1 Timing offset 392

F.5.2 Window length 392

F.5.3 Window length for normal CP 392

F.5.4 Window length for Extended CP 393

F.5.5 Window length for PRACH 394

F.6 Averaged EVM 395

F.7 Spectrum Flatness 396

F.8 396

F.9 396

F.10 EVM for UL MIMO 396

F10.1 General 396

F10.2 MIMO Equalization 397

F10.3 Layer processing 397

Annex G (normative): 399

G.0 General 399

G.1 Measurement Point 399

G.2 Relative Phase Error Measurement 400

G.2.1 Symbols and subcarriers used 400

G.2.2 CFO (carrier frequency offset) correction 400

G.2.3 Steps of the measurement method 400

Annex H (informative): Void 401

Annex I (informative): Void 401

Annex J (informative): Void 401

Annex K (informative): Void 401

Annex L (normative): ModifiedMPR-Behavior 401

L.1 Indication of modified MPR behavior 401

Annex M (informative): Change history 403