|  |  |
| --- | --- |
| 3GPP TS 38.307 V15.10.0 (2022-03) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  Requirements on User Equipments (UEs)  supporting a release-independent frequency band  (Release 15) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 4

1 Scope 6

2 References 6

3 Definitions, symbols and abbreviations 6

3.1 Definitions 6

3.2 Symbols 7

3.3 Abbreviations 7

4 General 7

5 Release independent features for NR frequency range 1 8

5.1 Additional NR operating bands and UE power classes for NR frequency range 1 8

5.2 Additional NR CA configurations for NR frequency range 1 8

5.2.1 Intra-band CA 8

5.2.2 Inter-band CA 9

5.3 Additional NR SUL configurations for NR frequency range 1 9

5.4 Other release independent features for NR frequency range 1 10

5.5 Other release independent requirements for NR frequency range 1 10

6 Release independent features for NR frequency range 2 11

6.1 Additional NR operating bands and UE power classes for NR frequency range 2 11

6.2 Additional NR CA configurations for NR frequency range 2 11

6.2.1 Intra-band CA 11

7 Release independent features for NR interworking between NR frequency range 1 and NR frequency range 2 12

7.1 Additional NR inter-band CA configurations between frequency range 1 and frequency range 2 12

7.2 Additional Inter-band NR-DC configurations between frequency range 1 and frequency range 2 13

8 Release independent features for NR interworking between NR and E-UTRA 13

8.1 Additional EN-DC configurations 13

8.1.1 Intra-band EN-DC 13

8.1.2 Inter-band EN-DC 14

8.1.2.1 Inter-band EN-DC within frequency range 1 14

8.1.2.2 Inter-band EN-DC including frequency range 2 15

8.1.2.3 Inter-band EN-DC including frequency range 1 and frequency range 2 15

Annex A (informative): Frequency arrangement for overlapping operating bands 16

Annex B (informative): Change history 16

# Foreword

This Technical Specification has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document specifies requirements for Rel-15 UEs supporting release independent features like:

- additional NR operating bands and power classes on top of Rel-15 of TS 38.101 [2-5] and TS 38.133 [6];

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 38.101-1: NR; User Equipment (UE) radio transmission and reception; Part 1: Range 1 Standalone

[3] 3GPP TS 38.101-2: NR; User Equipment (UE) radio transmission and reception; Part 2: Range 2 Standalone

[4] 3GPP TS 38.101-3: NR; User Equipment (UE) radio transmission and reception; Part 3: Range 1 and Range 2 Interworking operation with other radios

[5] 3GPP TS 38.101-4: NR; User Equipment (UE) radio transmission and reception; Part 4: UE performance requirements

[6] 3GPP TS 38.133: NR; Requirements for support of radio resource management

[7] 3GPP TS 38.306: NR; User Equipment (UE) radio access capabilities

# 3 Definitions, symbols and abbreviations

## 3.1 Definitions

For the purposes of the present document, the terms and definitions given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

**release independent**: applicable to some frozen releases, starting from a certain release Rel-M

NOTE 1: Normally, a feature is introduced only in the latest open release Rel-N and future releases are based on the previous one so that future releases inherit the requirements of this feature. Introducing a feature "in a release independent way from Rel-M onwards" (M<N) means it was decided by TSG RAN that this feature would be also beneficial in previous, already frozen releases starting with Rel-M until Rel-(N-1). In order to avoid touching TS 38.101 [2-5] or TS 38.133 [6] of these frozen releases, the corresponding requirements are captured in TS 38.307 via pointers to [2-5] or [6] of the release in which the feature was introduced.

NOTE 2: Release independent does not mean applicable to all releases.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

N Release in which a feature is introduced into TS 38.101 [2-5] or TS 38.133 [6]

M Release from which onwards (including release M) a feature is release independent

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

BW Bandwidth

CA Carrier Aggregation

CC Component carrier

DL Downlink

EN-DC Dual connectivity between E-UTRA and NR

FDD Frequency Division Duplex

FR1 Frequency range 1

FR2 Frequency range 2

NR New radio

PMI Precoding Matrix Indicator

REL Release

SDL Supplementary downlink

SUL Supplementary uplink

TDD Time Division Duplex

UE User Equipment

UL Uplink

# 4 General

TSG-RAN has agreed for certain features (see the following clauses) to introduce them in a "release independent way".

This means for each feature:

- it is "introduced" in a release N, i.e. TS 38.101 [2-5] and TS 38.133 [6] of release N define certain UE requirements for this feature; the feature is indicated in the tables of the following clauses;

- it is "release independent" starting from a release M (M<N); M for the given feature is provided in the tables of the following clauses;

- UEs supporting this feature have to fulfil additional requirements in release M or higher which are specified in one or more Annexes of TS 38.307 of release N; the applicable Annexes for a given feature are provided in the tables of the following clauses.

The applicable UE Categories are specified in TS 38.306 [7] according to the release to which the UE conforms.

In the table of release independent features in subsequent clauses, "FDD, TDD" refers to CA or EN-DC configuration composed by only FDD bands or only TDD bands, respectively. "FDD and TDD" refers to CA or EN-DC configuration including both FDD and TDD bands. "SDL and FDD, SDL and TDD" refers to CA configuration including both SDL and FDD bands or both SDL and TDD bands, respectively. "TDD and SUL" refers to SUL configuration including both TDD and SUL bands. "FDD and TDD and SUL" refers to EN-DC configuration including both FDD, TDD and SUL bands. Unless stated otherwise, the release independent for the band combinations are from Rel-15.

When a new feature is introduced only the latest release of release independent spec needs to be updated. The latest release of release independent spec refers to the release which the new feature is introduced in. If an RF feature introduced in the same release as the release which the feature is independent from, (i.e. M=N), the common UE RF requirements table in annex B.4 is specified from release N+1, otherwise the common UE RF requirements table is specified from release N.

# 5 Release independent features for NR frequency range 1

## 5.1 Additional NR operating bands and UE power classes for NR frequency range 1

Requirements for a Rel-15 UE for additional NR operating bands power classes and UE channel bandwidth compared to TS 38.101-1 of Rel-15 [2] are introduced via this clause.

Table 5.1-1: NR operating bands

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 38.307 of the release in which the band was introduced) |
| Operating bands | FDD, TDD, SDL, SUL | Rel-15 |  |

Table 5.1-2: NR UE power class

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 38.307 of the release in which the power class was introduced) |
| Power Class 1 | FDD | Rel-15 |  |
| Power Class 2 | TDD | Rel-15 |  |
| Power Class 3 | FDD, TDD, SUL | Rel-15 |  |

Table 5.1-3: NR UE channel bandwidth

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 38.307 of the release in which the UE channel bandwidth was introduced) |
| UE channel bandwidth | FDD, TDD, SUL, SDL | Rel-15 |  |

## 5.2 Additional NR CA configurations for NR frequency range 1

### 5.2.1 Intra-band CA

Requirements for a Rel-15 UE for additional NR intraband CA configurations within FR1 compared to TS 38.101-1 of Rel-15 [2] are introduced via this clause.

Table 5.2.1-1: NR intra-band CA within FR1

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | CA BW Class | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Intra-band contiguous CA configurations within FR1 | DL | C, D, E, G, H, I, J, K, L | TDD | Rel-15 |  |
| UL | A | TDD | Rel-15 |  |

### 5.2.2 Inter-band CA

Requirements for a Rel-15 UE for additional NR inter-band CA configurations within FR1 compared to TS 38.101-1 of Rel-15 [2] are introduced via this clause.

Table 5.2.2-1: NR inter-band CA within FR1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | Maximum number of bands | number of CCs | CA BW Classes | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Inter-band CA configurations within NR FR1 | DL | 2 | 2 | A | TDD, FDD, SDL and FDD, SDL and TDD | Rel-15 |  |
| UL | 2 | 2 | A | TDD, FDD and TDD | Rel-15 |  |

## 5.3 Additional NR SUL configurations for NR frequency range 1

Requirements for a Rel-15 UE for additional NR SUL configurations within FR1 compared to TS 38.101-1 of Rel-15 [2] are introduced via this clause.

Table 5.3-1: NR SUL within FR1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | number of bands | number of CCs | CA BW Classes | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the SUL configuration was introduced) |
| Inter-band SUL configurations within NR FR1 | DL | 1 | 1 | A | TDD | Rel-15 |  |
| UL | 2 | 2 | A | TDD and SUL | Rel-15 |  |

## 5.4 Other release independent features for NR frequency range 1

This clause covers requirements for a Rel-15 UE coming from all other release independent features that are not covered under clause 5.1, 5.2 and 5.3, e.g. generic baseband requirements or requirements that are not band/CA/SUL configuration specific.

Table 5.4-1: Additional requirements of other release independent features

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Release  independent from | Requirements to be fulfilled  (see 38.307 of the REL when the feature was introduced) | Further information |
| RRM requirements for high speed train scenario | Rel-15 (NOTE 1) | Table C.1-1 | Rel-16 WI NR\_HST introduced band independent RRM requirements: see Table C.1-1 |
| UE demodulation requirements for high speed train scenario | Rel-15 (NOTE 1) | Table C.2-1 | Rel-16 WI NR\_HST introduced band independent UE demodulation requirements: see Table C.2-1 |
| RF requirements for 4Rx UEs | Rel-15 |  |  |
| NOTE 1: Rel-15 UEs supporting the high speed train are assumed to read the Rel-16 high speed train scenario information, which is broadcast to all UEs. | | | |

## 5.5 Other release independent requirements for NR frequency range 1

This clause covers requirements for a Rel-15 UE coming from all other release independent requirements with the corresponding features introduced in Rel-15.

Table 5.5-1: Release independent requirements with the corresponding features introduced in Rel-15

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Release  independent from | Requirements to be fulfilled  (see 38.307 of the REL when the feature was introduced) | Further information |
| Precoding matrix indicator (PMI) reporting requirements for TypeI-SinglePanel and TypeII Codebooks with more than 8TX and up to 32TX | Rel-15 | Table D.1-1, Table D.2-1 | Rel-16 NR\_perf\_enh-Perf WI introduced band independent PMI reporting requirements for 16TX and 32TX TypeI-SinglePanel Codebook, and 16TX TypeII Codebook. |
| PDSCH demoulation requirements with LTE CRS rate matching for TDD band | Rel-15 | Table E.1-1 | Rel-16 NR\_perf\_enh-Perf WI introduced band independent PDSCH demodulation requirements with LTE CRS rate matching for TDD band. |

# 6 Release independent features for NR frequency range 2

## 6.1 Additional NR operating bands and UE power classes for NR frequency range 2

Requirements for a Rel-15 UE for additional NR operating bands power classes and UE channel bandwidth compared to TS 38.101-2 of Rel-15 [3] are introduced via this clause.

Table 6.1-1: NR operating bands

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 38.307 of the release in which the band was introduced) |
| Operating bands | TDD | Rel-15 |  |

Table 6.1-2: NR UE power class

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 38.307 of the release in which the band was introduced) |
| Power Class 1, 2, 3, 4 | TDD | Rel-15 |  |

Table 6.1-3: NR UE channel bandwidth

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 38.307 of the release in which the UE channel bandwidth was introduced) |
| UE channel bandwidth | TDD | Rel-15 |  |

## 6.2 Additional NR CA configurations for NR frequency range 2

### 6.2.1 Intra-band CA

Requirements for a Rel-15 UE for additional NR intra-band CA configurations within FR2 compared to TS 38.101-2 of Rel-15 [3] are introduced via this clause.

Table 6.2.1-1: NR intra-band contiguous CA within FR2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | CA BW Class | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Intra-band contiguous CA configurations within FR2 | DL | B, C, D, E, F, G, H, I, J, K, L, M, O, P, Q | TDD | Rel-15 |  |
| UL | B, D, E, F, G, H, I, J, K, L, M, O, P, Q | TDD | Rel-15 |

Table 6.2.1-2: NR non-contiguous intra-band CA within FR2

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | number of sub-blocks | maximum number of CCs within a sub-block | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Intra-band non-contiguous CA configurations within FR2 | DL | 2 | 4 | TDD | Rel-15 |  |
| 3 | 1 | TDD | Rel-15 |
| 4 | 1 | TDD | Rel-15 |

# 7 Release independent features for NR interworking between NR frequency range 1 and NR frequency range 2

## 7.1 Additional NR inter-band CA configurations between frequency range 1 and frequency range 2

Requirements for a Rel-15 UE for additional NR inter-band CA configurations between FR1 and FR2 compared to TS 38.101-3 of Rel-15 [4] are introduced via this clause.

Table 7.1-1: NR inter-band CA between FR1 and FR2

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | number of bands | maximum number of CCs | CA BW Classes | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Inter-band CA configurations for NR interworking between FR1 and FR2 | DL FR1 | 1 | 2 | A, C | FDD, TDD | Rel-15 |  |
| DL FR2 | 1 | 4 | A, D, E, F | TDD | Rel-15 |  |
| UL FR1 | 1 | 1 | A | FDD, TDD | Rel-15 |  |
| UL FR2 | 1 | 1 | A | TDD | Rel-15 |  |

## 7.2 Additional Inter-band NR-DC configurations between frequency range 1 and frequency range 2

Requirements for a Rel-15 UE for additional Inter-band NR-DC configurations between FR1 and FR2 compared to TS 38.101-3 of Rel-15 [4] are introduced via this clause.

Table 7.2-1: Inter-band NR-DC between FR1 and FR2

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | number of bands | maximum number of CCs | CA BW Classes | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Inter-band DC configurations for NR interworking between FR1 and FR2 | DL FR1 | 1 | 2 | A, C | TDD | Rel-15 |  |
| DL FR2 | 1 | 8 | A, D, E, F, G, H, I, J, K, L, M | TDD | Rel-15 |  |
| UL FR1 | 1 | 1 | A | TDD | Rel-15 |  |
| UL FR2 | 1 | 1 | A | TDD | Rel-15 |  |

# 8 Release independent features for NR interworking between NR and E-UTRA

## 8.1 Additional EN-DC configurations

### 8.1.1 Intra-band EN-DC

Requirements for a Rel-15 UE for additional EN-DC intra-band configurations within FR1 compared to TS 38.101-3 of Rel-15 [4] are introduced via this clause.

Table 8.1.1-0: EN-DC intra-band UE power class

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 38.307 of the release in which the band was introduced) |
| Intra-band contiguous EN-DC power class 2 | TDD | Rel-15 |  |
| Intra-band contiguous EN-DC power class 3 | FDD, TDD | Rel-15 |  |
| Intra-band non-contiguous EN-DC power class 2 | TDD | Rel-15 |  |
| Intra-band non-contiguous EN-DC power class 3 | FDD, TDD | Rel-15 |  |

Table 8.1.1-1: EN-DC contiguous intra-band configurations within FR1

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | maximum number of E-UTRA CCs | maximum number of NR CCs | Duplex-mode | Release  independent from | **requirements to be fulfilled**  (see 38.307 of the REL in which the CA configuration was introduced) |
| Intra-band contiguous EN-DC | DL | 3 | 1 | FDD, TDD | Rel-15 |  |
| UL | 1 | 1 | FDD, TDD | Rel-15 |  |

Table 8.1.1-2: EN-DC non-contiguous intra-band configurations within FR1

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | maximum number of sub-blocks | maximum number of E-UTRA CCs | maximum number of NR CCs | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Intra-band EN-DC | DL | 2 | 3 | 1 | FDD, TDD | Rel-15 |  |
| UL | 2 | 1 | 1 | FDD, TDD | Rel-15 |  |

### 8.1.2 Inter-band EN-DC

#### 8.1.2.1 Inter-band EN-DC within frequency range 1

Requirements for a Rel-15 UE for additional EN-DC interband configurations within FR1 compared to TS 38.101-3 of Rel-15 [4] are introduced via this clause.

Table 8.1.2.1-0: EN-DC inter-band UE power class

|  |  |  |  |
| --- | --- | --- | --- |
| Feature | Duplex-mode | Release  independent from | Requirements to be fulfilled  (see TS 38.307 of the release in which the band was introduced) |
| Inter-band EN-DC Power Class 2 | TDD | Rel-15 | Table B.4.6-1 |
| Inter-band EN-DC Power Class 3 | FDD, TDD, FDD and TDD | Rel-15 |

Table 8.1.2.1-1: EN-DC inter-band configurations without SUL within FR1

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | maximum number of E-UTRA bands | maximum number of E-UTRA CCs | maximum number of NR bands | maximum number of NR CCs | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Inter-band EN-DC | DL | 4 | 5 | 2 | 2 | FDD, TDD,  FDD and TDD | Rel-15 |  |
| UL | 1 | 2 | 1 | 1 | FDD, TDD, FDD and TDD | Rel-15 |  |

Table 8.1.2.1-2: EN-DC inter-band configurations with SUL within FR1

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | maximum number of E-UTRA bands | maximum number of E-UTRA CCs | maximum number of NR bands | maximum number of NR CCs | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Inter-band EN-DC | DL | 2 | 3 | 1 | 1 | FDD, TDD,  FDD and TDD | Rel-15 |  |
| UL | 1 | 1 | 2 | 2 | FDD, TDD,  FDD and TDD, FDD and TDD and SUL | Rel-15 |  |

#### 8.1.2.2 Inter-band EN-DC including frequency range 2

Requirements for a Rel-15 UE for additional EN-DC inter-band configurations including FR2 compared to TS 38.101-3 of Rel-15 [4] are introduced via this clause.

Table 8.1.2.2-1: EN-DC inter-band configurations including FR2

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | number of E-UTRA bands | maximum number of E-UTRA CCs | number of NR bands | maximum number of NR CCs | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Inter-band EN-DC | DL | 4 | 5 | 1 | 8 | TDD, FDD and TDD | Rel-15 |  |
| UL | 1 | 2 | 1 | 8 | TDD, FDD and TDD | Rel-15 |  |

#### 8.1.2.3 Inter-band EN-DC including frequency range 1 and frequency range 2

Requirements for a Rel-15 UE for additional EN-DC inter-band configurations including FR1 and FR2 compared to TS 38.101-3 of Rel-15 [4] are introduced via this clause.

Table 8.1.2.3-1: EN-DC inter-band configurations including FR1 and FR2

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Feature | DL/UL | maximum number of E-UTRA bands | maximum number of E-UTRA CCs | maximum number of NR  bands | maximum number of NR  CCs | Duplex-mode | Release  independent from | requirements to be fulfilled  (see 38.307 of the REL in which the CA configuration was introduced) |
| Inter-band EN-DC | DL FR1 | 4 | 4 | 1 | 2 | TDD, FDD | Rel-15 |  |
| DL FR2 | 1 | 4 | TDD | Rel-15 |  |
| UL FR1 | 1 | 1 | 1 | 1 | FDD, TDD | Rel-15 |  |
| UL FR2 | 1 | 1 | TDD, | Rel-15 |  |

Annex A (informative):  
Frequency arrangement for overlapping operating bands

The following information is provided in order to assist a UE derive the DL NR-ARFCN and UL NR-ARFCN in a multi-band environment, in which multiple overlapping operating bands may be indicated in the fields *freqBandIndicatorNR* and *MultiFrequencyBandListNR-SIB*.

The overlapping bands, independent of release, which may be indicated in a cell are shown in Table A-1 for applicable NR operating bands. The DL NR-ARFCN and UL NR-ARFCN are derived according to TS 38.101-1 Rel-15.

Table A-1: Overlapping bands (multi-band environments) for each NR band

|  |  |  |
| --- | --- | --- |
| NR  Operating Band | Overlapping NR operating  bands | Duplex Mode |
| n2 | n25 | FDD |
| n25 | n2 | FDD |
| n38 | n41 | TDD |
| n41 | n38 | TDD |
| n77 | n78 | TDD |
| n78 | n77 | TDD |
| n80 | n86 | SUL |
| n86 | n80 | SUL |

Annex B (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2017-09 | RAN4#85 | R4-1712166 |  |  |  | Skeleton TS | 0.0.1 |
| 2018-03 | RAN4#86 | R4-1802107 |  |  |  | TS 38.307 v0.1.0 | 0.1.0 |
| 2018-06 | RAN#80 | RP-180988 |  |  |  | v1.0.0 submitted for plenary approval | 1.0.0 |
| 2018-06 | RAN#80 |  |  |  |  | Approved by plenary – Rel-15 spec under change control | 15.0.0 |
| 2018-09 | RAN#81 | RP-181896 | 0001 |  | F | CR for FR2 Power Classes in TS38.307 | 15.1.0 |
| 2018-12 | RAN#82 | RP-182362 | 0002 | 2 | B | CR for TS 38.307 | 15.2.0 |
| 2019-06 | RAN#84 | RP-191237 | 0005 |  | B | Addition of missing features for TS 38.307 | 15.3.0 |
| 2019-12 | RAN#86 | RP-193019 | 0010 |  | B | CR for REL-15 TS 38.307 for PC2 EN-DC TDD+TDD | 15.4.0 |
| 2019-12 | RAN#86 | RP-193036 | 0013 |  | F | Adding SDL to 38.307 | 15.4.0 |
| 2020-03 | RAN#87 | RP-200404 | 0017 | 1 | B | 38.307 CR power class REL-15 | 15.5.0 |
| 2020-06 | RAN#88 | RP-200986 | 0021 |  | F | Maintenance CR to 38307 on a reference spec number R15 | 15.6.0 |
| 2020-12 | RAN#90 | RP-202485 | 0039 |  | F | CR to TS 38.307 Release independence support of new channel bandwidth from Rel-15 | 15.7.0 |
| 2020-12 | RAN#90 | RP-202485 | 0031 | 1 | F | CR on adding NR ovelapping bands list in TS38.307 in Rel-15 | 15.7.0 |
| 2020-12 | RAN#90 | RP-202422 | 0033 | 1 | B | CR on release independent for Rel.16 NR HST RRM requirements | 15.7.0 |
| 2020-12 | RAN#90 | RP-202422 | 0034 | 1 | B | CR on release independent for Rel.16 NR HST UE demodulation requirements | 15.7.0 |
| 2021-03 | RAN#91 | RP-210065 | 0043 | 1 | B | Draft CR for TS 38.307 on UE demodulation performance requirements (Rel-15) | 15.8.0 |
| 2021-03 | RAN#91 | RP-210078 | 0046 |  | F | CR on release independent for Rel-16 NR HST UE demodulation requirements | 15.8.0 |
| 2021-09 | RAN#93 | RP-211921 | 0069 |  | F | CR to TS 38.307 on the definition of the duplex-mode for the band configurations | 15.9.0 |
| 2022-03 | RAN#95 | RP-220337 | 0091 |  | F | Big CR for TS 38.307 Maintenance (Rel-15) | 15.10.0 |
| 2022-03 | RAN#95 | RP-220352 | 0094 |  | F | CR for release independent for 4Rx support for NR band | 15.10.0 |