|  |  |
| --- | --- |
| 3GPP TS 38.133 V16.14.0 (2022-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  Requirements for support of radio resource management  (Release 16) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 42

1 Scope 44

2 References 44

3 Definitions, symbols and abbreviations 45

3.1 Definitions 45

3.2 Symbols 46

3.3 Abbreviations 47

3.4 Test tolerances 50

3.5 Frequency bands grouping 50

3.5.1 Introduction 50

3.5.2 NR operating bands in FR1 50

3.5.3 NR operating bands in FR2 51

3.6 Applicability of requirements in this specification version 51

3.6.1 RRC connected state requirements in DRX 52

3.6.2 Number of serving carriers 52

3.6.2.1 Number of serving carriers for SA 52

3.6.2.2 Number of serving carriers for EN-DC 52

3.6.2.3 Number of serving carriers for NE-DC 52

3.6.2.4 Number of serving carriers for NR-DC 53

3.6.3 Applicability for intra-band FR2 53

3.6.4 Applicability for FR2 UE power classes 53

3.6.5 Applicability for SDL bands 53

3.6.6 Applicability of requirements for NGEN-DC operation 53

3.6.7 Applicability of QCL 53

3.6.9 Applicability of requirements for scheduling availability 54

3.6.10 Applicability of requirements for measurement restrictions 54

4 SA: RRC\_IDLE state mobility 54

4.1 Cell Selection 54

4.2 Cell Re-selection 54

4.2.1 Introduction 54

4.2.2 Requirements 55

4.2.2.1 UE measurement capability 55

4.2.2.2 Measurement and evaluation of serving cell 55

4.2.2.3 Measurements of intra-frequency NR cells 56

4.2.2.4 Measurements of inter-frequency NR cells 57

4.2.2.5 Measurements of inter-RAT E-UTRAN cells 59

4.2.2.6 Maximum interruption in paging reception 61

4.2.2.7 General requirements 61

4.2.2.8 Minimum requirement at transitions 61

4.2.2.9 Measurements of intra-frequency NR cells for UE configured with relaxed measurement criterion 62

4.2.2.9.1 Introduction 62

4.2.2.9.2 Measurements for UE fulfilling low mobility criterion 62

4.2.2.9.3 Measurements for UE fulfilling not-at-cell edge criterion 63

4.2.2.9.4 Measurements for UE fulfilling low mobility and not-at-cell edge criteria 64

4.2.2.10 Measurements of inter-frequency NR cells for UE configured with relaxed measurement criterion 64

4.2.2.10.1 Introduction 64

4.2.2.10.2 Measurements for UE fulfilling low mobility criterion 64

4.2.2.10.3 Measurements for UE fulfilling not-at-cell edge criterion 65

4.2.2.10.4 Measurements for UE fulfilling low mobility and not-at-cell edge criterion 66

4.2.2.11 Measurements of inter-RAT E-UTRAN cells for UE configured with relaxed measurement criterion 67

4.2.2.11.1 Introduction 67

4.2.2.11.2 Measurements for UE fulfilling low mobility criterion 67

4.2.2.11.3 Measurements for UE fulfilling with not-at-cell edge criterion 68

4.2.2.11.4 Measurements for UE fulfilling low mobility and not-at-cell edge criterion 69

4.2A Cell Re-selection when subject to CCA 69

4.2A.1 Introduction 69

4.2A.2 Requirements 70

4.2A.2.1 UE measurement capability 70

4.2A.2.2 Measurement and evaluation when subject to CCA on the serving cell 70

4.2A.2.3 Measurements of intra-frequency NR cells when subject to CCA on the serving cell and target cell 71

4.2A.2.4 Measurements of inter-frequency NR cells when subject to CCA on the target cell 72

4.2A.2.5 Measurements of inter-RAT E-UTRAN cells when subject to CCA on the serving cell 74

4.2A.2.6 Maximum interruption in paging reception when subject to CCA on the target cell 74

4.2A.2.7 General requirements 74

4.3 Minimization of Drive Tests (MDT) 75

4.3.1 Introduction 75

4.3.2 Measurement Requirements 75

4.3.3 Requirements for Relative Time Stamp Accuracy 75

4.3.4 Requirements for Relative Time Stamp Accuracy for RRC Connection Establishment Failure Log Reporting 76

4.3.5 Requirements for Relative Time Stamp Accuracy for Radio Link Failure and Handover Failure Log Reporting 76

4.4 Idle Mode CA/DC Measurements 76

4.4.1 Introduction 76

4.4.2 Measurement Requirements 76

4.4.2.1 Detected cell requirement during state transition and Idle mode 76

4.4.2.2 Measurements of inter-frequency CA/DC candidate cells 77

4.4.2.3 Measurements on serving cell 78

4.4.2.4 Measurements of E-UTRAN inter-RAT DC candidate cells 78

5 SA: RRC\_INACTIVE state mobility 80

5.1 Cell Re-selection 80

5.1.1 Introduction 80

5.1.2 Requirements 80

5.1.2.1 UE measurement capability 80

5.1.2.2 Measurement and evaluation of serving cell 80

5.1.2.3 Measurements of intra-frequency NR cells 80

5.1.2.4 Measurements of inter-frequency NR cells 80

5.1.2.5 Measurements of inter-RAT E-UTRAN cells 80

5.1.2.6 Maximum interruption in paging reception 80

5.1.2.7 General requirements 80

5.1A Cell Re-selection with CCA 80

5.1A.1 Introduction 80

5.1A.2 Requirements 81

5.1A.2.1 UE measurement capability 81

5.1A.2.2 Measurement and evaluation when CCA is used on the serving cell 81

5.1A.2.3 Measurements of intra-frequency NR cells when CCA is used on the serving cell and target cell 81

5.1A.2.4 Measurements of inter-frequency NR cells when CCA is used on the target cell 81

5.1A.2.5 Measurements of inter-RAT E-UTRAN cells when CCA is used on the serving cell 81

5.1A.2.6 Maximum interruption in paging reception when CCA is used on the target cell 81

5.1A.2.7 General requirements 81

5.2 Void 81

5.3 Minimization of Drive Tests (MDT) 81

5.3.1 Introduction 81

5.3.2 Measurement Requirements 82

5.3.3 Requirements for Relative Time Stamp Accuracy 82

5.3.4 Requirements for Relative Time Stamp Accuracy for RRC Connection Establishment Failure Log Reporting 82

5.3.5 Requirements for Relative Time Stamp Accuracy for Radio Link Failure and Handover Failure Log Reporting 82

5.3.6 Requirements for Relative Time Stamp Accuracy for RRC Resume Failure Log Reporting 82

5.4 Idle Mode CA/DC Measurements 82

5.4.1 Introduction 82

5.4.2 Measurement Requirements 82

5.4.2.1 Detected cell requirement during state transition and Idle mode 83

5.4.2.2 Measurements of inter-frequency CA/DC candidate cells 83

5.4.2.3 Measurements on serving cell 83

5.4.2.4 Measurements on E-UTRAN inter-RAT DC candidate cells 83

6 RRC\_CONNECTED state mobility 83

6.1 Handover 83

6.1.1 NR Handover 83

6.1.1.1 Introduction 83

6.1.1.2 NR FR1 - NR FR1 Handover 83

6.1.1.2.1 Handover delay 83

6.1.1.2.2 Interruption time 83

6.1.1.3 NR FR2- NR FR1 Handover 84

6.1.1.3.1 Handover delay 84

6.1.1.3.2 Interruption time 84

6.1.1.4 NR FR2- NR FR2 Handover 85

6.1.1.4.1 Handover delay 85

6.1.1.4.2 Interruption time 85

6.1.1.5 NR FR1- NR FR2 Handover 86

6.1.1.5.1 Handover delay 86

6.1.1.5.2 Interruption time 86

6.1.2 NR Handover to other RATs 87

6.1.2.1 NR – E-UTRAN Handover 87

6.1.2.1.1 Introduction 87

6.1.2.1.2 Handover delay 87

6.1.2.1.3 Interruption time 87

6.1.2.2 NR – UTRAN Handover 88

6.1.2.2.1 Introduction 88

6.1.2.2.2 Handover delay 88

6.1.2.2.3 Interruption time 88

6.1.3 NR DAPS Handover 89

6.1.3.1 Introduction 89

6.1.3.2 NR FR1 - NR FR1 DAPS Handover 89

6.1.3.2.1 DAPS handover delay 89

6.1.3.2.2 Interruption time 90

6.1.3.3 NR FR2- NR FR1 DAPS Handover 92

6.1.3.3.1 DAPS handover delay 92

6.1.3.3.2 Interruption time 92

6.1.3.4 NR FR1- NR FR2 DAPS Handover 93

6.1.3.4.1 DAPS handover delay 93

6.1.3.4.2 Interruption time 93

6.1.4 NR Conditional Handover 94

6.1.4.1 Introduction 94

6.1.4.2 NR FR1 – NR FR1 conditional handover 94

6.1.4.3 NR FR2 – NR FR1 conditional handover 95

6.1.4.4 NR FR2 – NR FR2 conditional handover 96

6.1.4.4.1 Handover delay 96

6.1.4.4.2 Measurement time 96

6.1.4.4.3 Preparation time 96

6.1.4.4.4 Interruption time 96

6.1.4.5 NR FR1 – NR FR2 conditional handover 97

6.1A Void 97

6.1A.1 Void 97

6.1A.1.1 Void 97

6.1A.1.2 Void 97

6.1A.1.2.1 Void 97

6.1A.1.2.2 Void 97

6.1B Handover to target cell using CCA 97

6.1B.1 NR Handover 97

6.1B.1.1 Introduction 97

6.1B.1.2 NR FR1 - NR FR1 Handover 98

6.1B.1.2.1 Handover delay 98

6.1B.1.2.2 Interruption time 98

6.2 RRC Connection Mobility Control 99

6.2.1 SA: RRC Re-establishment 99

6.2.1.1 Introduction 99

6.2.1.2 Requirements 99

6.2.1.2.1 UE Re-establishment delay requirement 99

6.2.1A RRC Re-establishment with CCA 100

6.2.1A.1 Introduction 100

6.2.1A.2 Requirements 101

6.2.1A.2.1 UE Re-establishment with CCA delay requirement 101

6.2.2 Random access 103

6.2.2.1 Introduction 103

6.2.2.2 Requirements for 4-step RA type 103

6.2.2.2.1 Contention based random access 103

6.2.2.2.2 Non-Contention based random access 104

6.2.2.2.3 UE behaviour when configured with supplementary UL 105

6.2.2.3 Requirements for 2-step RA type 105

6.2.2.3.1 Contention based random access 105

6.2.2.3.2 Non-Contention based random access 106

6.2.2.3.3 UE behaviour when configured with supplementary UL 107

6.2.2A Random access when CCA is used on target frequency 107

6.2.2A.1 Introduction 107

6.2.2A.2 Requirements for 4-step RA type 107

6.2.2A.2.1 Contention based random access 107

6.2.2A.2.2 Non-Contention based random access 108

6.2.2A.3 Requirements for 2-step RA type 109

6.2.2A.3.1 Contention based random access 110

6.2.2A.3.2 Non-Contention based random access 111

6.2.3 SA: RRC Connection Release with Redirection 112

6.2.3.1 Introduction 112

6.2.3.2 Requirements 112

6.2.3.2.1 RRC connection release with redirection to NR 112

6.2.3.2.2 RRC connection release with redirection to E-UTRAN 113

6.2.3.2.3 RRC connection release with redirection to NR carrier subject to CCA 113

7 Timing 114

7.1 UE transmit timing 114

7.1.1 Introduction 114

7.1.2 Requirements 115

7.1.2.1 Gradual timing adjustment 116

7.1.2.2 Void 116

7.2 UE timer accuracy 116

7.2.1 Introduction 116

7.2.2 Requirements 117

7.3 Timing advance 117

7.3.1 Introduction 117

7.3.2 Requirements 117

7.3.2.1 Timing Advance adjustment delay 117

7.3.2.2 Timing Advance adjustment accuracy 117

7.4 Cell phase synchronization accuracy 117

7.4.1 Definition 117

7.4.2 Minimum requirements 117

7.5 Maximum Transmission Timing Difference 118

7.5.1 Introduction 118

7.5.2 Minimum Requirements for inter-band EN-DC 118

7.5.2.1 Minimum Requirements for inter-band synchronous EN-DC 118

7.5.3 Minimum Requirements for intra-band EN-DC 119

7.5.4 Minimum Requirements for NR Carrier Aggregation 119

7.5.5 Minimum Requirements for inter-band NE-DC 119

7.5.5.1 Minimum Requirements for inter-band synchronous NE-DC 120

7.5.6 Minimum Requirements for inter-band NR DC 120

7.6 Maximum Receive Timing Difference 121

7.6.1 Introduction 121

7.6.2 Minimum Requirements for inter-band EN-DC 121

7.6.2.1 Minimum Requirements for inter-band synchronous EN-DC 121

7.6.3 Minimum Requirements for intra-band EN-DC 122

7.6.4 Minimum Requirements for NR Carrier Aggregation 122

7.6.5 Minimum Requirements for inter-band NE-DC 123

7.6.5.1 Minimum Requirements for inter-band synchronous NE-DC 123

7.6.6 Minimum Requirements for inter-band NR DC 124

7.7 *deriveSSB-IndexFromCell* tolerance 124

7.7.1 Minimum requirements 124

7.8 Void 125

8 Signalling characteristics 125

8.1 Radio Link Monitoring 125

8.1.1 Introduction 125

8.1.2 Requirements for SSB based radio link monitoring 126

8.1.2.1 Introduction 126

8.1.2.2 Minimum requirement 127

8.1.2.3 Measurement restrictions for SSB based RLM 128

8.1.3 Requirements for CSI-RS based radio link monitoring 129

8.1.3.1 Introduction 129

8.1.3.2 Minimum requirement 130

8.1.3.3 Measurement restrictions for CSI-RS based RLM 132

8.1.4 Minimum requirement at transitions 132

8.1.5 Minimum requirement for UE turning off the transmitter 133

8.1.6 Minimum requirement for L1 indication 133

8.1.7 Scheduling availability of UE during radio link monitoring 133

8.1.7.1 Scheduling availability of UE performing radio link monitoring with a same subcarrier spacing as PDSCH/PDCCH on FR1 133

8.1.7.2 Scheduling availability of UE performing radio link monitoring with a different subcarrier spacing than PDSCH/PDCCH on FR1 133

8.1.7.3 Scheduling availability of UE performing radio link monitoring on FR2 134

8.1.7.4 Scheduling availability of UE performing radio link monitoring on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR-DC 134

8.1A Radio Link Monitoring with CCA on Target Frequency 134

8.1A.1 Introduction 134

8.1A.2 Requirements for SSB Based Radio Link Monitoring 135

8.1A.2.1 Introduction 135

8.1A.2.2 Minimum Requirement 136

8.1A.3 Minimum requirement at transitions 137

8.1A.4 Minimum requirement for UE turning off the transmitter 138

8.1A.5 Minimum requirement for L1 indication 138

8.1A.6 Scheduling availability of UE during radio link monitoring 138

8.1A.6.1 Scheduling availability of UE performing radio link monitoring with the same subcarrier spacing as PDSCH/PDCCH 138

8.1A.6.2 Scheduling availability of UE performing radio link monitoring with a different subcarrier spacing than PDSCH/PDCCH 138

8.2 Interruption 139

8.2.1 EN-DC Interruption 139

8.2.1.1 Introduction 139

8.2.1.2 Requirements 139

8.2.1.2.1 Interruptions at transitions between active and non-active during DRX 139

8.2.1.2.2 Interruptions at transitions from non-DRX to DRX 140

8.2.1.2.3 Interruptions at SCell addition/release 140

8.2.1.2.4 Interruptions at SCell activation/deactivation 141

8.2.1.2.5 Interruptions during measurements on SCC 142

8.2.1.2.6 Interruptions at UL carrier RRC reconfiguration 143

8.2.1.2.7 Interruptions due to Active BWP switching Requirement 144

8.2.1.2.8 Interruptions at direct SCell activation and hibernation 145

8.2.1.2.9 Interruptions at SCell hibernation 145

8.2.1.2.10 Interruptions at SCell activation/deactivation with multiple downlink SCells 146

8.2.1.2.11 Interruptions due to UE-specific CBW change 146

8.2.1.2.12 Interruptions at NR SRS carrier based switching 146

8.2.1.2.13 Interruptions at E-UTRA SRS carrier based switching 147

8.2.1.2.14 DL Interruptions at switching between two uplink carriers 148

8.2.1.2.15 Interruptions due to SCell dormancy 149

8.2.1.2.16 Interruptions when identifying CGI of an NR cell with autonomous gaps 149

8.2.1.2.17 Interruptions when identifying CGI of an E-UTRA cell with autonomous gaps 150

8.2.2 SA: Interruptions with Standalone NR Carrier Aggregation 150

8.2.2.1 Introduction 150

8.2.2.2 Requirements 151

8.2.2.2.1 Interruptions at SCell addition/release 151

8.2.2.2.2 Interruptions at SCell activation/deactivation 152

8.2.2.2.3 Interruptions during measurements on deactivated SCC 153

8.2.2.2.4 Interruptions at UL carrier RRC reconfiguration 154

8.2.2.2.5 Interruptions due to Active BWP switching Requirement 154

8.2.2.2.6 Interruptions at inter-frequency SFTD measurement 155

8.2.2.2.7 Interruptions at SCell activation/deactivation with multiple downlink SCells 156

8.2.2.2.8 Interruptions due to UE-specific CBW change 156

8.2.2.2.9 Interruptions at NR SRS carrier based switching 157

8.2.2.2.10 DL Interruptions at UE switching between two uplink carriers 158

8.2.2.2.11 Interruptions at direct SCell activation 159

8.2.2.2.12 Interruptions due to SCell dormancy 159

8.2.2.2.13 Interruptions at transitions between active and non-active during DRX 159

8.2.2.2.14 Interruptions when identifying CGI of an NR cell with autonomous gaps 160

8.2.2.2.15 Interruptions when identifying CGI of an E-UTRA cell with autonomous gaps 160

8.2.3 NE-DC Interruptions 161

8.2.3.1 Introduction 161

8.2.3.2 Requirements 161

8.2.3.2.1 Interruptions at transitions between active and non-active during DRX 161

8.2.3.2.2 Interruptions at transitions from non-DRX to DRX 162

8.2.3.2.3 Interruptions at PSCell/SCell addition/release 162

8.2.3.2.4 Interruptions at SCell activation/deactivation 163

8.2.3.2.5 Interruptions during measurements on SCC 164

8.2.3.2.6 Interruptions at UL carrier RRC reconfiguration 165

8.2.3.2.7 Interruptions due to Active BWP switching Requirement 166

8.2.3.2.8 Interruptions at direct SCell activation and hibernation 166

8.2.3.2.9 Interruptions at SCell hibernation 166

8.2.3.2.10 Interruptions at SCell activation/deactivation with multiple downlink SCells 167

8.2.3.2.11 Interruptions at NR SRS carrier based switching 167

8.2.3.2.12 Interruptions at E-UTRA SRS carrier based switching 168

8.2.3.2.13 Interruptions due to SCell dormancy 169

8.2.3.2.14 Interruptions when identifying CGI of an NR cell with autonomous gaps 170

8.2.3.2.15 Interruptions when identifying CGI of an E-UTRA cell with autonomous gaps 170

8.2.3.2.16 Interruptions due to UE-specific CBW change 171

8.2.4 NR-DC: Interruptions 171

8.2.4.1 Introduction 171

8.2.4.2 Requirements 172

8.2.4.2.1 Interruptions at PSCell/SCell addition/release 172

8.2.4.2.3 Interruptions during measurements on SCC 173

8.2.4.2.4 Interruptions at UL carrier RRC reconfiguration 173

8.2.4.2.5 Interruptions due to Active BWP switching Requirement 174

8.2.4.2.6 Interruptions at transitions between active and non-active during DRX 174

8.2.4.2.7 Interruptions at transitions from non-DRX to DRX 174

8.2.4.2.8 Interruptions at SCell activation/deactivation with multiple downlink SCells 175

8.2.4.2.9 Interruptions at NR SRS carrier based switching 175

8.2.4.2.10 Interruptions at direct SCell activation 176

8.2.4.2.11 Interruptions when identifying CGI of an NR cell with autonomous gaps 177

8.2.4.2.12 Interruptions when identifying CGI of an E-UTRA cell with autonomous gaps 177

8.2.4.2.13 Interruptions due to SCell dormancy 178

8.2.4.2.14 Interruptions due to UE-specific CBW change 178

8.2.4.2A Void 179

8.2.4.2A.1 Void 179

8.2.4.2A.2 Void 179

8.2.4.2A.3 Void 179

8.3 SCell Activation and Deactivation Delay 179

8.3.1 Introduction 179

8.3.2 SCell Activation Delay Requirement for Deactivated SCell 179

8.3.3 SCell Deactivation Delay Requirement for Activated SCell 183

8.3.4 Direct SCell Activation at SCell addition 183

8.3.5 Direct SCell Activation at Handover 185

8.3.7 SCell Activation Delay Requirement for Deactivated SCell with Multiple Downlink SCells 187

8.3.8 SCell Deactivation Delay Requirement for Activated SCell with Multiple Downlink SCells 191

8.3.9 Direct SCell Activation of Multiple Downlink SCells at SCell addition 191

8.3.10 Direct SCell Activation of Multiple Downlink SCells at Handover 192

8.3A SCell Activation and Deactivation Delay in Carriers with CCA 194

8.3A.1 Introduction 194

8.3A.2 SCell Activation Delay Requirement for Deactivated SCell 194

8.3A.3 SCell Deactivation Delay Requirement for Activated SCell 197

8.4 UE UL carrier RRC reconfiguration delay 197

8.4.1 Introduction 197

8.4.2 UE UL carrier configuration delay requirement 197

8.4.3 UE UL carrier deconfiguration delay requirement 197

8.5 Link Recovery Procedures 198

8.5.1 Introduction 198

8.5.2 Requirements for SSB based beam failure detection 198

8.5.2.1 Introduction 198

8.5.2.2 Minimum requirement 199

8.5.2.3 Measurement restriction for SSB based beam failure detection 200

8.5.3 Requirements for CSI-RS based beam failure detection 201

8.5.3.1 Introduction 201

8.5.3.2 Minimum requirement 202

8.5.3.3 Measurement restrictions for CSI-RS beam failure detection 204

8.5.4 Minimum requirement for L1 indication 205

8.5.5 Requirements for SSB based candidate beam detection 205

8.5.5.1 Introduction 205

8.5.5.2 Minimum requirement 205

8.5.5.3 Measurement restriction for SSB based candidate beam detection 207

8.5.6 Requirements for CSI-RS based candidate beam detection 208

8.5.6.1 Introduction 208

8.5.6.2 Minimum requirement 208

8.5.6.3 Measurement restriction for CSI-RS based candidate beam detection 210

8.5.7 Scheduling availability of UE during beam failure detection 211

8.5.7.1 Scheduling availability of UE performing beam failure detection with a same subcarrier spacing as PDSCH/PDCCH on FR1 211

8.5.7.2 Scheduling availability of UE performing beam failure detection with a different subcarrier spacing than PDSCH/PDCCH on FR1 211

8.5.7.3 Scheduling availability of UE performing beam failure detection on FR2 211

8.5.7.4 Scheduling availability of UE performing beam failure detection on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR DC 212

8.5.8 Scheduling availability of UE during candidate beam detection 212

8.5.8.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH on FR1 212

8.5.8.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH on FR1 212

8.5.8.3 Scheduling availability of UE performing L1-RSRP measurement on FR2 212

8.5.8.4 Scheduling availability of UE performing L1-RSRP measurement on FR1 or FR2 in case of FR1-FR2 inter-band CA and NR-DC 213

8.5.9 Requirements for Beam Failure Recovery in SCell 213

8.5.9.1 Introduction 213

8.5.9.2 Requirement 213

8.5.10 Minimum requirement at transitions for beam failure detection 213

8.5A Link Recovery Procedures when CCA is used on target frequency 214

8.5A.1 Introduction 214

8.5A.2 Requirements for SSB based beam failure detection 214

8.5A.2.1 Introduction 214

8.5A.2.2 Minimum requirement 215

8.5A.2.3 Measurement restriction for SSB based beam failure detection 215

8.5A.4 Minimum requirement for L1 indication 216

8.5A.5 Requirements for SSB based candidate beam detection 216

8.5A.5.1 Introduction 216

8.5A.5.2 Minimum requirement 216

8.5A.5.3 Measurement restriction for SSB based candidate beam detection 217

8.5A.7 Scheduling availability of UE during beam failure detection 217

8.5A.7.1 Scheduling availability of UE performing beam failure detection with a same subcarrier spacing as PDSCH/PDCCH 217

8.5A.7.2 Scheduling availability of UE performing beam failure detection with a different subcarrier spacing than PDSCH/PDCCH 217

8.5A.8 Scheduling availability of UE during candidate beam detection 217

8.5A.8.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH 218

8.5A.8.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH 218

8.6 Active BWP switch delay 218

8.6.1 Introduction 218

8.6.2 DCI and timer based BWP switch delay on a single CC 218

8.6.2A DCI based BWP switch delay on multiple CCs 219

8.6.2A.1 Simultaneous DCI based BWP switch delay on multiple CCs 219

8.6.2A.2 Non-simultaneous DCI based BWP switch delay on multiple CCs 221

8.6.2B Timer based BWP switch delay on multiple CCs 221

8.6.2B.1 Simultaneous timer based BWP switch delay on multiple CCs 221

8.6.2B.2 Non-simultaneous timer based BWP switch delay on multiple CCs 222

8.6.3 RRC based BWP switch delay on a single CC 222

8.6.3A RRC based BWP switch delay on multiple CCs 223

8.6.3A.1 Simultaneous RRC based BWP switch delay on multiple CCs 223

8.6.3A.2 Non-simultaneous RRC based BWP switch delay on multiple CCs 223

8.6.4 BWP switch delay on Consistent UL CCA recovery 224

8.7 Void 224

8.8 NE-DC: E-UTRAN PSCell Addition and Release Delay 224

8.8.1 Introduction 224

8.8.2 E-UTRAN PSCell Addition Delay Requirement 224

8.8.3 E-UTRAN PSCell Release Delay Requirement 225

8.9 NR-DC: PSCell Addition and Release Delay 225

8.9.1 Introduction 225

8.9.2 PSCell Addition Delay Requirement 225

8.9.3 PSCell Release Delay Requirement 226

8.10 Active TCI state switching delay 226

8.10.4 DCI based TCI state switch delay 228

8.10.5 RRC based TCI state switch delay 228

8.10.6 Active TCI state list update delay 228

8.10A Active TCI state switching delay with CCA 229

8.10A.1 Introduction 229

8.10A.2 Known conditions for TCI state 229

8.10A.3 MAC-CE based TCI state switch delay 229

8.10A.4 DCI based TCI state switch delay 230

8.10A.5 RRC based TCI state switch delay 230

8.10A.6 Active TCI state list update delay 231

8.11 PSCell Change 231

8.11A void 232

8.11B Conditional PSCell Change 232

8.11B.1 Introduction 232

8.11B.2 Conditoinal PSCell Change delay 232

8.11B.2.1 Measurement time 232

8.12 Uplink spatial relation switch delay 233

8.12.1 Introduction 233

8.12.2 Known conditions for spatial relation when associated with DL-RS 233

8.12.3 MAC-CE based spatial relation switch delay 233

8.12.4 DCI based spatial relation switch delay 234

8.12.5 RRC based spatial relation switch delay 234

8.13 UE-specific CBW change 235

8.13.1 Introduction 235

8.13.2 UE-specific CBW change delay 235

8.14 Pathloss reference signal switching delay 235

8.14.1 Introduction 235

8.14.2 Known conditions for pathloss reference signal 235

8.14.3 MAC-CE based pathloss reference signal switch delay 236

9 Measurement Procedure 236

9.1 General measurement requirement 236

9.1.1 Introduction 236

9.1.2 Measurement gap 237

9.1.2.1 EN-DC: Measurement Gap Sharing 248

9.1.2.1a SA: Measurement Gap Sharing 248

9.1.2.1b NE-DC: Measurement Gap Sharing 249

9.1.2.1c NR-DC: Measurement Gap Sharing 250

9.1.3 UE Measurement capability 251

9.1.3.1 EN-DC: Monitoring of multiple layers using gaps 251

9.1.3.1a SA: Monitoring of multiple layers using gaps 251

9.1.3.1b NE-DC: Monitoring of multiple layers using gaps 252

9.1.3.1c NR-DC: Monitoring of multiple layers using gaps 252

9.1.3.2 EN-DC: Maximum allowed layers for multiple monitoring 253

9.1.3.2a SA: Maximum allowed layers for multiple monitoring 254

9.1.3.2b NE-DC: Maximum allowed layers for multiple monitoring 254

9.1.3.2c NR-DC: Maximum allowed layers for multiple monitoring 255

9.1A.3.2 Void 256

9.1.3A UE Measurement capability under operation mode with CCA 256

9.1.3A.1 EN-DC: Monitoring of multiple layers using gaps under CCA 256

9.1.3A.1A SA: Monitoring of multiple layers using gaps under CCA 256

9.1.3A.2 EN-DC: Maximum allowed layers for multiple monitoring under CCA 256

9.1A.3.2a Void 257

9.1.3A.2A SA: Maximum allowed layers for multiple monitoring under CCA 257

9.1.4 Capabilities for Support of Event Triggering and Reporting Criteria 257

9.1.4.1 Introduction 257

9.1.4.2 Requirements 257

9.1.5 Carrier-specific scaling factor 261

9.1.5.1 Monitoring of multiple layers outside gaps 261

9.1.5.1.1 EN-DC mode: carrier-specific scaling factor for SSB-based, CSI-RS based L3 measurements and RSSI and channel occupancy measurements performed outside gaps 263

9.1.5.1.2 SA mode: carrier-specific scaling factor for SSB-based, CSI-RS based L3 measurements and RSSI and channel occupancy measurements performed outside gaps 264

9.1.5.1.3 NR-DC mode: carrier-specific scaling factor for SSB-based and CSI-RS based L3 measurements performed outside gaps 265

9.1.5.1.4 NE-DC mode: carrier-specific scaling factor for SSB-based and CSI-RS based measurements performed outside gaps 266

9.1.5.2 Monitoring of multiple layers within gaps 267

9.1.5.2.1 EN-DC mode: carrier-specific scaling factor for SSB, CSI-RS-based L3 measurements and RSSI and channel occupancy measurements performed within gaps 268

9.1.5.2.2 SA mode: carrier-specific scaling factor for SSB, CSI-RS-based L3 measurements and RSSI and channel occupancy measurements performed within gaps 270

9.1.5.2.3 NE-DC: carrier-specific scaling factor for SSB-based and CSI-RS based L3 measurements performed within gaps 271

9.1.5.2.4 NR-DC: carrier-specific scaling factor for SSB-based and CSI-RS-based L3 measurements performed within gaps 273

9.1.5.2.5 SA mode: carrier-specific scaling factor for PRS-based measurements performed within gaps 275

9.1.5.2.6 NE-DC: carrier-specific scaling factor for PRS-based measurements performed within gaps 275

9.1.5.2.7 NR-DC: carrier-specific scaling factor for PRS-based measurements performed within gaps 275

9.1.6 Minimum requirement at transitions 275

9.2 NR intra-frequency measurements 276

9.2.1 Introduction 276

9.2.2 Requirements applicability 276

9.2.3 Number of cells and number of SSB 277

9.2.3.1 Requirements for FR1 277

9.2.3.2 Requirements for FR2 277

9.2.4 Measurement Reporting Requirements 277

9.2.4.1 Periodic Reporting 277

9.2.4.2 Event-triggered Periodic Reporting 277

9.2.4.3 Event Triggered Reporting 277

9.2.5 Intrafrequency measurements without measurement gaps 278

9.2.5.1 Intrafrequency cell identification 278

9.2.5.2 Measurement period 281

9.2.5.3 Scheduling availability of UE during intra-frequency measurements 282

9.2.5.3.1 Scheduling availability of UE performing measurements in TDD bands on FR1 283

9.2.5.3.2 Scheduling availability of UE performing measurements with a different subcarrier spacing than PDSCH/PDCCH on FR1 283

9.2.5.3.3 Scheduling availability of UE performing measurements on FR2 283

9.2.5.3.4 Scheduling availability of UE performing measurements on FR1 or FR2 in case of FR1-FR2 inter-band CA 284

9.2.5.4 SFTD Measurements between PCell and PSCell 285

9.2.5.4.1 Introduction 285

9.2.5.4.2 SFTD Measurement delay 285

9.2.5.4.3 SFTD Measurement Reporting Delay 285

9.2.6 Intra-frequency measurements with measurement gaps 286

9.2.6.1 Void 286

9.2.6.2 Intra-frequency cell identification 286

9.2.6.3 Intrafrequency Measurement Period 287

9.2A NR intra-frequency measurements with CCA 288

9.2A.1 Introduction 288

9.2A.2 Requirements applicability 289

9.2A.3 Number of cells and number of SSB 289

9.2A.4 Measurement Reporting Requirements 289

9.2A.5 Intra-frequency measurements without measurement gaps 290

9.2A.5.2 Measurement period 292

9.2A.5.3 Scheduling availability of UE during intra-frequency measurements 293

9.2A.5.3.1 Scheduling availability of UE performing measurements in TDD bands 293

9.2A.5.3.2 Scheduling availability of UE performing measurements with a different subcarrier spacing than PDSCH/PDCCH 294

9.2A.6 Intra-frequency measurements with measurement gaps 294

9.2A.6.1 Intra-frequency cell identification 294

9.2A.6.2 Intra-frequency Measurement Period 295

9.2A.7 Intra-frequency RSSI and Channel occupancy measurements 296

9.2A.7.1 Intra-frequency RSSI measurements 296

9.2A.7.2 Intra-frequency Channel occupancy measurements 297

9.2A.7.3 Scheduling restriction during RSSI and Channel Occupancy measurements 298

9.3 NR inter-frequency measurements 298

9.3.1 Introduction 298

9.3.2 Requirements applicability 299

9.3.2.1 Void 299

9.3.2.2 Void 299

9.3.3 Number of cells and number of SSB 299

9.3.3.1 Requirements for FR1 299

9.3.3.2 Requirements for FR2 299

9.3.4 Inter-frequency measurement with measurement gaps 300

9.3.4.1 Void 301

9.3.4.2 Void 301

9.3.5 Inter-frequency measurements 301

9.3.5.1 Void 302

9.3.5.2 Void 302

9.3.5.3 Void 302

9.3.6 Inter-frequency measurements reporting requirements 302

9.3.6.1 Periodic Reporting 302

9.3.6.2 Event-triggered Periodic Reporting 302

9.3.6.3 Event-triggered Reporting 302

9.3.7 Void 303

9.3.8 Inter-frequency SFTD measurement requirements 303

9.3.8.1 Introduction 303

9.3.8.2 SFTD Measurement delay 303

9.3.8.3 SFTD Measurement reporting delay 304

9.3.9 Inter frequency measurements without measurement gaps 304

9.3.9.1 Inter frequency Cell identification 304

9.3.9.2 Measurement period 306

9.3.9.3 Scheduling availability of UE during inter-frequency measurements 306

9.3.9.3.1 Scheduling availability of UE performing measurements in TDD bands on FR1 306

9.3.9.3.2 Scheduling availability of UE performing measurements with a different subcarrier spacing than PDSCH/PDCCH on FR1 307

9.3.9.3.3 Scheduling availability of UE performing measurements on FR2 307

9.3.9.3.4 Scheduling availability of UE performing measurements on FR1 or FR2 in case of FR1-FR2 inter-band CA 308

9.3A NR inter-frequency measurements in carrier frequencies with CCA 308

9.3A.1 Introduction 308

9.3A.2 Requirements applicability 308

9.3A.3 Number of cells and number of SSB 309

9.3A.3.1 Requirements 309

9.3A.4 Inter-frequency cell identification 309

9.3A.5 Inter-frequency measurements 310

9.3A.6 NR Inter-frequency measurements reporting requirements 311

9.3A.6.1 Periodic Reporting 311

9.3A.6.2 Event-triggered Periodic Reporting 311

9.3A.6.3 Event-triggered Reporting 311

9.3A.8 Inter-frequency RSSI measurements 311

9.3A.9 Inter-frequency channel occupancy measurements 312

9.4 Inter-RAT measurements 312

9.4.1 Introduction 312

9.4.2 NR − E-UTRAN FDD measurements 314

9.4.2.1 Introduction 314

9.4.2.2 Requirements when no DRX is used 314

9.4.2.3 Requirements when DRX is used 315

9.4.2.4 Measurement reporting requirements 316

9.4.2.4.1 Periodic Reporting 316

9.4.2.4.2 Event-Triggered Periodic Reporting 316

9.4.2.4.3 Event-Triggered Reporting 316

9.4.3 NR − E-UTRAN TDD measurements 316

9.4.3.1 Introduction 316

9.4.3.2 Requirements when no DRX is used 316

9.4.3.3 Requirements when DRX is used 317

9.4.3.4 Measurement reporting requirements 319

9.4.3.4.1 Periodic Reporting 319

9.4.3.4.2 Event-Triggered Periodic Reporting 319

9.4.3.4.3 Event-Triggered Reporting 319

9.4.4 Inter-RAT RSTD measurements 319

9.4.4.1 NR − E-UTRAN FDD RSTD measurements 319

9.4.4.1.1 Introduction 319

9.4.4.1.2 Requirements 320

9.4.4.2 NR − E-UTRAN TDD RSTD measurements 323

9.4.4.2.1 Introduction 323

9.4.4.2.2 Requirements 324

9.4.5 Inter-RAT E-CID measurements 327

9.4.5.1 NR−E-UTRAN FDD E-CID RSRP and RSRQ measurements 327

9.4.5.1.1 Introduction 327

9.4.5.1.2 Requirements 327

9.4.5.1.3 Measurement Reporting Delay 327

9.4.5.2 NR−E-UTRAN TDD E-CID RSRP and RSRQ measurements 327

9.4.5.2.1 Introduction 327

9.4.5.2.2 Requirements 327

9.4.5.2.3 Measurement Reporting Delay 328

9.4.6 NR − UTRAN FDD measurements 328

9.4.6.1 Introduction 328

9.4.6.2 Requirements when no DRX is used 328

9.4.6.3 Requirements when DRX is used 329

9.4.7 NR – E-UTRAN measurements with autonomous gaps 331

9.4.7.1 CGI identification of an E-UTRA cell with autonomous gaps 331

9.4.7.2 CGI reporting delay 331

9.5 L1-RSRP measurements for Reporting 332

9.5.1 Introduction 332

9.5.2 Requirements applicability 332

9.5.3 Measurement Reporting Requirements 332

9.5.3.1 Periodic Reporting 333

9.5.3.2 Semi-Persistent Reporting 333

9.5.3.3 Aperiodic Reporting 333

9.5.4 L1-RSRP measurement requirements 333

9.5.4.1 SSB based L1-RSRP Reporting 333

9.5.4.2 CSI-RS based L1-RSRP Reporting 335

9.5.4A Void 338

9.5.4A.1 Void 338

9.5.5 Measurement restriction for CSI-RS and SSB for L1-RSRP measurement 338

9.5.5.1 Measurement restriction for SSB based L1-RSRP 338

9.5.5.2 Measurement restriction for CSI-RS based L1-RSRP 338

9.5.6 Scheduling availability of UE during L1-RSRP measurement 339

9.5.6.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH on FR1 339

9.5.6.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH on FR1 339

9.5.6.3 Scheduling availability of UE performing L1-RSRP measurement on FR2 340

9.5.6.4 Scheduling availability of UE performing L1-RSRP measurement on FR1 or FR2 in case of FR1-FR2 inter-band CA 340

9.5A L1-RSRP measurements for Reporting under CCA 341

9.5A.1 Introduction 341

9.5A.2 Requirements applicability 341

9.5A.3 Measurement Reporting Requirements 341

9.5A.3.1 Periodic Reporting 341

9.5A.3.2 Semi-Persistent Reporting 342

9.5A.3.3 Aperiodic Reporting 342

9.5A.4 L1-RSRP measurement requirements 342

9.5A.4.1 SSB based L1-RSRP Reporting 342

9.5A.5 Measurement restriction for L1-RSRP measurement 343

9.5A.5.1 Measurement restriction for SSB based L1-RSRP 343

9.5A.6 Scheduling availability of UE during L1-RSRP measurement 343

9.5A.6.1 Scheduling availability of UE performing L1-RSRP measurement with a same subcarrier spacing as PDSCH/PDCCH 343

9.5A.6.2 Scheduling availability of UE performing L1-RSRP measurement with a different subcarrier spacing than PDSCH/PDCCH 344

9.5A.6.3 Scheduling availability of UE performing L1-RSRP measurement in case of FR1-FR2 inter-band CA 344

9.6 NE-DC: Measurements 344

9.6.1 Introduction 344

9.6.2 SFTD Measurements 344

9.6.2.1 Introduction 344

9.6.2.2 SFTD Measurement requirements 344

9.7 Cross Link Interference measurements 345

9.7.1 Introduction 345

9.7.2 SRS-RSRP measurements 345

9.7.2.1 Introduction 345

9.7.2.2 Requirements applicability 345

9.7.2.3 Measurement Reporting Requirements 346

9.7.2.3.1 Periodic Reporting 346

9.7.2.3.2 Event-triggered Periodic Reporting 346

9.7.2.3.3 Event Triggered Reporting 346

9.7.2.4 Measurement capability 346

9.7.2.5 SRS-RSRP measurement period 346

9.7.3 CLI-RSSI measurements 347

9.7.3.1 Introduction 347

9.7.3.2 Requirements applicability 347

9.7.3.3 Measurement Reporting Requirements 347

9.7.3.3.1 Periodic Reporting 347

9.7.3.3.2 Event-triggered Periodic Reporting 347

9.7.3.3.3 Event Triggered Reporting 347

9.7.3.4 Measurement capability 348

9.7.3.5 CLI-RSSI measurement period 348

9.7.4 Scheduling availability of UE during CLI measurements 348

9.7.4.1 Scheduling availability of UE performing measurement on FR1 348

9.7.4.2 Scheduling availability of UE performing measurement on FR2 348

9.8 L1-SINR measurements for Reporting 349

9.8.1 Introduction 349

9.8.2 Requirements applicability 349

9.8.3 Measurement Reporting Requirements 350

9.8.3.1 Periodic Reporting 350

9.8.3.2 Semi-Persistent Reporting 350

9.8.3.3 Aperiodic Reporting 351

9.8.4 L1-SINR measurement requirements 351

9.8.4.1 L1-SINR reporting with CSI-RS based CMR and no dedicated IMR configured 351

9.8.4.3 L1-SINR reporting with CSI-RS based CMR and dedicated IMR configured 354

9.8.5 Measurement restriction for L1-SINR measurement 356

9.8.5.1 Measurement restriction if SSB configured for L1-SINR Measurement 356

9.8.5.2 Measurement restriction if CSI-RS configured for L1-SINR measurement 357

9.8.5.3 Measurement restriction if CSI-IM configured for L1-SINR measurement 357

9.8.6 Scheduling availability of UE during L1-SINR measurement 358

9.8.6.1 Scheduling availability of UE performing L1-SINR measurement with a same subcarrier spacing as PDSCH/PDCCH on FR1 358

9.8.6.2 Scheduling availability of UE performing L1-SINR measurement with a different subcarrier spacing than PDSCH/PDCCH on FR1 358

9.8.6.4 Scheduling availability of UE performing L1-SINR measurement on FR1 or FR2 in case of FR1-FR2 inter-band CA 359

9.9 NR measurements for positioning 359

9.9.1 Introduction 359

9.9.2 RSTD measurements 360

9.9.2.1 Introduction 360

9.9.2.2 Requirements Applicability 360

9.9.2.3 Measurement Capability 360

9.9.2.4 Measurement Reporting Requirements 360

9.9.2.4.1 Void 360

9.9.2.4.2 Void 360

9.9.2.4.3 Void 360

9.9.2.5 Measurements Period Requirements 360

9.9.2.6 Void 362

9.9.3 PRS-RSRP measurements 362

9.9.3.1 Introduction 362

9.9.3.2 Requirements applicability 362

9.9.3.3 Measurement Capability 362

9.9.3.4 Measurement Reporting Requirements 363

9.9.3.5 Measurement Period Requirements 363

9.9.4 UE Rx-Tx time difference measurements 365

9.9.4.1 Introduction 365

9.9.4.2 Requirements Applicability 365

9.9.4.3 Measurement Capability 365

9.9.4.4 Measurement Reporting Requirements 365

9.9.4.5 Measurement Period Requirements 365

9.9.5 NR E-CID measurements 368

9.9.5.1 Introduction 368

9.9.5.2 Measurement Requirements 368

9.9.5.2.1 Intra-frequency Measurement Requirements 368

9.9.5.2.2 Inter-frequency Measurement Requirements 368

9.9.5.2.3 Measurement Reporting Delay 369

9.10 CSI-RS based L3 measurements 369

9.10.1 Introduction 369

9.10.2 CSI-RS based intra-frequency measurements 369

9.10.2.1 Introduction 369

9.10.2.2 Requirements applicability 370

9.10.2.3 Number of cells and number of CSI-RS 371

9.10.2.3.1 Requirements for FR1 371

9.10.2.3.2 Requirements for FR2 371

9.10.2.4 Measurement Reporting Requirements 371

9.10.2.4.1 Periodic Reporting 371

9.10.2.4.2 Event-triggered Periodic Reporting 372

9.10.2.4.3 Event Triggered Reporting 372

9.10.2.5 Intra-frequency measurements without measurement gaps 372

9.10.2.6 Scheduling availability of UE during CSI-RS based intra-frequency measurements 373

9.10.2.6.1 Scheduling availability of UE performing CSI-RS based measurements in TDD bands 373

9.10.2.6.2 Scheduling availability of UE performing CSI-RS based measurements in FR2 374

9.10.3 CSI-RS based Inter-frequency measurements 374

9.10.3.1 Introduction 374

9.10.3.2 Requirements applicability 374

9.10.3.3 Number of cells and number of CSI-RS resources 375

9.10.3.3.1 Requirements for FR1 375

9.10.3.3.2 Requirements for FR2 375

9.10.3.4 Measurements reporting requirements 375

9.10.3.4.1 Periodic Reporting 375

9.10.3.4.2 Event-triggered Periodic Reporting 375

9.10.3.4.3 Event-triggered Reporting 376

9.10.3.5 Inter frequency measurements with measurement gaps 376

9.11 NR measurements with autonomous gaps 377

9.11.1 Introduction 377

9.11.2 CGI identification of an NR cell with autonomous gaps 377

9.11.3 CGI reporting delay 378

10 Measurement Performance requirements 378

10.1 NR measurements 378

10.1.1 Introduction 378

10.1.2 Intra-frequency RSRP accuracy requirements for FR1 379

10.1.2.1 Intra-frequency SS-RSRP accuracy requirements 379

10.1.2.1.1 Absolute SS-RSRP Accuracy 379

10.1.2.1.2 Relative SS-RSRP Accuracy 380

10.1.2.2 Void 381

10.1.2.3 Intra-frequency CSI-RSRP accuracy requirements 381

10.1.2.3.1 Absolute CSI-RSRP Accuracy 381

10.1.2.3.2 Relative CSI-RSRP Accuracy 382

10.1.2B Intra-frequency RSRP accuracy requirements for FR1 for CA/DC Idle Mode Measurements 383

10.1.2B.1 Intra-frequency SS-RSRP accuracy requirements 383

10.1.2B.1.1 Absolute SS-RSRP Accuracy 383

10.1.3 Intra-frequency RSRP accuracy requirements for FR2 384

10.1.3.1 Intra-frequency SS-RSRP accuracy requirements 384

10.1.3.1.1 Absolute SS-RSRP Accuracy 384

10.1.3.1.2 Relative SS-RSRP Accuracy 385

10.1.3.2 Void 386

10.1.3.3 Intra-frequency CSI-RSRP accuracy requirements 386

10.1.3.3.1 Absolute CSI-RSRP Accuracy 386

10.1.3.3.2 Relative CSI-RSRP Accuracy 386

10.1.3B Intra-frequency RSRP accuracy requirements for FR2 for CA/DC Idle Mode Measurements 387

10.1.3B.1 Intra-frequency SS-RSRP accuracy requirements 387

10.1.3B.1.1 Absolute SS-RSRP Accuracy 388

10.1.4 Inter-frequency RSRP accuracy requirements for FR1 388

10.1.4.1 Inter-frequency SS-RSRP accuracy requirements 388

10.1.4.1.1 Absolute Accuracy of SS-RSRP in FR1 388

10.1.4.1.2 Relative Accuracy of SS-RSRP in FR1 389

10.1.4.2 Void 390

10.1.4.3 Inter-frequency CSI-RSRP accuracy requirements 390

10.1.4.3.1 Absolute Accuracy of CSI-RSRP in FR1 390

10.1.4.3.2 Relative Accuracy of CS-RSRP in FR1 391

10.1.4B Inter-frequency RSRP accuracy requirements for FR1 for CA/DC Idle Mode Measurements 392

10.1.4B.1 Inter-frequency SS-RSRP accuracy requirements 392

10.1.4B.1.1 Absolute Accuracy of SS-RSRP in FR1 392

10.1.5 Inter-frequency RSRP accuracy requirements for FR2 393

10.1.5.1 Inter-frequency SS-RSRP accuracy requirements 393

10.1.5.1.1 Absolute SS-RSRP Accuracy 393

10.1.5.1.2 Relative SS-RSRP Accuracy 394

10.1.5.2 Void 395

10.1.5.3 Inter-frequency CSI-RSRP accuracy requirements 395

10.1.5.3.1 Absolute CSI-RSRP Accuracy 395

10.1.5.3.2 Relative CSI-RSRP Accuracy 395

10.1.5B Inter-frequency RSRP accuracy requirements for FR2 for CA/DC Idle Mode Measurements 396

10.1.6 RSRP Measurement Report Mapping 397

10.1.7 Intra-frequency RSRQ accuracy requirements for FR1 399

10.1.7.1 Intra-frequency SS-RSRQ accuracy requirements in FR1 399

10.1.7.1.1 Absolute SS-RSRQ Accuracy in FR1 399

10.1.7.2 Intra-frequency CSI-RSRQ accuracy requirements 400

10.1.7.2.1 Absolute CSI-RSRQ Accuracy 400

10.1.7B Intra-frequency RSRQ accuracy requirements for FR1 for CA/DC Idle Mode Measurements 401

10.1.7B.1 Intra-frequency SS-RSRQ accuracy requirements in FR1 401

10.1.7B.1.1 Absolute SS-RSRQ Accuracy in FR1 401

10.1.8 Intra-frequency RSRQ accuracy requirements for FR2 402

10.1.8.1 Intra-frequency SS-RSRQ accuracy requirements in FR2 402

10.1.8.1.1 Absolute SS-RSRQ Accuracy in FR2 402

10.1.8.2 Intra-frequency CSI-RSRQ accuracy requirements 403

10.1.8.2.1 Absolute CSI-RSRQ Accuracy 403

10.1.8B Intra-frequency RSRQ accuracy requirements for FR2 for CA/DC Idle Mode Measurements 404

10.1.8B.1 Intra-frequency SS-RSRQ accuracy requirements in FR2 404

10.1.8B.1.1 Absolute SS-RSRQ Accuracy in FR2 404

10.1.9 Inter-frequency RSRQ accuracy requirements for FR1 405

10.1.9.1 Inter-frequency SS-RSRQ accuracy requirements in FR1 405

10.1.9.1.1 Absolute Accuracy of SS-RSRQ in FR1 405

10.1.9.1.2 Relative Accuracy of SS-RSRQ in FR1 406

10.1.9.2 Inter-frequency CSI-RSRQ accuracy requirements 407

10.1.9.2.1 Absolute CSI-RSRQ Accuracy 407

10.1.9.2.2 Relative CSI-RSRQ Accuracy 408

10.1.9B Inter-frequency RSRQ accuracy requirements for FR1 for CA/DC Idle Mode Measurements 409

10.1.9B.1 Inter-frequency SS-RSRQ accuracy requirements in FR1 409

10.1.9B.1.1 Absolute Accuracy of SS-RSRQ in FR1 409

10.1.10 Inter-frequency RSRQ accuracy requirements for FR2 410

10.1.10.2 Inter-frequency CSI-RSRQ accuracy requirements 412

10.1.10.2.1 Absolute CSI-RSRQ Accuracy 412

10.1.10.2.2 Relative CSI-RSRQ Accuracy 412

10.1.10B Inter-frequency RSRQ accuracy requirements for FR2 for CA/DC Idle Mode Measurements 413

10.1.10B.1 Inter-frequency SS-RSRQ accuracy requirements in FR2 413

10.1.10B.1.1 Absolute Accuracy of SS-RSRQ in FR2 413

10.1.11 RSRQ report mapping 414

10.1.12 Intra-frequency SINR accuracy requirements for FR1 415

10.1.12.2 Intra-frequency CSI-SINR accuracy requirements in FR1 415

10.1.12.2.1 Absolute CSI-SINR Accuracy in FR1 415

10.1.13 Intra-frequency SINR accuracy requirements for FR2 416

10.1.13.2 Intra-frequency CSI-SINR accuracy requirements in FR2 417

10.1.13.2.1 Absolute CSI-SINR Accuracy in FR2 417

10.1.14 Inter-frequency SINR accuracy requirements for FR1 418

10.1.14.2 Inter-frequency CSI-SINR accuracy requirements in FR1 420

10.1.14.2.1 Aboslute Accuracy of CSI-SINR in FR1 420

10.1.15 Inter-frequency SINR accuracy requirements for FR2 422

10.1.15.2 Inter-frequency CSI-SINR accuracy requirements in FR2 424

10.1.15.2.1 Aboslute Accuracy of CSI-SINR in FR2 424

10.1.15.2.2 Relative Accuracy of CSI-SINR in FR2 424

10.1.16 SINR report mapping 425

10.1.17 Power Headroom 426

10.1.18 PCMAX,c,f 427

10.1.19 L1-RSRP accuracy requirements for FR1 427

10.1.20 L1-RSRP accuracy requirements for FR2 431

10.1.21 SFTD accuracy requirements 434

10.1.22 CLI measurement accuracy requirements 438

10.1.24.3.1 Absolute PRS-RSRP Measurement Report Mapping 442

10.1.24.3.2 Differential Report Mapping for PRS-RSRP Measurement 442

10.1.23 RSTD Measurements 444

10.1.23.1 Introduction 444

10.1.23.2 Measurement Accuracy Requirements 445

10.1.23.3 Report mapping 450

10.1.23.3.1 Absolute DL RSTD Measurement Reporting 450

10.1.23.3.2 Differential Reporting for DL RSTD Measurement 452

10.1.23.3.3 Additional Path Report Mapping for DL RSTD 454

10.1.24 PRS-RSRP Measurements 456

10.1.24.1 Introduction 456

10.1.24.2 Measurement Accuracy Requirements 456

10.1.24.2.1 Absolute PRS RSRP accuracy 456

10.1.24.3 Report mapping 460

10.1.24.3.1 Absolute PRS-RSRP Measurement Report Mapping 460

10.1.24.3.2 Differential Report Mapping for PRS-RSRP Measurement 461

10.1.25 UE Rx-Tx Time Difference Measurements 463

10.1.25.1 Introduction 463

10.1.25.2 Measurement Accuracy Requirements 464

10.1.25.3 Report mapping 470

10.1.25.3.1 Absolute UE Rx-Tx Measurement Report Mapping 470

10.1.25.3.2 Differential UE Rx-Tx Measurement Report Mapping 472

10.1.25.3.3 Additional Path Report Mapping for UE Rx-Tx Time Difference 473

10.1.26 FR2 P-MPR report 475

10.1.26.1 Report mapping 475

10.1.27 L1-SINR accuracy requirements for FR1 475

10.1.27.1 L1-SINR accuracy requirements with CSI-RS based CMR and no dedicated IMR configured 475

10.1.27.1.1 Absolute Accuracy 475

10.1.27.1.2 Relative Accuracy 476

10.1.27.2 L1-SINR accuracy requirements with SSB based CMR and dedicated IMR configured 477

10.1.27.2.1 Absolute Accuracy 477

10.1.27.2.2 Relative Accuracy 478

10.1.27.3 L1-SINR accuracy requirements with CSI-RS based CMR and dedicated IMR configured 480

10.1.27.3.1 Absolute Accuracy 480

10.1.27.3.2 Relative Accuracy 482

10.1.28 L1-SINR accuracy requirements for FR2 483

10.1.28.1 L1-SINR accuracy requirements with CSI-RS based CMR and no dedicated IMR configured 483

10.1.28.1.1 Absolute Accuracy 483

10.1.28.1.2 Relative Accuracy 484

10.1.28.2 L1-SINR accuracy requirements with SSB based CMR and dedicated IMR configured 485

10.1.28.2.1 Absolute Accuracy 485

10.1.28.2.2 Relative Accuracy 486

10.1.28.3 L1-SINR accuracy requirements with CSI-RS based CMR and dedicated IMR configured 487

10.1.28.3.1 Absolute Accuracy 487

10.1.28.3.2 Relative Accuracy 488

10.1.29 Intra-frequency RSRQ accuracy requirements under CCA 490

10.1.29.1 Intra-frequency SS-RSRQ accuracy requirements in FR1 490

10.1.29.1.1 Absolute SS-RSRQ Accuracy 490

10.1.30 Inter-frequency RSRQ accuracy requirements under CCA 490

10.1.30.1 Inter-frequency SS-RSRQ accuracy requirements in FR1 490

10.1.30.1.1 Aboslute Accuracy of SS-RSRQ 490

10.1.30.1.2 Relative Accuracy of SS-RSRQ 491

10.1.31 Intra-frequency SINR accuracy requirements under CCA 492

10.1.32 Inter-frequency SINR accuracy requirements under CCA 492

10.1.33 L1-RSRP accuracy requirements under CCA 494

10.1.34 RSSI measurements under CCA 495

10.1.34.1 Intra-frequency absolute RSSI measurement accuracy requirements in FR1 495

10.1.34.2 Inter-frequency absolute RSSI measurement accuracy requirements in FR1 495

10.1.34.3 RSSI measurement report mapping 496

10.1.35 Channel occupancy measurements under CCA 496

10.1.35.1 Intra-frequency channel occupancy measurement accuracy requirements in FR1 496

10.1.35.2 Inter-frequency channel occupancy measurement accuracy requirements in FR1 496

10.1.36 Intra-frequency RSRP accuracy requirements under CCA 497

10.1.36.1 Intra-frequency SS-RSRP accuracy requirements in FR1 497

10.1.36.1.1 Absolute SS-RSRP Accuracy 497

10.1.36.1.2 Relative SS-RSRP Accuracy 497

10.1.37 Inter-frequency RSRP accuracy requirements under CCA 498

10.1.37.1 Inter-frequency SS-RSRP accuracy requirements in FR1 498

10.1.37.1.1 Absolute Accuracy of SS-RSRP 498

10.1.37.1.2 Relative Accuracy of SS-RSRP 499

10.2 E-UTRAN measurements 499

10.2.1 Introduction 499

10.2.2 E-UTRAN RSRP measurements 500

10.2.3 E-UTRAN RSRQ measurements 500

10.2.4 E-UTRAN RSTD measurements 500

10.2.5 E-UTRAN RS-SINR measurements 500

10.2.6 E-UTRAN RSRP measurements for CA/DC Idle Mode Measurements 500

10.2.7 E-UTRAN RSRQ measurements for CA/DC Idle Mode Measurements 501

10.3 UTRAN FDD Measurements 501

10.3.1 UTRAN FDD CPICH RSCP 501

10.3.2 UTRAN FDD CPICH Ec/No 502

10.4 V2X measurements 502

10.4.1 Introduction 502

10.4.2 Intra-frequency PSBCH-RSRP accuracy requirements for FR1 503

10.4.2.1 PSBCH-RSRP Absolute Accuracy 503

10.4.2.2 PSBCH-RSRP Relative Accuracy 503

10.4.3 Intra-Frequency SL-RSSI Measurement Accuracy Requirements for FR1 504

10.4.3.1 Absolute SL-RSSI Accuracy 504

10.4.4 Intra-Frequency L1 SL-RSRP Measurement Accuracy Requirements for FR1 504

10.4.4.1 Absolute L1 SL-RSRP Accuracy 504

11 Void 505

12 V2X Requirements 505

12.1 Introduction 505

12.2 UE Transmit Timing 506

12.2.1 Introduction 506

12.2.2 GNSS as synchronization reference source 506

12.2.3 NR Cell as synchronization reference source 506

12.2.4 E-URTAN Cell as synchronization reference source 507

12.2.5 SyncRef UE as synchronization reference source 507

12.3 Initiation/Cease of SLSS Transmissions 507

12.3.1 Introduction 507

12.3.1.1 Initiation/Cease of SLSS transmissions with NR cell as synchronization reference source 507

12.3.1.2 Initiation/Cease of SLSS transmissions with EUTRAN cell as synchronization reference source 508

12.3.1.3 Initiation/Cease of SLSS transmissions with GNSS as synchronization reference source 509

12.3.1.4 Initiation/Cease of SLSS transmissions with SyncRef UE as synchronization reference source 509

12.4 Selection / Reselection of V2X Synchronization Reference Source 510

12.5 L1 SL-RSRP measurements 511

12.5.1 Introduction 511

12.5.2 SL-RSRP measurements 511

12.6 Congestion Control measurements 511

12.7 Interruption 511

12.7.1 Interruptions to WAN due to V2X Sidelink Communication 511

12.7.2 V2X Sidelink Communication Dropping due to synchronization source change 512

12.7.3 Interruptions to WAN due to switching between E-UTRA V2X Sidelink and NR V2X Sidelink 514

12.8 Reliability of GNSS signal 514

12.9 Scheduling availability 514

12.9.1 Scheduling availability of UE switching between E-UTRA sidelink and NR sidelink 514

13 Measurement Performance Requirements for NR gNB 515

13.1 UL-RTOA 515

13.1.1 Report mapping 515

13.2 gNB Rx-Tx time difference 517

13.2.1 Report mapping 517

13.2.2 Measurement Accuracy Requirements 519

13.2.2.1 Introduction 519

13.2.2.2 Requirements 519

13.3 UL SRS RSRP measurement 520

13.3.1 Report mapping 520

13.3.2 Measurement accuracy requirements 521

13.3.2.1 Introduction 521

13.3.2.2 Requirements 521

13.4 AoA/ZoA 522

13.4.1 Report mapping 522

Annex A (normative): Test Cases 423

A.1 Purpose of annex 423

A.2 Requirement classification for statistical testing 423

A.2.1 Types of requirements in TS 38.133 423

A.2.1.1 Time and delay requirements on UE higher layer actions 423

A.2.1.2 Measurements of power levels, relative powers and time 423

A.2.1.3 Implementation requirements 424

A.2.1.4 Physical layer timing requirements 424

A.2.1.5 Requirements under CCA 424

A.3 RRM test configurations 425

A.3.1 Reference measurement channels 425

A.3.1.1 PDSCH 425

A.3.1.1.1 FDD 425

A.3.1.1.2 TDD 426

A.3.1A Reference measurement channels under CCA 429

A.3.1A.1 PDSCH 429

A.3.1A.1.1 TDD 429

A.3.1A.2 CORESET for RMSI scheduling 430

A.3.1A.2.1 TDD 430

A.3.1A.3 CORESET for RMC scheduling 431

A.3.1A.3.1 TDD 431

A.3.1A.4 TDD UL/DL configuration 432

A.3.1A.5 RMC burst transmission model 432

A.3.1.2 CORESET for RMSI scheduling 433

A.3.1.2.1 FDD 433

A.3.1.2.2 TDD 434

A.3.1.3 CORESET for RMC scheduling 437

A.3.1.3.1 FDD 437

A.3.1.3.2 TDD 438

A.3.1.4 TDD UL/DL configuration 441

A.3.2 OFDMA channel noise generator (OCNG) 442

A.3.2.1 Generic OFDMA Channel Noise Generator (OCNG) 442

A.3.2.1.1 OCNG pattern 1: Generic OCNG pattern for all unused REs 442

A.3.2.1.2 OCNG pattern 2: Generic OCNG pattern for all unused REs for 2AoA setup 443

A.3.2.1.3 OCNG pattern 3: Generic OCNG pattern for unused REs in the same bandwidth as CORESET 443

A.3.2.1.4 OCNG pattern 4: Generic OCNG pattern for all unused REs outside SSB slot(s) 444

A.3.2.2 Void 445

A.3.3 Reference DRX configurations 445

A.3.3.1 DRX Configuration 1: DRX cycle = 40 ms and TAT = 500 ms 445

A.3.3.2 DRX Configuration 2: DRX cycle = 640 ms and TAT = 500 ms 445

A.3.3.3 DRX Configuration 3: DRX cycle = 40 ms and TAT = Infinity 445

A.3.3.4 DRX Configuration 4: DRX cycle = 160 ms and TAT = Infinity 446

A.3.3.5 DRX Configuration 5: DRX cycle = 320 ms and TAT = Infinity 446

A.3.3.6 DRX Configuration 6: DRX cycle = 320 ms and TAT = 500 ms 446

A.3.3.7 DRX Configuration 7: DRX cycle = 640 ms and TAT = Infinity 447

A.3.3.8 DRX Configuration 8: DRX cycle = 320 ms and TAT = Infinity 447

A.3.3.9 DRX Configuration 9: DRX cycle = 40 ms and TAT = 500 ms 447

A.3.3.10 DRX Configuration 10: DRX cycle = 640 ms and TAT = 500 ms 448

A.3.3.11 DRX Configuration 11: DRX cycle = 20 ms and TAT = Infinity 448

A.3.3.12 DRX Configuration 12: DRX cycle = 640 ms and TAT = Infinity 448

A.3.4 Test Cases with Different Channel Bandwidths 448

A.3.4.1 Test Cases with Different E-UTRA Channel Bandwidths 448

A.3.4.1.1 Introduction 448

A.3.4.1.2 Principle of testing 449

A.3.5 Test Cases for Synchronous and Asynchronous DC Operations 449

A.3.5.1 EN-DC Test Cases for Synchronous and Asynchronous EN-DC Operations 449

A.3.5.1.1 Introduction 449

A.3.5.1.2 Principle of Testing 449

A.3.6 Antenna configurations 449

A.3.6.1 Antenna configurations for FR1 449

A.3.6.1.1 Antenna connection for 4 Rx capable UEs 449

A.3.6.1.1.1 Introduction 449

A.3.6.1.1.2 Principle of testing 449

A.3.6.2 Antenna configurations for FR2 452

A.3.6A Antenna configurations with unlicensed bands 452

A.3.6A.1 Antenna configurations for FR1 452

A.3.6A.1.1 Antenna connection for 4 Rx capable UEs 452

A.3.6A.1.1.1 Introduction 452

A.3.6A.1.1.2 Principle of testing 452

A.3.7 EN-DC test setup 454

A.3.7.1 Introduction 454

A.3.7.2 E-UTRAN Serving Cell Parameters 454

A.3.7.2.1 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR1 454

A.3.7.2.2 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR2 455

A.3.7A NR FR1-FR2 test setup 456

A.3.7B EN-DC test setup with unlicensed bands 457

A.3.7B.1 Introduction 457

A.3.7B.2 E-UTRAN Serving Cell Parameters 457

A.3.7B.2.1 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) under CCA in FR1 457

A.3.7C LTE-FR1/FR2 test setup 458

A.3.7D NE-DC test setup 458

A.3.7D.1 Introduction 458

A.3.7D.2 E-UTRAN Serving Cell Parameters 458

A.3.7D.2.1 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR1 458

A.3.7D.2.2 E-UTRAN Serving Cell Parameters for Tests with NR Cell(s) in FR2 458

A.3.8 PRACH configurations 458

A.3.8.1 Introduction 458

A.3.8.2 PRACH configurations in FR1 459

A.3.8.2.1 FR1 PRACH configuration 1 459

A.3.8.2.2 FR1 PRACH configuration 2 459

A.3.8.2.3 FR1 PRACH configuration 3 460

A.3.8.2.4 FR1 PRACH configuration 4 461

A.3.8.3 PRACH configurations in FR2 462

A.3.8.3.1 FR2 PRACH configuration 1 462

A.3.8.3.2 FR2 PRACH configuration 2 463

A.3.8.3.3 FR2 PRACH configuration 3 464

A.3.8.3.4 FR2 PRACH configuration 4 465

A.3.8A PRACH configurations under CCA 466

A.3.8A.1 Introduction 466

A.3.8A.2 PRACH configurations in FR1 466

A.3.8A.2.1 FR1 PRACH configuration 1 under CCA 466

A.3.8A.2.2 FR1 PRACH configuration 2 under CCA 467

A.3.9 BWP configurations 468

A.3.9.1 Introduction 468

A.3.9.2 Downlink BWP configurations 469

A.3.9.2.1 Initial BWP 469

A.3.9.2.2 Dedicated BWP 469

A.3.9.3 Uplink BWP configurations 469

A.3.9.3.1 Initial BWP 469

A.3.9.3.2 Dedicated BWP 470

A.3.10 SSB Configurations 470

A.3.10.1 SSB Configurations for FR1 470

A.3.10.1.1 SSB pattern 1 in FR1: SSB allocation for SSB SCS=15 kHz in 10 MHz 470

A.3.10.1.5 SSB pattern 5 in FR1: SSB allocation for SSB SCS=15 kHz starting from odd SFN in 10 MHz 472

A.3.10A SSB Configurations under CCA 477

A.3.10A.1 SSB Configurations under CCA for FR1 477

A.3.10A.1.1 SSB pattern 1 under CCA for semi-static channel access: SSB allocation for SSB SCS=30kHz in 40MHz 477

A.3.10A.1.2 SSB pattern 2 under CCA for dynamic channel access: SSB allocation for SSB SCS=30kHz in 40MHz 478

A.3.10A.1.3 SSB pattern 3 under CCA for semi-static channel access: SSB allocation for SSB SCS=30 kHz in 40 MHz 478

A.3.10A.1.4 SSB pattern 4 under CCA for dynamic channel access: SSB allocation for SSB SCS=30 kHz in 40 MHz 479

A.3.11 SMTC Configurations 479

A.3.11.1 SMTC pattern 1: SMTC period = 20 ms with SMTC duration = 1 ms 479

A.3.11.2 SMTC pattern 2: SMTC period = 20 ms with SMTC duration = 5 ms 479

A.3.11.3 SMTC pattern 3: SMTC period = 160 ms with SMTC duration = 1 ms 480

A.3.11.4 SMTC pattern 4: SMTC period = 20 ms with SMTC duration = 1 ms 480

A.3.11.5 SMTC pattern 5: SMTC period = 20 ms with SMTC duration = 5 ms 480

A.3.11.6 SMTC pattern 6: SMTC period = 20 ms with SMTC duration = 5 ms 480

A.3.12 Test Cases with Different CC Configurations 480

A.3.12.1 EN-DC Test Cases with Different EN-DC Configurations 480

A.3.12.1.1 Introduction 480

A.3.12.1.2 Principle of testing 481

A.3.12.2 Carrier Aggregation Test Cases with Different CA Configurations 481

A.3.12.2.1 Introduction 481

A.3.12.2.2 Principle of testing 481

A.3.13 Test Cases in SA and EN-DC Operations 481

A.3.13.1 Introduction 481

A.3.13.2 Principle of Testing 481

A.3.13A Test Cases involving E-UTRA/FR1 and FR2 carriers 482

A.3.13A.1 Introduction 482

A.3.13A.2 Principle of Testing in EN-DC 482

A.3.13A.3 Principle of Testing in SA 482

A.3.13B Test Cases for EN-DC and NE-DC Operations 483

A.3.13B.1 Active BWP switch Test Cases for EN-DC and NE-DC Operations 483

A.3.13B.1.1 Introduction 483

A.3.13B.1.2 Principle of Testing 483

A.3.13B.2 SFTD accuracy Test Cases for EN-DC and NE-DC Operations 483

A.3.13B.2.1 Introduction 483

A.3.13B.2.2 Principle of Testing 483

A.3.14 CSI-RS configurations 484

A.3.14.1 FDD 484

A.3.14.2 TDD 486

A.3.15 Angle of Arrival (AoA) for FR2 RRM test cases 491

A.3.15.1 Setup 1: Single AoA in Rx beam peak direction 491

A.3.15.2 Setup 2: Single AoA in non Rx beam peak direction 491

A.3.15.2.1 Setup 2a: Single AoA in non Rx beam peak direction without change in direction 491

A.3.15.2.2 Setup 2b: Single AoA in non Rx beam peak direction with change in direction 492

A.3.15.3 Setup 3: 2 AoAs 492

A.3.15.4 Setup 4: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak 492

A.3.15.4.1 Setup 4a: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak without change in direction 492

A.3.15.4.2 Setup 4b: 2 AoAs, 1 AoA in Rx beam peak direction, 1 in non Rx beam peak with change in direction 492

A.3.16 TCI State Configuration 493

A.3.16.1 Introduction 493

A.3.16.2 TCI states 493

A.3.17 Configurations of CSI-RS for tracking 493

A.3.17.1 Configuration of CSI-RS for tracking for FR1 493

A.3.17.1.1 FDD 493

A.3.17.1.2 TDD 494

A.3.17.2 Configuration of CSI-RS for tracking for FR2 495

A.3.17.2.1 TDD 495

A.3.18 Additional definitions related to OTA testing for FR2 RRM test cases 496

A.3.18.1 Introduction 496

A.3.18.2 PRACH Power Measurement 496

A.3.19 Test applicability for DAPS handover 496

A.3.19.1 Introduction 496

A.3.19.2 Principle of testing 496

A.3.20 MsgA configurations 497

A.3.20.1 Introduction 497

A.3.20.2 MsgA configurations in FR1 497

A.3.20.2.1 FR1 MsgA configuration 1 497

A.3.20.2.2 FR1 MsgA configuration 2 498

A.3.20.3 MsgA configurations in FR2 500

A.3.20.3.1 FR2 MsgA configuration 1 500

A.3.20.3.2 FR2 MsgA configuration 2 501

A.3.20A MsgA configurations under CCA 503

A.3.20A.1 Introduction 503

A.3.20A.2 MsgA configurations in FR1 503

A.3.20A.2.1 FR1 MsgA configuration 1 under CCA 503

A.3.20A.2.2 FR1 MsgA configuration 2 under CCA 504

A.3.21 V2X sidelink communication 507

A.3.21.1 Introduction 507

A.3.21.2 Reference resource pool configurations for V2X Sidelink Communication 507

A.3.21.3 Reference measurement channels for V2X Sidelink Communication 511

A.3.22 CSI-IM configurations 511

A.3.22.1 FDD 511

A.3.22.2 TDD 512

A.3.23 Spatial Relation Configuration 514

A.3.23.1 Introduction 514

A.3.23.2 Spatial Relation 514

A.3.24 SRS configuration 515

A.3.25 Channel bandwidth (CBW) configurations 517

A.3.25.1 DL UE specific CBW 517

A.3.25.2 UL UE specific CBW 518

A.3.26 CCA model 518

A.3.26.1 Introduction 518

A.3.26.2 CCA model for operation on a carrier frequency with CCA in FR1 518

A.3.26.2.1 DL CCA model 518

A.3.26.2.2 UL CCA model 519

A.3.27 Test Cases with at Least One Cell on a Carrier Frequency with CCA 520

A.3.27.1 Introduction 520

A.3.27.2 NR Standalone Tests with NR SCell under CCA and All Other NR Cells in FR1 520

A.3.27.3 EN-DC Tests with NR PSCell under CCA and Other NR Cells in FR1 520

A.3.27.4 NR Standalone Tests with NR PCell under CCA and Other NR Cells in FR1 520

A.3.27.5 E-UTRA Standalone Tests with at Least One NR Cell under CCA 521

A.3.28 Discovery Burst Transmission Window configuration under CCA 521

A.3.28.1 DBT Window pattern 1: DBT Window period = 20 ms with DBT Window duration = 1 ms 521

A.3.29 Testing principles for UE capable of only NR bands with shared spectrum access 521

A.3.29.1 Introduction 521

A.3.29.2 Principle of testing for UE capable of EN-DC with only NR bands with shared spectrum access 521

A.3.29.3 Principle of testing for UE capable of SA operation with only NR bands with shared spectrum access 522

A.3.30 CSI-RS configurations for RRM 522

A.3.30.1 FDD 522

A.3.30.2 TDD 523

A.3.31 PRS Configurations 525

A.3.31.1. PRS Configurations for FR1 525

A.3.31.1.1. PRS pattern 1 in FR1: SCS=15 KHz 525

A.3.31.1.2. PRS pattern 2 in FR1: SCS=30 KHz 526

A.3.31.2. PRS Configurations for FR2 526

A.3.31.2.1. PRS pattern 1 in FR2: SCS=120 KHz 526

A.4 EN-DC tests with all NR cells in FR1 527

A.4.1 Void 527

A.4.2 Void 527

A.4.3 RRC\_CONNECTED state mobility 527

A.4.3.1 Void 527

A.4.3.2 RRC Connection Mobility Control 527

A.4.3.2.1 Void 527

A.4.3.2.2 Random Access 527

A.4.3.2.2.1 4-step RA type contention based random access test in FR1 for PSCell in EN-DC 527

A.4.3.2.2.2 4-step RA type non-contention based random access test in FR1 for PSCell in EN-DC 531

A.4.3.2.2.3 2-step RA type contention based random access test in FR1 for PSCell in EN-DC 535

A.4.3.2.2.4 2-step RA type non-contention based random access test in FR1 for PSCell in EN-DC 539

A.4.3.2.3 Void 543

A.4.4 Timing 543

A.4.4.1 UE transmit timing 543

A.4.4.1.1 NR UE Transmit Timing Test for FR1 543

A.4.4.1.1.1 Test Purpose and environment 543

A.4.4.1.1.2 Test requirements 547

A.4.4.2 UE timer accuracy 547

A.4.4.3 Timing advance 547

A.4.4.3.1 EN-DC FR1 timing advance adjustment accuracy 547

A.4.4.3.1.1 Test Purpose and Environment 547

A.4.4.3.1.2 Test Parameters 547

A.4.4.3.1.3 Test Requirements 551

A.4.5 Signaling characteristics 551

A.4.5.1 Radio link Monitoring 551

A.4.5.1.1 Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with SSB-based RLM RS in non-DRX mode 552

A.4.5.1.1.1 Test Purpose and Environment 552

A.4.5.1.1.2 Test Requirements 556

A.4.5.1.2 Radio Link Monitoring In-sync Test for FR1 PSCell configured with SSB-based RLM RS in non-DRX mode 556

A.4.5.1.2.1 Test Purpose and Environment 556

A.4.5.1.2.2 Test Requirements 562

A.4.5.1.3 Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with SSB-based RLM RS in DRX mode 562

A.4.5.1.3.1 Test Purpose and Environment 562

A.4.5.1.3.2 Test Requirements 568

A.4.5.1.4 Radio Link Monitoring In-sync Test for FR1 PSCell configured with SSB-based RLM RS in DRX mode 568

A.4.5.1.4.1 Test Purpose and Environment 568

A.4.5.1.4.2 Test Requirements 573

A.4.5.1.5 EN-DC Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with CSI-RS-based RLM in non-DRX mode 573

A.4.5.1.5.1 Test Purpose and Environment 573

A.4.5.1.5.2 Test Requirements 579

A.4.5.1.6 EN-DC Radio Link Monitoring In-sync Test for FR1 PSCell configured with CSI-RS-based RLM in non-DRX mode 579

A.4.5.1.6.1 Test Purpose and Environment 579

A.4.5.1.6.2 Test Requirements 585

A.4.5.1.7 EN-DC Radio Link Monitoring Out-of-sync Test for FR1 PSCell configured with CSI-RS-based RLM in DRX mode 585

A.4.5.1.7.1 Test Purpose and Environment 585

A.4.5.1.7.2 Test Requirements 590

A.4.5.1.8 EN-DC Radio Link Monitoring In-sync Test for FR1 PSCell configured with CSI-RS-based RLM in DRX mode 591

A.4.5.1.8.1 Test Purpose and Environment 591

A.4.5.1.8.2 Test Requirements 596

A.4.5.2 Interruption 596

A.4.5.2.1 E-UTRAN – NR FR1 interruptions at transitions between active and non-active during DRX in synchronous EN-DC 596

A.4.5.2.1.1 Test Purpose and Environment 596

A.4.5.2.1.2 Test Requirements 600

A.4.5.2.2 E-UTRAN – NR FR1 interruptions at transitions between active and non-active during DRX in asynchronous EN-DC 600

A.4.5.2.2.1 Test Purpose and Environment 600

A.4.5.2.2.2 Test Requirements 604

A.4.5.2.3 E-UTRAN – NR FR1 interruptions during measurements on deactivated NR SCC in synchronous EN-DC 604

A.4.5.2.3.1 Test Purpose and Environment 604

A.4.5.2.3.2 Test Requirements 609

A.4.5.2.4 E-UTRAN – NR FR1 interruptions during measurements on deactivated NR SCC in asynchronous EN-DC 610

A.4.5.2.4.1 Test Purpose and Environment 610

A.4.5.2.4.2 Test Requirements 614

A.4.5.2.5 E-UTRAN – NR FR1 interruptions during measurements on deactivated E-UTRAN SCC in synchronous EN-DC 615

A.4.5.2.5.1 Test Purpose and Environment 615

A.4.5.2.5.2 Test Requirements 619

A.4.5.2.6 E-UTRAN – NR FR1 interruptions during measurements on deactivated E-UTRAN SCC in asynchronous EN-DC 619

A.4.5.2.6.1 Test Purpose and Environment 619

A.4.5.2.6.2 Test Requirements 623

A.4.5.2.7 Void 623

A.4.5.2.8 E-UTRAN - NR FR1 interruptions at NR SRS carrier based switching in asynchronous EN-DC 623

A.4.5.2.8.1 Test Purpose and Environment 623

A.4.5.2.8.2 Test Requirements 626

A.4.5.2.9 E-UTRAN – NR interruptions at E-UTRA SRS carrier based switching 627

A.4.5.2.9.1 Test Purpose and Environment 627

A.4.5.2.9.2 Test Requirements 631

A.4.5.3 SCell Activation and Deactivation Delay 632

A.4.5.3.1 SCell Activation and deactivation of known SCell in FR1 for 160ms SCell measurement cycle 632

A.4.5.3.1.1 Test Purpose and Environment 632

A.4.5.3.1.2 Test Requirements 638

A.4.5.3.2 SCell Activation and deactivation of known SCell in FR1 for 640ms SCell measurement cycle 639

A.4.5.3.2.1 Test Purpose and Environment 639

A.4.5.3.2.2 Test Requirements 639

A.4.5.3.3 SCell Activation and deactivation of unknown SCell in FR1 639

A.4.5.3.3.1 Test Purpose and Environment 639

A.4.5.3.3.2 Test Requirements 640

A.4.5.3.4 SCell Activation and deactivation of multiple unknown SCells in FR1 with single activation/deactivation command 641

A.4.5.3.4.1 Test Purpose and Environment 641

A.4.5.3.4.2 Test Requirements 645

A.4.5.3.5 Direct SCell activation at SCell addition of known SCell in FR1 645

A.4.5.3.5.1 Test Purpose and Environment 645

A.4.5.3.5.2 Test Requirements 652

A.4.5.4 UE UL carrier RRC reconfiguration Delay 652

A.4.5.4.1 UE UL carrier RRC reconfiguration Delay 652

A.4.5.4.1.1 Test Purpose and Environment 652

A.4.5.4.1.2 Test Requirements 660

A.4.5.5 Beam Failure Detection and Link recovery procedures 661

A.4.5.5.1 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in non-DRX mode 661

A.4.5.5.1.1 Test Purpose and Environment 661

A.4.5.5.1.2 Test Requirements 666

A.4.5.5.2 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in DRX mode 666

A.4.5.5.2.1 Test Purpose and Environment 666

A.4.5.5.2.2 Test Requirements 672

A.4.5.5.3 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with CSI-RS-based BFD and LR in non-DRX mode 672

A.4.5.5.3.1 Test Purpose and Environment 672

A.4.5.5.3.2 Test Requirements 678

A.4.5.5.4 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with CSI-RS-based BFD and LR in DRX mode 678

A.4.5.5.4.1 Test Purpose and Environment 678

A.4.5.5.4.2 Test Requirements 684

A.4.5.5.5 EN-DC Beam Failure Detection and Link Recovery Test for FR1 SCell configured with CSI-RS-based BFD and SSB-based LR in non-DRX mode 684

A.4.5.5.5.1 Test Purpose and Environment 684

A.4.5.5.5.2 Test Requirements 690

A.4.5.5.6 EN-DC Beam Failure Detection and Link Recovery Test for FR1 SCell configured with CSI-RS-based BFD and SSB-based LR in DRX mode 690

A.4.5.5.6.1 Test Purpose and Environment 690

A.4.5.5.6.2 Test Requirements 697

A.4.5.6 Active BWP switch 698

A.4.5.6.1 DCI-based and Timer-based Active BWP Switch 698

A.4.5.6.1.1 E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in synchronous EN-DC 698

A.4.5.6.1.2 E-UTRAN – NR PSCell FR1 DL active BWP switch with FR1 SCell in non-DRX in synchronous EN-DC 703

A.4.5.6.2 RRC-based Active BWP Switch 709

A.4.5.6.3 Simultaneous DCI-based and Timer-based Active BWP Switch on multiple CCs 713

A.4.5.6.3.1 Simultaneous E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in EN-DC on multiple CCs 713

A.4.5.6.3.1.1 Test Purpose and Environment 713

A.4.5.6.3.1.2 Test Requirements 719

A.4.5.6.4 SCell dormancy switch 719

A.4.5.6.4.1 E-UTRAN – NR FR1 PSCell SCell dormancy switch of single FR1 SCell outside active time 719

A.4.5.6.4.1.1 Test Purpose and Environment 719

A.4.5.6.4.1.2 Test Requirements 727

A.4.5.6.4.2 E-UTRAN – NR FR1 PSCell SCell dormancy switch of two FR1 SCells inside active time 727

A.4.5.6.4.2.1 Test Purpose and Environment 727

A.4.5.6.4.2.2 Test Requirements 739

A.4.5.6.5 Simultaneous RRC-based Active BWP Switch on multiple CCs 740

A.4.5.6.5.1 E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in synchronous EN-DC on multiple CCs 740

A.4.5.6.5.1.1 Test Purpose and Environment 740

A.4.5.6.5.1.2 Test Requirements 744

A.4.5.7 PSCell addition and release delay 744

A.4.5.7.1 Addition and Release Delay of known NR PSCell 744

A.4.5.7.1.1 Test purpose and environment 744

A.4.5.7.1.2 Test Requirements 748

A.4.5.8 DL Interruptions at switching between two uplink carriers 749

A.4.5.8.1 Test Purpose and Environment 749

A.4.5.8.2 Test Requirements 752

A.4.5.9 UE specific CBW change 753

A.4.5.9.1 UE specific CBW change on FR1 NR PSCell with non-DRX in synchronous EN- DC 753

A.4.5.9.1.1 Test Purpose and Environment 753

A.4.5.9.1.2 Test Requirements 757

A.4.6 Measurement procedure 757

A.4.6.1 Intra-frequency Measurements 757

A.4.6.1.1 EN-DC event triggered reporting tests without gap under non-DRX 757

A.4.6.1.1.1 Test purpose and Environment 757

A.4.6.1.1.2 Test parameters 757

A.4.6.1.1.3 Test Requirements 761

A.4.6.1.2 EN-DC event triggered reporting tests without gap under DRX 761

A.4.6.1.2.1 Test purpose and Environment 761

A.4.6.1.2.2 Test parameters 761

A.4.6.1.2.2 Test Requirements 765

A.4.6.1.3 EN-DC event triggered reporting tests with per-UE gaps under non-DRX 765

A.4.6.1.3.1 Test purpose and Environment 765

A.4.6.1.3.2 Test parameters 765

A.4.6.1.3.3 Test Requirements 769

A.4.6.1.4 EN-DC event triggered reporting tests with per-UE gaps under DRX 769

A.4.6.1.4.1 Test purpose and Environment 769

A.4.6.1.4.2 Test parameters 769

A.4.6.1.4.3 Test Requirements 773

A.4.6.1.5 EN-DC event triggered reporting tests without gap under non-DRX with SSB index reading 773

A.4.6.1.5.1 Test purpose and Environment 773

A.4.6.1.5.2 Test parameters 773

A.4.6.1.5.3 Test Requirements 775

A.4.6.1.6 EN-DC event triggered reporting tests with SSB index reading with per-UE gaps 776

A.4.6.1.6.1 Test purpose and Environment 776

A.4.6.1.6.2 Test parameters 776

A.4.6.1.6.3 Test Requirements 778

A.4.6.1.7 EN-DC event triggered reporting tests under DRX for UE configured with highSpeedMeasFlag-r16 779

A.4.6.1.7.1 Test purpose and Environment 779

A.4.6.1.7.2 Test parameters 779

A.4.6.1.7.3 Test Requirements 783

A.4.6.2 Inter-frequency Measurements 783

A.4.6.2.1 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is not used 783

A.4.6.2.1.1 Test Purpose and Environment 783

A.4.6.2.1.2 Test Requirements 787

A.4.6.2.2 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is used 787

A.4.6.2.2.1 Test Purpose and Environment 787

A.4.6.2.2.2 Test Requirements 791

A.4.6.2.3 Void 792

A.4.6.2.4 Void 792

A.4.6.2.5 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is not used 792

A.4.6.2.5.1 Test Purpose and Environment 792

A.4.6.2.5.2 Test Requirements 796

A.4.6.2.6 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is used 797

A.4.6.2.6.1 Test Purpose and Environment 797

A.4.6.2.6.2 Test Requirements 801

A.4.6.2.7 Void 802

A.4.6.2.8 Void 802

A.4.6.3 Void 802

A.4.6.4 L1-RSRP measurement for beam reporting 802

A.4.6.4.1 SSB based L1-RSRP measurement when DRX is not used 802

A.4.6.4.1.1 Test Purpose and Environment 802

A.4.6.4.1.2 Test parameters 802

A.4.6.4.1.3 Test Requirements 805

A.4.6.4.2 SSB based L1-RSRP measurement when DRX is used 805

A.4.6.4.2.1 Test Purpose and Environment 805

A.4.6.4.2.2 Test parameters 806

A.4.6.4.2.3 Test Requirements 809

A.4.6.4.3 CSI-RS based L1-RSRP measurement when DRX is not used 809

A.4.6.4.3.1 Test Purpose and Environment 809

A.4.6.4.3.2 Test parameters 810

A.4.6.4.3.3 Test Requirements 813

A.4.6.4.4 CSI-RS based L1-RSRP measurement when DRX is used 813

A.4.6.4.4.1 Test Purpose and Environment 813

A.4.6.4.4.2 Test parameters 814

A.4.6.4.4.3 Test Requirements 816

A.4.6.4.5 SSB based L1-RSRP measurement when DRX is used for UE configured with *highSpeedMeasFlag-r16* 816

A.4.6.4.5.1 Test Purpose and Environment 816

A.4.6.4.5.2 Test parameters 817

A.4.6.4.5.3 Test Requirements 820

A.4.6.5 CLI measurements 820

A.4.6.5.1 SRS-RSRP measurement with non-DRX 820

A.4.6.5.1.1 Test Purpose and Environment 820

A.4.6.5.1.2 Test Parameters 821

A.4.6.5.1.3 Test Requirements 824

A.4.6.5.2 CLI-RSSI measurement with non-DRX 824

A.4.6.5.2.1 Test Purpose and Environment 824

A.4.6.5.2.2 Test Parameters 825

A.4.6.5.2.3 Test Requirements 826

A.4.6.6 Measurements with autonomous gaps 827

A.4.6.6.1 EN-DCintra-frequency CGI identification of NR FR1 cell with autonomous gaps in synchronous EN-DC 827

A.4.6.6.1.1 Test Purpose and Environment 827

A.4.6.6.1.2 Test Requirements 831

A.4.6.7 L1-SINR measurement for beam reporting 831

A.4.6.7.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR when DRX is not used 831

A.4.6.7.1.1 Test Purpose and Environment 831

A.4.6.7.1.2 Test parameters 832

A.4.6.7.1.3 Test Requirements 835

A.4.6.7.2 L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is used 835

A.4.6.7.2.1 Test Purpose and Environment 835

A.4.6.7.2.2 Test parameters 836

A.4.6.7.2.3 Test Requirements 839

A.4.6.7.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is used 839

A.4.6.7.3.1 Test Purpose and Environment 839

A.4.6.7.3.2 Test parameters 840

A.4.6.7.3.3 Test Requirements 843

A.4.6.8 CSI-RS based intra-frequency Measurement 843

A.4.6.8.1 EN-DC event triggered reporting tests without gap under DRX 843

A.4.6.8.1.1 Test purpose and Environment 843

A.4.6.8.1.2 Test Requirements 846

A.4.6.9 CSI-RS based inter-frequency Measurement 847

A.4.6.9.1 EN-DC event triggered reporting tests for FR1 cell when non-DRX is used 847

A.4.6.9.1.1 Test Purpose and Environment 847

A.4.6.9.1.2 Test Requirements 850

A.4.7 Measurement Performance requirements 851

A.4.7.1 SS-RSRP 851

A.4.7.1.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 851

A.4.7.1.1.1 Test Purpose and Environment 851

A.4.7.1.1.2 Test parameters 851

A.4.7.1.1.3 Test Requirements 855

A.4.7.1.2 EN-DC inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 855

A.4.7.1.2.1 Test Purpose and Environment 855

A.4.7.1.2.2 Test parameters 856

A.4.7.1.2.3 Test Requirements 860

A.4.7.1.3 Void 860

A.4.7.2 SS-RSRQ 860

A.4.7.2.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 860

A.4.7.2.1.1 Test Purpose and Environment 860

A.4.7.2.1.2 Test Parameters 861

A.4.7.2.1.3 Test Requirements 866

A.4.7.2.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 866

A.4.7.2.2.1 Test Purpose and Environment 866

A.4.7.2.2.2 Test Parameters 866

A.4.7.2.2.3 Test Requirements 870

A.4.7.3 SS-SINR 871

A.4.7.3.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 871

A.4.7.3.1.1 Test Purpose and Environment 871

A.4.7.3.1.2 Test Parameters 871

A.4.7.3.1.3 Test Requirements 875

A.4.7.3.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 875

A.4.7.3.2.1 Test Purpose and Environment 875

A.4.7.3.2.2 Test Parameters 875

A.4.7.3.2.3 Test Requirements 880

A.4.7.4 L1-RSRP measurement for beam reporting 880

A.4.7.4.1 SSB based L1-RSRP measurement 880

A.4.7.4.1.1 Test Purpose and Environment 880

A.4.7.4.1.2 Test parameters 881

A.4.7.4.1.3 Test Requirements 884

A.4.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 884

A.4.7.4.2.1 Test Purpose and Environment 884

A.4.7.4.2.2 Test parameters 885

A.4.7.4.2.3 Test Requirements 888

A.4.7.5 SFTD accuracy 888

A.4.7.5.1 SFTD accuracy 888

A.4.7.5.1.1 Test Purpose and Environment 888

A.4.7.5.1.2 Test Parameters 888

A.4.7.5.1.3 Test Requirements 893

A.4.7.5.2 Void 893

A.4.7.5.3 Void 893

A.4.7.6 CLI measurements 893

A.4.7.6.1 EN-DC SRS-RSRP measurement accuracy with FR1 serving cell 893

A.4.7.6.1.1 Test Purpose and Environment 893

A.4.7.6.1.2 Test parameters 894

A.4.7.6.1.3 Test Requirements 899

A.4.7.6.2 EN-DC CLI-RSSI measurement accuracy with FR1 serving cell 899

A.4.7.6.2.1 Test Purpose and Environment 899

A.4.7.6.2.2 Test parameters 900

A.4.7.6.2.3 Test Requirements 903

A.4.7.7 L1-SINR measurement for beam reporting 903

A.4.7.7.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off 903

A.4.7.7.1.1 Test Purpose and Environment 903

A.4.7.7.1.2 Test parameters 904

A.4.7.7.1.3 Test Requirements 908

A.4.7.7.2 L1-SINR measurement with SSB based CMR and dedicated IMR 908

A.4.7.7.2.1 Test Purpose and Environment 908

A.4.7.7.2.2 Test parameters 909

A.4.7.7.2.3 Test Requirements 913

A.4.7.7.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR 913

A.4.7.7.3.1 Test Purpose and Environment 913

A.4.7.7.3.2 Test parameters 914

A.4.7.7.3.3 Test Requirements 917

A.4.7.8 CSI-RSRP 917

A.4.7.8.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 917

A.4.7.8.1.1 Test Purpose and Environment 917

A.4.7.8.1.2 Test parameters 918

A.4.7.8.1.3 Test Requirements 921

A.4.7.8.2 EN-DC inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 921

A.4.7.8.2.1 Test Purpose and Environment 921

A.4.7.8.2.2 Test parameters 922

A.4.7.8.2.3 Test Requirements 925

A.4.7.9 CSI-RSRQ 926

A.4.7.9.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 926

A.4.7.9.1.1 Test Purpose and Environment 926

A.4.7.9.1.2 Test Parameters 926

A.4.7.9.1.3 Test Requirements 931

A.4.7.9.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 931

A.4.7.9.2.1 Test Purpose and Environment 931

A.4.7.9.2.2 Test Parameters 931

A.4.7.2.2.3 Test Requirements 936

A.4.7.10 CSI-SINR 936

A.4.7.10.1 EN-DC Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 936

A.4.7.10.1.1 Test Purpose and Environment 936

A.4.7.10.1.2 Test Parameters 937

A.4.7.10.1.3 Test Requirements 940

A.4.7.10.2 EN-DC Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 940

A.4.7.10.2.1 Test Purpose and Environment 940

A.4.7.10.2.2 Test Parameters 940

A.4.7.10.2.3 Test Requirements 943

A.4.8 Void 944

A.4A NE-DC test with all NR cells in FR1 944

A.4A.1 Signaling characteristics 944

A.4A.1.1 E-UTRAN PSCell addition 944

A.4A.1.1.1 Test purpose and environment 944

A.4A.1.1.2 Test Requirements 948

A.4A.1.2 Active BWP switch 949

A.4A.1.2.1 E-UTRAN PSCell – NR PCell FR1 DCI-based and Timer-based DL active BWP switch in non-DRX in synchronous NE-DC 949

A.4A.1.2.1.1 Test Purpose and Environment 949

A.4A.1.2.1.2 Test Requirements 953

A.4A.2 Measurement performance 954

A.4A.2.1 SFTD accuracy 954

A.4A.2.1.1 SFTD accuracy 954

A.4A.2.1.1.1 Test Purpose 954

A.4A.2.1.1.2 Test Environment 954

A.4A.2.1.1.3 Test Requirements 957

A.5 EN-DC tests with one or more NR cells in FR2 958

A.5.1 Void 958

A.5.2 Void 958

A.5.3 RRC\_CONNECTED state mobility 958

A.5.3.1 Void 958

A.5.3.2 RRC Connection Mobility Control 958

A.5.3.2.1 Void 958

A.5.3.2.2 Random Access 958

A.5.3.2.2.1 4-step RA type contention based random access test in FR2 for PSCell/SCell in EN-DC 958

A.5.3.2.2.2 4-step RA type non-contention based random access test in FR2 for PSCell/SCell in EN-DC 961

A.5.3.2.2.3 2-step RA type contention based random access test in FR2 for PSCell/SCell in EN-DC 967

A.5.3.2.2.4 2-step RA type non-contention based random access test in FR2 for PSCell/SCell in EN-DC 970

A.5.3.2.3 Void 974

A.5.4 Timing 974

A.5.4.1 UE transmit timing 974

A.5.4.1.1 NR UE Transmit Timing Test for FR2 974

A.5.4.1.1.1 Test Purpose and environment 974

A.5.4.1.1.2 Test requirements 977

A.5.4.2 UE timer accuracy 978

A.5.4.3 Timing advance 978

A.5.4.3.1 EN-DC FR2 timing advance adjustment accuracy 978

A.5.4.3.1.1 Test Purpose and Environment 978

A.5.4.3.1.2 Test Parameters 978

A.5.4.3.1.3 Test Requirements 982

A.5.5 Signaling characteristics 982

A.5.5.1 Radio link Monitoring 982

A.5.5.1.1 Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with SSB-based RLM RS in non-DRX mode 982

A.5.5.1.1.1 Test Purpose and Environment 982

A.5.5.1.1.2 Test Requirements 986

A.5.5.1.2 Radio Link Monitoring In-sync Test for FR2 PSCell configured with SSB-based RLM RS in non-DRX mode 987

A.5.5.1.2.1 Test Purpose and Environment 987

A.5.5.1.2.2 Test Requirements 990

A.5.5.1.3 Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with SSB-based RLM RS in DRX mode 991

A.5.5.1.3.1 Test Purpose and Environment 991

A.5.5.1.3.2 Test Requirements 995

A.5.5.1.4 Radio Link Monitoring In-sync Test for FR2 PSCell configured with SSB-based RLM RS in DRX mode 995

A.5.5.1.4.1 Test Purpose and Environment 995

A.5.5.1.4.2 Test Requirements 999

A.5.5.1.5 EN-DC Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with CSI-RS-based RLM in non-DRX mode 999

A.5.5.1.6 EN-DC Radio Link Monitoring In-sync Test for FR2 PSCell configured with CSI-RS-based RLM in non-DRX mode 1003

A.5.5.1.7 EN-DC Radio Link Monitoring Out-of-sync Test for FR2 PSCell configured with CSI-RS-based RLM in DRX mode 1007

A.5.5.1.8 EN-DC Radio Link Monitoring In-sync Test for FR2 PSCell configured with CSI-RS-based RLM in DRX mode 1012

A.5.5.1.8.2 Test Requirements 1016

A.5.5.1.9 EN-DC Radio Link Monitoring UE Scheduling Restrictions on FR2 1017

A.5.5.1.9.1 Test Purpose and Environment 1017

A.5.5.1.9.2 Test Requirements 1019

A.5.5.2 Interruption 1019

A.5.5.2.1 E-UTRAN – NR FR2 interruptions at transitions between active and non-active during DRX in synchronous EN-DC 1019

A.5.5.2.1.1 Test Purpose and Environment 1019

A.5.5.2.1.2 Test Requirements 1022

A.5.5.2.2 E-UTRAN – NR FR2 interruptions at transitions between active and non-active during DRX in asynchronous EN-DC 1022

A.5.5.2.2.1 Test Purpose and Environment 1022

A.5.5.2.2.2 Test Requirements 1025

A.5.5.2.3 E-UTRAN – NR FR2 interruptions during measurements on deactivated NR SCC in synchronous EN-DC 1025

A.5.5.2.3.1 Test Purpose and Environment 1025

A.5.5.2.3.2 Test Requirements 1029

A.5.5.2.4 E-UTRAN – NR FR2 interruptions during measurements on deactivated NR SCC in asynchronous EN-DC 1029

A.5.5.2.4.1 Test Purpose and Environment 1029

A.5.5.2.4.2 Test Requirements 1032

A.5.5.2.5 E-UTRAN – NR FR2 interruptions during measurements on deactivated E-UTRAN SCC in synchronous EN-DC 1033

A.5.5.2.5.1 Test Purpose and Environment 1033

A.5.5.2.5.2 Test Requirements 1036

A.5.5.2.6 E-UTRAN – NR FR2 interruptions during measurements on deactivated E-UTRAN SCC in asynchronous EN-DC 1037

A.5.5.2.6.1 Test Purpose and Environment 1037

A.5.5.2.6.2 Test Requirements 1039

A.5.5.2.7 E-UTRAN – NR FR2 interruptions at E-UTRA SRS carrier based switching 1040

A.5.5.2.7.1 Test Purpose and Environment 1040

A.5.5.2.7.2 Test Requirements 1043

A.5.5.2.8 E-UTRAN – NR FR2 interruptions at NR SRS carrier based switching 1043

A.5.5.2.8.1 Test Purpose and Environment 1043

A.5.5.2.8.3 Test Requirements 1045

A.5.5.3 SCell Activation and Deactivation Delay 1045

A.5.5.3.1 SCell Activation and deactivation of SCell in FR2 intra-band 1045

A.5.5.3.1.1 Test Purpose and Environment 1045

A.5.5.3.1.2 Test Requirements 1048

A.5.5.3.2 SCell Activation and deactivation of known SCell in FR1 for 160ms SCell measurement cycle 1048

A.5.5.3.2.1 Test Purpose and Environment 1048

A.5.5.3.2.2 Test Requirements 1052

A.5.5.3.3 Void 1052

A.5.5.3.4 Void 1052

A.5.5.3.5 SCell Activation and deactivation of SCell in FR2 1052

A.5.5.3.5.1 Test Purpose and Environment 1052

A.5.5.3.5.2 Test Requirements 1055

A.5.5.3.6 Multiple SCell Activation and deactivation of one unknown SCell and one known SCell in FR2 1056

A.5.5.3.6.1 Test Purpose and Environment 1056

A.5.5.3.6.2 Test Requirements 1060

A.5.5.3.7 Direct SCell activation at SCell addition of known SCell in FR2 1061

A.5.5.3.7.1 Test Purpose and Environment 1061

A.5.5.3.7.2 Test Requirements 1064

A.5.5.4 Void 1064

A.5.5.5 Beam Failure Detection and Link recovery procedures 1064

A.5.5.5.1 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with SSB-based BFD and LR in non-DRX mode 1064

A.5.5.5.1.1 Test Purpose and Environment 1064

A.5.5.5.1.2 Test Requirements 1068

A.5.5.5.2 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with SSB-based BFD and LR in DRX mode 1068

A.5.5.5.2.1 Test Purpose and Environment 1068

A.5.5.5.2.2 Test Requirements 1072

A.5.5.5.3 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with CSI-RS-based BFD and LR in non-DRX mode 1072

A.5.5.5.3.1 Test Purpose and Environment 1072

A.5.5.5.3.2 Test Requirements 1076

A.5.5.5.4 EN-DC Beam Failure Detection and Link Recovery Test for FR2 PSCell configured with CSI-RS-based BFD and LR in DRX mode 1076

A.5.5.5.4.1 Test Purpose and Environment 1076

A.5.5.5.4.2 Test Requirements 1080

A.5.5.5.5 EN-DC scheduling availability restriction during Beam Failure Detection and Link Recovery for FR2 PSCell configured with SSB-based BFD and LR in non-DRX mode 1080

A.5.5.5.5.1 Test Purpose and Environment 1080

A.5.5.5.5.2 Test Requirements 1084

A.5.5.5.6 EN-DC Beam Failure Detection and Link Recovery Test for FR2 SCell configured with CSI-RS-based BFD and LR in non-DRX mode 1084

A.5.5.5.6.1 Test Purpose and Environment 1084

A.5.5.5.6.2 Test Requirements 1088

A.5.5.5.7 EN-DC Beam Failure Detection and Link Recovery Test for FR2 SCell configured with CSI-RS-based BFD and LR in DRX mode 1088

A.5.5.5.7.1 Test Purpose and Environment 1088

A.5.5.5.7.2 Test Requirements 1092

A.5.5.6 Active BWP switch 1092

A.5.5.6.1 DCI-based and Timer-based Active BWP Switch 1092

A.5.5.6.1.1 E-UTRAN – NR PSCell FR2 DL active BWP switch with non-DRX in synchronous EN-DC 1092

A.5.5.6.1.1.1 Test Purpose and Environment 1092

A.5.5.6.1.1.2 Test Requirements 1096

A.5.5.6.1.2 E-UTRAN – NR PSCell FR2 with FR2 SCell DL active BWP switch in non-DRX in synchronous EN-DC 1096

A.5.5.6.2 RRC-based Active BWP Switch 1101

A.5.5.6.3 Simultaneous DCI-based and Timer-based Active BWP Switch on multiple CCs 1105

A.5.5.6.3.1 E-UTRAN – NR PSCell FR2 and NR SCell FR2 DL active BWP switch on multiple CCs in synchronous EN-DC 1105

A.5.5.6.3.1.1 Test Purpose and Environment 1105

A.5.5.6.3.1.2 Test Requirements 1109

A.5.5.6.4 SCell dormancy switch 1109

A.5.5.6.4.1 E-UTRAN – NR FR2 PSCell SCell dormancy switch of single FR2 SCell inside active time 1109

A.5.5.6.4.1.1 Test Purpose and Environment 1109

A.5.5.6.4.1.2 Test Requirements 1113

A.5.5.6.4.2 E-UTRAN – NR FR1 PSCell SCell dormancy switch of two FR2 SCells outside active time 1113

A.5.5.6.4.2.1 Test Purpose and Environment 1113

A.5.5.6.4.2.2 Test Requirements 1120

A.5.5.6.5 Simultaneous RRC-based Active BWP Switch on multiple CCs 1120

A.5.5.7 PSCell addition and release delay 1123

A.5.5.7.1 Addition and Release Delay of NR PSCell 1123

A.5.5.7.1.1 Test purpose and environment 1123

A.5.5.7.1.2 Test Requirements 1127

A.5.5.8 Active TCI state switch delay 1128

A.5.5.8.1 MAC-CE based active TCI state switch 1128

A.5.5.8.1.1 E-UTRAN – NR PSCell FR2 active TCI state switch for a known TCI state 1128

A.5.5.8.1.1.1 Test Purpose and Environment 1128

A.5.5.8.1.1.2 Test Requirements 1131

A.5.5.8.2 RRC based active TCI state switch 1131

A.5.5.8.2.1 E-UTRAN – NR PSCell FR2 active TCI state switch for a known TCI state 1131

A.5.5.8.2.1.1 Test Purpose and Environment 1131

A.5.5.8.2.1.2 Test Requirements 1135

A.5.5.9 Uplink spatial relation switch delay 1135

A.5.5.9.1 MAC-CE based uplink spatial relation switch 1135

A.5.5.9.1.1 E-UTRAN – NR PSCell FR2 uplink spatial relation switch for a known spatial relation 1135

A.5.5.9.1.1.1 Test Purpose and Environment 1135

A.5.5.9.1.1.2 Test Requirements 1138

A.5.5.9.2 RRC based spatial relation switch 1138

A.5.5.9.2.1 E-UTRAN – NR PSCell FR2 spatial relation switch associated with a known DL-RS 1138

A.5.5.9.2.1.1 Test Purpose and Environment 1138

A.5.5.9.2.1.2 Test Requirements 1141

A.5.5.10 UE specific CBW change 1141

A.5.5.10.1 UE specific CBW change on FR2 NR PSCell 1141

A.5.5.10.1.1 Test Purpose and Environment 1141

A.5.5.10.1.2 Test Requirements 1144

A.5.6 Measurement procedure 1145

A.5.6.1 Intra-frequency Measurements 1145

A.5.6.1.1 EN-DC event triggered reporting test without gap under non-DRX 1145

A.5.6.1.1.1 Test purpose and Environment 1145

A.5.6.1.1.2 Test Requirements 1148

A.5.6.1.2 EN-DC event triggered reporting test without gap under DRX 1148

A.5.6.1.2.1 Test purpose and Environment 1148

A.5.6.1.2.2 Test Requirements 1150

A.5.6.1.3 EN-DC event triggered reporting test with per-UE gaps under non-DRX 1151

A.5.6.1.3.1 Test purpose and Environment 1151

A.5.6.1.3.2 Test Requirements 1155

A.5.6.1.4 EN-DC event triggered reporting test with per-UE gaps under DRX 1155

A.5.6.1.4.1 Test purpose and Environment 1155

A.5.6.1.4.2 Test Requirements 1158

A.5.6.2 Inter-frequency Measurements 1159

A.5.6.2.1 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is not used 1159

A.5.6.2.1.1 Test Purpose and Environment 1159

A.5.6.2.1.2 Test Requirements 1162

A.5.6.2.2 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is used 1162

A.5.6.2.2.1 Test Purpose and Environment 1162

A.5.6.2.2.2 Test Requirements 1166

A.5.6.2.3 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is not used 1166

A.5.6.2.3.1 Test Purpose and Environment 1166

A.5.6.2.3.2 Test Requirements 1170

A.5.6.2.4 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is used 1170

A.5.6.2.4.1 Test Purpose and Environment 1170

A.5.6.2.4.2 Test Requirements 1174

A.5.6.2.5 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is not used 1174

A.5.6.2.5.1 Test Purpose and Environment 1174

A.5.6.2.5.2 Test Requirements 1179

A.5.6.2.6 EN-DC event triggered reporting tests for FR2 cell without SSB time index detection when DRX is used 1179

A.5.6.2.6.1 Test Purpose and Environment 1179

A.5.6.2.6.2 Test Requirements 1183

A.5.6.2.7 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is not used 1183

A.5.6.2.7.1 Test Purpose and Environment 1183

A.5.6.2.7.2 Test Requirements 1188

A.5.6.2.8 EN-DC event triggered reporting tests for FR2 cell with SSB time index detection when DRX is used 1188

A.5.6.2.8.1 Test Purpose and Environment 1188

A.5.6.2.8.2 Test Requirements 1193

A.5.6.3 L1-RSRP measurement for beam reporting 1193

A.5.6.3.1 SSB based L1-RSRP measurement when DRX is not used 1193

A.5.6.3.1.1 Test Purpose and Environment 1193

A.5.6.3.1.2 Test parameters 1193

A.5.6.3.1.3 Test Requirements 1195

A.5.6.3.2 SSB based L1-RSRP measurement when DRX is used 1195

A.5.6.3.2.1 Test Purpose and Environment 1195

A.5.6.3.2.2 Test parameters 1196

A.5.6.3.2.3 Test Requirements 1198

A.5.6.3.3 CSI-RS based L1-RSRP measurement when DRX is not used 1198

A.5.6.3.3.1 Test Purpose and Environment 1198

A.5.6.3.3.2 Test parameters 1199

A.5.6.3.3.3 Test Requirements 1201

A.5.6.3.4 CSI-RS based L1-RSRP measurement when DRX is used 1202

A.5.6.3.4.1 Test Purpose and Environment 1202

A.5.6.3.4.2 Test parameters 1202

A.5.6.3.4.3 Test Requirements 1204

A.5.6.4 CLI measurements 1205

A.5.6.4.1 SRS-RSRP measurement with DRX 1205

A.5.6.4.1.1 Test Purpose and Environment 1205

A.5.6.4.1.2 Test Parameters 1205

A.5.6.4.1.3 Test Requirements 1207

A.5.6.4.2 CLI-RSSI measurement with DRX 1207

A.5.6.4.2.1 Test Purpose and Environment 1207

A.5.6.4.2.2 Test Parameters 1208

A.5.6.4.2.3 Test Requirements 1210

A.5.6.5 Measurements with autonomous gaps 1210

A.5.6.5.1 EN-DC inter-frequency CGI identification of NR neighbor cell in FR2 1210

A.5.6.5.1.1 Test Purpose and Environment 1210

A.5.6.5.1.2 Test Requirements 1213

A.5.6.6 L1-SINR measurement for beam reporting 1214

A.5.6.6.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured when DRX is used 1214

A.5.6.6.1.1 Test Purpose and Environment 1214

A.5.6.6.1.2 Test parameters 1214

A.5.6.6.1.3 Test Requirements 1216

A.5.6.6.2 L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is not used 1216

A.5.6.6.2.1 Test Purpose and Environment 1216

A.5.6.6.2.2 Test parameters 1217

A.5.6.6.2.3 Test Requirements 1220

A.5.6.6.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is not used 1220

A.5.6.6.3.1 Test Purpose and Environment 1220

A.5.6.6.3.2 Test parameters 1221

A.5.6.6.3.3 Test Requirements 1223

A.5.6.7 CSI-RS based Intra-frequency Measurements 1223

A.5.6.7.1 EN-DC event triggered reporting test without gap under non-DRX 1223

A.5.6.7.1.1 Test purpose and Environment 1223

A.5.6.7.1.2 Test Requirements 1226

A.5.6.8 CSI-RS based Inter-frequency Measurements 1226

A.5.6.8.1 EN-DC event triggered reporting tests for NR FR2 cell when DRX is used 1226

A.5.6.8.1.1 Test Purpose and Environment 1226

A.5.6.8.1.2 Test Requirements 1230

A.5.7 Measurement Performance requirements 1230

A.5.7.1 SS-RSRP 1231

A.5.7.1.1 EN-DC intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1231

A.5.7.1.1.1 Test Purpose and Environment 1231

A.5.7.1.1.2 Test parameters 1231

A.5.7.1.1.3 Test Requirements 1233

A.5.7.1.2 EN-DC inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1234

A.5.7.1.2.1 Test Purpose and Environment 1234

A.5.7.1.2.2 Test parameters 1234

A.5.7.1.2.3 Test Requirements 1238

A.5.7.1.3 EN-DC inter-frequency measurement accuracy with FR1 serving cell and FR2 target cell 1239

A.5.7.1.3.1 Test Purpose and Environment 1239

A.5.7.1.3.2 Test parameters 1239

A.5.7.1.3.3 Test Requirements 1242

A.5.7.2 SS-RSRQ 1243

A.5.7.2.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1243

A.5.7.2.1.1 Test Purpose and Environment 1243

A.5.7.2.1.2 Test Parameters 1243

A.5.7.2.1.3 Test Requirements 1245

A.5.7.2.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1246

A.5.7.2.2.1 Test Purpose and Environment 1246

A.5.7.2.2.2 Test Parameters 1246

A.5.7.2.2.3 Test Requirements 1248

A.5.7.3 SS-SINR 1248

A.5.7.3.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1248

A.5.7.3.1.1 Test Purpose and Environment 1248

A.5.7.3.1.2 Test Parameters 1248

A.5.7.3.1.3 Test Requirements 1250

A.5.7.3.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1250

A.5.7.3.2.1 Test Purpose and Environment 1250

A.5.7.3.2.2 Test Parameters 1250

A.5.7.3.2.3 Test Requirements 1252

A.5.7.4 L1-RSRP measurement for beam reporting 1252

A.5.7.4.1 SSB based L1-RSRP measurement 1252

A.5.7.4.1.1 Test Purpose and Environment 1252

A.5.7.4.1.2 Test parameters 1253

A.5.7.4.1.3 Test Requirements 1255

A.5.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 1256

A.5.7.4.2.1 Test Purpose and Environment 1256

A.5.7.4.2.2 Test parameters 1256

A.5.7.4.2.3 Test Requirements 1258

A.5.7.5 CLI measurements 1259

A.5.7.5.1 EN-DC SRS-RSRP measurement accuracy with FR2 serving cell 1259

A.5.7.5.1.1 Test Purpose and Environment 1259

A.5.7.5.1.2 Test parameters 1259

A.5.7.5.1.3 Test Requirements 1262

A.5.7.5.2 EN-DC CLI-RSSI measurement accuracy with FR2 serving cell 1263

A.5.7.5.2.1 Test Purpose and Environment 1263

A.5.7.5.2.2 Test parameters 1263

A.5.7.5.2.3 Test Requirements 1265

A.5.7.6 L1-SINR measurement for beam reporting 1266

A.5.7.6.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off 1266

A.5.7.6.1.1 Test Purpose and Environment 1266

A.5.7.6.1.2 Test parameters 1266

A.5.7.6.1.3 Test Requirements 1268

A.5.7.6.2 L1-SINR measurement with SSB based CMR and dedicated IMR 1268

A.5.7.6.2.1 Test Purpose and Environment 1268

A.5.7.6.2.2 Test parameters 1269

A.5.7.6.2.3 Test Requirements 1271

A.5.7.6.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR 1272

A.5.7.6.3.1 Test Purpose and Environment 1272

A.5.7.6.3.2 Test parameters 1272

A.5.7.6.3.3 Test Requirements 1274

A.5.7.7 CSI-RSRP 1274

A.5.7.7.1 EN-DC intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1274

A.5.7.7.1.2 Test parameters 1275

A.5.7.7.1.3 Test Requirements 1277

A.5.7.7.2 EN-DC inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 1278

A.5.7.7.2.1 Test Purpose and Environment 1278

A.5.7.7.2.2 Test parameters 1278

A.5.7.7.2.3 Test Requirements 1282

A.5.7.8 CSI-RSRQ 1283

A.5.7.8.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 target cell 1283

A.5.7.8.1.1 Test Purpose and Environment 1283

A.5.7.8.1.2 Test Parameters 1283

A.5.7.8.1.3 Test Requirements 1285

A.5.7.8.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1285

A.5.7.8.2.1 Test Purpose and Environment 1285

A.5.7.8.2.2 Test Parameters 1285

A.5.7.9 CSI-SINR 1287

A.5.7.9.1 EN-DC Intra-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1287

A.5.7.9.1.1 Test Purpose and Environment 1287

A.5.7.9.1.2 Test Parameters 1287

Table A.5.7.9.1.2-1: CSI-SINR Intra frequency CSI-SINR supported test configurations 1288

A.5.7.9.1.3 Test Requirements 1290

A.5.7.9.2 EN-DC Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 1290

A.5.7.9.2.1 Test Purpose and Environment 1290

A.5.7.9.2.2 Test Parameters 1290

A.5.7.9.2.3 Test Requirements 1293

A.5.8 Void 1293

A.6 NR standalone tests with all NR cells in FR1 1011

A.6.1 SA: RRC\_IDLE state mobility 1011

A.6.1.1 Cell re-selection to NR 1011

A.6.1.1.1 Cell reselection to FR1 intra-frequency NR case 1011

A.6.1.1.1.1 Test Purpose and Environment 1011

A.6.1.1.1.2 Test Parameters 1011

A.6.1.1.1.3 Test Requirements 1015

A.6.1.1.2 Cell reselection to FR1 inter-frequency NR case 1015

A.6.1.1.2.1 Test Purpose and Environment 1015

A.6.1.1.2.2 Test Parameters 1015

A.6.1.1.2.3 Test Requirements 1019

A.6.1.1.3 Cell reselection to FR1 intra-frequency NR case for UE fulfilling low mobility relaxed measurement criterion 1019

A.6.1.1.3.1 Test Purpose and Environment 1019

A.6.1.1.3.2 Test Parameters 1019

A.6.1.1.3.3 Test Requirements 1024

A.6.1.1.4 Cell reselection to FR1 intra-frequency NR case for UE fulfilling not-at-cell edge relaxed measurement criterion 1024

A.6.1.1.4.1 Test Purpose and Environment 1024

A.6.1.1.4.2 Test Parameters 1024

A.6.1.1.4.3 Test Requirements 1028

A.6.1.1.5 Cell reselection to FR1 inter-frequency NR case for UE fulfilling low mobility relaxed measurement criterion 1028

A.6.1.1.5.1 Test Purpose and Environment 1028

A.6.1.1.5.2 Test Parameters 1028

A.6.1.1.5.3 Test Requirements 1032

A.6.1.1.6 Cell reselection to FR1 inter-frequency NR case for UE fulfilling not-at-cell edge relaxed measurement criterion 1033

A.6.1.1.6.1 Test Purpose and Environment 1033

A.6.1.1.6.2 Test Parameters 1033

A.6.1.1.6.3 Test Requirements 1037

A.6.1.1.7 Cell reselection to FR1 intra-frequency NR case for UE configured with *highSpeedMeasFlag-r16* 1038

A.6.1.1.7.1 Test Purpose and Environment 1038

A.6.1.1.7.2 Test Parameters 1038

A.6.1.1.7.3 Test Requirements 1042

A.6.1.2 Inter-RAT E-UTRAN cell re-selection 1042

A.6.1.2.1 Cell reselection to higher priority E-UTRAN 1042

A.6.1.2.1.1 Test Purpose and Environment 1042

A.6.1.2.1.2 Test Parameters 1042

A.6.1.2.1.3 Test Requirements 1045

A.6.1.2.2 Cell reselection to lower priority E-UTRAN 1046

A.6.1.2.2.1 Test Purpose and Environment 1046

A.6.1.2.2.2 Test Parameters 1046

A.6.1.2.2.3 Test Requirements 1049

A.6.1.2.3 Cell reselection to lower priority E-UTRAN for UE fulfilling low mobility relaxed measurement criterion 1050

A.6.1.2.3.1 Test Purpose and Environment 1050

A.6.1.2.3.2 Test Parameters 1050

A.6.1.2.3.3 Test Requirements 1053

A.6.1.2.4 Cell reselection to lower priority E-UTRAN for UE fulfilling not-at-cell edge relaxed measurement criterion 1054

A.6.1.2.4.1 Test Purpose and Environment 1054

A.6.1.2.4.2 Test Parameters 1054

A.6.1.2.4.3 Test Requirements 1057

A.6.1.2.5.3 Test Requirements 1061

A.6.2 SA: RRC\_INACTIVE state mobility 1062

A.6.3 RRC\_CONNECTED state mobility 1062

A.6.3.1 Handover 1062

A.6.3.1.1 Intra-frequency handover from FR1 to FR1; known target cell 1062

A.6.3.1.1.1 Test Purpose and Environment 1062

A.6.3.1.1.2 Test Parameters 1062

A.6.3.1.1.3 Test Requirements 1066

A.6.3.1.2 Intra-frequency handover from FR1 to FR1; unknown target cell 1066

A.6.3.1.2.1 Test Purpose and Environment 1066

A.6.3.1.2.2 Test Parameters 1066

A.6.3.1.2.3 Test Requirements 1070

A.6.3.1.3 Inter-frequency handover from FR1 to FR1; unknown target cell 1070

A.6.3.1.3.1 Test Purpose and Environment 1070

A.6.3.1.3.2 Test Parameters 1070

A.6.3.1.3.3 Test Requirements 1074

A.6.3.1.4 SA NR - E-UTRAN handover 1074

A.6.3.1.4.1 Test Purpose and Environment 1074

A.6.3.1.4.2 Test Requirements 1080

A.6.3.1.5 SA NR - E-UTRAN handover with unknown target cell 1080

A.6.3.1.5.1 Test Purpose and Environment 1080

A.6.3.1.5.2 Test Requirements 1086

A.6.3.1.6 SA NR - UTRAN FDD handover 1086

A.6.3.1.6.1 Test Purpose and Environment 1086

A.6.3.1.6.2 Test Requirements 1090

A.6.3.1.7 Intra-frequency synchronous DAPS handover in FR1 1090

A.6.3.1.7.1 Test Purpose and Environment 1090

A.6.3.1.7.2 Test Parameters 1090

A.6.3.1.7.3 Test Requirements 1094

A.6.3.1.8 Intra-frequency asynchronous DAPS handover in FR1 1095

A.6.3.1.8.1 Test Purpose and Environment 1095

A.6.3.1.8.2 Test Parameters 1095

A.6.3.1.8.3 Test Requirements 1099

A.6.3.1.9 Intra-band inter-frequency synchronous DAPS handover test in SA for FR1 1100

A.6.3.1.9.1 Test Purpose and Environment 1100

A.6.3.1.9.2 Test Parameters 1100

A.6.3.1.9.3 Test Requirements 1104

A.6.3.1.10 Intra-band inter-frequency asynchronous DAPS handover test in SA for FR1 1104

A.6.3.1.10.1 Test Purpose and Environment 1104

A.6.3.1.10.2 Test Parameters 1104

A.6.3.1.10.3 Test Requirements 1107

A.6.3.1.11 Inter-band inter-frequency synchronous DAPS handover from FR1 to FR1 1107

A.6.3.1.11.1 Test Purpose and Environment 1107

A.6.3.1.11.2 Test Parameters 1107

A.6.3.1.11.3 Test Requirements 1114

A.6.3.1.12 Inter-band inter-frequency asynchronous DAPS handover from FR1 to FR1 1114

A.6.3.1.12.1 Test Purpose and Environment 1114

A.6.3.1.12.2 Test Parameters 1114

A.6.3.1.12.3 Test Requirements 1122

A.6.3.2 RRC Connection Mobility Control 1122

A.6.3.2.1 SA: RRC Re-establishment 1122

A.6.3.2.1.1 Intra-frequency RRC Re-establishment in FR1 1122

A.6.3.2.1.2 Inter-frequency RRC Re-establishment in FR1 1126

A.6.3.2.1.3 Intra-frequency RRC Re-establishment in FR1 without serving cell timing 1130

A.6.3.2.2 Random Access 1134

A.6.3.2.2.1 4-step RA type contention based random access test in FR1 for NR standalone 1134

A.6.3.2.2.2 4-step RA type non-contention based random access test in FR1 for NR standalone 1139

A.6.3.2.2.3 2-step RA type contention based random access test in FR1 for NR standalone 1143

A.6.3.2.2.4 2-step RA type non-contention based test in FR1 for NR standalone 1148

A.6.3.2.3 SA: RRC Connection Release with Redirection 1152

A.6.3.2.3.1 Redirection from NR in FR1 to NR in FR1 1152

A.6.3.2.3.2 Redirection from NR in FR1 to E-UTRAN 1156

A.6.3.3 Conditional handover 1163

A.6.3.3.1 Intra-frequency conditional handover from FR1 to FR1 1163

A.6.3.3.1.1 Test Purpose and Environment 1163

A.6.3.3.1.2 Test Parameters 1163

A.6.3.3.1.3 Test Requirements 1167

A.6.3.3.2 Inter-frequency conditional handover from FR1 to FR1 1167

A.6.3.3.2.1 Test Purpose and Environment 1167

A.6.3.3.2.2 Test Parameters 1167

A.6.3.3.2.3 Test Requirements 1171

A.6.4 Timing 1171

A.6.4.1 UE transmit timing 1171

A.6.4.1.1 NR UE Transmit Timing Test for FR1 1171

A.6.4.1.1.1 Test Purpose and environment 1171

A.6.4.1.1.2 Test requirements 1175

A.6.4.2 UE timer accuracy 1175

A.6.4.3 Timing advance 1175

A.6.4.3.1 SA FR1 timing advance adjustment accuracy 1175

A.6.4.3.1.1 Test Purpose and Environment 1175

A.6.4.3.1.2 Test Parameters 1175

A.6.4.3.1.3 Test Requirements 1179

A.6.5 Signalling characteristics 1179

A.6.5.1 Radio link Monitoring 1179

A.6.5.1.1 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with SSB-based RLM RS in non-DRX mode 1180

A.6.5.1.1.1 Test Purpose and Environment 1180

A.6.5.1.1.2 Test Requirements 1185

A.6.5.1.2 Radio Link Monitoring In-sync Test for FR1 PCell configured with SSB-based RLM RS in non-DRX mode 1185

A.6.5.1.2.1 Test Purpose and Environment 1185

A.6.5.1.2.2 Test Requirements 1191

A.6.5.1.3 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with SSB-based RLM RS in DRX mode 1191

A.6.5.1.3.1 Test Purpose and Environment 1191

A.6.5.1.3.2 Test Requirements 1197

A.6.5.1.4 Radio Link Monitoring In-sync Test for FR1 PCell configured with SSB-based RLM RS in DRX mode 1197

A.6.5.1.4.1 Test Purpose and Environment 1197

A.6.5.1.4.2 Test Requirements 1203

A.6.5.1.5 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with CSI-RS-based RLM in non-DRX mode 1203

A.6.5.1.5.1 Test Purpose and Environment 1203

A.6.5.1.5.2 Test Requirements 1209

A.6.5.1.6 Radio Link Monitoring In-sync Test for FR1 PCell configured with CSI-RS-based RLM in non-DRX mode 1209

A.6.5.1.6.1 Test Purpose and Environment 1209

A.6.5.1.6.2 Test Requirements 1214

A.6.5.1.7 Radio Link Monitoring Out-of-sync Test for FR1 PCell configured with CSI-RS-based RLM in DRX mode 1214

A.6.5.1.7.1 Test Purpose and Environment 1214

A.6.5.1.7.2 Test Requirements 1218

A.6.5.1.8 Radio Link Monitoring In-sync Test for FR1 PCell configured with CSI-RS-based RLM in DRX mode 1218

A.6.5.1.8.1 Test Purpose and Environment 1218

A.6.5.1.8.2 Test Requirements 1224

A.6.5.2 Interruption 1224

A.6.5.2.1 Interruptions during measurements on deactivated NR SCC in FR1 1224

A.6.5.2.1.2 Test Requirements 1228

A.6.5.2.2 SA interruptions at NR SRS carrier based switching 1229

A.6.5.2.2.1 Test Purpose and Environment 1229

A.6.5.2.2.2 Test Parameters 1229

A.6.5.2.2.3 Test Requirements 1231

A.6.5.3 SCell Activation and Deactivation Delay 1232

A.6.5.3.1 SCell Activation and deactivation of known SCell in FR1 in non-DRX for 160ms SCell measurement cycle 1232

A.6.5.3.1.1 Test Purpose and Environment 1232

A.6.5.3.1.2 Test Requirements 1237

A.6.5.3.2 SCell Activation and deactivation of known SCell in FR1 in non-DRX for 640 ms SCell measurement cycle 1238

A.6.5.3.2.1 Test Purpose and Environment 1238

A.6.5.3.2.2 Test Requirements 1238

A.6.5.3.3 SCell Activation and deactivation of unknown SCell in FR1 in non-DRX 1238

A.6.5.3.3.1 Test Purpose and Environment 1238

A.6.5.3.3.2 Test Requirements 1239

A.6.5.3.4 Direct SCell activation at SCell addition of known SCell in FR1 1239

A.6.5.3.4.1 Test Purpose and Environment 1239

A.6.5.3.4.2 Test Requirements 1243

A.6.5.3.5 Direct SCell activation at handover with known SCell in FR1 1243

A.6.5.3.5.1 Test Purpose and Environment 1243

A.6.5.3.5.2 Test Requirements 1248

A.6.5.4 UE UL carrier RRC reconfiguration Delay 1249

A.6.5.4.1 UE UL carrier RRC reconfiguration Delay 1249

A.6.5.4.1.1 Test Purpose and Environment 1249

A.6.5.4.1.2 Test Requirements 1259

A.6.5.4.2 Void 1260

A.6.5.5 Beam Failure Detection and Link recovery procedures 1260

A.6.5.5.1 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in non-DRX mode 1260

A.6.5.5.1.1 Test Purpose and Environment 1260

A.6.5.5.2 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in DRX mode 1265

A.6.5.5.2.1 Test Purpose and Environment 1265

A.6.5.5.2.2 Test Requirements 1272

A.6.5.5.3 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with CSI-RS-based BFD and LR in non-DRX mode 1272

A.6.5.5.3.1 Test Purpose and Environment 1272

A.6.5.5.3.2 Test Requirements 1278

A.6.5.5.4 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with CSI-RS-based BFD and LR in DRX mode 1278

A.6.5.5.4.1 Test Purpose and Environment 1278

A.6.5.5.4.2 Test Requirements 1284

A.6.5.5.5 Beam Failure Detection and Link Recovery Test for FR1 SCell configured with CSI-RS-based BFD and SSB-based LR in non-DRX mode 1284

A.6.5.5.5.1 Test Purpose and Environment 1284

A.6.5.5.5.2 Test Requirements 1288

A.6.5.5.6 Beam Failure Detection and Link Recovery Test for FR1 SCell configured with CSI-RS-based BFD and SSB-based LR in DRX mode 1289

A.6.5.5.6.1 Test Purpose and Environment 1289

A.6.5.5.6.2 Test Requirements 1293

A.6.5.6 Active BWP switch 1293

A.6.5.6.1 DCI-based and Timer-based Active BWP Switch 1293

A.6.5.6.1.1 NR FR1- NR FR1 DL active BWP switch of SCell with non-DRX in SA 1293

A.6.5.6.1.2 NR FR1 DL active BWP switch with non-DRX in SA 1300

A.6.5.6.2 RRC-based Active BWP Switch 1304

A.6.5.6.2.1 NR FR1 DL active BWP switch of Cell with non-DRX in SA 1304

A.6.5.6.3 Simultaneous DCI-based and Timer-based Active BWP Switch on multiple CCs 1308

A.6.5.6.3.1 NR FR1- NR FR1 DL active BWP switch on multiple CCs with non-DRX in SA 1308

A.6.5.6.3.1.1 Test Purpose and Environment 1308

A.6.5.6.3.1.2 Test Requirements 1315

A.6.5.6.4 SCell dormancy switch 1315

A.6.5.6.4.1 NR FR1 PCell SCell dormancy switch of single FR1 SCell outside active time 1315

A.6.5.6.4.2 NR FR1 PCell SCell dormancy switch of two FR1 SCells inside active time 1321

A.6.5.6.5 Simultaneous RRC-based Active BWP Switch on multiple CCs 1328

A.6.5.6.5.1 NR FR1- NR FR1 DL active BWP switch on multiple CCs with non-DRX in SA 1328

A.6.5.7 DL interruptions at switching between two uplink carriers 1333

A.6.5.7.1 DL interruptions at switching between two uplink carriers in FDD-TDD CA 1333

A.6.5.7.1.1 Test Purpose and Environment 1333

A.6.5.7.1.2 Test Requirements 1337

A.6.5.7.2 DL interruptions at switching between two uplink carriers in TDD-TDD CA 1337

A.6.5.7.2.1 Test Purpose and Environment 1337

A.6.5.7.2.2 Test Requirements 1341

A.6.5.8 UE specific CBW change 1341

A.6.5.8.1 UE specific CBW change on PCell in FR1 in non-DRX 1341

A.6.5.8.1.1 Test Purpose and Environment 1341

A.6.5.8.1.2 Test Requirements 1345

A.6.5.9 Pathloss reference signal switching delay 1345

A.6.5.9.1 MAC-CE based pathloss reference signal switch delay 1345

A.6.5.9.1.1 Test Purpose and Environment 1345

A.6.5.9.1.2 Test Requirements 1348

A.6.6 Measurement procedure 1349

A.6.6.1 Intra-frequency Measurements 1349

A.6.6.1.1 SA event triggered reporting tests without gap under non-DRX 1349

A.6.6.1.1.1 Test purpose and Environment 1349

A.6.6.1.1.2 Test parameters 1349

A.6.6.1.1.3 Test Requirements 1353

A.6.6.1.2 SA event triggered reporting tests without gap under DRX 1353

A.6.6.1.2.1 Test purpose and Environment 1353

A.6.6.1.2.2 Test parameters 1353

A.6.6.1.2.3 Test Requirements 1357

A.6.6.1.3 SA event triggered reporting tests with per-UE gaps under non-DRX 1357

A.6.6.1.3.1 Test purpose and Environment 1357

A.6.6.1.3.2 Test parameters 1357

A.6.6.1.3.3 Test Requirements 1361

A.6.6.1.4 SA event triggered reporting tests with per-UE gaps under DRX 1361

A.6.6.1.4.1 Test purpose and Environment 1361

A.6.6.1.4.2 Test parameters 1361

A.6.6.1.4.3 Test Requirements 1365

A.6.6.1.5 SA event triggered reporting tests without gap under non-DRX with SSB index reading 1365

A.6.6.1.5.1 Test purpose and Environment 1365

A.6.6.1.5.2 Test parameters 1365

A.6.6.1.5.3 Test Requirements 1367

A.6.6.1.6 SA event triggered reporting tests with per-UE gaps under non-DRX with SSB index reading 1368

A.6.6.1.6.1 Test purpose and Environment 1368

A.6.6.1.6.2 Test parameters 1368

A.6.6.1.6.3 Test Requirements 1369

A.6.6.1.7 SA event triggered reporting tests under DRX for UE configured with highSpeedMeasFlag-r16 1370

A.6.6.1.7.1 Test purpose and Environment 1370

A.6.6.1.7.2 Test parameters 1370

A.6.6.1.7.3 Test Requirements 1374

A.6.6.2 Inter-frequency Measurements 1374

A.6.6.2.1 SA event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 1374

A.6.6.2.1.1 Test Purpose and Environment 1374

A.6.6.2.1.2 Test Requirements 1378

A.6.6.2.2 SA event triggered reporting tests for FR1 without SSB time index detection when DRX is used 1378

A.6.6.2.2.1 Test Purpose and Environment 1378

A.6.6.2.2.2 Test Requirements 1383

A.6.6.2.3 Void 1384

A.6.6.2.4 Void 1384

A.6.6.2.5 SA event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 1384

A.6.6.2.5.1 Test Purpose and Environment 1384

A.6.6.2.5.2 Test Requirements 1388

A.6.6.2.6 SA event triggered reporting tests for FR1 with SSB time index detection when DRX is used 1388

A.6.6.2.6.1 Test Purpose and Environment 1388

A.6.6.2.6.2 Test Requirements 1393

A.6.6.2.7 Void 1394

A.6.6.2.8 Void 1394

A.6.6.2.9 SA event triggered reporting tests with additional mandatory gap pattern 1394

A.6.6.2.9.1 Test Purpose and Environment 1394

A.6.6.2.9.2 Test Requirements 1397

A.6.6.2.10 SA event triggered reporting tests for FR1 when DRX is used 1397

A.6.6.2.10.1 Test Purpose and Environment 1397

A.6.6.2.10.2 Test Requirements 1401

A.6.6.2.11 SA event triggered reporting tests for FR1 without gap when DRX is not used 1402

A.6.6.2.11.1 Test Purpose and Environment 1402

A.6.6.2.11.2 Test Requirements 1405

A.6.6.3 Inter-RAT Measurements 1405

A.6.6.3.1 SA NR - E-UTRAN event-triggered reporting in non-DRX in FR1 1405

A.6.6.3.1.1 Test Purpose and Environment 1405

A.6.6.3.1.2 Test Requirements 1411

A.6.6.3.2 SA NR - E-UTRAN event-triggered reporting in DRX in FR1 1411

A.6.6.3.2.1 Test Purpose and Environment 1411

A.6.6.3.2.2 Test Requirements 1418

A.6.6.3.3 SA NR - E-UTRAN event-triggered reporting in DRX in FR1 for UE configured with highSpeedMeasFlag-r16 1418

A.6.6.3.3.1 Test Purpose and Environment 1418

A.6.6.3.3.2 Test Requirements 1425

A.6.6.4 L1-RSRP measurement for beam reporting 1425

A.6.6.4.1 SSB based L1-RSRP measurement when DRX is not used 1425

A.6.6.4.1.1 Test Purpose and Environment 1425

A.6.6.4.1.2 Test parameters 1425

A.6.6.4.1.3 Test Requirements 1428

A.6.6.4.2 SSB based L1-RSRP measurement when DRX is used 1428

A.6.6.4.2.1 Test Purpose and Environment 1428

A.6.6.4.2.2 Test parameters 1429

A.6.6.4.2.3 Test Requirements 1432

A.6.6.4.3 CSI-RS based L1-RSRP measurement when DRX is not used 1432

A.6.6.4.3.1 Test Purpose and Environment 1432

A.6.6.4.3.2 Test parameters 1433

A.6.6.4.3.3 Test Requirements 1436

A.6.6.4.4 CSI-RS based L1-RSRP measurement when DRX is used 1436

A.6.6.4.4.1 Test Purpose and Environment 1436

A.6.6.4.4.2 Test parameters 1437

A.6.6.4.4.3 Test Requirements 1440

A.6.6.4.5 SSB based L1-RSRP measurement when DRX is used for UE configured with *highSpeedMeasFlag-r16* 1440

A.6.6.4.5.1 Test Purpose and Environment 1440

A.6.6.4.5.2 Test parameters 1441

A.6.6.4.5.3 Test Requirements 1444

A.6.6.5 1444

A.6.6.5.1 SA NR - UTRAN FDD event-triggered reporting in non-DRX in FR1 1444

A.6.6.5.1.1 Test Purpose and Environment 1444

A.6.6.5.1.2 Test Requirements 1448

A.6.6.6 CLI measurements 1448

A.6.6.6.1 SRS-RSRP measurement with DRX 1448

A.6.6.6.1.1 Test Purpose and Environment 1448

A.6.6.6.1.2 Test Parameters 1449

A.6.6.6.1.3 Test Requirements 1452

A.6.6.6.2 CLI-RSSI measurement with DRX 1452

A.6.6.6.2.1 Test Purpose and Environment 1452

A.6.6.6.2.2 Test Parameters 1453

A.6.6.6.2.3 Test Requirements 1455

A.6.6.7 NR measurements with autonomous gaps 1455

A.6.6.7.1 SA intra-frequency CGI identification of NR neighbor cell in FR1 1455

A.6.6.7.1.1 Test Purpose and Environment 1455

A.6.6.7.1.2 Test Parameters 1455

A.6.6.7.1.3 Test Requirements 1458

A.6.6.7.2 Identification of a new CGI of inter-RAT E-UTRA cell using autonomous gaps in NR SA 1458

A.6.6.7.2.1 Test Purpose and Environment 1458

A.6.6.7.2.2 Test Requirements 1461

A.6.6.8 L1-SINR measurement for beam reporting 1462

A.6.6.8.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured when DRX is used 1462

A.6.6.8.1.1 Test Purpose and Environment 1462

A.6.6.8.2 L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is not used 1465

A.6.6.8.2.1 Test Purpose and Environment 1465

A.6.6.8.2.2 Test parameters 1466

A.6.6.8.2.3 Test Requirements 1470

A.6.6.8.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is not used 1470

A.6.6.8.3.1 Test Purpose and Environment 1470

A.6.6.8.3.2 Test parameters 1471

A.6.6.8.3.3 Test Requirements 1474

A.6.6.9 Idle Mode CA/DC Measurements 1474

A.6.6.9.1 SA Idle mode CA/DC measurement for FR1 1474

A.6.6.9.1.1 Test Purpose and Environment 1474

A.6.6.9.1.2 Test Requirements 1481

A.6.6.10 CSI-RS based intra-frequency Measurements 1481

A.6.6.10.1 SA event triggered reporting tests without gap under non-DRX 1481

A.6.6.10.1.1 Test purpose and Environment 1481

A.6.6.10.1.2 Test Requirements 1484

A.6.6.11 CSI-RS based inter-frequency Measurements 1484

A.6.6.11.1 SA event triggered reporting tests with gap under DRX 1484

A.6.6.11.1.1 Test Purpose and Environment 1484

A.6.6.11.1.2 Test Requirements 1488

A.6.6.12 RSTD measurements 1488

A. 6.6.12.1 NR RSTD measurement reporting delay test case for single positioning frequency layer in FR1 SA 1488

A. 6.6.12.1.1 Test Purpose and Environment 1488

A.6.6.12.1.2 Test Requirements 1496

A. 6.6.12.2 NR RSTD measurement reporting delay test case for dual positioning frequency layers in FR1 SA 1496

A. 6.6.12.2.1 Test Purpose and Environment 1496

A.6.6.12.2.2 Test Requirements 1503

A.6.6.13 PRS-RSRP measurements 1503

A.6.6.13.1 PRS-RSRP reporting delay test case for single positioning frequency layer 1503

A.6.6.13.1.1 Test purpose and Environment 1503

A.6.6.13.1.2 Test Requirements 1507

A.6.6.13.2 PRS-RSRP reporting delay test case for dual positioning frequency layer 1507

A.6.6.13.2.1 Test purpose and Environment 1507

A.6.6.13.2.2 Test Requirements 1511

A.6.6.14 UE Rx-Tx time difference measurements 1511

A.6.6.14.1 UE Rx-Tx time difference measurement for single positioning frequency layer in FR1 SA 1511

A.6.6.14.1.1 Test purpose and environment 1511

A.6.6.14.1.2 Test requirements 1515

A.6.6.14.2 UE Rx-Tx time difference measurement for dual positioning frequency layers in FR1 SA 1515

A.6.6.14.2.1 Test purpose and environment 1515

A.6.6.14.2.2 Test requirements 1519

A.6.6.15 Idle Mode measurements of inter-RAT CA candidate cells for early reporting 1519

A.6.6.15.1 Test Purpose and Environment 1519

A.6.6.15.2 Test Requirements 1526

A.6.7 Measurement Performance requirements 1527

A.6.7.1 SS-RSRP 1527

A.6.7.1.1 SA: intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 1527

A.6.7.1.1.1 Test Purpose and Environment 1527

A.6.7.1.1.2 Test parameters 1527

A.6.7.1.1.3 Test Requirements 1532

A.6.7.1.2 SA inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 1532

A.6.7.1.2.1 Test Purpose and Environment 1532

A.6.7.1.2.2 Test parameters 1532

A.6.7.1.2.3 Test Requirements 1536

A.6.7.1.3 Void 1536

A.6.7.2 SS-RSRQ 1536

A.6.7.2.1 SA: Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1536

A.6.7.2.1.1 Test Purpose and Environment 1536

A.6.7.2.1.2 Test Parameters 1537

A.6.7.2.1.3 Test Requirements 1542

A.6.7.2.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1542

A.6.7.2.2.1 Test Purpose and Environment 1542

A.6.7.2.2.2 Test Parameters 1542

A.6.7.2.2.3 Test Requirements 1547

A.6.7.3 SS-SINR 1547

A.6.7.3.1 SA intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1547

A.6.7.3.1.1 Test Purpose and Environment 1547

A.6.7.3.1.2 Test Parameters 1548

A.6.7.3.1.3 Test Requirements 1552

A.6.7.3.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1552

A.6.7.3.2.1 Test Purpose and Environment 1552

A.6.7.3.2.2 Test Parameters 1552

A.6.7.3.2.3 Test Requirements 1558

A.6.7.4 L1-RSRP measurement for beam reporting 1559

A.6.7.4.1 SSB based L1-RSRP measurement 1559

A.6.7.4.1.1 Test Purpose and Environment 1559

A.6.7.4.1.2 Test parameters 1559

A.6.7.4.1.3 Test Requirements 1563

A.6.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 1563

A.6.7.4.2.1 Test Purpose and Environment 1563

A.6.7.4.2.2 Test parameters 1564

A.6.7.4.2.3 Test Requirements 1568

A.6.7.5 E-UTRAN RSRP 1568

A.6.7.5.1 SA: inter-RAT measurement accuracy with FR1 serving cell 1568

A.6.7.5.1.1 Test Purpose and Environment 1568

A.6.7.5.1.2 Test parameters 1569

A.6.7.5.1.3 Test Requirements 1575

A.6.7.6 E-UTRAN RSRQ 1576

A.6.7.6.1 SA: inter-RAT measurement accuracy with FR1 serving cell 1576

A.6.7.6.1.1 Test Purpose and Environment 1576

A.6.7.6.1.2 Test parameters 1576

A.6.7.6.1.3 Test Requirements 1581

A.6.7.7 E-UTRAN RS-SINR 1582

A.6.7.7.1 SA: inter-RAT measurement accuracy with FR1 serving cell 1582

A.6.7.7.1.1 Test Purpose and Environment 1582

A.6.7.7.1.2 Test parameters 1582

A.6.7.7.1.3 Test Requirements 1588

A.6.7.8 CLI measurements 1589

A.6.7.8.1 SA SRS-RSRP measurement accuracy with FR1 serving cell 1589

A.6.7.8.1.1 Test Purpose and Environment 1589

A.6.7.8.1.2 Test parameters 1589

A.6.7.8.1.3 Test Requirements 1595

A.6.7.8.2 SA CLI-RSSI measurement accuracy with FR1 serving cell 1595

A.6.7.8.2.1 Test Purpose and Environment 1595

A.6.7.8.2.2 Test parameters 1596

A.6.7.8.2.3 Test Requirements 1599

A.6.7.9 L1-SINR measurement for beam reporting 1600

A.6.7.9.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off 1600

A.6.7.9.1.1 Test Purpose and Environment 1600

A.6.7.9.1.2 Test parameters 1600

A.6.7.9.1.3 Test Requirements 1604

A.6.7.9.2 L1-SINR measurement with SSB based CMR and dedicated IMR 1604

A.6.7.9.2.1 Test Purpose and Environment 1604

A.6.7.9.2.2 Test parameters 1605

A.6.7.9.2.3 Test Requirements 1610

A.6.7.9.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR 1610

A.6.7.9.3.1 Test Purpose and Environment 1610

A.6.7.9.3.2 Test parameters 1610

A.6.7.9.3.3 Test Requirements 1615

A.6.7.10 CSI-RSRP 1615

A.6.7.10.1 SA: intra-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 1615

A.6.7.10.1.1 Test Purpose and Environment 1615

A.6.7.10.1.2 Test parameters 1616

A.6.7.10.1.3 Test Requirements 1621

A.6.7.10.2 SA inter-frequency case measurement accuracy with FR1 serving cell and FR1 target cell 1621

A.6.7.10.2.1 Test Purpose and Environment 1621

A.6.7.10.2.2 Test parameters 1621

A.6.7.10.2.3 Test Requirements 1626

A.6.7.11 CSI-RSRQ 1626

A.6.7.11.1 SA: Intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1626

A.6.7.11.1.1 Test Purpose and Environment 1626

A.6.7.11.1.2 Test Parameters 1626

A.6.7.11.1.3 Test Requirements 1631

A.6.7.11.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1631

A.6.7.11.2.1 Test Purpose and Environment 1631

A.6.7.11.2.2 Test Parameters 1631

A.6.7.11.2.3 Test Requirements 1636

A.6.7.12 CSI-SINR 1637

A.6.7.12.1 SA intra-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1637

A.6.7.12.1.1 Test Purpose and Environment 1637

A.6.7.12.1.2 Test Parameters 1637

A.6.7.12.1.3 Test Requirements 1641

A.6.7.12.2 SA Inter-frequency measurement accuracy with FR1 serving cell and FR1 target cell 1642

A.6.7.12.2.1 Test Purpose and Environment 1642

A.6.7.12.2.2 Test Parameters 1642

A.6.7.12.2.3 Test Requirements 1648

A.6.7.13 RSTD measurements 1648

A.6.7.13.1 RSTD measurement accuracy test case for single positioning frequency layer 1648

A.6.7.13.1.1 Test purpose and Environment 1648

A.6.7.13.1.2 Test Requirements 1651

A.6.7.13.2 RSTD measurement accuracy test case for dual positioning frequency layer 1651

A.6.7.13.2.1 Test purpose and Environment 1651

A.6.7.13.2.2 Test Requirements 1655

A.6.7.14 PRS-RSRP measurements 1655

A.6.7.14.1 SA: measurement accuracy with PRS in FR1 1655

A.6.7.14.1.1 Test Purpose and Environment 1655

A.6.7.14.1.2 Test parameters 1656

A.6.7.14.1.3 Test Requirements 1660

A.6.7.15 UE Rx-Tx time difference measurements 1660

A.6.7.15.1 UE Rx-Tx time difference measurement accuracy for single positioning frequency layer in FR1 SA 1660

A.6.7.15.1.1 Test purpose and environment 1660

A.6.7.15.1.2 Test parameters 1661

A.6.7.15.1.3 Test requirements 1664

A.7.1 SA: RRC\_IDLE state mobility 1665

A.7.1.1 Cell re-selection to NR 1665

A.7.1.1.1 Cell reselection to FR2 intra-frequency NR case 1665

A.7.1.1.1.1 Test Purpose and Environment 1665

A.7.1.1.1.2 Test Parameters 1665

A.7.1.1.1.3 Test Requirements 1668

A.7.1.1.2 Cell reselection to FR2 inter-frequency NR case 1668

A.7.1.1.2.1 Test Purpose and Environment 1668

A.7.1.1.2.2 Test Parameters 1669

A.7.1.1.2.3 Test Requirements 1671

A.7.1.1.3 Cell reselection to FR2 intra-frequency NR case for UE fulfilling low mobility relaxed measurement criterion 1671

A.7.1.1.3.1 Test Purpose and Environment 1671

A.7.1.1.3.2 Test Parameters 1671

A.7.1.1.3.3 Test Requirements 1674

A.7.1.1.4 Cell reselection to FR2 intra-frequency NR case for UE fulfilling not-at-cell edge relaxed measurement criterion 1674

A.7.1.1.4.1 Test Purpose and Environment 1674

A.7.1.1.4.2 Test Parameters 1674

A.7.1.1.4.3 Test Requirements 1677

A.7.1.1.5 Cell reselection to FR2 inter-frequency NR case for UE fulfilling low mobility relaxed measurement criterion 1677

A.7.1.1.5.1 Test Purpose and Environment 1677

A.7.1.1.5.2 Test Parameters 1677

A.7.1.1.5.3 Test Requirements 1680

A.7.1.1.6 Cell reselection to FR2 inter-frequency NR case for UE fulfilling not-at-cell edge relaxed measurement criterion 1680

A.7.1.1.6.1 Test Purpose and Environment 1680

A.7.1.1.6.2 Test Parameters 1680

A.7.1.1.6.3 Test Requirements 1683

A.7.2 SA: RRC\_INACTIVE state mobility 1683

A.7.3 RRC\_CONNECTED state mobility 1683

A.7.3.1 Handover 1683

A.7.3.1.1 Inter-frequency handover from FR1 to FR2; unknown target cell 1683

A.7.3.1.1.1 Test Purpose and Environment 1683

A.7.3.1.1.2 Test Parameters 1683

A.7.3.1.1.3 Test Requirements 1687

A.7.3.1.2 Intra-frequency handover from FR2 to FR2; unknown target cell 1687

A.7.3.1.2.1 Test Purpose and Environment 1687

A.7.3.1.2.2 Test Parameters 1687

A.7.3.1.2.3 Test Requirements 1690

A.7.3.1.3 Inter-frequency handover from FR2 to FR2; unknown target cell 1690

A.7.3.1.3.1 Test Purpose and Environment 1690

A.7.3.1.3.2 Test Parameters 1690

A.7.3.1.3.3 Test Requirements 1691

A.7.3.1.4 Inter-band inter-frequency synchronous DAPS handover from FR1 to FR2 1692

A.7.3.1.4.1 Test Purpose and Environment 1692

A.7.3.1.4.2 Test Parameters 1692

A.7.3.1.4.3 Test Requirements 1699

A.7.3.1.5 Inter-band inter-frequency asynchronous DAPS handover from FR1 to FR2 1699

A.7.3.1.5.1 Test Purpose and Environment 1699

A.7.3.1.5.2 Test Parameters 1699

A.7.3.1.5.3 Test Requirements 1706

A.7.3.2 RRC Connection Mobility Control 1706

A.7.3.2.1 SA: RRC Re-establishment 1706

A.7.3.2.1.1 Intra-frequency RRC Re-establishment in FR2 1706

A.7.3.2.1.2 Inter-frequency RRC Re-establishment in FR2 1709

A.7.3.2.1.3 Intra-frequency RRC Re-establishment in FR2 without serving cell timing 1712

A.7.3.2.1.3.1 Test Purpose and Environment 1712

A.7.3.2.1.3.2 Test Requirements 1714

A.7.3.2.2 Random Access 1715

A.7.3.2.2.1 4-step RA type contention based random access test in FR2 for NR Standalone 1715

A.7.3.2.2.2 4-step RA type non-contention based random access test in FR2 for NR Standalone 1719

A.7.3.2.2.3 2-step RA type contention based random access test in FR2 for NR Standalone 1724

A.7.3.2.2.4 2-step RA type non-contention based random access test in FR2 for NR Standalone 1727

A.7.3.2.3 SA: RRC Connection Release with Redirection 1730

A.7.3.2.3.1 Redirection from NR in FR2 to NR in FR2 1730

A.7.3.3 Conditional Handover 1734

A.7.3.3.1 Intra-frequency conditional handover from FR2 to FR2 1734

A.7.3.3.1.1 Test Purpose and Environment 1734

A.7.3.3.1.2 Test Parameters 1734

A.7.3.3.1.2.3 Test Requirements 1737

A.7.3.3.2 Inter-frequency conditional handover from FR2 to FR2; unknown target cell 1737

A.7.3.3.2.1 Test Purpose and Environment 1737

A.7.3.3.2.2 Test Parameters 1737

A.7.3.3.2.3 Test Requirements 1740

A.7.4 Timing 1740

A.7.4.1 UE transmit timing 1740

A.7.4.1.1 NR UE Transmit Timing Test for FR2 1740

A.7.4.1.1.1 Test Purpose and environment 1740

A.7.4.1.1.2 Test requirements 1743

A.7.4.2 UE timer accuracy 1743

A.7.4.3 Timing advance 1743

A.7.4.3.1 SA FR2 timing advance adjustment accuracy 1743

A.7.4.3.1.1 Test Purpose and Environment 1743

A.7.4.3.1.2 Test Parameters 1743

A.7.4.3.1.3 Test Requirements 1747

A.7.5 Signaling characteristics 1747

A.7.5.1 Radio link Monitoring 1747

A.7.5.1.1 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with SSB-based RLM RS in non-DRX mode 1747

A.7.5.1.1.1 Test Purpose and Environment 1747

A.7.5.1.1.2 Test Requirements 1750

A.7.5.1.2 Radio Link Monitoring In-sync Test for FR2 PCell configured with SSB-based RLM RS in non-DRX mode 1751

A.7.5.1.2.1 Test Purpose and Environment 1751

A.7.5.1.2.2 Test Requirements 1755

A.7.5.1.3 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with SSB-based RLM RS in DRX mode 1756

A.7.5.1.3.1 Test Purpose and Environment 1756

A.7.5.1.3.2 Test Requirements 1760

A.7.5.1.4 Radio Link Monitoring In-sync Test for FR2 PCell configured with SSB-based RLM RS in DRX mode 1760

A.7.5.1.4.1 Test Purpose and Environment 1760

A.7.5.1.4.2 Test Requirements 1765

A.7.5.1.5 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with CSI-RS-based RLM in non-DRX mode 1765

A.7.5.1.5.1 Test Purpose and Environment 1765

A.7.5.1.5.2 Test Requirements 1770

A.7.5.1.6 Radio Link Monitoring In-sync Test for FR2 PCell configured with CSI-RS-based RLM in non-DRX mode 1770

A.7.5.1.6.1 Test Purpose and Environment 1770

A.7.5.1.6.2 Test Requirements 1774

A.7.5.1.7 Radio Link Monitoring Out-of-sync Test for FR2 PCell configured with CSI-RS-based RLM in DRX mode 1774

A.7.5.1.7.1 Test Purpose and Environment 1774

A.7.5.1.7.2 Test Requirements 1778

A.7.5.1.8 Radio Link Monitoring In-sync Test for FR2 PCell configured with CSI-RS-based RLM in DRX mode 1778

A.7.5.1.8.1 Test Purpose and Environment 1778

A.7.5.1.8.2 Test Requirements 1783

A.7.5.1.9 UE Radio Link Monitoring Scheduling Restrictions on FR2 1783

A.7.5.1.9.1 Test Purpose and Environment 1783

A.7.5.1.9.2 Test Requirements 1786

A.7.5.2 Interruption 1786

A.7.5.2.1 Interruptions during measurements on deactivated NR SCC in FR2 1786

A.7.5.2.2 SA interruptions at NR SRS carrier-based switching 1790

A.7.5.2.2.1 Test Purpose and Environment 1790

A.7.5.2.2.2 Test Parameters 1790

A.7.5.2.2.3 Test Requirements 1792

A.7.5.3 SCell Activation and Deactivation Delay 1792

A.7.5.3.1 SCell Activation and deactivation for SCell in FR2 intra-band in non-DRX 1792

A.7.5.3.1.1 Test Purpose and Environment 1792

A.7.5.3.1.2 Test Requirements 1794

A.7.5.3.2 SCell Activation and deactivation for FR1+FR2 inter-band with target SCell in FR2 1794

A.7.5.3.2.1 Test Purpose and Environment 1794

A.7.5.3.2.2 Test Requirements 1798

A.7.5.3.3 SCell Activation and deactivation for SCell in FR2 inter-band in non-DRX 1799

A.7.5.3.3.1 Test Purpose and Environment 1799

A.7.5.3.3.2 Test Requirements 1802

A.7.5.3.4 Direct SCell activation at SCell addition of known SCell in FR2 1803

A.7.5.3.4.1 Test Purpose and Environment 1803

A.7.5.3.4.2 Test Requirements 1806

A.7.5.3.5 Direct SCell activation at handover with known SCell in FR2 1807

A.7.5.3.5.1 Test Purpose and Environment 1807

A.7.5.3.5.2 Test Requirements 1809

A.7.5.4 Void 1810

A.7.5.5 Beam Failure Detection and Link recovery procedures 1810

A.7.5.5.1 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with SSB-based BFD and LR in non-DRX mode 1810

A.7.5.5.1.1 Test Purpose and Environment 1810

A.7.5.5.1.2 Test Requirements 1814

A.7.5.5.2 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with SSB-based BFD and LR in DRX mode 1814

A.7.5.5.2.1 Test Purpose and Environment 1814

A.7.5.5.2.2 Test Requirements 1818

A.7.5.5.3 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with CSI-RS-based BFD and LR in non-DRX mode 1818

A.7.5.5.3.1 Test Purpose and Environment 1818

A.7.5.5.3.2 Test Requirements 1822

A.7.5.5.4 Beam Failure Detection and Link Recovery Test for FR2 PCell configured with CSI-RS-based BFD and LR in DRX mode 1822

A.7.5.5.4.1 Test Purpose and Environment 1822

A.7.5.5.4.2 Test Requirements 1826

A.7.5.5.5 Scheduling availability restriction during Beam Failure Detection and Link Recovery for FR2 PCell configured with SSB-based BFD and LR in non-DRX mode 1826

A.7.5.5.5.1 Test Purpose and Environment 1826

A.7.5.5.5.2 Test Requirements 1830

A.7.5.5.6 Beam Failure Detection and Link Recovery Test for FR2 SCell configured with CSI-RS-based BFD and LR in non-DRX mode 1830

A.7.5.5.6.1 Test Purpose and Environment 1830

A.7.5.5.6.2 Test Requirements 1834

A.7.5.5.7 Beam Failure Detection and Link Recovery Test for FR2 SCell configured with CSI-RS-based BFD and LR in DRX mode 1834

A.7.5.5.7.1 Test Purpose and Environment 1834

A.7.5.5.7.2 Test Requirements 1838

A.7.5.6 Active BWP switch 1838

A.7.5.6.1 DCI-based and Timer-based Active BWP Switch 1838

A.7.5.6.1.1 NR FR2- NR FR2 DL active BWP switch of SCell with non-DRX in SA 1838

A.7.5.6.1.2 NR FR1- NR FR2 DL active BWP switch of SCell with non-DRX in SA A.7.5.6.1.2.1 Test Purpose and Environment 1843

A.7.5.6.1.3 NR FR2 DL active BWP switch with non-DRX in SA 1848

A.7.5.6.1.3.1 Test Purpose and Environment 1848

A.7.5.6.1.3.2 Test Requirements 1851

A.7.5.6.2 RRC-based Active BWP Switch 1851

A.7.5.6.3 Simultaneous DCI-based and Timer-based Active BWP Switch on multiple CCs 1855

A.7.5.6.3.1 Active BWP switch on multiple SCells with non-DRX in SA 1855

A.7.5.6.4 SCell dormancy switch 1858

A.7.5.6.4.1 NR FR2 PCell SCell dormancy switch of single FR2 SCell inside active time 1858

A.7.5.6.4.2 NR FR1 PCell SCell dormancy switch of two FR2 SCells outside active time 1863

A.7.5.6.4.2.2 Test Requirements 1868

A.7.5.6.5 Simultaneous RRC-based Active BWP Switch on multiple CCs 1868

A.7.5.6.5.1 Active BWP switch on multiple SCells with non-DRX in SA 1868

A.7.5.7 PSCell addition and release delay 1873

A.7.5.7.1 Addition and Release Delay of known NR PSCell 1873

A.7.5.7.1.1 Test Purpose and Environment 1873

A.7.5.7.2 Addition and Release Delay of unknown NR PSCell 1876

A.7.5.7.2.1 Test Purpose and Environment 1876

A.7.5.7.2.2 Test Requirements 1879

A.7.5.8 Active TCI state switch delay 1879

A.7.5.8.1 MAC-CE based active TCI state switch 1879

A.7.5.8.2 RRC based active TCI state switch 1883

A.7.5.9 Uplink spatial relation switch delay 1887

A.7.5.9.1 MAC-CE based Spatial Relation switch 1887

A.7.5.9.1.1 NR PCell FR2 spatial relation associated with known DL-RS 1887

A.7.5.9.1.1.2 Test Requirements 1890

A.7.5.9.2 RRC based spatial relation switch 1890

A.7.5.9.2.1 NR PCell FR2 spatial relation switch associated with a known DL-RS 1890

A.7.5.9.2.1.1 Test Purpose and Environment 1890

A.7.5.9.2.1.2 Test Requirements 1893

A.7.5.10 UE specific CBW change 1893

A.7.5.10.1 NR FR2 UE specific CBW change of PCell with non-DRX in SA 1893

A.7.5.10.1.1 Test Purpose and Environment 1893

A.7.5.10.1.2 Test Requirements 1896

A.7.6 Measurement procedure 1897

A.7.6.1 Intra-frequency Measurements 1897

A.7.6.1.1 SA event triggered reporting test without gap under non-DRX 1897

A.7.6.1.1.1 Test purpose and Environment 1897

A.7.6.1.1.2 Test Requirements 1899

A.7.6.1.2 SA event triggered reporting test without gap under DRX 1900

A.7.6.1.2.1 Test purpose and Environment 1900

A.7.6.1.2.2 Test Requirements 1902

A.7.6.1.3 SA event triggered reporting test with per-UE gaps under non-DRX 1903

A.7.6.1.3.1 Test purpose and Environment 1903

A.7.6.1.3.2 Test Requirements 1906

A.7.6.1.4 SA event triggered reporting test with per-UE gaps under DRX 1906

A.7.6.1.4.1 Test purpose and Environment 1906

A.7.6.1.4.2 Test Requirements 1909

A.7.6.2 Inter-frequency Measurements 1910

A.7.6.2.1 SA event triggered reporting tests For FR2 without SSB time index detection when DRX is not used (PCell in FR2) 1910

A.7.6.2.1.1 Test Purpose and Environment 1910

A.7.6.2.1.2 Test Requirements 1913

A.7.6.2.2 SA event triggered reporting tests For FR2 without SSB time index detection when DRX is used (PCell in FR2) 1913

A.7.6.2.2.1 Test Purpose and Environment 1913

A.7.6.2.2.2 Test Requirements 1917

A.7.6.2.3 SA event triggered reporting tests For FR2 with SSB time index detection when DRX is not used (PCell in FR2) 1917

A.7.6.2.3.1 Test Purpose and Environment 1917

A.7.6.2.3.2 Test Requirements 1921

A.7.6.2.4 SA event triggered reporting tests For FR2 with SSB time index detection when DRX is used (PCell in FR2) 1921

A.7.6.2.4.1 Test Purpose and Environment 1921

A.7.6.2.4.2 Test Requirements 1925

A.7.6.2.5 SA event triggered reporting tests for FR2 without SSB time index detection when DRX is not used (PCell in FR1) 1925

A.7.6.2.5.1 Test Purpose and Environment 1925

A.7.6.2.5.2 Test Requirements 1929

A.7.6.2.6 SA event triggered reporting tests for FR2 without SSB time index detection when DRX is used (PCell in FR1) 1930

A.7.6.2.6.1 Test Purpose and Environment 1930

A.7.6.2.6.2 Test Requirements 1934

A.7.6.2.7 SA event triggered reporting tests for FR2 with SSB time index detection when DRX is not used (PCell in FR1) 1935

A.7.6.2.7.1 Test Purpose and Environment 1935

A.7.6.2.7.2 Test Requirements 1939

A.7.6.2.8 SA event triggered reporting tests for FR2 with SSB time index detection when DRX is used (PCell in FR1) 1940

A.7.6.2.8.1 Test Purpose and Environment 1940

A.7.6.2.8.2 Test Requirements 1944

A.7.6.2.9 SA event triggered reporting tests For FR2 without SSB time index detection when DRX is not used (PCell in FR2) (rel16 additional mandatory gap pattern 17) 1945

A.7.6.2.9.1 Test Purpose and Environment 1945

A.7.6.2.9.2 Test Requirements 1948

A.7.6.2.10 SA event triggered reporting test without gap under non-DRX 1948

A.7.6.2.10.1 Test Purpose and Environment 1948

A.7.6.2.10.2 Test Requirements 1950

A.7.6.2.11 SA event triggered reporting test without gap under DRX 1950

A.7.6.2.11.1 Test Purpose and Environment 1950

A.7.6.2.11.2 Test Requirements 1953

A.7.6.3 L1-RSRP measurement for beam reporting 1954

A.7.6.3.1 SSB based L1-RSRP measurement when DRX is not used 1954

A.7.6.3.1 SSB based L1-RSRP measurement when DRX is not used 1954

A.7.6.3.1.1 Test Purpose and Environment 1954

A.7.6.3.1.2 Test parameters 1954

A.7.6.3.1.3 Test Requirements 1956

A.7.6.3.2 SSB based L1-RSRP measurement when DRX is used 1956

A.7.6.3.2.1 Test Purpose and Environment 1956

A.7.6.3.2.2 Test parameters 1957

A.7.6.3.2.3 Test Requirements 1959

A.7.6.3.3 CSI-RS based L1-RSRP measurement when DRX is not used 1959

A.7.6.3.3.1 Test Purpose and Environment 1959

A.7.6.3.3.2 Test parameters 1960

A.7.6.3.3.3 Test Requirements 1962

A.7.6.3.4 CSI-RS based L1-RSRP measurement when DRX is used 1963

A.7.6.3.4.1 Test Purpose and Environment 1963

A.7.6.3.4.2 Test parameters 1963

A.7.6.3.3.3 Test Requirements 1965

A.7.6.4 CLI measurements 1966

A.7.6.4.1 SRS-RSRP measurement with non-DRX 1966

A.7.6.4.1.1 Test Purpose and Environment 1966

A.7.6.4.1.2 Test Parameters 1966

A.7.6.4.1.3 Test Requirements 1968

A.7.6.4.2 CLI-RSSI measurement with non-DRX 1968

A.7.6.4.2.1 Test Purpose and Environment 1968

A.7.6.4.2.2 Test Parameters 1969

A.7.6.4.2.3 Test Requirements 1970

A.7.6.5 NR Measurements with autonomous gaps 1971

A.7.6.5.1 SA interfrequency CGI reporting in autonomous gaps test (PCell in FR2) 1971

A.7.6.5.1.1 Test Purpose and Environment 1971

A.7.6.5.1.2 Test Requirements 1974

A.7.6.6 L1-SINR measurement for beam reporting 1974

A.7.6.6.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured when DRX is not used 1974

A.7.6.6.1.1 Test Purpose and Environment 1974

A.7.6.6.1.2 Test parameters 1974

A.7.6.6.1.3 Test Requirements 1976

A.7.6.6.2 L1-SINR measurement with SSB based CMR and dedicated IMR when DRX is used 1976

A.7.6.6.2.1 Test Purpose and Environment 1976

A.7.6.6.2.2 Test parameters 1977

A.7.6.6.2.3 Test Requirements 1979

A.7.6.6.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR configured when DRX is used 1980

A.7.6.6.3.1 Test Purpose and Environment 1980

A.7.6.6.3.2 Test parameters 1980

A.7.6.6.3.3 Test Requirements 1982

A.7.6.7 CSI-RS based intra-frequency Measurements 1982

A.7.6.7.1 SA event triggered reporting test without gap under DRX for CSI-RS based intra-frequency measurement 1982

A.7.6.7.1.1 Test purpose and Environment 1982

A.7.6.7.1.2 Test Requirements 1985

A.7.6.8 CSI-RS based inter-frequency Measurements 1985

A.7.6.8.1 SA event triggered reporting tests for FR2 CSI-RS based measurement when non-DRX is used (PCell in FR2) 1985

A.7.6.8.1.1 Test Purpose and Environment 1985

A.7.6.2.2.2 Test Requirements 1989

A.7.6.9 RSTD measurements 1989

A.7.6.9.1 NR RSTD measurement reporting delay test case for single positioning frequency layer in FR2 SA 1989

A.7.6.9.1.1 Test Purpose and Environment 1989

A.7.6.9.1.2 Test Requirements 1995

A.7.6.9.2 NR RSTD measurement reporting delay test case for dual positioning frequency layers in FR2 SA 1995

A.7.6.9.2.1 Test Purpose and Environment 1995

A.7.6.9.2.2 Test Requirements 2002

A.7.6.10 PRS-RSRP measurements 2002

A.7.6.10.1 PRS-RSRP reporting delay test case for single positioning frequency layer 2002

A.7.6.10.1.1 Test Purpose and Environment 2002

A.7.6.10.1.2 Test Requirements 2006

A.7.6.10.2 PRS-RSRP reporting delay test case for dual positioning frequency layer 2006

A.7.6.10.2.1 Test Purpose and Environment 2006

A.7.6.10.2.2 Test Requirements 2009

A.7.6.11 UE Rx-Tx time difference measurements 2009

A.7.6.11.1 UE Rx-Tx time difference measurements for single positioning frequency layer in FR2 SA 2009

A.7.6.11.1.1 Test purpose and environment 2009

A.7.6.11.1.2 Test requirements 2013

A.7.6.11.2 UE Rx-Tx time difference measurement period for dual positioning frequency layers in FR2 SA 2013

A.7.6.11.2.1 Test purpose and environment 2013

A.7.6.11.2.2 Test requirements 2017

A.7.7 Measurement Performance requirements 2017

A.7.7.1 SS-RSRP 2017

A.7.7.1.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2017

A.7.7.1.1.1 Test Purpose and Environment 2017

A.7.7.1.1.2 Test parameters 2018

A.7.7.1.1.3 Test Requirements 2022

A.7.7.1.2 SA inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2023

A.7.7.1.2.1 Test Purpose and Environment 2023

A.7.7.1.2.2 Test parameters 2023

A.7.7.1.2.3 Test Requirements 2027

A.7.7.1.3 SA inter-frequency measurement accuracy with FR1 serving cell and FR2 target cell 2028

A.7.7.1.3.1 Test Purpose and Environment 2028

A.7.7.1.3.2 Test parameters 2028

A.7.7.1.3.3 Test Requirements 2032

A.7.7.2 SS-RSRQ 2032

A.7.7.2.1 SA intra-frequency measurement accuracy with FR2 serving cell and FR2 target cell 2032

A.7.7.2.1.1 Test Purpose and Environment 2032

A.7.7.2.1.2 Test Parameters 2032

A.7.7.2.1.3 Test Requirements 2034

A.7.7.2.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 2034

A.7.7.2.2.1 Test Purpose and Environment 2034

A.7.7.2.2.2 Test Parameters 2034

A.7.7.2.2.3 Test Requirements 2036

A.7.7.3 SS-SINR 2036

A.7.7.3.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2036

A.7.7.3.1.1 Test Purpose and Environment 2036

A.7.7.3.1.2 Test Parameters 2036

A.7.7.3.1.3 Test Requirements 2039

A.7.7.3.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 2039

A.7.7.3.2.1 Test Purpose and Environment 2039

A.7.7.3.2.2 Test Parameters 2039

A.7.7.3.2.3 Test Requirements 2041

A.7.7.4 L1-RSRP measurement for beam reporting 2041

A.7.7.4.1 SSB based L1-RSRP measurement 2041

A.7.7.4.1.1 Test Purpose and Environment 2041

A.7.7.4.1.2 Test parameters 2042

A.7.7.4.1.3 Test Requirements 2044

A.7.7.4.2 CSI-RS based L1-RSRP measurement on resource set with repetition off 2045

A.7.7.4.2.1 Test Purpose and Environment 2045

A.7.7.4.2.2 Test parameters 2045

A.7.7.4.2.3 Test Requirements 2047

A.7.7.5 CLI measurements 2048

A.7.7.5.1 SA SRS-RSRP measurement accuracy with FR2 serving cell 2048

A.7.7.5.1.1 Test Purpose and Environment 2048

A.7.7.5.1.2 Test parameters 2048

A.7.7.5.1.3 Test Requirements 2051

A.7.7.5.2 SA CLI-RSSI measurement accuracy with FR2 serving cell 2052

A.7.7.5.2.1 Test Purpose and Environment 2052

A.7.7.5.2.2 Test parameters 2052

A.7.7.5.2.3 Test Requirements 2054

A.7.7.6 L1-SINR measurement for beam reporting 2055

A.7.7.6.1 L1-SINR measurement with CSI-RS based CMR and no dedicated IMR configured and CSI-RS resource set with repetition off 2055

A.7.7.6.1.1 Test Purpose and Environment 2055

A.7.7.6.1.2 Test parameters 2055

A.7.7.6.1.3 Test Requirements 2057

A.7.7.6.2 L1-SINR measurement with SSB based CMR and dedicated IMR 2057

A.7.7.6.2.1 Test Purpose and Environment 2057

A.7.7.6.2.2 Test parameters 2058

A.7.7.6.2.3 Test Requirements 2060

A.7.7.6.3 L1-SINR measurement with CSI-RS based CMR and dedicated IMR 2060

A.7.7.6.3.1 Test Purpose and Environment 2060

A.7.7.6.3.2 Test parameters 2061

A.7.7.6.3.3 Test Requirements 2063

A.7.7.7 CSI-RSRP 2063

A.7.7.7.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2063

A.7.7.7.1.1 Test Purpose and Environment 2063

A.7.7.7.1.2 Test parameters 2064

A.7.7.7.1.3 Test Requirements 2067

A.7.7.7.2 SA inter-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2068

A.7.7.7.2.1 Test Purpose and Environment 2068

A.7.7.7.2.2 Test parameters 2068

A.7.7.7.2.3 Test Requirements 2071

A.7.7.8 CSI-RSRQ 2071

A.7.7.8.1 SA intra-frequency measurement accuracy with FR2 serving cell and FR2 target cell 2071

A.7.7.8.1.1 Test Purpose and Environment 2071

A.7.7.8.1.2 Test Parameters 2072

A.7.7.8.1.3 Test Requirements 2074

A.7.7.8.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 2074

A.7.7.8.2.1 Test Purpose and Environment 2074

A.7.7.8.2.2 Test Parameters 2074

A.7.7.8.2.3 Test Requirements 2076

A.7.7.9 CSI-SINR 2076

A.7.7.9.1 SA intra-frequency case measurement accuracy with FR2 serving cell and FR2 target cell 2076

A.7.7.9.1.1 Test Purpose and Environment 2076

A.7.7.9.1.2 Test Parameters 2076

A.7.7.9.1.3 Test Requirements 2079

A.7.7.9.2 SA Inter-frequency measurement accuracy with FR2 serving cell and FR2 TDD target cell 2079

A.7.7.9.2.2 Test Parameters 2079

A.7.7.9.2.3 Test Requirements 2081

A.7.7.10 RSTD measurements 2081

A.7.7.10.1 RSTD measurement accuracy test case for single positioning frequency layer 2081

A.7.7.10.1.1 Test purpose and Environment 2081

A.7.7.10.1.2 Test Requirements 2084

A.7.7.10.2 RSTD measurement accuracy test case for dual positioning frequency layer 2084

A.7.7.10.2.1 Test purpose and Environment 2084

A.7.7.10.2.2 Test Requirements 2087

A.7.7.11 PRS-RSRP measurements 2087

A.7.7.11.1 SA measurement accuracy with PRS in FR2 2087

A.7.7.11.1.1 Test Purpose and Environment 2087

A.7.7.11.1.2 Test parameters 2087

A.7.7.11.1.3 Test Requirements 2091

A.7.7.12 UE Rx-Tx time difference measurements 2092

A.7.7.12.1 UE Rx-Tx time difference measurement accuracy for single positioning frequency layer in FR2 SA 2092

A.7.7.12.1.1 Test purpose and environment 2092

A.7.7.12.1.2 Test parameters 2092

A.7.7.12.1.3 Test requirements 2095

A.8 E-UTRA standalone tests for NR RRM 2095

A.8.1 Void 2096

A.8.2 RRC\_IDLE state mobility 2096

A.8.2.1 Inter-RAT NR Cell re-selection 2096

A.8.2.1.1 E-UTRA Cell reselection to higher priority NR target Cell in FR1 2096

A.8.2.1.1.1 Test Purpose and Environment 2096

A.8.2.1.1.2 Test Requirements 2101

A.8.2.1.2 E-UTRA Cell reselection to lower priority NR target Cell in FR1 for UE configured with highSpeedInterRAT-NR-r16 2102

A.8.2.1.2.1 Test Purpose and Environment 2102

A.8.2.1.2.2 Test Requirements 2107

A.8.2.2 E-UTRA – NR Inter-RAT Early Measruement Reporting 2108

A.8.2.2.1 E-UTRA – NR Early Measurement Reporting for NR in FR1 2108

A.8.2.2.1.1 Test Purpose and Environment 2108

A.8.2.2.1.2 Test Requirements 2113

A.8.2.2.2 E-UTRA – NR Early Measurement Reporting for NR in FR2 2113

A.8.2.2.2.1 Test Purpose and Environment 2113

A.8.2.2.2.2 Test Requirements 2116

A.8.3 RRC\_CONNECTED state mobility 2117

A.8.3.1 Handover 2117

A.8.3.1.1 E-UTRAN - NR handover in FR1 2117

A.8.3.1.1.1 Test Purpose and Environment 2117

A.8.3.1.1.2 Test Requirements 2122

A.8.4 Measurement procedure 2122

A.8.4.1 E-UTRA – NR Inter-RAT SFTD Measurement Delay 2122

A.8.4.1.1 E-UTRA – NR Inter-RAT SFTD Measurement Delay in non-DRX 2122

A.8.4.1.1.1 Test Purpose and Environment 2122

A.8.4.1.1.2 Test Requirements 2124

A.8.4.1.2 E-UTRA – NR Inter-RAT SFTD Measurement Delay in DRX 2125

A.8.4.1.2.1 Test Purpose and Environment 2125

A.8.4.1.2.2 Test Requirements 2126

A.8.4.2 E-UTRA – NR Inter-RAT Measurements 2126

A.8.4.2.1 NR Inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 2126

A.8.4.2.1.1 Test Purpose and Environment 2126

A.8.4.2.1.2 Test Requirements 2131

A.8.4.2.2 NR Inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is used 2131

A.8.4.2.2.1 Test Purpose and Environment 2131

A.8.4.2.2.2 Test Requirements 2135

A.8.4.2.3 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 2135

A.8.4.2.3.1 Test Purpose and Environment 2135

A.8.4.2.3.2 Test Requirements 2140

A.8.4.2.4 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is used 2140

A.8.4.2.4.1 Test Purpose and Environment 2140

A.8.4.2.4.2 Test Requirements 2144

A.8.4.2.5 NR Inter-RAT event triggered reporting tests for FR2 without SSB time index detection when DRX is not used 2144

A.8.4.2.5.1 Test Purpose and Environment 2144

A.8.4.2.5.2 Test Requirements 2146

A.8.4.2.6 NR Inter-RAT event triggered reporting tests for FR2 without SSB time index detection when DRX is used 2147

A.8.4.2.6.1 Test Purpose and Environment 2147

A.8.4.2.6.2 Test Requirements 2149

A.8.4.2.7 NR Inter-RAT event triggered reporting tests for FR2 with SSB time index detection when DRX is not used 2150

A.8.4.2.7.1 Test Purpose and Environment 2150

A.8.4.2.7.2 Test Requirements 2152

A.8.4.2.8 NR Inter-RAT event triggered reporting tests for FR2 with SSB time index detection when DRX is used 2153

A.8.4.2.8.1 Test Purpose and Environment 2153

A.8.4.2.8.2 Test Requirements 2155

A.8.4.2.9 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection in DRX for UE configured with highSpeedInterRAT-NR-r16 2156

A.8.4.2.9.1 Test Purpose and Environment 2156

A.8.4.2.9.2 Test Requirements 2162

A.8.5 Measurement performance 2162

A.8.5.1 SFTD accuracy 2162

A.8.5.1.1 SFTD accuracy 2162

A.8.5.1.1.1 Test Purpose 2162

A.8.5.1.1.2 Test Environment 2162

A.8.5.1.1.3 Test Requirements 2168

A.8.5.2 E-UTRA – NR Inter-RAT Measurement Performance requirements 2168

A.8.5.2.1.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 2168

A.8.5.2.1.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 2173

A.8.5.2.1.2.1 Test Purpose and Environment 2173

A.8.5.2.1.2.2 Test Parameters 2173

A.8.5.2.1.2.3 Test Requirements 2175

A.8.5.2.2 SS-RSRQ 2175

A.8.5.2.2.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 2175

A.8.5.2.2.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 2180

A.8.5.2.2.2.1 Test Purpose and Environment 2180

A.8.5.2.2.2.2 Test Parameters 2180

A.8.5.2.2.2.3 Test Requirements 2182

A.8.5.2.3 SS-SINR 2182

A.8.5.2.3.1 E-UTRAN – NR inter-RAT measurements with FR1 target cell 2182

A.8.5.2.3.2 E-UTRAN – NR inter-RAT measurements with FR2 target cell 2186

A.8.5.2.3.2.1 Test Purpose and Environment 2186

A.8.5.2.3.2.2 Test Parameters 2186

A.8.5.2.3.2.3 Test Requirements 2188

A.9 V2X Tests 2189

A.9.1 V2X Tests in FR1 2189

A.9.1.1 Test for V2X UE Transmit Timing 2189

A.9.1.1.1 Test for GNSS as Synchronization Reference Source 2189

A.9.1.1.1.1 Test Purpose and Environment 2189

A.9.1.1.1.2 Test requirements 2189

A.9.1.1.2 Test for SyncRef UE as Synchronization Reference Source 2189

A.9.1.1.2.1 Test Purpose and Environment 2189

A.9.1.1.2.2 Test requirements 2190

A.9.1.1.3 Test for FR1 NR Cell as Synchronization Reference Source 2190

A.9.1.1.3.1 Test Purpose and Environment 2190

A.9.1.1.3.2 Test requirements 2193

A.9.1.2 Test for Initiation/Cease of S-SSB Transmission with V2X Sidelink Communication 2193

A.9.1.2.1 Test for FR1 NR Cell as synchronization reference source without gap under non-DRX 2193

A.9.1.2.1.1 Test Purpose and Environment 2193

A.9.1.2.1.2 Test Requirements 2197

A.9.1.2.2 Test for SyncRef UE as synchronization reference source 2197

A.9.1.2.2.1 Test Purpose and Environment 2197

A.9.1.2.2.2 Test Requirements 2198

A.9.1.3 Test for V2X Synchronization Reference Selection/Reselection 2199

A.9.1.3.1 Test for GNSS configured as the highest priority 2199

A.9.1.3.1.1 Test Purpose and Environment 2199

A.9.1.3.1.2 Test Requirements 2201

A.9.1.3.2 Test for FR1 NR Cell configured as the highest priority 2203

A.9.1.3.2.1 Test Purpose and Environment 2203

A.9.1.3.2.2 Test Requirements 2205

A.9.1.4 Test for L1 SL-RSRP Measurement 2206

A.9.1.4.1 Test for V2X UE Autonomous Resource Selection/Reselection 2206

A.9.1.4.1.1 Test Purpose and Environment 2206

A.9.1.4.1.2 Test Requirements 2209

A.9.1.4.2 Test for V2X UE Resource Pre-emption 2209

A.9.1.4.2.1 Test Purpose and Environment 2209

A.9.1.4.2.2 Test Requirements 2213

A.9.1.4.3 Test for V2X UE Resource Re-evaluation 2213

A.9.1.4.3.1 Test Purpose and Environment 2213

A.9.1.4.3.2 Test Requirements 2220

A.9.1.5 Test for Congestion Control Measurement 2220

A.9.1.5.1 Test Purpose and Environment 2220

A.9.1.5.2 Test Requirements 2226

A.9.1.6 Test for Interruption 2226

A.9.1.6.1 Test for Interruption to WAN due to V2X Sidelink Communication 2226

A.9.1.6.1.1 Test Purpose and Environment 2226

A.9.1.6.1.2 Test Requirements 2229

A.10 EN-DC Tests with NR PSCell under CCA and Other NR Cells in FR1 2229

A.10.1 RRC\_CONNECTED state mobility 2229

A.10.1.1 RRC connection mobility control 2229

A.10.1.1.1 Random Access 2229

A.10.1.1.1.1 4-step RA type contention-based random access for NR PSCell with CCA 2229

A.10.1.1.1.1.1 Test Purpose and Environment 2229

A.10.1.1.1.1.2 Test Requirements 2232

A.10.1.1.1.1.2.1 Random Access Preamble Transmission 2232

A.10.1.1.1.1.2.2 Random Access Response Reception 2232

A.10.1.1.1.1.2.3 No Random Access Response Reception 2233

A.10.1.1.1.1.2.4 Receiving an UL grant for msg3 retransmission 2233

A.10.1.1.1.1.2.5 Contention Resolution Timer expiry 2233

A.10.1.1.1.2 4-step RA type non-contention based random access for NR PSCell with CCA 2234

A.10.1.1.1.2.1 Test Purpose and Environment 2234

A.10.1.1.1.2.2 Test Requirements 2237

A.10.1.1.1.2.2.1 SSB-based Random Access Preamble Transmission 2237

A.10.1.1.1.2.2.2 Random Access Response Reception 2238

A.10.1.1.1.2.2.3 No Random Access Response Reception 2238

A.10.1.1.1.3 2-step RA type contention-based random access for NR PSCell with CCA 2238

A.10.1.1.1.3.1 Test Purpose and Environment 2238

A.10.1.1.1.3.2 Test Requirements 2242

A.10.1.1.1.3.2.1 MsgA Transmission 2242

A.10.1.1.1.3.2.2 MsgB Reception 2242

A.10.1.1.1.3.2.3 No MsgB Reception 2243

A.10.1.1.1.4 2-step RA type non-contention based random access for NR PSCell with CCA 2243

A.10.1.1.1.4.1 Test Purpose and Environment 2243

A.10.1.1.1.4.2 Test Requirements 2247

A.10.1.1.1.4.2.1 MsgA Transmission 2247

A.10.1.1.1.4.2.2 MsgB Reception 2248

A.10.1.1.1.4.2.3 No MsgB Reception 2248

A.10.2 Timing 2249

A.10.2.1 UE transmit timing 2249

A.10.2.2 UE timing advance 2253

A.10.3 Signalling characteristics 2256

A.10.3.1 Radio link monitoring 2256

A.10.3.1.1 Introduction 2256

A.10.3.1.2 Radio link monitoring out-of-sync test for PSCell configured with SSB-based RLM RS in non-DRX mode 2257

A.10.3.1.2.1 Test purpose and environment 2257

A.10.3.1.2.2 Test requirements 2262

A.10.3.1.3 Radio link monitoring in-sync test for PSCell configured with SSB-based RLM RS in non-DRX mode 2262

A.10.3.1.3.1 Test purpose and environment 2262

A.10.3.1.3.2 Test requirements 2268

A.10.3.1.4 Radio link monitoring out-of-sync test for PSCell configured with SSB-based RLM RS in DRX mode 2268

A.10.3.1.4.1 Test purpose and environment 2268

A.10.3.1.4.2 Test requirements 2268

A.10.3.1.5 Radio link monitoring in-sync test for PSCell configured with SSB-based RLM RS in DRX mode 2268

A.10.3.1.5.1 Test purpose and environment 2268

A.10.3.1.5.2 Test requirements 2268

A.10.3.2 Interruption 2268

A.10.3.2.1 E-UTRAN – NR interruptions during SCell operations with CCA 2268

A.10.3.2.1.1 Test Purpose and Environment 2268

A.10.3.2.1.2 Test Requirements 2273

A.10.3.3 SCell activation and deactivation delay 2273

A.10.3.3.2 SCell Activation and Deactivation of known NR SCell with NR PSCell and NR SCell under CCA, 640 ms SCell measurement cycle 2278

A.10.3.3.2.1 Test Purpose and Environment 2278

A.10.3.3.2.2 Test Requirements 2279

A.10.3.3.3 SCell Activation and Deactivation of unknown NR SCell with NR PSCell and NR SCell under CCA 2279

A.10.3.3.3.1 Test Purpose and Environment 2279

A.10.3.3.3.2 Test Requirements 2280

A.10.3.4 Beam failure detection and link recovery procedures 2280

A.10.3.4.1 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in non-DRX mode 2280

A.10.3.4.1.1 Test Purpose and Environment 2280

A.10.3.4.1.2 Test Requirements 2285

A.10.3.4.2 EN-DC Beam Failure Detection and Link Recovery Test for FR1 PSCell configured with SSB-based BFD and LR in DRX mode 2285

A.10.3.4.2.1 Test Purpose and Environment 2285

A.10.3.4.2.2 Test Requirements 2291

A.10.3.5 Active BWP switching 2291

A.10.3.5.1 UL active BWP switch delay with consistent UL LBT failure on PSCell subject to UL CCA in EN-DC 2291

A.10.3.5.1.1 Test Purpose and Environment 2291

A.10.3.5.1.2 Test Requirements 2296

A.10.3.5.2 DCI-based and Timer-based Active BWP Switch 2297

A.10.3.5.2.1 E-UTRAN – NR PSCell FR1 DL active BWP switch in non-DRX in synchronous EN-DC 2297

A.10.3.5.2.2 E-UTRAN – NR PSCell FR1 DL active BWP switch with FR1 SCell in non-DRX in synchronous EN-DC 2300

A.10.3.5.3 RRC-based Active BWP Switch 2304

A.10.3.6 PSCell addition and release delay 2308

A.10.3.6.1 Addition and Release Delay of known NR PSCell on the carrier under CCA 2308

A.10.3.6.1.1 Test purpose and environment 2308

A.10.3.6.1.2 Test Requirements 2312

A.10.3.7 Void 2313

A.10.4 Measurement procedure 2313

A.10.4.1 Intra-frequency measurements 2313

A.10.4.1.1 Event-triggered reporting tests on PSCC without gaps under non-DRX 2313

A.10.4.1.1.1 Test purpose and environment 2313

A.10.4.1.1.2 Test parameters 2313

A.10.4.1.1.3 Test Requirements 2313

A.10.4.1.2 Event-triggered reporting tests on PSCC without gaps under DRX 2314

A.10.4.1.2.1 Test purpose and environment 2314

A.10.4.1.2.2 Test parameters 2314

A.10.4.1.2.3 Test Requirements 2314

A.10.4.1.3 Event-triggered reporting tests on PSCC with per-UE gaps under non-DRX 2314

A.10.4.1.3.1 Test purpose and environment 2314

A.10.4.1.3.2 Test parameters 2314

A.10.4.1.3.3 Test Requirements 2314

A.10.4.1.4 Event-triggered reporting tests on PSCC with per-UE gaps under DRX 2315

A.10.4.1.4.1 Test purpose and environment 2315

A.10.4.1.4.2 Test parameters 2315

A.10.4.1.4.3 Test Requirements 2315

A.10.4.1.5 Event-triggered reporting tests on SCC without gaps under non-DRX 2315

A.10.4.1.5.1 Test purpose and environment 2315

A.10.4.1.5.2 Test parameters 2315

A.10.4.1.5.3 Test Requirements 2315

A.10.4.1.6 Event-triggered reporting tests on SCC without gaps under DRX 2316

A.10.4.1.6.1 Test purpose and environment 2316

A.10.4.1.6.2 Test parameters 2316

A.10.4.1.6.3 Test Requirements 2316

A.10.4.1.7 Event-triggered reporting tests on SCC with per-UE gaps under non-DRX 2316

A.10.4.1.7.1 Test purpose and environment 2316

A.10.4.1.7.2 Test parameters 2316

A.10.4.1.7.3 Test Requirements 2316

A.10.4.1.8 Event-triggered reporting tests on SCC with per-UE gaps under DRX 2317

A.10.4.1.8.1 Test purpose and environment 2317

A.10.4.1.8.2 Test parameters 2317

A.10.4.1.8.3 Test Requirements 2317

A.10.4.1.9 RSSI measurement reporting on PSCC 2317

A.10.4.1.9.1 Test purpose and environment 2317

A.10.4.1.9.2 Test parameters 2317

A.10.4.1.10 Channel occupancy measurement reporting on PSCC 2318

A.10.4.1.10.1 Test purpose and environment 2318

A.10.4.1.10.2 Test parameters 2318

A.10.4.1.11 RSSI measurement reporting on SCC 2318

A.10.4.1.11.1 Test purpose and environment 2318

A.10.4.1.11.2 Test parameters 2318

A.10.4.1.12 Channel occupancy measurement reporting on SCC 2319

A.10.4.1.12.1 Test purpose and environment 2319

A.10.4.1.12.2 Test parameters 2319

A.10.4.2 Inter-frequency measurements 2319

A.10.4.2.1 RSSI measurement reporting 2319

A.10.4.2.1.1 Test purpose and environment 2319

A.10.4.2.1.2 Test parameters 2319

A.10.4.2.2 Channel occupancy measurement reporting 2320

A.10.4.2.2.1 Test purpose and environment 2320

A.10.4.2.2.2 Test parameters 2320

A.10.4.2.3 EN-DC event triggered reporting tests for FR1 with CCA cell without SSB time index detection when DRX is not used 2320

A.10.4.2.3.1 Test Purpose and Environment 2320

A.10.4.2.3.2 Test Requirements 2325

A.10.4.2.4 EN-DC event triggered reporting tests for FR1 cell with CCA without SSB time index detection when DRX is used 2326

A.10.4.2.4.1 Test Purpose and Environment 2326

A.10.4.2.4.2 Test Requirements 2330

A.10.4.2.5 EN-DC event triggered reporting tests for FR1 cell with CCA with SSB time index detection when DRX is not used 2331

A.10.4.2.5.1 Test Purpose and Environment 2331

A.10.4.2.5.2 Test Requirements 2335

A.10.4.2.6 EN-DC event triggered reporting tests for FR1 cell with CCA with SSB time index detection when DRX is used 2336

A.10.4.2.6.1 Test Purpose and Environment 2336

A.10.4.2.6.2 Test Requirements 2340

A.10.4.2.7 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is not used 2341

A.10.4.2.7.1 Test Purpose and Environment 2341

A.10.4.2.7.2 Test Requirements 2347

A.10.4.2.8 EN-DC event triggered reporting tests for FR1 cell without SSB time index detection when DRX is used 2347

A.10.4.2.8.1 Test Purpose and Environment 2347

A.10.4.2.8.2 Test Requirements 2353

A.10.4.2.9 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is not used 2354

A.10.4.2.9.1 Test Purpose and Environment 2354

A.10.4.2.9.2 Test Requirements 2359

A.10.4.2.10 EN-DC event triggered reporting tests for FR1 cell with SSB time index detection when DRX is used 2359

A.10.4.2.10.1 Test Purpose and Environment 2359

A.10.4.2.10.2 Test Requirements 2365

A.10.4.3 L1-RSRP measurements for beam reporting 2366

A.10.4.3.1 SSB based L1-RSRP measurement on PSCC when DRX is not used 2366

A.10.4.3.1.1 Test Purpose and Environment 2366

A.10.4.3.1.2 Test parameters 2366

A.10.4.3.1.3 Test Requirements 2368

A.10.4.3.2 SSB based L1-RSRP measurement on PSCC when DRX is used 2369

A.10.4.3.2.1 Test Purpose and Environment 2369

A.10.4.3.2.2 Test parameters 2369

A.10.4.3.2.3 Test Requirements 2371

A.10.4.3.3 SSB based L1-RSRP measurement on SCC when DRX is not used 2372

A.10.4.3.3.1 Test Purpose and Environment 2372

A.10.4.3.3.2 Test parameters 2372

A.10.4.3.3.3 Test Requirements 2375

A.10.4.3.4 SSB based L1-RSRP measurement on SCC when DRX is used 2376

A.10.4.3.4.1 Test Purpose and Environment 2376

A.10.4.3.4.2 Test parameters 2376

A.10.4.3.4.3 Test Requirements 2379

A.10.4.4 E-UTRAN−NR inter-RAT measurements on NR carrier frequency under CCA 2380

A.10.4.4.1 E-UTRA-NR inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 2380

A.10.4.4.1.1 Test Purpose and Environment 2380

A.10.4.4.1.2 Test Requirements 2384

A.10.4.4.2 E-UTRA-NR inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is used 2385

A.10.4.4.2.1 Test Purpose and Environment 2385

A.10.4.4.2.2 Test Requirements 2390

A.10.4.4.3 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 2391

A.10.4.4.3.1 Test Purpose and Environment 2391

A.10.4.4.3.2 Test Requirements 2395

A.10.4.4.4 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is used 2396

A.10.4.4.4.1 Test Purpose and Environment 2396

A.10.4.4.4.2 Test Requirements 2401

A.10.5 Measurement performance 2402

A.10.5.1 SS-RSRP 2402

A.10.5.1.1 Intra-frequency measurement accuracy on a CCA serving cell 2402

A.10.5.1.1.1 Test Purpose and Environment 2402

A.10.5.1.1.2 Test parameters 2402

A.10.5.1.1.3 Test Requirements 2405

A.10.5.1.2 Inter-frequency measurement accuracy with FR1 CCA serving cell and FR1 CCA target cell 2405

A.10.5.1.2.1 Test Purpose and Environment 2405

A.10.5.1.2.2 Test parameters 2405

A.10.5.1.2.3 Test Requirements 2409

A.10.5.2 SS-RSRQ 2409

A.10.5.2.1 Intra-frequency measurement accuracy with FR1 CCA serving cell and FR1 CCA target cell 2409

A.10.5.2.1.1 Test Purpose and Environment 2409

A.10.5.2.1.2 Test Parameters 2409

A.10.5.2.1.3 Test Requirements 2412

A.10.5.2.2 Inter-frequency measurement accuracy with FR1 CCA serving cell and FR1 CCA target cell 2412

A.10.5.2.2.1 Test Purpose and Environment 2412

A.10.5.2.2.2 Test Parameters 2412

A.10.5.2.2.3 Test Requirements 2415

A.10.5.3 SS-SINR 2415

A.10.5.3.1 Intra-frequency measurement accuracy on PSCC 2415

A.10.5.3.1.1 Test Purpose and Environment 2415

A.10.5.3.1.2 Test Parameters 2415

A.10.5.3.1.3 Test Requirements 2418

A.10.5.3.2 Inter-frequency measurement accuracy on PSCC 2418

A.10.5.3.2.1 Test Purpose and Environment 2418

A.10.5.3.2.2 Test Parameters 2418

A.10.5.3.2.3 Test Requirements 2422

A.10.5.3.3 Intra-frequency measurement accuracy on SCC 2422

A.10.5.3.3.1 Test Purpose and Environment 2422

A.10.5.3.3.2 Test Parameters 2422

A.10.5.3.3.3 Test Requirements 2425

A.10.5.4 L1-RSRP measurement for beam reporting with CCA serving cell 2425

A.10.5.4.1 SSB based L1-RSRP measurement 2425

A.10.5.4.1.1 Test Purpose and Environment 2425

A.10.5.4.1.2 Test parameters 2426

A.10.5.4.1.3 Test Requirements 2428

A.10.5.5 RSSI 2428

A.10.5.5.1 RSSI measurement accuracy on PSCC with CCA 2428

A.10.5.5.1.1 Test Purpose and Environment 2428

A.10.5.5.1.2 Test parameters 2428

A.10.5.5.1.3 Test Requirements 2431

A.10.5.5.2 RSSI measurement accuracy on SCC with CCA 2431

A.10.5.5.2.1 Test Purpose and Environment 2431

A.10.5.5.2.2 Test parameters 2431

A.10.5.5.2.3 Test Requirements 2434

A.10.5.5.3 Inter-frequency RSSI measurement accuracy on a carrier with CCA 2434

A.10.5.5.3.1 Test Purpose and Environment 2434

A.10.5.5.3.2 Test parameters 2434

A.10.5.5.3.3 Test Requirements 2438

A.10.5.6 Channel occupancy 2438

A.10.5.6.1 Channel occupancy measurement accuracy on PSCC with CCA 2438

A.10.5.6.1.1 Test Purpose and Environment 2438

A.10.5.6.1.2 Test parameters 2438

A.10.5.6.1.3 Test Requirements 2442

A.10.5.6.2 Channel occupancy measurement accuracy on SCC with CCA 2442

A.10.5.6.2.1 Test Purpose and Environment 2442

A.10.5.6.2.2 Test parameters 2442

A.10.5.6.2.3 Test Requirements 2445

A.10.5.6.3 Inter-frequency channel occupancy measurement accuracy on a carrier with CCA 2445

A.10.5.6.3.1 Test Purpose and Environment 2445

A.10.5.6.3.2 Test parameters 2445

A.10.5.6.3.3 Test Requirements 2449

A.11 NR Standalone Tests with NR PCell under CCA and Other NR Cells in FR1 2449

A.11.1 RRC\_IDLE state mobility 2449

A.11.1.1 Cell re-selection with both source and target NR carrier frequencies under CCA 2449

A.11.1.1.1 Cell reselection to FR1 intra-frequency NR cells when subject to CCA on the serving and target cell 2449

A.11.1.1.1.1 Test Purpose and Environment 2449

A.11.1.1.1.2 Test Parameters 2450

A.11.1.1.1.3 Test Requirements 2453

A.11.1.1.2 Cell reselection to FR1 inter-frequency NR case when subject to CCA on the serving and target cell 2453

A.11.1.1.2.1 Test Purpose and Environment 2453

A.11.1.1.2.2 Test Parameters 2453

A.11.1.1.2.3 Test Requirements 2457

A.11.1.2 Cell re-selection to NR with source NR carrier frequency under CCA 2457

A.11.1.2.1 Cell reselection to FR1 inter-frequency NR case when serving cell is subject to CCA 2457

A.11.1.2.1.1 Test Purpose and Environment 2457

A.11.1.2.1.2 Test Parameters 2458

A.11.1.2.1.3 Test Requirements 2464

A.11.1.3 Cell re-selection from NR carrier with target NR carrier frequency under CCA 2465

A.11.1.3.1 Cell reselection to FR1 inter-frequency NR case when target cell is subject to CCA 2465

A.11.1.3.1.1 Test Purpose and Environment 2465

A.11.1.3.1.2 Test Parameters 2465

A.11.1.3.1.3 Test Requirements 2470

A.11.1.4 Inter-RAT cell re-selection to E-UTRAN with source NR carrier frequency under CCA 2471

A.11.1.4.1 Cell reselection to higher priority E-UTRAN when serving cell is subject to CCA 2471

A.11.1.4.1.1 Test Purpose and Environment 2471

A.11.1.4.1.2 Test Parameters 2471

A.11.1.4.1.3 Test Requirements 2474

A.11.1.4.2 Cell reselection to lower priority E-UTRAN when serving cell is subject to CCA 2475

A.11.1.4.2.1 Test Purpose and Environment 2475

A.11.1.4.2.2 Test Requirements 2477

A.11.2 RRC\_CONNECTED state mobility 2478

A.11.2.1 Handover 2478

A.11.2.1.1 Intra-frequency handover from FR1 carrier under CCA to FR1 carrier under CCA; known target cell 2478

A.11.2.1.1.1 Test Purpose and Environment 2478

A.11.2.1.1.2 Test Parameters 2478

A.11.2.1.1.3 Test Requirements 2481

A.11.2.1.2 Intra-frequency handover from FR1 carrier under CCA to FR1 carrier under CCA; unknown target cell 2481

A.11.2.1.2.1 Test Purpose and Environment 2481

A.11.2.1.2.2 Test Parameters 2481

A.11.2.1.2.3 Test Requirements 2484

A.11.2.1.3 Inter-frequency handover from FR1 carrier under CCA to FR1 carrier under CCA; unknown target cell 2484

A.11.2.1.3.1 Test Purpose and Environment 2484

A.11.2.1.3.2 Test Parameters 2484

A.11.2.1.3.3 Test Requirements 2487

A.11.2.1.4 Inter-frequency handover from FR1 carrier under CCA to FR1; known target cell 2487

A.11.2.1.4.1 Test Purpose and Environment 2487

A.11.2.1.4.2 Test Parameters 2487

A.11.2.1.4.3 Test Requirements 2491

A.11.2.1.5 Inter-frequency handover from FR1 carrier under CCA to FR1; unknown target cell 2492

A.11.2.1.5.1 Test Purpose and Environment 2492

A.11.2.1.5.2 Test Parameters 2492

A.11.2.1.5.3 Test Requirements 2495

A.11.2.1.6 Inter-frequency handover from FR1 to FR1 carrier under CCA; unknown target cell 2496

A.11.2.1.6.1 Test Purpose and Environment 2496

A.11.2.1.6.2 Test Parameters 2496

A.11.2.1.6.3 Test Requirements 2499

A.11.2.1.7 SA NR FR1 carrier under CCA - E-UTRAN handover with known target cell 2500

A.11.2.1.7.1 Test Purpose and Environment 2500

A.11.2.1.7.2 Test Requirements 2506

A.11.2.1.8 SA NR FR1 carrier under CCA - E-UTRAN handover with unknown target cell 2506

A.11.2.1.8.1 Test Purpose and Environment 2506

A.11.2.1.8.2 Test Requirements 2511

A.11.2.2 RRC connection mobility control 2511

A.11.2.2.1 RRC re-establishment 2511

A.11.2.2.1.1 Intra-frequency RRC Re-establishment with CCA in FR1 2511

A.11.2.2.1.2 Inter-frequency RRC Re-establishment with CCA in FR1 2514

A.11.2.2.1.3 Intra-frequency RRC Re-establishment with CCA in FR1 without serving cell timing 2518

A.11.2.2.1.4 Inter-frequency RRC Re-establishment from NR FR1 carrier without CCA to NR FR1 carrier under CCA 2521

A.11.2.2.2 Random Access 2526

A.11.2.2.2.1 4-step RA type contention-based random access for NR PCell with CCA 2526

A.11.2.2.2.1.1 Test Purpose and Environment 2526

A.11.2.2.2.1.2 Test Requirements 2529

A.11.2.2.2.1.2.1 Random Access Preamble Transmission 2529

A.11.2.2.2.1.2.2 Random Access Response Reception 2529

A.11.2.2.2.1.2.3 No Random Access Response Reception 2530

A.11.2.2.2.1.2.4 Receiving an UL grant for msg3 retransmission 2530

A.11.2.2.2.1.2.5 Reception of an Incorrect Message over Temporary C-RNTI 2530

A.11.2.2.2.1.2.6 Reception of a Correct Message over Temporary C-RNTI 2531

A.11.2.2.2.1.2.7 Contention Resolution Timer expiry 2531

A.11.2.2.2.2 4-step RA type non-contention based random access for NR PSCell with CCA 2531

A.11.2.2.2.2.1 Test Purpose and Environment 2531

A.11.2.2.2.2.2 Test Requirements 2534

A.11.2.2.2.2.2.1 SSB-based Random Access Preamble Transmission 2534

A.11.2.2.2.2.2.2 Random Access Response Reception 2535

A.11.2.2.2.2.2.3 No Random Access Response Reception 2535

A.11.2.2.2.3 2-step RA type contention-based random access for NR PCell with CCA 2535

A.11.2.2.2.3.1 Test Purpose and Environment 2535

A.11.2.2.2.3.2 Test Requirements 2539

A.11.2.2.2.3.2.1 MsgA Transmission 2539

A.11.2.2.2.3.2.2 MsgB Reception 2539

A.11.2.2.2.3.2.3 No MsgB Reception 2540

A.11.2.2.2.4 2-step RA type non-contention-based random access for NR PCell with CCA 2540

A.11.2.2.2.4.1 Test Purpose and Environment 2540

A.11.2.2.2.4.2 Test Requirements 2544

A.11.2.2.2.4.2.1 MsgA Transmission 2544

A.11.2.2.2.4.2.2 MsgB Reception 2545

A.11.2.2.2.4.2.3 No MsgB Reception 2545

A.11.2.2.3 RRC connection release with redirection 2546

A.11.2.2.3.1 Redirection from NR FR1 carrier under CCA to NR FR1 carrier under CCA 2546

A.11.3 Timing 2554

A.11.3.1 UE transmit timing 2554

A.11.3.2 UE timing advance 2558

A.11.3.2.1 UE Timing Advance Adjustment Accuracy with PCell under DL CCA 2558

A.11.3.2.1.1 Test Purpose and Environment 2558

A.11.3.2.1.2 Test Parameters 2558

A.11.3.2.1.3 Test Requirements 2562

A.11.4 Signalling characteristics 2562

A.11.4.1 Radio link monitoring 2562

A.11.4.1.1 Introduction 2562

A.11.4.1.2 Radio link monitoring out-of-sync test for PCell configured with SSB-based RLM RS in non-DRX mode 2563

A.11.4.1.2.1 Test purpose and environment 2563

A.11.4.1.2.2 Test requirements 2567

A.11.4.1.3 Radio link monitoring in-sync test for PCell configured with SSB-based RLM RS in non-DRX mode 2567

A.11.4.1.3.1 Test purpose and environment 2567

A.11.4.1.3.2 Test requirements 2573

A.11.4.1.4 Radio link monitoring out-of-sync test for PCell configured with SSB-based RLM RS in DRX mode 2573

A.11.4.1.4.1 Test purpose and environment 2573

A.11.4.1.4.2 Test requirements 2573

A.11.4.1.5 Radio link monitoring in-sync test for PCell configured with SSB-based RLM RS in DRX mode 2573

A.11.4.1.5.1 Test purpose and environment 2573

A.11.4.1.5.2 Test requirements 2573

A.11.4.2 Interruption 2574

A.11.4.2.1 NR interruptions during Scell operations with CCA on PCell and SCell 2574

A.11.4.2.1.1 Test Purpose and Environment 2574

A.11.4.2.1.2 Test Requirements 2578

A.11.4.3 SCell activation and deactivation delay 2578

A.11.4.3.2 SCell Activation and Deactivation of known SCell with PCell and SCell under CCA, 640 ms SCell measurement cycle 2583

A.11.4.3.2.1 Test Purpose and Environment 2583

A.11.4.3.2.2 Test Requirements 2584

A.11.4.4 Beam failure detection and link recovery procedures 2585

A.11.4.4.1 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in non-DRX mode 2585

A.11.4.4.1.1 Test Purpose and Environment 2585

A.11.4.4.1.2 Test Requirements 2591

A.11.4.4.2 Beam Failure Detection and Link Recovery Test for FR1 PCell configured with SSB-based BFD and LR in DRX mode 2591

A.11.4.4.2.1 Test Purpose and Environment 2591

A.11.4.4.2.2 Test Requirements 2597

A.11.4.5 Active BWP switching 2597

A.11.4.5.1 UL active BWP switch delay with consistent UL LBT failure on PCell subject to UL CCA 2597

A.11.4.5.1.2 Test Requirements 2601

A.11.4.6 Void 2611

A.11.5 Measurement procedure 2611

A.11.5.1 Intra-frequency measurements 2611

A.11.5.1.1 Event-triggered reporting tests on PCC without gaps under non-DRX 2611

A.11.5.1.1.1 Test purpose and environment 2611

A.11.5.1.1.2 Test parameters 2611

A.11.5.1.1.3 Test Requirements 2611

A.11.5.1.2 Event-triggered reporting tests on PCC without gaps under DRX 2612

A.11.5.1.2.1 Test purpose and environment 2612

A.11.5.1.2.2 Test parameters 2612

A.11.5.1.2.3 Test Requirements 2612

A.11.5.1.3 Event-triggered reporting tests on PCC with per-UE gaps under non-DRX 2612

A.11.5.1.3.1 Test purpose and environment 2612

A.11.5.1.3.2 Test parameters 2612

A.11.5.1.3.3 Test Requirements 2612

A.11.5.1.4 Event-triggered reporting tests on PCC with per-UE gaps under DRX 2613

A.11.5.1.4.1 Test purpose and environment 2613

A.11.5.1.4.2 Test parameters 2613

A.11.5.1.4.3 Test Requirements 2613

A.11.5.1.5 Event-triggered reporting tests on SCC without gaps under non-DRX 2613

A.11.5.1.5.1 Test purpose and environment 2613

A.11.5.1.5.2 Test parameters 2613

A.11.5.1.6 Event-triggered reporting tests on SCC without gaps under DRX 2614

A.11.5.1.6.1 Test purpose and environment 2614

A.11.5.1.6.2 Test parameters 2614

A.11.5.1.6.3 Test Requirements 2614

A.11.5.1.7 Event-triggered reporting tests on SCC with per-UE gaps under non-DRX 2614

A.11.5.1.7.1 Test purpose and environment 2614

A.11.5.1.7.2 Test parameters 2614

A.11.5.1.7.3 Test Requirements 2614

A.11.5.1.8 Event-triggered reporting tests on SCC with per-UE gaps under DRX 2615

A.11.5.1.8.1 Test purpose and environment 2615

A.11.5.1.8.2 Test parameters 2615

A.11.5.1.8.3 Test Requirements 2615

A.11.5.1.9 RSSI measurement reporting on PCC 2615

A.11.5.1.9.1 Test purpose and environment 2615

A.11.5.1.9.2 Test parameters 2615

A.11.5.1.10 Channel occupancy measurement reporting on PCC 2615

A.11.5.1.10.1 Test purpose and environment 2615

A.11.5.1.10.2 Test parameters 2616

A.11.5.1.11 RSSI measurement reporting on SCC 2616

A.11.5.1.11.1 Test purpose and environment 2616

A.11.5.1.11.2 Test parameters 2616

A.11.5.1.12 Channel occupancy measurement reporting on SCC 2616

A.11.5.1.12.1 Test purpose and environment 2616

A.11.5.1.12.2 Test parameters 2616

A.11.5.2 Inter-frequency measurements 2617

A.11.5.2.1 RSSI measurement reporting 2617

A.11.5.2.1.1 Test purpose and environment 2617

A.11.5.2.1.2 Test parameters 2617

A.11.5.2.2 Channel occupancy measurement reporting 2617

A.11.5.2.2.1 Test purpose and environment 2617

A.11.5.2.2.2 Test parameters 2617

A.11.5.2.3 Event triggered reporting tests for FR1 with CCA without SSB time index detection when DRX is not used 2618

A.11.5.2.3.1 Test Purpose and Environment 2618

A.11.5.2.3.2 Test Requirements 2622

A.11.5.2.4 Event triggered reporting tests for FR1 with CCA without SSB time index detection when DRX is used 2623

A.11.5.2.4.1 Test Purpose and Environment 2623

A.11.5.2.4.2 Test Requirements 2628

A.11.5.2.5 Event triggered reporting tests for FR1 with CCA with SSB time index detection when DRX is not used 2628

A.11.5.2.5.1 Test Purpose and Environment 2628

A.11.5.2.5.2 Test Requirements 2632

A.11.5.2.6 Event triggered reporting tests for FR1 with CCA with SSB time index detection when DRX is used 2633

A.11.5.2.6.1 Test Purpose and Environment 2633

A.11.5.2.6.2 Test Requirements 2638

A.11.5.2.7 Event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 2638

A.11.5.2.7.1 Test Purpose and Environment 2638

A.11.5.2.7.2 Test Requirements 2642

A.11.5.2.8 Event triggered reporting tests for FR1 without SSB time index detection when DRX is used 2643

A.11.5.2.8.1 Test Purpose and Environment 2643

A.11.5.2.8.2 Test Requirements 2648

A.11.5.2.9 Event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 2648

A.11.5.2.9.1 Test Purpose and Environment 2648

A.11.5.2.9.2 Test Requirements 2653

A.11.5.2.10 Event triggered reporting tests for FR1 with SSB time index detection when DRX is used 2654

A.11.5.2.10.1 Test Purpose and Environment 2654

A.11.5.2.10.2 Test Requirements 2659

A.11.5.3 Inter-RAT E-UTRAN measurements 2660

A.11.5.4 L1-RSRP measurements for beam reporting 2660

A.11.5.4.1 SSB based L1-RSRP measurement when DRX is not used 2660

A.11.5.4.1.1 Test Purpose and Environment 2660

A.11.5.4.1.2 Test parameters 2660

A.11.5.4.1.3 Test Requirements 2662

A.11.5.4.2 SSB based L1-RSRP measurement when DRX is used 2662

A.11.5.4.2.1 Test Purpose and Environment 2662

A.11.5.4.2.2 Test parameters 2663

A.11.5.4.2.3 Test Requirements 2665

A.11.5.4.3 SSB based L1-RSRP measurement on SCC when DRX is not used 2665

A.11.5.4.3.1 Test Purpose and Environment 2665

A.11.5.4.3.2 Test parameters 2666

A.11.5.4.3.3 Test Requirements 2669

A.11.5.4.4 SSB based L1-RSRP measurement on SCC when DRX is used 2670

A.11.5.4.4.1 Test Purpose and Environment 2670

A.11.5.4.4.2 Test parameters 2670

A.11.5.4.4.3 Test Requirements 2673

A.11.6 Measurement performance 2674

A.11.6.1 SS-RSRP 2674

A.11.6.1.1 Intra-frequency measurement accuracy on a carrier frequency with CCA 2674

A.11.6.1.1.1 Test Purpose and Environment 2674

A.11.6.1.1.2 Test parameters 2674

A.11.6.1.1.3 Test Requirements 2676

A.11.6.1.2 Intra-frequency measurement accuracy on SCC on a carrier frequency with CCA 2676

A.11.6.1.2.1 Test Purpose and Environment 2676

A.11.6.1.2.2 Test parameters 2676

A.11.6.1.2.3 Test Requirements 2678

A.11.6.2 SS-RSRQ 2678

A.11.6.2.1 Intra-frequency measurement accuracy 2678

A.11.6.2.1.1 Test Purpose and Environment 2678

A.11.6.2.1.2 Test Parameters 2678

A.11.6.2.1.3 Test Requirements 2681

A.11.6.2.2 Inter-frequency measurement accuracy 2681

A.11.6.2.2.1 Test Purpose and Environment 2681

A.11.6.2.2.2 Test Parameters 2681

A.11.6.2.2.3 Test Requirements 2684

A.11.6.2.3 Intra-frequency measurement accuracy on SCC 2684

A.11.6.2.3.1 Test Purpose and Environment 2684

A.11.6.2.3.2 Test Parameters 2684

A.11.6.2.3.3 Test Requirements 2687

A.11.6.2.4 Inter-frequency measurement accuracy 2687

A.11.6.2.4.1 Test Purpose and Environment 2687

A.11.6.2.4.2 Test Parameters 2687

A.11.6.2.4.3 Test Requirements 2696

A.11.6.3 SS-SINR 2696

A.11.6.3.1 Intra-frequency measurement accuracy 2696

A.11.6.3.1.1 Test Purpose and Environment 2696

A.11.6.3.1.2 Test Parameters 2696

A.11.6.3.1.3 Test Requirements 2699

A.11.6.3.2 Inter-frequency measurement accuracy 2699

A.11.6.3.2.1 Test Purpose and Environment 2699

A.11.6.3.2.2 Test Parameters 2699

A.11.6.3.2.3 Test Requirements 2702

A.11.6.3.3 Intra-frequency measurement accuracy on SCC 2702

A.11.6.3.3.1 Test Purpose and Environment 2702

A.11.6.3.3.2 Test Parameters 2702

A.11.6.3.3.3 Test Requirements 2705

A.11.6.3.4 Inter-frequency measurement accuracy 2705

A.11.6.3.4.1 Test Purpose and Environment 2705

A.11.6.3.4.2 Test Parameters 2705

A.11.6.3.4.3 Test Requirements 2713

A.11.6.4 L1-RSRP measurement for beam reporting with CCA serving cell 2713

A.11.6.4.1 SSB based L1-RSRP measurement 2713

A.11.6.4.1.1 Test Purpose and Environment 2713

A.11.6.4.1.2 Test parameters 2714

A.11.6.4.1.3 Test Requirements 2717

A.11.6.5 RSSI 2717

A.11.6.5.1 Intra-frequency RSSI measurement accuracy on PCC with CCA 2717

A.11.6.5.1.1 Test Purpose and Environment 2717

A.11.6.5.1.2 Test parameters 2717

A.11.6.5.1.3 Test Requirements 2720

A.11.6.5.2 Intra-frequency RSSI measurement accuracy on SCC with CCA 2720

A.11.6.5.2.1 Test Purpose and Environment 2720

A.11.6.5.2.2 Test parameters 2720

A.11.6.5.2.3 Test Requirements 2723

A.11.6.5.3 Inter-frequency RSSI measurement accuracy on a carrier with CCA 2723

A.11.6.5.3.1 Test Purpose and Environment 2723

A.11.6.5.3.2 Test parameters 2723

A.11.6.5.3.3 Test Requirements 2726

A.11.6.6 Channel occupancy 2726

A.11.6.6.1 Intra-frequency channel occupancy measurement accuracy on PCC with CCA 2726

A.11.6.6.1.1 Test Purpose and Environment 2726

A.11.6.6.1.2 Test parameters 2726

A.11.6.6.1.3 Test Requirements 2730

A.11.6.6.2 Intra-frequency channel occupancy measurement accuracy on SCC with CCA 2730

A.11.6.6.2.1 Test Purpose and Environment 2730

A.11.6.6.2.2 Test parameters 2730

A.11.6.6.2.3 Test Requirements 2733

A.11.6.6.3 Inter-frequency channel occupancy measurement accuracy on a carrier with CCA 2733

A.11.6.6.3.1 Test Purpose and Environment 2733

A.11.6.6.3.2 Test parameters 2733

A.11.6.6.3.3 Test Requirements 2736

A.11.6.7 E-UTRAN RSRP 2736

A.11.6.8 E-UTRAN RSRQ 2736

A.11.6.9 E-UTRAN SINR 2736

A.12 E-UTRA Standalone Tests with at Least One NR Cell under CCA 2736

A.12.1 RRC\_IDLE state mobility 2736

A.12.1.1 Inter-RAT cell re-selection to NR on a carrier frequency with CCA 2736

A.12.1.1.1 E-UTRA Cell reselection to higher priority NR target Cell in FR1 when target cell is subject to CCA 2736

A.12.1.1.1.1 Test Purpose and Environment 2736

A.12.1.1.1.2 Test Requirements 2742

A.12.2 RRC\_CONNECTED state mobility 2743

A.12.2.1 Handover 2743

A.12.2.1.1 E-UTRAN - NR with CCA handover 2743

A.12.2.1.1.1 Test Purpose and Environment 2743

A.12.2.1.1.2 Test Requirements 2748

A.12.3 Signalling characteristics 2749

A.12.3.1 Interruptions 2749

A.12.4 Measurement procedure 2749

A.12.4.1 E-UTRAN−NR inter-RAT SFTD measurements 2749

A.12.4.1.1 E-UTRA – NR Inter-RAT SFTD Measurement Delay with NR under CCA in non-DRX 2749

A.12.4.1.1.1 Test Purpose and Environment 2749

A.12.4.1.1.2 Test Requirements 2753

A.12.4.2 E-UTRAN−NR inter-RAT measurements on NR carrier frequency under CCA 2753

A.12.4.2.1 E-UTRA-NR inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is not used 2753

A.12.4.2.1.1 Test Purpose and Environment 2753

A.12.4.2.1.2 Test Requirements 2757

A.12.4.2.2 E-UTRA-NR inter-RAT event triggered reporting tests for FR1 without SSB time index detection when DRX is used 2758

A.12.4.2.2.1 Test Purpose and Environment 2758

A.12.4.2.2.2 Test Requirements 2762

A.12.4.2.3 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is not used 2762

A.12.4.2.3.1 Test Purpose and Environment 2762

A.12.4.2.3.2 Test Requirements 2766

A.12.4.2.4 NR Inter-RAT event triggered reporting tests for FR1 with SSB time index detection when DRX is used 2767

A.12.4.2.4.1 Test Purpose and Environment 2767

A.12.4.2.4.2 Test Requirements 2771

A.12.4.2.5 RSSI measurement reporting 2771

A.12.4.2.5.1 Test purpose and environment 2771

A.12.4.2.5.2 Test parameters 2771

A.12.4.2.6 Channel occupancy measurement reporting 2772

A.12.4.2.6.1 Test purpose and environment 2772

A.12.4.2.6.2 Test parameters 2772

A.12.5 Measurement performance 2772

A.12.5.1 E-UTRAN−NR SFTD 2772

A.12.5.2 E-UTRAN−NR SS-RSRP 2778

A.12.5.3 E-UTRAN−NR SS-RSRQ 2778

A.12.5.4 E-UTRAN−NR SS-SINR 2778

A.12.5.5 E-UTRAN−NR RSSI 2778

A.12.5.6 E-UTRAN−NR channel occupancy 2778

A.13 NR Standalone Tests with NR SCell under CCA and All Other NR Cells in FR1 2778

A.13.1 Timing 2778

A.13.1.1 UE transmit timing 2778

A.13.1.2 Timing advance 2778

A.13.2 Signalling characteristics 2778

A.13.2.1 Interruption 2778

A.13.2.1.1 NR interruptions during SCell operations with CCA on SCell 2778

A.13.2.1.1.1 Test Purpose and Environment 2778

A.13.2.1.1.2 Test Requirements 2782

A.13.2.2 SCell activation and deactivation delay 2782

A.13.2.2.2 SCell Activation and Deactivation of known SCell under CCA, 640 ms SCell measurement cycle 2787

A.13.2.2.2.1 Test Purpose and Environment 2787

A.13.2.2.2.2 Test Requirements 2788

A.13.2.2.3 SCell Activation and Deactivation of unknown SCell under CCA 2788

A.13.2.2.3.1 Test Purpose and Environment 2788

A.13.2.2.3.2 Test Requirements 2789

A.13.2.3 Void 2789

A.13.3 Measurement procedure 2789

A.13.3.1 Intra-frequency measurements 2789

A.13.3.1.1 Event-triggered reporting tests on SCC without gaps under non-DRX 2789

A.13.3.1.1.1 Test purpose and environment 2789

A.13.3.1.1.2 Test parameters 2789

A.13.3.1.1.3 Test Requirements 2794

A.13.3.1.2 Event-triggered reporting tests on SCC without gaps under DRX 2794

A.13.3.1.2.1 Test purpose and environment 2794

A.13.3.1.2.2 Test parameters 2794

A.13.3.1.2.3 Test Requirements 2799

A.13.3.1.3 Event-triggered reporting tests on SCC with per-UE gaps under non-DRX 2799

A.13.3.1.3.1 Test purpose and environment 2799

A.13.3.1.3.2 Test parameters 2799

A.13.3.1.3.3 Test Requirements 2804

A.13.3.1.4 Event-triggered reporting tests on SCC with per-UE gaps under DRX 2804

A.13.3.1.4.1 Test purpose and environment 2804

A.13.3.1.4.2 Test parameters 2804

A.13.3.1.4.3 Test Requirements 2809

A.13.3.1.5 RSSI measurement reporting on SCC 2809

A.13.3.1.5.1 Test purpose and environment 2809

A.13.3.1.5.2 Test parameters 2809

A.13.3.1.6 Channel occupancy measurement reporting on SCC 2811

A.13.3.1.6.1 Test purpose and environment 2811

A.13.3.1.6.2 Test parameters 2812

A.13.3.2 Inter-frequency measurements 2812

A.13.3.2.1 RSSI measurement reporting 2812

A.13.3.2.1.1 Test purpose and environment 2812

A.13.3.2.1.2 Test parameters 2812

A.13.3.2.2 Channel occupancy measurement reporting 2813

A.13.3.2.2.1 Test purpose and environment 2813

A.13.3.2.2.2 Test parameters 2813

A.13.3.2.3 Event triggered reporting tests for FR1 with CCA without SSB time index detection when DRX is not used 2813

A.13.3.2.3.1 Test Purpose and Environment 2813

A.13.3.2.3.2 Test Requirements 2819

A.13.3.2.4 Event triggered reporting tests for FR1 with CCA without SSB time index detection when DRX is used 2819

A.13.3.2.4.1 Test Purpose and Environment 2819

A.13.3.2.4.2 Test Requirements 2824

A.13.3.2.5 Event triggered reporting tests for FR1 with CCA with SSB time index detection when DRX is not used 2825

A.13.3.2.5.1 Test Purpose and Environment 2825

A.13.3.2.5.2 Test Requirements 2830

A.13.3.2.6 Event triggered reporting tests for FR1 with CCA with SSB time index detection when DRX is used 2830

A.13.3.2.6.1 Test Purpose and Environment 2830

A.13.3.2.6.2 Test Requirements 2836

A.13.3.3 L1-RSRP measurements for beam reporting 2837

A.13.3.3.1 SSB based L1-RSRP measurement when DRX is not used 2837

A.13.3.3.1.1 Test Purpose and Environment 2837

A.13.3.3.1.2 Test parameters 2837

A.13.3.3.1.3 Test Requirements 2842

A.13.3.3.2 SSB based L1-RSRP measurement when DRX is used 2842

A.13.3.3.2.1 Test Purpose and Environment 2842

A.13.3.3.2.2 Test parameters 2842

A.13.3.3.2.3 Test Requirements 2846

A.13.4 Measurement performance 2846

A.13.4.1 SS-RSRP 2846

A.13.4.1.1 Intra-frequency measurement accuracy on a carrier frequency with CCA 2846

A.13.4.1.1.1 Test Purpose and Environment 2846

A.13.4.1.1.2 Test parameters 2846

A.13.4.1.1.3 Test Requirements 2848

A.13.4.2 SS-RSRQ 2848

A.13.4.2.1 Intra-frequency measurement accuracy on SCC 2848

A.13.4.2.1.1 Test Purpose and Environment 2848

A.13.4.2.1.2 Test Parameters 2848

A.13.4.2.1.3 Test Requirements 2856

A.13.4.3 SS-SINR 2856

A.13.4.3.1 Intra-frequency measurement accuracy on SCC 2856

A.13.4.3.1.1 Test Purpose and Environment 2856

A.13.4.3.1.2 Test Parameters 2856

A.13.4.3.1.3 Test Requirements 2862

A.13.4.4 L1-RSRP measurement for beam reporting with CCA serving cell 2863

A.13.4.4.1 SSB based L1-RSRP measurement 2863

A.13.4.4.1.1 Test Purpose and Environment 2863

A.13.4.4.1.2 Test parameters 2863

A.13.4.4.1.3 Test Requirements 2867

A.13.4.5 RSSI 2867

A.13.4.5.1 Intra-frequency RSSI measurement accuracy on a carrier with CCA 2867

A.13.4.5.1.1 Test Purpose and Environment 2867

A.13.4.5.1.2 Test parameters 2867

A.13.4.5.1.3 Test Requirements 2871

A.13.4.5.2 Inter-frequency RSSI measurement accuracy on a carrier with CCA 2871

A.13.4.5.2.1 Test Purpose and Environment 2871

A.13.4.5.2.2 Test parameters 2871

A.13.4.5.2.3 Test Requirements 2875

A.13.4.6 Channel occupancy 2875

A.13.4.6.1 Intra-frequency channel occupancy measurement accuracy on SCC with CCA 2875

A.13.4.6.1.1 Test Purpose and Environment 2875

A.13.4.6.1.2 Test parameters 2875

A.13.4.6.1.3 Test Requirements 2879

A.13.4.6.2 Inter-frequency channel occupancy measurement accuracy on a carrier with CCA 2879

A.13.4.6.2.1 Test Purpose and Environment 2879

A.13.4.6.2.2 Test parameters 2879

A.13.4.6.2.3 Test Requirements 2883

Annex B (normative): Conditions for RRM requirements applicability for operating bands 1818

B.1 Conditions for NR RRC\_IDLE state mobility 1818

B.1.1 Introduction 1818

B.1.2 Conditions for measurements on NR intra-frequency cells for cell re-selection 1818

B.1.3 Conditions for measurements on NR inter-frequency cells for cell re-selection 1819

B.2 Conditions for UE measurements procedures and performance requirements in RRC\_CONNECTED state 1820

B.2.1 Introduction 1820

B.2.1.1 General 1820

B.2.1.2 Derivation of Minimum SSB\_RP values for FR1 1820

B.2.1.3 Derivation of Minimum SSB\_RP values for FR2 1820

B.2.1.3.1 Minimum SSB\_RP values for Rx Beam Peak angle of arrival 1820

B.2.1.3.2 Minimum SSB\_RP values for angle of arrival within Spherical coverage 1821

B.2.1.4 Gain to SS-RSRP and CSI-RSRP measurement point for FR1 1821

B.2.1.5 Gain to SS-RSRP and CSI-RSRP measurement point for FR2 1822

B.2.1.5.1 Gain to SS-RSRP and CSI-RSRP measurement point for Rx Beam Peak angle of arrival 1822

B.2.1.5.2 Gain to SS-RSRP measurement point for different frequency 1822

B.2.1.5.3 Alignment of Rough beam to Rx beam Peak 1822

B.2.1.6 Gain to PRS-RSRP measurement point for FR2 1823

B.2.1.6.1 Gain to PRS-RSRP measurement point for Rx Beam Peak angle of arrival 1823

B.2.2 Conditions for NR intra-frequency measurements 1824

B.2.3 Conditions for NR inter-frequency measurements 1825

B.2.4 Conditions for NR L1-RSRP reporting 1826

B.2.4.1 Conditions for SSB based L1-RSRP reporting 1826

B.2.4.2 Conditions for CSI-RS based L1-RSRP reporting 1827

B.2.5 Conditions for RRC connection release with redirection to NR 1829

B.2.6 Void 1830

B.2.6.1 Void 1830

B.2.6.2 Void 1830

B.2.7 Conditions for SRS-RSRP measurements 1830

B.2.8 Conditions for NR L1-SINR reporting 1831

B.2.8.1 Conditions for L1-SINR reporting with CSI-RS based CMR and no dedicated IMR configured 1831

B.2.8.2 Conditions for L1-SINR reporting with SSB based CMR and dedicated IMR configured 1832

B.2.8.2.1 L1-SINR reporting with SSB based CMR and dedicated ZP-IMR configured 1832

B.2.8.2.2 L1-SINR reporting with SSB based CMR and dedicated NZP-IMR configured 1832

B.2.8.3 Conditions for L1-SINR reporting with CSI-RS based CMR and dedicated IMR configured 1834

B.2.8.3.1 L1-SINR reporting with CSI-RS based CMR and dedicated ZP-IMR configured 1834

B.2.8.3.2 L1-SINR reporting with CSI-RS based CMR and dedicated NZP-IMR configured 1835

B.2.9 Conditions for NR intra-frequency measurements under CCA 1836

B.2.10 Conditions for NR inter-frequency measurements under CCA 1836

B.2.11 Conditions for NR L1-RSRP reporting under CCA 1836

B.2.11.1 Conditions for SSB based L1-RSRP reporting 1836

B.2.12 Conditions for NR CSI-RS based intra-frequency measurements 1837

B.2.13 Conditions for NR CSI-RS based inter-frequency measurements 1838

B.2.14 Conditions for NR PRS-based measurements 1840

B.3 RRM Requirements Exceptions 1841

B.3.1 Introduction 1841

B.3.2 Receiver sensitivity relaxation for CA 1841

B.3.2.1 Receiver sensitivity relaxation for UE supporting CA in FR1 1841

B.3.2.2 Receiver sensitivity relaxation for UE configured with CA in FR1 1842

B.3.2.2.1 Inter-band carrier aggregation 1842

B.3.2.2.2 Reference sensitivity exceptions due to UL harmonic interference for CA 1842

B.3.2.2.3 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 1842

B.3.2.3 Receiver sensitivity relaxation for UE supporting CA in FR2 1842

B.3.2.4 Receiver sensitivity relaxation for UE configured with CA in FR2 1842

B.3.2.4.1 Intra-band contiguous carrier aggregation 1842

B.3.2.4.2 Intra-band non-contiguous carrier aggregation 1843

B.3.3 Receiver sensitivity relaxation for DC 1843

B.3.3.1 Receiver sensitivity relaxation for EN-DC 1843

B.3.3.2 Receiver sensitivity relaxation for NE-DC 1843

B.3.4 Receiver sensitivity relaxation for SUL 1843

B.3.4.1 Receiver sensitivity relaxation for UE supporting SUL in FR1 1843

B.3.4.2 Receiver sensitivity relaxation for UE configured with SUL in FR1 1843

B.3.4.2.1 Reference sensitivity exceptions due to UL harmonic interference for SUL 1843

B.4 Conditions for V2X 1843

B.4.1 Test parameters for GNSS signals 1843

B.4.2 Conditions for PSBCH-RSRP Accuracy Requirements 1844

B.4.3 Conditions for Selection/Reselection to Intra-frequency SyncRef UE 1844

B.4.4 Conditions for L1 SL-RSRP Accuracy Requirements 1844

Annex C (informative): Change history 1846