3GPP TS 36.213 V16.9.0 (2022-09)

Technical Specification

3rd Generation Partnership Project;

Technical Specification Group Radio Access Network;

Evolved Universal Terrestrial Radio Access (E-UTRA);

Physical layer procedures

(Release 16)

** 

The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.  
The present document has not been subject to any approval process by the 3GPPOrganisational Partners and shall not be implemented.  
This Specification is provided for future development work within 3GPPonly. The Organisational Partners accept no liability for any use of this Specification.  
Specifications and reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organisational Partners' Publications Offices.

Keywords

E-UTRA, radio, layer 1

***3GPP***

Postal address

3GPP support office address

650 Route des Lucioles – Sophia Antipolis

Valbonne – France

Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16

Internet

http://www.3gpp.org

***Copyright Notification***

No part may be reproduced except as authorized by written permission.  
The copyright and the foregoing restriction extend to reproduction in all media.

© 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

All rights reserved.

UMTS™ is a Trade Mark of ETSI registered for the benefit of its members

3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  
LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners

GSM® and the GSM logo are registered and owned by the GSM Association

Contents

Foreword 8

1 Scope 9

2 References 9

3 Symbols and abbreviations 10

3.1 Symbols 10

3.2 Abbreviations 10

4 Synchronization procedures 12

4.1 Cell search 12

4.2 Timing synchronization 12

4.2.1 Radio link monitoring 12

4.2.2 Inter-cell synchronization 12

4.2.3 Transmission timing adjustments 12

4.3 Timing for Secondary Cell Activation / Deactivation 14

5 Power control 15

5.1 Uplink power control 15

5.1.1 Physical uplink shared channel 16

5.1.1.1 UE behaviour 16

5.1.1.2 Power headroom 31

5.1.2 Physical uplink control channel 34

5.1.2.1 UE behaviour 34

5.1.3 Sounding Reference Symbol (SRS) 40

5.1.3.1 UE behaviour 40

5.1.3.2 Power headroom for Type3 report 43

5.1.4 Power allocation for EUTRA dual connectivity 43

5.1.4.1 Dual connectivity power control Mode 1 44

5.1.4.2 Dual connectivity power control Mode 2 51

5.1.4a Power allocation for dual active protocol stack 55

5.1.5 Power allocation for PUCCH-SCell 56

5.2 Downlink power allocation 57

5.2.1 eNodeB Relative Narrowband TX Power (RNTP) restrictions 59

6 Random access procedure 61

6.1 Physical non-synchronized random access procedure 61

6.1.1 Timing 62

6.2 Random Access Response Grant 63

7 Physical downlink shared channel related procedures 68

7.1 UE procedure for receiving the physical downlink shared channel 69

7.1.1 Single-antenna port scheme 88

7.1.2 Transmit diversity scheme 88

7.1.3 Large delay CDD scheme 89

7.1.4 Closed-loop spatial multiplexing scheme 89

7.1.5 Multi-user MIMO scheme 89

7.1.5A Dual layer scheme 89

7.1.5B Up to 8 layer transmission scheme 89

7.1.6 Resource allocation 89

7.1.6.1 Resource allocation type 0 91

7.1.6.2 Resource allocation type 1 92

7.1.6.3 Resource allocation type 2 93

7.1.6.4 PDSCH starting position 96

7.1.6.4A PDSCH starting position for BL/CE UEs 98

7.1.6.5 Physical Resource Block (PRB) bundling 98

7.1.7 Modulation order and transport block size determination 100

7.1.7.1 Modulation order and redundancy version determination 103

7.1.7.2 Transport block size determination 109

7.1.7.2.1 Transport blocks not mapped to two or more layer spatial multiplexing 114

7.1.7.2.2 Transport blocks mapped to two-layer spatial multiplexing 123

7.1.7.2.3 Transport blocks mapped for DCI Format 1C and DCI Format 6-2 123

7.1.7.2.4 Transport blocks mapped to three-layer spatial multiplexing 124

7.1.7.2.5 Transport blocks mapped to four-layer spatial multiplexing 124

7.1.7.2.6 Transport blocks mapped for BL/CE UEs configured with CEModeB and PDSCH bandwidth up to 1.4MHz 125

7.1.7.2.7 Transport blocks mapped for BL/CE UEs *SystemInformationBlockType1-BR* 126

7.1.7.2.8 Transport blocks mapped for UEs configured with *ce-pdsch-maxBandwidth-config* value of 5 MHz or with *pdsch-MaxBandwidth-SC-MTCH* value of 24 PRBs 126

7.1.7.3 Redundancy Version determination for Format 1C 126

7.1.8 Storing soft channel bits 127

7.1.9 PDSCH resource mapping parameters 127

7.1.10 Antenna ports quasi co-location for PDSCH 129

7.1.11 PDSCH subframe assignment for BL/CE UE 130

7.2 UE procedure for reporting Channel State Information (CSI) 132

7.2.1 Aperiodic CSI Reporting using PUSCH 142

7.2.2 Periodic CSI Reporting using PUCCH 168

7.2.3 Channel Quality Indicator (CQI) definition 209

7.2.4 Precoding Matrix Indicator (PMI) definition 223

7.2.5 Channel-State Information – Reference Signal (CSI-RS) definition 251

7.2.6 Channel-State Information – Interference Measurement (CSI-IM) Resource definition 253

7.2.7 Zero Power CSI-RS Resource definition 253

7.2.8 CSI-RS Activation / Deactivation 253

7.3 UE procedure for reporting HARQ-ACK 254

7.3.1 FDD HARQ-ACK reporting procedure 258

7.3.2 TDD HARQ-ACK reporting procedure 263

7.3.2.1 TDD HARQ-ACK reporting procedure for same UL/DL configuration 263

7.3.2.2 TDD HARQ-ACK reporting procedure for different UL/DL configurations 279

7.3.3 FDD-TDD HARQ-ACK reporting procedure for primary cell frame structure type 1 286

7.3.4 FDD-TDD HARQ-ACK reporting procedure for primary cell frame structure type 2 288

8 Physical uplink shared channel related procedures 290

8.0 UE procedure for transmitting the physical uplink shared channel 291

8.0.1 Single-antenna port scheme 318

8.0.2 Closed-loop spatial multiplexing scheme 318

8.1 Resource allocation for PDCCH/EPDCCH/SPDCCH with uplink DCI format 319

8.1.1 Uplink resource allocation type 0 319

8.1.2 Uplink resource allocation type 1 320

8.1.3 Uplink resource allocation type 2 320

8.1.4 Uplink resource allocation type 3 321

8.1.5 Uplink resource allocation type 4 322

8.1.5.1 UL Resource Block Groups 322

8.1.6 Uplink resource allocation type 5 323

8.2 UE sounding procedure 325

8.3 UE HARQ-ACK procedure 337

8.3A Autonomous uplink feedback procedure 339

8.4 UE PUSCH hopping procedure 339

8.4.1 Type 1 PUSCH hopping 340

8.4.2 Type 2 PUSCH hopping 340

8.5 UE Reference Symbol (RS) procedure 341

8.6 Modulation order, redundancy version and transport block size determination 342

8.6.1 Modulation order and redundancy version determination 342

8.6.2 Transport block size determination 350

8.6.3 Control information MCS offset determination 357

8.7 UE transmit antenna selection 361

8.8 Transmission timing adjustments 361

9 Physical downlink control channel procedures 361

9.1 UE procedure for determining physical downlink control channel assignment 362

9.1.1 PDCCH assignment procedure 362

9.1.2 PHICH assignment procedure 366

9.1.3 Control Format Indicator (CFI) assignment procedure 369

9.1.4 EPDCCH assignment procedure 370

9.1.4.1 EPDCCH starting position 377

9.1.4.2 Antenna ports quasi co-location for EPDCCH 377

9.1.4.3 Resource mapping parameters for EPDCCH 378

9.1.4.4 PRB-pair indication for EPDCCH 378

9.1.5 MPDCCH assignment procedure 379

9.1.5.1 MPDCCH starting position 387

9.1.5.2 Antenna ports quasi co-location for MPDCCH 387

9.1.5.3 Preconfigured Uplink Resource ACK/fallback procedure 387

9.1.6 SPDCCH assignment procedure 387

9.1.6.1 Resource mapping parameters for SPDCCH 389

9.1.6.2 PRB-pair indication for SPDCCH 389

9.1.6.3 Physical Resource Block (PRB) bundling for DMRS-based SPDCCH 390

9.1.6.4 Antenna ports quasi co-location for DMRS-based SPDCCH 390

9.2 PDCCH/EPDCCH/MPDCCH/SPDCCH validation for semi-persistent scheduling 391

9.2A PDCCH/EPDCCH validation for autonomous uplink transmissions 393

9.3 PDCCH/EPDCCH/MPDCCH/SPDCCH control information procedure 394

10 Physical uplink control channel procedures 395

10.1 UE procedure for determining physical uplink control channel assignment 396

10.1.1 PUCCH format information 401

10.1.2 FDD HARQ-ACK feedback procedures 408

10.1.2.1 FDD HARQ-ACK procedure for one configured serving cell 408

10.1.2.2 FDD HARQ-ACK procedures for more than one configured serving cell 411

10.1.2.2.1 PUCCH format 1b with channel selection HARQ-ACK procedure 412

10.1.2.2.2 PUCCH format 3 HARQ-ACK procedure 415

10.1.2.2.3 PUCCH format 4 HARQ-ACK procedure 417

10.1.2.2.4 PUCCH format 5 HARQ-ACK procedure 420

10.1.3 TDD HARQ-ACK feedback procedures 421

10.1.3.1 TDD HARQ-ACK procedure for one configured serving cell 423

10.1.3.2 TDD HARQ-ACK procedure for more than one configured serving cell 437

10.1.3.2.1 PUCCH format 1b with channel selection HARQ-ACK procedure 437

10.1.3.2.2 PUCCH format 3 HARQ-ACK procedure 453

10.1.3.2.3 PUCCH format 4 HARQ-ACK procedure 461

10.1.3.2.4 PUCCH format 5 HARQ-ACK procedure 477

10.1.3A FDD-TDD HARQ-ACK feedback procedures for primary cell frame structure type 2 477

10.1.4 HARQ-ACK Repetition procedure 479

10.1.5 Scheduling Request (SR) procedure 480

10.2 Uplink HARQ-ACK timing 482

11 Physical Multicast Channel (PMCH) related procedures 488

11.1 UE procedure for receiving the PMCH 488

11.2 UE procedure for receiving MCCH and system information change notification 491

12 Assumptions independent of physical channel 491

13 Uplink/Downlink configuration determination procedure for Frame Structure Type 2 492

13.1 UE procedure for determining eIMTA-uplink/downlink configuration 493

13A Subframe configuration for Frame Structure Type 3 494

14 UE procedures related to Sidelink 497

14.1 Physical Sidelink Shared Channel related procedures 498

14.1.1 UE procedure for transmitting the PSSCH 498

14.1.1.1 UE procedure for determining subframes for transmitting PSSCH for sidelink transmission mode 1 500

14.1.1.1.1 Determination of subframe indicator bitmap 500

14.1.1.2 UE procedure for determining resource blocks for transmitting PSSCH for sidelink transmission mode 1 503

14.1.1.2.1 PSSCH resource allocation for sidelink transmission mode 1 503

14.1.1.2.2 PSSCH frequency hopping for sidelink transmission mode 1 504

14.1.1.3 UE procedure for determining subframes for transmitting PSSCH for sidelink transmission mode 2 504

14.1.1.4 UE procedure for determining resource blocks for transmitting PSSCH for sidelink transmission mode 2 505

14.1.1.4A UE procedure for determining subframes and resource blocks for transmitting PSSCH for sidelink transmission mode 3 505

14.1.1.4B UE procedure for determining subframes and resource blocks for transmitting PSSCH and reserving resources for sidelink transmission mode 4 506

14.1.1.4C UE procedure for determining subframes and resource blocks for PSSCH transmission associated with an SCI format 1 506

14.1.1.5 UE procedure for PSSCH power control 507

14.1.1.6 UE procedure for determining the subset of resources to be reported to higher layers in PSSCH resource selection in sidelink transmission mode 4 and in sensing measurement in sidelink transmission mode 3 509

14.1.1.7 Conditions for selecting resources when the number of HARQ transmissions is two in sidelink transmission mode 4 512

14.1.2 UE procedure for receiving the PSSCH 512

14.1.3 UE procedure for determining resource block pool and subframe pool for sidelink transmission mode 2 513

14.1.5 UE procedure for determining resource block pool and subframe pool for sidelink transmission mode 3 and 4 514

14.2 Physical Sidelink Control Channel related procedures 515

14.2.1 UE procedure for transmitting the PSCCH 515

14.2.1.1 UE procedure for determining subframes and resource blocks for transmitting PSCCH for sidelink transmission mode 1 518

14.2.1.2 UE procedure for determining subframes and resource blocks for transmitting PSCCH for sidelink transmission mode 2 518

14.2.1.3 UE procedure for PSCCH power control 518

14.2.2 UE procedure for receiving the PSCCH 520

14.2.3 UE procedure for determining resource block pool and subframe pool for PSCCH 520

14.2.4 UE procedure for determining resource block pool for PSCCH in sidelink transmission mode 3 and 4 521

15 Void 524

16 UE Procedures related to narrowband IoT 525

16.1 Synchronization procedures 525

16.1.1 Cell search 525

16.1.2 Timing synchronization 525

16.2 Power control 525

16.2.1 Uplink power control 525

16.2.1.1 Narrowband physical uplink shared channel 525

16.2.1.1.1 UE behaviour 525

16.2.1.1.2 Power headroom 526

16.2.1.2 SR 527

16.2.1.2.1 UE behaviour 527

16.2.2 Downlink power allocation 527

16.3 Random access procedure 528

16.3.1 Physical non-synchronized random access procedure 528

16.3.2 Timing 528

16.3.3 Narrowband random access response grant 529

16.4 Narrowband physical downlink shared channel related procedures 531

16.4.1 UE procedure for receiving the narrowband physical downlink shared channel 531

16.4.1.1 Single-antenna port scheme 535

16.4.1.2 Transmit diversity scheme 535

16.4.1.3 Resource allocation 535

16.4.1.4 NPDSCH starting position 538

16.4.1.5 Modulation order and transport block size determination 539

16.4.1.5.1 Transport blocks not mapped for *SystemInformationBlockType1-NB* 539

16.4.1.5.2 Transport blocks mapped for *SystemInformationBlockType1-NB* 540

16.4.2 UE procedure for reporting ACK/NACK 540

16.5 Narrowband physical uplink shared channel related procedures 542

16.5.1 UE procedure for transmitting format 1 narrowband physical uplink shared channel 542

16.5.1.1 Resource allocation 545

16.5.1.2 Modulation order, redundancy version and transport block size determination 546

16.5.2 UE procedure for NPUSCH retransmission 548

16.5.3 UE procedure for transmitting SR 548

16.6 Narrowband physical downlink control channel related procedures 548

16.6.1 NPDCCH starting position 554

16.6.2 NPDCCH control information procedure 554

16.6.3 NPDCCH validation for semi-persistent scheduling 555

16.6.4 Preconfigured uplink resource ACK/fallback procedure 555

16.7 Assumptions independent of physical channel related to narrowband IoT 555

16.8 UE procedure for acquiring cell-specific reference signal sequence and raster offset 555

16.9 UE procedure for receiving narrowband wake up signal 556

17 Wake-up signal related procedures for BL/CE UE 557

Annex A (informative): Change history 558