|  |  |
| --- | --- |
| 3GPP TS 38.101-3 V17.8.0 (2022-12) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 3: Range 1 and Range 2 Interworking operation with other radios  (Release 17) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 18

1 Scope 20

2 References 20

3 Definitions, symbols and abbreviations 21

3.1 Definitions 21

3.2 Symbols 21

3.3 Abbreviations 21

4 General 22

4.1 Relationship between minimum requirements and test requirements 22

4.2 Applicability of minimum requirements 23

4.3 Specification suffix information 24

5 Operating bands and channel arrangement 24

5.1 General 24

5.2 Operating bands 24

5.2A Operating bands for CA 25

5.2A.1 Inter-band CA between FR1 and FR2 25

5.2B Operating bands for DC 28

5.2B.1 General 28

5.2B.2 Void 29

5.2B.3 Void 29

5.2B.4 Void 29

5.2B.5 Void 29

5.2B.6 Void 29

5.2B.7 Void 29

5.2E Operating bands for V2X 29

5.2E.1 Intra-band V2X bands 29

5.2E.2 Inter-band V2X bands 29

5.3 UE Channel bandwidth 30

5.3A UE Channel bandwidth for CA 30

5.3A.1 Inter-band CA between FR1 and FR2 30

5.3B UE Channel bandwidth for EN-DC 30

5.3B.0 General 30

5.3B.1 Intra-band EN-DC in FR1 31

5.3B.1.1 General 31

5.3B.1.2 BCS for Intra-band contiguous EN-DC 31

5.3B.1.3 BCS for Intra-band non-contiguous EN-DC 35

5.3C Void 39

5.3D Void 39

5.3E UE Channel bandwidth for V2X 39

5.3E.0 General 39

5.3E.1 Intra-band contiguous V2X in FR1 40

5.3E.2 Intra-band non-contiguous V2X in FR1 40

5.3E.3 Inter-band V2X in FR1 40

5.4 Void 40

5.4A Channel arrangement for CA 40

5.4B Channel arrangement for DC 41

5.4B.0 General 41

5.4B.1 Channel spacing for intra-band EN-DC carriers 41

5.5 Configuration 42

5.5A Configuration for CA 42

5.5A.1 Inter-band CA configurations between FR1 and FR2 42

5.5B Configuration for DC 333

5.5B.1 General 333

5.5B.2 Intra-band contiguous EN-DC 334

5.5B.3 Intra-band non-contiguous EN-DC 334

5.5B.4 Inter-band EN-DC within FR1 336

5.5B.4.1 Inter-band EN-DC configurations within FR1 (two bands) 336

5.5B.4.2 Inter-band EN-DC configurations within FR1 (three bands) 347

5.5B.4.3 Inter-band EN-DC configurations within FR1 (four bands) 387

5.5B.4.4 Inter-band EN-DC configurations within FR1 (five bands) 440

5.5B.4.5 Inter-band EN-DC configurations within FR1 (six bands) 467

5.5B.4a Inter-band NE-DC within FR1 472

5.5B.4a.1 Inter-band NE-DC configurations within FR1 (two bands) 472

5.5B.4a.2 Inter-band NE-DC configurations within FR1 (three bands) 473

5.5B.4a.3 Inter-band NE-DC configurations within FR1 (four bands) 474

5.5B.4a.4 Inter-band NE-DC configurations within FR1 (five bands) 474

5.5B.5 Inter-band EN-DC including FR2 475

5.5B.5.1 Inter-band EN-DC configurations including FR2 (two bands) 475

5.5B.5.2 Inter-band EN-DC configurations including FR2 (three bands) 506

5.5B.5.3 Inter-band EN-DC configurations including FR2 (four bands) 545

5.5B.5.4 Inter-band EN-DC configurations including FR2 (five bands) 580

5.5B.5.5 Void 592

5.5B.5a Inter-band NE-DC including FR2 592

5.5B.5a.1 Inter-band NE-DC configurations including FR2 (two bands) 592

5.5B.5a.2 Inter-band NE-DC configurations including FR2 (three bands) 594

5.5B.5a.3 Inter-band NE-DC configurations including FR2 (four bands) 598

5.5B.5a.4 Inter-band NE-DC configurations including FR2 (five bands) 600

5.5B.6 Inter-band EN-DC including FR1 and FR2 601

5.5B.6.1 Void 601

5.5B.6.2 Inter-band EN-DC configurations including FR1 and FR2 (three bands) 601

5.5B.6.3 Inter-band EN-DC configurations including FR1 and FR2 (four bands) 616

5.5B.6.4 Inter-band EN-DC configurations including FR1 and FR2 (five bands) 641

5.5B.6.5 Inter-band EN-DC configurations including FR1 and FR2 (six bands) 660

5.5B.7 Inter-band NR-DC between FR1 and FR2 665

5.5B.7.0 General 665

5.5B.7.1 Inter-band NR-DC configurations between FR1 and FR2 (two bands) 666

5.5B.7.2 Inter-band NR-DC configurations between FR1 and FR2 (three bands) 681

5.5B.7.3 Inter-band NR-DC configurations between FR1 and FR2 (four bands) 696

5.5C Void 700

5.5D Void 700

5.5E Configuration for V2X operation 700

5.5E.1 General 700

5.5E.2 Intra-band contiguous V2X operation in FR1 701

5.5E.3 Intra-band non-contiguous V2X operation in FR1 701

5.5E.4 Inter-band V2X operation in FR1 701

5.5E.4.1 Inter-band V2X configurations within FR1 (two bands) 701

6 Transmitter characteristics 692

6.1 General 692

6.2 Void 692

6.2A Transmitter power for CA 692

6.2A.1 UE maximum output power for CA 692

6.2A.1.1 Inter-band CA between FR1 and FR2 692

6.2A.2 UE maximum output power reduction for CA 692

6.2A.2.1 Inter-band CA between FR1 and FR2 692

6.2A.3 UE additional maximum output power reduction for CA 692

6.2A.4 Configured output power for CA 692

6.2A.4.1 Configured output power level 692

6.2A.4.2 ΔTIB,c for CA 693

6.2A.4.2.1 ΔTIB,c for Inter-band CA between FR1 and FR2 693

6.2B Transmitter power for DC 693

6.2B.1 UE maximum output power for DC 693

6.2B.1.1 Intra-band contiguous EN-DC 693

6.2B.1.2 Intra-band non-contiguous EN-DC 695

6.2B.1.3 Inter-band EN-DC within FR1 696

6.2B.1.3a Inter-band NE-DC within FR1 703

6.2B.1.4 Inter-band EN-DC including FR2 704

6.2B.1.4a Inter-band NE-DC including FR2 704

6.2B.1.5 Inter-band EN-DC including both FR1 and FR2 704

6.2B.2 UE maximum output power reduction for DC 704

6.2B.2.0 General 704

6.2B.2.1 Intra-band contiguous EN-DC 705

6.2B.2.1.1 General 705

6.2B.2.1.2 MPR for power class 3 and power class 2 705

6.2B.2.2 Intra-band non-contiguous EN-DC 706

6.2B.2.2.1 General 706

6.2B.2.2.2 MPR for power class 3 and power class 2 707

6.2B.2.3 Inter-band EN-DC within FR1 707

6.2B.2.3a Inter-band NE-DC within FR1 707

6.2B.2.4 Inter-band EN-DC including FR2 707

6.2B.2.4a Inter-band NE-DC including FR2 708

6.2B.2.5 Inter-band EN-DC including both FR1 and FR2 708

6.2B.3 UE additional maximum output power reduction for EN-DC 708

6.2B.3.1 Intra-band contiguous EN-DC 708

6.2B.3.1.0 General 708

6.2B.3.1.1 A-MPR for DC\_(n)71AA 708

6.2B.3.1.2 A-MPR for NS\_04 710

6.2B.3.2 Intra-band non-contiguous EN-DC 712

6.2B.3.2.0 General 712

6.2B.3.2.1 A-MPR for NS\_04 712

6.2B.3.3 Inter-band EN-DC within FR1 714

6.2B.3.3A Inter-band NE-DC within FR1 717

6.2B.3.4 Inter-band EN-DC including FR2 718

6.2B.3.4A Inter-band NE-DC including FR2 718

6.2B.3.5 Inter-band EN-DC including both FR1 and FR2 718

6.2B.4 Configured output power for DC 718

6.2B.4.1 Configured output power level 718

6.2B.4.1.1 Intra-band contiguous EN-DC 718

6.2B.4.1.2 Intra-band non-contiguous EN-DC 723

6.2B.4.1.3a Inter-band NE-DC within FR1 728

6.2B.4.1.4 Inter-band EN-DC including FR2 731

6.2B.4.1.4a Inter-band NE-DC including FR2 731

6.2B.4.1.5 Inter-band EN-DC including both FR1 and FR2 731

6.2B.4.2 ΔTIB,c for DC 731

6.2B.4.2.0 General 731

6.2B.4.2.1 Intra-band contiguous EN-DC 732

6.2B.4.2.2 Intra-band non-contiguous EN-DC 732

6.2B.4.2.3 Inter-band EN-DC within FR1 733

6.2B.4.2.3.1 ΔTIB,c for EN-DC two bands 733

6.2B.4.2.3.2 ΔTIB,c for EN-DC three bands 742

6.2B.4.2.3.3 ΔTIB,c for EN-DC four bands 778

6.2B.4.2.3.4 ΔTIB,c for EN-DC five bands 820

6.2B.4.2.3.5 ΔTIB,c for EN-DC six bands 839

6.2B.4.2.3a Inter-band NE-DC within FR1 841

6.2B.4.2.4 Inter-band EN-DC including FR2 842

6.2B.4.2.4.1 ΔTIB,c for EN-DC two bands 842

6.2B.4.2.4.2 ΔTIB,c for EN-DC three bands 842

6.2B.4.2.4.3 ΔTIB,c for EN-DC four bands 842

6.2B.4.2.4.4 ΔTIB,c for EN-DC five bands 842

6.2B.4.2.4.5 Void 842

6.2B.4.2.4a Inter-band NE-DC including FR2 842

6.2B.4.2.5 Inter-band EN-DC including both FR1 and FR2 842

6.2B.4.2.5.1 ΔTIB,c for EN-DC three bands 842

6.2B.4.2.5.2 ΔTIB,c for EN-DC four bands 843

6.2B.4.2.5.3 ΔTIB,c for EN-DC five bands 843

6.2B.4.2.5.4 ΔTIB,c for EN-DC six bands 843

6.2B.5 Configured output power for NR-DC 843

6.2B.5.1 Configured output power level 843

6.2B.5.1.1 Inter-band NR-DC between FR1 and FR2 843

6.2E Transmitter power for V2X in FR1 843

6.2E.1 UE maximum output power for V2X 843

6.2E.1.1 UE maximum output power for Intra-band contiguous V2X 843

6.2E.1.2 UE maximum output power for Intra-band non-contiguous V2X 843

6.2E.1.3 UE maximum output power for Inter-band V2X 844

6.2E.2 UE maximum output power reduction for V2X 844

6.2E.2.1 UE maximum output power reduction for Intra-band V2X 844

6.2E.2.2 UE maximum output power reduction for Inter-band V2X 844

6.2E.3 UE additional maximum output power reduction for V2X 845

6.2E.3.1 UE additional maximum output power reduction for Intra-band V2X 845

6.2E.3.2 UE additional maximum output power reduction for Inter-band V2X 845

6.2E.4 Configured output power for V2X 845

6.2E.4.1 UE configured output power for Intra-band V2X 845

6.2E.4.2 UE configured output power for Inter-band V2X 845

6.3 Output power dynamics 846

6.3A Output power dynamics for CA 846

6.3B Output power dynamics for DC 846

6.3B.0 General 846

6.3B.1 Output power dynamics for EN-DC with UL sharing from UE perspective 847

6.3B.1.1 E-UTRA and NR switching time mask for TDM based UL sharing from UE perspective 847

6.3B.1a Output power dynamics for NE-DC with UL sharing from UE perspective 848

6.3B.2 Output power dynamics for intra-band EN-DC without dual PA capability 848

6.3B.3 Output power dynamics for intra-band EN-DC with dual PA capability 849

6.3B.4 Output power dynamics for switching between two uplink carriers 849

6.3B.4.1 E-UTRA and NR switching time mask between two uplink carriers 849

6.3B.5 Output power dynamics for inter-band EN-DC 850

6.3E Output power dynamics for V2X 851

6.3E.1 General 851

6.3E.2 Output power dynamics for intra-band V2X operation 851

6.3E.3 Output power dynamics for inter-band V2X con-current operation 851

6.4 Void 851

6.4A Transmit signal quality for CA 851

6.4A.1 Frequency error for CA 851

6.4A.2 Transmit modulation quality for CA 851

6.4B Transmit signal quality for DC 852

6.4B.1 Frequency error for DC 852

6.4B.1.1 Frequency error for Intra-band contiguous EN-DC 852

6.4B.1.2 Frequency error for Intra-band non-contiguous EN-DC 852

6.4B.1.3 Frequency error for inter-band EN-DC within FR1 852

6.4B.1.3a Frequency error for inter-band NE-DC within FR1 852

6.4B.1.4 Frequency error for inter-band EN-DC including FR2 852

6.4B.1.4a Frequency error for inter-band NE-DC including FR2 852

6.4B.1.5 Frequency error for inter-band EN-DC including both FR1 and FR2 852

6.4B.2 Transmit modulation quality for DC 852

6.4B.2.1 Transmit modulation quality for Intra-band contiguous EN-DC 852

6.4B.2.1.1 Error Vector Magnitude 852

6.4B.2.1.2 Carrier leakage 853

6.4B.2.1.3 In-band emissions 853

6.4B.2.2 Transmit modulation quality for Intra-band non-contiguous EN-DC 853

6.4B.2.2.1 Error Vector Magnitude 853

6.4B.2.2.2 Carrier leakage 853

6.4B.2.2.3 In-band emissions 853

6.4B.2.3a Transmit modulation quality for Inter-band NE-DC within FR1 853

6.4B.2.4 Transmit modulation quality for Inter-band EN-DC including FR2 854

6.4B.2.4a Transmit modulation quality for Inter-band NE-DC including FR2 854

6.4B.2.5 Transmit modulation quality for inter-band EN-DC including both FR1 and FR2 854

6.4E Transmit signal quality for V2X operation in FR1 854

6.4E.1 Frequency error for V2X 854

6.4E.2 Transmit modulation quality for V2X 854

6.4E.2.1 Transmit modulation quality for Intra-band V2X 854

6.4E.2.2.1 Error Vector Magnitude 854

6.4E.2.2.2 Carrier leakage 855

6.4E.2.2.3 In-band emissions 855

6.4E.2.2 Transmit modulation quality for Inter-band V2X 855

6.5 Void 855

6.5A Output RF spectrum emissions for CA 855

6.5A.1 Occupied bandwidth for CA 855

6.5A.2 Out-of-band emissions for CA 855

6.5A.3 Spurious emissions for CA 855

6.5A.3.1 Inter-band CA between FR1 and FR2 855

6.5A.4 Transmit intermodulation for CA 855

6.5B Output RF spectrum emissions for DC 855

6.5B.1 Occupied bandwidth for EN-DC 855

6.5B.1.1 Intra-band contiguous EN-DC 855

6.5B.1.2 Intra-band non-contiguous EN-DC 856

6.5B.1.3 Inter-band EN-DC within FR1 856

6.5B.1.3a Inter-band NE-DC within FR1 856

6.5B.1.4 Inter-band EN-DC including FR2 856

6.5B.1.4a Inter-band NE-DC including FR2 856

6.5B.1.5 Inter-band EN-DC including both FR1 and FR2 856

6.5B.2 Out-of-band emissions for DC 856

6.5B.2.1 Intra-band contiguous EN-DC 856

6.5B.2.1.1 Spectrum emissions mask 856

6.5B.2.1.2 Additional spectrum emissions mask 857

6.5B.2.1.2.1 Requirements for network signalled value "NS\_35" 857

6.5B.2.1.2.2 Requirements for network signalled value "NS\_04" 857

6.5B.2.1.3 Adjacent channel leakage ratio 858

6.5B.2.2 Intra-band non-contiguous EN-DC 858

6.5B.2.2.1 Spectrum emissions mask 858

6.5B.2.2.2 Additional spectrum emissions mask 858

6.5B.2.2.3 Adjacent channel leakage ratio 858

6.5B.2.3 Inter-band EN-DC within FR1 858

6.5B.2.3a Inter-band NE-DC within FR1 858

6.5B.2.4 Inter-band EN-DC including FR2 859

6.5B.2.4a Inter-band NE-DC including FR2 859

6.5B.2.5 Inter-band EN-DC including both FR1 and FR2 859

6.5B.3 Spurious emissions for DC 859

6.5B.3.1 Intra-band contiguous EN-DC 859

6.5B.3.1.1 General spurious emissions 859

6.5B.3.1.2 Spurious emission band UE co-existence 859

6.5B.3.2 Intra-band non-contiguous EN-DC 860

6.5B.3.2.1 General spurious emissions 860

6.5B.3.2.2 Spurious emission band UE co-existence 860

6.5B.3.3 Inter-band EN-DC within FR1 861

6.5B.3.3.2 Spurious emission band UE co-existence 862

6.5B.3.3a Inter-band NE-DC within FR1 896

6.5B.3.3a.1 General spurious emissions 896

6.5B.3.3a.2 Spurious emission band UE co-existence 896

6.5B.3.4 Inter-band EN-DC including FR2 898

6.5B.3.4.0 General spurious emission 898

6.5B.3.4.1 Spurious emission band UE co-existence 898

6.5B.3.4a Inter-band NE-DC including FR2 898

6.5B.3.4a.1 Spurious emission band UE co-existence 898

6.5B.3.5 Inter-band EN-DC including both FR1 and FR2 898

6.5B.3.5.0 General spurious emission 898

6.5B.3.5.1 Spurious emission band UE co-existence 898

6.5B.4 Additional spurious emissions 899

6.5B.4.1 General 899

6.5B.4.1.1 Void 899

6.5B.4.2 Intra-band contiguous EN-DC 899

6.5B.4.2.1 Minimum requirement (network signalled value "NS\_04") 899

6.5B.4.3 Intra-band non-contiguous EN-DC 899

6.5B.4.3.1 Minimum requirement (network signalled value "NS\_04") 899

6.5B.4.4 Inter-band EN-DC within FR1 900

6.5B.4.4a Inter-band NE-DC within FR1 900

6.5B.4.5 Inter-band EN-DC including FR2 900

6.5B.4.6 Inter-band EN-DC including both FR1 and FR2 900

6.5B.5 Transmit intermodulation for DC 900

6.5B.5.1 Intra-band contiguous EN-DC 900

6.5B.5.2 Intra-band non-contiguous EN-DC 900

6.5B.5.3 Inter-band EN-DC within FR1 900

6.5B.5.3a Inter-band NE-DC within FR1 900

6.5B.5.4 Inter-band EN-DC including FR2 900

6.5B.5.4a Inter-band NE-DC including FR2 900

6.5B.5.5 Inter-band EN-DC including both FR1 and FR2 901

6.5E Output RF spectrum emissions for V2X operation in FR1 901

6.5E.1 Occupied bandwidth 901

6.5E.1.1 Intra-band V2X 901

6.5E.1.2 inter-band V2X con-current operation 901

6.5E.2 Out-of-band emissions 901

6.5E.2.1 Intra-band V2X 901

6.5E.2.2 Inter-band V2X con-current operation 901

6.5E.3 Spurious emissions 901

6.5E.3.1 Intra-band V2X 901

6.5E.3.1.1 General spurious emissions 901

6.5E.3.1.2 Spurious emission band UE co-existence 901

6.5E.3.2 Inter-band V2X con-current operation 901

6.5E.3.2.1 General spurious emissions 901

6.5E.3.2.2 Spurious emission band UE co-existence 902

6.5E.4 Transmit intermodulation 904

6.5E.4.1 Intra-band V2X 904

6.5E.4.2 Inter-band V2X con-current operation 904

6.6B Beam correspondence for DC 904

6.6B.1 Void 904

6.6B.2 Void 904

6.6B.3 Void 904

6.6B.4 Inter-band EN-DC including FR2 904

6.6B.4a Inter-band NE-DC including FR2 904

6.6B.5 Inter-band EN-DC including both FR1 and FR2 904

7 Receiver characteristics 905

7.1 General 905

7.2 Void 906

7.3 Void 906

7.3A Reference sensitivity for CA 906

7.3A.1 General 906

7.3A.2 Reference sensitivity power level for CA 906

7.3A.3 ΔRIB,c for CA 906

7.3A.3.1 ΔRIB,c for Inter-band CA between FR1 and FR2 906

7.3A.4 Void 907

7.3B Reference sensitivity level for DC 907

7.3B.1 General 907

7.3B.2 Reference sensitivity for DC 907

7.3B.2.1 Intra-band contiguous EN-DC 907

7.3B.2.2 Intra-band non-contiguous EN-DC 909

7.3B.2.3 Inter-band EN-DC within FR1 909

7.3B.2.3.0 General 909

7.3B.2.3.1 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1 909

7.3B.2.3.2 Reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1 916

7.3B.2.3.3 Void 919

7.3B.2.3.4 Reference sensitivity exceptions due to cross band isolation for EN-DC in NR FR1 919

7.3B.2.3.5 MSD for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 926

7.3B.2.3.5.1 MSD test points for intermodulation interference due to dual uplink operation for PC3 EN-DC in NR FR1 involving two bands 927

7.3B.2.3.5.2 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving three bands 936

7.3B.2.3.5.3 Void 1057

7.3B.2.3.5.4 MSD test points for intermodulation interference due to dual uplink operation for EN-DC in NR FR1 involving four bands 1057

7.3B.2.3.6 Reference sensitivity exceptions due to Tx non-linearity interference in 1st or 2nd adjacent channel of UL band for EN-DC in NR FR1 1057

7.3B.2.3a Inter-band NE-DC within FR1 1058

7.3B.2.3a.0 General 1058

7.3B.2.3a.1 Reference sensitivity exceptions due to UL harmonic interference for NE-DC in NR FR1 1058

7.3B.2.3a.2 Reference sensitivity exceptions due to receiver harmonic mixing for NE-DC in NR FR1 1058

7.3B.2.3a.3 Reference sensitivity exceptions due to cross band isolation for NE-DC in NR FR1 1058

7.3B.2.3a.4 MSD for intermodulation interference due to dual uplink operation for NE-DC in NR FR1 1059

7.3B.2.4 Inter-band EN-DC including FR2 1059

7.3B.2.4.1 Void 1059

7.3B.2.5 Inter-band EN-DC including both FR1 and FR2 1059

7.3B.2.5.1 Reference sensitivity exceptions due to UL harmonic interference for EN-DC including both FR1 and FR2 1059

7.3B.3 ΔRIB,c, ΔRIBNC for DC 1059

7.3B.3.0 General 1059

7.3B.3.1 Intra-band contiguous EN-DC 1061

7.3B.3.2 Intra-band non-contiguous EN-DC 1061

7.3B.3.3 Inter-band EN-DC within FR1 1068

7.3B.3.3.1 ΔRIB,c for EN-DC in two bands 1068

7.3B.3.3.2 ΔRIB,c for EN-DC three bands 1072

7.3B.3.3.3 ΔRIB,c for EN-DC four bands 1093

7.3B.3.3.4 ΔRIB,c for EN-DC five bands 1124

7.3B.3.3.5 ΔRIB,c for EN-DC six bands 1139

7.3B.3.3a Inter-band NE-DC within FR1 1141

7.3B.3.4 Inter-band EN-DC including FR2 1141

7.3B.3.4.1 ΔRIB,c for EN-DC in two bands 1141

7.3B.3.4.2 ΔRIB,c for EN-DC three bands 1141

7.3B.3.4.3 ΔRIB,c for EN-DC four bands 1142

7.3B.3.4.4 ΔRIB,c for EN-DC five bands 1142

7.3B.3.4.5 Void 1142

7.3B.3.4a Inter-band NE-DC including FR2 1142

7.3B.3.5 Inter-band EN-DC including both FR1 and FR2 1142

7.3B.3.5.2 ΔRIB,c for EN-DC three bands 1142

7.3B.3.5.3 ΔRIB,c for EN-DC four bands 1142

7.3B.3.5.4 ΔRIB,c for EN-DC five bands 1142

7.3B.3.5.5 ΔRIB,c for EN-DC six bands 1142

7.3E Reference sensitivity for V2X operation in FR1 1143

7.3E.1 General 1143

7.3E.2 Reference sensitivity for V2X 1143

7.3E.2.1 Intra-band contiguous V2X 1143

7.3E.2.2 Intra-band non-contiguous V2X 1143

7.3E.2.3 Inter-band V2X con-current operation 1143

7.3E.2.3.0 General 1143

7.3E.2.3.1 Reference sensitivity exception due to UL harmonic problem 1144

7.4 Void 1145

7.4A Maximum input level for CA 1145

7.4B Maximum input level for DC in FR1 1145

7.4B.1 Intra-band contiguous EN-DC in FR1 1145

7.4B.2 Intra-band non-contiguous EN-DC in FR1 1145

7.4B.3 Inter-band EN-DC within FR1 1145

7.4B.3a Inter-band NE-DC within FR1 1145

7.4B.4 Inter-band EN-DC including FR2 1145

7.4B.4a Inter-band NE-DC including FR2 1145

7.4B.5 Inter-band EN-DC including both FR1 and FR2 1146

7.4E Maximum input level for V2X operation in FR1 1146

7.5 Void 1146

7.5A Adjacent channel selectivity for CA 1146

7.5B Adjacent channel selectivity for DC in FR1 1146

7.5B.1 Intra-band contiguous EN-DC in FR1 1146

7.5B.2 Intra-band non-contiguous EN-DC in FR1 1147

7.5B.3 Inter-band EN-DC within FR1 1147

7.5B.3a Inter-band NE-DC within FR1 1147

7.5B.4 Inter-band EN-DC including FR2 1147

7.5B.4a Inter-band NE-DC including FR2 1147

7.5E Adjacent channel selectivity for V2X operation in FR1 1148

7.6 Void 1148

7.6A Blocking characteristics for CA 1148

7.6B Blocking characteristics for DC in FR1 1148

7.6B.1 General 1148

7.6B.2 In-band blocking for DC in FR1 1148

7.6B.2.1 Intra-band contiguous EN-DC in FR1 1148

7.6B.2.2 Intra-band non-contiguous EN-DC in FR1 1148

7.6B.2.3 Inter-band EN-DC within FR1 1148

7.6B.2.3a Inter-band NE-DC within FR1 1149

7.6B.2.4 Inter-band EN-DC including FR2 1149

7.6B.2.4a Inter-band NE-DC including FR2 1149

7.6B.2.5 Inter-band EN-DC including both FR1 and FR2 1149

7.6B.2.6 Power imbalance for type 2 UE of inter-band EN-DC with overlapping DL bands 1149

7.6B.3 Out-of-band blocking for DC in FR1 1150

7.6B.3.1 Intra-band contiguous EN-DC in FR1 1150

7.6B.3.2 Intra-band non-contiguous EN-DC in FR1 1151

7.6B.3.3 Inter-band EN-DC within FR1 1151

7.6B.3.3a Inter-band NE-DC within FR1 1152

7.6B.3.4 Inter-band EN-DC including FR2 1152

7.6B.3.4a Inter-band NE-DC including FR2 1153

7.6B.3.5 Inter-band EN-DC including both FR1 and FR2 1153

7.6B.4 Narrow band blocking for DC in FR1 1153

7.6B.4.1 Intra-band contiguous EN-DC in FR1 1153

7.6B.4.2 Intra-band non-contiguous EN-DC in FR1 1153

7.6B.4.3 Inter-band EN-DC within FR1 1153

7.6B.4.3a Inter-band NE-DC within FR1 1153

7.6B.4.4 Inter-band EN-DC including FR2 1154

7.6B.4.4a Inter-band NE-DC including FR2 1154

7.6B.4.5 Inter-band EN-DC including both FR1 and FR2 1154

7.6E Blocking characteristics for V2X in FR1 1154

7.7 Void 1154

7.7A Spurious response for CA 1154

7.7B Spurious response for DC in FR1 1154

7.7B.1 Intra-band contiguous EN-DC in FR1 1154

7.7B.2 Intra-band non-contiguous EN-DC in FR1 1154

7.7B.3 Inter-band EN-DC within FR1 1155

7.7B.4a Inter-band NE-DC including FR2 1155

7.7B.5 Inter-band EN-DC including both FR1 and FR2 1155

7.7E Spurious response for V2X in FR1 1155

7.8 Void 1155

7.8A Intermodulation characteristics for CA 1155

7.8B Intermodulation characteristics for DC in FR1 1156

7.8B.1 General 1156

7.8B.2 Wide band Intermodulation 1156

7.8B.2.1 Intra-band contiguous EN-DC in FR1 1156

7.8B.2.2 Intra-band non-contiguous EN-DC in FR1 1156

7.8B.2.3 Inter-band EN-DC within FR1 1156

7.8B.2.3a Inter-band NE-DC within FR1 1156

7.8B.2.4 Inter-band EN-DC including FR2 1156

7.8B.2.4a Inter-band NE-DC including FR2 1156

7.8B.2.5 Inter-band EN-DC including both FR1 and FR2 1157

7.8E Intermodulation characteristics for V2X operation in FR1 1157

7.9 Void 1157

7.9A Spurious emissions for CA 1157

7.9B Spurious emissions for DC in FR1 1157

7.9B.1 Intra-band contiguous EN-DC in FR1 1157

7.9B.2 Intra-band non-contiguous EN-DC in FR1 1157

7.9B.3 Inter-band EN-DC within FR1 1157

7.9B.3a Inter-band NE-DC within FR1 1157

7.9B.4 Inter-band EN-DC including FR2 1157

7.9B.4a Inter-band NE-DC including FR2 1157

Annex A (normative): Measurement channels 1094

A.1 General 1094

A.2 UL reference measurement channels for E-UTRA TDD Config 2 1094

A.2.1 General 1094

A.2.2 Reference measurement channels for E-UTRA 1095

A.2.2.1 Full RB allocation 1095

A.2.2.1.1 QPSK 1095

A.2.2.1.2 16-QAM 1096

A.2.2.1.3 64-QAM 1097

A.2.2.1.4 256 QAM 1098

A.2.2.2 Partial RB allocation 1099

A.2.2.2.1 QPSK 1099

A.2.2.2.3 64-QAM 1105

A.2.2.2.4 256 QAM 1108

A.3 DL reference measurement channels for E-UTRA 1111

A.3.1 General 1111

A.3.1.1 QPSK 1112

A.3.1.2 64-QAM 1113

A.3.1.3 256-QAM 1114

Annex B: Void 1114

Annex C: Void 1114

Annex D: Void 1114

Annex E: Void 1115

Annex F: Void 1115

Annex G: Void 1115

Annex H (normative): Modified MPR behavior 1115

Annex I (normative): Dual uplink interferer 1116

Annex J: Void 1116

Annex K: Void 1116

Annex L (informative): Change history 1117