Email discussion [R16\_NR\_RRM]

# Topic #1: Rel-16 NR RRM Enhancements WI

## Initial comments

**Topic 1-1: Revised WID (RP-201112)**

* Background: Revised WID RP-201112 proposes to remove “Non-simultaneous UL carrier operation in FR2” objective from WID
* Companies are encouraged to give input on the need for such a modification.

|  |  |
| --- | --- |
| **Company Name** | **Comments** |
| Qualcomm | Revised WID is ok. |
| CATT | Ok with the Revised WID. |
| NTT DOCOMO | The proposed revision looks O.K to us |
| ZTE | WID revision is fine. |
| vivo | Ok with revised WID |
| Intel | We support the revision. |
| Nokia | The revised WID and removal of “Non-simultaneous UL carrier operation in FR2” objective are ok and it is aligned with the corresponding update to the FR2 UE RF WID |
|  |  |

**Topic 1-2: Exception sheet (RP-201113)**

* Background: Exception sheet provides a full list of remaining open issues.
* Companies are encouraged to provide comments whether the exception sheet includes all the remaining open issues, or anything is missing.

|  |  |
| --- | --- |
| **Company Name** | **Comments** |
| Qualcomm | Exception sheet is inclusive of all remaining open issues. |
| vivo | Exception sheets provides a full list of remaining open issues. |
| Intel | Exception sheet lists all the remaining open issues. It is OK. |
| Nokia | All the open items should be kept in the exception sheet as proposed |
|  |  |
|  |  |

**Topic 1-3: Down-scoping and prioritization of the remaining open issues (RP-201099, RP-201114)**

* Background: RP-201099, RP-201114 provide proposals on possible down-scoping of the WI remaining issues.
* Companies are encouraged to provide views on:
* Companies are encouraged to provide views on:
  + Whether any of the issues below shall be down-scoped in Rel-16 and postponed to Rel-17?
    - Issue 1: UL spatial relation change requirement for BC bit-0 UE
    - Issue 2: SRS carrier switching requirement for inter-band FR2 CA
    - Issue 3: Multiple SCell activation/deactivation requirement in FR2 inter-band CA
    - Issue 4: RRM requirements for CBM in FR2 inter-band CA
    - Other issues to be down-scoped
  + How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?

|  |  |
| --- | --- |
| Company Name | Comments |
| Huawei | For RRM requirements for CBM in FR2 inter-band CA, we hope a conclusion shall be draw in R16.  The following items can be put in Rel-17   * Requirement for BC bit-0 UE in 2. UL spatial relation change   Multiple SCell activation/deactivation in FR2 inter-band CA |
| Qualcomm | Issue 1: UL spatial relation change   * Requirement for BC bit-0: ok to defer to R17 * Whether UE should meet initial Tx timing accuracy requirements after UL spatial relation switch: ok to defer one-shot timing accuracy to R17   Issue 2: SRS carrier switching for inter-band FR2 CA:   * Interruption requirements for inter-band and case 1/2/3: ok to defer to R17. Have to wait for RF conclusion anyways.   Issue 3: Multiple SCell activation/deactivation in inter-band FR2 CA   * Ok to defer to R17 for CBM UEs  given the current state of MRTD discussion for CBM   Issue 4: RRM requirements for CBM in inter-band FR2 CA:   * Ok to defer to R17 for CBM UEs  given the current state of MRTD discussion for CBM   Other issues to defer to R17:   * BWP switching on multiple CCs: RRM requirement for partial overlapped timer-based BWP switching on multiple CCs is not essential for R16   How to handle the remaining open issues in case they are not down-scoped: revisit the remaining issues in RAN#89-e and decide. |
| NTT DOCOMO | We're fine to down-scope Issue 2 to 4.  On Issue 1, if it is down-scoped, the signalling bit itself should be removed |
| Apple | Most of remaining open issues have been discussed for many meeting cycles with no compromise from either sides. It would be less likely they can be easily resolved beyond Aug. meeting. It is suggested no further extension in RAN#89e and drop all unsolved issues from the WI scope. Some special cases can be considered in TEI but the bar should be high. To be more focused in RAN4#96e, the follow items are suggested to down scope from WI in RAN#88e.   * Requirement for BC bit-0 UE * Interruptions for inter-band SRS carrier switching in FR2 are waiting for RF room conclusion * Multiple SCell activation/deactivation in FR2 inter-band CA    On CBM, we should follow the WF in RAN4#95e. |
| MTK | Issue 1: UL spatial relation change requirement for BC bit-0 UE   * Requirement for BIT-0 UE can be postponed to R17. * Whether UE should meet initial transmit timing accuracy requirements should be removed from R16, since RAN4 already agreed not to introduce one-shot timing adjustment requirement in R16.   Issue 2: SRS carrier switching requirement for inter-band FR2 CA   * Interruptions for inter-band SRS carrier switching in FR2 can be postponed to R17. Since   Issue 3: Multiple SCell activation/deactivation requirement in FR2 inter-band CA   * OK to be postponed to R17   Issue 4: RRM requirements for CBM in FR2 inter-band CA   * OK to be postponed to R17   One question: does this also include MRTD requirement? |
| OPPO | Issue 2: SRS carrier switching requirement for inter-band FR2 CA  Issue 3: Multiple SCell activation/deactivation requirement in FR2 inter-band CA  Issue 4: RRM requirements for CBM in FR2 inter-band CA  Ok to defer to R17 for issue 2/3/4 considering RF progress on FR2 inter-band CA |
| ZTE | Issue 1: UL spatial relation change   * Requirement for BC bit-0: Fine to move to R17 * Whether UE should meet initial Tx timing accuracy requirements after UL spatial relation switch: We think it is important to ensure uplink transmit timing following QCL-ed DL-RS after UL spatial relation switch. The DL receiving timing of QCL-ed DL-RS could be much different than cell timing reference. Without adjusting uplink timing accordingly the gNB demodulation performance could be degraded significantly.   In addition this is different from one shot timing adjustment discussion, which was mainly to handle active TCI state switch and UE autonomous RX beam switch. We don't think UL spatial relation switch was covered by one shot timing adjustment discussion.  So our preference is to have some technical discussion on this in the Aug. meeting. If there is no consensus, it should be moved to R17 WIs.  Issue 2: SRS carrier switching for inter-band FR2 CA:   * It is dependent on RF conclusion. If there is no possbility to have any conclusion in RF room in Aug. meeting then it it fine to move to R17.   Issue 3: Multiple SCell activation/deactivation in inter-band FR2 CA   * Ok to move to R17   Issue 4: RRM requirements for CBM in inter-band FR2 CA:   * Ok to move to R17   How to handle the remaining open issues in case they are not down-scoped:  Move to R17 if no conclusion in Aug. meeting. |
| vivo | Issue 1: UL spatial relation change requirement for BC bit-0 UE   * Ok for BIT-0 UE to be postponed to R17.   Issue 2: SRS carrier switching requirement for inter-band FR2 CA   * Interruptions for inter-band SRS carrier switching in FR2 : ok to be postponed to R17.   Issue 3: Multiple SCell activation/deactivation requirement in FR2 inter-band CA   * OK to be postponed to R17   Issue 4: RRM requirements for CBM in FR2 inter-band CA   * OK to be postponed to R17 |
| Intel | * Whether any of the issues below shall be down-scoped in Rel-16 and postponed to Rel-17?   + Issue 1: UL spatial relation change requirement for BC bit-0 UE   + Issue 2: SRS carrier switching requirement for inter-band FR2 CA   + Issue 3: Multiple SCell activation/deactivation requirement in FR2 inter-band CA   + Issue 4: RRM requirements for CBM in FR2 inter-band CA   + Other issues to be down-scoped   Intel: we are fine to the down-scoping of issue 1~4 above.   * How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?   Intel: we should try to complete the other remaining open issues as much as possible. The decision can be made in RAN#89e. |
| Nokia | No down-scope now as many Rel-16 requirements areas have not been progressing sufficiently well and more time for completing Rel-16 is needed for many WID. FR2 UE RF work also need to continue in the August meeting and the discussion of RF and RRM topics should be coordinated in the August meeting. The need for down-scoping should be checked again in the September RAN. |
| Moderator (Intel) | Based on feedbacks there is a common understanding that current exception list is complete RP-201113 and needs to be revised to remove down-scoped objectives  **Proposal: Revise RP-201113 (Intel, ZTE, Apple) to include updated list of open issues based on Topic 1-3** |
|  |  |

## Intermediate moderator summary (Tue June 30th)

**Topic 1-1: Revised WID (RP-201112)**

* Based on comments there is a common understanding that revised WID RP-201112 is agreeable
* **Proposal 1: Approve RP-201112**

**Topic 1-2: Exception sheet (RP-201113)**

* Based on comments there is a common understanding that current exception list is complete RP-201113 and needs to be revised to remove down-scoped objectives
* **Proposal 2: Revise RP-201113 (Intel, ZTE, Apple) to include updated list of open issues based on Topic 1-3 (if any further down-scoping is agreed)**

**Topic 1-3: Down-scoping and prioritization of the remaining open issues (RP-201099, RP-201114)**

* Issue 1: UL spatial relation change requirement for BC bit-0 UE
  + Majority companies prefer to remove issue 1. One company suggests to remove signalling if the objective is removed. One company prefers no down-scoping.
    - Remove: Huawei, QC, Apple, MTK, ZTE, vivo, Intel
    - Keep: Nokia
    - DCM: if it is down-scoped, the signalling bit itself should be removed
  + Further clarifications from Nokia are encouraged in the next round since the open issue is not related to FR2 inter-band CA.
  + Further clarifications from DCM are encouraged on details of proposal the next round (i.e. from which release the signalling shall be removed).
  + Companies are encouraged to provide views on how to handle BC bit-0 signalling
  + Based on company’s feedback recommend follow the majority view and remove the open issue and further discuss the signalling aspect. Alternative approach is to deprioritize discussion in RAN4 #96e.
  + **Proposal 3:** 
    - **Do not define requirements for Issue 1 in Rel-16 and remove open issue from the exception sheet**
    - **Further discuss whether any impact on BC bit-0 signalling**
* Issue 2: SRS carrier switching requirement for inter-band FR2 CA
  + Majority companies prefer to remove issue 2 from the exception sheet. Two companies propose to continue discussion in Aug meeting.
    - Remove: QC, Apple, DCM, MTK, OPPO, vivo, Intel
    - Keep: Nokia, ZTE
    - ZTE: It is dependent on RF conclusion. If there is no possibility to have any conclusion in RF room in Aug meeting then it is fine to move to R17.
  + Further clarifications from ZTE and Nokia are encouraged on how the open issue can be resolved in RAN4 #96e (e.g. even if RF session reaches the conclusion, RRM room may not have time to conclude).
  + Recommend follow the majority view and remove the open issue. Alternative approach is to deprioritize discussion in RAN4 #96e.
  + **Proposal 4: Do not define requirements for Issue 2 in Rel-16 and remove open issue from the exception sheet**
* Issue 3: Multiple SCell activation/deactivation requirement in FR2 inter-band CA
  + Majority companies prefer to remove Issue 3 from the exception sheet. One company prefers no down-scoping.
    - Remove: Huawei, Apple, DCM, MTK, OPPO, ZTE, vivo, Intel
    - Keep: Nokia
  + Further clarifications from Nokia are encouraged on how the open issue can be resolved in RAN4 #96e (e.g. even if RF session reaches the conclusion, RRM room may not have time to conclude).
  + Recommend follow the majority view and remove the open issue. Alternative approach is to deprioritize discussion in RAN4 #96e.
  + **Proposal 5: Do not define requirements for Issue 3 in Rel-16 and remove open issue from the exception sheet**
* Issue 4: RRM requirements for CBM in FR2 inter-band CA
  + Summary of initial round comments: Majority of companies prefer to remove Issue 4. Three companies prefer to continue discussion in Aug.
    - Remove: DCM, MTK, OPPO, ZTE, vivo, Intel
    - Keep: Huawei, Nokia
    - Apple: follow WF in RAN4 #95e
    - MTK: does this apply to MRTD?
      * Moderator: technically MRTD is in scope of FR2 RF WI and Issue 4 does not apply.
  + Recommend continue discussion to identify possible compromise (e.g. deprioritize selected sub-issues related to CBM)
  + **Proposal 6:** 
    - **Option 1: Do not define requirements for Issue 4 and remove from the exception sheet.**
    - **Option 2: Continue discussion in RAN4 #96e for Issue 4. In case the requirements are not finalized in RAN4 #96e, no Rel-16 requirements will be introduced.**
      * **Note: based on WF mentioned by Apple**
    - **Option 3: Deprioritize work on a subset of CBM related requirements (e.g. beam management, scheduling restriction, measurement restriction, SCell activation delay, interruption)**
      * **Note: see details of open issues in R4-2008998**
* Issue 5: Whether UE should meet initial Tx timing accuracy requirements after UL spatial relation switch
  + Additional issue was identified during the discussion
  + 2 companies suggest to deprioritize this and 1 company to keep
    - Remove: QC, MTK
    - Keep: ZTE
  + **Proposal 7: Continue discussion and collect other companies’ views**
* Issue 6: BWP switching on multiple CCs: RRM requirement for partial overlapped timer-based BWP switching on multiple CCs
  + Additional issue was identified during the discussion
  + 1 company suggests to deprioritize this
  + **Proposal 8: Continue discussion and collect other companies’ views**
* How to handle the remaining open issues in case they are not down-scoped?
  + Diverse views among the companies were observed.
  + **Proposal 9: Postpone discussion on handling non-down-scoped issues to Sep.**

## Intermediate summary comments

**Moderator: Companies are encouraged to provide comments on the proposals and questions intermediate summary in Section 1.2 in the table below**

|  |  |
| --- | --- |
| Company Name | Comments |
| Ericsson | On issues 1, 2, 3 and 5) we are fine to down scope.  On issue 4:  In our view MRTD discussed under RF requirements for FR2 is related to issue 4 since this is all about inter-band CA FR2. So if option 1 or option 3 is agreed then we should also defer MRTD discussion to Rel-17. In that case MRTD which is an RRM issue and not RF, should be under RRM enhancement WI.  On issue 6: we do NOT agree to down prioritize, “RRM requirement for partial overlapped timer-based BWP switching on multiple CCs”. RAN4 has made considerable progress on BWP switching on multiple CCs for all cases and we expect all requirements can be completed in August. The scenarios for which partial overlap BWP switching are already very limited. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Topic #2: Rel-16 NR L3 CSI-RS measurements WI

## Initial comments

**Topic 2-1: Revised WID (RP-200921)**

* Companies are encouraged to give input whether a revised WID is agreeable.

|  |  |
| --- | --- |
| Company Name | Comments |
| Qualcomm | We are fine with the minor changes. |
| ZTE | Fine with the WID revision. |
| Intel | The revision is OK. |
| Huawei | We would like to keep 38306 and 38331 as impacted specifications. New UE capabilities for CSI-RS measurement have not been excluded, and we even have two new capabilities in [] in the RAN4 feature list from RAN4#95 (R4-2009174) |

**Topic 2-2: Exception sheet (RP-200920)**

* Background: Exception sheet provides a full list of remaining open issues.
* Companies are encouraged to provide comments whether the exception sheet includes all remaining open issues or anything is missing.

|  |  |
| --- | --- |
| Company Name | Comments |
| Qualcomm | This RP is for RRM enhancement not CSI-RS L3, which should be [RP-200920](http://www.3gpp.org/ftp/TSG_RAN/TSG_RAN/TSGR_88e/Docs/RP-200920.zip), in which the open issues are completely listed. |
| CATT | Yes, exception is in RP-200920. |
| Intel | RP-200920 is OK. |

**Topic 2-3: Down-scoping and prioritization of the remaining open issues (RP-201230, RP-201099)**

* Background: RP-201230, RP-201099 provide proposals on possible down-scoping and prioritization of the WI remaining issues.
* Companies are encouraged to provide views on:
  + Whether any of the issues below shall be down-scoped in Rel-16 and postponed to Rel-17?
    - Issue 1: CSI-RS configuration applicability
    - Issue 2: Necessity to define requirements for {D=1 with PRBs ≥ 96}
    - Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell
    - Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources
    - Issue 5: CMTC for CSI-RS L3 measurement and time-restriction restriction on CSI-RS resources configuration
    - Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement
    - Other?
  + How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?

|  |  |
| --- | --- |
| Company Name | Comments |
| Huawei | For “CSI-RS configuration applicability: whether to define requirements for {D=1 with PRBs ≥ 96” a conclusion should be drawn in Rel-16 that the configuration is forbidden.  For “Whether or not to introduce new UE capability for minimum separation between two slots with CSIRS resource”, the separation is needed in Rel-16 since UE needs the processing time.  The following items can be put in Rel-17  The collision case between L1 measurement of serving cell and CSI-RS L3 measurement of neighbour cell |
| CMCC | Issue 1 and issue 2 seems to be the same issue.  Issue 1-5, we are OK to down scope them in Rel-16 and postpone to Rel-17.  For Issue 6 “Scheduling restriction and measurement restriction for CSI-RS measurement”, it is necessaary to specify the related requirements in Rel-16. In detail, issue 6 includes three parts: mixed numerology of serving data and CSI-RS L3 mobility, CSI-RS intra-f measurement in TDD band, RX beam sweeping. All of thses need to be considered and specify UE behaviour in Rel-16 to guarantee the system performance. And the scheduling restriction specified for SSB can be used as baseline to save RAN4 efforts. |
| Qualcomm | Issue 1: CSI-RS configuration applicability  Issue 2: Necessity to define requirements for {D=1 with PRBs ≥ 96}   * {D=3 with PRB>=48} is the majority agreed configuration for Rel-16. The above configuration is not essential for R16 and is ok to defer to R17.   Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell   * we prefer to keep the discussion on this in Rel-16 and hope a conclusion can be reached in RAN4#96-e.   Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources   * agree to continue discussing in Rel-16 to address the concern in the UE processing timeline to deal with back to back CSI-RS L3 slots..   Issue 5: CMTC for CSI-RS L3 measurement and time-restriction restriction on CSI-RS resources configuration   * CMTC specification depends on other WGs which are officially finished in Rel-16 so we agree to postpone it to Rel-17.   Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement   * Prefer to continue discussing in Rel-16 as it affects the UE implementation.   Other issues to be down-scoped  whether UE is required to perform Rx beam sweeping for CSI-RS based L3  measurement can be down-scoped or postponed to Rel-17 as it requires further discussions/complexity in UE specific to FR2, e.g. the processing delay w.r.t whether to sweep the UE Rx beams.  How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?  revisit the remaining issues in RAN#89-e and decide. |
| CATT | As the rapporteur company of this WI, we could understand the willing to do more work for this WI in Rel-16. However considering the remaining work and low efficient of E-meeting, the top priority now is to ensure Q3 discussion is focused as much as possible so that we can complete this WI in a timely manner in Rel-16.To this end, I propose to consider a minimum set of exception list and do further enhancement in Rel-17 for others.  As shown in our paper RP-201230, we are ok to have further discussion for issue 1-5 in Rel-17. And it seems Issue 3 have already converged to majority views in May meeting. maybe we can have a try for issue 3. |
| Apple | All issues listed can be down scoped from Rel-16 WI as proposed in RP-201099. For issue 5, it is important to introduce this feature. However, due to time limitation, we are OK should be postponed to Rel-17 since time domain restriction has been agreed in the last RAN4 meeting |
| MTK | Issue 1: CSI-RS configuration applicability   * This item is not very clear to us. Some clarification is needed   Issue 2: Necessity to define requirements for {D=1 with PRBs ≥ 96}   * Remove this from exception sheet. This issue has been discussed several meetings without conclusion, while there is already a majority view on {D=3 with PRBs ≥ 48}   Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell   * This one is not controversial and can be kept.   Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources   * Keep in Rel-16 is OK, although we are not 100% confident if conclusion can be reached in Aug.   Issue 5: CMTC for CSI-RS L3 measurement and time-restriction restriction on CSI-RS resources configuration   * Time domain restriction is a prerequisite to discuss CSSF within gap requirement. We can agree to have **no new signaling for CMTC**, but a certain time-domain restriction (either re-using SMTC or other signaling) is certainly needed to conclude this WI.   Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement   * This part is important but certainly there is no sufficient time for discussion. As a compromise, we are OK to postpone it to Rel-17.   Other issues to be down-scoped   * If it is agreed to have no time domain restriction to be specified in R16, then we should also remove inter-frequency requirements in Rel-16. Because the inter-frequency requirements is deeply coupled with time-domain restriction in both CSSF and delay requirement. For intra-frequency requirement, its corresponding CSSF does not depend on any time-domain restriction.   How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?  Handled in a R17 RRM basket WI (to be discussed in Sep RP meeting) |
| OPPO | Issue 2: Necessity to define requirements for {D=1 with PRBs ≥ 96}   * FFS in Rel-17 if possible   Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell   * Agree with CATT that we could have a try in Aug.   Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources   * Also not sure we can reach conclusion in Aug. OK to postpone it to Rel-17.   Issue 5: CMTC for CSI-RS L3 measurement and time-restriction restriction on CSI-RS resources configuration   * OK with CMTC to be postponed to Rel-17, considering time domain restriction has been agreed in last RAN4 meeting.   Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement   * We could have a try in Aug. If no conclusion then OK to postpone it to Rel-17.   How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?  Agree to be handled and decided in Sep RAN meeting |
| ZTE | Issue 1: CSI-RS configuration applicability   * The issue is not clear.   Issue 2: Necessity to define requirements for {D=1 with PRBs≥ 96}   * It is important to define requirments for  {D=1 with PRBs≥ 96} since the overhead issue is quite significant with D=3 for CSI-RS based mobility and usally lager BW may be configured. In addition the interference due to high density CSI-RS for L3  mobility is also a big issue. If this is delayed to R17 there will be legacy UE issue that NW cannot take advantage of D=1. So RAN4 is to define requirements for {D=1 with PRBs≥ 96} in R16.   Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell   * This can be further discussed in Aug. meeting   Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources   * Move to R17 for further discussion.   Issue 5: CMTC for CSI-RS L3 measurement and time-restriction restriction on CSI-RS resources configuration   * CMTC may be discussed in R17. * When defining RRM requirements, time-restriction on CSI-RS resources configuration can be further discussed in Aug. meeting.   Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement   * This absolutely should be further discussed in Aug. meeting. At least it needs to figure out what the impact will be if there is no requirements for scheduling restriction and measurement restriction.   How to handle the remaining open issues in case they are not down-scoped:   * Move to R17 if no conclusion in Aug. meeting. |
| vivo | Issue 1-2 Necessity to define requirements for {D=1 with PRBs ≥ 96}:  We prefer down-scoping of this issue to later release.  Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell.  We are fine to discuss this in R16.  Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources  We are fine to discuss this in R16.  Issue 5: CMTC for CSI-RS L3 measurement and time-restriction restriction on CSI-RS resources configuration  We think time-restriction for CSI-RS should not be moved to R17 since this is already agreed in R16, based on R4-2009009. The details can be discussed and decided in future RAN4 meetings.  On CMTC, it is also agreed in R4-2009009 that is should be discussed in R17.  Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement  We think this should be within R16 scope and is one basic feature.  How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?  We see quite high possibility that the issues that are not down-scoped can not be finished in RAN4  August.  We should discuss them in RAN 89e. Maybe further extension or exception(e.g. square bracket or main-tainence in CR phase) is needed. |
| Intel | * Issue 1: CSI-RS configuration applicability * Issue 2: Necessity to define requirements for {D=1 with PRBs ≥ 96}   OK to defer to R17.   * Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell   OK to defer to R17. If no UE capability is introduced, is it common understanding that UE is NOT required to handle simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell as baseline?   * Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources   OK to defer to R17. But what’s the baseline assumption for R16 UE?   * Issue 5: CMTC for CSI-RS L3 measurement and time-restriction restriction on CSI-RS resources configuration   OK to defer the concept to R17. But some time domain restriction is still needed.   * Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement   OK to defer to R17.  How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?  Revisit in RANP#89e. |
| Xiaomi | Issue 2: Necessity to define requirements for {D=1 with PRBs ≥ 96}   * OK to defer to Rel-17   Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell   * This issue is not controversial, it can be further discussed in Aug meeting.   Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources   * OK to postpone to Rel-17, this issue has not been converged according to discussion in previous meetings.   Issue 5: CMTC for CSI-RS L3 measurement and time-restriction restriction on CSI-RS resources configuration   * Considering time domain restriction has been agreed in last RAN4 meeting, not sure it is necessary to introduced it in Rel-17.   Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement   * Support CMCC’s view, the requirement for scheduling restriction shall be specified in Rel-16. Otherwise, it will impact UE behaviors.   How to handle the remaining open issues in case they are not down-scoped in RAN 88e and not finalized in Aug 2020?   * Similar view as other companies, they can be handled and decided in Sep RAN meeting |

## Intermediate moderator summary (Tue June 30th)

**Topic 2-1: Revised WID (RP-200921)**

* Most companies are ok with Revised WID. One company suggest to keep 38.306 and 38.331 specs in WID
* **Proposal 1: Revise RP-200921 and keep 38.306 and 38.331 specs in WID**

**Topic 2-2: Exception sheet (RP-200920)**

* Common understanding that current exception list is complete RP-200920 and needs to be revised to remove down-scoped objectives
* **Proposal 2: Revise RP-200920 (CATT) to include updated list of open issues based on Topic 2-3 (if any)**

**Topic 2-3: Down-scoping and prioritization of the remaining open issues (****RP-201230, RP-201099)**

* Issue 1: CSI-RS configuration applicability
  + Company views.
    - Remove: CMCC, CATT, Apple
    - Several companies commented Issues 1 and 2 are same
    - MTK/ZTE: clarifications needed
  + CATT is encouraged to provide further clarifications on the opens issue since it comes from RP-201230
* Issue 2: Necessity to define requirements for {D=1 with PRBs ≥ 96}
  + Majority of companies propose to remove this open issue from the exception sheet. One company prefers to keep it and one company suggests to preclude such configuration.
    - Remove: CMCC, QC, CATT, Apple, MTK, OPPO, vivo, Intel, Xiaomi
    - Keep: ZTE (define requirements)
    - Huawei: configuration needs to be forbidden
  + Recommend to follow the majority view and remove the open issue.
  + To ZTE, based on moderators understanding there was a long discussion in RAN4 whether requirements shall be introduced and no consensus was reached.
  + Further clarifications from Huawei are encouraged on how the configuration can be forbidden.
  + **Proposal 3: Do not define requirements for Issue 2 in Rel-16 and remove open issue from the exception sheet**
* Issue 3: New UE capability on the simultaneous reception of CSI-RS of neighbour cell and SSB of serving cell
  + Diverse views and no consensus to remove the open issue from the exception sheet
    - Remove: CMCC, Apple, Intel
    - Keep: QC, MTK, OPPO, CATT(?), ZTE, vivo, Xiaomi
  + **Proposal 4: Keep Issue 3 in exception sheet and further discuss in Aug.**
* Issue 4: New UE capability on minimum separation between two slots with CSI-RS resources
  + Diverse views and no consensus to remove the open issue from the exception sheet
    - Remove: CMCC, CATT, Apple, OPPO, ZTE, Intel
    - Keep: Huawei, QC, MTK, vivo
  + **Proposal 5: Keep Issue 4 in exception sheet and further discuss in Aug.**
* Issue 5: CMTC for CSI-RS L3 measurement and time-domain restriction on CSI-RS resources configuration
  + Company views.
    - Remove: CMCC, QC, CATT, Apple, OPPO, ZTE, vivo, Xiaomi, Intel
    - Keep: MTK, Intel
    - Intel: some time domain restriction is still needed
    - MTK: no new signaling for CMTC but a certain time-domain restriction (either re-using SMTC or other signaling) is certainly needed to conclude this WI
  + Recommend follow the majority view and remove the open issue.
  + Companies are also encouraged to provide alternative options if some part of the Issue 5 can be down-scoped
  + **Proposal 6: Do not define requirements for Issue 2 in Rel-16 and remove open issue from the exception sheet**
* Issue 6: Scheduling restriction and measurement restriction for CSI-RS measurement
  + Diverse views and no consensus to remove the open issue from the exception sheet
    - Remove: CATT, Apple, MTK, Intel
    - Keep: CMCC, QC, OPPO, ZTE, vivo, Xiaomi
  + **Proposal 7: Keep Issue 6in exception sheet and further discuss in Aug.**
* Issue 7: The collision case between L1 measurement of serving cell and CSI-RS L3 measurement of neighbour cell
  + Additional issue identified during the discussion by one company
  + **Proposal 8: Continue discussion and collect other companies’ views on Issue 7**
* Issue 8: Whether UE is required to perform Rx beam sweeping for CSI-RS based L3  measurement
  + Additional issue identified during the discussion by one company
  + **Proposal 9: Continue discussion and collect other companies’ views on Issue 8**
* Issue 9: Remove inter-frequency requirements if issue 5 is removed
  + Additional issue identified during the discussion by one company
  + **Proposal 10: Continue discussion and collect other companies’ views on Issue 9**
* How to handle the remaining open issues in case they are not down-scoped?
  + Diverse views.
  + **Proposal 11: Postpone discussion on handling non-down-scoped issues to Sep.**

## Intermediate summary comments

**Moderator: Companies are encouraged to provide comments on the proposals and questions intermediate summary in Section 2.2 in the table below**

|  |  |
| --- | --- |
| Company Name | Comments |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Topic #3: Rel-16 NR Positioning WI

## Initial comments

**Topic 3-1: RP-200899 Status report of WI: NR positioning support; rapporteur: Intel Corporation**

* Background: QC raised a flag for SR – “the list of RAN4 open issues is not completely accurate and needs further discussion. Correspondingly, the exception sheet in RP-200900 will need to be updated”
* Q1: Whether any updates to the SR are needed

|  |  |
| --- | --- |
| Company Name | Comments |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Topic 3-2: RP-200900 Rel-16 WI Exception for Core part: NR positioning support**

* Background:
  + E/// raised a flag: “The exception sheet lists, “Report mapping” for RSTD as an open issue. This is related to performance part and should be removed. Core aspects (signaling) are complete and RAN4 already sent LS to RAN2 in RAN4#94-ebis.”
  + MTK raised a flag: “The current scope for Q3 discussion is too wide, including implicitly the impact to Rel-15 L3 measurement. It is challenging to conclude everything in a single E-meeting in Q3. We suggest plenary to discuss possible down scoping or prioritization for this WI.”
  + Intel submitted a discussion paper RP-201117 with the views on the remaining RAN4 open issues handling for Rel-16 NR Positioning WI
* Q1: Whether the exception sheet includes all remaining open issues, or any updates or downscoping needed?

|  |  |
| --- | --- |
| Company Name | Comments |
| Ericsson | On exception sheet: our view is that report mapping specification work in 38.133 being part of section 10 is clearly a performance part and should not be listed as core part. RAN4 has well defined separation between core and performance aspects which should be followed.  On down scoping: We do NOT agree to down scope any of the items listed in the exception sheet (RP-200900). These are also essential elements which need to be completed. If any issue is not completed in August then this should be discussed in Sept plenary. So in our view the current exception sheet is fine except report mapping (that is part of performance as stated above) needs to be removed. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Intermediate summary (Tue June 30th)

**Moderator:** No comments were collected due to late thread triggering. Recommend to further collect comments by Wed. Please use the tables in Section 3.1 to provide the comments.