3GPP RAN TSG Meeting #92-e RP-21xxxx

Electronic meeting, June 14 – 18, 2021

**Agenda item:** 9.7.4.8

**Source:** Moderator (Nokia)

**Title:** Email discussion summary of [92-e-22-RF-FR2-WI]

**Document for:** Information

# Introduction

In RAN#92-e, an email thread [92-e-22-RF-FR2-WI] is assigned to discuss the following tdocs: RP-211174, 1175, 1394, 1395, 1460.

The plan is to discuss on the proposed changes to the WID first. Then the rapporteur can update the WID, if needed, based on the outcome of this email thread.

# Topic #1: RP-211174 and RP-211175

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| RP-211174 and RP-211175 | Nokia, Nokia Shanghai Bell | This WID revision proposes to   * To put this objective on hold until there is a operator request for band combination. **Study and if feasible define UE RF requirements for inter-band CA within the same freq. group (e.g. 28GHz + 28GHz) for (IBM) based on explicitly requested band combinations** * Remove these objectives from UL gaps for self-calibration and monitoring.   + **PA efficiency and power consumption**   + **Transceiver calibration due to temperature variation** * Add a new objective   + **Enhancement of beam correspondence during initial access and RRC\_INACTIVE state [RAN4 RF]**      - **SSB-based without UL beam sweeping**     - **For initial access, verification of beam correspondence based on msg1 spherical coverage (at least)** |

## Company views

**Is WID revision acceptable?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Ericsson | We are fine with the proposed updates/revisions. |
| Apple | We are fine with the revisions as described in the first two bullet points but have concern on the third bullet point to add a new objective for “Enhancement of beam correspondence during initial access and RRC\_INACTIVE state”. We think UE beam correspondence can be well verified in the connected mode. There is no need and not practical to define new requirements for beam correspondence based on msg1 spherical coverage during initial access. If a UE can successfully enter the connected mode, that already implies the UE can pass the requirement for initial access. |
| Qualcomm | We support the amendment, especially considering the SDT motivation |
| MTK | We have concern on the new objective to be added. If the intention is to check UE’s beam correspondence for rough beam, we think it is already covered by existing RRM test cases, e.g.,   * A.7.3.2.1.2 Inter-frequency RRC Re-establishment in FR2   + Beam type: rough   + AoA setup #3: 2 AoAs which are from the set of directions corresponding to the EIS spherical coverage percentile of the DUT as defined in clause 7.3.4 of TS 38.101-2 [19] for each UE power class. The relative angular offset between the directions (AoAs) of the 2 active probes, shall be changed for each test iteration.   Since RRC re-establishment is a mandatory test for FR2 standalone UE, we wonder what additional goal is to be achieved via this new objective. |
| Intel | We are ok with the first two updates (putting inter-band objective on hold and removing PA efficiency and Transceiver calibration from UL gap objectives).  Regarding the new objective for beam correspondence, the LS R1-2106309 asks RAN4 whether there is a need to define the beam correspondence requirements for Small Data Transmission (Configured Grant SDT and/or Random Access SDT) in RRC\_INACTIVE state. Further discussion in RAN4 is needed before considering this objective. Also, the discussion has already taken place in the previous meetings and there was no consensus to define initial access BC. |
| Nokia | Yes, we support this WID revision. |

## Initial Summary

# Topic #2: RP-211394 and RP-211395

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| RP-211394 and RP-211395 | Huawei, HiSilicon | Add a new objective under UL gaps for self-calibration and monitoring.   * **Coherent uplink MIMO** |

## Company views

**Is the proposed new objective agreeable?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Apple | We are okay with the objective. |
| Intel | The objective is fine |
| Nokia | No  Like discussed in the last RAN4 meeting this objective should not be added to the WID. Instead the study for phase I should continue and companies proposing UL gaps for coherent UL MIMO need to first show that this proposal will provide testable performance gains compared to the current requirements without UL gaps. RAN4 has already agreed that these studies can be done under the current WID without revisions. |

## Initial Summary

# Topic #3: RP-211460

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| RP-211460 | MediaTek Inc. | * **Proposal 1: Plenary intervention is needed to resolve current situation on MRTD and MTTD for FR2 inter band CA with CBM in RAN4.** * **Proposal 2: If MRTD 260ns is not agreeable, remove** **CBM related objectives in the WID.** |

## Company views

**Is MRTD 260ns for CBM UE agreeable? If not is CBM related objectives removed from WID?**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Ericsson | We do NOT agree with MRTD of 260 ns for CBM. We suggest to keep the current objective on CBM in the WID.  In R4-2108037, “WF on RRM requirements for FR2 Inter-band DL CA and UL CA” was approved. It has 3 options and option 2 (3 us but with degradation after certain value) was new. Companies are investigating different options until August meeting. |
| Apple | We agree that MRTD should be less than half of the CP length for 120kHz SCS for CBM and 260ns defined for intra-band DL CA can also be specified for inter-band DL CA from the same frequency group. If there is no demand for inter-band CA from the same frequency group, we think the CBM objective can be removed from the WID. |
| Qualcomm | We are ok with restricting the MRTD for CBM UEs to 260 ns. Given the current deadlock on MRTD value, we can consider a value greater than 260 ns for CBM UEs only if an agreeable requirement framework to verify MRTD capability is developed. |
| MTK | This issue has been discussed for roughly 2 years. If compromise is possible, it should not have remained open at this moment. Also, since companies have been insisting their positions for 2 years, we do not see the difficulty to keep the same position for 1 or 2 more meetings.  This issue has consumed non-trivial GTW online time for almost every meeting. As RAN4 workload remains high in this year, we suggest to serious consider whether to keep this objective in the WI scope. |
| Intel | We would like to further look at the possibility of convergence on any of the options in the next WG meeting. Our observation is that there are potential deployments which guarantee the TD within 260ns so that a CBM UE can work properly under. We also understand the typical MRTD value is always 3us though. The network deployment is transparent to UE. We believe it is fair to introduce a UE capability to indicate its MRTD handling ability so that the network understands it and configure CBM inter-band CA accordingly. Let’s try to converge in RAN4 for one more meeting if there is still no consensus, maybe the objective needs to be removed. |
| Nokia | Not acceptable  We could agree to remove the CBM objective from interband CA and leave it only for intraband CA. We would also like to agree an example band combination for IBM UEs within the same frequency group to allow progress of the work before an operator request for band combination. |

## Initial Summary

# Final proposals/recommendations