3GPP TSG-RAN WG2 Meeting #109-e R2-2001936

Online, 24 February – 6 March 2020

**Agenda item: 6.8.2.1**

**Source: Huawei, HiSilicon**

**Title: [Offline-612][POS] Summary on spatial relationship configuration**

**Document for: Discussion and Decision**

# 1 Introduction

This document provide the collection of summary for the following offline discussion.

* [AT109e][612][POS] Spatial relationship configuration (Huawei)

 Intended outcome: Summary of agreements on how the spatial relationship is determined for UL-involved cases and how SSB configuration is signalled. Summary in R2-2001936.

 Deadline: Wednesday 2020-03-04 1300 CET

This discussion focus on the following two aspects per online agreements:

- How the spatial relation for SRS is determined

- How SSB is signalled and how the signalling can be optimized

# 2 Discussion

## 2.1 Spatial relation for SRS

### Discussion#1: Spatial relation determination for SRS

During the e-meeting, companies provided their views on this, we observed the following three options

* Option 1: Spatial relation is determined by the serving gNB without LMF involvement.
	+ Additional supporting procedure may be needed, e.g. Xn exchange of PRS configuration, gNB to retrieve measurement from UE
* Option 2: Spatial relation is determined by the LMF
	+ Additional information may be needed in the NRPPa message (e.g. POSITIONING INFORMATION REQUEST)
* Option 3: Spatial relation is recommended by the LMF and determined by gNB
	+ Additional information may be needed in the NRPPa message (e.g. POSITIONING INFORMATION REQUEST)

***Companies are encouraged to provide their view on the options or provide other options***

|  |  |  |
| --- | --- | --- |
| Company  | Option | Comments |
| Ericsson | Option 1,Option 3(conditional) | We do not see Option 2 would work. Mainly because.* Only gNB is allowed to ask UE to provide RRM/Beam Sweep results. Even as part of ECID, UE is only supposed to provide what it has, it should not lead UE to perform additional RRM related measurements. In order to determine spatial relations efficiently, a very recent RRM (Beam Sweep result of Neighbor Beam/cells) is required. Thus, only gNB should be allowed to obtain such information from UE.
* It is also possible to configure existing SRS transmission as spatial relation for the new UL SRS transmission; and this is only possible for gNB to configure and determine.

LMF should only trigger positioning calculation related measurements. Otherwise, there is risk if LMF asks UE to (only) perform RRM measurements which should be avoided. It violates the architecture and procedure aspects.LMF may however as part of positioning procedure involving UL SRS transmission may inform, gNB how many resource sets/ spatial relations etc. is desired and how many cells/TRPs it wants to involve. Depending upon that gNB may determine the spatial relation. If LMF is able to obtain spatial relation without triggering beam sweep results from UE, then it is ok. Otherwise, the recommendation should be more based upon the accuracy QoS; such that how many resources etc. that is desired from LMF perspectives. It should be left to gNB to determine the SRS configuration and spatial relations based upon LMF recommendations.There should be just one NW node which should determine. There should not be two fragmented decisions; for example, PRS and SRS spatial relation in LMF and SRS (example Rel-15) and SRS (Rel-16) in gNB.For above reasons, we see gNB which configures UL SRS should determine the spatial relations. |
| Intel | Option 2 | RAN2 agreed for multi-RTT, all information is provided by the LMF as below Agreements:1 For Multi-RTT positioning, the DL-PRS information for the candidate TRPs are provided by an LMF to the UE in an LPP Provide Assistance Data message.2 The time/frequency occupancy of the DL-PRS required in the UL-PRS (SRS) information is provided as part of the DL-PRS assistance data for Multi-RTT positioning. UL-PRS (SRS) information includes an index/pointer to the relevant information in the DL-PRS assistance data (e.g., DL-PRS Resource Set ID/Resource ID).3 The time/frequency occupancy of the SSBs required in both, DL-PRS and UL-PRS is grouped in a single IE, and a pointer/index is used to reference the required information.We do not see the reason why different solution is needed for UL only positioning.  |
| vivo | Option1 | We thought that both LMF and gNB were able to configure but an interface anyhow is needed between LMF and gNB which will occupied the core network resource and when it is muti-RTT, a large waste of signals of CN.Also we all knew that gNB already knew the measurement configurations and also the measurement feedback, so it is more reasonable for gNB to decide the SSB.And we don’t need change LPP protocol as well because we couldn’t make a decision on LPP at RAN side.It is basically only gNB which can ask UE to perform radio resource measurements. Otherwise, it is fundamentally wrong that a CN node is doing so.Another reason is Each time If systeminfomation of SSB changed, LMF has to be informed and it is not reasonable. |
| Huawei | Option 3 | The neighbouring TRPs to receive SRS is selected by LMF, and the serving gNB cannot do that, so at least some assistance information is needed. How can Option 1 work for example, if serving gNB selects TRP #1, while LMF selects TRP #2? |
|  |  |  |
|  |  |  |
|  |  |  |

***Summary:***

***Proposal:***

### Discussion#2: Supporting procedure for spatial relation configuration for SRS

In [R2-2001237, R2-2000290], it has also been proposed that gNB should be allowed to retrieve RRM measurements from the UE to help setup the spatial relation information for the neighbouring cells.

**This is a new issue, related to RRC specification. It is not aligned with current procedure, based on this, the procedure will be:**

Step 1: the LMF needs to configure PRS first;

Step 2: the LMF asks the serving gNB to configure SRS;

Step 3: the gNB get PRS-RSRP via RRC;

Step 3: the gNB selects DL-PRS, and informs the SRS configuration +  spatial relationship reference to UE;

Step 4: the gNB forwards the configured SRS to the LMF;

|  |
| --- |
| But, the DL-PRS can’t support to report the measurement result to gNB. It may lead problem when the DL-PRS are configured for the spatial relation reference signal. Especially, the SSB can’t satisfy the requirement of positioning, such as, the hearability of SSB is worse because the neighbouring cell is so far, or the beam width of SSB can’t satisfy the requirement of beam selecting.Furthermore, it didn’t need any other measurement if the measurement of DL PRS is essential for RTT, OTDOA. Observation 3: The measurement of DL-PRS is essential for RTT and OTDOA.So, we proposal supporting the measurement report RSRP of DL-PRS to gNB for beam selecting when the DL-PRS are configured as the spatial relationship reference signal of SRS.**Proposal 2: Report the RSRP of DL-PRS to gNB by RRC when the DL-PRS are configured as the spatial relationship reference signal of SRS.** |

***Companies are encouraged to provide their view on the above issue whether it is necessary to report the RSRP of DL-PRS in the RRM measurement***

|  |  |  |
| --- | --- | --- |
| Company  | Option | Comments |
| Ericsson |  | The above steps and proposal look ok. |
| Intel | No | It is related to discussion 1. If the spatial relation is determined by the LMF, we do not need this information in the gNB.  |
| vivo |  | According current RRC structure that if we need config spacial relation ,we will need config all SRS config, we think add an “optional needM” after IE is possible to avoid repetition, that only the changed part should be configured.for example“UE changed its position，at first the special relation is ssb# 1，then find ssb# 2 is more suitable.” |
| Huawei | No | We think various procedure can be used, including* UL E-CID, from LMF to extract RRM measurement from gNB reported by UE (if supported)
* DL-E-CID, from from LMF to extract RRM measurement from UE directly
* Rough UE location estimate based on the serving cell, and beam direction of PRS
* Historic PRS measurement

Simply LMF utilize those procedures and recommend PRS/SSB to the serving gNB for it to configure spatial relation of SRS |
|  |  |  |
|  |  |  |
|  |  |  |

***Summary:***

***Proposal:***

## 2.2 SSB configuration signaling

The following options are observed based on the summary of LPP [1].

* Option 1 (R2-2000290): all configuration of T/F occupancy of the SSBs only by RRC.
* Option 2: all configurations of T/F occupancy of the SSBs only by LPP.
* Option 3 (R2-2000290): Parameters of T/F occupancy of the SSBs are configured when the UE requested
* Option 4 (R2-2000991): SSB in LPP and index in RRC (for multi-RTT).
* Option 5 (current CR): Duplication is allowed.

For multi-RTT positioning, we agreed that T/F occupancy for SSB will be grouped in a single IE, and use the pointer to reference the required information

3 The time/frequency occupancy of the SSBs required in both, DL-PRS and UL-PRS is grouped in a single IE, and a pointer/index is used to reference the required information.

In the following, we have separate questions dealing with DL-only, UL-only, and multi-RTT positioning, respectively.

### Discussion#3: SSB configuration for DL-only positioning

In the current running CR, the SSB configuration is under the DL PRS assistance data in the LPP message.

|  |
| --- |
| *– NR-SSB-Config*The IE *NR-SSB-Config* defines SSB configuration.-- ASN1STARTNR-SSB-Config-r16 ::= SEQUENCE {  trp-ID-r16 TRP-ID-r16, ss-PBCH-BlockPower-r16 INTEGER (-60..50), halfFrameIndex-r16 INTEGER (0..1), SSB-periodicity-r16 ENUMERATED { ms5, ms10, ms20, ms40, ms80, ms160, ...}, ssb-PositionsInBurst-r16 CHOICE { shortBitmap-r16 BIT STRING (SIZE (4)), mediumBitmap-r16 BIT STRING (SIZE (8)), longBitmap-r16 BIT STRING (SIZE (64)) } OPTIONAL, --Need OR ssbSubcarrierSpacing-r16 ENUMERATED {kHz15, kHz30, kHz60, kHz120, kHz240, ...}, sfn-SSB-Offset-r16 INTEGER (0..15), smtc-r16 SEQUENCE { periodicityAndOffset-r16 CHOICE { sf5 INTEGER (0..4), sf10 INTEGER (0..9), sf20 INTEGER (0..19), sf40 INTEGER (0..39), sf80 INTEGER (0..79), sf160 INTEGER (0..159) }, duration-r16 ENUMERATED { sf1, sf2, sf3, sf4, sf5, ... } }}-- ASN1STOP– *NR-DL-PRS-AssistanceData*The IE *NR-DL-PRS-AssistanceData* is used by the location server to provide DL-PRS assistance data. -- ASN1STARTNR-DL-PRS-AssistanceData-r16 ::= SEQUENCE { nr-DL-PRS-ReferenceInfo-r16 DL-PRS-IdInfo-r16 OPTIONAL, -- Need ON nr-DL-PRS-AssistanceDataList-r16 SEQUENCE (SIZE (1..nrMaxFreqLayers)) OF NR-DL-PRS-AssistanceDataPerFreq-r16, nr-SSB-Config-r16 SEQUENCE (SIZE (0..255)) OF NR-SSB-Config-r16, ...} |

***Companies are encouraged to provide their views.***

|  |  |
| --- | --- |
| Company  | Comments |
| Intel | RAN2 has agreed, T/F occupancy is provided in LPP for Multi-RTT. Same should be applied for DL only positioning. Agreements:1 For Multi-RTT positioning, the DL-PRS information for the candidate TRPs are provided by an LMF to the UE in an LPP Provide Assistance Data message.2 The time/frequency occupancy of the DL-PRS required in the UL-PRS (SRS) information is provided as part of the DL-PRS assistance data for Multi-RTT positioning. UL-PRS (SRS) information includes an index/pointer to the relevant information in the DL-PRS assistance data (e.g., DL-PRS Resource Set ID/Resource ID).3 The time/frequency occupancy of the SSBs required in both, DL-PRS and UL-PRS is grouped in a single IE, and a pointer/index is used to reference the required information. |
| vivo | Keep current implementation |
| Huawei | In LPP |
|  |  |
|  |  |
|  |  |
|  |  |

### Discussion#4: SSB configuration for UL-only positioning

In the current running CR, the SSB configuration for SRS for positioning is provided in SRS-Config under RRC configuration.

|  |
| --- |
| SRS-Type2-ResourceSet-r16 ::= SEQUENCE { srs-Type2-ResourceSetId-r16 SRS-Type2-ResourceSetId-r16, srs-Type2-ResourceIdList-r16 SEQUENCE (SIZE(1..maxNrofSRS-ResourcesPerSet)) OF SRS-Type2-ResourceId-r16 OPTIONAL, -- Cond Setup resourceType-r16 CHOICE { aperiodic-r16 SEQUENCE { aperiodicSRS-ResourceTriggerList-r16 SEQUENCE (SIZE(1..maxNrofSRS-TriggerStates-1)) OF INTEGER (1..maxNrofSRS-TriggerStates-1) OPTIONAL, -- Need M slotOffset-r16 INTEGER (1..32) OPTIONAL, -- Need S ... }, semi-persistent-r16 SEQUENCE { ... }, Periodic-r16 SEQUENCE { ... } }, alpha-r16 Alpha OPTIONAL, -- Need S p0-r16 INTEGER (-202..24) OPTIONAL, -- Cond Setup pathlossReferenceRS-r16 CHOICE { ssb-Index-16 SSB-Index, csi-RS-Index-r16 NZP-CSI-RS-ResourceId, ssb-r16 SSB-InfoNcell-r16, dl-PRS-r16 DL-PRS-Info-r16  } OPTIONAL, -- Need M ...}SRS-ResourceSetId ::= INTEGER (0..maxNrofSRS-ResourceSets-1)SRS-Type2-ResourceSetId-r16 ::= INTEGER (0..maxNrofSRS-ResourceSets-1)SRS-Type2-Resource-r16::= SEQUENCE { srs-Type2-ResourceId-r16 SRS-Type2-ResourceId-r16, transmissionComb-r16 CHOICE { n2-r16 SEQUENCE { combOffset-n2-r16 INTEGER (0..1), cyclicShift-n2-r16 INTEGER (0..7) }, n4-r16 SEQUENCE { combOffset-n4-16 INTEGER (0..3), cyclicShift-n4-r16 INTEGER (0..11) }, n8-r16 SEQUENCE { combOffset-n8-r16 INTEGER (0..7), cyclicShift-n8-r16 INTEGER (0..5) }, **...**}, resourceMapping-r16 SEQUENCE { startPosition-r16 INTEGER (0..13), nrofSymbols-r16 ENUMERATED {n1, n2, n4, n8, n12} }, freqDomainShift-r16 INTEGER (0..268), freqHopping-r16 SEQUENCE { c-SRS-r16 INTEGER (0..63)  }, groupOrSequenceHopping-r16 ENUMERATED { neither, groupHopping, sequenceHopping }, resourceType-r16 CHOICE { aperiodic-r16 SEQUENCE { ... }, semi-persistent-r16 SEQUENCE { periodicityAndOffset-sp-r16 SRS-PeriodicityAndOffset-v16xy, // Editor’s Note: Aperiodic and semi-persisetnt are FFS ... }, periodic-r16 SEQUENCE { periodicityAndOffset-p-r16 SRS-PeriodicityAndOffset-v16xy, ... } }, sequenceId-r16 INTEGER (0..65535), spatialRelation-r16 SRS-SpatialRelationInfo-r16 OPTIONAL, -- Need R ...}SRS-SpatialRelationInfo ::= SEQUENCE { servingCellId ServCellIndex OPTIONAL, -- Need S referenceSignal CHOICE { ssb-Index SSB-Index, csi-RS-Index NZP-CSI-RS-ResourceId, srs SEQUENCE { resourceId SRS-ResourceId, uplinkBWP BWP-Id } }}SRS-SpatialRelationInfo-r16 ::= SEQUENCE { servingCellId-r16 ServCellIndex OPTIONAL, -- Need S referenceSignal-r16 CHOICE { ssb-IndexServing-r16 SSB-Index,  csi-RS-IndexServing-r16 NZP-CSI-RS-ResourceId, srs-SpatialRelation-16 SEQUENCE { resourceSelection-r16 CHOICE { type1-r16 SRS-ResourceID type2-r16 SRS-Type2-ResourceID-r16 }  uplinkBWP-r16 BWP-Id }, ssbNcell-r16 SSB-InfoNcell-r16,  dl-PRS-r16 DL-PRS-Info-r16 }}SSB-Configuration-r16 ::= SEQUENCE { carrierFreq-r16 ARFCN-ValueNR, halfFrameIndex ENUMERATED {zero, one}, ssbSubcarrierSpacing-r16 SubcarrierSpacing, ssb-periodicity-r16 ENUMERATED { ms5, ms10, ms20, ms40, ms80, ms160, spare2,spare1 } OPTIONAL, -- Need S smtc-r16 SSB-MTC OPTIONAL, -- Need S sfn-Offset-r16 INTEGER (0..maxNumFFS), sfn-SSB-Offset-r16 INTEGER (0..15), ss-PBCH-BlockPower-r16 INTEGER (-60..50) OPTIONAL –- Cond Pathloss}SSB-InfoNcell-r16 ::= SEQUENCE { physicalCellId-r16 PhysCellId,  ssb-IndexNcell-r16 SSB-Index, ssb-Configuration-r16 SSB-Configuration-r16 OPTIONAL } |

***Companies are encouraged to provide their views on the signaling above in the current UL-only positioning for SSB configuration***

|  |  |
| --- | --- |
| Company  | Comments |
| Intel | For UL only, the only choice is to configure SSB in the RRC.  |
| vivo | Keep current implementation. |
| Huawei | In RRC. The full configuration of SSB will be provided in RRC as in the current running CR. We assume if LMF recommends gNB to configure SRS spatial relation in the assistance data, the full configuration of SSB should also be included in the assistance data. |
|  |  |
|  |  |
|  |  |
|  |  |

### Discussion#5: SSB configuration for multi-RTT positioning

As mentioned, we have made the agreement that, for multi-RTT positioning, the reference for UL and DL should be grouped in one IE and for UL and DL component, reference to the resource is given.

***Companies are encouraged to provide their views on the above issue.***

|  |  |
| --- | --- |
| Company  | Comments |
| Intel | SSB in LPP and index in RRC. RAN2 has agreed it.The time/frequency occupancy of the DL-PRS required in the UL-PRS (SRS) information is provided as part of the DL-PRS assistance data for Multi-RTT positioning. UL-PRS (SRS) information includes an index/pointer to the relevant information in the DL-PRS assistance data (e.g., DL-PRS Resource Set ID/Resource ID). |
| vivo | 1. For the method of how parameters be grouped in one IE, we proposed that: both LMF and RRC only configure index and T/F occupancy of the SSBs are configured when UE required. We do not limit whether LMF or RRC one component configures, but at one time only once configuration is needed and the other component only need check index to get the whole configurations.

We also need discuss which parameters need be grouped ,otherwise all the multi-RTT related SSB will need group which is not reasonable. |
| Huawei | First preference would be both in LPP and RRC. We do not see a big problem of duplicated configuration, as it can be a corner case and avoided by gNB. Note that for multi-RTT, the best candidate for SRS spatial relation should be PRS, instead of SSB, since PRS is already there and has better coverage than SSB. Second preference would be only in LPP. In this case, LMF recommends the SSB index, as part of the points mentioned in Discussion #1 and Discussion #2, to the serving gNB, which later forwards the SSB index in SRS configuration, without providing full configuration of SSB. |
|  |  |
|  |  |
|  |  |
|  |  |

***Proposal 2:***

# 3 Conclusions

TBD

# 4 References

1. R2-2001173 Summary on LPP for aganda 6.8.2.3 Intel Corporation discussion Rel-16 NR\_pos-Core