3GPP TSG-RAN WG2 #115-e Tdoc DocNumber

Electronic meeting, 16th – 27th August 2021

Agenda Item: 8.13.2.1

Source: Ericsson

Title: [AT115e][851][SON/MDT] CHO and DAPS related RLF reports (Ericsson)

Document for: Discussion, Decision

# 1 Introduction

This paper addresses the following email discussion:

* [AT115e][851][SON/MDT] CHO and DAPS related RLF reports (Ericsson)

**Scope:** Focus on the following proposals: P1, 7,8 and 9.

**Intended outcome**: Report with Agreements

**Deadline**: 11:00 UTC, Wednesday August 25th

Companies are invited to provide their comments by the deadline, i.e. **11:00 UTC, Wednesday August 25th**

# 2 Discussion

## 2.1 “Time D” definition

RAN2 has agreed to include in the RLF-Report, associated to CHO, the following timer:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| C | Time elapsed between the first CHO execution and the corresponding latest CHO configuration received for the selected target cell, i.e. timeSinceCHOReconfig. | Time of received CHO configuration | Time of CHO execution | Agreed in RAN2#112 |
| D | Time elapsed between CHO execution until the first HOF/RLF | Time of executing the first CHO | Time of first HOF/RLF | Agreed in RAN2#113 |

Related to timer D, the following proposal with three different options has been discussed during the online session at RAN2#115-e:

|  |
| --- |
| Proposal 1  Op1: For the Timer D, the TimeConnFailure is re-used with possible updates to indicate that it is started at CHO execution.  Op2: Timer D is computed by the network using timer C and legacy timeConnFailure.  Op3: Introduce a new Timer for Timer D “Time elapsed between CHO execution until the first HOF/RLF”. |

The above options imply the following:

**Option 1:** The “Time D” amounts to the timeConnFailure, which is supposed to start at CHO execution and stop when the HOF/RLF occurs.

**Option 2**: The timeConnFailure is supposed to start at reception of the CHO configuration and stop when the HOF/RLF occurs. The “Time D” is computed as the difference between timeConnFailure and “Time C”.

**Option 3:** A new timer (different from timeConnFailure) is used to represent the “Time D”. It starts at CHO execution and it stops when the HOF/RLF occurs.

Before selecting your preferences, Rapporteur invites companies to evaluate the following scenario already discussed during the online session and illustrated in the below Figure 1 for the various possible options:



Figure : Implications of the various options for the scenario discussed during the online session.

**Description of scenario in Figure 1:** The UE receives and ordinary HO command for HO from cell A to cell B. The UE moves in cell B and it receives a CHO configuration. However, before executing the CHO to cell C, the UE experiences an RLF, and as a consequence it logs the RLF-Report.

* Implications of Option 1/3 in the scenario in Figure 1: Both Option 1 and Option 3 assumes that the time D starts at CHO execution. Hence, when the UE experiences an RLF in cell B before the CHO execution, the timeConnFailure associated to the previous HO is still up and running. It will then represent the time elapsed since the HO command execution in cell A until the RLF in cell B. Once the RLF-Report is retrieved, the network can use this timeConnFailure as in legacy operations, i.e. to evaluate whether the HO from cell A to cell B was “too early” or if the cell B was “too late” with the HO.
* Implications of Option 2 in the scenario Figure 1: In Option 2, the timeConnFailure is started at reception of the CHO configuration. This implies that the previous timeConnFailure that was started at HO from cell A to cell B is overwritten. Hence, when the RLF occurs in cell B, the UE only includes the timeConnFailure started at CHO configuration. Once the RLF-Report is retrieved, the network may not know how to interpret the value of timeConnFailure and to properly use it for the “too early/too late” evaluation as it happens in legacy. For example, cell A, i.e. the previous PCell, does not know that the UE was configured with CHO at the time of RLF, hence it will think that the timeConnFailure represents the time since the HO from cell A to cell B, but in fact the UE had restarted the timeConnFailure and hence it would represent the time since the CHO configuration reception.   
  The above creates ambiguity in the interpretation of timeConnFailure, and consequently it may lead to erroneous HO classifications.

**Differences between Option 1 and Option 3:** Both Option 1 and Option 3 seem to behave similarly for the Scenario in Figure 1. However, related to standardization impact, if Option 3 is selected, RAN2 should discuss how to deal with the timeConnFailure if the CHO is executed. In legacy, when the RLF-Report is logged the UE shall include the timeConnFailure. However, If RAN2 selects option 3, it seems that the UE shall not include the timeConnFailure if the last HO was a CHO, and only this new Timer D should be included.

Rapporteur would like to ask companies which options are preferred.

* **Q1: Which option do you prefer to represent the Time D?**
  + **Option 1:** The “Time D” amounts to the timeConnFailure, which is supposed to start at CHO execution and stop when the HOF/RLF occurs.
  + **Option 2**: The timeConnFailure is supposed to start at reception of the CHO configuration and stop when the HOF/RLF occurs. The “Time D” amounts to the difference between timeConnFailure and “Time C”
  + **Option 3:** A new timer (different from timeConnFailure) is used to represent the “Time D”. It starts at CHO execution and it stops when the HOF/RLF occurs.

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1/2/3** | **Comments** |
| **Qualcomm** | Option 2 | As the network has sent a new CHO configuration, therefore the RLF report should include the failure information corresponding to the new configuration (received in cell B). From the UE perspective, if UE has received a new configuration, then the reference point is set to the latest configuration. Setting the reference point to CHO execution is quite bad from the UE perspective, as UE has to remember all the timeline until RLF or new CHO execution happens (since the reception of CHO configuration in cell A). For example, if UE receives the new CHO configuration in cell B just after HO, but if CHO execution or RLF doesn’t happen for a very long duration. Then, UE has to remember about CHO execution in cell A until RLF. Therefore, we should avoid inter-mixing two failures and the reference point should be set as CHO configuration reception.  The scenario argued seems a corner case. The argued scenario can be avoided by the network side, where the network can send the new CHO configuration after the expiration of the threshold set for detection of early handover failure, then the issue raised by Ericsson will not happen. I am not sure, why a network implementation wants to send a new CHO configuration just after a successful CHO. Isn’t it like encouraging ping-pong? |
| **OPPO** | Option 1 | The given scenario is definitely not a corner case. UE performing consecutive HOs is a possible usual case, especially during mobility in car along road or in train. Overwritting the TimeConnFailure is a serious problem we would like to avoid, since it will results in unsuccssuful optimization of HO from cell A to cell B in the given scenario.  Comparing with option 1 and option 3, we would like to insist on using timeConnFailure IE. Introducing a new IE will bring additional complexity to the RRC spec. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.2 DAPS-related

The following proposals were discussed during the online session:

|  |
| --- |
| Proposal 7 For the case of RLF in source cell after DAPS fallback, the RLF report includes the legacy timeConnFailure, that represents in this case the time between DAPS HO execution and RLF in source cell after fallback.  Proposal 8 For the case of RLF in source cell after DAPS fallback, include in the RLF report an indication that a “DAPS fallback” occurred before the RLF.  Proposal 9 For the case of RLF in target cell after successful DAPS HO, the RLF-Report includes an handover type indicator indicating that the last handover before the RLF was a DAPS HO. |

### 2.2.1 On Proposal 7

Proposal 7 is on how to represent the time elapsed since the last HO execution and the RLF in source cell after the fallback. In the email discussion [1], the following options were discussed:

* **Option 1:** Introduce a new timer, e.g. timeSinceDAPSExecution, to represent the time elapsed between the HO execution and the RLF in the source after the fallback.
* **Option-2:** Reuse timeConnFailure to represent the time elapsed between the HO execution and the RLF in the source after the fallback.
* **Option-3**:

**We have already agreed on this:**

For the case of RLF in source cell while performing DAPS HO (i.e. before fallback), the follow time information is included in the RLF-Report:

a. timeConnSourceFailure: The time elapsed since DAPS HO execution until RLF occurs in source cell while performing DAPS HO ~~before the fallback~~

Note: here we can remove (before the fallback) and fallback indicator can be used to represent if the RLF at source has happened before or after fallback. timeConnSourceFailure is used together with fallback indication to represent RLF related timer for source in DAPS HO

We can reuse timeConnSourceFailure for the information related to RLF at source after DAPS HOF. A fallback indicator together with this timer value should be sufficient.

Furthermore, for proposal 8, the fallback indicator is basically an indicator to represent whether the RLF at source happened before or after the fallback.

Rapporteur’s note: if Option 1 is selected, RAN2 may need to discuss how to handle the existing timeConnFailure in the procedural text. Today, the timeConnFailure is included by the UE whenever there is an RLF. On the other hand, with Option 1, it seems that the UE should be prevented from including the timeConnFailure if there is an RLF in the source cell after the fallback. Otherwise both timeConnFailure and timeSinceDAPSExecution timers will be included which does not make sense.

* **Q2: Which of the above options do you prefer to represent in the RLF report the time since the last DAPS HO execution in case the RLF occurs in source cell after fallback?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1 / Option 2** | **Comments** |
| **Qualcomm** | Option 3 | Reuse already agreed on timer ***timeConnSourceFailure***with the fallback indicator to represent this timer. |
| **OPPO** | Option 3 | It is more clear to use timer ***timeConnSourceFailure*** with the fallback indicator to represent this timer, especially considering that timeConnSourceFailure has been agreed. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### 2.2.1 On Proposal 8/9

Proposal 8/9 are essentially discussing the same issue. Hence, they will be treated together.

In particular, Proposal 8 is about the need of a DAPS fallback indicator, in case there is an RLF in the source cell after the DAPS fallback.

Proposal 9 is about including in the RLF-Report a DAPS handover type indicator in case an RLF occurs in the target cell after the DAPS HO.

Rapporteur´s note: Irrespective of whether the RLF occurs in the source cell after DAPS fallback, or in the target cell after DAPS HO, the current RLF report does not allow the network to figure out that this RLF occurred after a DAPS HO.   
In case of RLF in source cell after DAPS fallback, the network will see that the previousPCellID and the failedPCellID in the RLF-Report are the same, but these two cell IDs may be the same also in case of intra-cell HO.   
Similarly, in case of RLF in target cell, the network cannot know that the last performed HO was a DAPS HO.  
This information may be beneficial because the configuration of DAPS HO parameters may be different from the configuration of the ordinary HO parameters, hence DAPS HO indicator may be used to optimize the corresponding HO parameters.

* **Q3: Do you believe that it is beneficial to include in the RLF-Report an indicator indicating that the last executed HO before the RLF was a DAPS HO?**
  + **Option 1:** Yes, both in case of RLF in the target cell after DAPS HO, and RLF in source cell after DAPS fallback
  + **Option 2:** Yes, but only in case of RLF in the target cell after DAPS HO
  + **Option 3:** Yes, but only in case of RLF in source cell after DAPS fallback
  + **Option 4:** No

|  |  |  |
| --- | --- | --- |
| **Company** | **Option 1/2/3/4** | **Comments** |
| **Qualcomm** | No (Option 4) | If we agree on option 3 for question 2, we don’t need an indicator existing fields should be sufficient. For example, if RLF at the source happens before the DAPS HOF or successful DAPS HO, we will set fallback indicator as False and timeConnSourceFailure, as the time since CHO execution until RLF. If DAPS HO also fails after RLF to the source, we will set timeConnFailure as the time since the execution of DAPS HO failure until RLF at target.  For example, if we consider timeConnSourceFailure always captures the time value since the reception of DAPS config until RLF at source if UE has received DAPS config previously. Then, the presence of timeConnFailure itself will dictate if RLF at the target cell has happened after DAPS HO or not. Furthermore, the fallback indication is sufficient to represent if RLF has happened in the source cell after fallback or before.  I believe that if we are creating a new timer, we should use that to the maximum extent and avoid introducing the new fields when it can be covey from existing or agreed on IEs. |
| **OPPO** | Option 2 | Agreeing on option 3 for Q2 only address the issue on proposal 8. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Conclusion

**To be updated**

# References

1. R2-2108425, [Post114-e][850][SON MDT] Modeling of CHO and DAPS related RLF reports (Ericsson), RAN2#115-e