3GPP TSG-RAN WG2 Meeting #118 Electronic R2-22xxxxx

Online, May 9th – 20th, 2022

**Agenda item: 5.1.4.3**

**Source: NTT DOCOMO INC. (Moderator)**

**Title: [Draft] Summary of [AT118-e][020][NR1516] UE capabilities I (NTT DOCOMO)**

**Document for: Discussion and Decision**

# 1 Introduction

This document is to report on the following offline discussion:

* [AT118-e][020][NR1516] UE capabilities I (NTT DOCOMO)

Scope: Treat R2-2205118, R2-2205119, R2-2205121, R2-2204472, R2-2206063, R2-2206064, R2-2204419, R2-2204840, R2-2204841, R2-2205451, R2-2205452, R2-2206000, R2-2206001

Ph1 Determine agreeable parts, Ph2 for agreeable parts agree CRs (offline agreement, CB online only if necessary).

Intended outcome: Report, Agreed CRs

Deadline: Schedule 1

This discussion follows Schedule 1, which is organized as follows.

Discussions with Deadline **Schedule 1**:

A **first round** with **Deadline for comments W1 Thursd May 12th 1200 UTC** to settle scope what is agreeable etc

A Final round with **Final deadline W2 Wednesd May 18th 1200 UTC** to settle details / agree CRs etc.

Additional deadlines check points etc if needed are defined by the Rapporteur of each discussion respectively. In case some parts of an email discussion need more time, doesn’t converge, need on-line treatment, then please contact the chair.

# 2 Contact Points

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Docomo (moderator) | Masato Taniguchi | masato.taniguchi.mf@nttdocomo.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Discussion (1st round)

## 3.1 R4 - Simultaneous Rx/Tx

[1] R2-2205118 Clarification on simultaneous Rx/Tx capability per band pair NTT DOCOMO, INC. CR Rel-15 38.306 15.16.0 0708 - F NR\_newRAT-Core

[2] R2-2205119 Clarification on simultaneous Rx/Tx capability per band pair NTT DOCOMO, INC. CR Rel-16 38.306 16.8.0 0709 - A NR\_newRAT-Core

[3] R2-2205121 Clarification on simultaneous Rx/Tx capability per band pair NTT DOCOMO, INC. CR Rel-17 38.306 17.0.0 0710 - A NR\_newRAT-Core

According to the contributions, RAN4 discussed when the per-band-pair simultaneous Rx/Tx capability should be mandatory and the following agreements were made, which were captured in Rel-15 TS 38.101 series (R4-2206610, R4-2206616)

Agreement:

Proposal 1: For inter-band EN-DC, NE-DC, NR CA, NR DC and SUL configurations, If mandatory simultaneous RxTx capability apply for a band configuration, mandatory simultaneous RxTx capability also apply for the band pair of the configuration when the applicable configuration is a subset of a higher order band configuration.

Proposal 2: Clarification in Proposal 1 should apply from Rel-15 TS 38.101 series.

The CRs propose to reflect the agreement to 38.306 by adding the following text.

*Otherwise, for the band pairs where the mandatory simultaneous Rx/Tx capability applies as specified in <reference to 38.101-x series>, the UE shall set the corresponding bits to “1”.*

The CRs also propose to clarify that Per-BC capability signalling should be used if the UE supports the capability for all *applicable* band pairs, as simultaneous Rx/Tx capability is not applicable to certain band combinations or band pairs, e.g. intra-band band pairs.

**Question 1: Do companies agree with the intention of R2-2205118 [1] and its mirror CRs[2][3]?**

|  |  |  |
| --- | --- | --- |
| Company | Yes or No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.2 R4 - *maxNumberCSI-RS-RRM-RS-SINR*

[4] R2-2204472 LS on the applicability of mixed numerology on UE capability maxNumberCSI-RS-RRM-RS-SINR (R4-2206828; contact: Apple) RAN4 LS in Rel-17 NR\_CSIRS\_L3meas To:RAN1, RAN2

Chair: The LS indicates a Rel-16 WI and Rel-17 applicability

[5] R2-2206063 Clarification on the applicability of mixed numerology on UE capability maxNumberCSI-RS-RRM-RS-SINR Apple Inc CR Rel-16 38.306 16.8.0 0740 - F NR\_CSIRS\_L3meas

[6] R2-2206064 Clarification on the applicability of mixed numerology on UE capability maxNumberCSI-RS-RRM-RS-SINR Apple Inc CR Rel-17 38.306 17.0.0 0741 - A NR\_CSIRS\_L3meas

According to [5] [6]**,** RAN4 made the below agreement that for the case of mixed numerology in R4-2205655:

*the number of CSI-RS resources in any duration that equals to the length of a slot is no larger than UE capability maxNumberCSI-RS-RRM-RS-SINR*

the number of CSI-RS resources in any duration that equals to the length of a slot is no larger than UE capability *maxNumberCSI-RS-RRM-RS-SINR*.

* When there are mixed numerologies, the length of a slot is defined based on the smallest SCS

The RAN4 LS [4] states that RAN4 concludes the UE capability of *maxNumberCSI-RS-RRM-RS-SINR* and the related requirements should be specified based on the duration associated with the slot of minimum SCS in case of mixed numerologies. The CRs[5][6] propose to add the following text to reflect this.

***maxNumberCSI-RS-RRM-RS-SINR***

Defines the maximum number of CSI-RS resources for RRM and RS-SINR measurement across all measurement frequencies per slot. If UE supports any of *csi-RSRP-AndRSRQ-MeasWithSSB*, *csi-RSRP-AndRSRQ-MeasWithoutSSB*, and *csi-SINR-Meas*, UE shall report this capability.

NOTE: A slot is based on minimum SCS among all measurement frequencies configured for RRM and RS-SINR measurement.

**Question 2: Do companies agree with the intention of R2-2206063 [5] and R2-2206064 [6]?**

|  |  |  |
| --- | --- | --- |
| Company | Yes or No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.3 L1

[7] R2-2204419 LS on updated Rel-16 RAN1 UE features lists for NR after RAN1#108-e (R1-2202764; contact: NTT DOCOMO) RAN1 LS in Rel-16 TEI16, NR\_CLI\_RIM-Core, NR\_eMIMO-Core, NR\_Mob\_enh-Core, LTE\_NR\_DC\_CA\_enh-Core, NR\_unlic-Core, NR\_2step\_RACH-Core, NR\_IAB-Core, NR\_L1enh\_URLLC-Core, NR\_UE\_pow\_sav-Core, NR\_pos-Core, 5G\_V2X\_NRSL-Core, NR\_IIOT-Core To:RAN2 Cc:RAN4

[8] R2-2204840 Correction to multi-DCI multi-TRP and new UE capability to limit PDCCH monitoring Intel Corporation CR Rel-16 38.306 16.8.0 0704 - F NR\_eMIMO-Core, TEI16

[9] R2-2204841 New UE capability to limit PDCCH monitoring Intel Corporation CR Rel-16 38.331 16.8.0 2999 - F NR\_eMIMO-Core, TEI16

The CRs [8] and [9] are to update 38.306 and 38.331 based on the updated R1 UE feature list [7].

1. Clarify how the multi-DCI multi-TRP PUSCH operation is supported by existing FGs on the field description of multiDCI-MultiTRP-r16.
2. Introduce a new capability to limit PDCCH monitoring with a single span of three contiguous OFDM symbols that is within the first four OFDM symbols in a slot.

**Question 3: Do companies agree with the intention of R2-2204840 [8] and R2-2204841 [9]?**

|  |  |  |
| --- | --- | --- |
| Company | Yes or No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

[10] R2-2205451 Correction on the UE capability description of the overlapping PDSCH in Rel-17 Xiaomi Communications, Samsung CR Rel-17 38.306 17.0.0 0716 - F TEI16

[11] R2-2205452 Correction on the UE capability description of the overlapping PDSCH in Rel-16 Xiaomi Communications, Samsung CR Rel-16 38.306 16.8.0 0717 - A TEI16

According to the contributions, in 38.822, the UE indicating the support of *overlapPDSCHsInTimePartiallyFreq-r16* shall also indicate the support of the “Prerequisite feature” 16-2a-0 *overlapPDSCHsFullyFreqTime-r16*. However the field description of *overlapPDSCHsInTimePartiallyFreq-*r16 in 38.306 says that the “Prerequisite feature” of *overlapPDSCHsInTimePartiallyFreq-r16* is *multiDCI-MultiTRP-r16*. The CRs propose to correct the field description of *overlapPDSCHsInTimePartiallyFreq-r16* that the UE indicating the support of *overlapPDSCHsInTimePartiallyFreq-r16* shall also indicate the support of *overlapPDSCHsFullyFreqTime-r16*.

**Question 4: Do companies agree with the intention of R2-2205451 [10] and R2-2205452 [11]?**

|  |  |  |
| --- | --- | --- |
| Company | Yes or No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

[12] R2-2206000 bwp-SwitchingDelay conditionally mandatory capability Qualcomm Incorporated CR Rel-15 38.306 15.16.0 0734 - F NR\_newRAT-Core

[13] R2-2206001 bwp-SwitchingDelay conditionally mandatory capability Qualcomm Incorporated CR Rel-16 38.306 16.8.0 0735 - F NR\_newRAT-Core

The contributions point out that the support of *bwp-SwitchingDelay* capability by the UE depends on the support of the BWP switch feature while per the current spec “*bwp-SwitchingDelay*” is classified as a mandatory capability without including any dependency on the support of the BWP switch feature, which is causing interoperability issue between UE and network during testing.

The CRs propose to clarify the dependency on the BWP switching feature in 38.306.

**Question 5: Do companies agree with the intention of R2-2206000 [12] and R2-2206001 [13]?**

|  |  |  |
| --- | --- | --- |
| Company | Yes or No | Comments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 5 Summary of 1st Round Discussion

# 6 Discussion (2nd round)

# 7 Conclusion

# References

R4 - Simu Rx/Tx

[1] R2-2205118 Clarification on simultaneous Rx/Tx capability per band pair NTT DOCOMO, INC. CR Rel-15 38.306 15.16.0 0708 - F NR\_newRAT-Core

[2] R2-2205119 Clarification on simultaneous Rx/Tx capability per band pair NTT DOCOMO, INC. CR Rel-16 38.306 16.8.0 0709 - A NR\_newRAT-Core

[3] R2-2205121 Clarification on simultaneous Rx/Tx capability per band pair NTT DOCOMO, INC. CR Rel-17 38.306 17.0.0 0710 - A NR\_newRAT-Core

R4 - maxNumberCSI-RS

[4] R2-2204472 LS on the applicability of mixed numerology on UE capability maxNumberCSI-RS-RRM-RS-SINR (R4-2206828; contact: Apple) RAN4 LS in Rel-17 NR\_CSIRS\_L3meas To:RAN1, RAN2

Chair: The LS indicates a Rel-16 WI and Rel-17 applicability

[5] R2-2206063 Clarification on the applicability of mixed numerology on UE capability maxNumberCSI-RS-RRM-RS-SINR Apple Inc CR Rel-16 38.306 16.8.0 0740 - F NR\_CSIRS\_L3meas

[6] R2-2206064 Clarification on the applicability of mixed numerology on UE capability maxNumberCSI-RS-RRM-RS-SINR Apple Inc CR Rel-17 38.306 17.0.0 0741 - A NR\_CSIRS\_L3meas

L1

[7] R2-2204419 LS on updated Rel-16 RAN1 UE features lists for NR after RAN1#108-e (R1-2202764; contact: NTT DOCOMO) RAN1 LS in Rel-16 TEI16, NR\_CLI\_RIM-Core, NR\_eMIMO-Core, NR\_Mob\_enh-Core, LTE\_NR\_DC\_CA\_enh-Core, NR\_unlic-Core, NR\_2step\_RACH-Core, NR\_IAB-Core, NR\_L1enh\_URLLC-Core, NR\_UE\_pow\_sav-Core, NR\_pos-Core, 5G\_V2X\_NRSL-Core, NR\_IIOT-Core To:RAN2 Cc:RAN4

[8] R2-2204840 Correction to multi-DCI multi-TRP and new UE capability to limit PDCCH monitoring Intel Corporation CR Rel-16 38.306 16.8.0 0704 - F NR\_eMIMO-Core, TEI16

[9] R2-2204841 New UE capability to limit PDCCH monitoring Intel Corporation CR Rel-16 38.331 16.8.0 2999 - F NR\_eMIMO-Core, TEI16

[10] R2-2205451 Correction on the UE capability description of the overlapping PDSCH in Rel-17 Xiaomi Communications, Samsung CR Rel-17 38.306 17.0.0 0716 - F TEI16

[11] R2-2205452 Correction on the UE capability description of the overlapping PDSCH in Rel-16 Xiaomi Communications, Samsung CR Rel-16 38.306 16.8.0 0717 - A TEI16

[12] R2-2206000 bwp-SwitchingDelay conditionally mandatory capability Qualcomm Incorporated CR Rel-15 38.306 15.16.0 0734 - F NR\_newRAT-Core

[13] R2-2206001 bwp-SwitchingDelay conditionally mandatory capability Qualcomm Incorporated CR Rel-16 38.306 16.8.0 0735 - F NR\_newRAT-Core