**3GPP TSG-RAN3 #110-e R3-207202**

Online, November 2nd – November 13th 2020

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.413** | **CR** | **1799** | **rev** |  | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Enabling URI configuration within Trace Activation over S1 |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | RAN3 |
|  |  |
| ***Work item code:*** | NR\_SON\_MDT-CORE |  | ***Date:*** | 2020-11-11 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | To enable the URI confiugation in the Trace Activattion IE over the S1 interface  |
|  |  |
|  ***Summary of change:*** | In this contribution we make a proposal to enable the URI confiugation in the Trace Activattion IE over the S1 interface, which has been confirmed by SA5 to be already supported in their specificationsImpact AnalysisThis CR has limited functional impact. The CR has limited ASN.1 impacts. |
|  |  |
| ***Consequences if not approved:*** | There is inconsistency between the RAN3 andSA5 specifications and it is not possible to enable the URI confiugation in the Trace Activattion IE over the S1 interface |
|  |  |
| ***Clauses affected:*** | 9.2.1.4, 9.2.2.x (new), 9.3.4, 9.3.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **Y** |  |  Other core specifications  | TS36.423 CR **1565** |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

#### 9.2.1.4 Trace Activation

Defines parameters related to a trace activation.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| E-UTRAN Trace ID | M |  | OCTET STRING (SIZE(8)) | The E-UTRAN Trace ID IE is composed of the following: Trace Reference defined in TS 32.422 [10] (leftmost 6 octets, with PLMN information coded as in 9.2.3.8), andTrace Recording Session Reference defined in TS 32.422 [10] (last 2 octets). |  |  |
| Interfaces To Trace | M |  | BIT STRING (SIZE(8)) | Each position in the bitmap represents an eNB or en-gNB interface:first bit =S1-MME, second bit =X2, third bit =Uu, fourth bit =F1-C, fifth bit =E1:other bits reserved for future use. Value ‘1’ indicates ‘should be traced’. Value ‘0’ indicates ‘should not be traced’. |  |  |
| Trace depth | M |  | ENUMERATED(minimum, medium, maximum, MinimumWithoutVendorSpecificExtension,MediumWithoutVendorSpecificExtension,MaximumWithoutVendorSpecificExtension, …) | Defined in TS 32.422 [10]. |  |  |
| Trace Collection Entity IP Address | M |  | Transport Layer Address 9.2.2.1 | For File based Reporting. Defined in TS 32.422 [10].This IE is ignored if the *Trace Collection Entity URI* IE is present |  |  |
| MDT Configuration | O |  | 9.2.1.81 |  | YES | ignore |
| UE Application layer measurement configuration | O |  | 9.2.1.128 |  | YES | Ignore |
| MDT Configuration NR | O |  | OCTET STRING | Defined in TS 38.413 [44]. Only the immediate MDT configurations are included in the IE in this version of the specification. | YES | ignore |
| Trace Collection Entity URI | O |  | URI 9.2.2.x | For Streaming based Reporting.Defined in TS 32.422 [10]Replaces Trace Collection Entity IP Address if present | YES | ignore |

<<<<<<<<<<<<<<<<<<<< End of 1st Change >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 2nd Change >>>>>>>>>>>>>>>>>>>>

#### 9.2.2.x URI

This IE is an URI.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| URI | M |  | VisibleString | String representing URI (Uniform Resource Identifier) |

<<<<<<<<<<<<<<<<<<<< End of 2nd Change >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 3rd Change >>>>>>>>>>>>>>>>>>>>

### 9.3.4 Information Element Definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

S1AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) s1ap (1) version1 (1) s1ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 id-E-RABInformationListItem,

 id-E-RABItem,

 id-GUMMEIType,

 id-Bearers-SubjectToStatusTransfer-Item,

 id-Time-Synchronisation-Info,

 id-x2TNLConfigurationInfo,

 id-eNBX2ExtendedTransportLayerAddresses,

 id-MDTConfiguration,

 id-Time-UE-StayedInCell-EnhancedGranularity,

 id-HO-Cause,

 id-M3Configuration,

 id-M4Configuration,

 id-M5Configuration,

 id-MDT-Location-Info,

 id-SignallingBasedMDTPLMNList,

 id-MobilityInformation,

 id-ULCOUNTValueExtended,

 id-DLCOUNTValueExtended,

 id-ReceiveStatusOfULPDCPSDUsExtended,

 id-eNBIndirectX2TransportLayerAddresses,

 id-Muting-Availability-Indication,

 id-Muting-Pattern-Information,

 id-NRrestrictioninEPSasSecondaryRAT,

 id-NRrestrictionin5GS,

 id-Synchronisation-Information,

 id-uE-HistoryInformationFromTheUE,

 id-LoggedMBSFNMDT,

 id-SON-Information-Report,

 id-RecommendedCellItem,

 id-RecommendedENBItem,

 id-ProSeUEtoNetworkRelaying,

 id-ULCOUNTValuePDCP-SNlength18,

 id-DLCOUNTValuePDCP-SNlength18,

 id-ReceiveStatusOfULPDCPSDUsPDCP-SNlength18,

 id-M6Configuration,

 id-M7Configuration,

 id-RAT-Type,

 id-extended-e-RAB-MaximumBitrateDL,

 id-extended-e-RAB-MaximumBitrateUL,

 id-extended-e-RAB-GuaranteedBitrateDL,

 id-extended-e-RAB-GuaranteedBitrateUL,

 id-extended-uEaggregateMaximumBitRateDL,

 id-extended-uEaggregateMaximumBitRateUL,

 id-SecondaryRATDataUsageReportItem,

 id-E-RABUsageReportItem,

 id-UEAppLayerMeasConfig,

 id-serviceType,

 id-UnlicensedSpectrumRestriction,

 id-CNTypeRestrictions,

 id-DownlinkPacketLossRate,

 id-UplinkPacketLossRate,

 id-BluetoothMeasurementConfiguration,

 id-WLANMeasurementConfiguration,

 id-LastNG-RANPLMNIdentity,

 id-PSCellInformation,

 id-IMSvoiceEPSfallbackfrom5G,

 id-RequestTypeAdditionalInfo,

 id-AdditionalRRMPriorityIndex,

 id-ContextatSource,

 id-IntersystemMeasurementConfiguration,

 id-SourceNodeID,

 id-NB-IoT-RLF-Report-Container,

 id-MDTConfigurationNR,

 id-DAPSRequestInfo,

 id-DAPSResponseInfoList,

 id-DAPSResponseInfoItem,

 id-Bearers-SubjectToEarlyStatusTransfer-Item,

 id-TraceCollectionEntityURI,

 maxnoofCSGs,

 maxnoofE-RABs,

 maxnoofErrors,

 maxnoofBPLMNs,

 maxnoofPLMNsPerMME,

 maxnoofTACs,

 maxnoofEPLMNs,

 maxnoofEPLMNsPlusOne,

 maxnoofForbLACs,

 maxnoofForbTACs,

 maxnoofCellsinUEHistoryInfo,

 maxnoofCellID,

 maxnoofDCNs,

 maxnoofEmergencyAreaID,

 maxnoofTAIforWarning,

 maxnoofCellinTAI,

 maxnoofCellinEAI,

 maxnoofeNBX2TLAs,

 maxnoofeNBX2ExtTLAs,

 maxnoofeNBX2GTPTLAs,

 maxnoofRATs,

 maxnoofGroupIDs,

 maxnoofMMECs,

 maxnoofTAforMDT,

 maxnoofCellIDforMDT,

 maxnoofMDTPLMNs,

 maxnoofCellsforRestart,

 maxnoofRestartTAIs,

 maxnoofRestartEmergencyAreaIDs,

 maxnoofMBSFNAreaMDT,

 maxEARFCN,

 maxnoofCellsineNB,

 maxnoofRecommendedCells,

 maxnoofRecommendedENBs,

 maxnooftimeperiods,

 maxnoofCellIDforQMC,

 maxnoofTAforQMC,

 maxnoofPLMNforQMC,

 maxnoofBluetoothName,

 maxnoofWLANName,

 maxnoofConnectedengNBs,

 maxnoofPC5QoSFlows,

 maxnooffrequencies,

 maxNARFCN,

 maxRS-IndexCellQual

FROM S1AP-Constants

<<<<<<<<<<<<<<<<<<<< End of 3rd Change >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 4th Change >>>>>>>>>>>>>>>>>>>>

TraceActivation ::= SEQUENCE {

 e-UTRAN-Trace-ID E-UTRAN-Trace-ID,

 interfacesToTrace InterfacesToTrace,

traceDepth TraceDepth,

traceCollectionEntityIPAddress TransportLayerAddress,

 iE-Extensions ProtocolExtensionContainer { { TraceActivation-ExtIEs} } OPTIONAL,

 ...

}

TraceActivation-ExtIEs S1AP-PROTOCOL-EXTENSION ::= {

-- Extension for Rel-10 to support MDT --

 { ID id-MDTConfiguration CRITICALITY ignore EXTENSION MDT-Configuration PRESENCE optional }|

-- Extension for Rel-15 to support QMC –

 { ID id-UEAppLayerMeasConfig CRITICALITY ignore EXTENSION UEAppLayerMeasConfig PRESENCE optional }|

 { ID id-MDTConfigurationNR CRITICALITY ignore EXTENSION MDT-ConfigurationNR PRESENCE optional }|

 { ID id-TraceCollectionEntityURI CRITICALITY ignore EXTENSION URI\_address PRESENCE optional },

 ...

}

**-- TEXT OMITTED –**

-- U

**-- TEXT OMITTED –**

URI\_address ::= VisibleString

UserLocationInformation ::= SEQUENCE {

 eutran-cgi EUTRAN-CGI,

 tai TAI,

 iE-Extensions ProtocolExtensionContainer { { UserLocationInformation-ExtIEs} } OPTIONAL,

 ...

}

UserLocationInformation-ExtIEs S1AP-PROTOCOL-EXTENSION ::= {

 { ID id-PSCellInformation CRITICALITY ignore EXTENSION PSCellInformation PRESENCE optional},

 ...

}

**-- TEXT OMITTED –**

### 9.3.6 Constant Definitions

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

S1AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) s1ap (1) version1 (1) s1ap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM S1AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-HandoverPreparation ProcedureCode ::= 0

id-HandoverResourceAllocation ProcedureCode ::= 1

id-HandoverNotification ProcedureCode ::= 2

id-PathSwitchRequest ProcedureCode ::= 3

id-HandoverCancel ProcedureCode ::= 4

id-E-RABSetup ProcedureCode ::= 5

id-E-RABModify ProcedureCode ::= 6

id-E-RABRelease ProcedureCode ::= 7

id-E-RABReleaseIndication ProcedureCode ::= 8

id-InitialContextSetup ProcedureCode ::= 9

id-Paging ProcedureCode ::= 10

id-downlinkNASTransport ProcedureCode ::= 11

id-initialUEMessage ProcedureCode ::= 12

id-uplinkNASTransport ProcedureCode ::= 13

id-Reset ProcedureCode ::= 14

id-ErrorIndication ProcedureCode ::= 15

id-NASNonDeliveryIndication ProcedureCode ::= 16

id-S1Setup ProcedureCode ::= 17

id-UEContextReleaseRequest ProcedureCode ::= 18

id-DownlinkS1cdma2000tunnelling ProcedureCode ::= 19

id-UplinkS1cdma2000tunnelling ProcedureCode ::= 20

id-UEContextModification ProcedureCode ::= 21

id-UECapabilityInfoIndication ProcedureCode ::= 22

id-UEContextRelease ProcedureCode ::= 23

id-eNBStatusTransfer ProcedureCode ::= 24

id-MMEStatusTransfer ProcedureCode ::= 25

id-DeactivateTrace ProcedureCode ::= 26

id-TraceStart ProcedureCode ::= 27

id-TraceFailureIndication ProcedureCode ::= 28

id-ENBConfigurationUpdate ProcedureCode ::= 29

id-MMEConfigurationUpdate ProcedureCode ::= 30

id-LocationReportingControl ProcedureCode ::= 31

id-LocationReportingFailureIndication ProcedureCode ::= 32

id-LocationReport ProcedureCode ::= 33

id-OverloadStart ProcedureCode ::= 34

id-OverloadStop ProcedureCode ::= 35

id-WriteReplaceWarning ProcedureCode ::= 36

id-eNBDirectInformationTransfer ProcedureCode ::= 37

id-MMEDirectInformationTransfer ProcedureCode ::= 38

id-PrivateMessage ProcedureCode ::= 39

id-eNBConfigurationTransfer ProcedureCode ::= 40

id-MMEConfigurationTransfer ProcedureCode ::= 41

id-CellTrafficTrace ProcedureCode ::= 42

id-Kill ProcedureCode ::= 43

id-downlinkUEAssociatedLPPaTransport ProcedureCode ::= 44

id-uplinkUEAssociatedLPPaTransport ProcedureCode ::= 45

id-downlinkNonUEAssociatedLPPaTransport ProcedureCode ::= 46

id-uplinkNonUEAssociatedLPPaTransport ProcedureCode ::= 47

id-UERadioCapabilityMatch ProcedureCode ::= 48

id-PWSRestartIndication ProcedureCode ::= 49

id-E-RABModificationIndication ProcedureCode ::= 50

id-PWSFailureIndication ProcedureCode ::= 51

id-RerouteNASRequest ProcedureCode ::= 52

id-UEContextModificationIndication ProcedureCode ::= 53

id-ConnectionEstablishmentIndication ProcedureCode ::= 54

id-UEContextSuspend ProcedureCode ::= 55

id-UEContextResume ProcedureCode ::= 56

id-NASDeliveryIndication ProcedureCode ::= 57

id-RetrieveUEInformation ProcedureCode ::= 58

id-UEInformationTransfer ProcedureCode ::= 59

id-eNBCPRelocationIndication ProcedureCode ::= 60

id-MMECPRelocationIndication ProcedureCode ::= 61

id-SecondaryRATDataUsageReport ProcedureCode ::= 62

id-UERadioCapabilityIDMapping ProcedureCode ::= 63

id-HandoverSuccess ProcedureCode ::= 64

id-eNBEarlyStatusTransfer ProcedureCode ::= 65

id-MMEEarlyStatusTransfer ProcedureCode ::= 66

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Extension constants

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxPrivateIEs INTEGER ::= 65535

maxProtocolExtensions INTEGER ::= 65535

maxProtocolIEs INTEGER ::= 65535

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxnoofCSGs INTEGER ::= 256

maxnoofE-RABs INTEGER ::= 256

maxnoofTAIs INTEGER ::= 256

maxnoofTACs INTEGER ::= 256

maxnoofErrors INTEGER ::= 256

maxnoofBPLMNs INTEGER ::= 6

maxnoofPLMNsPerMME INTEGER ::= 32

maxnoofEPLMNs INTEGER ::= 15

maxnoofEPLMNsPlusOne INTEGER ::= 16

maxnoofForbLACs INTEGER ::= 4096

maxnoofForbTACs INTEGER ::= 4096

maxnoofIndividualS1ConnectionsToReset INTEGER ::= 256

maxnoofCellsinUEHistoryInfo INTEGER ::= 16

maxnoofCellsineNB INTEGER ::= 256

maxnoofTAIforWarning INTEGER ::= 65535

maxnoofCellID INTEGER ::= 65535

maxnoofDCNs INTEGER ::= 32

maxnoofEmergencyAreaID INTEGER ::= 65535

maxnoofCellinTAI INTEGER ::= 65535

maxnoofCellinEAI INTEGER ::= 65535

maxnoofeNBX2TLAs INTEGER ::= 2

maxnoofeNBX2ExtTLAs INTEGER ::= 16

maxnoofeNBX2GTPTLAs INTEGER ::= 16

maxnoofRATs INTEGER ::= 8

maxnoofGroupIDs INTEGER ::= 65535

maxnoofMMECs INTEGER ::= 256

maxnoofCellIDforMDT INTEGER ::= 32

maxnoofTAforMDT INTEGER ::= 8

maxnoofMDTPLMNs INTEGER ::= 16

maxnoofCellsforRestart INTEGER ::= 256

maxnoofRestartTAIs INTEGER ::= 2048

maxnoofRestartEmergencyAreaIDs INTEGER ::= 256

maxEARFCN INTEGER ::= 262143

maxnoofMBSFNAreaMDT INTEGER ::= 8

maxnoofRecommendedCells INTEGER ::= 16

maxnoofRecommendedENBs INTEGER ::= 16

maxnooftimeperiods INTEGER ::= 2

maxnoofCellIDforQMC INTEGER ::= 32

maxnoofTAforQMC INTEGER ::= 8

maxnoofPLMNforQMC INTEGER ::= 16

maxnoofBluetoothName INTEGER ::= 4

maxnoofWLANName INTEGER ::= 4

maxnoofConnectedengNBs INTEGER ::= 256

maxnoofPC5QoSFlows INTEGER ::= 2048

maxnooffrequencies INTEGER ::= 64

maxNARFCN INTEGER ::= 32

maxRS-IndexCellQual INTEGER ::= 16

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-MME-UE-S1AP-ID ProtocolIE-ID ::= 0

id-HandoverType ProtocolIE-ID ::= 1

id-Cause ProtocolIE-ID ::= 2

id-SourceID ProtocolIE-ID ::= 3

id-TargetID ProtocolIE-ID ::= 4

id-eNB-UE-S1AP-ID ProtocolIE-ID ::= 8

id-E-RABSubjecttoDataForwardingList ProtocolIE-ID ::= 12

id-E-RABtoReleaseListHOCmd ProtocolIE-ID ::= 13

id-E-RABDataForwardingItem ProtocolIE-ID ::= 14

id-E-RABReleaseItemBearerRelComp ProtocolIE-ID ::= 15

id-E-RABToBeSetupListBearerSUReq ProtocolIE-ID ::= 16

id-E-RABToBeSetupItemBearerSUReq ProtocolIE-ID ::= 17

id-E-RABAdmittedList ProtocolIE-ID ::= 18

id-E-RABFailedToSetupListHOReqAck ProtocolIE-ID ::= 19

id-E-RABAdmittedItem ProtocolIE-ID ::= 20

id-E-RABFailedtoSetupItemHOReqAck ProtocolIE-ID ::= 21

id-E-RABToBeSwitchedDLList ProtocolIE-ID ::= 22

id-E-RABToBeSwitchedDLItem ProtocolIE-ID ::= 23

id-E-RABToBeSetupListCtxtSUReq ProtocolIE-ID ::= 24

id-TraceActivation ProtocolIE-ID ::= 25

id-NAS-PDU ProtocolIE-ID ::= 26

id-E-RABToBeSetupItemHOReq ProtocolIE-ID ::= 27

id-E-RABSetupListBearerSURes ProtocolIE-ID ::= 28

id-E-RABFailedToSetupListBearerSURes ProtocolIE-ID ::= 29

id-E-RABToBeModifiedListBearerModReq ProtocolIE-ID ::= 30

id-E-RABModifyListBearerModRes ProtocolIE-ID ::= 31

id-E-RABFailedToModifyList ProtocolIE-ID ::= 32

id-E-RABToBeReleasedList ProtocolIE-ID ::= 33

id-E-RABFailedToReleaseList ProtocolIE-ID ::= 34

id-E-RABItem ProtocolIE-ID ::= 35

id-E-RABToBeModifiedItemBearerModReq ProtocolIE-ID ::= 36

id-E-RABModifyItemBearerModRes ProtocolIE-ID ::= 37

id-E-RABReleaseItem ProtocolIE-ID ::= 38

id-E-RABSetupItemBearerSURes ProtocolIE-ID ::= 39

id-SecurityContext ProtocolIE-ID ::= 40

id-HandoverRestrictionList ProtocolIE-ID ::= 41

id-UEPagingID ProtocolIE-ID ::= 43

id-pagingDRX ProtocolIE-ID ::= 44

id-TAIList ProtocolIE-ID ::= 46

id-TAIItem ProtocolIE-ID ::= 47

id-E-RABFailedToSetupListCtxtSURes ProtocolIE-ID ::= 48

id-E-RABReleaseItemHOCmd ProtocolIE-ID ::= 49

id-E-RABSetupItemCtxtSURes ProtocolIE-ID ::= 50

id-E-RABSetupListCtxtSURes ProtocolIE-ID ::= 51

id-E-RABToBeSetupItemCtxtSUReq ProtocolIE-ID ::= 52

id-E-RABToBeSetupListHOReq ProtocolIE-ID ::= 53

id-GERANtoLTEHOInformationRes ProtocolIE-ID ::= 55

id-UTRANtoLTEHOInformationRes ProtocolIE-ID ::= 57

id-CriticalityDiagnostics ProtocolIE-ID ::= 58

id-Global-ENB-ID ProtocolIE-ID ::= 59

id-eNBname ProtocolIE-ID ::= 60

id-MMEname ProtocolIE-ID ::= 61

id-ServedPLMNs ProtocolIE-ID ::= 63

id-SupportedTAs ProtocolIE-ID ::= 64

id-TimeToWait ProtocolIE-ID ::= 65

id-uEaggregateMaximumBitrate ProtocolIE-ID ::= 66

id-TAI ProtocolIE-ID ::= 67

id-E-RABReleaseListBearerRelComp ProtocolIE-ID ::= 69

id-cdma2000PDU ProtocolIE-ID ::= 70

id-cdma2000RATType ProtocolIE-ID ::= 71

id-cdma2000SectorID ProtocolIE-ID ::= 72

id-SecurityKey ProtocolIE-ID ::= 73

id-UERadioCapability ProtocolIE-ID ::= 74

id-GUMMEI-ID ProtocolIE-ID ::= 75

id-E-RABInformationListItem ProtocolIE-ID ::= 78

id-Direct-Forwarding-Path-Availability ProtocolIE-ID ::= 79

id-UEIdentityIndexValue ProtocolIE-ID ::= 80

id-cdma2000HOStatus ProtocolIE-ID ::= 83

id-cdma2000HORequiredIndication ProtocolIE-ID ::= 84

id-E-UTRAN-Trace-ID ProtocolIE-ID ::= 86

id-RelativeMMECapacity ProtocolIE-ID ::= 87

id-SourceMME-UE-S1AP-ID ProtocolIE-ID ::= 88

id-Bearers-SubjectToStatusTransfer-Item ProtocolIE-ID ::= 89

id-eNB-StatusTransfer-TransparentContainer ProtocolIE-ID ::= 90

id-UE-associatedLogicalS1-ConnectionItem ProtocolIE-ID ::= 91

id-ResetType ProtocolIE-ID ::= 92

id-UE-associatedLogicalS1-ConnectionListResAck ProtocolIE-ID ::= 93

id-E-RABToBeSwitchedULItem ProtocolIE-ID ::= 94

id-E-RABToBeSwitchedULList ProtocolIE-ID ::= 95

id-S-TMSI ProtocolIE-ID ::= 96

id-cdma2000OneXRAND ProtocolIE-ID ::= 97

id-RequestType ProtocolIE-ID ::= 98

id-UE-S1AP-IDs ProtocolIE-ID ::= 99

id-EUTRAN-CGI ProtocolIE-ID ::= 100

id-OverloadResponse ProtocolIE-ID ::= 101

id-cdma2000OneXSRVCCInfo ProtocolIE-ID ::= 102

id-E-RABFailedToBeReleasedList ProtocolIE-ID ::= 103

id-Source-ToTarget-TransparentContainer ProtocolIE-ID ::= 104

id-ServedGUMMEIs ProtocolIE-ID ::= 105

id-SubscriberProfileIDforRFP ProtocolIE-ID ::= 106

id-UESecurityCapabilities ProtocolIE-ID ::= 107

id-CSFallbackIndicator ProtocolIE-ID ::= 108

id-CNDomain ProtocolIE-ID ::= 109

id-E-RABReleasedList ProtocolIE-ID ::= 110

id-MessageIdentifier ProtocolIE-ID ::= 111

id-SerialNumber ProtocolIE-ID ::= 112

id-WarningAreaList ProtocolIE-ID ::= 113

id-RepetitionPeriod ProtocolIE-ID ::= 114

id-NumberofBroadcastRequest ProtocolIE-ID ::= 115

id-WarningType ProtocolIE-ID ::= 116

id-WarningSecurityInfo ProtocolIE-ID ::= 117

id-DataCodingScheme ProtocolIE-ID ::= 118

id-WarningMessageContents ProtocolIE-ID ::= 119

id-BroadcastCompletedAreaList ProtocolIE-ID ::= 120

id-Inter-SystemInformationTransferTypeEDT ProtocolIE-ID ::= 121

id-Inter-SystemInformationTransferTypeMDT ProtocolIE-ID ::= 122

id-Target-ToSource-TransparentContainer ProtocolIE-ID ::= 123

id-SRVCCOperationPossible ProtocolIE-ID ::= 124

id-SRVCCHOIndication ProtocolIE-ID ::= 125

id-NAS-DownlinkCount ProtocolIE-ID ::= 126

id-CSG-Id ProtocolIE-ID ::= 127

id-CSG-IdList ProtocolIE-ID ::= 128

id-SONConfigurationTransferECT ProtocolIE-ID ::= 129

id-SONConfigurationTransferMCT ProtocolIE-ID ::= 130

id-TraceCollectionEntityIPAddress ProtocolIE-ID ::= 131

id-MSClassmark2 ProtocolIE-ID ::= 132

id-MSClassmark3 ProtocolIE-ID ::= 133

id-RRC-Establishment-Cause ProtocolIE-ID ::= 134

id-NASSecurityParametersfromE-UTRAN ProtocolIE-ID ::= 135

id-NASSecurityParameterstoE-UTRAN ProtocolIE-ID ::= 136

id-DefaultPagingDRX ProtocolIE-ID ::= 137

id-Source-ToTarget-TransparentContainer-Secondary ProtocolIE-ID ::= 138

id-Target-ToSource-TransparentContainer-Secondary ProtocolIE-ID ::= 139

id-EUTRANRoundTripDelayEstimationInfo ProtocolIE-ID ::= 140

id-BroadcastCancelledAreaList ProtocolIE-ID ::= 141

id-ConcurrentWarningMessageIndicator ProtocolIE-ID ::= 142

id-Data-Forwarding-Not-Possible ProtocolIE-ID ::= 143

id-ExtendedRepetitionPeriod ProtocolIE-ID ::= 144

id-CellAccessMode ProtocolIE-ID ::= 145

id-CSGMembershipStatus ProtocolIE-ID ::= 146

id-LPPa-PDU ProtocolIE-ID ::= 147

id-Routing-ID ProtocolIE-ID ::= 148

id-Time-Synchronisation-Info ProtocolIE-ID ::= 149

id-PS-ServiceNotAvailable ProtocolIE-ID ::= 150

id-PagingPriority ProtocolIE-ID ::= 151

id-x2TNLConfigurationInfo ProtocolIE-ID ::= 152

id-eNBX2ExtendedTransportLayerAddresses ProtocolIE-ID ::= 153

id-GUMMEIList ProtocolIE-ID ::= 154

id-GW-TransportLayerAddress ProtocolIE-ID ::= 155

id-Correlation-ID ProtocolIE-ID ::= 156

id-SourceMME-GUMMEI ProtocolIE-ID ::= 157

id-MME-UE-S1AP-ID-2 ProtocolIE-ID ::= 158

id-RegisteredLAI ProtocolIE-ID ::= 159

id-RelayNode-Indicator ProtocolIE-ID ::= 160

id-TrafficLoadReductionIndication ProtocolIE-ID ::= 161

id-MDTConfiguration ProtocolIE-ID ::= 162

id-MMERelaySupportIndicator ProtocolIE-ID ::= 163

id-GWContextReleaseIndication ProtocolIE-ID ::= 164

id-ManagementBasedMDTAllowed ProtocolIE-ID ::= 165

id-PrivacyIndicator ProtocolIE-ID ::= 166

id-Time-UE-StayedInCell-EnhancedGranularity ProtocolIE-ID ::= 167

id-HO-Cause ProtocolIE-ID ::= 168

id-VoiceSupportMatchIndicator ProtocolIE-ID ::= 169

id-GUMMEIType ProtocolIE-ID ::= 170

id-M3Configuration ProtocolIE-ID ::= 171

id-M4Configuration ProtocolIE-ID ::= 172

id-M5Configuration ProtocolIE-ID ::= 173

id-MDT-Location-Info ProtocolIE-ID ::= 174

id-MobilityInformation ProtocolIE-ID ::= 175

id-Tunnel-Information-for-BBF ProtocolIE-ID ::= 176

id-ManagementBasedMDTPLMNList ProtocolIE-ID ::= 177

id-SignallingBasedMDTPLMNList ProtocolIE-ID ::= 178

id-ULCOUNTValueExtended ProtocolIE-ID ::= 179

id-DLCOUNTValueExtended ProtocolIE-ID ::= 180

id-ReceiveStatusOfULPDCPSDUsExtended ProtocolIE-ID ::= 181

id-ECGIListForRestart ProtocolIE-ID ::= 182

id-SIPTO-Correlation-ID ProtocolIE-ID ::= 183

id-SIPTO-L-GW-TransportLayerAddress ProtocolIE-ID ::= 184

id-TransportInformation ProtocolIE-ID ::= 185

id-LHN-ID ProtocolIE-ID ::= 186

id-AdditionalCSFallbackIndicator ProtocolIE-ID ::= 187

id-TAIListForRestart ProtocolIE-ID ::= 188

id-UserLocationInformation ProtocolIE-ID ::= 189

id-EmergencyAreaIDListForRestart ProtocolIE-ID ::= 190

id-KillAllWarningMessages ProtocolIE-ID ::= 191

id-Masked-IMEISV ProtocolIE-ID ::= 192

id-eNBIndirectX2TransportLayerAddresses ProtocolIE-ID ::= 193

id-uE-HistoryInformationFromTheUE ProtocolIE-ID ::= 194

id-ProSeAuthorized ProtocolIE-ID ::= 195

id-ExpectedUEBehaviour ProtocolIE-ID ::= 196

id-LoggedMBSFNMDT ProtocolIE-ID ::= 197

id-UERadioCapabilityForPaging ProtocolIE-ID ::= 198

id-E-RABToBeModifiedListBearerModInd ProtocolIE-ID ::= 199

id-E-RABToBeModifiedItemBearerModInd ProtocolIE-ID ::= 200

id-E-RABNotToBeModifiedListBearerModInd ProtocolIE-ID ::= 201

id-E-RABNotToBeModifiedItemBearerModInd ProtocolIE-ID ::= 202

id-E-RABModifyListBearerModConf ProtocolIE-ID ::= 203

id-E-RABModifyItemBearerModConf ProtocolIE-ID ::= 204

id-E-RABFailedToModifyListBearerModConf ProtocolIE-ID ::= 205

id-SON-Information-Report ProtocolIE-ID ::= 206

id-Muting-Availability-Indication ProtocolIE-ID ::= 207

id-Muting-Pattern-Information ProtocolIE-ID ::= 208

id-Synchronisation-Information ProtocolIE-ID ::= 209

id-E-RABToBeReleasedListBearerModConf ProtocolIE-ID ::= 210

id-AssistanceDataForPaging ProtocolIE-ID ::= 211

id-CellIdentifierAndCELevelForCECapableUEs ProtocolIE-ID ::= 212

id-InformationOnRecommendedCellsAndENBsForPaging ProtocolIE-ID ::= 213

id-RecommendedCellItem ProtocolIE-ID ::= 214

id-RecommendedENBItem ProtocolIE-ID ::= 215

id-ProSeUEtoNetworkRelaying ProtocolIE-ID ::= 216

id-ULCOUNTValuePDCP-SNlength18 ProtocolIE-ID ::= 217

id-DLCOUNTValuePDCP-SNlength18 ProtocolIE-ID ::= 218

id-ReceiveStatusOfULPDCPSDUsPDCP-SNlength18 ProtocolIE-ID ::= 219

id-M6Configuration ProtocolIE-ID ::= 220

id-M7Configuration ProtocolIE-ID ::= 221

id-PWSfailedECGIList ProtocolIE-ID ::= 222

id-MME-Group-ID ProtocolIE-ID ::= 223

id-Additional-GUTI ProtocolIE-ID ::= 224

id-S1-Message ProtocolIE-ID ::= 225

id-CSGMembershipInfo ProtocolIE-ID ::= 226

id-Paging-eDRXInformation ProtocolIE-ID ::= 227

id-UE-RetentionInformation ProtocolIE-ID ::= 228

id-UE-Usage-Type ProtocolIE-ID ::= 230

id-extended-UEIdentityIndexValue ProtocolIE-ID ::= 231

id-RAT-Type ProtocolIE-ID ::= 232

id-BearerType ProtocolIE-ID ::= 233

id-NB-IoT-DefaultPagingDRX ProtocolIE-ID ::= 234

id-E-RABFailedToResumeListResumeReq ProtocolIE-ID ::= 235

id-E-RABFailedToResumeItemResumeReq ProtocolIE-ID ::= 236

id-E-RABFailedToResumeListResumeRes ProtocolIE-ID ::= 237

id-E-RABFailedToResumeItemResumeRes ProtocolIE-ID ::= 238

id-NB-IoT-Paging-eDRXInformation ProtocolIE-ID ::= 239

id-V2XServicesAuthorized ProtocolIE-ID ::= 240

id-UEUserPlaneCIoTSupportIndicator ProtocolIE-ID ::= 241

id-CE-mode-B-SupportIndicator ProtocolIE-ID ::= 242

id-SRVCCOperationNotPossible ProtocolIE-ID ::= 243

id-NB-IoT-UEIdentityIndexValue ProtocolIE-ID ::= 244

id-RRC-Resume-Cause ProtocolIE-ID ::= 245

id-DCN-ID ProtocolIE-ID ::= 246

id-ServedDCNs ProtocolIE-ID ::= 247

id-UESidelinkAggregateMaximumBitrate ProtocolIE-ID ::= 248

id-DLNASPDUDeliveryAckRequest ProtocolIE-ID ::= 249

id-Coverage-Level ProtocolIE-ID ::= 250

id-EnhancedCoverageRestricted ProtocolIE-ID ::= 251

id-UE-Level-QoS-Parameters ProtocolIE-ID ::= 252

id-DL-CP-SecurityInformation ProtocolIE-ID ::= 253

id-UL-CP-SecurityInformation ProtocolIE-ID ::= 254

id-extended-e-RAB-MaximumBitrateDL ProtocolIE-ID ::= 255

id-extended-e-RAB-MaximumBitrateUL ProtocolIE-ID ::= 256

id-extended-e-RAB-GuaranteedBitrateDL ProtocolIE-ID ::= 257

id-extended-e-RAB-GuaranteedBitrateUL ProtocolIE-ID ::= 258

id-extended-uEaggregateMaximumBitRateDL ProtocolIE-ID ::= 259

id-extended-uEaggregateMaximumBitRateUL ProtocolIE-ID ::= 260

id-NRrestrictioninEPSasSecondaryRAT ProtocolIE-ID ::= 261

id-UEAppLayerMeasConfig ProtocolIE-ID ::= 262

id-UE-Application-Layer-Measurement-Capability ProtocolIE-ID ::= 263

id-SecondaryRATDataUsageReportList ProtocolIE-ID ::= 264

id-SecondaryRATDataUsageReportItem ProtocolIE-ID ::= 265

id-HandoverFlag ProtocolIE-ID ::= 266

id-E-RABUsageReportItem ProtocolIE-ID ::= 267

id-SecondaryRATDataUsageRequest ProtocolIE-ID ::= 268

id-NRUESecurityCapabilities ProtocolIE-ID ::= 269

id-UnlicensedSpectrumRestriction ProtocolIE-ID ::= 270

id-CE-ModeBRestricted ProtocolIE-ID ::= 271

id-LTE-M-Indication ProtocolIE-ID ::= 272

id-DownlinkPacketLossRate ProtocolIE-ID ::= 273

id-UplinkPacketLossRate ProtocolIE-ID ::= 274

id-UECapabilityInfoRequest ProtocolIE-ID ::= 275

id-serviceType ProtocolIE-ID ::= 276

id-AerialUEsubscriptionInformation ProtocolIE-ID ::= 277

id-Subscription-Based-UE-DifferentiationInfo ProtocolIE-ID ::= 278

id-EndIndication ProtocolIE-ID ::= 280

id-EDT-Session ProtocolIE-ID ::= 281

id-CNTypeRestrictions ProtocolIE-ID ::= 282

id-PendingDataIndication ProtocolIE-ID ::= 283

id-BluetoothMeasurementConfiguration ProtocolIE-ID ::= 284

id-WLANMeasurementConfiguration ProtocolIE-ID ::= 285

id-WarningAreaCoordinates ProtocolIE-ID ::= 286

id-NRrestrictionin5GS ProtocolIE-ID ::= 287

id-PSCellInformation ProtocolIE-ID ::= 288

id-LastNG-RANPLMNIdentity ProtocolIE-ID ::= 290

id-ConnectedengNBList ProtocolIE-ID ::= 291

id-ConnectedengNBToAddList ProtocolIE-ID ::= 292

id-ConnectedengNBToRemoveList ProtocolIE-ID ::= 293

id-EN-DCSONConfigurationTransfer-ECT ProtocolIE-ID ::= 294

id-EN-DCSONConfigurationTransfer-MCT ProtocolIE-ID ::= 295

id-IMSvoiceEPSfallbackfrom5G ProtocolIE-ID ::= 296

id-TimeSinceSecondaryNodeRelease ProtocolIE-ID ::= 297

id-RequestTypeAdditionalInfo ProtocolIE-ID ::= 298

id-AdditionalRRMPriorityIndex ProtocolIE-ID ::= 299

id-ContextatSource ProtocolIE-ID ::= 300

id-IAB-Authorized ProtocolIE-ID ::= 301

id-IAB-Node-Indication ProtocolIE-ID ::= 302

id-IAB-Supported ProtocolIE-ID ::= 303

id-DataSize ProtocolIE-ID ::= 304

id-Ethernet-Type ProtocolIE-ID ::= 305

id-NRV2XServicesAuthorized ProtocolIE-ID ::= 306

id-NRUESidelinkAggregateMaximumBitrate ProtocolIE-ID ::= 307

id-PC5QoSParameters ProtocolIE-ID ::= 308

id-IntersystemSONConfigurationTransferMCT ProtocolIE-ID ::= 309

id-IntersystemSONConfigurationTransferECT ProtocolIE-ID ::= 310

id-IntersystemMeasurementConfiguration ProtocolIE-ID ::= 311

id-SourceNodeID ProtocolIE-ID ::= 312

id-NB-IoT-RLF-Report-Container ProtocolIE-ID ::= 313

id-UERadioCapabilityID ProtocolIE-ID ::= 314

id-UERadioCapability-NR-Format ProtocolIE-ID ::= 315

id-MDTConfigurationNR ProtocolIE-ID ::= 316

id-DAPSRequestInfo ProtocolIE-ID ::= 317

id-DAPSResponseInfoList ProtocolIE-ID ::= 318

id-DAPSResponseInfoItem ProtocolIE-ID ::= 319

id-NotifySourceeNB ProtocolIE-ID ::= 320

id-eNB-EarlyStatusTransfer-TransparentContainer ProtocolIE-ID ::= 321

id-Bearers-SubjectToEarlyStatusTransfer-Item ProtocolIE-ID ::= 322

id-WUS-Assistance-Information ProtocolIE-ID ::= 323

id-NB-IoT-PagingDRX ProtocolIE-ID ::= 324

id-TraceCollectionEntityURI ProtocolIE-ID ::= XXX

END

<<<<<<<<<<<<<<<<<<<< End of Changes >>>>>>>>>>