**3GPP TSG-RAN3 #110-e R3-207203**

Online, November 2nd – November 13th 2020

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.423** | **CR** | **1565** | **rev** |  | **Current version:** | **16.3.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Enabling URI configuration within Trace Activation over X2 |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | RAN3 |
|  |  |
| ***Work item code:*** | NR\_SON\_MDT-CORE |  | ***Date:*** | 2020-11-11 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | To enable the URI confiugation in the Trace Activattion IE over the X2 interface  |
|  |  |
|  ***Summary of change:*** | In this contribution we make a proposal to enable the URI confiugation in the Trace Activattion IE over the S1 interface, which has been confirmed by SA5 to be already supported in their specificationsImpact AnalysisThis CR has limited functional impact. The CR has limited ASN.1 impacts. |
|  |  |
| ***Consequences if not approved:*** | There is inconsistency between the RAN3 andSA5 specifications and it is not possible to enable the URI confiugation in the Trace Activattion IE over the X2 interface |
|  |  |
| ***Clauses affected:*** | 9.2.2, 9.2.x (new), 9.3.5, 9.3.7 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **Y** |  |  Other core specifications  | TS36.413 CR **1799** |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<<<<<<<<<<<<<<<<<<<< 1st Change >>>>>>>>>>>>>>>>>>>>

9.2.2 Trace Activation

Defines parameters related to trace activation.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| E-UTRAN Trace ID | M |  | OCTET STRING (8) | The E-UTRAN Trace ID IE is composed of the following: Trace Reference defined in TS 32.422 [6] (leftmost 6 octets, with PLMN information coded as in 9.2.4), andTrace Recording Session Reference defined in TS 32.422 [6] (last 2 octets) | – |  |
| Interfaces To Trace | M |  | BIT STRING (8) | Each position in the bitmap represents a eNB interface:first bit =S1-MME, second bit =X2, third bit =Uu, fourth bit = F1-C, fifth bit = E1.Other bits reserved for future use. Value ‘1’ indicates ‘should be traced’. Value ‘0’ indicates ‘should not be traced’. | – |  |
| Trace Depth | M |  | ENUMERATED(minimum, medium, maximum,MinimumWithoutVendorSpecificExtension,MediumWithoutVendorSpecificExtension,MaximumWithoutVendorSpecificExtension, ...) | Defined in TS 32.421 [7] | – |  |
| Trace Collection Entity IP Address | M |  | BIT STRING (1..160,…) | For File based Reporting. Defined in TS 32.422 [6].For details on the Transport Layer Address, see TS 36.424 [8], TS 36.414 [19] . This IE is ignored if the *Trace Collection Entity URI* IE is present | \_ |  |
| MDT Configuration | O |  | 9.2.56 |  | YES | ignore |
| UE Application layer measurement configuration | O |  | 9.2.121 |  | YES | ignore |
| MDT Configuration NR | O |  | OCTET STRING | Defined in TS 38.413 [39]. Only the immediate MDT configurations are included in the IE in this version of the specification. | YES | ignore |
| Trace Collection Entity URI | O |  | URI 9.2.x | For Streaming based Reporting.Defined in TS 32.422 [11]Replaces Trace Collection Entity IP Address if present | YES | ignore |

<<<<<<<<<<<<<<<<<<<< End of 1st Change >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 2nd Change >>>>>>>>>>>>>>>>>>>>

9.2.x URI

This IE is an URI.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| URI | M |  | VisibleString | String representing URI (Uniform Resource Identifier) |

<<<<<<<<<<<<<<<<<<<< End of 2nd Change >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 3rd Change >>>>>>>>>>>>>>>>>>>>

9.3.5 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) x2ap (2) version1 (1) x2ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 id-E-RAB-Item,

 id-Number-of-Antennaports,

 id-MBSFN-Subframe-Info,

 id-PRACH-Configuration,

 id-CSG-Id,

 id-MDTConfiguration,

 id-SignallingBasedMDTPLMNList,

 id-MultibandInfoList,

 id-FreqBandIndicatorPriority,

 id-NeighbourTAC,

 id-Time-UE-StayedInCell-EnhancedGranularity,

 id-MBMS-Service-Area-List,

 id-HO-cause,

 id-eARFCNExtension,

 id-DL-EARFCNExtension,

 id-UL-EARFCNExtension,

 id-M3Configuration,

 id-M4Configuration,

 id-M5Configuration,

 id-MDT-Location-Info,

 id-NRrestrictioninEPSasSecondaryRAT,

 id-NRrestrictionin5GS,

 id-AdditionalSpecialSubframe-Info,

 id-UEID,

 id-enhancedRNTP,

 id-ProSeUEtoNetworkRelaying,

 id-M6Configuration,

 id-M7Configuration,

 id-OffsetOfNbiotChannelNumberToDL-EARFCN,

 id-OffsetOfNbiotChannelNumberToUL-EARFCN,

 id-AdditionalSpecialSubframeExtension-Info,

 id-BandwidthReducedSI,

 id-extended-e-RAB-MaximumBitrateDL,

 id-extended-e-RAB-MaximumBitrateUL,

 id-extended-e-RAB-GuaranteedBitrateDL,

 id-extended-e-RAB-GuaranteedBitrateUL,

 id-extended-uEaggregateMaximumBitRateDownlink,

 id-extended-uEaggregateMaximumBitRateUplink,

 id-E-RABUsageReport-Item,

 id-SecondaryRATUsageReport-Item,

 id-UEAppLayerMeasConfig,

 id-DL-scheduling-PDCCH-CCE-usage,

 id-UL-scheduling-PDCCH-CCE-usage,

 id-DownlinkPacketLossRate,

 id-UplinkPacketLossRate,

 id-serviceType,

 id-ProtectedEUTRAResourceIndication,

 id-NRS-NSSS-PowerOffset,

 id-NSSS-NumOccasionDifferentPrecoder,

 id-CNTypeRestrictions,

 id-BluetoothMeasurementConfiguration,

 id-WLANMeasurementConfiguration,

 id-ECGI,

 id-NRCGI,

 id-MeNBCoordinationAssistanceInformation,

 id-SgNBCoordinationAssistanceInformation,

 id-NRNeighbourInfoToAdd,

 id-LastNG-RANPLMNIdentity,

 id-BPLMN-ID-Info-EUTRA,

 id-NBIoT-UL-DL-AlignmentOffset,

 id-UnlicensedSpectrumRestriction,

 id-CarrierList,

 id-FrequencyShift7p5khz,

 id-NPRACHConfiguration,

 id-MDTConfigurationNR,

 id-CSI-RSTransmissionIndication,

 id-QoS-Mapping-Information,

 id-IntendedTDD-DL-ULConfiguration-NR,

 id-TraceCollectionEntityURI,

 maxnoofBearers,

 maxCellineNB,

 maxEARFCN,

 maxEARFCNPlusOne,

 newmaxEARFCN,

 maxInterfaces,

 maxnoofBands,

 maxnoofBPLMNs,

 maxnoofAdditionalPLMNs,

 maxnoofCells,

 maxnoofEPLMNs,

 maxnoofEPLMNsPlusOne,

 maxnoofForbLACs,

 maxnoofForbTACs,

 maxnoofNeighbours,

 maxnoofPRBs,

 maxNrOfErrors,

 maxPools,

 maxnoofMBSFN,

 maxnoofTAforMDT,

 maxnoofCellIDforMDT,

 maxnoofMBMSServiceAreaIdentities,

 maxnoofMDTPLMNs,

 maxnoofCoMPHypothesisSet,

 maxnoofCoMPCells,

 maxUEReport,

 maxCellReport,

 maxnoofPA,

 maxCSIProcess,

 maxCSIReport,

 maxSubband,

 maxnooftimeperiods,

 maxnoofCellIDforQMC,

 maxnoofTAforQMC,

 maxnoofPLMNforQMC,

 maxUEsinengNBDU,

 maxnoofProtectedResourcePatterns,

 maxnoNRcellsSpectrumSharingWithE-UTRA,

 maxnoofNrCellBands,

 maxnoofBluetoothName,

 maxnoofWLANName,

 maxofNRNeighbours,

 maxnoofextBPLMNs,

 maxnoofTLAs,

 maxnoofGTPTLAs,

 maxnoofTNLAssociations,

 maxnoofCellsinCHO, maxnoofPC5QoSFlows,

 maxnoofSSBAreas,

 maxnoofNRSCSs,

 maxnoofNRPhysicalResourceBlocks,

 maxnoofNonAnchorCarrierFreqConfig

FROM X2AP-Constants

 <<<<<<<<<<<<<<<<<<<< End of 3rd Change >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 4th Change >>>>>>>>>>>>>>>>>>>>

TraceActivation ::= SEQUENCE {

 eUTRANTraceID EUTRANTraceID,

 interfacesToTrace InterfacesToTrace,

traceDepth TraceDepth,

traceCollectionEntityIPAddress TraceCollectionEntityIPAddress,

 iE-Extensions ProtocolExtensionContainer { {TraceActivation-ExtIEs} } OPTIONAL,

 ...

}

TraceActivation-ExtIEs X2AP-PROTOCOL-EXTENSION ::= {

 { ID id-MDTConfiguration CRITICALITY ignore EXTENSION MDT-Configuration PRESENCE optional}|

 { ID id-UEAppLayerMeasConfig CRITICALITY ignore EXTENSION UEAppLayerMeasConfig PRESENCE optional}|

 { ID id-MDTConfiguration CRITICALITY ignore EXTENSION MDT-ConfigurationNR PRESENCE optional}|

 { ID id-TraceCollectionEntityURI CRITICALITY ignore EXTENSION URI\_address PRESENCE optional},

 ...

}

<<<<<<<<<<<<<<<<<<<< End of 3rd Change >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 4th Change >>>>>>>>>>>>>>>>>>>>

UnlicensedSpectrumRestriction ::= ENUMERATED {

 unlicensed-restricted,

 ...

}

URI\_address ::= VisibleString

UsableABSInformation ::= CHOICE {

 fdd UsableABSInformationFDD,

 tdd UsableABSInformationTDD,

 ...

}

<<<<<<<<<<<<<<<<<<<< End of 4th Change >>>>>>>>>>>>>>>>>>>>

**-- TEXT OMITTED –**

<<<<<<<<<<<<<<<<<<<< 5th Change >>>>>>>>>>>>>>>>>>>>

9.3.7 Constant definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

X2AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

eps-Access (21) modules (3) x2ap (2) version1 (1) x2ap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM X2AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-handoverPreparation ProcedureCode ::= 0

id-handoverCancel ProcedureCode ::= 1

id-loadIndication ProcedureCode ::= 2

id-errorIndication ProcedureCode ::= 3

id-snStatusTransfer ProcedureCode ::= 4

id-uEContextRelease ProcedureCode ::= 5

id-x2Setup ProcedureCode ::= 6

id-reset ProcedureCode ::= 7

id-eNBConfigurationUpdate ProcedureCode ::= 8

id-resourceStatusReportingInitiation ProcedureCode ::= 9

id-resourceStatusReporting ProcedureCode ::= 10

id-privateMessage ProcedureCode ::= 11

id-mobilitySettingsChange ProcedureCode ::= 12

id-rLFIndication ProcedureCode ::= 13

id-handoverReport ProcedureCode ::= 14

id-cellActivation ProcedureCode ::= 15

id-x2Release ProcedureCode ::= 16

id-x2APMessageTransfer ProcedureCode ::= 17

id-x2Removal ProcedureCode ::= 18

id-seNBAdditionPreparation ProcedureCode ::= 19

id-seNBReconfigurationCompletion ProcedureCode ::= 20

id-meNBinitiatedSeNBModificationPreparation ProcedureCode ::= 21

id-seNBinitiatedSeNBModification ProcedureCode ::= 22

id-meNBinitiatedSeNBRelease ProcedureCode ::= 23

id-seNBinitiatedSeNBRelease ProcedureCode ::= 24

id-seNBCounterCheck ProcedureCode ::= 25

id-retrieveUEContext ProcedureCode ::= 26

id-sgNBAdditionPreparation ProcedureCode ::= 27

id-sgNBReconfigurationCompletion ProcedureCode ::= 28

id-meNBinitiatedSgNBModificationPreparation ProcedureCode ::= 29

id-sgNBinitiatedSgNBModification ProcedureCode ::= 30

id-meNBinitiatedSgNBRelease ProcedureCode ::= 31

id-sgNBinitiatedSgNBRelease ProcedureCode ::= 32

id-sgNBCounterCheck ProcedureCode ::= 33

id-sgNBChange ProcedureCode ::= 34

id-rRCTransfer ProcedureCode ::= 35

id-endcX2Setup ProcedureCode ::= 36

id-endcConfigurationUpdate ProcedureCode ::= 37

id-secondaryRATDataUsageReport ProcedureCode ::= 38

id-endcCellActivation ProcedureCode ::= 39

id-endcPartialReset ProcedureCode ::= 40

id-eUTRANRCellResourceCoordination ProcedureCode ::= 41

id-SgNBActivityNotification ProcedureCode ::= 42

id-endcX2Removal ProcedureCode ::= 43

id-dataForwardingAddressIndication ProcedureCode ::= 44

id-gNBStatusIndication ProcedureCode ::= 45

id-deactivateTrace ProcedureCode ::= 46

id-traceStart ProcedureCode ::= 47

id-endcConfigurationTransfer ProcedureCode ::= 48

id-handoverSuccess ProcedureCode ::= 49

id-conditionalHandoverCancel ProcedureCode ::= 50

id-earlyStatusTransfer ProcedureCode ::= 51

id-cellTrafficTrace ProcedureCode ::= 52

id-endcresourceStatusReporting ProcedureCode ::= 53

id-endcresourceStatusReportingInitiation ProcedureCode ::= 54

id-f1CTrafficTransfer ProcedureCode ::= 55

id-UERadioCapabilityIDMapping ProcedureCode ::= 56

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxEARFCN INTEGER ::= 65535

maxEARFCNPlusOne INTEGER ::= 65536

newmaxEARFCN INTEGER ::= 262143

maxInterfaces INTEGER ::= 16

maxCellineNB INTEGER ::= 256

maxnoofBands INTEGER ::= 16

maxnoofBearers INTEGER ::= 256

maxNrOfErrors INTEGER ::= 256

maxnoofPDCP-SN INTEGER ::= 16

maxnoofEPLMNs INTEGER ::= 15

maxnoofEPLMNsPlusOne INTEGER ::= 16

maxnoofForbLACs INTEGER ::= 4096

maxnoofForbTACs INTEGER ::= 4096

maxnoofBPLMNs INTEGER ::= 6

maxnoofAdditionalPLMNs INTEGER ::= 6

maxnoofNeighbours INTEGER ::= 512

maxnoofPRBs INTEGER ::= 110

maxPools INTEGER ::= 16

maxnoofCells INTEGER ::= 16

maxnoofMBSFN INTEGER ::= 8

maxFailedMeasObjects INTEGER ::= 32

maxnoofCellIDforMDT INTEGER ::= 32

maxnoofTAforMDT INTEGER ::= 8

maxnoofMBMSServiceAreaIdentities INTEGER ::= 256

maxnoofMDTPLMNs INTEGER ::= 16

maxnoofCoMPHypothesisSet INTEGER ::= 256

maxnoofCoMPCells INTEGER ::= 32

maxUEReport INTEGER ::= 128

maxCellReport INTEGER ::= 9

maxnoofPA INTEGER ::= 3

maxCSIProcess INTEGER ::= 4

maxCSIReport INTEGER ::= 2

maxSubband INTEGER ::= 14

maxofNRNeighbours INTEGER ::= 1024

maxCellinengNB INTEGER ::= 16384

-- maxnoofNRCarriers INTEGER ::= 32

maxnooftimeperiods INTEGER ::= 2

maxnoofCellIDforQMC INTEGER ::= 32

maxnoofTAforQMC INTEGER ::= 8

maxnoofPLMNforQMC INTEGER ::= 16

maxUEsinengNBDU INTEGER ::= 8192

maxnoofProtectedResourcePatterns INTEGER ::= 16

maxnoNRcellsSpectrumSharingWithE-UTRA INTEGER ::= 64

maxnoofNrCellBands INTEGER ::= 32

maxnoofBluetoothName INTEGER ::= 4

maxnoofWLANName INTEGER ::= 4

maxnoofextBPLMNs INTEGER ::= 12

maxnoofTLAs INTEGER ::= 16

maxnoofGTPTLAs INTEGER ::= 16

maxnoofTNLAssociations INTEGER ::= 32

maxnoofCellsinCHO INTEGER ::= 8

maxnoofPC5QoSFlows INTEGER ::= 2048

maxnoofSSBAreas INTEGER ::= 64

maxnoofNRSCSs INTEGER ::= 5

maxnoofNRPhysicalResourceBlocks INTEGER ::= 275

maxnoofNonAnchorCarrierFreqConfig INTEGER ::= 15

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-E-RABs-Admitted-Item ProtocolIE-ID ::= 0

id-E-RABs-Admitted-List ProtocolIE-ID ::= 1

id-E-RAB-Item ProtocolIE-ID ::= 2

id-E-RABs-NotAdmitted-List ProtocolIE-ID ::= 3

id-E-RABs-ToBeSetup-Item ProtocolIE-ID ::= 4

id-Cause ProtocolIE-ID ::= 5

id-CellInformation ProtocolIE-ID ::= 6

id-CellInformation-Item ProtocolIE-ID ::= 7

id-New-eNB-UE-X2AP-ID ProtocolIE-ID ::= 9

id-Old-eNB-UE-X2AP-ID ProtocolIE-ID ::= 10

id-TargetCell-ID ProtocolIE-ID ::= 11

id-TargeteNBtoSource-eNBTransparentContainer ProtocolIE-ID ::= 12

id-TraceActivation ProtocolIE-ID ::= 13

id-UE-ContextInformation ProtocolIE-ID ::= 14

id-UE-HistoryInformation ProtocolIE-ID ::= 15

id-UE-X2AP-ID ProtocolIE-ID ::= 16

id-CriticalityDiagnostics ProtocolIE-ID ::= 17

id-E-RABs-SubjectToStatusTransfer-List ProtocolIE-ID ::= 18

id-E-RABs-SubjectToStatusTransfer-Item ProtocolIE-ID ::= 19

id-ServedCells ProtocolIE-ID ::= 20

id-GlobalENB-ID ProtocolIE-ID ::= 21

id-TimeToWait ProtocolIE-ID ::= 22

id-GUMMEI-ID ProtocolIE-ID ::= 23

id-GUGroupIDList ProtocolIE-ID ::= 24

id-ServedCellsToAdd ProtocolIE-ID ::= 25

id-ServedCellsToModify ProtocolIE-ID ::= 26

id-ServedCellsToDelete ProtocolIE-ID ::= 27

id-Registration-Request ProtocolIE-ID ::= 28

id-CellToReport ProtocolIE-ID ::= 29

id-ReportingPeriodicity ProtocolIE-ID ::= 30

id-CellToReport-Item ProtocolIE-ID ::= 31

id-CellMeasurementResult ProtocolIE-ID ::= 32

id-CellMeasurementResult-Item ProtocolIE-ID ::= 33

id-GUGroupIDToAddList ProtocolIE-ID ::= 34

id-GUGroupIDToDeleteList ProtocolIE-ID ::= 35

id-SRVCCOperationPossible ProtocolIE-ID ::= 36

id-Measurement-ID ProtocolIE-ID ::= 37

id-ReportCharacteristics ProtocolIE-ID ::= 38

id-ENB1-Measurement-ID ProtocolIE-ID ::= 39

id-ENB2-Measurement-ID ProtocolIE-ID ::= 40

id-Number-of-Antennaports ProtocolIE-ID ::= 41

id-CompositeAvailableCapacityGroup ProtocolIE-ID ::= 42

id-ENB1-Cell-ID ProtocolIE-ID ::= 43

id-ENB2-Cell-ID ProtocolIE-ID ::= 44

id-ENB2-Proposed-Mobility-Parameters ProtocolIE-ID ::= 45

id-ENB1-Mobility-Parameters ProtocolIE-ID ::= 46

id-ENB2-Mobility-Parameters-Modification-Range ProtocolIE-ID ::= 47

id-FailureCellPCI ProtocolIE-ID ::= 48

id-Re-establishmentCellECGI ProtocolIE-ID ::= 49

id-FailureCellCRNTI ProtocolIE-ID ::= 50

id-ShortMAC-I ProtocolIE-ID ::= 51

id-SourceCellECGI ProtocolIE-ID ::= 52

id-FailureCellECGI ProtocolIE-ID ::= 53

id-HandoverReportType ProtocolIE-ID ::= 54

id-PRACH-Configuration ProtocolIE-ID ::= 55

id-MBSFN-Subframe-Info ProtocolIE-ID ::= 56

id-ServedCellsToActivate ProtocolIE-ID ::= 57

id-ActivatedCellList ProtocolIE-ID ::= 58

id-DeactivationIndication ProtocolIE-ID ::= 59

id-UE-RLF-Report-Container ProtocolIE-ID ::= 60

id-ABSInformation ProtocolIE-ID ::= 61

id-InvokeIndication ProtocolIE-ID ::= 62

id-ABS-Status ProtocolIE-ID ::= 63

id-PartialSuccessIndicator ProtocolIE-ID ::= 64

id-MeasurementInitiationResult-List ProtocolIE-ID ::= 65

id-MeasurementInitiationResult-Item ProtocolIE-ID ::= 66

id-MeasurementFailureCause-Item ProtocolIE-ID ::= 67

id-CompleteFailureCauseInformation-List ProtocolIE-ID ::= 68

id-CompleteFailureCauseInformation-Item ProtocolIE-ID ::= 69

id-CSG-Id ProtocolIE-ID ::= 70

id-CSGMembershipStatus ProtocolIE-ID ::= 71

id-MDTConfiguration ProtocolIE-ID ::= 72

id-ManagementBasedMDTallowed ProtocolIE-ID ::= 74

id-RRCConnSetupIndicator ProtocolIE-ID ::= 75

id-NeighbourTAC ProtocolIE-ID ::= 76

id-Time-UE-StayedInCell-EnhancedGranularity ProtocolIE-ID ::= 77

id-RRCConnReestabIndicator ProtocolIE-ID ::= 78

id-MBMS-Service-Area-List ProtocolIE-ID ::= 79

id-HO-cause ProtocolIE-ID ::= 80

id-TargetCellInUTRAN ProtocolIE-ID ::= 81

id-MobilityInformation ProtocolIE-ID ::= 82

id-SourceCellCRNTI ProtocolIE-ID ::= 83

id-MultibandInfoList ProtocolIE-ID ::= 84

id-M3Configuration ProtocolIE-ID ::= 85

id-M4Configuration ProtocolIE-ID ::= 86

id-M5Configuration ProtocolIE-ID ::= 87

id-MDT-Location-Info ProtocolIE-ID ::= 88

id-ManagementBasedMDTPLMNList ProtocolIE-ID ::= 89

id-SignallingBasedMDTPLMNList ProtocolIE-ID ::= 90

id-ReceiveStatusOfULPDCPSDUsExtended ProtocolIE-ID ::= 91

id-ULCOUNTValueExtended ProtocolIE-ID ::= 92

id-DLCOUNTValueExtended ProtocolIE-ID ::= 93

id-eARFCNExtension ProtocolIE-ID ::= 94

id-UL-EARFCNExtension ProtocolIE-ID ::= 95

id-DL-EARFCNExtension ProtocolIE-ID ::= 96

id-AdditionalSpecialSubframe-Info ProtocolIE-ID ::= 97

id-Masked-IMEISV ProtocolIE-ID ::= 98

id-IntendedULDLConfiguration ProtocolIE-ID ::= 99

id-ExtendedULInterferenceOverloadInfo ProtocolIE-ID ::= 100

id-RNL-Header ProtocolIE-ID ::= 101

id-x2APMessage ProtocolIE-ID ::= 102

id-ProSeAuthorized ProtocolIE-ID ::= 103

id-ExpectedUEBehaviour ProtocolIE-ID ::= 104

id-UE-HistoryInformationFromTheUE ProtocolIE-ID ::= 105

id-DynamicDLTransmissionInformation ProtocolIE-ID ::= 106

id-UE-RLF-Report-Container-for-extended-bands ProtocolIE-ID ::= 107

id-CoMPInformation ProtocolIE-ID ::= 108

id-ReportingPeriodicityRSRPMR ProtocolIE-ID ::= 109

id-RSRPMRList ProtocolIE-ID ::= 110

id-MeNB-UE-X2AP-ID ProtocolIE-ID ::= 111

id-SeNB-UE-X2AP-ID ProtocolIE-ID ::= 112

id-UE-SecurityCapabilities ProtocolIE-ID ::= 113

id-SeNBSecurityKey ProtocolIE-ID ::= 114

id-SeNBUEAggregateMaximumBitRate ProtocolIE-ID ::= 115

id-ServingPLMN ProtocolIE-ID ::= 116

id-E-RABs-ToBeAdded-List ProtocolIE-ID ::= 117

id-E-RABs-ToBeAdded-Item ProtocolIE-ID ::= 118

id-MeNBtoSeNBContainer ProtocolIE-ID ::= 119

id-E-RABs-Admitted-ToBeAdded-List ProtocolIE-ID ::= 120

id-E-RABs-Admitted-ToBeAdded-Item ProtocolIE-ID ::= 121

id-SeNBtoMeNBContainer ProtocolIE-ID ::= 122

id-ResponseInformationSeNBReconfComp ProtocolIE-ID ::= 123

id-UE-ContextInformationSeNBModReq ProtocolIE-ID ::= 124

id-E-RABs-ToBeAdded-ModReqItem ProtocolIE-ID ::= 125

id-E-RABs-ToBeModified-ModReqItem ProtocolIE-ID ::= 126

id-E-RABs-ToBeReleased-ModReqItem ProtocolIE-ID ::= 127

id-E-RABs-Admitted-ToBeAdded-ModAckList ProtocolIE-ID ::= 128

id-E-RABs-Admitted-ToBeModified-ModAckList ProtocolIE-ID ::= 129

id-E-RABs-Admitted-ToBeReleased-ModAckList ProtocolIE-ID ::= 130

id-E-RABs-Admitted-ToBeAdded-ModAckItem ProtocolIE-ID ::= 131

id-E-RABs-Admitted-ToBeModified-ModAckItem ProtocolIE-ID ::= 132

id-E-RABs-Admitted-ToBeReleased-ModAckItem ProtocolIE-ID ::= 133

id-E-RABs-ToBeReleased-ModReqd ProtocolIE-ID ::= 134

id-E-RABs-ToBeReleased-ModReqdItem ProtocolIE-ID ::= 135

id-SCGChangeIndication ProtocolIE-ID ::= 136

id-E-RABs-ToBeReleased-List-RelReq ProtocolIE-ID ::= 137

id-E-RABs-ToBeReleased-RelReqItem ProtocolIE-ID ::= 138

id-E-RABs-ToBeReleased-List-RelConf ProtocolIE-ID ::= 139

id-E-RABs-ToBeReleased-RelConfItem ProtocolIE-ID ::= 140

id-E-RABs-SubjectToCounterCheck-List ProtocolIE-ID ::= 141

id-E-RABs-SubjectToCounterCheckItem ProtocolIE-ID ::= 142

id-CoverageModificationList ProtocolIE-ID ::= 143

id-ReportingPeriodicityCSIR ProtocolIE-ID ::= 145

id-CSIReportList ProtocolIE-ID ::= 146

id-UEID ProtocolIE-ID ::= 147

id-enhancedRNTP ProtocolIE-ID ::= 148

id-ProSeUEtoNetworkRelaying ProtocolIE-ID ::= 149

id-ReceiveStatusOfULPDCPSDUsPDCP-SNlength18 ProtocolIE-ID ::= 150

id-ULCOUNTValuePDCP-SNlength18 ProtocolIE-ID ::= 151

id-DLCOUNTValuePDCP-SNlength18 ProtocolIE-ID ::= 152

id-UE-ContextReferenceAtSeNB ProtocolIE-ID ::= 153

id-UE-ContextKeptIndicator ProtocolIE-ID ::= 154

id-New-eNB-UE-X2AP-ID-Extension ProtocolIE-ID ::= 155

id-Old-eNB-UE-X2AP-ID-Extension ProtocolIE-ID ::= 156

id-MeNB-UE-X2AP-ID-Extension ProtocolIE-ID ::= 157

id-SeNB-UE-X2AP-ID-Extension ProtocolIE-ID ::= 158

id-LHN-ID ProtocolIE-ID ::= 159

id-FreqBandIndicatorPriority ProtocolIE-ID ::= 160

id-M6Configuration ProtocolIE-ID ::= 161

id-M7Configuration ProtocolIE-ID ::= 162

id-Tunnel-Information-for-BBF ProtocolIE-ID ::= 163

id-SIPTO-BearerDeactivationIndication ProtocolIE-ID ::= 164

id-GW-TransportLayerAddress ProtocolIE-ID ::= 165

id-Correlation-ID ProtocolIE-ID ::= 166

id-SIPTO-Correlation-ID ProtocolIE-ID ::= 167

id-SIPTO-L-GW-TransportLayerAddress ProtocolIE-ID ::= 168

id-X2RemovalThreshold ProtocolIE-ID ::= 169

id-CellReportingIndicator ProtocolIE-ID ::= 170

id-BearerType ProtocolIE-ID ::= 171

id-resumeID ProtocolIE-ID ::= 172

id-UE-ContextInformationRetrieve ProtocolIE-ID ::= 173

id-E-RABs-ToBeSetupRetrieve-Item ProtocolIE-ID ::= 174

id-NewEUTRANCellIdentifier ProtocolIE-ID ::= 175

id-V2XServicesAuthorized ProtocolIE-ID ::= 176

id-OffsetOfNbiotChannelNumberToDL-EARFCN ProtocolIE-ID ::= 177

id-OffsetOfNbiotChannelNumberToUL-EARFCN ProtocolIE-ID ::= 178

id-AdditionalSpecialSubframeExtension-Info ProtocolIE-ID ::= 179

id-BandwidthReducedSI ProtocolIE-ID ::= 180

id-MakeBeforeBreakIndicator ProtocolIE-ID ::= 181

id-UE-ContextReferenceAtWT ProtocolIE-ID ::= 182

id-WT-UE-ContextKeptIndicator ProtocolIE-ID ::= 183

id-UESidelinkAggregateMaximumBitRate ProtocolIE-ID ::= 184

id-uL-GTPtunnelEndpoint ProtocolIE-ID ::= 185

id-DL-scheduling-PDCCH-CCE-usage ProtocolIE-ID ::= 193

id-UL-scheduling-PDCCH-CCE-usage ProtocolIE-ID ::= 194

id-UEAppLayerMeasConfig ProtocolIE-ID ::= 195

id-extended-e-RAB-MaximumBitrateDL ProtocolIE-ID ::= 196

id-extended-e-RAB-MaximumBitrateUL ProtocolIE-ID ::= 197

id-extended-e-RAB-GuaranteedBitrateDL ProtocolIE-ID ::= 198

id-extended-e-RAB-GuaranteedBitrateUL ProtocolIE-ID ::= 199

id-extended-uEaggregateMaximumBitRateDownlink ProtocolIE-ID ::= 200

id-extended-uEaggregateMaximumBitRateUplink ProtocolIE-ID ::= 201

id-NRrestrictioninEPSasSecondaryRAT ProtocolIE-ID ::= 202

id-SgNBSecurityKey ProtocolIE-ID ::= 203

id-SgNBUEAggregateMaximumBitRate ProtocolIE-ID ::= 204

id-E-RABs-ToBeAdded-SgNBAddReqList ProtocolIE-ID ::= 205

id-MeNBtoSgNBContainer ProtocolIE-ID ::= 206

id-SgNB-UE-X2AP-ID ProtocolIE-ID ::= 207

id-RequestedSplitSRBs ProtocolIE-ID ::= 208

id-E-RABs-ToBeAdded-SgNBAddReq-Item ProtocolIE-ID ::= 209

id-E-RABs-Admitted-ToBeAdded-SgNBAddReqAckList ProtocolIE-ID ::= 210

id-SgNBtoMeNBContainer ProtocolIE-ID ::= 211

id-AdmittedSplitSRBs ProtocolIE-ID ::= 212

id-E-RABs-Admitted-ToBeAdded-SgNBAddReqAck-Item ProtocolIE-ID ::= 213

id-ResponseInformationSgNBReconfComp ProtocolIE-ID ::= 214

id-UE-ContextInformation-SgNBModReq ProtocolIE-ID ::= 215

id-E-RABs-ToBeAdded-SgNBModReq-Item ProtocolIE-ID ::= 216

id-E-RABs-ToBeModified-SgNBModReq-Item ProtocolIE-ID ::= 217

id-E-RABs-ToBeReleased-SgNBModReq-Item ProtocolIE-ID ::= 218

id-E-RABs-Admitted-ToBeAdded-SgNBModAckList ProtocolIE-ID ::= 219

id-E-RABs-Admitted-ToBeModified-SgNBModAckList ProtocolIE-ID ::= 220

id-E-RABs-Admitted-ToBeReleased-SgNBModAckList ProtocolIE-ID ::= 221

id-E-RABs-Admitted-ToBeAdded-SgNBModAck-Item ProtocolIE-ID ::= 222

id-E-RABs-Admitted-ToBeModified-SgNBModAck-Item ProtocolIE-ID ::= 223

id-E-RABs-Admitted-ToBeReleased-SgNBModAck-Item ProtocolIE-ID ::= 224

id-E-RABs-ToBeReleased-SgNBModReqdList ProtocolIE-ID ::= 225

id-E-RABs-ToBeModified-SgNBModReqdList ProtocolIE-ID ::= 226

id-E-RABs-ToBeReleased-SgNBModReqd-Item ProtocolIE-ID ::= 227

id-E-RABs-ToBeModified-SgNBModReqd-Item ProtocolIE-ID ::= 228

id-E-RABs-ToBeReleased-SgNBChaConfList ProtocolIE-ID ::= 229

id-E-RABs-ToBeReleased-SgNBChaConf-Item ProtocolIE-ID ::= 230

id-E-RABs-ToBeReleased-SgNBRelReqList ProtocolIE-ID ::= 231

id-E-RABs-ToBeReleased-SgNBRelReq-Item ProtocolIE-ID ::= 232

id-E-RABs-ToBeReleased-SgNBRelConfList ProtocolIE-ID ::= 233

id-E-RABs-ToBeReleased-SgNBRelConf-Item ProtocolIE-ID ::= 234

id-E-RABs-SubjectToSgNBCounterCheck-List ProtocolIE-ID ::= 235

id-E-RABs-SubjectToSgNBCounterCheck-Item ProtocolIE-ID ::= 236

id-RRCContainer ProtocolIE-ID ::= 237

id-SRBType ProtocolIE-ID ::= 238

id-Target-SgNB-ID ProtocolIE-ID ::= 239

id-HandoverRestrictionList ProtocolIE-ID ::= 240

id-SCGConfigurationQuery ProtocolIE-ID ::= 241

id-SplitSRB ProtocolIE-ID ::= 242

id-NRUeReport ProtocolIE-ID ::= 243

id-InitiatingNodeType-EndcX2Setup ProtocolIE-ID ::= 244

id-InitiatingNodeType-EndcConfigUpdate ProtocolIE-ID ::= 245

id-RespondingNodeType-EndcX2Setup ProtocolIE-ID ::= 246

id-RespondingNodeType-EndcConfigUpdate ProtocolIE-ID ::= 247

id-NRUESecurityCapabilities ProtocolIE-ID ::= 248

id-PDCPChangeIndication ProtocolIE-ID ::= 249

id-ServedEUTRAcellsENDCX2ManagementList ProtocolIE-ID ::= 250

id-CellAssistanceInformation ProtocolIE-ID ::= 251

id-Globalen-gNB-ID ProtocolIE-ID ::= 252

id-ServedNRcellsENDCX2ManagementList ProtocolIE-ID ::= 253

id-UE-ContextReferenceAtSgNB ProtocolIE-ID ::= 254

id-SecondaryRATUsageReport ProtocolIE-ID ::= 255

id-ActivationID ProtocolIE-ID ::= 256

id-MeNBResourceCoordinationInformation ProtocolIE-ID ::= 257

id-SgNBResourceCoordinationInformation ProtocolIE-ID ::= 258

id-ServedEUTRAcellsToModifyListENDCConfUpd ProtocolIE-ID ::= 259

id-ServedEUTRAcellsToDeleteListENDCConfUpd ProtocolIE-ID ::= 260

id-ServedNRcellsToModifyListENDCConfUpd ProtocolIE-ID ::= 261

id-ServedNRcellsToDeleteListENDCConfUpd ProtocolIE-ID ::= 262

id-E-RABUsageReport-Item ProtocolIE-ID ::= 263

id-Old-SgNB-UE-X2AP-ID ProtocolIE-ID ::= 264

id-SecondaryRATUsageReportList ProtocolIE-ID ::= 265

id-SecondaryRATUsageReport-Item ProtocolIE-ID ::= 266

id-ServedNRCellsToActivate ProtocolIE-ID ::= 267

id-ActivatedNRCellList ProtocolIE-ID ::= 268

id-SelectedPLMN ProtocolIE-ID ::= 269

id-UEs-ToBeReset ProtocolIE-ID ::= 270

id-UEs-Admitted-ToBeReset ProtocolIE-ID ::= 271

id-RRCConfigIndication ProtocolIE-ID ::= 272

id-DownlinkPacketLossRate ProtocolIE-ID ::= 273

id-UplinkPacketLossRate ProtocolIE-ID ::= 274

id-SubscriberProfileIDforRFP ProtocolIE-ID ::= 275

id-serviceType ProtocolIE-ID ::= 276

id-AerialUEsubscriptionInformation ProtocolIE-ID ::= 277

id-SGNB-Addition-Trigger-Ind ProtocolIE-ID ::= 278

id-MeNBCell-ID ProtocolIE-ID ::= 279

id-RequestedSplitSRBsrelease ProtocolIE-ID ::= 280

id-AdmittedSplitSRBsrelease ProtocolIE-ID ::= 281

id-NRS-NSSS-PowerOffset ProtocolIE-ID ::= 282

id-NSSS-NumOccasionDifferentPrecoder ProtocolIE-ID ::= 283

id-ProtectedEUTRAResourceIndication ProtocolIE-ID ::= 284

id-InitiatingNodeType-EutranrCellResourceCoordination ProtocolIE-ID ::= 285

id-RespondingNodeType-EutranrCellResourceCoordination ProtocolIE-ID ::= 286

id-DataTrafficResourceIndication ProtocolIE-ID ::= 287

id-SpectrumSharingGroupID ProtocolIE-ID ::= 288

id-ListofEUTRACellsinEUTRACoordinationReq ProtocolIE-ID ::= 289

id-ListofEUTRACellsinEUTRACoordinationResp ProtocolIE-ID ::= 290

id-ListofEUTRACellsinNRCoordinationReq ProtocolIE-ID ::= 291

id-ListofNRCellsinNRCoordinationReq ProtocolIE-ID ::= 292

id-ListofNRCellsinNRCoordinationResp ProtocolIE-ID ::= 293

id-E-RABs-AdmittedToBeModified-SgNBModConfList ProtocolIE-ID ::= 294

id-E-RABs-AdmittedToBeModified-SgNBModConf-Item ProtocolIE-ID ::= 295

id-UEContextLevelUserPlaneActivity ProtocolIE-ID ::= 296

id-ERABActivityNotifyItemList ProtocolIE-ID ::= 297

id-InitiatingNodeType-EndcX2Removal ProtocolIE-ID ::= 298

id-RespondingNodeType-EndcX2Removal ProtocolIE-ID ::= 299

id-RLC-Status ProtocolIE-ID ::= 300

id-CNTypeRestrictions ProtocolIE-ID ::= 301

id-uLpDCPSnLength ProtocolIE-ID ::= 302

id-BluetoothMeasurementConfiguration ProtocolIE-ID ::= 303

id-WLANMeasurementConfiguration ProtocolIE-ID ::= 304

id-NRrestrictionin5GS ProtocolIE-ID ::= 305

id-dL-Forwarding ProtocolIE-ID ::= 306

id-E-RABs-DataForwardingAddress-List ProtocolIE-ID ::= 307

id-E-RABs-DataForwardingAddress-Item ProtocolIE-ID ::= 308

id-Subscription-Based-UE-DifferentiationInfo ProtocolIE-ID ::= 309

id-GNBOverloadInformation ProtocolIE-ID ::= 310

id-dLPDCPSnLength ProtocolIE-ID ::= 311

id-secondarysgNBDLGTPTEIDatPDCP ProtocolIE-ID ::= 312

id-secondarymeNBULGTPTEIDatPDCP ProtocolIE-ID ::= 313

id-lCID ProtocolIE-ID ::= 314

id-duplicationActivation ProtocolIE-ID ::= 315

id-ECGI ProtocolIE-ID ::= 316

id-RLCMode-transferred ProtocolIE-ID ::= 317

id-E-RABs-Admitted-ToBeReleased-SgNBRelReqAckList ProtocolIE-ID ::= 318

id-E-RABs-Admitted-ToBeReleased-SgNBRelReqAck-Item ProtocolIE-ID ::= 319

id-E-RABs-ToBeReleased-SgNBRelReqdList ProtocolIE-ID ::= 320

id-E-RABs-ToBeReleased-SgNBRelReqd-Item ProtocolIE-ID ::= 321

id-NRCGI ProtocolIE-ID ::= 322

id-MeNBCoordinationAssistanceInformation ProtocolIE-ID ::= 323

id-SgNBCoordinationAssistanceInformation ProtocolIE-ID ::= 324

id-new-drb-ID-req ProtocolIE-ID ::= 325

id-endcSONConfigurationTransfer ProtocolIE-ID ::= 326

id-NRNeighbourInfoToAdd ProtocolIE-ID ::= 327

id-NRNeighbourInfoToModify ProtocolIE-ID ::= 328

id-DesiredActNotificationLevel ProtocolIE-ID ::= 329

id-LocationInformationSgNBReporting ProtocolIE-ID ::= 330

id-LocationInformationSgNB ProtocolIE-ID ::= 331

id-LastNG-RANPLMNIdentity ProtocolIE-ID ::= 332

id-EUTRANTraceID ProtocolIE-ID ::= 333

id-additionalPLMNs-Item ProtocolIE-ID ::= 334

id-InterfaceInstanceIndication ProtocolIE-ID ::= 335

id-BPLMN-ID-Info-EUTRA ProtocolIE-ID ::= 336

id-BPLMN-ID-Info-NR ProtocolIE-ID ::= 337

id-NBIoT-UL-DL-AlignmentOffset ProtocolIE-ID ::= 338

id-ERABs-transferred-to-MeNB ProtocolIE-ID ::= 339

id-AdditionalRRMPriorityIndex ProtocolIE-ID ::= 340

id-LowerLayerPresenceStatusChange ProtocolIE-ID ::= 341

id-FastMCGRecovery-SN-to-MN ProtocolIE-ID ::= 342

id-RequestedFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 343

id-AvailableFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 344

id-RequestedFastMCGRecoveryViaSRB3Release ProtocolIE-ID ::= 345

id-ReleaseFastMCGRecoveryViaSRB3 ProtocolIE-ID ::= 346

id-FastMCGRecovery-MN-to-SN ProtocolIE-ID ::= 347

id-PartialListIndicator ProtocolIE-ID ::= 348

id-MaximumCellListSize ProtocolIE-ID ::= 349

id-MessageOversizeNotification ProtocolIE-ID ::= 350

id-CellandCapacityAssistInfo ProtocolIE-ID ::= 351

id-TNLConfigurationInfo ProtocolIE-ID ::= 352

id-TNLA-To-Add-List ProtocolIE-ID ::= 353

id-TNLA-To-Update-List ProtocolIE-ID ::= 354

id-TNLA-To-Remove-List ProtocolIE-ID ::= 355

id-TNLA-Setup-List ProtocolIE-ID ::= 356

id-TNLA-Failed-To-Setup-List ProtocolIE-ID ::= 357

id-UnlicensedSpectrumRestriction ProtocolIE-ID ::= 358

id-UEContextReferenceatSourceNGRAN ProtocolIE-ID ::= 359

id-EPCHandoverRestrictionListContainer ProtocolIE-ID ::= 360

id-CHOinformation-REQ ProtocolIE-ID ::= 361

id-CHOinformation-ACK ProtocolIE-ID ::= 362

id-DAPSRequestInfo ProtocolIE-ID ::= 363

id-RequestedTargetCellID ProtocolIE-ID ::= 364

id-CandidateCellsToBeCancelledList ProtocolIE-ID ::= 365

id-DAPSResponseInfo ProtocolIE-ID ::= 366

id-ProcedureStage ProtocolIE-ID ::= 367

id-CHO-DC-Indicator ProtocolIE-ID ::= 368

id-Ethernet-Type ProtocolIE-ID ::= 369

id-NRV2XServicesAuthorized ProtocolIE-ID ::= 370

id-NRUESidelinkAggregateMaximumBitRate ProtocolIE-ID ::= 371

id-PC5QoSParameters ProtocolIE-ID ::= 372

id-NPRACHConfiguration ProtocolIE-ID ::= 373

id-NBIoT-RLF-Report-Container ProtocolIE-ID ::= 374

id-MDTConfigurationNR ProtocolIE-ID ::= 375

id-PrivacyIndicator ProtocolIE-ID ::= 376

id-TraceCollectionEntityIPAddress ProtocolIE-ID ::= 377

id-UERadioCapabilityID ProtocolIE-ID ::= 378

id-SNtriggered ProtocolIE-ID ::= 379

id-CSI-RSTransmissionIndication ProtocolIE-ID ::= 380

id-DLCarrierList ProtocolIE-ID ::= 381

id-TargetCellInNGRAN ProtocolIE-ID ::= 382

id-eNB-Measurement-ID-ENDC ProtocolIE-ID ::= 383

id-engNB-Measurement-ID-ENDC ProtocolIE-ID ::= 384

id-TDDULDLConfigurationCommonNR ProtocolIE-ID ::= 385

id-CarrierList ProtocolIE-ID ::= 386

id-ULCarrierList ProtocolIE-ID ::= 387

id-FrequencyShift7p5khz ProtocolIE-ID ::= 388

id-SSB-PositionsInBurst ProtocolIE-ID ::= 389

id-NRCellPRACHConfig ProtocolIE-ID ::= 390

id-CellToReport-ENDC ProtocolIE-ID ::= 391

id-CellToReport-ENDC-Item ProtocolIE-ID ::= 392

id-CellMeasurementResult-ENDC ProtocolIE-ID ::= 393

id-CellMeasurementResult-ENDC-Item ProtocolIE-ID ::= 394

id-IABNodeIndication ProtocolIE-ID ::= 395

id-QoS-Mapping-Information ProtocolIE-ID ::= 396

id-F1CTrafficContainer ProtocolIE-ID ::= 397

id-IABInformation ProtocolIE-ID ::= 398

id-IntendedTDD-DL-ULConfiguration-NR ProtocolIE-ID ::= 399

id-UERadioCapability ProtocolIE-ID ::= 400

id-TraceCollectionEntityURI ProtocolIE-ID ::= XXX

END

-- ASN1STOP

<<<<<<<<<<<<<<<<<<<< End of Changes >>>>>>>>>>>>>>>>>>>>