3GPP TSG-RAN WG3 #111-e R3-210989

25 January - 4 February 2021

**Agenda item: 10.2.1.1**

**Source: Huawei (moderator)**

**Title: CB: # 1001\_SONMDT\_PCISelect - Summary of email discussion**

**Document for: Approval**

# 1 Introduction

This paper provides summary of discussions on the following CB:

**CB: #** **1001\_SONMDT\_PCISelect**

**- Discuss and attempt to agree the stage-2 TP**

(HW - moderator)

Summary of offline disc [R3-210989](Inbox\\R3-210989.zip)

# 2 For the Chairman’s Notes

[To be completed]

# 3 Discussion

In [R3-210441](file:///D:\RAN3\111e\Docs\R3-210441.zip), it is proposed that:

**Proposal: It is proposed to agree on the stag 2 TP in Annex to enable the gNB restrict the PCI list when selecting a new PCI from the PCI list for a NR cell in case of distributed PCI selection.**

The reason is that in LTE, the eNB will restrict the PCI list by removing some PCIs which are used by neighbour cells. And in NR, the gNB cannot randomly select a PCI in the list as the PCI value for a NR cell. Without any description in stage 2 may make the specification ambiguous and mislead the product implementation.

**Please provide your view on the above proposal.**

|  |  |  |
| --- | --- | --- |
| Company | Agree on the TP? (Yes/No) | Comment |
|  |  |  |

**Any comments on the TP if any can be provided here.**

|  |  |
| --- | --- |
| Company | Comments on the TP |
|  |  |

# 4 Conclusion, Recommendations [if needed]

If needed

# 5 References

|  |  |
| --- | --- |
| [R3-210441](Docs\R3-210441.zip) | (TP for SON BL CR for TS 38.300):Further clarification on distributed PCI selection (Huawei) |