3GPP TSG-RAN WG3 #111-e R3-210996

Online, January 25th - Feburary 4th, 2021

Agenda Item: 10.2.3

Source: CMCC (moderator)

Title: Support of inter-system inter-RAT energy saving

Document for: Discussion and Decision

# Introduction

**CB: # 1008\_SONMDT\_InterSystemEnergy**

**- Minimum activation time?**

**- NG-RAN node preventing camping and handovers?**

**- Cell status information in Inter-System SON Information Report message in S1AP and NGAP?**

**- Applicability of new state for intra-system energy saving**

**- May also discuss other issues based on papers submitted**

**- Try to reach high-level agreements in the first phase, proceed to TPs in the second phase of the email discussion**

(CMCC - moderator)

Summary of offline disc [R3-210996](file:///C%3A%5CUsers%5Ccmcc%5CDocuments%5CWeChat%20Files%5Cliangzai936046%5CFileStorage%5CFile%5C2021-01%5CInbox%5CR3-210996.zip)

Since the views from the papers proposed in RAN3#111-e meeting are relatively consistent, we hope to reach high-level agreements in the first phase and proceed to TPs in the second phase of the email discussion.

# For the Chairman’s Notes

TBD

# Discussion

## Minimum Activation Time

Based on the reference paper [1][3], it is proposed to add the minimum activation time IE in the cell activation request to avoid ping-pong effect. The minimum activation time is a period of time the requesting node wants the cells to be activated before switching off. For the reference, the description of inter-RAT energy saving for E-UTRA cell case in TS 36.300 is specified that

*If basic coverage is ensured by UTRAN or GERAN cells, the eNB owning the capacity booster cell may receive a re-activation request from a GERAN or UTRAN node by means of the MME Direct Information Transfer procedure over S1. The eNB owning the capacity booster cell may also receive from the sending GERAN or UTRAN node the minimum time before that cell switches off;*

*The eNB owning the concerned cell may choose to delay or not to send indication(s) if the sending GERAN or UTRAN node has included the minimum activation time in the re-activation request.*

**Question 1: Do you agree with introducing minimum activation time for inter-system inter-RAT energy saving?**

|  |  |
| --- | --- |
| Company | Comment |
|  |  |
|  |  |
|  |  |
|  |  |

## NG-RAN Node Preventing Camping and Handovers

[1] proposed the standard should not specify that re-activated NR cell shall prevent new user from camping or accessing services during the minimum activation period to avoid ping-pong switching on/off.

The moderator found this refers to the description in TS 36.300 which is related to minimum activation time,

*The eNB owning the capacity booster cell may also receive from the sending GERAN or UTRAN node the minimum time before that cell switches off; during this time, the same eNB may prevent idle mode UEs from camping on the cell and may prevent incoming handovers to the same cell.*

**However, there is no such kind of description in the current TS 38.300 for inter-system inter-RAT energy saving. The corresponding TP makes some changes to the intra-system energy saving part which seems Rel-16 correction, not within the scope of Rel-17.**

**Question: What’s your view on this proposal of standard should not specify that re-activated NR cell shall prevent new user from camping or accessing services during the minimum activation period to avoid ping-pong switching on/off?**

|  |  |
| --- | --- |
| Company | Comment |
|  |  |
|  |  |
|  |  |
|  |  |

## Cell Status

Based on the reference paper [2], a low power consumption cell status information is introduced that the NR gNB could inform this status to 4G eNB to forbid UEs with high data rate service to be handover to 5G network for the purpose of reducing the power consumption. For idle UE or inactive UE, this status does not change any mobility strategy.

**Question: Do you agree with introducing new cell status information in Rel-17?**

|  |  |
| --- | --- |
| Company | Comment |
|  |  |
|  |  |
|  |  |
|  |  |

## Applicability of Cell Status Information in NG/S1 messages

Based on the reference paper [2], if the new cell status is adopted, the cell status information is carried in the existing Inter-System SON Information Report message in S1AP and NGAP.

**Proposal: If the new cell status is adopted, the cell status information is carried in the existing Inter-System SON Information Report message in S1AP and NGAP.**

**Question: Companies are invited to give your views on the proposal 3.**

|  |  |
| --- | --- |
| Company | Comment |
|  |  |
|  |  |
|  |  |
|  |  |

# Conclusion, Recommendations [if needed]

If needed

# References

1. R3-210567 Consideration on inter-system inter-RAT energy saving, ZTE.
2. R3-210839 Further Discussion on new Cell Status for Energy Saving Operation, China Telcom.
3. R3-210909 Discussion on inter-system inter-RAT energy saving, CMCC.