**3GPP T****SG-RAN WG3 Meeting #110-e R3-210997**

**Online, 25th January – 5th February 2020**

Agenda Item: 10.2.4

Source: Ericsson

Title: Summary of Discussion for SONMDT\_InterSystemLoad

Document for: Discussion, Decision

# Introduction

A Summary of Offline Discussions has been assigned to the topic of SONMDT\_InterSystemLoad.

The discussion has been summarised as follows in the meeting minutes:

**CB: # 1009\_SONMDT\_InterSystemLoad**

**CAC is enough? Other parameters (PRB utilization, Number of RRC connections, Number of active UEs, TNL Load, Hardware Load, etc.)?**

**Load information in HO signaling?**

**New threshold-based method?**

**May also discuss other issues based on papers submitted**

**Try to reach high-level agreements in the first phase, proceed to TPs in the second phase of the email discussion**

**(E/// - moderator)**

The following was agreed so far:

Introduce Inter System Load Balancing mechanisms on the basis of the solution available in E-UTRAN

Introduce Inter System Load Balancing by means of mechanisms that resemble or reuse the SON Configuration Transfer IE for the purpose of configuring load balancing metrics and reporting load balancing measurements

Use S1: eNB CONFIGURATION TRANSFER, S1: MME CONFIGURATION TRANSFER, NG: UL RAN CONFIGURATION TRANSFER and NG: DL RAN CONFIGURATION TRANSFER for the transfer of inter system load balancing via means of mechanisms that resemble or reuse the SON Configuration Transfer IEs. It is FFS whether further details on the signaling part need to be introduced

Adopt signaling of the Composite Available Capacity (Cell Capacity Class value and Capacity Value) for inter system MLB

Adoption of further MLB metrics is FFS

Event Based Reporting and Periodic Reporting (only in case specific conditions are met), are agreed to be supported for inter system MLB. The mechanism should avoid excessive signaling

Introduce a new mechanism for Inter System Status Request/Response/Update over NG: UL RAN CONFIGURATION TRANSFER and NG: DL RAN CONFIGURATION TRANSFER, via modification of the Inter-System SON Information IE

Introduce a new mechanism for Inter System Status Request/Response/Update over S1: UL RAN CONFIGURATION TRANSFER and S1: DL RAN CONFIGURATION TRANSFER, via reuse of the Inter-System SON Configuration Transfer IE

Support periodic inter system load reporting with periodicity not lower than 1000ms and threshold-based load reporting, subject to confirmation from CT

We do not support per slice load information for inter system load balancing in the current release

Support an explicitly signaled threshold configuration for inter system load information reporting; details are FFS

Agree to CAC encoding as defined in LTE, e.g. in TS36.413, as a starting point. Whether CAC is encoded according to the sender’s rules is FFS

Whether to support the Number of active UEs for inter system load balancing is FFS

*It is FFS whether to support signaling of PRB utilization for inter system load balancing in the current release;*

*It is FFS whether to support signaling of the Number of RRC connections for inter system load balancing in the current release;*

*It is FFS whether to support signaling of the TNL Available Capacity for inter system load balancing in the current release;*

*To be continued...*

# For the Chairman’s Notes

**[To be added]**

# Discussion

## Signalling mechanisms for Inter System Load Balancing

In past RAN3 meetings it was agreed that

Introduce a new mechanism for Inter System Status Request/Response/Update over NG: UL RAN CONFIGURATION TRANSFER and NG: DL RAN CONFIGURATION TRANSFER, via modification of the Inter-System SON Information IE

Introduce a new mechanism for Inter System Status Request/Response/Update over S1: UL RAN CONFIGURATION TRANSFER and S1: DL RAN CONFIGURATION TRANSFER, via reuse of the Inter-System SON Configuration Transfer IE

Support periodic inter system load reporting with periodicity not lower than 1000ms and threshold-based load reporting, subject to confirmation from CT

Support an explicitly signaled threshold configuration for inter system load information reporting; details are FFS

The above agreements point at a signalling solution for Inter System Load Balancing, where load information is either exchanged periodically, or where load information is exchanged at the occurrence of specific events.

In [1], a new proposal for signalling load information across systems is made. Namely, it is proposed to support the inclusion of load information as part of the inter system HO preparation signalling.

**Companies are invited to provide their view on whether Inter System load information exchange should happen also by means of including load information in the HO preparation signalling.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Load Info within HO preparation: Yes/No**  | **Comments** |
| Ericsson | No | The periodic and event-based reporting mechanisms enables all levels of LB information signalling granularity. Including LB info in HO preparation signalling may delay the HO preparation due to the need of deriving LB info before messages are signaled. Also, the procedure would be more error prone, in case any issue with Load Metrics is encountered at the receiver.  |
| Nokia | Yes | The other forms of reporting require additional signaling. Including the information in the HO signaling could help. |

## CAC encoding

One of the FFSs that remain to be solved is the following:

Agree to CAC encoding as defined in LTE, e.g. in TS36.413, as a starting point. Whether CAC is encoded according to the sender’s rules is FFS

In [2] and [3] it is proposed to adopt the rule of encoding CAC as per LTE specifications (i.e. as per TS36.413). In [5] it is proposed to report CAC according to the sender’s specifications of reference.

**Companies are invited to provide their views on the preferred way to encode the CAC for inter system load balancing**

|  |  |  |
| --- | --- | --- |
| **Company** | **Follow LTE Encoding/Encode as per senders specs**  | **Comments** |
| Ericsson | Follow LTE Encoding | We would prefer to avoid impacts on LTE and therefore we would like to avoid that LTE needs to understand the new CAC structure supported in NR.  |
| Nokia | Neutral | As long as CAC is used, it does not matter – it is defined in nearly identical way in LTE and in NR. |

## Inter System Load Metrics

A number of load metrics were discussed for inter system load balancing. It was already agreed to exchange the CAC, however the following FFS have been captured:

Whether to support the Number of active UEs for inter system load balancing is FFS

*It is FFS whether to support signaling of PRB utilization for inter system load balancing in the current release;*

*It is FFS whether to support signaling of the Number of RRC connections for inter system load balancing in the current release;*

*It is FFS whether to support signaling of the TNL Available Capacity for inter system load balancing in the current release;*

[1], [2] and [3] state that reporting the CAC is sufficient for inter system load balancing. In particular, the following observations were made concerning other load metrics:

* Even if PRB concept is valid for both LTE and NR, only a subcarrier spacing of 15 kHz is possible for LTE, which may be not the same as the one used in NR. This means that in general there is no common interpretation of PRB usage between LTE and NR
* The number of RRC connections can’t be interpreted if the total limit is not known. In light of the RRC Inactive feature, different implementation of RRC available states in LTE and NR provide different views in the two RATs
* The number of active UEs refers to UEs in RRC\_CONNECTED state for which there is data available for transmission or reception. This metric requires full knowledge of the resource structure of the sending node, as well as knowledge of the resource utilization. It is difficult to ensure such understanding between E-UTRAN and NG-RAN, hence we prefer to not use this metric for Inter-System MLB purposes.
* The TNL load information is different in LTE and in NR thus causing extra implementation burden; it should instead be included in the Composite Available Capacity

On the other hand, [5] proposes to signal between LTE and NR PRB usage, Number of RRC Connections and number of Active UEs. While [4] proposes that“The Number of active UEs, RRC Connections, TNL Capacity Indicator and PRB Utilization could be considered to transmit from gNB to eNB, while the Hardware Load, S1 TNL Load and PRB Utilization could be considered to transmit from eNB to gNB”

**In order to move forward, companies are invited to provide their view on the load metrics for inter system load balancing that are considered essential for Rel17**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Ericsson | CAC is the most important metric. We propose to use CAC for Rel17  |
| Nokia | CAC, same like Ericsson above. |

## Threshold structure for Inter System Load Balancing

In [3], [5] and [6] it is proposed to adopt a new threshold scheme different from the one use in LTE. This threshold scheme defines up to two thresholds, where the reporting event is triggered if the load metric goes below a threshold, or above a threshold or if the metric is in between thresholds.

In [2] a modification of the LTE threshold mechanism is proposed, where a subset of the range of values for the reported metric can be selected and where such subset is divided in equal parts by means of thresholds.

**Companies are invited to express their view on the threshold mechanisms preferred for inter system load balancing**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Ericsson | We prefer the mechanism with up to two thresholds defined in [3] because it allows to set thresholds in a flexible way (i.e. without keeping the rule of equal partitioning of the metrics values range). Such flexibility is needed to cope with both cases of load balancing (equal load across systems) and cases of load steering (higher loads in more capable systems). |
| Nokia | For simplicity, even threshold ranges are sufficient in Rel.17. More detailed information could be obtained if load info is appended to HO signalling. |

# Conclusion, Recommendations

# References

[1] R3-210078, Additional method for the inter-RAT load information exchange (Nokia, Nokia Shanghai Bell)

[2] R3-210400, (TP for SON BLCR for 38.413) Inter-System Load Balancing (Huawei)

[3] R3-210683, (TP for SON for TS 38.413, TS 38.300, TS 36.300): Inter-System Load Balancing BL CR (Ericsson)

[4] R3-210802, Further Discussion on Inter-system Load Balancing in NR (ZTE, China Telecom, China Unicom)

[5] R3-210897, More thoughts on inter-system load balancing (CMCC)

[6] R3-210804, (TP for SON BL CR 38.413) Inter-system Load Balancing (ZTE, China Telecom, China Unicom)