**3GPP TSG-RAN WG3 Meeting #111-e *R3-211188***

**25 Jan- 5 Feb 2021**

**Online**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.463** | **CR** | **0568** | **rev** | **1** | **Current version:** | **16.4.0** |  |
|  |
| *For* ***[HE](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)******[LP](http://www.3gpp.org/3G_Specs/CRs.htm%22%20%5Cl%20%22_blank)*** *on using this form: comprehensive instructions can be found at <http://www.3gpp.org/Change-Requests>.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Update on QoS monitoring control |
|  |  |
| ***Source to WG:*** | ZTE |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2020-1-11 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | According to TS29.512:*If the PCF receives the request to disable the QoS monitoring from the AF, the PCF shall update the PCC rule with the "refQosMon" attribute set to NULL. The PCF may also remove the corresponding QoS Monitoring Data if no PCC rule is referring to it.*Therefore, the Full control of QoS monitoring should be supported in RAN side. |
|  |  |
| ***Summary of change:*** | Extend the value of the *QoS Monitoring Request* IE.Impact Analysis:Impact assessment towards the previous version of the specification (same release): This CR has isolate impact on the QoS monitoring over NG.This CR has ASN.1 impact with backward compatible way. |
|  |  |
| ***Consequences if not approved:*** | The Full control of QoS monitoring for the QoS flow can not be supported which brings gap between CN and RAN. |
|  |  |
| ***Clauses affected:*** | 9.3.1.26, 9.4.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev 1:Add new “stop” value in QoS Monitoring Request IE and update semantics description |

<<<<<<<<<<<<<<<<<<<< Start of the First Change >>>>>>>>>>>>>>>>>>>>

#### 9.3.1.26 QoS Flow Level QoS Parameters

This IE defines the QoS parameters to be applied to a QoS Flow.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| CHOICE *QoS Characteristics* | M |  |  |  | - |  |
| >*Non-dynamic 5QI* |  |  |  |  |  |  |
| >>Non Dynamic 5QI Descriptor | M |  | 9.3.1.27 |  | - |  |
| >*Dynamic 5QI* |  |  |  |  |  |  |
| >>Dynamic 5QI Descriptor | M |  | 9.3.1.28 |  | - |  |
| NG-RAN Allocation and Retention Priority | M |  | 9.3.1.29 |  | - |  |
| GBR QoS Flow Information | O |  | 9.3.1.30 | This IE shall be present for GBR QoS Flows and is ignored otherwise. | - |  |
| Reflective QoS Attribute | O |  | ENUMERATED (subject to, …) | Details in TS 23.501 [20]. This IE applies to Non-GBR flows only and is ignored otherwise. | - |  |
| Additional QoS Flow Information | O |  | ENUMERATED (more likely, …) | This IE indicates that traffic for this QoS flow is likely to appear more often than traffic for other flows established for the PDU Session. | - |  |
| Paging Priority Indicator (PPI) | O |  | 9.3.1.55 |  | - |  |
| RDI | O |  | ENUMERATED (enabled, …) | Indicates whether Reflective QoS flow to DRB mapping should be applied. | - |  |
| QoS Monitoring Request | O |  | ENUMERATED (UL, DL, Both, …, stop) | Indicates to measure UL, or DL, or both UL/DL delays for the associated QoS flow or stop the corresponding QoS monitoring. | YES | ignore |

<<<<<<<<<<<<<<<<<<<< End of the First Change >>>>>>>>>>>>>>>>>>>>

9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

QosMonitoringRequest ::= ENUMERATED {ul, dl, both, ..., stop}

<<<<<<<<<<<<<<<<<<<< End of the Change >>>>>>>>>>>>>>>>>>>>