**3GPP T****SG-RAN WG3 Meeting #110-e R3-210988**

**Online, 25th January – 5th February 2020**

Agenda Item: 31.2.1

Source: Ericsson

Title: Summary of Discussion for Local\_NG-RANnode\_ID

Document for: Discussion, Decision

# Introduction

A Summary of Offline Discussions has been assigned to the topic of Local\_NG-RANnode\_ID.

The discussion has been summarised as follows in the meeting minutes:

**CB: # 23\_Local\_NG-RANnode\_ID**

**HW**

**further clarify the possible solution for gNB ID resolution from I-RNTI, especially on the observations raised**

**any new solution shall support the following requirements:**

**1) Work well in multi-vendor scenario**

**2) Support Network Sharing**

**3) Avoid any collision or confusion**

**4) Solution should be backward compatible**

**ZTE**

**discuss whether a short gNB ID would be needed in I-RNTI.**

**three alternatives to address the ambiguity caused by different lengths of (short) NG-RAN Node IDs:**

**Alt1: length of the (short) NG-RAN Node ID part in I-RNTI is fixed in the specification, as that for Resume ID in LTE.**

**Alt2: length of (short) NG-RAN Node ID part in I-RNTI is explicitly sent to the new NG-RAN node with the I-RNTI.**

**Alt3: length of (short) NG-RAN Node ID part in I-RNTI is self-contained in the I-RNTI, e.g., to separate 3bits in I-RNTI for using as I-RNTI structure indication.**

**Nok**

**Specify sol2: the bits encoding the old gNB ID pointer are simply generated taking the modulo value of the true gNB ID (no XnAP impact)**

**E///,AT&T,Vz**

**agree on a standardized structure of the I-RNTI. Two options:**

**Opt1: the I-RNTI structure includes a Local gNB Identifier and a UE Context identifier. The length in bits of the Local gNB Identifier and the length in bit of the UE Context identifier are identical in the complete PLMN. More than one Local gNB Identifiers can be assigned per RAN node.**

**Opt2: the I-RNTI structure includes an I-RNTI profile of fixed length, a Local gNB Identifier and a UE Context Identifier. The length of the Local gNB Identifier and the length of the UE Context Identifier are encoded in the I-RNTI profile.**

**- To be considered in the discussion: are principles in 0448 agreeable as basis to further guide selection? Is it possible at all to avoid st3 impact? If st3 impact is unavoidable, which option is preferable?**

**- check details; merge/revise as needed**

(E/// - moderator)

# For the Chairman’s Notes

**[To be added]**

# Discussion

At RAN3-110e the following agreements were taken concerning the topic of Local NG-RAN Node ID for RRC Inactive:

**A standardized solution enabling an inter vendor interoperable way for an NG RAN node to deduce the identity of another NG RAN node from the received I-RNTI is needed**

**Agree on the benefits of a solution that allows at least some flexibility in the selection of the Local Node ID length; further details FFS**

**To be discussed as TEI17; we start only on this topic in RAN3 #111-e (Jan. 2021)**

**- The solution should be based on standardized multi-vendor interoperable signaling. The exact solution is FFS**

Based on past discussions, the following sections try to reach convergence on solution related aspects

## I-RNTI Formatting

In [2], [3], [4] solutions are proposed to fulfil the requirements agreed in RAN3-110e. On the other hand, in [1] there are no references to a specific solution apart to the one described in the informative Annex C of TS38.300.

However, the agreements taken in RAN3-110e confirmed that the solution described in the informative text of Annex C of TS38.300 is not sufficient and that:

**A standardized solution enabling an inter vendor interoperable way for an NG RAN node to deduce the identity of another NG RAN node from the received I-RNTI is needed**

The agreement mentions that the identity of an NG-RAN node needs to be deduced from the received I-RNTI.

In [2], [3], [4], the solutions proposed imply the inclusion of a local (short) NG-RAN node ID as part of the I-RNTI, which would allow the identification of an NG-RAN node locally.

**Companies are invited to state whether they are favourable to the inclusion of a short Local NG-RAN Node ID as part of the I-RNTI, which can serve the purpose of locally identifying the NG-RAN node that assigned the I-RNTI.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Ericsson | Yes | There are no standardized solutions on how to structure the I-RNTI and on how to deduce from it the identity of a neighbor NG-RAN node. This is at the source of the problem of interoperability and lack of flexibility for RRC Resume procedures. It is essential that a standardized solution is achieved, where a local identifier is included in the I-RNTI |
|  |  |  |

## Solution Flexibility

[2] and [4] present solutions that are based on the signaling of assistance information over the Xn interface between neighbor nodes, where such information help the NG-RAN nodes to derive the Local NG-RAN Node ID from an I-RNTI.

Solutions in [2] and [4] enable a flexible assignment of the maximum number of Inactive UE contexts per NG-RAN node by means of allowing each NG-RAN Node to adopt a different Local NG-RAN Node ID length and to signal it to neighbor nodes over Xn.

In [3] on the other end, a solution is proposed where the number of Inactive UE Contexts that an NG-RAN node can handle is fixed for all NG-RAN nodes. In this solution each node is configured with the length of the Local NG-RAN Node ID contained in the I-RNTI and each NG-RAN node knows that the Local NG-RAN Node ID is calculated as the “modulo(x)” operation (x is fixed) over the Global NG-RAN Node ID. Hence by fixing the Local NG-RAN Node ID length, the maximum number of RRC Inactive contexts per RAN node is also fixed.

**Companies are invited to express their view on whether the solution to be agreed by RAN3 shall allow for a flexible assignment of the maximum number of Inactive UE contexts per NG-RAN node or whether the maximum number of Inactive UE contexts per NG-RAN node should be fixed.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Flexible/Fixed** | **Comments** |
| Ericsson | Flexible | It is essential that the maximum number of Inactive UE Contexts per NG-RAN node is flexible. This is because different nodes will have different capacity and geographical coverage and for that they will serve different numbers of Inactive UEs |
|  |  |  |

## Configuration Based vs Signalling Based solutions

Solutions proposed in [2] and [4] are based on Xn signaling. These solutions minimize the need for configuration at the RAN because an NG-RAN node learns how to derive the Local NG-RAN node ID of a neighbor node by means of information (e.g. the neighbor node’s Local ID) received from neighbor nodes over Xn.

These solutions may be subject to Local NG-RAN Node ID conflicts, where two neighbor nodes assign the same Local NG-RAN Node ID. Resolution of such conflicts may require a new assignment of the Local NG-RAN Node ID and a new round of signaling to neighbor nodes.

The solution described in [3] is not based on the exchange of the Local NG-RAN Node ID via Xn. Instead, the solution derives the Local NG-RAN Node ID as the “modulo(x)” operation over the Global NG-RAN Node ID. In this solution conflicts are also possible. When a conflict occurs in the solution in [3] it is assumed that the Global NG-RAN Node ID of the node in conflict would need to be re-selected and re-configured at the NG-RAN node.

In [1] on the other hand, there are hints to a solution where conflicts shall not occur. This solution is only possible by means of centralized configuration of the Local NG-RAN Node ID at each NG-RAN node. Such centralized configuration shall happen across different RAN vendors’ and across different sharing operators’ domains. The advantage would be that there would not be Local NG-RAN Node ID conflicts. The disadvantage would be that a centralized configuration mechanism would need to be in place across sharing operators and, in order to achieve intervendor interoperability, across different RAN vendors. The latter would require standardization of the solution in SA5.

**Companies are invited to express their view on what type of solution shall RAN3 select in order to achieve flexible assignment of the Local NG-RAN Node ID length, inter vendor interoperability and interworking in RAN sharing scenarios.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Signalling Based/OAM Configuration Based** | **Comments** |
| Ericsson | Signalling Based | A solution based on Xn signalling is natively inter-vendor interoperable. Any updates to the signaled information happens automatically between RAN nodes, without the need of centralized configuration and therefore without the need for inter vendor/inter operator coordination. A solution based on OAM configuration needs detailed specification in SA5 to achieve inter vendor interoperability. However, it would not work in inter operator cases (RAN sharing) because inter operators OAM communication is not specified, hence it cannot be interoperable. Besides, in an OAM configuration based solution, any changes to the Local NG-RAN Node ID would need central coordination, which is usually time and resource consuming. |
|  |  |  |

# Conclusion, Recommendations

# References

[1] R3-210448, Discussion on NG-RAN node ID resolution from I-RNTI (Huawei)

[2] R3-210195, Discussion on I-RNTI partitioning (ZTE)

[3] R3-210422, Local NG-RAN node identifier (Nokia, Nokia Shanghai Bell)

[4] R3-210734, Node Identifier for RRC Inactive (Ericsson, AT&T, Verizon Wireless)