**3GPP TSG-RAN WG3 #111-e R3-211361**

**25 Jan ~ 05 Feb, 2021, E-Meeting**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **37.473** | **CR** | **0006** | **rev** | **1** | **Current version:** | **16.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR to 37.473 on miscellaneous corrections | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, China Unicomm, Orange, TIM | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | LTE\_NR\_arch\_evo-Core | | | | |  | ***Date:*** | | | 2021-01-25 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | There still remain some errors in the spec, which should be corrected, such as:   1. The IE type and reference of the IE *SIB type* in 9.3.1.33 is INTEGER (4,... 7, 9…15,,..32, ...), while the ASN.1 is INTEGER (2..32,...), they are not aligned. 2. The IE *Associated SCell List* is an extra IE which is actually not used. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * To correct the type and reference of the IE *SIB type* in 9.3.1.33 * To remove the IE *Associated SCell List* in 9.2.2.8 and 9.3.1.56   Impact Analysis:  Impact assessment towards the previous version of the specification (same release):  This CR has isolated functional impact with the previous version of the specification (same release).  The impact can be considered isolated because the change only affects the inactivity monitoing function. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | There are still some erros in the spec. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 9.2.2.8, 9.3.1.33, 9.3.1.56 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

<<<<<<<<<<<<<<<<<<<< Changes Begin >>>>>>>>>>>>>>>>>>>>

#### 9.2.2.8 UE CONTEXT MODIFICATION RESPONSE

This message is sent by the ng-eNB-DU to confirm the modification of a UE context.

Direction: ng-eNB-DU → ng-eNB-CU.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| ng-eNB-CU UE W1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| ng-eNB-DU UE W1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Resource Coordination Transfer Container | O |  | OCTET STRING | Includes the *MR-DC Resource Coordination Information* IE as defined in TS 38.423 [7] for NGEN-DC and NE-DC cases. | YES | ignore |
| DU To CU RRC Information | O |  | 9.3.1.58 |  | YES | reject |
| **DRB Setup List** |  | *0..1* |  | The List of DRBs which are successfully established. | YES | ignore |
| **>DRB Setup Item IEs** |  | *1 .. <maxnoofDRBs>* |  |  | EACH | ignore |
| >>DRB ID | M |  | 9.3.1.8 |  | - |  |
| >>DL UP TNL Information | M |  | UP Transport Layer Information  9.3.2.1 | ng-eNB-DU endpoint of the W1 transport bearer. For delivery of DL PDUs. | - |  |
| **DRB Modified List** |  | *0..1* |  | The List of DRBs which are successfully modified. | YES | ignore |
| **>DRB Modified Item IEs** |  | *1 .. <maxnoofDRBs>* |  |  | EACH | ignore |
| >>DRB ID | M |  | 9.3.1.8 |  | - |  |
| >>DL UP TNL Information | M |  | UP Transport Layer Information  9.3.2.1 | ng-eNB-DU endpoint of the W1 transport bearer. For delivery of DL PDUs. | - |  |
| >>RLC Status | O |  | 9.3.1.49 | Indicates the RLC has been re-established at the ng-eNB-DU. | YES | ignore |
| **SRB Failed to be Setup List** |  | *0..1* |  | The List of SRBs which are failed to be established. | YES | ignore |
| **>SRB Failed to be Setup Item IEs** |  | *1 .. <maxnoofSRBs>* |  |  | EACH | ignore |
| >>SRB ID | M |  | 9.3.1.7 |  | - |  |
| >>Cause | O |  | 9.3.1.2 |  | - |  |
| **DRB Failed to be Setup List** |  | *0..1* |  | The List of DRBs which are failed to be setup. | YES | ignore |
| **>DRB Failed to be Setup Item IEs** |  | *1 .. <maxnoofDRBs>* |  |  | EACH | ignore |
| >>DRB ID | M |  | 9.3.1.8 |  | - |  |
| >>Cause | O |  | 9.3.1.2 |  | - |  |
| **SCell Failed To Setup List** |  | *0..1* |  |  | YES | ignore |
| **>SCell Failed to Setup Item** |  | *1 .. <maxnoofSCells>* |  |  | EACH | ignore |
| >>SCell ID | M |  | E-UTRAN CGI  9.3.1.12 | SCell Identifier in ng-eNB | - |  |
| >>Cause | O |  | 9.3.1.2 |  | - |  |
| **DRB Failed to be Modified List** |  | 0..1 |  | The List of DRBs which are failed to be modified. | YES | ignore |
| **>DRB Failed to be Modified Item IEs** |  | *1 .. <maxnoofDRBs>* |  |  | EACH | ignore |
| >>DRB ID | M |  | 9.3.1.8 |  | - |  |
| >>Cause | O |  | 9.3.1.2 |  | - |  |
| Inactivity Monitoring Response | O |  | ENUMERATED (Not-supported, ...) |  | YES | reject |
| C-RNTI | O |  | 9.3.1.29 | C-RNTI allocated at the ng-eNB-DU | YES | ignore |
|  |  |  |  |  |  |  |
| **SRB Setup List** |  | *0..1* |  |  | YES | ignore |
| **>SRB Setup Item** |  | *1 .. <maxnoofSRBs>* |  |  | EACH | ignore |
| >>SRB ID | M |  | 9.3.1.7 |  | - |  |
| **SRB Modified List** |  | *0..1* |  |  | YES | ignore |
| **>SRB Modified Item** |  | *1 .. <maxnoofSRBs>* |  |  | EACH | ignore |
| >>SRB ID | M |  | 9.3.1.7 |  | - |  |

<<<<<<<<<<<<<<<<<<<< Next Changes Begin >>>>>>>>>>>>>>>>>>>>

#### 9.3.1.33 ng-eNB-CU System Information

This IE contains the system information encoded by the ng-eNB-CU.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** |
| **SIB type to Be Updated List** |  | *1* |  |  |
| **>SIB type to Be Updated Item IEs** |  | *1... <maxnoofSIBTypes>* |  |  |
| >>SIB type | M |  | INTEGER (2..32, ...) | Indicates a certain SIB block, e.g. 2 means sibType2, 3 for sibType3, etc. Values 2, 3, 8 and 16 are not applicable in this version of the specification. |
| >>SIB message | M |  | OCTET STRING | SIB message containing SIB as defined in TS 36.331 [1]. |
| >>Value Tag | M |  | INTEGER (0..31, ...) |  |

<<<<<<<<<<<<<<<<<<<< Next Changes Begin >>>>>>>>>>>>>>>>>>>>

#### 9.3.1.56 void







<<<<<<<<<<<<<<<<<<<< Next Changes Begin >>>>>>>>>>>>>>>>>>>>

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

Candidate-SpCell-Item,

Cause,

Cells-Failed-to-be-Activated-List-Item,

Cells-Status-Item,

Cells-to-be-Activated-List-Item,

Cells-to-be-Deactivated-List-Item,

C-RNTI,

CriticalityDiagnostics,

CUtoDURRCInformation,

DRB-Activity-Item,

DRBID,

DRBs-FailedToBeModified-Item,

DRBs-FailedToBeSetup-Item,

DRBs-FailedToBeSetupMod-Item,

DRB-Notify-Item,

DRBs-ModifiedConf-Item,

DRBs-Modified-Item,

DRBs-Required-ToBeModified-Item,

DRBs-Required-ToBeReleased-Item,

DRBs-Setup-Item,

DRBs-SetupMod-Item,

DRBs-ToBeModified-Item,

DRBs-ToBeReleased-Item,

DRBs-ToBeSetup-Item,

DRBs-ToBeSetupMod-Item,

DRXCycle,

DUtoCURRCInformation,

EUTRANQoS,

NGENB-CU-UE-W1AP-ID,

NGENB-DU-UE-W1AP-ID,

NGENB-DU-ID,

NGENB-DU-Served-Cells-Item,

NGENB-DU-System-Information,

InactivityMonitoringRequest,

InactivityMonitoringResponse,

NotificationControl,

EUTRANCGI,

EUTRANPCI,

Potential-SpCell-Item,

RAT-FrequencyPriorityInformation,

ResourceCoordinationTransferContainer,

RRCContainer,

RRCReconfigurationCompleteIndicator,

SCellIndex,

SCell-ToBeRemoved-Item,

SCell-ToBeSetup-Item,

SCell-ToBeSetupMod-Item,

SCell-FailedtoSetup-Item,

SCell-FailedtoSetupMod-Item,

ServCellIndex,

Served-Cell-Information,

Served-Cells-To-Add-Item,

Served-Cells-To-Delete-Item,

Served-Cells-To-Modify-Item,

SRBID,

SRBs-FailedToBeSetup-Item,

SRBs-FailedToBeSetupMod-Item,

SRBs-Required-ToBeReleased-Item,

SRBs-ToBeReleased-Item,

SRBs-ToBeSetup-Item,

SRBs-ToBeSetupMod-Item,

SRBs-Modified-Item,

SRBs-Setup-Item,

SRBs-SetupMod-Item,

TransactionID,

TransmissionActionIndicator,

DUtoCURRCContainer,

PagingCell-Item,

UEIdentityIndexValue,

UE-associatedLogicalW1-ConnectionItem,

PagingDRX,

PagingIdentity,

PWSSystemInformation,

Broadcast-To-Be-Cancelled-Item,

Cells-Broadcast-Cancelled-Item,

E-UTRAN-CGI-List-For-Restart-Item,

PWS-Failed-E-UTRAN-CGI-Item,

RepetitionPeriod,

NumberofBroadcastRequest,

Cells-To-Be-Broadcast-Item,

Cells-Broadcast-Completed-Item,

Cancel-all-Warning-Messages-Indicator,

NotificationInformation,

EUTRA-NR-CellResourceCoordinationReq-Container,

EUTRA-NR-CellResourceCoordinationReqAck-Container,

RequestType,

PLMN-Identity,

BitRate,

NGENBDUOverloadInformation,

ResourceCoordinationTransferInformation,

IgnoreResourceCoordinationRequestContainer

FROM W1AP-IEs

PrivateIE-Container{},

ProtocolExtensionContainer{},

ProtocolIE-Container{},

ProtocolIE-ContainerPair{},

ProtocolIE-SingleContainer{},

W1AP-PRIVATE-IES,

W1AP-PROTOCOL-EXTENSION,

W1AP-PROTOCOL-IES,

W1AP-PROTOCOL-IES-PAIR

FROM W1AP-Containers

id-Candidate-SpCell-List,

id-Cause,

id-Cancel-all-Warning-Messages-Indicator,

id-NotificationInformation,

id-Cells-Failed-to-be-Activated-List,

id-Cells-Status-List,

id-Cells-to-be-Activated-List,

id-Cells-to-be-Deactivated-List,

id-ConfirmedUEID,

id-C-RNTI,

id-CUtoDURRCInformation,

id-CriticalityDiagnostics,

id-DRB-Activity-List,

id-DRBs-FailedToBeModified-List,

id-DRBs-FailedToBeSetup-List,

id-DRBs-FailedToBeSetupMod-List,

id-DRBs-ModifiedConf-List,

id-DRBs-Modified-List,

id-DRB-Notify-List,

id-DRBs-Required-ToBeModified-List,

id-DRBs-Required-ToBeReleased-List,

id-DRBs-Setup-List,

id-DRBs-SetupMod-List,

id-DRBs-ToBeModified-List,

id-DRBs-ToBeReleased-List,

id-DRBs-ToBeSetup-List,

id-DRBs-ToBeSetupMod-List,

id-DRXCycle,

id-DUtoCURRCInformation,

id-ngeNB-CU-UE-W1AP-ID,

id-ngeNB-DU-UE-W1AP-ID,

id-ngeNB-DU-ID,

id-ngeNB-DU-Served-Cells-List,

id-InactivityMonitoringRequest,

id-InactivityMonitoringResponse,

id-oldngeNB-DU-UE-W1AP-ID,

id-Potential-SpCell-List,

id-RAT-FrequencyPriorityInformation,

id-ResetType,

id-ResourceCoordinationTransferContainer,

id-RRCContainer,

id-RRCReconfigurationCompleteIndicator,

id-SCell-FailedtoSetup-List,

id-SCell-FailedtoSetupMod-List,

id-SCell-ToBeRemoved-List,

id-SCell-ToBeSetup-List,

id-SCell-ToBeSetupMod-List,

id-Served-Cells-To-Add-List,

id-Served-Cells-To-Delete-List,

id-Served-Cells-To-Modify-List,

id-ServCellIndex,

id-SpCell-ID,

id-SRBID,

id-SRBs-FailedToBeSetup-List,

id-SRBs-FailedToBeSetupMod-List,

id-SRBs-Required-ToBeReleased-List,

id-SRBs-ToBeReleased-List,

id-SRBs-ToBeSetup-List,

id-SRBs-ToBeSetupMod-List,

id-SRBs-Modified-List,

id-SRBs-Setup-List,

id-SRBs-SetupMod-List,

id-TransactionID,

id-TransmissionActionIndicator,

id-UE-associatedLogicalW1-ConnectionListResAck,

id-DUtoCURRCContainer,

id-EUTRANCGI,

id-PagingCell-List,

id-PagingDRX,

id-UEIdentityIndexValue,

id-PagingIdentity,

id-PWSSystemInformation,

id-RepetitionPeriod,

id-NumberofBroadcastRequest,

id-Cells-To-Be-Broadcast-List,

id-Cells-Broadcast-Completed-List,

id-Broadcast-To-Be-Cancelled-List,

id-Cells-Broadcast-Cancelled-List,

id-E-UTRAN-CGI-List-For-Restart-List,

id-PWS-Failed-E-UTRAN-CGI-List,

id-EUTRA-NR-CellResourceCoordinationReq-Container,

id-EUTRA-NR-CellResourceCoordinationReqAck-Container,

id-RequestType,

id-ServingPLMN,

id-NGENB-DU-UE-AMBR-UL,

id-NGENBDUOverloadInformation,

id-ResourceCoordinationTransferInformation,

id-IgnoreResourceCoordinationRequestContainer,

maxCellinngeNBDU,

maxnoofCandidateSpCells,

maxnoofDRBs,

maxnoofErrors,

maxnoofIndividualW1ConnectionsToReset,

maxnoofPotentialSpCells,

maxnoofSCells,

maxnoofSRBs,

maxnoofPagingCells,

maxnoofTNLAssociations,

maxCellineNB,

maxnoofUEIDs

<<<<<<<<<<<<<<<<<<<< Next Changes Begin >>>>>>>>>>>>>>>>>>>>

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- UE CONTEXT MODIFICATION RESPONSE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

UEContextModificationResponse ::= SEQUENCE {

protocolIEs ProtocolIE-Container { { UEContextModificationResponseIEs} },

...

}

UEContextModificationResponseIEs W1AP-PROTOCOL-IES ::= {

{ ID id-ngeNB-CU-UE-W1AP-ID CRITICALITY reject TYPE NGENB-CU-UE-W1AP-ID PRESENCE mandatory }|

{ ID id-ngeNB-DU-UE-W1AP-ID CRITICALITY reject TYPE NGENB-DU-UE-W1AP-ID PRESENCE mandatory }|

{ ID id-ResourceCoordinationTransferContainer CRITICALITY ignore TYPE ResourceCoordinationTransferContainer PRESENCE optional }|

{ ID id-DUtoCURRCInformation CRITICALITY reject TYPE DUtoCURRCInformation PRESENCE optional}|

{ ID id-DRBs-SetupMod-List CRITICALITY ignore TYPE DRBs-SetupMod-List PRESENCE optional}|

{ ID id-DRBs-Modified-List CRITICALITY ignore TYPE DRBs-Modified-List PRESENCE optional}|

{ ID id-SRBs-FailedToBeSetupMod-List CRITICALITY ignore TYPE SRBs-FailedToBeSetupMod-List PRESENCE optional }|

{ ID id-DRBs-FailedToBeSetupMod-List CRITICALITY ignore TYPE DRBs-FailedToBeSetupMod-List PRESENCE optional }|

{ ID id-SCell-FailedtoSetupMod-List CRITICALITY ignore TYPE SCell-FailedtoSetupMod-List PRESENCE optional }|

{ ID id-DRBs-FailedToBeModified-List CRITICALITY ignore TYPE DRBs-FailedToBeModified-List PRESENCE optional }|

{ ID id-InactivityMonitoringResponse CRITICALITY reject TYPE InactivityMonitoringResponse PRESENCE optional }|

{ ID id-C-RNTI CRITICALITY ignore TYPE C-RNTI PRESENCE optional }|

{ ID id-SRBs-SetupMod-List CRITICALITY ignore TYPE SRBs-SetupMod-List PRESENCE optional }|

{ ID id-SRBs-Modified-List CRITICALITY ignore TYPE SRBs-Modified-List PRESENCE optional },

...

}

DRBs-SetupMod-List ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBs-SetupMod-Item

DRBs-Modified-List::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBs-Modified-Item

SRBs-SetupMod-List ::= SEQUENCE (SIZE(1..maxnoofSRBs)) OF SRBs-SetupMod-Item

SRBs-Modified-List ::= SEQUENCE (SIZE(1..maxnoofSRBs)) OF SRBs-Modified-Item

DRBs-FailedToBeModified-List ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBs-FailedToBeModified-Item

SRBs-FailedToBeSetupMod-List ::= SEQUENCE (SIZE(1..maxnoofSRBs)) OF SRBs-FailedToBeSetupMod-Item

DRBs-FailedToBeSetupMod-List ::= SEQUENCE (SIZE(1..maxnoofDRBs)) OF DRBs-FailedToBeSetupMod-Item

SCell-FailedtoSetupMod-List ::= SEQUENCE (SIZE(1..maxnoofSCells)) OF SCell-FailedtoSetupMod-Item

<<<<<<<<<<<<<<<<<<<< Next Changes Begin >>>>>>>>>>>>>>>>>>>>

-- A

AdditionalSIBMessageList ::= SEQUENCE (SIZE(1..maxnoofAdditionalSIBs)) OF AdditionalSIBMessageList-Item

AdditionalSIBMessageList-Item ::= SEQUENCE {

additionalSIB OCTET STRING,

iE-Extensions ProtocolExtensionContainer { { AdditionalSIBMessageList-Item-ExtIEs} } OPTIONAL

}

AdditionalSIBMessageList-Item-ExtIEs W1AP-PROTOCOL-EXTENSION ::= {

...

}

AllocationAndRetentionPriority ::= SEQUENCE {

priorityLevel PriorityLevel,

pre-emptionCapability Pre-emptionCapability,

pre-emptionVulnerability Pre-emptionVulnerability,

iE-Extensions ProtocolExtensionContainer { {AllocationAndRetentionPriority-ExtIEs} } OPTIONAL,

...

}

AllocationAndRetentionPriority-ExtIEs W1AP-PROTOCOL-EXTENSION ::= {

...

}

AvailablePLMNList ::= SEQUENCE (SIZE(1..maxnoofBPLMNs)) OF AvailablePLMNList-Item

<<<<<<<<<<<<<<<<<<<< Next part, for information against the change >>>>>>>>>>>>>>>>>>>>

SIB1-message ::= OCTET STRING

SIB2-message ::= OCTET STRING

SIB3-message ::= OCTET STRING

SIB8-message ::= OCTET STRING

SIB16-message ::= OCTET STRING

SibtypetobeupdatedListItem ::= SEQUENCE {

sIBtype INTEGER (2..32,...),

sIBmessage OCTET STRING,

valueTag INTEGER (0..31,...),

iE-Extensions ProtocolExtensionContainer { { SibtypetobeupdatedListItem-ExtIEs } } OPTIONAL,

...

}

SibtypetobeupdatedListItem-ExtIEs W1AP-PROTOCOL-EXTENSION ::= {

...

}

SliceSupportList ::= SEQUENCE (SIZE(1.. maxnoofSliceItems)) OF SliceSupportItem

SliceSupportItem ::= SEQUENCE {

sNSSAI SNSSAI,

iE-Extensions ProtocolExtensionContainer { { SliceSupportItem-ExtIEs } } OPTIONAL,

...

}

SliceSupportItem-ExtIEs W1AP-PROTOCOL-EXTENSION ::= {

...

}

<<<<<<<<<<<<<<<<<<<< Next Changes Begin >>>>>>>>>>>>>>>>>>>>

id-Cancel-all-Warning-Messages-Indicator ProtocolIE-ID ::= 79

id-NGENB-DU-UE-AMBR-UL ProtocolIE-ID ::= 80

id-ServingPLMN ProtocolIE-ID ::= 81

id-NGENBDUOverloadInformation ProtocolIE-ID ::= 82

id-ResourceCoordinationTransferInformation ProtocolIE-ID ::= 83

id-SRBs-Setup-List ProtocolIE-ID ::= 85

id-SRBs-SetupMod-List ProtocolIE-ID ::= 86

id-SRBs-Modified-List ProtocolIE-ID ::= 87

id-IgnoreResourceCoordinationRequestContainer ProtocolIE-ID ::= 88

id-NotificationInformation ProtocolIE-ID ::= 89

id-AdditionalSIBMessageList ProtocolIE-ID ::= 90

<<<<<<<<<<<<<<<<<<<< Changes End >>>>>>>>>>>>>>>>>>>>