**3GPP TSG-RAN WG3 Meeting #114-e R3-216145**

**E-meeting, 1-11 Nov 2021**

**Title:** (TP for SON BLCR for TS 38.423): TP on SCG RA report

**Source:** Huawei

**Agenda item:** 8.1

**Document Type:** Discussion

# 1. Introduction

This document contains the TP for SON BLCR for TS 38.423 to reflect the agreement achieved in the meeting.

# Annex – TP for SON BLCR for TS 38.423

<<<<<<<<<<<<<<<<<<<< Changes Begin >>>>>>>>>>>>>>>>>>>>

#### 9.1.3.25 ACCESS AND MOBILITY INDICATION

This message is sent by NG-RAN node1 to transfer access and mobility related information to NG-RAN node2.

Direction: NG-RAN node 1 → NG-RAN node 2.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | ignore |
| **RACH Report List** |  | *0..1* |  |  | YES | ignore |
| >RACH Report List Item |  | 1 .. <maxnoofRACHReports> |  |  | EACH | ignore |
| >>RACH Report Container | O |  | OCTET STRING | *RA-ReportList-r16* IE as defined in subclause 6.2.2 in TS 38.331 [10]. | YES | ignore |
| >>UE Assistant Identifier | O |  | NG-RAN node UE XnAP ID  9.2.3.16 |  | YES | ignore |
| **Successful HO Report List** |  | *0..1* |  |  | YES | ignore |
| >Successful HO Report List Item |  | 1 .. <maxnoofSuccessfulHOReports> |  |  | EACH | ignore |
| >> Successful HO Report Container | O |  | OCTET STRING | FFS on the definition | YES | ignore |