**3GPP TSG-RAN WG3 Meeting #114-e R3-21xxxx**

**E-meeting, 1-11 Nov 2021**

**Title:** (TP for SON BLCR for TS 38.423): TP on SCG RA report

**Source:** Huawei

**Agenda item:** 8.1

**Document Type:** Discussion

# 1. Introduction

This document contains the TP for SON BLCR for TS 38.423 to reflect the following agreement:

Each item within the RACH Report Information List should optionally contain an “UE Assistant Identifier”. This IE is not included if the MN is not sure whether the corresponding RA report is associated with the UE context currently used in the SN.

# Annex – TP for SON BLCR for TS 38.423

<<<<<<<<<<<<<<<<<<<< Changes Begin >>>>>>>>>>>>>>>>>>>>

#### 9.1.3.25 ACCESS AND MOBILITY INDICATION

This message is sent by NG-RAN node1 to transfer access and mobility related information to NG-RAN node2.

Direction: NG-RAN node 1 → NG-RAN node 2.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.3.1 |  | YES | ignore |
| **RACH Report List** |  | *0..1* |  |  | YES | ignore |
| >RACH Report List Item |  | 1 .. <maxnoofRACHReports> |  |  | EACH | ignore |
| >>RACH Report Container | O |  | OCTET STRING | *RA-ReportList-r16* IE as defined in subclause 6.2.2 in TS 38.331 [10]. | YES | ignore |
| >>UE Assistant Identifier | O |  | NG-RAN node UE XnAP ID9.2.3.16 |  | YES | ignore |
| **Successful HO Report List** |  | *0..1* |  |  | YES | ignore |
|  >Successful HO Report List Item |  | 1 .. <maxnoofSuccessfulHOReports> |  |  | EACH | ignore |
|  >> Successful HO Report Container | O |  | OCTET STRING | FFS on the definition | YES | ignore |