**3GPP TSG-RAN WG3 Meeting #114-e *R3-21xxxx***

**E-meeting, 1-11 Nov 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **36.423** | **CR** | **1645** | **rev** | **1** | **Current version:** | 16.7.0 |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Direct data forwarding for mobility between DC and SA | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, Samsung | | | | | | | | | |
| ***Source to TSG:*** | R3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | Direct\_data\_fw\_NR-Core | | | | |  | ***Date:*** | | | 2021-11-01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Last RAN3-113-e meeting further discussed the direct forwarding involving MR-DC with a set of agreements (see SoD in R3-214151).    This CR contains changes to support direct data forwarding for handover from SA to EN-DC | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | For inter-system handover from the SA to EN-DC,   * Introduce the *Source RAN Node ID* in the SGNB ADDITION REQUEST message, so that the SN can check the direct data forwarding path availability with the source node, and includes the *Direct Data Forwarding Path Availability* IE SGNB ADDITION REQUEST ACKNOWLEDGE message.   **Impact assessment towards the previous version of the specification (same release):**  This CR has an isolated impact towards the previous version of the specification (same release). This CR has an impact under functional point of view.  The impact can be considered isolated since it impacts the direct data forwarding for inter-system handover. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The direct data forwarding may not be supported for handovers from SA to EN-DC. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 8.7.4.2, 9.1.4.1, 9.1.4.2, 9.2.aaa, 9.3.4, 9.3.5, 9.3.7 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |
| --- |
| **Change Begins** |

### 8.7.4 SgNB Addition Preparation

#### 8.7.4.1 General

The purpose of the SgNB Addition Preparation procedure is to request the en-gNB to allocate resources for EN-DC connectivity operation for a specific UE.

The procedure uses UE-associated signalling.

#### 8.7.4.2 Successful Operation



Figure 8.7.4.2-1: SgNB Addition Preparation, successful operation

**<Unchanged Text Omitted>**

If the *UE Radio Capability ID* IE is contained in the SGNB ADDITION REQUEST message, the en-gNB shall, if supported, store this information and use it as specified in TS 23.401 [12].

If the SGNB ADDITION REQUEST message contains the *IAB Node Indication* IE, the en-gNB shall, if supported, consider that the request is for an IAB node.

For each requested E-RAB configured as MN-terminated split bearer/SCG bearer, if the *QoS Mapping Information* IE is contained in the *GTP Tunnel Endpoint* IE in the SGNB ADDITION REQUEST ACKNOWLEDGE message, the MeNB shall, if supported, use it to set DSCP and/or flow label fields for the downlink IP packets which are transmitted from MeNB to en-gNB through the GTP tunnels indicated by the *GTP Tunnel Endpoint* IE.

If the *Source NG-RAN Node ID* IE is included in the SGNB ADDITION REQUEST message, the en-gNB shall, if supported, use it to decide the direct data forwarding path availability with the indicated Source NG-RAN Node, and if the direct data forwarding path is available, include the *Direct Forwarding Path Availability* IE in the SGNB ADDITION REQUEST ACKNOWLEDGE message.

**<Unchanged Text Omitted>**

#### 9.1.4.1 SGNB ADDITION REQUEST

This message is sent by the MeNB to the en-gNB to request the preparation of resources for EN-DC operation for a specific UE

Direction: MeNB → en-gNB.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.13 |  | YES | reject |
| MeNB UE X2AP ID | M |  | eNB UE X2AP ID  9.2.24 | Allocated at the MeNB | YES | reject |
| NR UE Security Capabilities | M |  | 9.2.107 |  | YES | reject |
| SgNB Security Key | M |  | 9.2.101 | The S-KgNB which is provided by the MeNB, see TS 33.401 [18]. | YES | reject |
| SgNB UE Aggregate Maximum Bit Rate | M |  | UE Aggregate Maximum Bit Rate  9.2.12 | The UE Aggregate Maximum Bit Rate is split into MeNB UE Aggregate Maximum Bit Rate and SgNB UE Aggregate Maximum Bit Rate which are enforced by MeNB and en-gNB respectively. | YES | reject |
| Selected PLMN | O |  | PLMN Identity  9.2.4 | The selected PLMN of the SCG in the en-gNB. | YES | ignore |
| Handover Restriction List | O |  | 9.2.3 |  | YES | ignore |
| **E-RABs To Be Added List** |  | *1* |  |  | YES | reject |
| **>E-RABs To Be Added Item** |  | *1 .. <maxnoofBearers>* |  |  | EACH | reject |
| >>E-RAB ID | M |  | 9.2.23 |  | – |  |
| >>DRB ID | M |  | 9.2.122 |  | – |  |
| >>EN-DC Resource Configuration | M |  | EN-DC Resource Configuration 9.2.108 | Indicates the PDCP and Lower Layer MCG/SCG configuration. | – |  |
| >>CHOICE *Resource Configuration* | M |  |  |  |  |  |
| >>>*PDCP present in SN* |  |  |  | This choice tag is used if the *PDCP at SgNB* IE in the *EN-DC Resource Configuration* IE is set to the value "present". |  |  |
| >>>>Full E-RAB Level QoS Parameters | M |  | E-RAB Level QoS Parameters 9.2.9 | Includes the E-RAB level QoS parameters as received on S1-MME. | – |  |
| >>>>Maximum MCG admittable E-RAB Level QoS Parameters | C-ifMCGandSCGpresent\_GBR |  | GBR QoS Information 9.2.10 | Includes the GBR QoS Information admittable by the MCG. | – |  |
| >>>>DL Forwarding | O |  | 9.2.5 |  | – |  |
| >>>>MeNB DL GTP Tunnel Endpoint at MCG | C-ifMCGpresent |  | GTP Tunnel Endpoint 9.2.1 | MeNB endpoint of the X2-U transport bearer at MCG. For delivery of DL PDCP PDUs. | – |  |
| >>>>S1 UL GTP Tunnel Endpoint | M |  | GTP Tunnel Endpoint 9.2.1 | SGW endpoint of the S1-U transport bearer. For delivery of UL PDUs from the en-gNB. | – |  |
| >>>>RLC Mode | O |  | RLC Mode  9.2.119 | Indicates the RLC mode at the MeNB for PDCP transfer to en-gNB. | YES | ignore |
| >>>>Bearer Type | O |  | 9.2.92 |  | YES | ignore |
| >>>>Ethernet Type | O |  | 9.2.157 |  | YES | ignore |
| >>>*PDCP not present in SN* |  |  |  | This choice tag is used if the *PDCP at SgNB* IE in the *EN-DC Resource Configuration* IE is set to the value "not present". |  |  |
| >>>>Requested SCG E-RAB Level QoS Parameters | M |  | E-RAB Level QoS Parameters 9.2.9 | Includes E-RAB level QoS parameters requested to be provided by the SCG. | – |  |
| >>>>MeNB UL GTP Tunnel Endpoint at PDCP | M |  | GTP Tunnel Endpoint 9.2.1 | MeNB endpoint of the X2-U transport bearer. For delivery of UL PDCP PDUs. | – |  |
| >>>>Secondary MeNB UL GTP Tunnel Endpoint at PDCP | O |  | GTP Tunnel Endpoint 9.2.1 | MeNB endpoint of the X2-U transport bearer. For delivery of UL PDCP PDUs in case of PDCP duplication. | – |  |
| >>>>RLC Mode | M |  | RLC Mode  9.2.119 | Indicates the RLC mode to be used in the assisting node. | – |  |
| >>>>UL Configuration | C-ifMCGandSCGpresent |  | 9.2.118 | Information about UL usage in the en-gNB. | – |  |
| >>>>UL PDCP SN Length | O |  | PDCP SN Length  9.2.133 | Indicates the PDCP SN length of the bearer for the UL. | YES | ignore |
| >>>>DL PDCP SN Length | O |  | PDCP SN Length  9.2.133 | Indicates the PDCP SN length of the bearer for the DL. | YES | ignore |
| >>>>Duplication activation | O |  | 9.2.137 | Indicated the initial staus of PDCP duplication. | YES | ignore |
| MeNB to SgNB Container | M |  | OCTET STRING | Includes the *CG-ConfigInfo* message as defined in TS 38.331 [31]. | YES | reject |
| SgNB UE X2AP ID | O |  | en-gNB UE X2AP ID  9.2.100 | Allocated at the en-gNB. | YES | reject |
| Expected UE Behaviour | O |  | 9.2.70 |  | YES | ignore |
| MeNB UE X2AP ID Extension | O |  | Extended eNB UE X2AP ID  9.2.86 | Allocated at the MeNB. | YES | reject |
| Requested split SRBs | O |  | ENUMERATED (srb1, srb2, srb1&2, ...) | Indicates that resources for Split SRB are requested. | YES | reject |
| MeNB Resource Coordination Information | O |  | 9.2.116 | Information used to coordinate resources utilisation between MeNB and en-gNB. | YES | ignore |
| SGNB Addition Trigger Indication | O |  | ENUMERATED (SN change, inter-eNB HO, intra-eNB HO, ...) | This IE indicates the trigger for SGNB Addition procedure. | YES | reject |
| Subscriber Profile ID for RAT/Frequency priority | O |  | 9.2.25 |  | YES | ignore |
| MeNB Cell ID | M |  | ECGI  9.2.14 | Indicates the cell ID for PCell in MeNB. | YES | reject |
| Desired Activity Notification Level | O |  | 9.2.141 |  | YES | ignore |
| Trace Activation | O |  | 9.2.2 |  | YES | ignore |
| Location Information at SgNB reporting | O |  | ENUMERATED (pscell, ...) | Indicates that the user’s location information is to be provided. | YES | ignore |
| Masked IMEISV | O |  | 9.2.69 |  | YES | ignore |
| Additional RRM Policy Index | O |  | 9.2.25a |  | YES | ignore |
| Requested Fast MCG recovery via SRB3 | O |  | ENUMERATED (true, ...) | Indicates that the resources for fast MCG recovery via SRB3 are requested. | YES | ignore |
| UE Context Reference at Source NG-RAN | O |  | RAN UE NGAP ID 9.2.152 |  | YES | ignore |
| Management Based MDT Allowed | O |  | 9.2.59 |  | YES | ignore |
| Management Based MDT PLMN List | O |  | MDT PLMN List  9.2.64 |  | YES | ignore |
| UE Radio Capability ID | O |  | 9.2.171 |  | YES | reject |
| IAB Node Indication | O |  | ENUMERATED (true, ...) |  | YES | Reject |
| Source NG-RAN Node ID | O |  | Global RAN Node ID  9.2.aaa |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofBearers | Maximum no. of E-RABs. Value is 256. |

|  |  |
| --- | --- |
| Condition | Explanation |
| ifMCGandSCGpresent | This IE shall be present if, for the E-RAB requested to be added, the *MCG resources* and *SCG resources* IEs in the *EN-DC Resource Configuration* IE are set to the value "present". |
| ifMCGpresent | This IE shall be present if, for the E-RAB requested to be added, the *MCG resources* IE in the *EN-DC Resource Configuration* IE is set to the value "present". |
| C-ifMCGandSCGpresent\_GBR | This IE shall be present if, for the E-RAB requested to be added, the *MCG resources* and *SCG resources* IEs in the *EN-DC Resource Configuration* IE are set to the value "present", and *GBR QoS Information* IE is present in *Full E-RAB Level QoS Parameters* IE. |

#### 9.1.4.2 SGNB ADDITION REQUEST ACKNOWLEDGE

This message is sent by the en-gNB to confirm the MeNB about the SgNB addition preparation.

Direction: en-gNB → MeNB.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.2.13 |  | YES | reject |
| MeNB UE X2AP ID | M |  | eNB UE X2AP ID  9.2.24 | Allocated at the MeNB. | YES | reject |
| SgNB UE X2AP ID | M |  | en-gNB UE X2AP ID  9.2.100 | Allocated at the en-gNB. | YES | reject |
| **E-RABs Admitted To Be Added List** |  | *1* |  |  | YES | ignore |
| **>E-RABs Admitted To Be Added Item** |  | *1 .. <maxnoofBearers>* |  |  | EACH | ignore |
| >>E-RAB ID | M |  | 9.2.23 |  | – |  |
| >>EN-DC Resource Configuration | M |  | EN-DC Resource Configuration 9.2.108 | Indicates the PDCP and Lower Layer MCG/SCG configuration. | – |  |
| >>CHOICE *Resource Configuration* | M |  |  |  |  |  |
| *>>>PDCP present in SN* |  |  |  | This choice tag is used if the *PDCP at SgNB* IE in the *EN-DC Resource Configuration* IE is set to the value "present". |  |  |
| >>>>S1 DL GTP Tunnel Endpoint at the SgNB | M |  | GTP Tunnel Endpoint 9.2.1 | en-gNB endpoint of the S1 transport bearer. For delivery of DL PDUs. | – |  |
| >>>>SgNB UL GTP Tunnel Endpoint at PDCP | C-ifMCGpresent |  | GTP Tunnel Endpoint 9.2.1 | en-gNB endpoint of the X2-U transport bearer at PDCP. For delivery of UL PDCP PDUs. | – |  |
| >>>>RLC Mode | C-ifMCGpresent |  | RLC Mode  9.2.119 | Indicates the RLC mode. | – |  |
| >>>>DL Forwarding GTP Tunnel Endpoint | O |  | GTP Tunnel Endpoint 9.2.1 | Identifies the X2 transport bearer used for forwarding of DL PDUs | – |  |
| >>>>UL Forwarding GTP Tunnel Endpoint | O |  | GTP Tunnel Endpoint 9.2.1 | Identifies the X2 transport bearer used for forwarding of UL PDUs | – |  |
| >>>>Requested MCG E-RAB Level QoS Parameters | C-ifMCGandSCGpresent\_GBRpresent |  | E-RAB Level QoS Parameters 9.2.9 | Includes E-RAB level QoS parameters requested to be provided by the MCG. | – |  |
| >>>>UL Configuration | C-ifMCGandSCGpresent |  | 9.2.118 | Information about UL usage in the MeNB. | – |  |
| >>>>UL PDCP SN Length | O |  | PDCP SN Length  9.2.133 | Indicates the PDCP SN length of the bearer for the UL. | YES | ignore |
| >>>>DL PDCP SN Length | O |  | PDCP SN Length  9.2.133 | Indicates the PDCP SN length of the bearer for the DL. | YES | ignore |
| >>>*PDCP not present in SN* |  |  |  | This choice tag is used if the *PDCP at SgNB* IE in the *EN-DC Resource Configuration* IE is set to the value "not present". |  |  |
| >>>>SgNB DL GTP Tunnel Endpoint at SCG | M |  | GTP Tunnel Endpoint 9.2.1 | SgNB endpoint of the X2-U transport bearer at the SCG. For delivery of DL PDCP PDUs. | – |  |
| >>>>Secondary SgNB DL GTP Tunnel Endpoint at SCG | O |  | GTP Tunnel Endpoint 9.2.1 | SgNB endpoint of the X2-U transport bearer at the SCG. For delivery of DL PDCP PDUs in case of PDCP duplication | – |  |
| >>>>LCID | O |  | 9.2.138 | LCID for the primary path in case of PDCP duplication | YES | ignore |
| E-RABs Not Admitted List | O |  | E-RAB List  9.2.28 | A value for *E-RAB ID* shall only be present once in*E-RABs Admitted**List* IE and in *E-RABs Not Admitted List* IE. | YES | ignore |
| SgNB to MeNB Container | M |  | OCTET STRING | Includes the *CG-Config* message as defined in TS 38.331[31]. | YES | reject |
| Criticality Diagnostics | O |  | 9.2.7 |  | YES | ignore |
| MeNB UE X2AP ID Extension | O |  | Extended eNB UE X2AP ID  9.2.86 | Allocated at the MeNB | YES | reject |
| Admitted split SRBs | O |  | ENUMERATED (srb1, srb2, srb1&2, ...) | Indicates admitted SRBs | YES | reject |
| SgNB Resource Coordination Information | O |  | 9.2.117 | Information used to coordinate resources utilisation between en-gNB and MeNB. | YES | ignore |
| RRC config indication | O |  | 9.2.132 | Indicates the type of RRC configuration used at the en-gNB. | YES | reject |
| Location Information at SgNB | O |  | 9.2.142 | Contains information to support localisation of the UE | YES | ignore |
| Available fast MCG recovery via SRB3 | O |  | ENUMERATED (true, ...) | Indicates the fast MCG recovery via SRB3 is enabled. | YES | Ignore |
| Direct Forwarding Path Availability | O |  | ENUMERATED (direct path available, …) | Indicates direct forwarding path is available between the en-gNB and source RAN node for inter-system handover. | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofBearers | Maximum no. of E-RABs. Value is 256 |

|  |  |
| --- | --- |
| Condition | Explanation |
| ifMCGpresent | This IE shall be present if, for the E-RAB admitted to be added, the *MCG resources* IE in the *EN-DC Resource Configuration* IE is set to the value "present". |
| ifMCGandSCGpresent | This IE shall be present if, for the E-RAB admitted to be added, the *MCG resources* and *SCG resources* IEs in the *EN-DC Resource Configuration* IE are set to the value "present". |
| C-ifMCGandSCGpresent\_GBRpresent | This IE shall be present if, for the E-RAB admitted to be added, the *MCG resources* and *SCG resources* IEs in the *EN-DC Resource Configuration* IE are set to the value "present", and the *GBR QoS Information* IE is present in the *Requested MCG E-RAB Level QoS Parameters* IE. |

**<Unchanged Text Omitted>**

#### 9.2.aaa Global RAN Node ID

This IE is used to globally identify an NG-RAN node.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| CHOICE *NG-RAN node* | M |  |  |  |
| *>gNB* |  |  |  |  |
| >>Global gNB ID | M |  | Global en-gNB ID  9.2.112 |  |

### 9.3.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for X2AP.

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**<Unchanged Text Omitted>**

UERadioCapability,

SFN-Offset,

IMSvoiceEPSfallbackfrom5G,

Global-RAN-NODE-ID

**<Unchanged Text Omitted>**

id-IntendedTDD-DL-ULConfiguration-NR,

id-UERadioCapability,

id-SFN-Offset,

id-DirectForwardingPathAvailability,

id-sourceNG-RAN-node,

**<Unchanged Text Omitted>**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- SGNB ADDITION REQUEST

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SgNBAdditionRequest ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{SgNBAdditionRequest-IEs}},

...

}

SgNBAdditionRequest-IEs X2AP-PROTOCOL-IES ::= {

{ ID id-MeNB-UE-X2AP-ID CRITICALITY reject TYPE UE-X2AP-ID PRESENCE mandatory}|

{ ID id-NRUESecurityCapabilities CRITICALITY reject TYPE NRUESecurityCapabilities PRESENCE mandatory}|

{ ID id-SgNBSecurityKey CRITICALITY reject TYPE SgNBSecurityKey PRESENCE mandatory}|

{ ID id-SgNBUEAggregateMaximumBitRate CRITICALITY reject TYPE UEAggregateMaximumBitRate PRESENCE mandatory}|

{ ID id-SelectedPLMN CRITICALITY ignore TYPE PLMN-Identity PRESENCE optional}|

{ ID id-HandoverRestrictionList CRITICALITY ignore TYPE HandoverRestrictionList PRESENCE optional}|

{ ID id-E-RABs-ToBeAdded-SgNBAddReqList CRITICALITY reject TYPE E-RABs-ToBeAdded-SgNBAddReqList PRESENCE mandatory}|

{ ID id-MeNBtoSgNBContainer CRITICALITY reject TYPE MeNBtoSgNBContainer PRESENCE mandatory}|

{ ID id-SgNB-UE-X2AP-ID CRITICALITY reject TYPE SgNB-UE-X2AP-ID PRESENCE optional}|

{ ID id-ExpectedUEBehaviour CRITICALITY ignore TYPE ExpectedUEBehaviour PRESENCE optional}|

{ ID id-MeNB-UE-X2AP-ID-Extension CRITICALITY reject TYPE UE-X2AP-ID-Extension PRESENCE optional}|

{ ID id-RequestedSplitSRBs CRITICALITY reject TYPE SplitSRBs PRESENCE optional}|

{ ID id-MeNBResourceCoordinationInformation CRITICALITY ignore TYPE MeNBResourceCoordinationInformation PRESENCE optional}|

{ ID id-SGNB-Addition-Trigger-Ind CRITICALITY reject TYPE SGNB-Addition-Trigger-Ind PRESENCE optional}|

{ ID id-SubscriberProfileIDforRFP CRITICALITY ignore TYPE SubscriberProfileIDforRFP PRESENCE optional}|

{ ID id-MeNBCell-ID CRITICALITY reject TYPE ECGI PRESENCE mandatory}|

{ ID id-DesiredActNotificationLevel CRITICALITY ignore TYPE DesiredActNotificationLevel PRESENCE optional}|

{ ID id-TraceActivation CRITICALITY ignore TYPE TraceActivation PRESENCE optional}|

{ ID id-LocationInformationSgNBReporting CRITICALITY ignore TYPE LocationInformationSgNBReporting PRESENCE optional}|

{ ID id-Masked-IMEISV CRITICALITY ignore TYPE Masked-IMEISV PRESENCE optional}|

{ ID id-AdditionalRRMPriorityIndex CRITICALITY ignore TYPE AdditionalRRMPriorityIndex PRESENCE optional}|

{ ID id-RequestedFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE RequestedFastMCGRecoveryViaSRB3 PRESENCE optional}|

{ ID id-UEContextReferenceatSourceNGRAN CRITICALITY ignore TYPE RAN-UE-NGAP-ID PRESENCE optional}|

{ ID id-ManagementBasedMDTallowed CRITICALITY ignore TYPE ManagementBasedMDTallowed PRESENCE optional }|

{ ID id-ManagementBasedMDTPLMNList CRITICALITY ignore TYPE MDTPLMNList PRESENCE optional }|

{ ID id-UERadioCapabilityID CRITICALITY reject TYPE UERadioCapabilityID PRESENCE optional}|

{ ID id-IABNodeIndication CRITICALITY reject TYPE IABNodeIndication PRESENCE optional}|

{ ID id-sourceNG-RAN-node-id CRITICALITY ignore TYPE Global-RAN-NODE-ID PRESENCE optional}, ...

}

**<Unchanged Text Omitted>**

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- SGNB ADDITION REQUEST ACKNOWLEDGE

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

SgNBAdditionRequestAcknowledge ::= SEQUENCE {

protocolIEs ProtocolIE-Container {{SgNBAdditionRequestAcknowledge-IEs}},

...

}

SgNBAdditionRequestAcknowledge-IEs X2AP-PROTOCOL-IES ::= {

{ ID id-MeNB-UE-X2AP-ID CRITICALITY reject TYPE UE-X2AP-ID PRESENCE mandatory}|

{ ID id-SgNB-UE-X2AP-ID CRITICALITY reject TYPE SgNB-UE-X2AP-ID PRESENCE mandatory}|

{ ID id-E-RABs-Admitted-ToBeAdded-SgNBAddReqAckList CRITICALITY ignore TYPE E-RABs-Admitted-ToBeAdded-SgNBAddReqAckList PRESENCE mandatory}|

{ ID id-E-RABs-NotAdmitted-List CRITICALITY ignore TYPE E-RAB-List PRESENCE optional}|

{ ID id-SgNBtoMeNBContainer CRITICALITY reject TYPE SgNBtoMeNBContainer PRESENCE mandatory}|

{ ID id-CriticalityDiagnostics CRITICALITY ignore TYPE CriticalityDiagnostics PRESENCE optional}|

{ ID id-MeNB-UE-X2AP-ID-Extension CRITICALITY reject TYPE UE-X2AP-ID-Extension PRESENCE optional}|

{ ID id-AdmittedSplitSRBs CRITICALITY reject TYPE SplitSRBs PRESENCE optional}|

{ ID id-SgNBResourceCoordinationInformation CRITICALITY ignore TYPE SgNBResourceCoordinationInformation PRESENCE optional}|

{ ID id-RRCConfigIndication CRITICALITY reject TYPE RRC-Config-Ind PRESENCE optional}|

{ ID id-LocationInformationSgNB CRITICALITY ignore TYPE LocationInformationSgNB PRESENCE optional}|

{ ID id-AvailableFastMCGRecoveryViaSRB3 CRITICALITY ignore TYPE AvailableFastMCGRecoveryViaSRB3 PRESENCE optional }|

{ ID id-DirectForwardingPathAvailability CRITICALITY ignore TYPE DirectForwardingPathAvailability PRESENCE optional },

...

}

**<Unchanged Text Omitted>**

DirectForwardingPathAvailability ::= ENUMERATED {direct-path-available, ...}

### 9.3.5 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**<Unchanged Text Omitted>**

Global-RAN-NODE-ID ::= CHOICE {

gNB GlobalGNB-ID,

choice-extension ProtocolIE-Single-Container { { Global-RAN-NODE-ID-ExtIEs} }

}

Global-RAN-NODE-ID-ExtIEs X2AP-PROTOCOL-IES ::= {

...

}

**<Unchanged Text Omitted>**

### 9.3.7 Constant definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-CHO-DC-EarlyDataForwarding ProtocolIE-ID ::= 407

id-IMSvoiceEPSfallbackfrom5G ProtocolIE-ID ::= 408

id-DirectForwardingPathAvailability ProtocolIE-ID ::= aaa

id-sourceNG-RAN-node-id ProtocolIE-ID ::= bbb

|  |
| --- |
| **Change Ends** |