**3GPP TSG-RAN WG3 #114bis-e R3-22xxxx**

**17-26 Jan 2022 Online**

**Title:** **TP to TS38.463 on the support of SDT in E1 interface**

**Source: China telecom**

**Agenda item: 24.4**

**Document for:** **Discussion and Decision**

////////////////////////////////////////////////////////////////////////start of change////////////////////////////////////////////////////////////////////////

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply.   
An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

5GC 5G Core Network

5QI 5G QoS Identifier

CAG Closed Access Group

CGI Cell Global Identifier

CHO Conditional Handover

CN Core Network

CP Control Plane

CPC Conditional PSCell Change

DAPS Dual Active Protocol Stack

DL Downlink

EHC Ethernet Header Compression

EN-DC E-UTRA-NR Dual Connectivity

EPC Evolved Packet Core

IAB Integrated Access and Backhaul

MCG Master Cell Group

NID Network Identifier

NPN Non-Public Network

PNI-NPN Public Network Integrated Non-Public Network

NSSAI Network Slice Selection Assistance Information

RANAC RAN Area Code

SCG Secondary Cell Group

SDAP Service Data Adaptation Protocol

SDT Small Data Transmisson

SNPN Stand-alone Non-Public Network

S-NSSAI Single Network Slice Selection Assistance Information

TNLA Transport Network Layer Association

////////////////////////////////////////////////////////////////////////skip unchanged////////////////////////////////////////////////////////////////////////

#### 9.2.2.4 BEARER CONTEXT MODIFICATION REQUEST

This message is sent by the gNB-CU-CP to request the gNB-CU-UP to modify a bearer context.

Direction: gNB-CU-CP → gNB-CU-UP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **IE/Group Name** | **Presence** | **Range** | **IE type and reference** | **Semantics description** | **Criticality** | **Assigned Criticality** |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Security Information | O |  | 9.3.1.10 |  | YES | reject |
| UE DL Aggregate Maximum Bit Rate | O |  | Bit Rate 9.3.1.20 |  | YES | reject |
| UE DL Maximum Integrity Protected Data Rate | O |  | Bit Rate 9.3.1.20 | The Bit Rate is a portion of the UE’s Maximum Integrity Protected Data Rate, and is enforced by the gNB-CU-UP node. | YES | reject |
| Bearer Context Status Change | O |  | ENUMERATED (Suspend, Resume, …,Resumefor SDT) | Indicates the status of the Bearer Context, and Resumefor SDT indicates all the SDT bearers need to be resumed. | YES | reject |
| New UL TNL Information Required | O |  | ENUMERATED (required, …) | Indicates that new UL TNL information has been requested to be provided. | YES | reject |
| UE Inactivity Timer | O |  | Inactivity Timer  9.3.1.54 | Included if the Activity Notification Level is set to UE. | - | - |
| Data Discard Required | O |  | ENUMERATED (required, …) | Indicate to discard the DL user data in case of RAN paging failure. | YES | ignore |
| CHOICE *System* | O |  |  |  | YES | reject |
| *>E-UTRAN* |  |  |  |  |  |  |
| >>DRB To Setup List | O |  | DRB To Setup Modification List E-UTRAN  9.3.3.7 |  | YES | reject |
| >>DRB To Modify List | O |  | DRB To Modify List E-UTRAN  9.3.3.8 |  | YES | reject |
| >>DRB To Remove List | O |  | DRB To Remove List E-UTRAN  9.3.3.9 |  | YES | reject |
| >>Subscriber Profile ID for RAT/Frequency priority | O |  | 9.3.1.69 |  | YES | ignore |
| >>Additional RRM Policy Index | O |  | 9.3.1.70 |  | YES | ignore |
| *>NG-RAN* |  |  |  |  |  |  |
| >>PDU Session Resource To Setup List | O |  | PDU Session Resource To Setup Modification List  9.3.3.10 |  | YES | reject |
| >>PDU Session Resource To Modify List | O |  | 9.3.3.11 |  | YES | reject |
| >>PDU Session Resource To Remove List | O |  | 9.3.3.12 |  | YES | reject |
| RAN UE ID | O |  | OCTET STRING (SIZE(8)) |  | YES | ignore |
| gNB-DU ID | O |  | 9.3.1.65 |  | YES | ignore |
| Activity Notification Level | O |  | 9.3.1.67 |  | YES | ignore |

|  |  |
| --- | --- |
| **Range bound** | **Explanation** |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource | Maximum no. of PDU Sessions for a UE. Value is 256. |

////////////////////////////////////////////////////////////////////////skip unchanged////////////////////////////////////////////////////////////////////////

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

////////////////////////////////////////////////////////////////////////skip unchanged////////////////////////////////////////////////////////////////////////

-- B

BearerContextStatusChange ::= ENUMERATED {

suspend,

resume,

...

resumeforSDT

}

BitRate ::= INTEGER (0..4000000000000,...)

////////////////////////////////////////////////////////////////////////end of change////////////////////////////////////////////////////////////////////////