3GPP TSG-RAN WG3 #116-e R3-223691

Online, 9th - 19th May 2022

Agenda Item: 9.1.6.1.1

Source: Ericsson(moderator)

Title: CB: # MBS2\_Service\_Continuity - Summary of email discussion

Document for: Discussion

# Introduction

chair summary:

**CB: # MBS2\_Service\_Continuity**

**- FFS on "Consent to Apply Available Shared UP MBS QoS flow mapping", the related E1AP procedure on how the consent works?**

- affected spec: E1AP, 38401

- R3-223672 (ZTE) / R3-223282 R3-223283 R3-223284 (SS) / R3-223627 R3-223628 R3-223629 (HW)/ R3-223456 (Nokia)

**- Whether and how Rel-17 should support the possibility to modify both, RAN and CN side terminations of the shared NG-U bearer?**

- affected spec: NG-C

- R3-223379 (Ericsson)

**- Whether Data Forwarding Response MRB List IE within the MBS Session Information Response Target to Source List as an optional IE?**

- affected spec: XnAP

- R3-223379 Ericsson

**- Whether to have end marker from 5GC at handover from supporting to non-supporting node?**

- affected spec: 38300

- R3-223452 (Nokia)

**- How to apply data forwarding from supporting to non-supporting node?**

- affected spec: 38300

- R3-223604 (ZTE)

**- FFS whether to add an indication of which MBS session is active?**

- affected spec: 413/423

- R3-223077 R3-223078 HW / R3-223631QC / R3-223185 R3-223187 R3-223188 (NEC) / R3-223379 Ericsson

**- MBS Session Status indication in NGAP/XnAP?**

- affected spec: XnAP, NGAP

- R3-223185 R3-223187 R3-223188 (NEC),

**- Clean-up work on following specif found needed**

- 38401 38410 38420 38460 38470

- ref tdoc: R3-223096 (QC) etc.

**- LS out if needed (e.g., to RAN2/SA2)**

**- Capture agreements and provide CRs if agreeable, split work**

(E/// - moderator)

Summary of offline disc R3-223691

# For the Chairman’s Notes

to be added

# Discussion first round

## Whether to specify data forwarding from supporting to non-supporting gNB

This is related to R3-223604.

The moderator believes that actually proposes to not specify data forwarding down to all details in Rel-17. Those "details" especially encompass the specification of how to stop data forwarding.

Also the intention to provide clear statements to other TSGs/WGs, as outlined in the coversheet, if taken seriously, would need clarifications on statements regarding switch from MRB and DRB before HO.

The moderator suggests the following approach:

<<<<<<<<<<<<<<<<<<<< Begin of Changes >>>>>>>>>>>>>>>>>>>>

##### 16.10.5.3.3 Handover between Multicast supporting cell and Multicast non-supporting cell

During an active multicast MBS session, at mobility from an MBS-supporting NG-RAN node to an MBS non-supporting NG-RAN node, the target NG-RAN node sets up PDU Session Resources mapped to the multicast MBS Session. The 5GC infers from the absence of an "MBS-support" indication in the Path Switch Request message (Xn handover) or Handover Request Acknowledge message (NG handover) that MBS data packets delivery has to be switched to 5GC individual MBS traffic delivery as specified in TS 23.247 [45]. If data forwarding is applied, the source NG-RAN changes the QFI(s) in the forwarded packets to the associated unicast QFI(s) if respective mapping information is available.

NOTE 1: Further details for data forwarding are not specified and left to implementation.

NOTE 2: The source NG-RAN node may be aware that the target NG-RAN node is non-MBS supporting already before Handover Preparation.

<<<<<<<<<<<<<<<<<<<< Unmodified Text Omitted >>>>>>>>>>>>>>>>>>>>

NOTE 3: Mobility from a multicast supporting cell to a multicast non-supporting cell may be performed by switching the MRB configuration to a DRB configuration in the source gNB before handover. Details are left to implementation.

NOTE 4: A UE may be handed over to a target gNB not-supporting MBS without prior reconfiguration from MRB to the DRB in the source gNB. In this case, the AS configuration may not be comprehended by the target gNB causing full configuration.

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

Please provide your view whether and why you would prefer or not prefer such approach.

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | The moderator did his best to modify the existing text to accommodate the intention of the author of R3-223604. The moderator is also aware of the interrelation of NOTE 1 to the next topic. |
|  |  |
|  |  |

## End marker handling for mobility from supporting to non-supporting RAN node

This is related to R3-223452.

The draft CR in [x1] foresees a scheme where the end-marker that should stop forwarding of MBS data is provided outside the tunnels that deliver/forward the MBS data. Part of it is the assumption that SN/QFI information received within the end-marker at the (supporting source gNB's) UP entity serving the associated PDU Session tunnel is communicated to the (supporting source gNB's) UP entity serving the MBS session tunnel.

Please provide your view whether and why you would prefer or not prefer such approach.

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | The moderator's company would like to keep the 2 principles: 1) end-markers to indicate the end of a data stream are delivered within the tunnel where the data stream is provided. 2) interaction between 2 different UP entities in the gNB are not assumed and not specified.  The proposal does not seem to follow those principles. |
|  |  |
|  |  |

## Indication of MC MBS Session Status in XnAP and NGAP

### Check Common Understanding of the intended approach

The moderator would like to confirm with companies whether the following approach was intended for Xn/NG based mobility:

1. independent of the MBS Session state, the MBS Session IDs and, if inhomogeneous MBMS deployment needs to be supported, Associated QoS Information is provided to the target NG-RAN node.
2. Only if the MBS Session is active,   
   - on NG, the *Source NG-RAN Node to Target NG-RAN Node Transparent Container* IE  
   - on Xn, the *UE Context Information* IE   
   carries MBS Session information, so that a supporting NG-RAN node can immediately allocate MBS Session resources if the UE is the first to enter the target NG-RAN node for that MBS Session.

Please provide your view whether and why you would confirm the outlined common understand or why not.

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | The moderator believes that the above are the principles which were intended and agreed to be realized in TS work. This approach would follow the principle that session information is only provided on Xn/NG at HO if session resources are allocated at the source side. |
|  |  |
|  |  |

### Implications of the outlined "Common Understanding"

If the "common understanding" outlined in 3.3.1 can be confirmed, then there are two implications:

1. On both, Xn and NG, the information how to immediately allocate MBS Session Resources is not needed, if the MC MBS Session is deactivated. This is possible to be achieved on NG by not including the *MBS Session Information Source to Target List* IE within the Source *NG-RAN Node to Target NG-RAN Node Transparent Container*, on Xn, it seems that the mandatory presence of the *MBS QoS Flows to Add List* IE in the *MBS Session Information List* IE needs to be changed to optional.
2. The presence/absence of the information how to immediately allocate MBS Session Resources could serve as an indication on whether the session is active/deactivated. Nevertheless, there could be still a "status IE" included, if the moderator has overlooked a further reason why this is needed.

The moderator proposes

1. to change in XnAP the presence of the *MBS QoS Flows to Add List* IE in the *MBS Session Information List* IE needs to optional and
2. specify the presence/absence
   1. on NG, of the *MBS Session Information Source to Target List* IE within the Source *NG-RAN Node to Target NG-RAN Node Transparent Container*,
   2. on Xn, of the *MBS QoS Flows to Add List* IE in the *MBS Session Information List* IE

as an indication of the MC MBS Session Status (active/deactived).

1. to further discuss whether an explicit "session status IE" is necessary

Please provide your view whether and why you would support the outlined proposal or why not.

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | We would see the principles outlined in the "common understanding" very well captured in points a) and b) and are open to discuss any additional reason why an explicit session status is necessary or maybe beneficial from a message processing perspective. |
|  |  |
|  |  |

## E1: how to enable the gNB to adopt an "Available Shared UP MBS QoS flow mapping"

There are 3 different approaches outlined in the submitted papers:

1. network implementation/configuration, i.e. remove current possibilities available on E1AP
2. CU-CP provides its consent to any "available shared UP MBS QoS flow mapping"
3. CU-CP is enabled to request any already existing "available share UP MBS QoS flow mapping" at setup and modification and subsequently adopt to it in an additional step.

The moderator proposes to enable all 3 possibilities

The moderator would expect that the "network implementation" approach would not need any explicit specification work, while the other approaches would complement each other and should be allowed to exist concurrently.

Please provide your view whether and why you would agree on the moderator's proposal or why not.

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | The moderator believes that above approach would represent a nice compromise reflecting the different approaches the various companies have in mind. We believe that approach 2 and 3 have their merit in being realized (3 seems to require more steps as 2, but should not be precluded). Approach 1, i.e. preconfiguration instead of signalling is always possible for any optional feature. |
|  |  |
|  |  |

## Whether and how Rel-17 should support the possibility to modify moth, RAN and CN side terminations of the shared NG-U bearer for BC and MC

R3-223379 proposes to discuss whether Rel-17 specifications should foresee the possibility to modify RAN and CN side terminations for both BC and MC.

Please provide your view and reasoning.

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | As outlined in R3-223379 we believe that these possibilities are really missing and would appreciate them to be realized in Rel-17. |
|  |  |
|  |  |

## Presence of the *Data Forwarding Response MRB List* IE in the *Target NG-RAN Node to Source NG-RAN Node Transparent Container* IE

R3-223379 proposes to reconsider the presence of the *Data Forwarding Response MRB List* IE in the *Target NG-RAN Node to Source NG-RAN Node Transparent Container* IE, which is currently set to "mandatory".

Please provide your view and reasoning.

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | As outlined in our paper, we would regard the change of presence as a precaution for further protocol additions, where the data forwarding IE would not be the only IE to be included. |
|  |  |
|  |  |

## Addition of stage 2 text in TS 38.420

R3-223096 proposes to include stage 2 text into TS 38.420.

Please provide comments/support/etc on the proposal in R3-223096.

|  |  |
| --- | --- |
| Company | Comment |
| Ericsson | we would be fine with the CR. |
|  |  |
|  |  |

## Any other topic which the moderator unintentionally missed

Please add thing, the moderator has missed.

|  |  |
| --- | --- |
| Company | Comment |
|  |  |
|  |  |
|  |  |

# Conclusion, Recommendations [if needed]

If needed

# References

1. R3-223077 " MBS Session Status during Xn HO preparation (Huawei, CBN, China Unicom, Lenovo, Motorola Mobility)" CR TS 38.423
2. R3-223078 " MBS Session Status during NG HO preparation (Huawei, CBN, China Unicom, Lenovo, Motorola Mobility)" CR TS 38.413
3. R3-223096 "Alignment with rel-17 changes in XnAP (Qualcomm Incorporated)" CR TS 38.420
4. R3-223185 "Indication for inactive MBS session (NEC)" discussion
5. R3-223187 "MBS Session Status indication in NGAP interface (NEC)" CR TS 38.413
6. R3-223188 "MBS Session Status indication in Xn interface (NEC)" CR TS 38.423
7. R3-223282 "Discussion the editor’s notes related to consent (Samsung)" discussion
8. R3-223283 "Remove the editor’s notes related to consent information (Samsung)" CR TS 38.401
9. R3-223284 "Remove the editor’s notes related to consent information (Samsung)" CR TS 37.483
10. R3-223379 "Rel-17 MBS Corrections (Ericsson)" discussion
11. R3-223452 "Correction of MBS Data Forwarding (Nokia, Nokia Shanghai Bell, Huawei)", draft CR TS 38.300
12. R3-223456 "Correction of MBS Shared CU UP (Nokia, Nokia Shanghai Bell)" CR TS 37.483
13. R3-223604 "Correction on NR MBS mobility for 38300 (ZTE Corporation)", draft CR TS 38.300 Rel-17
14. R3-223627 "Consent information exchange between E1 interface (Huawei)" discussion
15. R3-223628 "Correction on the FFS consent information (Huawei)" CR TS 38.401
16. R3-223629 "Correction on the FFS consent information (Huawei)" CR TS 37.483
17. R3-223631"Open issues in NGAP and XnAP specs (Qualcomm Incorporated)" discussion
18. R3-223672 "Corrections to E1AP for NR MBS (ZTE)" CR TS 38.423