**3GPP TSG-RAN3 #116-e R3-223858**

**9 – 19 May 2022**

**Online**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.300** | **CR** | **0xxx** | **rev** |  | **Current version:** | **17.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Corrections for NR NTN |
|  |  |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell, CATT |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_NTN\_solutions |  | ***Date:*** | 2022-04-15 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | The mapping configuration for the Mapped Cell ID is incorrectly added as NOTE, while the other part of the mapping configuration is in the normative paragraph. |
|  |  |
| ***Summary of change:*** | Move the text for the mapped configuration from the NOTE paragraph to a normative paragrah.Impact Analysis:Impact assessment towards the previous version of the specification (same release): This CR has limited impact under funtional point of view, since it clarifies the mapping configuration for the Mapped Cell ID is configured in the RAN and Core Network. |
|  |  |
| ***Consequences if not approved:*** | The normative text remains in informative NOTE, and may cause issue for Mapped Cell ID.  |
|  |  |
| ***Clauses affected:*** | 16.14.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**<<<<<< START OF CHANGE >>>>>>**

### 16.14.5 NG-RAN signalling

The Cell Identity, as defined in TS 38.413 [26] and TS 38.423 [50], used in following cases may corresponds to a Mapped Cell ID, irrespective of the orbit of the NTN payload or the types of service links supported.

- The Cell Identity indicated by the gNB to the Core Network as part of the User Location Information;

- The Cell Identity used for Paging Optimization in NG interface;

- The Cell Identity used for Area of Interest;

- The Cell Identity used for PWS.

The Cell Identity included within the target identification of the handover messages allows identifying the correct target cell.

The Cell Identities used in the RAN Paging Area during Xn RAN paging allow the identification of the correct target cells for RAN paging.

NOTE 1: The Cell Identity used for RAN Paging is assumed to typically represent a Uu Cell ID.

The mapping between Mapped Cell IDs and geographical areas is configured in the RAN and Core Network.

NOTE 2: A specific geographical location may be mapped to multiple Mapped Cell ID(s), and such Mapped Cell IDs may be configured to indicate differerent geographical areas (e.g. overlapping and/or with different dimensions).

The gNB is responsible for constructing the Mapped Cell ID based on the UE location info received from the UE, if available. The mapping may be pre-configured (e.g., up to operator's policy) or up to implementation.

NOTE 3: As described in TS 23.501 [3], the User Location Information may enable the AMF to determine whether the UE is allowed to operate at its present location. Special Mapped Cell IDs may be used to indicate areas outside the serving PLMN's country.

The gNB reports the broadcasted TAC(s) of the selected PLMN to the AMF as part of ULI. In case the gNB knows the UE's location information, the gNB may determine the TAI the UE is currently located in and provide that TAI to the AMF as part of ULI.

**<<<<<< END OF CHANGE >>>>>>**