Title: [DRAFT] LS on transfer of SDT related information in case of SDT with UE context relocation

Response to: -

Release: Release 17

Work Item: NR\_SmallData\_INACTIVE-Core

Source: CATT (to be RAN3)

To: RAN2

Cc:

**Contact Person:**

Name: Jiancheng Sun

Tel. Number: -

E-mail Address: sunjiancheng@catt.cn

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

Attachments: n/a

**1. Overall Description:**

In case of SDT with UE context relocation, the old NG-RAN node shall include SDT Radio Bearer Configuration, i.e. SDT DRB list, SDT SRB (list), in Retrieval UE Context Response message.

To Transfer the SDT related information, RAN3 has decided to adopt the signalling based solution, i.e. adding an additional XnAP IE to Retrieval UE Context Response message.

RAN3 respectfully asks RAN2 to further confirm whether there’s any critical issue from RAN2 point of view.

**2. Actions:**

**To RAN2 group.**

**ACTION:** RAN3 respectfully asks RAN2 group to take above into account and confirm whether there’s any critical issue from RAN2 point of view.

**3. Date of Next RAN WG3 Meetings:**

RAN3 Meeting #117-e August 15 – 25, 2022 Electronic Meeting

RAN3 Meeting #117bis-e October 10 – 18, 2022 Electronic Meeting