**3GPP TSG RAN3 meeting #117-e R3-22xxxx**

15th Aug – 24 Aug 2022 Online

**Title:** LS on Support for Reporting of RAN Visible QoE Measurements

**Response to:** -

**Release:** Rel-17

**Work Item:** NR\_QoE-Core

**Source:** China Unicom (To be RAN3)

**To:** RAN2

**Cc:**

**Contact Person:**

**Name: Pei Li**

**E-mail Address: lip104@chinaunicom.cn**

**Send any reply LS to: 3GPP Liaisons Coordinator, [mailto:3GPPLiaison@etsi.org](mailto:3GPPLiaison@etsi.org" \t "_blank)**

**Attachments:** -

**1. Overall description:**

RAN3 agreed to discuss the R17 leftover issues in R18 for RAN visible QoE. The following agreement is captured in the following RAN3#117-e agreements:

* **UE should include QoS flow information in the RVQoE report to RAN.**
* **QoE reports can be transmitted to either MN or SN and the reporting leg (MCG or SCG) can be changed during the application session.**

The QoS flow ID(s) corresponding to the service that is measured should be transmitted from UE to NG-RAN, since one QMC measurement session may be associated with one or more QoS flows. The format of QoS Flow ID is INTEGER (0..63), and it is provided per *measConfigAppLayerId*.

**2. Actions:**

RAN3 respectfully asks RAN2 to take the above RAN3 agreements into account and provide the necessary RRC signalling support.

**3. Date of next TSG RAN WG3 meeting:**

RAN3#117bis-e 2022-10-10 - 2022-10-18 online

RAN3#118 2022-11-14 - 2022-11-18 TBD