3GPP TSG-RAN WG3 #119 R3-230931

27th February – 3rd March 2023

Athens, Greece

Agenda Item: 15.2.3

Source: CATT (moderator)

Title: Summary of Offline Discussion

Document for: Approval

# Introduction

This contribution capture the discussion on the following CB

**CB: # 37\_MBS2\_INACTIVE**

**- Try to convergence on the meaning of indication?**

(CATT - moderator)

Summary of offline disc [R3-230931](file:///C:\Users\liuaijuan\AppData\Local\Temp\360zip$Temp\360$0\Inbox\R3-230931.zip)

# For the Chairman’s Notes

Propose to capture the follows:

It is FFS which interpretation on the indication from CN to RAN should be adopted in RAN3：

Interpretation 1: UE is preferred to be kept in connected when receiving the related MBS session data.

Interpretation 2: The IE indicates that the UE requires preferential treatment within the multicast group, guaranteeing steady and prompt provision of system resources for data transmission and reception.

# Discussion

During the offline session, there are two interpretations on the indication from CN to RAN and it could not be converged.

Interpretation 1: UE is preferred to be kept in connected when receiving the related MBS session data.

Interpretation 2: The IE indicates that the UE requires preferential treatment within the multicast group, guaranteeing steady and prompt provision of system resources for data transmission and reception.

# Conclusion, Recommendations [if needed]

# References