**3GPP TSG-RAN WG3 Meeting #127-bis R3-25XXXX**

Wuhan, China, 7th – 11th April 2025

**Title:** (TPs to BL CR 38.410) Introduce NG Removal Function

**Source:** CMCC, Samsung, ZTE, CATT, Xiaomi, Nokia, Nokia Shanghai Bell, LG Electronics, NEC

**Agenda item:** 14.3

**Document Type:** Other

# Introduction

**This contribution proposes TP to describe NG Removal function in TS38.410.**

# 5. TP to BL CR for TS38.410 on NG Removal

<<<<<<<<<<<<<<<<<<<< Start of Changes >>>>>>>>>>>>>>>>>>>>

## 5.8 NG Interface Management function

The NG-interface management functions provide:

- means to ensure a defined start of NG-interface operation (reset);

- means to handle different versions of application part implementations and protocol errors (error indication).

- means to remove the interface instance between gNB and AMF in a controlled manner (removal).

<<<<<<<<<<<<<<<<<<<< End of Changes >>>>>>>>>>>>>>>>>>>>