**3GPP T****SG-RAN WG3 Meeting #127bis R3-252428**

**Wuhan, China, 7th – 11th April 2025**

**Agenda item:** 19.2

**Source:** CATT, Ericsson

**Title:** (TP to BL CR for 38.470) introduction of Evolution of NR duplex operation: Sub-band full duplex (SBFD)

**Document for:** Agreement

# Introduction

This paper reflects the agreements achieved in RAN3#127bis.

# TP to TS38.470

<<<< Start of change >>>

5.2 F1-C functions

<<<Unchanged part omitted>>>

5.2.x CLI mitigation function

The CLI mitigation function enables the transfer of CLI measurements and CLI mitigation request between gNB-DU and gNB-CU.

<<<Next change>>>

## 6.1 Control plane procedures

<<<Unchanged part omitted>>>

6.1. x CLI mitigation function

Editor’s Note: The name of procedure and message might be updated pending on further discussion.

The following procedures are used to report the result of CLI measurements and to request the CLI mitigation:

- CLI MEASUREMENT UPDATE

<<<< End of change >>>