**3GPP TSG-RAN3 Meeting #128 *R3-253841***

**Malta, Malta, 19th May 2025 - 23rd May 2025**

**Title:** **[Draft] LS on reporting status of Exposure of available bitrate**

**Response to:**

**Release: Release 19**

**Work Item: NR\_XR\_Ph3-Core**

**Source: [Ericsson to be] RAN3**

**To: SA2**

**Cc: CT4**

**Contact person:** Yazid Lyazidi

Yazid.lyazidi@ericsson.com

**Send any reply LS to:** 3GPP Liaisons Coordinator, mailto:3GPPLiaison@etsi.org

**Attachments:**

# 1 Overall description

RAN3 has discussed whether it is beneficial that NG-RAN node indicates the activation status (activated or deactivated) of available data rate reporting, at the PDU session setup and modification responses, Path Switch Request and Handover Request Acknowledge messages. This aligns with ECN Marking/Congestion reporting signalling.

RAN3 kindly asks SA2 if such activation status is beneficial from CN’s perspective.

# 2 Actions

**To SA2**

**ACTION:** RAN3 respectfully requests SA2 to provide feedback on the introduction of a status activation for Available Bitrate monitoring from gNB to SMF.

# 3 Dates of next TSG RAN WG 3 meetings

TSG-RAN3 Meeting #129 25-29 Aug 2025 Bangalore, IN

TSG-RAN3 Meeting #129-bis 13-17 Oct 2025 Prague, CZ