|  |
| --- |
| 3GPP TR 37.827 V0.2.0 (2021-08) |
| Technical Report |
| 3rd Generation Partnership Project;Technical Specification Group Radio Access Networks;Power Class 2 for EN-DC with xLTE band + yNR DL with 1LTE+1(TDD) NR UL band (x= 2, 3, 4, y=1; x=1, 2, y=2). (Release 17) |
|   |
| *5G-logo_175px* | 3GPP-logo_web |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP.The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented.This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification.Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. |

|  |
| --- |
|  |
| ***3GPP***Postal address3GPP support office address650 Route des Lucioles - Sophia AntipolisValbonne - FRANCETel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16Internethttp://www.3gpp.org |
| ***Copyright Notification***No part may be reproduced except as authorized by written permission.The copyright and the foregoing restriction extend to reproduction in all media.© 2020, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).All rights reserved.UMTS™ is a Trade Mark of ETSI registered for the benefit of its members3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational PartnersLTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational PartnersGSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 8

1 Scope 10

2 References 10

3 Definitions of terms, symbols and abbreviations 10

3.1 Terms 10

3.2 Symbols 10

3.3 Abbreviations 10

4 Background 10

4.1 TR maintenance 11

5 EN-DC Power Class 2: Specific Band Combination Part 11

5.1 DC\_2A-5A\_n77A 11

5.1.1 Transmitter Characteristics 11

5.1.1.1 Maximum Output Power 11

5.1.1.2 Co-existence study 11

5.1.2 Receiver Characteristics 11

5.1.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 11

5.1.2.1.1 Power class 2 Case A 11

5.1.2.1.2 Power class 2 Case B 12

5.2 DC\_2A-13A\_n77A 12

5.2.1 Transmitter Characteristics 12

5.2.1.1 Maximum Output Power 12

5.2.1.2 Co-existence study 12

5.2.2 Receiver Characteristics 12

5.2.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 12

5.2.2.1.1 Power class 2 Case A 12

5.2.2.1.2 Power class 2 Case B 13

5.3 DC\_2A-66A\_n77A 13

5.3.1 Transmitter Characteristics 13

5.3.1.1 Maximum Output Power 13

5.3.1.2 Co-existence study 13

5.3.2 Receiver Characteristics 13

5.3.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 13

5.3.2.1.1 Power class 2 Case A 13

5.3.2.1.2 Power class 2 Case B 14

5.4 DC\_5A-66A\_n77A 14

5.4.1 Transmitter Characteristics 14

5.4.1.1 Maximum Output Power 14

5.4.1.2 Co-existence study 14

5.4.2 Receiver Characteristics 14

5.4.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 14

5.4.2.1.1 Power class 2 Case A 14

5.4.2.1.2 Power class 2 Case B 15

5.5 DC\_13A-66A\_n77A 15

5.5.1 Transmitter Characteristics 15

5.5.1.1 Maximum Output Power 15

5.5.1.2 Co-existence study 15

5.5.2 Receiver Characteristics 15

5.5.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 15

5.5.2.1.1 Power class 2 Case A 15

5.5.2.1.2 Power class 2 Case B 16

5.6 DC\_2A\_n5A-n77A 16

5.6.1 Transmitter Characteristics 16

5.6.1.1 Maximum Output Power 16

5.6.1.2 Co-existence study 16

5.6.2 Receiver Characteristics 16

5.6.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 16

5.6.2.1.1 Power class 2 Case A 16

5.6.2.1.2 Power class 2 Case B 17

5.7 DC\_66A\_n2A-n77A 17

5.7.1 Transmitter Characteristics 17

5.7.1.1 Maximum Output Power 17

5.7.1.2 Co-existence study 17

5.7.2 Receiver Characteristics 17

5.7.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 17

5.7.2.1.1 Power class 2 Case A 17

5.7.2.1.2 Power class 2 Case B 18

5.8 DC\_66A\_n5A-n77A 18

5.8.1 Transmitter Characteristics 18

5.8.1.1 Maximum Output Power 18

5.8.1.2 Co-existence study 18

5.8.2 Receiver Characteristics 18

5.8.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 18

5.8.2.1.1 Power class 2 Case A 18

5.8.2.1.2 Power class 2 Case B 19

5.9 DC\_2-13\_n66-n77 19

5.9.1 Maximum Output Power 19

5.9.3 Co-existence study 19

5.10 DC\_2-13-66\_n77 20

5.10.1 Maximum Output Power 20

5.10.2 Configuration for EN-DC 20

5.10.3 Co-existence study 20

5.11 DC\_13-66\_n2-n77 20

5.11.1 Maximum Output Power 20

5.11.2 Co-existence study 20

5.12 DC\_2-66\_n5-n77 21

5.12.1 Maximum Output Power 21

5.12.3 Co-existence study 21

5.13 DC\_2-5-66\_n77 21

5.13.1 Maximum Output Power 21

5.13.3 Co-existence study 21

5.14 DC\_13\_n66-n77 22

5.14.1 Transmitter Characteristics 22

5.14.1.1 Maximum Output Power 22

5.14.1.3 Co-existence study 22

5.14.2 Receiver Characteristics 22

5.14.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 22

5.14.2.1.1 Power class 2 Case A 22

5.14.2.1.2 Power class 2 Case B 23

5.15 DC\_13\_n2-n77 23

5.15.1 Transmitter Characteristics 23

5.15.1.1 Maximum Output Power 23

5.15.1.3 Co-existence study 23

5.15.2 Receiver Characteristics 23

5.15.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 23

5.15.2.1.1 Power class 2 Case A 23

5.15.2.1.2 Power class 2 Case B 24

5.16 DC\_2A-66A\_n41A 24

5.16.1 Transmitter Characteristics 24

5.16.1.1 Maximum Output Power 24

5.16.1.2 Co-existence study 24

5.16.2 Receiver Characteristics 24

5.16.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 24

5.16.2.1.1 Power class 2 Case A 24

5.16.2.1.2 Power class 2 Case B 25

5.17 DC\_66\_n66-n77 25

5.17.1 Transmitter Characteristics 25

5.17.1.1 Maximum Output Power 25

5.17.1.2 Co-existence study 25

5.17.2 Receiver Characteristics 25

5.17.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 25

5.17.2.1.1 Power class 2 Case A 25

5.17.2.1.2 Power class 2 Case B 26

5.18 DC\_48-66\_n77 26

5.18.1 Transmitter Characteristics 26

5.18.1.1 Maximum Output Power 26

5.18.1.3 Co-existence study 26

5.18.2 Receiver Characteristics 26

5.18.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 26

5.19 DC\_13\_n5-n77 27

5.19.1 Transmitter Characteristics 27

5.19.1.1 Maximum Output Power 27

5.19.1.3 Co-existence study 27

5.19.2 Receiver Characteristics 27

5.19.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 27

5.19.2.1.1 Power class 2 Case A 27

5.19.2.1.2 Power class 2 Case B 27

5.20 DC\_5\_n66-n77 28

5.20.1 Transmitter Characteristics 28

5.20.1.1 Maximum Output Power 28

5.20.1.3 Co-existence study 28

5.20.2 Receiver Characteristics 28

5.20.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 28

5.20.2.1.1 Power class 2 Case A 28

5.20.2.1.2 Power class 2 Case B 29

5.21 DC\_5A\_n5A-n77A 29

5.21.1 Transmitter Characteristics 29

5.21.1.1 Maximum Output Power 29

5.21.1.3 Co-existence study 29

5.21.2 Receiver Characteristics 29

5.21.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 29

5.21.2.1.1 Power class 2 Case A 29

5.21.2.1.2 Power class 2 Case B 30

5.22 DC\_5\_n2-n77 30

5.22.1 Transmitter Characteristics 30

5.22.1.1 Maximum Output Power 30

5.22.1.3 Co-existence study 30

5.22.2 Receiver Characteristics 30

5.22.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 30

5.22.2.1.1 Power class 2 Case A 30

5.22.2.1.2 Power class 2 Case B 31

5.23 DC\_2\_n66-n77 31

5.23.1 Transmitter Characteristics 31

5.23.1.1 Maximum Output Power 31

5.23.1.3 Co-existence study 31

5.23.2 Receiver Characteristics 31

5.23.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 31

5.23.2.1.1 Power class 2 Case A 31

5.23.2.1.2 Power class 2 Case B 32

5.24 DC\_2-48\_n77 32

5.24.1 Transmitter Characteristics 32

5.24.1.1 Maximum Output Power 32

5.24.1.3 Co-existence study 32

5.24.2 Receiver Characteristics 32

5.24.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 32

5.25 DC\_2A\_n2A-n77A 33

5.25.1 Transmitter Characteristics 33

5.25.1.1 Maximum Output Power 33

5.25.1.3 Co-existence study 33

5.25.2 Receiver Characteristics 33

5.25.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 33

5.25.2.1.1 Power class 2 Case A 33

5.25.2.1.2 Power class 2 Case B 34

5.26 DC\_1A-5A\_n78A 34

5.26.1 Transmitter Characteristics 34

5.26.1.1 Maximum Output Power 34

5.26.1.2 Co-existence study 34

5.26.2 Receiver Characteristics 34

5.26.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 34

5.26.2.1.1 Power class 2 Case A 34

5.26.2.1.2 Power class 2 Case B 35

5.27 DC\_1A-n7A\_n78A 35

5.27.1 Transmitter Characteristics 35

5.27.1.1 Maximum Output Power 35

5.27.1.2 Co-existence study 35

5.27.2 Receiver Characteristics 36

5.27.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands 36

5.27.2.1.1 Power class 2 Case A 36

5.27.2.1.2 Power class 2 Case B 36

Annex A - Change history 37

**Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.Error! Bookmark not defined.**

# Foreword

This Technical Report has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document is a technical report Power Class 2 for EN-DC with xLTE band + yNR DL with 1LTE+1(TDD) NR UL band (x= 2, 3, 4, y=1; x=1, 2, y=2) under Rel-17 time frame. The purpose is to gather the relevant background information and studies in order to address relevant requirements for the Rel-17 EN-DC band combinations with Power Class 2 requested by proponents and captured in the WID...

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] RP-210816, “New WID on PC2 EN-DC with x LTE band + y NR band (x= 2, 3, 4, y=1; x=1, 2, y=2)”, RAN#91-e

# 3 Definitions of terms, symbols and abbreviations

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

**example:** text used to clarify abstract rules by applying them literally.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

<symbol> <Explanation>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

<ABBREVIATION> <Expansion>

# 4 Background

The present document is a technical report for Power Class 2 band combinations under Rel-17 timeframe. The document covers each band combination specific issues (i.e. one sub-clause defined per band combination)

## 4.1 TR maintenance

A single company is responsible for introducing all approved TPs in the current TR, i.e. TR editor. However, it is the responsibility of the contact person of each band combination to ensure that the TPs related to the band combination have been implemented.

# 5 EN-DC Power Class 2: Specific Band Combination Part

## 5.1 DC\_2A-5A\_n77A

### 5.1.1 Transmitter Characteristics

#### 5.1.1.1 Maximum Output Power

Table 5.1.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A | 266 | +2/-3 |
| DC\_5A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

####

#### 5.1.1.2 Co-existence study

According to the PC3 DC\_2A-5A\_n77A study in 37.717-21-11, the Rx impacts are identified as below,

* 3rd order IMD products generated by DC\_2\_5 uplink may fall into own Rx of band n77.
* 5th order IMD products generated by DC\_2\_n77 uplink may fall into own Rx of band 5.

Thus, additional MSD for IMD 3 and 5 should be considered to mitigate the impact of the interference for PC2 DC\_2A-5A\_n77A combination.

### 5.1.2 Receiver Characteristics

#### 5.1.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.1.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_2A-5A\_n77A are defined in table 5.1.2.2.1-1.

Table 5.1.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc (MHz) | UL/DL BW (MHz) | ULLCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_2A-5A\_n77A | 2 | 1907.5 | 5 | 25 | 1987.5 | N/A | N/A |
| 5 | 842.5 | 5 | 25 | 887.5 | 16.6 | IMD5 |
| n77 | 3305 | 5 | 25 | 3305 | N/A | N/A |
| 2 | 1907 | 5 | 25 | 1987 | 24.8 | IMD3 |
| 5 | 846.5 | 5 | 25 | 891.5 | N/A | N/A |
| n77 | 3680 | 5 | 25 | 3680 | N/A | N/A |

#### 5.1.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_2A-5A\_n77A are the same as the Case A defined in table 5.1.2.1.1-1.

## 5.2 DC\_2A-13A\_n77A

### 5.2.1 Transmitter Characteristics

#### 5.2.1.1 Maximum Output Power

Table 5.2.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A | 266 | +2/-3 |
| DC\_13A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.2.1.2 Co-existence study

According to the PC3 DC\_2A-13A\_n77A study in 37.717-21-11, the Rx impacts are identified as below,

* No IMD issue for Rx of band 13 with UL DC\_2\_n77.
* 3rd order IMD products generated by DC\_13\_n77 uplink may fall into own Rx of band 2

Thus, additional MSD for IMD 3 should be considered to mitigate the impact of the interference for PC2 DC\_2A-13A\_n77A combination.

### 5.2.2 Receiver Characteristics

#### 5.2.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.2.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_2A-13A\_n77A are defined in table 5.2.2.2.1-1.

Table 5.2.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc (MHz) | UL/DL BW (MHz) | ULLCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_2A-13A\_n77A | 2 | 1864 | 5 | 25 | 1944 | 24.2 | IMD3 |
| 13 | 783 | 5 | 25 | 752 | N/A | N/A |
| n77 | 3510 | 5 | 25 | 3510 | N/A | N/A |

#### 5.2.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_2A-13A\_n77A are the same as the Case A defined in table 5.2.2.1.1-1.

## 5.3 DC\_2A-66A\_n77A

### 5.3.1 Transmitter Characteristics

#### 5.3.1.1 Maximum Output Power

Table 5.3.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A | 266 | +2/-3 |
| DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.3.1.2 Co-existence study

According to the PC3 DC\_2A-66A\_n77A study in 37.717-21-11, the Rx impacts are identified as below,

* 2nd, 4th and 5th order IMD products generated by DC\_2\_n77 uplink may fall into own Rx of band 66
* 2nd, 4th and 5th order IMD products generated by DC\_66\_n77 uplink may fall into own Rx of band 2

Thus, additional MSD for IMD 3 and 5 should be considered to mitigate the impact of the interference for PC2 DC\_2A-66A\_n77A combination.

### 5.3.2 Receiver Characteristics

#### 5.3.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.3.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_2A-66A\_n77A are defined in table 5.3.2.2.1-1.

Table 5.3.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc (MHz) | UL/DL BW (MHz) | ULLCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_2A-66A\_n77A | 2 | 1855 | 5 | 25 | 1935 | N/A | N/A |
| 66 | 1765 | 5 | 25 | 2185 | 34.7 | IMD2 |
| n77 | 4040 | 5 | 25 | 4040 | N/A | N/A |
| 2 | 1905 | 5 | 25 | 1985 | M/A | N/A |
| 66 | 1720 | 5 | 25 | 2120 | 21.1 | IMD44 |
| n77 | 3595 | 5 | 25 | 3595 | N/A | N/A |
| 2 | 1880 | 5 | 25 | 1960 | 37.6 | IMD2 |
| 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |
| n77 | 3700 | 5 | 25 | 3700 | N/A | N/A |
| 2 | 1860 | 5 | 25 | 1940 | 19.8 | IMD44 |
| 66 | 1775 | 5 | 25 | 2195 | N/A | N/A |
| n77 | 3385 | 5 | 25 | 3385 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. |

#### 5.3.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_2A-66A\_n77A are the same as the Case A defined in table 5.3.2.1.1-1.

## 5.4 DC\_5A-66A\_n77A

### 5.4.1 Transmitter Characteristics

#### 5.4.1.1 Maximum Output Power

Table 5.4.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_5A\_n77A | 266 | +2/-3 |
| DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.4.1.2 Co-existence study

According to the PC3 DC\_5A-66A\_n77A study in 37.717-21-11, the Rx impacts are identified as below,

* The IMD3 of UL DC\_5A\_n77A may impact to band 66 Rx.

Thus, additional MSD for IMD 3 should be considered to mitigate the impact of the interference for PC2 DC\_5A-66A\_n77A combination.

### 5.4.2 Receiver Characteristics

#### 5.4.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.4.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_5A-66A\_n77A are defined in table 5.4.2.2.1-1.

Table 5.4.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

|  |
| --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** |
| **DC****Configuration** | **EUTRA and NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL CLRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_5A-66A\_n77A | 5 | 826.5 | 5 | 25 | 871.5 | N/A | N/A |
| 66 | 1742 | 5 | 25 | 2142 | 22.2 | IMD3 |
| n77 | 3795 | 10 | 50 | 3795 | N/A | N/A |

#### 5.4.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_5A-66A\_n77A are the same as the Case A defined in table 5.4.2.1.1-1.

## 5.5 DC\_13A-66A\_n77A

### 5.5.1 Transmitter Characteristics

#### 5.5.1.1 Maximum Output Power

Table 5.5.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_13A\_n77A | 266 | +2/-3 |
| DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.5.1.2 Co-existence study

According to the PC3 DC\_13A-66A\_n77A study in 37.717-21-11, the Rx impacts are identified as below,

* 3rd order IMD products generated by DC\_13\_n77 uplink may fall into own Rx of band 66.
* 3rd order IMD products generated by DC\_66\_n77 uplink may fall into own Rx of band 13

Thus, additional MSD for IMD 3 should be considered to mitigate the impact of the interference for PC2 DC\_13A-66A\_n77A combination.

### 5.5.2 Receiver Characteristics

#### 5.5.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.5.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_13A-66A\_n77A are defined in table 5.5.2.2.1-1.

Table 5.5.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc (MHz) | UL/DL BW (MHz) | ULLCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_13A-66A\_n77A | 13 | 777 | 5 | 25 | 746 | N/A | N/A |
| 66 | 1746 | 5 | 25 | 2146 | 25.3 | IMD3 |
| n77 | 3700 | 10 | 50 | 3700 | N/A | N/A |
| 13 | 781 | 5 | 25 | 750 | 23.4 | IMD3 |
| 66 | 1710 | 5 | 25 | 2110 | N/A | N/A |
| n77 | 4170 | 10 | 50 | 4170 | N/A | N/A |

#### 5.5.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_13A-66A\_n77A are the same as the Case A defined in table 5.5.2.1.1-1.

## 5.6 DC\_2A\_n5A-n77A

### 5.6.1 Transmitter Characteristics

#### 5.6.1.1 Maximum Output Power

Table 5.6.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.6.1.2 Co-existence study

According to the PC3 DC\_2A\_n5A-n77A study in 37.717-11-21, the Rx impacts are identified as below,

* 3rd and 5th order IMD generated by dual uplink of 2\_n5 may fall into own Rx of band n77.
* 5th order IMD generated by dual uplink of 2\_n77 may fall into own Rx of band n5.

Thus, additional MSD for IMD 3 and 5 should be considered to mitigate the impact of the interference for PC2 DC\_2A\_n5A-n77A combination.

### 5.6.2 Receiver Characteristics

#### 5.6.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.6.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_2A\_n5A-n77A are defined in table 5.6.2.2.1-1.

Table 5.6.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc (MHz) | UL/DL BW (MHz) | ULLCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_2A\_n5A-n77A | 2 | 1880 | 5 | 25 | 1960 | N/A | N/A |
|  | n5 | 830 | 5 | 25 | 875 | N/A | N/A |
|  | n77 | 3540 | 10 | 50 | 3540 | 24.5 | IMD3 |
|  | 2 | 1907 | 5 | 25 | 1987 | N/A | N/A |
|  | n5 | 844 | 5 | 25 | 889 | 16.6 | IMD5 |
|  | n77 | 3305 | 10 | 50 | 3305 | N/A | N/A |

#### 5.6.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_2A\_n5A-n77A are the same as the Case A defined in table 5.6.2.1.1-1.

## 5.7 DC\_66A\_n2A-n77A

### 5.7.1 Transmitter Characteristics

#### 5.7.1.1 Maximum Output Power

Table 5.7.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.7.1.2 Co-existence study

According to the PC3 DC\_66A\_n2A-n77A study in 37.717-11-21, the Rx impacts are identified as below,

* 2nd, 4th and 5th order IMD generated by dual uplink of 66\_n77 may fall into own Rx of band n2.
* 2nd and 4th order IMD generated by dual uplink of 66\_n2 may fall into own Rx of band n77.

Thus, additional MSD for IMD 2, 4 and 5 should be considered to mitigate the impact of the interference for PC2 DC\_66A\_n2A-n77A combination.

### 5.7.2 Receiver Characteristics

#### 5.7.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.7.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_66A\_n2A-n77A are defined in table 5.7.2.2.1-1.

Table 5.7.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** |
| --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL****LCRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_66A\_n2A-n77A | 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |
| n2 | 1880 | 5 | 25 | 1960 | N/A | N/A |
| n77 | 3620 | 10 | 50 | 3620 | 34.9 | IMD2 |
| 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |
| n2 | 1880 | 5 | 25 | 1960 | N/A | N/A |
| n77 | 3340 | 10 | 50 | 3340 | 20.9 | IMD44 |
| n2 | 1880 | 5 | 25 | 1960 | 37.6 | IMD2 |
| 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |
| n77 | 3700 | 10 | 50 | 3700 | N/A | N/A |
| n2 | 1880 | 5 | 25 | 1960 | 21.1 | IMD44 |
| 66 | 1770 | 5 | 25 | 2170 | N/A | N/A |
| n77 | 3350 | 10 | 50 | 3350 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. |

#### 5.7.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_66A\_n2A-n77A are the same as the Case A defined in table 5.7.2.1.1-1.

## 5.8 DC\_66A\_n5A-n77A

### 5.8.1 Transmitter Characteristics

#### 5.8.1.1 Maximum Output Power

Table 5.8.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.8.1.2 Co-existence study

According to the PC3 DC\_66A\_n5A-n77A study in 37.717-11-21, the Rx impacts are identified as below,

* 3rd 4th and 5th order IMD generated by dual uplink of 66\_n5 may fall into own Rx of band n77

Thus, additional MSD for IMD 3, 4 and 5 should be considered to mitigate the impact of the interference for PC2 DC\_66A\_n5A-n77A combination.

### 5.8.2 Receiver Characteristics

#### 5.8.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.8.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_66A\_n5A-n77A are defined in table 5.8.2.2.1-1.

Table 5.8.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** |
| --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL****LCRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_66A\_n5A-n77ADC\_66A-66A\_n5A-n77A | 66 | 1760 | 5 | 25 | 2160 | N/A | N/A |
| n5 | 830 | 5 | 25 | 875 | N/A | N/A |
| n77 | 3420 | 10 | 50 | 3420 | 24.9 | IMD3 |
| 66 | 1714 | 5 | 25 | 2114 | N/A | N/A |
| n5 | 827 | 5 | 25 | 872 | N/A | N/A |
| n77 | 4195 | 10 | 50 | 4195 | 24.1 | IMD44 |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. |

#### 5.8.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_66A\_n5A-n77A are the same as the Case A defined in table 5.8.2.1.1-1.

## 5.9 DC\_2-13\_n66-n77

### 5.9.1 Maximum Output Power

Table 5.9.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77ADC\_13A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.9.2 Configurations for EN-DC

Table 5.9.2-1: Inter-band EN-DC configurations within FR1 (four bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_2A-13A\_n66A-n77A | DC\_2A\_n77ADC\_13A\_n77A |

#### 5.9.3 Co-existence study

MSD have been defined for lower order combinations [2, 3]. No further MSD is needed for both Case A and B.

## 5.10 DC\_2-13-66\_n77

#### 5.10.1 Maximum Output Power

Table 5.10.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A, DC\_13A\_n77A, DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.10.2 Configuration for EN-DC

Table 5.10.2-1: Inter-band EN-DC configurations within FR1 (four bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_2A-13A-66A\_n77A  | DC\_2A\_n77A, DC\_13A\_n77A, DC\_66A\_n77A |

#### 5.10.3 Co-existence study

MSD have been defined for lower order combinations [2]. No further MSD is needed for both Case A and B.

## 5.11 DC\_13-66\_n2-n77

### 5.11.1 Maximum Output Power

Table 5.11.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_13A\_n77A, DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.11.2 Configurations for EN-DC

Table 5.11.2-1: Inter-band EN-DC configurations within FR1 (four bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_13A-66A\_n2A-n77A | DC\_13A\_n77A, DC\_66A\_n77A |

#### 5.11.2 Co-existence study

MSD have been defined for lower order combinations [2, 3]. No further MSD is needed for both Case A and B

## 5.12 DC\_2-66\_n5-n77

### 5.12.1 Maximum Output Power

Table 5.12.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_66A\_n77A, DC\_2A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.12.2 Configurations for EN-DC

Table 5.12.2-1: Inter-band EN-DC configurations within FR1 (four bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_2A-66A\_n5A-n77A | DC\_66A\_n77A, DC\_2A\_n77A |

#### 5.12.3 Co-existence study

MSD have been defined for lower order combinations [2]. No further MSD is needed for both Case A and B

## 5.13 DC\_2-5-66\_n77

### 5.13.1 Maximum Output Power

Table 5.13.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A, DC\_5A\_n77A, DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.13.2 Configurations for EN-DC

Table 5.13.2-1: Inter-band EN-DC configurations within FR1 (four bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_2A-5A-66A\_n77A | DC\_2A\_n77A, DC\_5A\_n77A, DC\_66A\_n77A |

#### 5.13.3 Co-existence study

MSD have been defined for lower order combinations [2]. No further MSD is needed for both Case A and B.

## 5.14 DC\_13\_n66-n77

### 5.14.1 Transmitter Characteristics

#### 5.14.1.1 Maximum Output Power

Table 5.14.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_13A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.14.1.2 Configurations for EN-DC

Table 5.14.1.2-1: Inter-band EN-DC configurations within FR1 (four bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_13A\_n66A-n77A | DC\_13A\_n77A |

#### 5.14.1.3 Co-existence study

According to the both PC3 DC\_13A\_n66A-n77A study in 37.717-11-21 and only DC\_13A\_n77A uplink configuration applied in this band combination, additional MSD due to IMD 3 to the band n66 from the configured uplink EN-DC should be considered to mitigate the impact of the interference to the PC2 DC\_13A\_n66A-n77A combination.

IMD generated by DC\_13A\_n77A that falls into the third band, n66

### 5.14.2 Receiver Characteristics

#### 5.14.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.14.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A of DC\_13A\_n66A-n77A are defined in table 5.14.2.1.1-1.

Table 5.14.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** |
| --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL****LCRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_13A\_n66A-n77A | 13 | 782 | 5 | 25 | 751 | N/A | N/A |
| n66 | 1756 | 5 | 25 | 2156 | 26.1 | IMD3 |
| n77 | 3720 | 10 | 50 | 3720 | N/A | N/A |

#### 5.14.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B of DC\_13A\_n66A-n77A are the same as the Case A defined in table 5.14.2.1.1-1.

## 5.15 DC\_13\_n2-n77

### 5.15.1 Transmitter Characteristics

#### 5.15.1.1 Maximum Output Power

Table 5.15.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_13A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.15.1.2 Configurations for EN-DC

Table 5.15.1.2-1: Inter-band EN-DC configurations within FR1 (four bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_13A\_n2A-n77A | DC\_13A\_n77A |

#### 5.15.1.3 Co-existence study

According to the both PC3 DC\_13A\_n2A-n77A study in 37.717-11-21 and only DC\_13A\_n77A uplink configuration applied in this band combination, additional MSD due to IMD 3 to the band n2 from the configured uplink EN-DC should be considered to mitigate the impact of the interference to the PC2 DC\_13A\_n66A-n77A combination.

### 5.15.2 Receiver Characteristics

#### 5.15.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.15.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A of DC\_13A\_n2A-n77A are defined in table 5.15.2.2.1-1.

Table 5.15.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** |
| --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL****LCRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_13A\_n2A-n77A | 13 | 782 | 5 | 25 | 751 | N/A | N/A |
| n2 | 1880 | 5 | 25 | 1960 | 25.0 | IMD3 |
| n77 | 3524 | 10 | 50 | 3524 | N/A | N/A |

#### 5.15.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B of DC\_13A\_n2A-n77A are the same as the Case A defined in table 5.15.2.1.1-1.

## 5.16 DC\_2A-66A\_n41A

### 5.16.1 Transmitter Characteristics

#### 5.16.1.1 Maximum Output Power

Table 5.16.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_66A\_n41A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.16.1.2 Co-existence study

According to the PC3 DC\_2A\_66A-n41A study in 37.716-21-11, the Rx impacts are identified as below,

* Co-existence analysis for DC\_2\_n41 shows that there is no impact from DC\_2\_n41 UL to Band 66 DL.
* Co-existence analysis for DC\_66\_n41 shows that there is IMD4 impact from DC\_66\_n41 UL to Band 2 DL.

Thus, additional MSD for IMD 4 should be considered to mitigate the impact of the interference for PC2 DC\_2A\_66A-n41A combination.

### 5.16.2 Receiver Characteristics

#### 5.16.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.16.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_2A\_66A-n41A are defined in table 5.16.2.2.1-1.

Table 5.16.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL****LCRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_2A-66A\_n41A | 2 | 1860 | 5 | 25 | 1940 | 22.6 | IMD4 |
| 66 | 1715 | 5 | 25 | 2115 | N/A | N/A |
| n41 | 2685 | 5 | 25 | 2685 | N/A | N/A |

#### 5.16.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_2A\_66A-n41A are the same as the Case A defined in table 5.16.2.1.1-1.

## 5.17 DC\_66\_n66-n77

### 5.17.1 Transmitter Characteristics

#### 5.17.1.1 Maximum Output Power

Table 5.17.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.17.1.2 Configurations for EN-DC

Table 5.17.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_66A\_n66A-n77A | DC\_66A\_n77A |

#### 5.17.1.2 Co-existence study

According to the PC2 coexistence studies performed in the lower order combinations, the Rx impacts are identified as below,

* For UL DC\_66A\_n77A configuration, IMD2 and IMD5 products fall into the band n66 Rx

Thus additional MSD exception should be considered to mitigate the impact of the interference.

### 5.17.2 Receiver Characteristics

#### 5.17.2.1  MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.17.2.1.1 Power class 2 Case A

Based on co-existence study, additional MSD are specified Table 5.17.2.1.1-1 for this dual connectivity configuration.

Table 5.17.2.1.1-1: MSD test points for SCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** |
| --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL****LCRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_66A\_n66A-n77A | 66 | 1730 | 5 | 25 | 2130 | N/A | N/A |
| n66 | 1770 | 5 | 25 | 2170 | 37 | IMD2 |
| n77 | 3900 | 10 | 50 | 3900 | N/A | N/A |
| 66 | 1730 | 5 | 25 | 2130 | N/A | N/A |
| n66 | 1770 | 5 | 25 | 2170 | 20 | IMD5 |
| n77 | 3680 | 10 | 50 | 3680 | N/A | N/A |

#### 5.17.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B configuration are same as the Case A defined in table 5.17.2.1.1-1.

## 5.18 DC\_48-66\_n77

### 5.18.1 Transmitter Characteristics

#### 5.18.1.1 Maximum Output Power

Table 5.18.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_66A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.18.1.2 Configurations for EN-DC

Table 5.18.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_48A-66A\_n77ADC\_48C-66A\_n77A | DC\_66A\_n77A |

#### 5.18.1.3 Co-existence study

According to coxeistence studies for the PC3 DC\_48A-66A\_n77A in TR 37.717-21-11, no harmonics and intermodulation products is present as the duplex mode for both band 48 and n77 is TDD and opertion in fully synchronizing in US.

### 5.18.2 Receiver Characteristics

#### 5.18.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

There is no additional MSD requirement for this PC2 band combination.

## 5.19 DC\_13\_n5-n77

### 5.19.1 Transmitter Characteristics

#### 5.19.1.1 Maximum Output Power

Table 5.19.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_13A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.19.1.2 Configurations for EN-DC

Table 5.19.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_13A\_n5A-n77A | DC\_13A\_n77A |

#### 5.19.1.3 Co-existence study

According to the PC3 DC\_13A\_n77A study in TR 37.717-21-11, the Rx impacts are identified as below,

* For UL DC\_13A\_n77A, IMD5 of the 2UL falls into band n5 Rx

Thus additional MSD should be considered to mitigate the impact of the interference.

### 5.19.2 Receiver Characteristics

#### 5.19.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.19.2.1.1 Power class 2 Case A

Based on co-existence study, additional MSD are specified Table 5.19.2.1.1-1 for this dual connectivity configuration.

Table 5.19.2.1.1-1: MSD test points for SCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DCConfiguration | EUTRA or NR band | UL Fc (MHz) | UL/DL BW (MHz) | UL LCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_13A\_n5A-n77A11 | n5 | 840 | 5 | 25 | 885 | 19.5 | IMD5 |
| 13 | 782 | 5 | 20 | 751 | N/A | N/A |
| n77 | 4013 | 10 | 50 | 4013 | N/A | N/A |
| NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. |

#### 5.19.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B configuratoin are same as the Case A defined in table 5.19.2.1.1-1.

## 5.20 DC\_5\_n66-n77

### 5.20.1 Transmitter Characteristics

#### 5.20.1.1 Maximum Output Power

Table 5.20.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_5A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

####

5.20.1.2 Configurations for EN-DC

Table 5.20.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_5A\_n66A-n77A | DC\_5A\_n77A |

#### 5.20.1.3 Co-existence study

For UL DC\_5A\_n77A, IMD3 generated by dual uplink of 5\_n77 may fall into own Rx of band n66.

Thus additional MSD exception should be considered to mitigate the impact of the interference.

### 5.20.2 Receiver Characteristics

#### 5.20.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.20.2.1.1 Power class 2 Case A

Based on co-existence study, additional MSD are specified Table 5.20.2.1.1-1 for this dual connectivity configuration.

Table 5.20.2.1.1-1: MSD test points for SCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

|  |
| --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** |
| **DC****Configuration** | **EUTRA and NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL CLRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_5A\_n66A-n77A | 5 | 826.5 | 5 | 25 | 871.5 | N/A | N/A |
| n66 | 1742 | 5 | 25 | 2142 | 22.2 | IMD3 |
| n77 | 3795 | 10 | 50 | 3795 | N/A | N/A |

#### 5.20.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B configuration are same as the Case A defined in table 5.20.2.1.1-1.

## 5.21 DC\_5A\_n5A-n77A

### 5.21.1 Transmitter Characteristics

#### 5.21.1.1 Maximum Output Power

Table 5.21.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_5A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.21.1.2 Configurations for EN-DC

Table 5.21.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_5A\_n5A-n77A | DC\_5A\_n77A |

#### 5.21.1.3 Co-existence study

According to the co-existence studies performed in the lower order combinations, the Rx impacts are identified as below,

* For UL DC\_5A\_n77A configuration, IMD4 and IMD5 products fall into the band n5 Rx

Thus additional MSD should be considered to mitigate the impact of the interference

### 5.21.2 Receiver Characteristics

#### 5.21.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.21.2.1.1 Power class 2 Case A

Based on co-existence study, additional MSD are specified Table 5.21.2.1.1-1 for this dual connectivity configuration.

Table 5.21.2.1.1-1: MSD test points for SCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NR EN-DC****Configuration** | **NR band** | **UL Fc****(MHz)** | **UL/DL BW****(MHz)** | **UL****CLRB** | **DL Fc (MHz)** | **MSD for PC2****(dB)** | **Duplex mode** | **Source of IMD** |
| DC\_5A\_n5A-n77A11 | 5 | 844 | 5 | 25 | 889 | N/A | FDD | N/A |
| n5 | 844 | 5 | 25 | 889 | 20.3 | FDD | IMD44 |
| n77 | 3421 | 10 | 50 | 3421 | N/A | TDD | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified.NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. |

#### 5.21.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B configuration are same as the Case A defined in table 5.21.2.1.1-1.

## 5.22 DC\_5\_n2-n77

### 5.22.1 Transmitter Characteristics

#### 5.22.1.1 Maximum Output Power

Table 5.22.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_5A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.22.1.2 Configurations for EN-DC

Table 5.22.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_5A\_n2A-n77A | DC\_5A\_n77A |

#### 5.22.1.3 Co-existence study

According to coexistence studies performed in the PC3 DC\_5A\_n2A-n77A configuration, the Rx impacts are identified as below

* For UL DC\_5A\_n77A, IMD3 of 2UL may fall into own Rx of band n2.

Thus additional MSD should be considered to mitigate the impact of the interference for DC\_5A\_n2A-n77A combination.

### 5.22.2 Receiver Characteristics

#### 5.22.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.22.2.1.1 Power class 2 Case A

Based on co-existence study, additional MSD are specified Table 5.22.2.1.1-1 for this dual connectivity configuration.

**Table 5.22.2.1.1-1: MSD test points for SCell due to dual uplink operation for PC2 EN-DC in NR FR1**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD |
| --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc (MHz) | UL/DL BW (MHz) | ULLCRB | DL Fc (MHz) | MSD (dB) | IMD order |
| DC\_5A\_n2A-n77A11 | n2 | 1907 | 5 | 25 | 1987 | 25.5 | IMD3 |
| 5 | 846.5 | 5 | 25 | 891.5 | N/A | N/A |
| n77 | 3680 | 5 | 25 | 3680 | N/A | N/A |
| NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. |

#### 5.22.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B configuratoin are same as the Case A defined in table 5.22.2.1.1-1.

## 5.23 DC\_2\_n66-n77

### 5.23.1 Transmitter Characteristics

#### 5.23.1.1 Maximum Output Power

Table 5.23.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.23.1.2 Configurations for EN-DC

Table 5.23.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_2A\_n66A-n77ADC\_2A-2A\_n66A-n77A | DC\_2A\_n77A |

#### 5.23.1.3 Co-existence study

Based on co-existence specified in 38.101-3 for the configuration,

* For UL DC\_2A\_n77A configuration, IMD2, IMD4 and IMD5 fall into own band n66 Rx.

Thus additional MSD should be considered to mitigate the impact of the interference.

### 5.23.2 Receiver Characteristics

#### 5.23.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.23.2.1.1 Power class 2 Case A

Based on co-existence study, additional MSD are specified Table 5.23.2.1.1-1 for this dual connectivity configuration.

Table 5.23.2.1.1-1: Reference sensitivity exceptions for Scell due to dual uplink operation for DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** |
| --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL****LCRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_2A\_n66A-n77ADC\_2A-2A\_n66A-n77A | 2 | 1855 | 5 | 25 | 1935 | N/A | N/A |
| n66 | 1715 | 5 | 25 | 2115 | 35.2 | IMD2 |
| n77 | 3970 | 10 | 50 | 3970 | N/A | N/A |
| 2 | 1900 | 5 | 25 | 1980 | N/A | N/A |
| n66 | 1760 | 5 | 25 | 2160 | 22.3 | IMD44 |
| n77 | 3540 | 10 | 50 | 3540 | N/A | N/A |
| NOTE 4: This UE channel bandwidth is optional in this release of the specification. |

#### 5.23.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B configuratoin are same as the Case A defined in table 5.23.2.1.1-1.

## 5.24 DC\_2-48\_n77

### 5.24.1 Transmitter Characteristics

#### 5.24.1.1 Maximum Output Power

Table 5.24.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.24.1.2 Configurations for EN-DC

Table 5.24.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_2A-48A\_n77ADC\_2A-48C\_n77ADC\_2A-48D\_n77A | DC\_2A\_n77A |

#### 5.24.1.3 Co-existence study

According to the co-existence studies performed, no IMD issue is identified for this configuration.

### 5.24.2 Receiver Characteristics

#### 5.24.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

There is no additional MSD requirement for this PC2 band combination.

## 5.25 DC\_2A\_n2A-n77A

### 5.25.1 Transmitter Characteristics

#### 5.25.1.1 Maximum Output Power

Table 5.25.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_2A\_n77A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

5.25.1.2 Configurations for EN-DC

Table 5.25.1.2-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DCConfiguration | Uplink EN-DCconfiguration |
| --- | --- |
| DC\_2A\_n2A-n77A | DC\_2A\_n77A |

#### 5.25.1.3 Co-existence study

According to the PC2 coexistence studies performed in the lower order combinations, the Rx impacts are identified as below,

* For UL DC\_2A\_n77A, IMD2, IMD4 and IMD5 products fall into the band n2 Rx

Thus additional MSD should be considered to mitigate the impact of the interference.

### 5.25.2 Receiver Characteristics

#### 5.25.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.25.2.1.1 Power class 2 Case A

Based on co-existence study, additional MSD are specified Table 5.25.2.1.1-1 for this dual connectivity configuration.

Table 5.25.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1

|  |  |  |
| --- | --- | --- |
| **Band / Channel bandwidth / NRB / Duplex mode** |  |  |
| **EN-DC** | **NR band** | **UL Fc** | **UL/DL BW** | **UL** | **DL Fc (MHz)** | **MSD for PC2** | **Duplex mode** | **Source of IMD** |
| **Configuration** | **(MHz)** | **(MHz)** | **CLRB** | **(dB)** |
| DC\_2A\_n2A-n77A | 2 | 1855 | 5 | 25 | 1935 | N/A | FDD | N/A |
| n2 | 1855 | 5 | 25 | 1935 | 32.0 | FDD | IMD2 |
| 34.75 |
| n77 | 3790 | 10 | 50 | 3790 | N/A | TDD | N/A |
| 2 | 1885 | 5 | 25 | 1965 | N/A | FDD | N/A |
| n2 | 1865 | 5 | 25 | 1945 | 20.0 | FDD | IMD44 |
| 22.75 |
| n77 | 3710 | 10 | 50 | 3710 | N/A | TDD | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified.NOTE 5: Applicable only if operation with 4 antenna ports is supported in the band with carrier aggregation configured. |

#### 5.25.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B configuration are same as the Case A defined in table 5.25.2.1.1-1.

## 5.26 DC\_1A-5A\_n78A

### 5.26.1 Transmitter Characteristics

#### 5.26.1.1 Maximum Output Power

Table 5.26.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_aA\_n78A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.26.1.2 Co-existence study

According to the PC3 DC\_1A\_5A-n78A study in 37.863-02-01, the Rx impacts are identified as below,

* Co-existence analysis for DC\_1\_n78 shows that there is IMD4 impact from DC\_1\_n78 UL to Band 1 and IMD5 impact from DC\_1\_n78 UL to Band 5 DL.
* Co-existence analysis for DC\_5\_n78 shows that there is IMD4 impact from DC\_5\_n78 UL to Band 5 DL and IMD3 impact from DC\_5\_n78 UL to Band 1 DL.

Thus, additional MSD for IMD 4 should be considered to mitigate the impact of the interference for PC2 DC\_1A\_5A-n78A combination.

### 5.26.2 Receiver Characteristics

#### 5.26.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.26.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_1A\_5A-n78A are defined in table 5.26.2.2.1-1.

Table 5.26.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

|  |
| --- |
| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD**  |
| **EN-DC Configuration** | **EUTRA and NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL LLRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_1A-5A\_n78A | 1 | 1930 | 5 | 25 | 2120 | 19.2 | IMD4 |
| 5 | 844 | 5 | 25 | 889 | N/A | N/A |
| n78 | 3670 | 10 | 52 | 3670 | N/A | N/A |
| DC\_1A-5A\_n78A | 1 | 1950 | 5 | 25 | 2140 | N/A | N/A |
| 5 | 844 | 5 | 25 | 889 | 19.2 | IMD4 |
| n78 | 3421 | 10 | 52 | 3421 | N/A | N/A |
| DC\_1A-5A\_n78A | 1 | 1932 | 5 | 25 | 2122 | 27.0 |  IMD3 |
| 5 | 829 | 5 | 25 | 874 | N/A | N/A |
| n78 | 3780 | 10 | 52 | 3780 | N/A | N/A |
| DC\_1A-5A\_n78A | 1 | 1975 | 5 | 25 | 2165 | N/A | N/A |
| 5 | 840 | 5 | 25 | 885 | 13.2 | IMD5 |
| n78 | 3405 | 10 | 52 | 3405 | N/A | N/A |

#### 5.26.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_1A\_5A-n78A are the same as the Case A defined in table 5.26.2.1.1-1.

## 5.27 DC\_1A-n7A\_n78A

### 5.27.1 Transmitter Characteristics

#### 5.27.1.1 Maximum Output Power

Table 5.27.1.1-1: Maximum output power for inter-band EN-DC (two bands)

| **EN-DC combination** | Power class 2 (dBm) | Tolerance (dB) |
| --- | --- | --- |
| DC\_aA\_n78A | 266 | +2/-3 |
| NOTE 6: The UE supports PC3 within E-UTRA cell group, and supports either PC3 or PC2 within NR cell group. Power class support within each individual cell group is signalled separately by the UE. |

#### 5.27.1.2 Co-existence study

According to the PC3 DC\_1A\_7A-n78A study in 37.863-02-01, the Rx impacts are identified as below,

* Co-existence analysis for DC\_1\_n78 shows that there is IMD4 impact from DC\_1\_n78 UL to Band 1 and Band 7 DL.
* Co-existence analysis for DC\_7\_n78 shows that there is IMD4 impact from DC\_7\_n78 UL to Band 1 DL.

Thus, additional MSD for IMD 4 should be considered to mitigate the impact of the interference for PC2 DC\_1A\_7A-n78A combination.

### 5.27.2 Receiver Characteristics

#### 5.27.2.1 MSD test points for intermodulation interference due to dual uplink operation for PC2 EN-DC in NR FR1 involving two bands

#### 5.27.2.1.1 Power class 2 Case A

The additional MSD due to intermodulation for PC2 Case A DC\_1A\_7A-n78A are defined in table 5.27.2.2.1-1.

Table 5.27.2.1.1-1: MSD test points for PCell due to dual uplink operation for PC2 EN-DC in NR FR1 (three bands)

|  |
| --- |
| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc (MHz)** | **UL/DL BW (MHz)** | **UL LLRB** | **DL Fc (MHz)** | **MSD (dB)** | **IMD order** |
| DC\_1A-7A\_n78A | 1 | 1930 | 5 | 25 | 2120 | 19.2 | IMD4 |
| 7 | 2550 | 5 | 25 | 2670 | N/A | N/A |
| n78 | 3670 | 10 | 52 | 3670 | N/A | N/A |
| DC\_1A-7A\_n78A | 1 | 1977.5 | 5 | 25 | 2167.5 | N/A | N/A |
| 7 | 2507.5 | 5 | 25 | 2627.5 | 20.2 | IMD4 |
| n78 | 3305 | 10 | 52 | 3305 | N/A | N/A |
| DC\_1A-7A\_n78A | 1 | 1950 | 5 | 25 | 2140 | 19.7 | IMD4 |
| 7 | 2510 | 10 | 50 | 2630 | N/A | N/A |
| n78 | 3580 | 10 | 52 | 3580 | N/A | N/A |

#### 5.27.2.1.2 Power class 2 Case B

The additional MSD due to intermodulation for PC2 Case B DC\_1A\_7A-n78A are the same as the Case A defined in table 5.27.2.1.1-1.

# Annex A - Change history

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Date** | **Meeting** | **TDoc** | **Subject/Comment** | **New version** |
| 2021-04 | 3GPP RAN4#98-bis-e | R4-2105489 | Initial versionImplemented TP’s from RAN4 #98-bis-e:R4-2105351, “TP for TR 37.xxx for DC\_2-5\_n77”, Verizon DenmarkR4-2105352, “TP for TR 37.xxx for DC\_2-13\_n77”, Verizon DenmarkR4-2105353, “TP for TR 37.xxx for DC\_2-66\_n77”, Verizon DenmarkR4-2105354, “TP for TR 37.xxx for DC\_5-66\_n77”, Verizon DenmarkR4-2105355, “TP for TR 37.xxx for DC\_13-66\_n77”, Verizon DenmarkR4-2105356, “TP for TR 37.xxx for DC\_2\_n5-n77”, Verizon DenmarkR4-2105357, “TP for TR 37.xxx for DC\_66\_n2-n77”, Verizon DenmarkR4-2105358, “TP for TR 37.xxx for DC\_66\_n5-n77”, Verizon Denmark | 0.0.1 |
| 2021-08 | 3GPP RAN4#100-e | R4-2113565 | Implemented TP’s from RAN4 #99-e:R4-2108901, TP for TR 37.827 for DC\_2-13\_n66-n77, Verizon DenmarkR4-2108902, TP for TR 37.827 for DC\_2-13-66\_n77, Verizon DenmarkR4-2108903, TP for TR 37.827 for DC\_13-66\_n2-n77, Verizon DenmarkR4-2108904, TP for TR 37.827 for DC\_2-66\_n5-n77, Verizon DenmarkR4-2108905, TP for TR 37.827 for DC\_2-5-66\_n77, Verizon DenmarkR4-2107837, TP for TR 37.827 for DC\_13\_n66-n77, Verizon DenmarkR4-2107838, TP for TR 37.827 for DC\_13\_n2-n77, Verizon DenmarkR4-2110957, TP for PC2 DC\_2\_66-n41, Huawei Tech.(UK) Co.. Ltd | 0.1.0 |
| 2021-08 | 3GPP RAN4#100-e | R4-2113566 | Implemented TP’s from RAN4 #100-e:R4-2112669, TP for TR 37.827 for DC\_66\_n66-n77, Verizon, SamsungR4-2112670, TP to TR 37.717-21-11 for DC\_48-66\_n77, Verizon, SamsungR4-2112672 TP for TR 37.827 for DC\_13\_n5-n77, Verizon, SamsungR4-2112673, TP for TR 37.827 for DC\_5\_n66-n77, Verizon, SamsungR4-2114940 TP for TR 37.827 for DC\_5\_n5-n77, Verizon, SamsungR4-2114941 TP for TR 37.827 for DC\_5\_n2-n77, Verizon, SamsungR4-2112679, TP for TR 37.827 for DC\_2\_n66-n77, Verizon, SamsungR4-2112681, TP for TR 37.827 for DC\_2-48\_n77, Verizon, SamsungR4-2114942, TP for TR 37.827 for DC\_2\_n2-n77, Verizon, SamsungR4-2114043, Text proposal for TR 37.827 to include DC\_1A-5A\_n78A, Huawei Tech.(UK) Co.. LtdR4-2114054, Text proposal for TR 37.827 to include DC\_1A-n7A\_n78A, Huawei Tech.(UK) Co.. Ltd | 0.2.0 |