|  |  |
| --- | --- |
| 3GPP TR 37.717-21-11 V0.8.0 (2022-03) | |
| Technical Report | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Networks;  Dual Connectivity of 2 bands LTE inter-band CA and 1 NR band (Release 17) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 9

1 Scope 11

2 References 11

3 Definitions of terms, symbols and abbreviations 11

3.1 Terms 11

3.2 Symbols 11

3.3 Abbreviations 12

4 Background 12

4.1 TR Maintenance 12

5 DC of 2 bands LTE inter-band CA and 1 NR band within FR1: Specific Band Combination Part 12

5.x DC\_a-b\_nc 12

5.x.1 Configurations for DC 12

5.x.2 Co-existence studies 12

5.x.3 ∆TIB and ∆RIB values 12

5.x.4 Reference sensitivity exceptions 13

5.1 DC\_3-19\_n1 13

5.1.1 Configurations for DC 13

5.1.2 Co-existence studies 13

5.1.3 ∆TIB and ∆RIB values 13

5.1.4 Reference sensitivity exceptions 14

5.2 DC\_3-21\_n1 14

5.2.1 Configurations for DC 14

5.2.2 Co-existence studies 14

5.2.3 ∆TIB and ∆RIB values 14

5.2.4 Reference sensitivity exceptions 15

5.3 DC\_3-42\_n1 15

5.3.1 Configurations for DC 15

5.3.2 Co-existence studies 15

5.3.3 ∆TIB and ∆RIB values 15

5.3.4 Reference sensitivity exceptions 16

5.4 DC\_19-21\_n1 16

5.4.1 Configurations for DC 16

5.4.2 Co-existence studies 16

5.4.3 ∆TIB and ∆RIB values 16

5.4.4 Reference sensitivity exceptions 17

5.5 DC\_19-42\_n1 17

5.5.1 Configurations for DC 17

5.5.2 Co-existence studies 17

5.5.3 ∆TIB and ∆RIB values 17

5.5.4 Reference sensitivity exceptions 18

5.6 DC\_21-42\_n1 18

5.6.1 Configurations for DC 18

5.6.2 Co-existence studies 18

5.6.3 ∆TIB and ∆RIB values 18

5.6.4 Reference sensitivity exceptions 19

5.7 DC\_1-32\_n28 19

5.7.1 Configurations for DC 19

5.7.2 Co-existence studies 20

5.7.3 ∆TIB and ∆RIB values 21

5.7.4 Reference sensitivity exceptions 21

5.7.5 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1 21

5.8 DC\_7-32\_n28 22

5.8.1 Configurations for DC 22

5.8.2 Co-existence studies 22

5.8.3 ∆TIB and ∆RIB values 24

5.8.4 Reference sensitivity exceptions 24

5.8.5 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1 24

5.9 DC\_7-32\_n78 25

5.9.1 Configurations for DC 25

5.9.2 Co-existence studies 25

5.9.3 ∆TIB and ∆RIB values 27

5.9.4 Reference sensitivity exceptions 27

5.10 DC\_20-32\_n28 28

5.10.1 Configurations for DC 28

5.10.2 Co-existence studies 28

5.10.3 ∆TIB and ∆RIB values 29

5.10.4 Reference sensitivity exceptions 30

5.10.5 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1 30

5.11 DC\_2-48\_n5 30

5.11.1 Configurations for DC 30

5.11.2 Co-existence studies 30

5.11.3 ∆TIB and ∆RIB values 30

5.11.4 Reference sensitivity exceptions 31

5.12 DC\_5-48\_n12 31

5.12.1 Configurations for DC 31

5.12.2 Co-existence studies 31

5.12.3 ∆TIB and ∆RIB values 31

5.12.4 Reference sensitivity exceptions 32

5.13 DC\_5-48\_n71 32

5.13.1 Configurations for DC 32

5.13.2 Co-existence studies 32

5.13.3 ∆TIB and ∆RIB values 32

5.13.4 Reference sensitivity exceptions 33

5.14 DC\_12-48\_n5 33

5.14.1 Configurations for DC 33

5.14.2 Co-existence studies 33

5.14.3 ∆TIB and ∆RIB values 33

5.14.4 Reference sensitivity exceptions 34

5.15 DC\_3\_(n)41 34

5.15.1 Configuration for DC 34

5.15.3 ∆TIB and ∆RIB values 34

5.15.4 REFSENS requirements 34

5.16 DC\_2A-48A\_n48A 35

5.16.2 Co-existence studies 35

5.17 DC\_48-66A\_n25A 35

5.17.2 Co-existence studies 36

5.18 DC\_48A-66A\_n48A 37

5.18.2 Co-existence studies 37

5.19 DC\_3-8\_n40 37

5.19.2 Co-existence studies 38

5.20 DC\_3-28\_n1 38

5.20.2 Co-existence studies 39

5.21 DC\_7-8\_n40 40

5.21.2 Co-existence studies 40

5.22 DC\_7-28\_n1 40

5.22.2 Co-existence studies 41

5.23 DC\_7-66\_n5 42

5.23.1 Configurations for DC 42

5.23.2 Co-existence studies 42

5.23.3 ∆TIB and ∆RIB values 44

5.23.4 Reference sensitivity exceptions 44

5.24 DC\_2-7\_n5 45

5.24.1 Configurations for DC 45

5.24.2 Co-existence studies 45

5.24.3 ∆TIB and ∆RIB values 47

5.24.4 Reference sensitivity exceptions 48

5.25 DC\_1-40\_n78 48

5.26 DC\_3-40\_n78 50

5.27 DC\_7-40\_n78 51

5.28 DC\_8-40\_n78 53

5.29 DC\_2-4\_n28 54

5.30 DC\_2-7\_n28 55

5.31 DC\_2-66\_n28 57

5.32 DC\_4-7\_n28 58

5.33 DC\_5-7\_n66 59

5.34 DC\_7-66\_n28 60

5.35 DC\_1-11\_n28 61

5.36 DC\_3-11\_n28 63

5.37 DC\_8-11\_n28 63

5.38 DC\_3-11\_n77 64

5.39.2 Configuration for DC 66

5.40.2 Configuration for DC 67

5.41.2 Configuration for DC 68

5.42.2 Configuration for DC 69

5.43.2 Configuration for DC 70

5.44 DC\_7-8\_n28 70

5.45 DC\_20-28\_n3 74

5.46 DC\_28-66\_n66 78

5.47 DC\_7-28\_n66 80

5.48 DC\_2-28\_n66 84

5.49 Void 88

5.50 Void 88

5.51 DC\_8-40\_n1 88

5.52 DC\_1-32\_n3 92

5.53 DC\_3-32\_n1 94

5.54 DC\_7-32\_n1 97

5.54.1 Configurations for DC 97

5.54.2 Co-existence studies 97

5.54.3 ∆TIB and ∆RIB values 98

5.54.4 Reference sensitivity exceptions 99

5.55 DC\_2-66\_n7 99

5.56 DC\_2-5\_n7 100

5.57 DC\_2-8\_n2 101

5.58 DC\_5-66\_n7 102

5.59 DC\_20-32\_n1 103

5.60 DC\_20-32\_n3 104

5.61 DC\_1-3\_n3 104

5.61.1 Configuration for DC 104

5.61.3 ∆TIB and ∆RIB values 105

5.61.4 REFSENS requirements 105

5.62 DC\_1-41\_n3 105

5.62.1 Configuration for DC 105

5.62.3 ∆TIB and ∆RIB values 105

5.62.4 REFSENS requirements 106

5.63 DC\_3-18\_n3 106

5.63.1 Configuration for DC 106

5.63.3 ∆TIB and ∆RIB values 106

5.63.4 REFSENS requirements 107

5.64 DC\_3-41\_n3 107

5.64.1 Configuration for DC 107

5.64.3 ∆TIB and ∆RIB values 107

5.64.4 REFSENS requirements 108

5.65 Void 108

5.66 DC\_7-66\_n77 and DC\_7-7-66\_n77 108

5.66.1 Configuration for DC 108

5.66.3 ∆TIB and ∆RIB values 109

5.66.4 REFSENS requirements 109

5.67 DC\_2-5\_n48 109

5.67.1 Configuration for DC 109

5.67.3 ∆TIB and ∆RIB values 110

5.67.4 REFSENS requirements 110

5.68 DC\_2-13\_n48 110

5.68.1 Configuration for DC 110

5.68.3 ∆TIB and ∆RIB values 111

5.68.4 REFSENS requirements 111

5.69 Void 111

5.70 DC\_5-46\_n66 111

5.70.1 Configuration for DC 111

5.70.3 ∆TIB and ∆RIB values 112

5.70.4 REFSENS requirements 112

5.71 DC\_5-66\_n48 and DC\_5-66-66\_n48 112

5.71.1 Configuration for DC 112

5.71.3 ∆TIB and ∆RIB values 113

5.71.4 REFSENS requirements 113

5.72 DC\_5-66\_n77 113

5.72.1 Configuration for DC 113

5.72.3 ∆TIB and ∆RIB values 114

5.72.4 REFSENS requirements 114

5.73 DC\_1-42\_n3 114

5.74 DC\_8-42\_n3 115

5.75 DC\_3-18\_n28 117

5.75.1 Configurations for DC 117

5.75.2 Co-existence studies 117

5.75.3 ∆TIB and ∆RIB values 117

5.75.4 Reference sensitivity exceptions 117

5.76 DC\_2-66\_n77 118

5.76.4 Reference sensitivity exceptions 120

5.77 DC\_2-48\_n77 121

5.77.4 Reference sensitivity exceptions 123

5.78 DC\_2-13\_n77 123

5.78.4 Reference sensitivity exceptions 125

5.79 DC\_2-5\_n77 126

5.79.4 Reference sensitivity exceptions 128

5.80 DC\_5-13\_n66 129

5.80.4 Reference sensitivity exceptions 131

5.81 DC\_13-66\_n77 131

5.82 DC\_13-66\_n5 134

5.82.4 Reference sensitivity exceptions 136

5.83 DC\_1-18\_n28 137

5.83.1 Configurations for DC 137

5.83.2 Co-existence studies 137

5.83.3 ∆TIB and ∆RIB values 137

5.83.4 Reference sensitivity exceptions 137

5.84 DC\_1-18\_n41 138

5.84.1 Configurations for DC 138

5.84.2 Co-existence studies 138

5.84.3 ∆TIB and ∆RIB values 138

5.84.4 Reference sensitivity exceptions 138

5.85 DC\_5-7\_n7 139

5.85.2 Co-existence studies 139

5.86 DC\_2-28\_n7 140

5.86.2 Co-existence studies 140

5.87 DC\_28-66\_n7 141

5.87.2 Co-existence studies 141

5.88 DC\_7-28\_n2 142

5.88.2 Co-existence studies 142

5.89 DC\_2-7\_n7 143

5.89.2 Co-existence studies 143

5.90 DC\_2A-71A\_n71A 144

5.90.2 Co-existence studies 144

5.91 DC\_66A-71A\_n71A 145

5.91.2 Co-existence studies 145

5.92 DC\_7-66\_n7/ DC\_7-66-66\_n7 145

5.93 DC\_2-7\_n77 148

5.93.1 Configurations for DC 148

5.93.2 Co-existence studies 148

5.93.3 ∆TIB and ∆RIB values 150

5.93.4 Reference sensitivity exceptions 151

5.94 Void 151

5.95 DC\_20-40\_n78 151

5.96 DC\_3-18\_n41 153

5.96.1 Configurations for DC 153

5.96.2 Co-existence studies 153

5.96.3 ∆TIB and ∆RIB values 153

5.96.4 Reference sensitivity exceptions 154

5.97 DC\_7-25\_n77 154

5.97.2 Co-existence studies 154

5.97.3 ∆TIB and ∆RIB values 156

5.97.4 Reference sensitivity exceptions 157

5.98 DC\_7-25\_n78 157

5.98.2 Co-existence studies 157

5.98.3 ∆TIB and ∆RIB values 159

5.98.4 Reference sensitivity exceptions 160

5.99 DC\_25-66\_n77 160

5.99.2 Co-existence studies 160

5.99.3 ∆TIB and ∆RIB values 162

5.99.4 Reference sensitivity exceptions 163

5.100 DC\_25-66\_n78 163

5.100.2 Co-existence studies 163

5.100.3 ∆TIB and ∆RIB values 165

5.100.4 Reference sensitivity exceptions 166

5.101 DC\_2-29\_n78 166

5.102 DC\_29-66\_n78 168

5.103 DC\_1-21\_n28 169

5.103.1 Configurations for DC 169

5.103.2 Co-existence studies 170

5.103.3 ∆TIB and ∆RIB values 170

5.103.4 Reference sensitivity exceptions 170

5.104 DC\_3-21\_n28 171

5.104.1 Configurations for DC 171

5.104.2 Co-existence studies 171

5.104.3 ∆TIB and ∆RIB values 171

5.104.4 Reference sensitivity exceptions 171

5.105 DC\_8-20\_n1 172

5.105.1 Configurations for DC 172

5.105.2 Co-existence studies 172

5.105.3 ∆TIB and ∆RIB values 175

5.105.4 Reference sensitivity exceptions 175

5.106 DC\_8-20\_n3 176

5.106.1 Configurations for DC 176

5.106.2 Co-existence studies 176

5.106.3 ∆TIB and ∆RIB values 179

5.106.4 Reference sensitivity exceptions 179

5.107 DC\_8-32\_n1 179

5.107.1 Configurations for DC 179

5.107.2 Co-existence studies 180

5.107.3 ∆TIB and ∆RIB values 181

5.107.4 Reference sensitivity exceptions 181

5.108.2 Configuration for DC 182

5.109.2 Configuration for DC 183

5.110.2 Configuration for DC 184

5.111.2 Configuration for DC 185

5.112.2 Configuration for DC 186

5.113.2 Configuration for DC 187

5.114.2 Configuration for DC 188

5.115.2 Configuration for DC 189

5.116.2 Configuration for DC 190

5.117.2 Configuration for DC 191

Annex A (informative): Change history 193

# Foreword

This Technical Report has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The present document is a technical report for Dual Connectivity of 2 bands LTE inter-band CA (2DL/1UL) and 1 NR band (1DL/1UL) under Rel-17 time frame. The purpose is to gather the relevant background information and studies in order to address Dual connectivity (DC) band combinations of 3 different bands DL with 2 different bands UL (2 different LTE bands and 1 NR band) for the Rel-17 band combinations. The actual requirements are added to the corresponding technical specification.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

…

[x] <doctype> <#>[ ([up to and including]{yyyy[-mm]|V<a[.b[.c]]>}[onwards])]: "<Title>".

It is preferred that the reference to 21.905 be the first in the list.

# 3 Definitions of terms, symbols and abbreviations

This clause and its three subclauses are mandatory. The contents shall be shown as "void" if the TS/TR does not define any terms, symbols, or abbreviations.

## 3.1 Terms

For the purposes of the present document, the terms given in 3GPP TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in 3GPP TR 21.905 [1].

Definition format (Normal)

**<defined term>:** <definition>.

**example:** text used to clarify abstract rules by applying them literally.

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

Symbol format (EW)

<symbol> <Explanation>

## 3.3 Abbreviations

For the purposes of the present document, the abbreviations given in 3GPP TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in 3GPP TR 21.905 [1].

Abbreviation format (EW)

<ABBREVIATION> <Expansion>

# 4 Background

The present document is a technical report for Dual Connectivity (EN-DC) of 2 bands LTE inter-band CA and 1 NR band under Rel-17 timeframe. The document covers each band combination specific issues (i.e. one sub-clause defined per band combination)

## 4.1 TR Maintenance

A single company is responsible for introducing all approved TPs in the current TR, i.e. TR editor. However, it is the responsibility of the contact person of each band combination to ensure that the TPs related to the band combination have been implemented.

# 5 DC of 2 bands LTE inter-band CA and 1 NR band within FR1: Specific Band Combination Part

## 5.x DC\_a-b\_nc

### 5.x.1 Configurations for DC

*<Editor’s note: it is required to use the same table format as in TS 38.101-3>*

Table 5.x.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
|  |  |

### 5.x.2 Co-existence studies

*<Text will be added.>*

### 5.x.3 ∆TIB and ∆RIB values

*<Editor’s note: it is required to use the same table format as in TS 38.101-3>*

Table 5.X.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
|  |  |  |
|  |  |
|  |  |

**Table 5.X.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
|  |  |  |
|  |  |
|  |  |

### 5.x.4 Reference sensitivity exceptions

< Editor’s note: text will be added only for reference sensitivity exceptions for intermodulation interference due to dual uplink operation for DC in NR FR1 involving three bands >

## 5.1 DC\_3-19\_n1

### 5.1.1 Configurations for DC

Table 5.1.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-19A\_n1A | DC\_3A\_n1A  DC\_19A\_n1A |

### 5.1.2 Co-existence studies

Based on co-existence studies of DC\_3\_n1 and DC\_19\_n1, own Rx impact of the 3rd band is the followings.

- IMD generated by DC\_3\_n1 uplink doesn’t fall into own Rx of band 19.

- IMD generated by DC\_19\_n1 uplink doesn’t fall into own Rx of band 3.

### 5.1.3 ∆TIB and ∆RIB values

For DC\_3-19\_n1, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_1-3-19, and are given in the tables below.

Table 5.1.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-19\_n1 | 3 | 0.3 |
| 19 | 0.3 |
| n1 | 0.3 |

**Table 5.1.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-19\_n1 | 3 | 0 |
| 19 | 0 |
| n1 | 0 |

### 5.1.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.2 DC\_3-21\_n1

### 5.2.1 Configurations for DC

Table 5.2.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-21A\_n1AX1,X2 | DC\_3A\_n1A  DC\_21A\_n1A |
| NOTE X1: The frequency range in band n1 is restricted for this band combination to 1940 - 1960 MHz for the UL and 2130-2150 MHz for the DL.  NOTE X2: The frequency range in band 3 is restricted for this band combination to 1765 - 1785 MHz for the UL and 1860-1880 MHz for the DL. | |

### 5.2.2 Co-existence studies

Based on co-existence studies of DC\_3\_n1 and DC\_21\_n1, own Rx impact of the 3rd band is the followings.

- 3rd order IMD products generated by DC\_3\_n1 uplink may fall into own Rx of band 21.

- 5th order IMD products generated by DC\_3\_n1 uplink may fall into own Rx of band 21.

- IMD generated by DC\_21\_n1 uplink doesn’t fall into own Rx of band 3.

### 5.2.3 ∆TIB and ∆RIB values

For DC\_3-21\_n1, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_1-3-21, and are given in the tables below.

Table 5.2.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-21\_n1 | 3 | 0.8 |
| 21 | 0.9 |
| n1 | 0.3 |

**Table 5.2.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-21\_n1 | 3 | 0.3 |
| 21 | 0.5 |
| n1 | 0 |

### 5.2.4 Reference sensitivity exceptions

When LTE CA 1-3-21 was introduced, IMD was calculated based on the frequency range that the operator actually owned, which resulted in that IMD3 and IMD5 doesn’t fall into own Rx of band 21. Therefore, there is no need to have MSD added. NOTE X1 and NOTE X2 in Table 5.2.1-1 indicate these frequency ranges.

## 5.3 DC\_3-42\_n1

### 5.3.1 Configurations for DC

Table 5.3.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-42A\_n1A | DC\_3A\_n1A  DC\_42A\_n1A |
| DC\_3A-42C\_n1A | DC\_3A\_n1A  DC\_42A\_n1A |

### 5.3.2 Co-existence studies

Based on co-existence studies of DC\_3\_n1 and DC\_42\_n1, own Rx impact of the 3rd band is the followings.

- 4th order IMD products generated by DC\_3\_n1 uplink may fall into own Rx of band 42.

- IMD generated by DC\_42\_n1 uplink doesn’t fall into own Rx of band 3.

### 5.3.3 ∆TIB and ∆RIB values

For DC\_3-42\_n1, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_1-3-42, and are given in the tables below.

Table 5.3.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-42\_n1 | 3 | 0.6 |
| 42 | 0.8 |
| n1 | 0.6 |

**Table 5.3.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-42\_n1 | 3 | 0.2 |
| 42 | 0.5 |
| n1 | 0.2 |

### 5.3.4 Reference sensitivity exceptions

As mentioned above, IMD4 of B3 and n1 to Band 42 Rx need to be addressed for REFSENS relaxation. For DC\_3-42\_n1, REFSENS exceptions are reused from the LTE combination CA\_1-3-42, and are given in the tables below.

Table 5.3.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_3A-42A\_n1A  DC\_3A-42C\_n1A | 3 | 1782.5 | 5 | 25 | 1877.5 | N/A | N/A |
| 42 | 3425 | 5 | 25 | 3425 | 13.0 | IMD4 |
| n1 | 1922.5 | 5 | 25 | 2112.5 | N/A | N/A |

## 5.4 DC\_19-21\_n1

### 5.4.1 Configurations for DC

Table 5.4.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_19A-21A\_n1A | DC\_19A\_n1A  DC\_21A\_n1A |

### 5.4.2 Co-existence studies

Based on co-existence studies of DC\_19\_n1 and DC\_21\_n1, own Rx impact of the 3rd band is the followings.

- IMD generated by DC\_19\_n1 uplink doesn’t fall into own Rx of band 21.

- IMD generated by DC\_21\_n1 uplink doesn’t fall into own Rx of band 19.

### 5.4.3 ∆TIB and ∆RIB values

For DC\_19-21\_n1, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_1-19-21, and are given in the tables below.

Table 5.4.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_19-21\_n1 | 19 | 0.3 |
| 21 | 0.4 |
| n1 | 0.3 |

**Table 5.4.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_19-21\_n1 | 19 | 0 |
| 21 | 0 |
| n1 | 0 |

### 5.4.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.5 DC\_19-42\_n1

### 5.5.1 Configurations for DC

Table 5.5.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_19A-42A\_n1AX1,X3 | DC\_19A\_n1A  DC\_42A\_n1A |
| DC\_19A-42C\_n1 AX1,X3 | DC\_19A\_n1A  DC\_42A\_n1A |
| NOTE X1: The frequency range in band n1 is restricted for this band combination to 1940 - 1960 MHz for the UL and 2130-2150 MHz for the DL.  NOTE X3: The frequency range in band 42 is restricted for this band combination to 3440 - 3520 MHz. | |

### 5.5.2 Co-existence studies

Based on co-existence studies of DC\_19\_n1 and DC\_42\_n1, own Rx impact of the 3rd band is the followings.

- 3rd order IMD products generated by DC\_19\_n1 uplink may fall into own Rx of band 42.

- 5th order IMD products generated by DC\_42\_n1 uplink may fall into own Rx of band 19.

### 5.5.3 ∆TIB and ∆RIB values

For DC\_19-42\_n1, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_1-19-42, and are given in the tables below.

Table 5.5.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_19-42\_n1 | 19 | 0.3 |
| 42 | 0.8 |
| n1 | 0.3 |

**Table 5.5.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_19-42\_n1 | 19 | 0 |
| 42 | 0.5 |
| n1 | 0 |

### 5.5.4 Reference sensitivity exceptions

When LTE CA 1-19-42 was introduced, IMD was calculated based on the frequency range that the operator actually owned, which resulted in that IMD3 doesn’t fall into own Rx of band 42 and IMD5 doesn’t fall into own Rx of band 19. Therefore, there is no need to have MSD added. NOTE X1 and NOTE X3 in Table 5.5.1-1 indicate these frequency ranges.

## 5.6 DC\_21-42\_n1

### 5.6.1 Configurations for DC

Table 5.6.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_21A-42A\_n1AX1,X3 | DC\_21A\_n1A  DC\_42A\_n1A |
| DC\_21A-42C\_n1 AX1,X3 | DC\_21A\_n1A  DC\_42A\_n1A |
| NOTE X1: The frequency range in band n1 is restricted for this band combination to 1940 - 1960 MHz for the UL and 2130-2150 MHz for the DL.  NOTE X3: The frequency range in band 42 is restricted for this band combination to 3440 - 3520 MHz. | |

### 5.6.2 Co-existence studies

Based on co-existence studies of DC\_21\_n1 and DC\_42\_n1, own Rx impact of the 3rd band is the followings.

- 2nd order IMD products generated by DC\_21\_n1 uplink may fall into own Rx of band 42.

- 2nd order IMD products generated by DC\_42\_n1 uplink may fall into own Rx of band 21.

### 5.6.3 ∆TIB and ∆RIB values

For DC\_21-42\_n1, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_1-21-42, and are given in the tables below.

Table 5.6.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_21-42\_n1 | 21 | 0.4 |
| 42 | 0.8 |
| n1 | 0.3 |

**Table 5.6.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_21-42\_n1 | 21 | 0 |
| 42 | 0.5 |
| n1 | 0 |

### 5.6.4 Reference sensitivity exceptions

When LTE CA 1-21-42 was introduced, IMD was calculated based on the frequency range that the operator actually owned, which resulted in that IMD2 doesn’t fall into own Rx of band 42. Therefore, we didn’t specify MSD for band 42. NOTE X1 and NOTE X3 in Table 5.6.1-1 indicate these frequency ranges.

IMD2 of B42 and n1 to Band 21 Rx need to be addressed for REFSENS relaxation. For DC\_21-42\_n1, REFSENS exceptions are reused from DC\_1-11\_n78, already defined in TS 38.101-3, due to similarity in frequency range.

Table 5.6.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_21A-42A\_n1A | 21 | 1452 | 5 | 25 | 1500 | 31.4 | IMD2 |
| 42 | 3450 | 10 | 50 | 3450 | N/A | N/A |
| n1 | 1950 | 5 | 25 | 2140 | N/A | N/A |

## 5.7 DC\_1-32\_n28

### 5.7.1 Configurations for DC

Table 5.7.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-32A\_n28A | DC\_1A\_n28A |

### 5.7.2 Co-existence studies

Table 5.7.2-1 lists the Band 1A + Band n28A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.7.2-1: Band 1 and Band n28 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 1920 | 1980 | | 703 | 748 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 3840 – 3960 | | | 1406 – 1496 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 5760 – 5940 | | | 2109 – 2244 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1172 – 1277 | | | 2623 – 2728 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 3092 – 3257 | | | 424 – 574 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 4543 – 4708 | | | 3326 – 3476 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 1890 – 2010 | | | 683 – 768 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5012 – 5237 | | | 129 – 324 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| |  | |  |
| IMD frequency limits (MHz) | 2344 – 2554 | | |  | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6463 – 6688 | | | 4029 – 4224 | | |
| Two-tone 4th order IMD products | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |  | |  |
| IMD frequency limits (MHz) | 5246 – 5456 | | |  | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 832 – 1072 | | | 6932 – 7217 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1596 – 1851 | | | 4264 – 4534 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4732 – 4972 | | | 8383 – 8668 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5949 – 6204 | | | 7166 – 7436 | | |

Based on Table 5.7.2-1,

- 2nd order harmonics may fall into the Rx of bands 11, 21, 32, 45, 46, 47, 75 and 76

- 3rd order harmonics may fall into the Rx frequencies of bands 1, 4, 10, 23, 65, 66 and 77

- 2nd order IMD may fall into Rx frequencies of bands 7 and 41

- 3rd order IMD may fall into Rx frequencies of bands 31, 42 and 77

- 4th order IMD may fall into Rx of bands 30, 40, 41, 46, 46 and 77

- 5th order IMD may fall into Rx frequencies of bands 3, 5, 6, 8, 9, 18, 19, 26, 27 and 35

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.7.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.7.2-2: 2UL Band 1 + Band n28 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD 5 |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD4 |
| 2400 | - | 2494 | Yes | Asia | IMD4 |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | Harmonic 3, IMD 4 |
| 5150 | - | 5350 | Yes | Europe | IMD 4 |
| 5470 | - | 5725 | Yes | IMD 4 |
| 5150 | - | 5825 | Yes | Asia | Harmonic 3, IMD 4 |

The requirements for coexistence with protected bands (including band 32) exist for DC\_1A\_n28A in 38101-3.

### 5.7.3 ∆TIB and ∆RIB values

Table 5.7.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1A-32A\_n28 | 1 | 0.3 |
| n28 | 0.7 |

**Table 5.7.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1A-32A\_n28 | 1 | 0 |
| 32 | 0 |
| n28 | 0.2 |

### 5.7.4 Reference sensitivity exceptions

No additional exceptions for IMD are required.

### 5.7.5 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1

The entries in tables 5.7.5-1 and 5.7.5-2 are to be added to TS38101-3 tables 7.3B.2.3.1-1 and 7.3B.2.3.1-2 respectively.

**Table 5.7.5-1: Reference sensitivity exceptions (MSD) due to UL harmonic for EN-DC in NR FR1**

| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| UL band | DL band | 5 MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 30 MHz (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n28 | 32 | 28.1 | 25.3 | 24.0 | 22.8 |  |  |  |  |  |  |  |  |

**Table 5.7.5-2: Uplink configuration for reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / UL RB allocation of the aggressor band | | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 30 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n28 | 32 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |

## 5.8 DC\_7-32\_n28

### 5.8.1 Configurations for DC

Table 5.8.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-32A\_n28A | DC\_7A\_n28A |

### 5.8.2 Co-existence studies

Table 5.8.2-1 lists the Band 7A + Band n28A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.8.2-1: Band 7 and Band n28 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2500 | 2570 | | 703 | 748 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5000 – 5140 | | | 1406 – 1496 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7500 – 5940 | | | 2109 – 2244 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1752 – 1867 | | | 3203 – 3318 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 4252 – 4437 | | | 1074 – 1164 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 5703 – 5888 | | | 3906 – 4066 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2470 – 2600 | | | 683 – 768 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 6752 – 7007 | | | 256 – 461 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| |  | |  |
| IMD frequency limits (MHz) | 3504 – 3734 | | |  | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 8203 – 8458 | | | 4029 – 4224 | | |
| Two-tone 4th order IMD products | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |  | |  |
| IMD frequency limits (MHz) | 6406 – 6636 | | |  | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 242 – 492 | | | 6932 – 7217 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 2756 – 3031 | | | 4264 – 4534 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5312 – 5562 | | | 8383 – 8668 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7109 – 7384 | | | 8906 – 9206 | | |

Based on Table 5.8.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 11, 21, 32, 45, 75 and 76

- 3rd order harmonics may fall into Rx frequencies of bands 1, 4, 10, 23, 65 and 66

- 2nd order IMD may fall into Rx frequencies of bands 3, 9, 35 and 77

- 3rd order IMD may fall into Rx frequencies of bands 46, 47 and 77

- 4th order IMD may fall into Rx frequencies of bands 22, 42, 43, 48 and 77

- 5th order IMD may fall into Rx frequencies of bands 31 and 46

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.8.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.8.2-2: 2UL Band 7 + Band n28 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD3 |
| 2400 | - | 2494 | Yes | Asia | IMD3 |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | IMD3, IMD5 |
| 5150 | - | 5350 | Yes | Europe | IMD 5 |
| 5470 | - | 5725 | Yes | IMD3, IMD5 |
| 5150 | - | 5825 | Yes | Asia | IMD3, IMD5 |

The requirements for coexistence with protected bands, excluding band 32, exist for DC\_7A\_n28A in 38101-3.

### 5.8.3 ∆TIB and ∆RIB values

Table 5.8.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n28 | 7 | 0.3 |
| n28 | 0.7 |

**Table 5.8.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n28 | 7 | 0 |
| 32 | 0 |
| n28 | 0.2 |

### 5.8.4 Reference sensitivity exceptions

The entries in tables 5.8.4-1 and 5.8.4-2 are to be added to TS38101-3 tables 7.3B.2.3.1-1 and 7.3B.2.3.1-2 respectively.

**Table 5.8.4-1: Reference sensitivity exceptions (MSD) due to UL harmonic for EN-DC in NR FR1**

| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| UL band | DL band | 5 MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 30 MHz (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n28 | 32 | 28.1 | 25.3 | 24.0 | 22.8 |  |  |  |  |  |  |  |  |

**Table 5.8.4-2: Uplink configuration for reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / UL RB allocation of the aggressor band | | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 30 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n28 | 32 | 12 | 25 | 25 | 25 |  |  |  |  |  |  |  |  |

### 5.8.5 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1

The entries in tables 5.8.5-1 and 5.8.5-2 are to be added to TS38101-3 tables 7.3B.2.3.1-1 and 7.3B.2.3.1-2 respectively.

**Table 5.8.5-1: Reference sensitivity exceptions (MSD) due to UL harmonic for EN-DC in NR FR1**

| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| UL band | DL band | 5 MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 30 MHz (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n28 | 32 | 28.1 | 25.3 | 24.0 | 22.8 |  |  |  |  |  |  |  |  |

**Table 5.8.5-2: Uplink configuration for reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / UL RB allocation of the aggressor band | | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 30 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n28 | 32 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |

## 5.9 DC\_7-32\_n78

### 5.9.1 Configurations for DC

Table 5.9.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-32A\_n78A | DC\_7A\_n78A |

### 5.9.2 Co-existence studies

Table 5.9.2-1 list the Band 7A + Band n78A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.9.2-1: Band 7 and Band n78 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2500 | 2570 | | 3300 | 3800 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5000 – 5140 | | | 6600 – 7600 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7500 – 7710 | | | 9900 – 11400 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 730 – 1300 | | | 5800 – 6370 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 1200 – 1840 | | | 4030 – 5030 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 8300 – 8940 | | | 9100 – 10170 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2400 – 2670 | | | 3280 – 3820 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 3700 – 4410 | | | 7330 – 8900 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| |  | |  |
| IMD frequency limits (MHz) | 1460 – 2600 | | |  | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 10800 – 11510 | | | 4029 – 4224 | | |
| Two-tone 4th order IMD products | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |  | |  |
| IMD frequency limits (MHz) | 11600 – 12740 | | |  | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 10630 – 12700 | | | 6932 – 7217 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 4760 – 6400 | | | 4264 – 4534 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 15700 – 17770 | | | 8383 – 8668 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 14900 – 16540 | | | 14100 – 15310 | | |

Based on Table 5.9.2-1,

- 2nd order IMD may fall into Rx frequencies of bands 5, 6, 8, 12, 13, 14, 17, 18, 19, 20, 26, 27, 28, 44, 46, 47, 67 and 68

- 3rd order IMD may fall into Rx frequencies of bands 3, 11, 21, 24, 32, 45, 75, 76 and 77

- 4th order IMD may fall into Rx frequencies of bands 1, 2, 3, 4, 9, 10, 11, 21, 23, 24, 25, 30, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 43, 45, 65, 66, 69, 70, 75 and 77

- 5th order IMD may fall into Rx frequencies of bands 5, 6, 8, 12, 13, 14, 17, 18, 19, 20, 26, 27, 28, 29, 31, 44, 46, 47, 67 and 68

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.9.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.9.2-2: 2UL Band 7 + Band n78 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD3, IMD4 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD3, IMD4 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD3, IMD4 |
| GPS | 1563 | - | 1587 | Yes |  | IMD3, IMD4 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD3, IMD4 |
| 2400 | - | 2494 | Yes | Asia | IMD3, IMD4 |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | IMD3, IMD5 |
| 5150 | - | 5350 | Yes | Europe | IMD5 |
| 5470 | - | 5725 | Yes | IMD5 |
| 5150 | - | 5825 | Yes | Asia | IMD2, IMD5 |

The requirements for coexistence with protected bands (including band 32) exist for DC\_7A\_n78A in 38101-3.

### 5.9.3 ∆TIB and ∆RIB values

Table 5.9.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n78 | 7 | 0.5 |
| n78 | 0.8 |

**Table 5.9.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n78 | 7 | 0 |
| 32 | 0 |
| n78 | 0.5 |

### 5.9.4 Reference sensitivity exceptions

**Table 5.9.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_7A-32A\_n78A | n78 | 3560.5 | 10 | 50 | 3560.5 | N/A | N/A |
| 7 | 2517.5 | 5 | 25 | 2637.5 | N/A | N/A |
| 32 | N/A | 5 | N/A | 1474.5 | 17.6 | IMD3 |
| n78 | 3311 | 10 | 50 | 3311 | N/A | N/A |
| 7 | 2565 | 5 | 25 | 2685 | N/A | N/A |
| 32 | N/A | 5 | N/A | 1492 | 4.9 | IMD4 |

## 5.10 DC\_20-32\_n28

### 5.10.1 Configurations for DC

Table 5.10.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_20A-32A\_n28A | DC\_20A\_n28A |

### 5.10.2 Co-existence studies

Table 5.10.2-1 lists the Band 20A + Band n28A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.10.2-1: Band 20 and Band n28 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 832 | 862 | | 703 | 748 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1664 – 1724 | | | 1406 – 1496 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2496 – 2586 | | | 2109 – 2244 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 84 – 159 | | | 1535 – 1610 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 916 – 1021 | | | 544 – 634 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 2367 – 2472 | | | 2238 – 2358 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 802 – 892 | | | 703 – 748 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 1748 – 1883 | | | 1247 – 1412 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| |  | |  |
| IMD frequency limits (MHz) | 168 – 318 | | |  | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 3199 – 3334 | | | 4029 – 4224 | | |
| Two-tone 4th order IMD products | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |  | |  |
| IMD frequency limits (MHz) | 3070 – 3220 | | |  | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1950 – 2160 | | | 6932 – 7217 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 385 – 580 | | | 4264 – 4534 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 3644 – 3854 | | | 8383 – 8668 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 3773 – 3968 | | | 3902 – 4082 | | |

Based on Table 5.10.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 11, 21, 32, 38, 41, 45, 69, 75 and 76

- 3rd order harmonics may fall into Rx frequencies of bands 1, 4, 10, 23, 65 and 66

- 2nd order IMD may fall into Rx frequencies of band 24

- 3rd order IMD may fall into Rx frequencies of bands 8, 30 and 40

- 4th order IMD may fall into Rx frequencies of bands 3, 9, 35, 39 and 77

- 5th order IMD may fall into Rx frequencies of bands 1, 2, 4, 7, 10, 25, 31, 34, 36, 38, 41, 43, 48, 65, 66, 69, 70 and 77

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.10.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.10.2-2: 2UL Band 20 + Band n28 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD 2 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD 2 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD 2 |
| GPS | 1563 | - | 1587 | Yes |  | IMD 2 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD 2 |
| 2400 | - | 2494 | Yes | Asia | IMD 2 |
| ISM band  (5GHz) | 5150 | - | 5925 | No | US |  |
| 5150 | - | 5350 | No | Europe |  |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | No | Asia |  |

The requirements for coexistence with protected bands (including band 32) exist for DC\_20A\_n28A in 38101-3.

### 5.10.3 ∆TIB and ∆RIB values

Table 5.10.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20A-32A\_n28 | 20 | 0.5 |
| n28 | 0.7 |

**Table 5.10.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20A-32A\_n28 | 20 | 0 |
| 32 | 0 |
| n28 | 0.2 |

### 5.10.4 Reference sensitivity exceptions

### The band 32 MSD due to the 2nd harmonic interferene from band n28 can refer to the definition in clause 5.8.4 of this TR.5.10.5 Reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1

The entries in tables 5.10.5-1 and 5.10.5-2 are to be added to TS38101-3 tables 7.3B.2.3.1-1 and 7.3B.2.3.1-2 respectively.

**Table 5.10.5-1: Reference sensitivity exceptions (MSD) due to UL harmonic for EN-DC in NR FR1**

| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| UL band | DL band | 5 MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 30 MHz (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n28 | 32 | 28.1 | 25.3 | 24.0 | 22.8 |  |  |  |  |  |  |  |  |

**Table 5.10.5-2: Uplink configuration for reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / UL RB allocation of the aggressor band | | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 30 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n28 | 32 | 8 | 16 | 25 | 25 |  |  |  |  |  |  |  |  |

## 5.11 DC\_2-48\_n5

### 5.11.1 Configurations for DC

Table 5.11.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-48A\_n5A | DC\_2A\_n5A  DC\_48A\_n5A |

### 5.11.2 Co-existence studies

When uplink is DC\_2A\_n5A there is IMD3 interfering band 48 downlink.

When uplink is DC\_48A\_n5A there is IMD3 interfering band 2 downlink.

### 5.11.3 ∆TIB and ∆RIB values

It is proposed to take the maximum relaxation values from DC\_2-n5 and DC\_48-n5.

Table 5.11.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-48\_n5 | 2 | 0.6 |
| 48 | 0.8 |
| n5 | 0.3 |

**Table 5.11.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-48\_n5 | 2 | 0.2 |
| 48 | 0.5 |
| n5 | 0.0 |

### 5.11.4 Reference sensitivity exceptions

The MSD levels are derived from the text proposal in R4-2010232 and R4-2014135.

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-48A\_n5A | 2 | 1870 | 5 | 25 | 1950 | 16.9 | IMD3 |
| 48 | 3610 | 10 | 50 | 3610 | N/A | N/A |
| n5 | 830 | 5 | 25 | 875 | N/A | N/A |
| 2 | 1890 | 5 | 25 | 1970 | N/A | N/A |
| 48 | 3570 | 5 | 25 | 3570 | 16.2 | IMD3 |
| n5 | 840 | 5 | 25 | 885 | N/A | N/A |

## 5.12 DC\_5-48\_n12

### 5.12.1 Configurations for DC

Table 5.12.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_5A-48A\_n12A | DC\_5A\_n12A  DC\_48A\_n12A |

### 5.12.2 Co-existence studies

When uplink is DC\_5A\_n12A there is IMD5 interfering band 48 downlink.

When uplink is DC\_48A\_n12A there is IMD5 interfering band 5 downlink.

### 5.12.3 ∆TIB and ∆RIB values

It is proposed to re-use relaxation values from E-UTRA CA\_5-12-48.

Table 5.12.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-48\_n12 | 5 | 0.8 |
| 48 | 0.3 |
| n12 | 0.4 |

**Table 5.12.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-48\_n12 | 5 | 0.5 |
| 48 | 0 |
| n12 | 0.3 |

### 5.12.4 Reference sensitivity exceptions

It is prosed to re-use the IMD5 MSD values from already specified configuration DC\_7A-28A\_n5A which is similar to DC\_5A-48A\_n12A.

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_5A-48A\_n12A | 5 | 830 | 5 | 25 | 875 | N/A | N/A |
| 48 | 3650 | 5 | 25 | 3650 | 4.4 | IMD5 |
| n12 | 705 | 5 | 25 | 735 | N/A | N/A |
| 5 | 830 | 5 | 25 | 875 | 5.9 | IMD5 |
| 48 | 3695 | 5 | 25 | 3695 | N/A | N/A |
| n12 | 705 | 5 | 25 | 735 | N/A | N/A |

## 5.13 DC\_5-48\_n71

### 5.13.1 Configurations for DC

Table 5.13.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_5A-48A\_n71A | DC\_5A\_n71A  DC\_48A\_n71A |

### 5.13.2 Co-existence studies

When uplink is DC\_5A\_n71A there is IMD5 interfering band 48 downlink.

When uplink is DC\_48A\_n71A there is IMD5 interfering band 5 downlink.

### 5.13.3 ∆TIB and ∆RIB values

It is proposed to take the maximum relaxation values from DC\_5\_n71 and DC\_48\_n71.

Table 5.13.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-48\_n71 | 5 | 0.5 |
| 48 | 0.3 |
| n71 | 0.5 |

**Table 5.13.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-48\_n71 | 5 | 0 |
| 48 | 0 |
| n71 | 0 |

### 5.13.4 Reference sensitivity exceptions

It is prosed to re-use the IMD5 MSD values from already specified configuration DC\_7A-28A\_n5A which is similar to DC\_5A-48A\_n71A.

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_5A-48A\_n71A | 5 | 830 | 5 | 25 | 875 | N/A | N/A |
| 48 | 3590 | 5 | 25 | 3590 | 4.4 | IMD5 |
| n71 | 690 | 5 | 25 | 644 | N/A | N/A |
| 5 | 835 | 5 | 25 | 880 | 5.9 | IMD5 |
| 48 | 3600 | 5 | 25 | 3600 | N/A | N/A |
| n71 | 680 | 5 | 25 | 634 | N/A | N/A |

## 5.14 DC\_12-48\_n5

### 5.14.1 Configurations for DC

Table 5.14.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_12A-48A\_n5A | DC\_12A\_n5A  DC\_48A\_n5A |

### 5.14.2 Co-existence studies

When uplink is DC\_12A\_n5A or DC\_48A\_n5A there is no IMD interfering 3rd band downlink.

### 5.14.3 ∆TIB and ∆RIB values

It is proposed to re-use relaxation values from E-UTRA CA\_5-12-48.

Table 5.14.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_12-48\_n5 | 12 | 0.4 |
| 48 | 0.3 |
| n5 | 0.8 |

**Table 5.14.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_12-48\_n5 | 12 | 0.3 |
| 48 | 0 |
| n5 | 0.5 |

### 5.14.4 Reference sensitivity exceptions

There is no need for additional REFSENS requirement.

## 5.15 DC\_3\_(n)41

### 5.15.1 Configuration for DC

**Table 5.15.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_3A\_(n)41AA | DC\_(n)41AA |

5.15.2 Co-existence study

Coexistence analysis has been captured into TR 37.716-21-11. There is no harmonic or IMD issues for the third band.

### 5.15.3 ∆TIB and ∆RIB values

For DC\_3­\_(n)41AA, the ΔTIB,c and ΔRIB,c values have been defined in TR 37.716-21-11

### 5.15.4 REFSENS requirements

There is no additional requirement for this band combination.

## 5.16 DC\_2A-48A\_n48A

5.16.1 Configurations for DC

Table 5.16.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_2A-48A\_n48A | DC\_2A\_n48A |

Note that DC\_48\_n48 is not used as uplink configuration.

### 5.16.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. No further analysis is needed.

5.16.3 ∆TIB and ∆RIB values

Table 5.16.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_2-48\_n48 | 2 | 0.6 |
| 48 | 0.8 |
| n48 |

Table 5.16.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_2-48\_n48 | 2 | 0.2 |
| 48 | 0.5 |
| n48 |

5.16.4 Reference sensitivity exceptions

REFSENS exceptions needed for DC\_2A-48A\_n48A due to band 48 uplink harmonic into band 2 is already specified in Table 7.3B.2.3.1-1 of TS 38.101-3.

## 5.17 DC\_48-66A\_n25A

5.17.1 Configurations for DC

Table 5.17.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_48A-66A\_n25A  DC\_48C-66A\_n25A  DC\_48D-66A\_n25A | DC\_48A\_n25A  DC\_66A\_n25A |

### 5.17.2 Co-existence studies

Co-existence studies have been performed for lower order combinations.

Co-existence analysis for DC\_48\_n25 UL shows that 4th IMD may fall into NR Band n48 DL. However, since 48 and n48 will be operated as synchronous in same UL/DL configuration there is no IMD problem. Further, a 4th IMD may fall in DL band 66.

Co-existence analysis for DC\_66\_n25 UL shows that 2nd HAM of band 66 may fall into the lowest 10MHz of NR Band n48 DL. This is already covered in Table 7.3B.2.3.1-1 and Table 7.3B.2.3.1-2 in 38.101-3. Further 2nd IMD might also fall in n48 DL

5.17.3 ∆TIB and ∆RIB values

Table 5.17.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_48-66\_n25 | 48 | 0.8 |
| 66 | 0.6 |
| n25 | 0.6 |

Table 5.17.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_48-66\_n25 | 48 | 0.5 |
| 66 | 0.2 |
| n25 | 0.2 |

5.17.4 Reference sensitivity exceptions

Based on the co-existence studies for DC\_48\_n25 and DC\_66A\_n25A it is found that MSD it needed.

Table 5.17.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_48A-66A\_n25A  DC\_48C-66A\_n25A  DC\_48D-66A\_n25A | 48 | 3630 | 20 | 100 | 3630 | N/A | N/A |
| 66 | 1730 | 5 | 25 | 2130 | 8.3 | IMD4 |
| n25 | 1883.3 | 5 | 25 | 1963.3 | N/A | N/A |
| 48 | 3620 | 10 | 50 | 3620 | 29.4 | IMD2 |
| 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |
| n25 | 1880 | 5 | 25 | 1960 | N/A | N/A |

## 5.18 DC\_48A-66A\_n48A

5.18.1 Configurations for DC

Table 5.18.2-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_48A-66A\_n48A | DC\_66A\_n48A |

Note that DC\_48\_n48 is not used as uplink configuration.

### 5.18.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. No further analysis is needed.

5.18.3 ∆TIB and ∆RIB values

Table 5.18.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_48-66\_n48 | 66 | 0.6 |
| 48 | 0.8 |
| n48 |

Table 5.18.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_48-66\_n48 | 66 | 0.2 |
| 48 | 0.5 |
| n48 |

5.18.4 Reference sensitivity exceptions

No REFSENS exceptions needed for DC\_48A-66A\_n48A.

## 5.19 DC\_3-8\_n40

5.19.1 Configurations for DC

Table 5.19.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_3A-8A\_n40A | DC\_3A\_n40A DC\_8A\_n40A |

### 5.19.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. Co-existence analysis for DC\_3\_n40 UL shows no impact to DL band 8,

Co-existence analysis for DC\_8\_n40 UL shows that 5th IMD may fall in DL band 3.

5.19.3 ∆TIB and ∆RIB values

Table 5.19.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_3-8\_n40 | 3 | 0.5 |
| 8 | 0.3 |
| n40 | 0.5 |

Table 5.19.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_3-8\_n40 | 3 | 0 |
| 8 | 0 |
| n40 | 0 |

5.19.4 Reference sensitivity exceptions

Based on co-existence studies additional MSD is needed.

Table 6. x.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_3A-8A\_n40A | 3 | 1779 | 5 | 25 | 1874 | 4 | IMD5 |
| 8 | 912 | 5 | 25 | 957 | N/A | N/A |
| n40 | 2305 | 5 | 25 | 2305 | N/A | N/A |

## 5.20 DC\_3-28\_n1

5.20.1 Configurations for DC

Table 5.20.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_3A-28A\_n1A | DC\_28A\_n1A DC\_3A\_n1A |

### 5.20.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. Co-existence analysis for DC\_28\_n1 UL shows that 3rd HAM might fall into DL band n1 This is already covered in Table 7.3B.2.3.1-1 and Table 7.3B.2.3.1-2 in 38.101-3. Further, is shows that 5th IMD may fall in DL band 3.

Co-existence analysis for DC\_3\_n1 UL shows no impact to DL band 28.

5.20.3 ∆TIB and ∆RIB values

Table 5.20.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_3-28\_n1 | 3 | 0.3 |
| 28 | 0.6 |
| n1 | 0.3 |

Table 5.20.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_3-28\_n1 | 3 | 0 |
| 28 | 0.2 |
| n1 | 0 |

5.20.4 Reference sensitivity exceptions

REFSENS exceptions needed due to band 28 uplink harmonic into band n1 is already specified for DC\_28A\_n1A.

The reference sensitivity exception (MSD) due to IMD5 for DC\_3-28\_n1 with UL DC\_28\_n1 is specified as below referring to the MSD for CA\_1A-3A-28A from 36.101.

Table 5.20.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_3A-28A\_n1A | 3 | 1725 | 5 | 25 | 1820 | 4 | IMD5 |
| 28 | 710 | 5 | 25 | 765 | N/A | N/A |
| n1 | 1975 | 5 | 25 | 2165 | N/A | N/A |

## 5.21 DC\_7-8\_n40

5.21.1 Configurations for DC

Table 5.21.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_7A-8A\_n40A | DC\_7A\_n40A DC\_8A\_n40A |

### 5.21.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. No further analysis is needed.

5.21.3 ∆TIB and ∆RIB values

Table 5.21.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_7-8\_n40 | 7 | 0.5 |
| 8 | 0.6 |
| n40 | 0.6 |

Table 5.21.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_7-8\_n40 | 7 | 0 |
| 8 | 0.2 |
| n40 | 0.5 |

5.21.4 Reference sensitivity exceptions

No further REFSENS exceptions needed.

## 5.22 DC\_7-28\_n1

5.22.1 Configurations for DC

Table 5.22.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_7A-28A\_n1A | DC\_28A\_n1A DC\_7A\_n1A |

### 5.22.2 Co-existence studies

Co-existence studies have been performed for lower order combinations.

Co-existence analysis for DC\_28\_n1 UL shows that 3rd HAM might fall into DL band n1 This is already covered in Table 7.3B.2.3.1-1 and Table 7.3B.2.3.1-2 in 38.101-3. Further, is shows that 2th IMD may fall in DL band 7.

Co-existence analysis for DC\_7\_n1 UL shows that 5th IMD may fall in DL band 28.

5.22.3 ∆TIB and ∆RIB values

Table 5.22.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_7-28\_n1 | 7 | 0.6 |
| 28 | 0.6 |
| n1 | 0.5 |

Table 5.22.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_7-28\_n1 | 7 | 0 |
| 28 | 0.2 |
| n1 | 0 |

5.22.4 Reference sensitivity exceptions

REFSENS exceptions needed due to band 28 uplink harmonic into band n1 is already specified for DC\_28A\_n1A.

Based on co-existence studies additional MSD is needed. The MSD levels are derived from the text proposal in R4-2011610 and R4-2010889.

Table 5.22.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_7A-28A\_n1A | 7 | 2535 | 5 | 25 | 2655 | N/A | N/A |
| 28 | 725 | 5 | 25 | 780 | 4.3 | IMD5 |
| n1 | 1950 | 5 | 25 | 2165 | N/A | N/A |
| 7 | 2545 | 5 | 25 | 2665 | 29.0 | IMD2 |
| 28 | 730 | 5 | 25 | 785 | N/A | N/A |
| n1 | 1935 | 5 | 25 | 2125 | N/A | N/A |

## 5.23 DC\_7-66\_n5

### 5.23.1 Configurations for DC

Table 5.23.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-66A\_n5A  DC\_7C-66A\_n5A  DC\_7A-66A-66A\_n5A  DC\_7C-66A-66A\_n5A  DC\_7A-7A-66A\_n5A  DC\_7A-7A-66A-66A\_n5A | DC\_7A\_n5A  DC\_66A\_n5A |

### 5.23.2 Co-existence studies

For UE coexistence study of Band 7 + Band n5, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.23.2-1.

**Table 5.23.2-1: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 824 | 849 | 2500 | 2570 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1648 | 1698 | 5000 | 5140 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2472 | 2547 | 7500 | 7710 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 3296 | 3396 | 10000 | 10280 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4120 | 4245 | 12500 | 12850 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1651 | 1746 | 3324 | 3419 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 922 | 802 | 4151 | 4316 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4148 | 4268 | 5824 | 5989 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 98 | 47 | 6651 | 6886 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4972 | 5117 | 8324 | 8534 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 3302 | 3492 | 6648 | 6838 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 726 | 896 | 9151 | 9456 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5796 | 5966 | 10824 | 11129 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 2668 | 2453 | 5802 | 6062 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 9148 | 9408 | 7472 | 7687 |

For UE coexistence study of Band 66 + Band n5, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.23.2-2

**Table 5.23.2-2: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 824 | 849 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1648 | 1698 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2472 | 2547 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 3296 | 3396 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4120 | 4245 | 8550 | 8900 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 861 | 956 | 2534 | 2629 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 132 | 12 | 2571 | 2736 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 3358 | 3478 | 4244 | 4409 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 692 | 837 | 4281 | 4516 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4182 | 4327 | 5954 | 6164 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 1722 | 1912 | 5068 | 5258 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1516 | 1686 | 5991 | 6296 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5006 | 5176 | 7664 | 7969 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 1088 | 873 | 3432 | 3692 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 6778 | 7038 | 5892 | 6107 |

Based on co-existence study as presented in the table 5.1.28.4-1 and 5.1.28.4-2, own Rx impact of the 3rd band is shown as the followings.

* 2nd order IMD generated by dual uplink of Band 66 + Band n5 may also fall into own Rx of band 7
* 3rd order IMD generated by dual uplink of Band 66 + Band n5 may also fall into own Rx of band 7

### 5.23.3 ∆TIB and ∆RIB values

Table 5.23.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-66\_n5  DC\_7-66-66\_n5  DC\_7-7-66\_n5  DC\_7-7-66-66\_n5 | 7 | 0.3 |
| 66 | 0.3 |
| n5 | 0.3 |

**Table 5.23.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-66\_n5  DC\_7-66-66\_n5  DC\_7-7-66\_n5  DC\_7-7-66-66\_n5 | 7 | 0 |
| 66 | 0 |
| n5 | 0 |

### 5.23.4 Reference sensitivity exceptions

Band 66 has similar UL frequency ranges as band 3, the MSD values for DC\_3-7\_n5 can be reused for DC\_7-66\_n5. Table 5.23.4-1 lists the MSD required for DC\_7-66\_n5.

**Table 5.23.4-1: MSD for the DC configuration due to IMD issue (three bands)**

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-66A\_n5A  DC\_7C-66A\_n5A  DC\_7A-66A-66A\_n5A  DC\_7C-66A-66A\_n5A  DC\_7A-7A-66A\_n5A  DC\_7A-7A-66A-66A\_n5A | 7 | 2505 | 10 | 50 | 2625 | 30.0 | IMD21 |
| 66 | 1775 | 10 | 50 | 2175 | N/A | N/A |
| n5 | 846.5 | 5 | 25 | 891.5 | N/A | N/A |
| NOTE 1: This band is subject to IMD3 also which MSD is not specified. | | | | | | | |

## 5.24 DC\_2-7\_n5

### 5.24.1 Configurations for DC

Table 5.24.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-7A\_n5A  DC\_2A-7C\_n5A  DC\_2A-7A-7A\_n5A | DC\_2A\_n5A  DC\_7A\_n5A |

### 5.24.2 Co-existence studies

For UE coexistence study of Band 7 + Band n5, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.24.2-1.

**Table 5.24.2-1: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 824 | 849 | 2500 | 2570 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1648 | 1698 | 5000 | 5140 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2472 | 2547 | 7500 | 7710 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 3296 | 3396 | 10000 | 10280 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4120 | 4245 | 12500 | 12850 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1651 | 1746 | 3324 | 3419 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 922 | 802 | 4151 | 4316 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4148 | 4268 | 5824 | 5989 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 98 | 47 | 6651 | 6886 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4972 | 5117 | 8324 | 8534 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 3302 | 3492 | 6648 | 6838 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 726 | 896 | 9151 | 9456 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5796 | 5966 | 10824 | 11129 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 2668 | 2453 | 5802 | 6062 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 9148 | 9408 | 7472 | 7687 |

For UE coexistence study of Band 2 + Band n5, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.24.2-2

**Table 5.24.2-2: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 824 | 849 | 1850 | 1910 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1648 | 1698 | 3700 | 3820 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2472 | 2547 | 5550 | 5730 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 3296 | 3396 | 7400 | 7640 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4120 | 4245 | 9250 | 9550 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1001 | 1086 | 2674 | 2759 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 262 | 152 | 2851 | 2996 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 3498 | 3608 | 4524 | 4669 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 562 | 697 | 4701 | 4906 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4322 | 4457 | 6374 | 6554 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 2002 | 2172 | 5348 | 5518 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1386 | 1546 | 6551 | 6816 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5146 | 5306 | 8224 | 8489 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 1348 | 1153 | 3852 | 4082 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 7198 | 7428 | 6172 | 6367 |

Based on co-existence study as presented in the table 5.24.2-1 and 5.24.2-2, own Rx impact of the 3rd band is shown as the followings.

* 2nd order IMD generated by dual uplink of Band 2 + Band n5 may also fall into own Rx of band 7

### 5.24.3 ∆TIB and ∆RIB values

Table 5.24.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-7\_n5  DC\_2-7-7\_n5 | 2 | 0.3 |
| 7 | 0.3 |
| n5 | 0.3 |

**Table 5.24.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-7\_n5  DC\_2-7-7\_n5 | 2 | 0 |
| 7 | 0 |
| n5 | 0 |

### 5.24.4 Reference sensitivity exceptions

By adjusting the centre frequency of uplink of Band 2+ Band n5, the MSD requirement due to 2nd order IMD for DC\_2-7\_n5 can be similar as the requirements of DC\_3-7\_n5. Table 5.1.28.4-3 lists the MSD required for DC\_2-7\_n5.

**Table 5.24.4-1: MSD for the DC configuration due to IMD issue (three bands)**

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-7A\_n5A  DC\_2A-7C\_n5A  DC\_2A-7A-7A\_n5A | 2 | 1855 | 10 | 50 | 1935 | N/A | N/A |
| 7 | 2575 | 10 | 50 | 2685 | 30.0 | IMD2 |
| n5 | 830 | 5 | 25 | 875 | N/A | N/A |

## 5.25 DC\_1-40\_n78

5.25.1 Operating bands for DC

Table 5.25.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_1-40\_n78 | CA\_1-40 | n78 | No |

5.25.2 Configurations for DC

Table 5.25.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_1A-40A\_n78A  DC\_1A-40C\_n78A | DC\_1A\_n78A  DC\_40A\_n78A | CA\_1A-40A  CA\_1A-40C | n78 |

5.25.3 Co-existence studies

Based on co-existence studies of Band 1 + Band n78 captured in 37.863-01-01, MSD shall be considered since

- 4th order IMD of the two bands may fall into Rx frequencies of band 1 and band 40.

And based on co-existence studies of Band 40 + Band n78 captured in 37.716-11-11, MSD shall be considered since

- 4th order IMD generated by dual uplink of the two bands may fall into own Rx of band 1.

- harmonic mixing generated by 2nd harmonic of n78 Tx and 3rd harmonic of band 40 Rx.

5.25.4 ∆TIB and ∆RIB values

Table 5.25.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-40-n78 | 1 | 0.6 |
| 40 | 0.35 |
| n78 | 0.85 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one NR band and without simultaneous Rx/Tx. | | |

**Table 5.25.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-40-n78 | 1 | 0.2 |
| 40 | 0.45 |
| n78 | 0.55 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one NR band and without simultaneous Rx/Tx. | | |

5.25.5 REFSENS requirements

As stated in 5.25.3, for MSD requirement caused by IMDs is specified below accordingly. To note that the MSD requirements are already defined for DC\_1A\_n40A-n78A in TS 38.101-3, among which the one for IMD4 on band n40 can be followed here for band 40 IMD4 impact. The requirements apply both to DC\_1A-40A\_n78A and DC\_1A-40C\_n78A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_1A-40A\_n78A  DC\_1A-40C\_n78A | 1 | 1930 | 5 | 25 | 2120 | N/A | N/A |
| 40 | 2340 | 5 | 25 | 2340 | 10.6 | IMD4 |
| n78 | 3450 | 10 | 50 | 3450 | N/A | N/A |
| DC\_1A-40A\_n78A  DC\_1A-40C\_n78A | 1 | 1950 | 5 | 25 | 2140 | 9.1 | IMD4 |
| 40 | 2360 | 5 | 25 | 2360 | N/A | N/A |
| n78 | 3430 | 10 | 50 | 3430 | N/A | N/A |

Other issues mentioned in 5.25.3 (i.e., harmonic mixing between band 40 Rx and n78 Tx, and MSD for band 1 caused by 4th IMD of band 1 and n78) had already been specified in the corresponding specs.

## 5.26 DC\_3-40\_n78

5.26.1 Operating bands for DC

Table 5.26.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_3-40\_n78 | CA\_3-40 | n78 | DC\_3\_n78 |

5.26.2 Configurations for DC

Table 5.26.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_3A-40A\_n78A  DC\_3A-40C\_n78A | DC\_3A\_n78A  DC\_40A\_n78A | CA\_3A-40A  CA\_3A-40C | n78 |

5.26.3 Co-existence studies

Based on co-existence studies of Band 3 + Band n78 captured in 37.863-01-01, MSD shall be considered since

- 2nd 4th and 5th order IMD of the two bands may fall into Rx frequencies of band 3

- 2nd harmonic of band 3 may fall into Rx frequencies of n78

- 5th order IMD of the two bands may fall into Rx frequencies of band 40

And based on co-existence studies of Band 40 + Band n78 captured in 37.716-11-11, MSD shall be considered since

- 4th order IMD generated by dual uplink of the two bands may fall into own Rx of band 3.

5.26.4 ∆TIB and ∆RIB values

Table 5.26.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-40-n78 | 3 | 0.6 |
| 40 | 0.35 |
| n78 | 0.85 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one NR band and without simultaneous Rx/Tx. | | |

**Table 5.26.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-40-n78 | 3 | 0.2 |
| 40 | 0.45 |
| n78 | 0.55 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one NR band and without simultaneous Rx/Tx. | | |

5.26.5 REFSENS requirements

As stated in 5.26.3, for MSD requirement caused by IMDs is specified below accordingly. To note that the MSD requirements are already defined for DC\_3A\_n40A-n78A in TS 38.101-3, among which the one for IMD4 on band n40 can be followed here for band 40 IMD4 impact. The below requirements apply both to DC\_3A-40A\_n78A and DC\_3A-40C\_n78A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_3A-40A\_n78A  DC\_3A-40C\_n78A | 3 | 1775 | 5 | 25 | 1870 | 9.1 | IMD4 |
| 40 | 2390 | 5 | 25 | 2390 | N/A | N/A |
| n78 | 3325 | 10 | 50 | 3325 | N/A | N/A |
| DC\_3A-40A\_n78A  DC\_3A-40C\_n78A | 3 | 1720 | 5 | 25 | 1815 | N/A | N/A |
| 40 | 2360 | 5 | 25 | 2360 | 4.4 | IMD5 |
| n78 | 3760 | 10 | 50 | 3760 | N/A | N/A |

Other issues mentioned in 5.26.3 (i.e., 2nd harmonic from band 3 and MSD for band 3 caused by 2nd, 4th and 5th IMD of band 3 and n78) had already been specified in the corresponding specs. To note that due to the high IMD impact, single UL is allowed between band 3 and band n78.

## 5.27 DC\_7-40\_n78

5.27.1 Operating bands for DC

Table 5.27.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_7-40\_n78 | CA\_7-40 | n78 | No |

5.27.2 Configurations for DC

Table 5.27.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_7A-40A\_n78A  DC\_7A-40C\_n78A | DC\_7A\_n78A  DC\_40A\_n78A | CA\_7A-40A  CA\_7A-40C | n78 |

5.27.3 Co-existence studies

Based on co-existence studies of Band 7 + Band n78 captured in 37.863-01-01, MSD shall be considered since

- 4th order IMD of the two bands may fall into Rx frequencies of band 40

And based on co-existence studies of Band 40 + Band n78 captured in 37.716-11-11, MSD shall be considered since

- 4th order IMD generated by dual uplink of the two bands may fall into Rx of band 7.

- harmonic mixing generated by 2nd harmonic of n78 Tx and 3rd harmonic of band 40 Rx.

5.27.4 ∆TIB and ∆RIB values

Table 5.27.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-40-n78 | 7 | 0.5 |
| 40 | 0.35 |
| n78 | 0.85 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one NR band and without simultaneous Rx/Tx. | | |

**Table 5.27.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-40-n78 | 7 | 0 |
| 40 | 0.45 |
| n78 | 0.55 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one NR band and without simultaneous Rx/Tx. | | |

5.27.5 REFSENS requirements

As stated in 5.27.3, for MSD requirement caused by IMDs is specified below accordingly. The requirements apply both to DC\_7A-40A\_n78A and DC\_7A-40C\_n78A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_7A-40A\_n78A  DC\_7A-40C\_n78A | 7 | 2510 | 5 | 25 | 2630 | 10.1 | IMD4 |
| 40 | 2310 | 5 | 25 | 2310 | N/A | N/A |
| n78 | 3625 | 10 | 50 | 3625 | N/A | N/A |
| DC\_7A-40A\_n78A  DC\_7A-40C\_n78A | 7 | 2510 | 5 | 25 | 2630 | N/A | N/A |
| 40 | 2310 | 5 | 25 | 2310 | 8.7 | IMD4 |
| n78 | 3785 | 10 | 50 | 3785 | N/A | N/A |

Other issues mentioned in 5.27.3 had already been specified in the corresponding specs.

## 5.28 DC\_8-40\_n78

5.28.1 Operating bands for DC

Table 5.28.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_8-40\_n78 | CA\_8-40 | n78 | No |

5.28.2 Configurations for DC

Table 5.28.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_8A-40A\_n78A  DC\_8A-40C\_n78A | DC\_8A\_n78A  DC\_40A\_n78A | CA\_8A-40A  CA\_8A-40C | n78 |

5.28.3 Co-existence studies

Based on co-existence studies of Band 8 + Band n78 captured in 37.863-01-01, MSD shall be considered since

- 4th order IMD of the two bands may fall into Rx frequencies of band 8

- 4th harmonic of the band 8 may fall into Rx frequencies of band n78

- 2nd order IMD of the two bands may fall into Rx frequencies of band 40, under the cases that band 40 is not in sync with band n78 in TDD configuration

And based on co-existence studies of Band 40 + Band n78 captured in 37.716-11-11, MSD shall be considered since

- 2nd and 3rd order IMD generated by dual uplink of the two bands may fall into own Rx of band 8.

- harmonic mixing generated by 2nd harmonic of n78 Tx and 3rd harmonic of band 40 Rx.

5.28.4 ∆TIB and ∆RIB values

Table 5.28.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8-40-n78 | 8 | 0.6 |
| 40 | 0.35 |
| n78 | 0.85 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one NR band and without simultaneous Rx/Tx. | | |

**Table 5.28.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8-40-n78 | 8 | 0.2 |
| 40 | 0.45 |
| n78 | 0.55 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one NR band and without simultaneous Rx/Tx. | | |

5.28.5 REFSENS requirements

As stated in 5.28.3, for MSD requirement caused by IMDs is specified below accordingly. The below requirements apply both to DC\_8A-40A\_n78A and DC\_8A-40C\_n78A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_8A-40A\_n78A  DC\_8A-40C\_n78A | 8 | 905 | 5 | 25 | 950 | 30.5 | IMD2 |
| 40 | 2380 | 5 | 25 | 2380 | N/A | N/A |
| n78 | 3330 | 10 | 50 | 3330 | N/A | N/A |
| DC\_8A-40A\_n78ADC\_8A-40C\_n78A | 8 | 890 | 5 | 25 | 935 | 19.8 | IMD3 |
| 40 | 2320 | 5 | 25 | 2320 | N/A | N/A |
| n78 | 3705 | 10 | 50 | 3705 | N/A | N/A |
| DC\_8A-40A\_n78A  DC\_8A-40C\_n78A | 8 | 910 | 5 | 25 | 955 | N/A | N/A |
| 40 | 2395 | 5 | 25 | 2395 | 28 | IMD2 |
| n78 | 3305 | 10 | 50 | 3305 | N/A | N/A |

Other issues mentioned in 5.28.3 had already been specified in the corresponding specs.

## 5.29 DC\_2-4\_n28

5.29.1 Configurations for DC

Table 5.29.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_2A-4A\_n28A | DC\_2A\_n28A  DC\_4A\_n28A |

5.29.2 Co-existence studies

Co-existence studies on DC\_4\_n28 and DC\_2\_n28 show own Rx impact of the 3rd band due to dual UL as following:

- IMD4 by dual UL of Band 4 and Band n28 may fall into Band 2 DL.

5.29.3 ∆TIB and ∆RIB values

For DC\_2-4\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_2-4-28, and are given in the tables below.

Table 5.29.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-4-n28 | 2 | 0.5 |
| 4 | 0.5 |
| n28 | 0.8 |

**Table 5.29.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-4-n28 | 2 | 0.3 |
| 4 | 0.3 |
| n28 | 0.5 |

5.29.4 REFSENS requirements

The MSD value for the impact on Band 2 DL by dual uplink of Band 4 + Band n28 stated in 5.29.2 is shown in the following table.

Table 5.29.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_2A-4A\_n28A | 2 | 1880 | 5 | 25 | 1960 | 11.0 | FDD | IMD4 |
| 4 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
| n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |

## 5.30 DC\_2-7\_n28

5.30.1 Configurations for DC

Table 5.30.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_2A-7A\_n28A | DC\_2A\_n28A  DC\_7A\_n28A |

5.30.2 Co-existence studies

Co-existence analysis from DC\_2\_n28 shows that there is IMD2 impact from DC\_2\_n28 UL to Band 7 DL. And there is no IMD impact from DC\_7\_n28 UL to Band 2 DL.

5.30.3 ∆TIB and ∆RIB values

For DC\_2-7\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_2-7-28, and are given in the tables below.

Table 5.30.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-7-n28 | 2 | 0.5 |
| 7 | 0.5 |
| n28 | 0.3 |

**Table 5.30.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-7-n28 | 2 | 0 |
| 7 | 0 |
| n28 | 0 |

5.30.4 REFSENS requirements

The MSD value for the impact on Band 7 DL by dual uplink of Band 2 + Band n28 stated in 5.30.2 is shown in the following table.

Table 5.30.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_2A-7A\_n28A | 2 | 1880 | 5 | 25 | 1960 | N/A | FDD | N/A |
| 7 | 1720 | 5 | 25 | 2120 | 29.0 | FDD | IMD2 |
| n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |

## 5.31 DC\_2-66\_n28

5.31.1 Configurations for DC

Table 5.31.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_2A-66A\_n28A | DC\_2A\_n28A  DC\_66A\_n28A |

5.31.2 Co-existence studies

Co-existence studies on DC\_28\_n66 and DC\_2\_n28 show the following own Rx impact of the 3rd band:

- IMD4 by dual UL of Band 66 and Band n28 may fall into Band 2 DL.

5.31.3 ∆TIB and ∆RIB values

For DC\_2-66\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_2-66-28, and are given in the tables below.

Table 5.31.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-66-n28 | 2 | 0.5 |
| 66 | 0.5 |
| n28 | 0.6 |

**Table 5.31.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-66-n28 | 2 | 0.3 |
| 66 | 0.3 |
| n28 | 0.2 |

5.31.4 REFSENS requirements

The MSD value for the impact on Band 2 DL by dual uplink of Band 66 + Band n28 stated in 5.31.2 is shown in the following table.

Table 5.31.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_2A-66A\_n28A | 2 | 1880 | 5 | 25 | 1960 | 11.0 | FDD | IMD4 |
| 66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
| n28 | 740 | 5 | 25 | 795 | N/A | FDD | N/A |

## 5.32 DC\_4-7\_n28

5.32.1 Configurations for DC

Table 5.32.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_4A-7A\_n28A | DC\_4A\_n28A  DC\_7A\_n28A |

5.32.2 Co-existence studies

Based on the co-existence studies of DC\_4\_n28 and DC\_7\_n28, own Rx impact of the 3rd band are the following:

- IMD3 by dual UL of Band 4 and Band n28 may fall into Band 7 DL.

5.32.3 ∆TIB and ∆RIB values

For DC\_4-7\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_4-7-28, and are given in the tables below.

Table 5.32.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_4-7-n28 | 4 | 0.5 |
| 7 | 0.5 |
| n28 | 0.6 |

**Table 5.32.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_4-7-n28 | 4 | 0.5 |
| 7 | 0.5 |
| n28 | 0.2 |

5.32.4 REFSENS requirements

The MSD values for own Rx impact of the 3rd band stated in 5.32.2 are shown in the following table.

Table 5.32.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_4A-7A\_n28A | 4 | 1715 | 5 | 25 | 2115 | N/A | FDD | N/A |
| 7 | 2565 | 5 | 25 | 2685 | 18.0 | FDD | IMD3 |
| n28 | 745 | 5 | 25 | 800 | N/A | FDD | N/A |

## 5.33 DC\_5-7\_n66

5.33.1 Configurations for DC

Table 5.33.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_5A-7A\_n66A  DC\_5A-7C\_n66A  DC\_5A-7A-7A\_n66A | DC\_5A\_n66A  DC\_7A\_n66A |

5.33.2 Co-existence studies

Co-existence studies on DC\_7\_n66 and DC\_5\_n66 show own Rx impact on the 3rd band due to dual uplink as follows:

- IMD3 of dual uplink of Band 7 and n66 may fall into Band 5 DL,

- IMD2 and IMD3 of dual uplink of Band 5 and n66 may fall into Band 7 DL.

5.33.3 ∆TIB and ∆RIB values

For DC\_5-7\_n66, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_5-7-66, and are given in the tables below.

Table 5.33.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-7-n66 | 5 | 0.3 |
| 7 | 0.5 |
| n66 | 0.5 |

**Table 5.33.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-7-n66 | 5 | 0 |
| 7 | 0.5 |
| n66 | 0.5 |

5.33.4 REFSENS requirements

The MSD values for own Rx impact of the 3rd band stated in 5.33.2 are shown in the following table. The MSD levels are derived from the text proposal in R4-2009928 and R4-2014128.

Table 5.33.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_5A-7A\_n66A  DC\_5A-7C\_n66A  DC\_5A-7A-7A\_n66A | 5 | 835 | 5 | 25 | 880 | 17.8 | FDD | IMD3 |
| 7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |
| 66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
| 5 | 846.5 | 5 | 25 | 891.5 | N/A | FDD | N/A |
| 7 | 2504 | 5 | 25 | 2624 | 29.0 | FDD | IMD21 |
| 66 | 1777.5 | 5 | 25 | 2177.5 | N/A | FDD | N/A |
| NOTE 1: This band is subject to IMD3 also which MSD is not specified. | | | | | | | | |

## 5.34 DC\_7-66\_n28

5.34.1 Configurations for DC

Table 5.34.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_7A-66A\_n28A | DC\_7A\_n28A  DC\_66A\_n28A |

5.34.2 Co-existence studies

Based on the co-existence studies of DC\_66\_n28 and DC\_7\_n28, own Rx impact of the 3rd band are the following:

- IMD3 by dual UL of Band 66 and Band n28 may fall into Band 7 DL.

5.34.3 ∆TIB and ∆RIB values

For DC\_7-66\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_4-7-28, and are given in the tables below.

Table 5.34.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-66-n28 | 2 | 0.5 |
| 66 | 0.5 |
| n28 | 0.6 |

**Table 5.34.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-66-n28 | 7 | 0.5 |
| 66 | 0.5 |
| n28 | 0.2 |

5.34.4 REFSENS requirements

The MSD values for own Rx impact of the 3rd band stated in 5.34.2 are shown in the following table.

Table 5.34.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_7A-66A\_n28A | 7 | 2565 | 5 | 25 | 2685 | 18.0 | FDD | IMD3 |
| 66 | 1715 | 5 | 25 | 2115 | N/A | FDD | N/A |
| n28 | 745 | 5 | 25 | 800 | N/A | FDD | N/A |

## 5.35 DC\_1-11\_n28

5.35.1 Configurations for DC\_1-11\_n28

Table 5.35.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_1A-11A\_n28A | DC\_1A\_n28A  DC\_11A\_n28A | CA\_1A-11A | n28A |

5.35.2 Co-existence studies

When Uplink EN-DC configuration is DC\_11A\_n28A, IMD2 and IMD3 of (B11 - n28) will fall into Rx band of Band 1. But considering the current situation that Band 11 is operated only by a certain operators in Japan, the frequency ranges can be limited as follows.

* Operator X: B11 (UL:1427.9-1437.9 / DL:1475.9-1485.9 MHz), B1 (UL:1960-1980 / DL:2150-2170 MHz), n28 (UL:738-748 / DL:793-803 MHz)
* Opeartor Y: B11 (UL:1437.9-1447.9 / DL:1485.9-1495.9 MHz), B1 (UL:1920-1940 / DL:2110-2130 MHz), n28 (UL:718-728 / DL:773-783 MHz)

Based on the existing frequency restriction in Japan, RAN4 only need to analyze the IMD2 problem as follow

* IMD2 by dual uplink DC\_11\_n28 will fall into the own Rx band of Band 1
* IMD3 by dual uplink DC\_11\_n28 is not specified due to the current operator spectrum holding.

5.35.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.35.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_1-11\_n28 | 1 | 0.3 |
| 11 | 0.4 |
| n28 | 0.6 |

Table 5.35.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_1-11\_n28 | 1 | 0 |
| 11 | 0 |
| n28 | 0.2 |

5.35.4 Reference sensitivity exceptions

As mentioned above, IMD2 of B11 and n28 to Band 1 Rx need to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.35.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_1A-11A\_n28A | 11 | 1440 | 5 | 25 | 1488 | N/A | N/A |
| n28 | 710 | 5 | 25 | 765 | N/A | N/A |
| 1 | 1960 | 5 | 25 | 2150 | 28.3 | IMD2 |
| DC\_1A-11A\_n28A | 11 | 1440 | 5 | 5 | 1488 | N/A | N/A |
| n28 | 710 | 5 | 5 | 765 | N/A | N/A |
| 1 | 1975 | 5 | 5 | 2165 | N/A1 | IMD3 |

## 5.36 DC\_3-11\_n28

5.36.1 Configurations for DC\_3-11\_n28

Table 5.36.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_3A-11A\_n28A | DC\_3A\_n28A  DC\_11A\_n28A | CA\_3A-11A | n28A |

5.36.2 Co-existence studies

There is no additional harmonic and intermodulation impact for the additional band receiver.

5.36.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.36.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_3-11\_n28 | 3 | 0.8 |
| 11 | 0.9 |
| n28 | 0.6 |

Table 5.36.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_3-11\_n28 | 3 | 0.3 |
| 11 | 0.5 |
| n28 | 0.2 |

5.36.4 Reference sensitivity exceptions

As mentioned in 5.36.2, REFSENS exceptions are not expected.

## 5.37 DC\_8-11\_n28

5.37.1 Configurations for DC\_8-11\_n28

Table 5.37.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_8A-11A\_n28A | DC\_8A\_n28A  DC\_11A\_n28A | CA\_8A-11A | n28A |

5.37.2 Co-existence studies

There is no additional harmonic and intermodulation impact for the additional band receiver.

5.37.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.37.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_8-11\_n28 | 8 | 0.6 |
| 11 | 0.4 |
| n28 | 0.6 |

Table 5.37.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_8-11\_n28 | 8 | 0.2 |
| 11 | 0 |
| n28 | 0.2 |

5.37.4 Reference sensitivity exceptions

As mentioned in 5.37.2, REFSENS exceptions are not expected.

## 5.38 DC\_3-11\_n77

5.38.1 Configurations for DC\_3-11\_n77

Table 5.38.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_3A-11A\_n77A | DC\_3A\_n77A  DC\_11A\_n77A | CA\_3A-11A | n77A |
| DC\_3A-11A\_n77(2A) | DC\_3A\_n77A  DC\_11A\_n77A | CA\_3A-11A | n77(2A) |

5.38.2 Co-existence studies

When Uplink EN-DC configuration is DC\_3A\_n77A, (1) IMD4 of (B3 - n77) will fall into Rx band of Band 11. When Uplink EN-DC configuration is DC\_11A\_n77A, (2) IMD2 and (3) IMD5 of (B11 - n77) will fall into Rx band of Band 3.

But considering the current situation that Band 11 is operated only by a certain operators in Japan, the frequency ranges can be limited as follows.

- Operator X: B11 (UL:1427.9-1437.9 / DL:1475.9-1485.9 MHz), B3 (UL:1750-1765 / DL:1845-1860 MHz), n77 (3400-3440 / 3560-3600 / 3900-4000 MHz)

- Opeartor Y: B11 (UL:1437.9-1447.9 / DL:1485.9-1495.9 MHz), B3 (UL:1710-1730 / DL:1805-1825 MHz), n77 (3520-3560 / 3700-3800 / 4000-4100 MHz)

Then the own Rx impact can be simplified as below.

* IMD4 of (B3-n77) will fall into Rx band of Band 11.
* IMD5 of (B11-n77) will fall into Rx band of Band 3.

5.38.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.38.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_3-11\_n77 | 3 | 0.8 |
| 11 | 0.9 |
| n77 | 0.8 |

Table 5.38.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_3-11\_n77 | 3 | 0.3 |
| 11 | 0.5 |
| n77 | 0.5 |

5.38.4 Reference sensitivity exceptions

As mentioned above, IMD4 of B3 and n77 to Band11 Rx and IMD5 of B11 and n77 to Band3 Rx need to be addressed for REFSENS relaxation. Based on the exceptions of DC\_3-21\_n77, the following values are proposed:

Table 5.38.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_3A-11A\_n77A  DC\_3A-11A\_n77(2A) | 3 | 1720 | 5 | 25 | 1815 | N/A | FDD | N/A |
| n77 | 3675 | 10 | 50 | 3675 | N/A | TDD | N/A |
| 11 | 1443 | 5 | 25 | 1491 | 8.8 | FDD | IMD4 |
| 11 | 1435.4 | 5 | 25 | 1483.4 | N/A | FDD | N/A |
| n77 | 3905 | 10 | 50 | 3905 | N/A | TDD | N/A |
| 3 | 1753 | 5 | 25 | 1848 | 3.4 | FDD | IMD5Y |
| Note Y: This band is also subject to IMD2 which is not specified. The frequency range below 3400MHz in n77 is not used for this combination. | | | | | | | | |

5.39 DC\_2-12\_n5

5.39.1 Operating bands for EN-DC

Table 5.39.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 2-12\_n5 | CA\_2-12 | n5 |  |

### 5.39.2 Configuration for DC

Table 5.39.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-12A\_n5A | DC\_2A\_n5A DC\_12A\_n5A | DC\_2A-12A | n5A |

5.39.3 ∆TIB and ∆RIB values

For DC\_2-12\_n5, the ΔTIB,c and ΔRIB,c values are reused from LTE combination CA\_2-5-12 and are given in the tables below.

**Table 5.39.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-12\_n5 | 2 | 0.3 |
| 12 | 0.4 |
| n5 | 0.8 |

**Table 5.39.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-12\_n5 | 2 | 0 |
| 12 | 0.3 |
| n5 | 0.5 |

5.39.4 REFSENS requirements

There is IMD5 impact from DC\_12\_n5 UL affecting band 2 DL. MSD derived from DC\_7A-28A\_n5A and DC\_20A\_n7A-n28A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-12A\_n5A | 2 | 1900 | 5 | 25 | 1980 | 5.9 | IMD5 |
| 12 | 705 | 5 | 25 | 735 | N/A | N/A |
| n5 | 840 | 5 | 25 | 885 | N/A | N/A |

5.40 DC\_2-5\_n12

5.40.1 Operating bands for EN-DC

Table 5.40.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 2-5\_n12 | CA\_2-5 | n12 |  |

### 5.40.2 Configuration for DC

Table 5.40.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-5A\_n12A | DC\_2A\_n12A DC\_5A\_n12A | DC\_2A-5A | n12A |

5.40.3 ∆TIB and ∆RIB values

For DC\_2-5\_n12, the ΔTIB,c and ΔRIB,c values are reused from LTE combination CA\_2-5-12 and are given in the tables below.

**Table 5.40.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-5\_n12 | 2 | 0.3 |
| 5 | 0.8 |
| n12 | 0.4 |

**Table 5.40.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-5\_n12 | 2 | 0 |
| 5 | 0.5 |
| n12 | 0.3 |

5.40.4 REFSENS requirements

There is IMD5 impact from DC\_5\_n12 UL affecting band 2 DL. MSD derived from DC\_7A-28A\_n5A and DC\_20A\_n7A-n28A.

Band 5 is also affected by IMD5 from UL DC\_2A\_n12A, but MSD value is not specified as there is only partial overlap of IMD5 with DL carrier

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-5A\_n12A6 | 2 | 1900 | 5 | 25 | 1980 | 5.9 | IMD5 |
| 5 | 840 | 5 | 25 | 885 | N/A | N/A |
| n12 | 705 | 5 | 25 | 735 | N/A | N/A |
| NOTE 6: Band 5 is also affected by IMD5 from UL DC\_2A\_n12A, but MSD value is not specified as there is only partial overlap of IMD5 with DL carrier | | | | | | | |

5.41 DC\_5-66\_n12

5.41.1 Operating bands for EN-DC

Table 5.41.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 5-66\_n12 | CA\_5-66 | n12 |  |

### 5.41.2 Configuration for DC

Table 5.41.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_5A-66A\_n12A | DC\_5A\_n12A DC\_66A\_n12A | DC\_5A-66A | n12A |

5.41.3 ∆TIB and ∆RIB values

For DC\_5-66\_n12, the ΔTIB,c and ΔRIB,c values are reused from LTE combination CA\_5-12-66 and are given in the tables below.

**Table 5.41.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-66\_n12 | 5 | 0.3 |
| 66 | 0.8 |
| n12 | 0.8 |

**Table 5.41.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-66\_n12 | 5 | 0 |
| 66 | 0.5 |
| n12 | 0.5 |

5.41.4 REFSENS requirements

There is no need to define MSD.

5.42 DC\_66\_(n)5

5.42.1 Operating bands for EN-DC

Table 5.42.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_66-(n)5 | CA\_66-5 | n5 |  |

### 5.42.2 Configuration for DC

Table 5.42.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_66A-(n)5AA | DC\_66A\_n5A  DC\_(n)5AA1 | CA\_66A-5A | n5A |
| NOTE1: Only single switched UL is supported | | | |

5.42.3 ∆TIB and ∆RIB values

For DC\_66\_(n)5 the ΔTIB,c and ΔRIB,c values are derived from DC\_66\_n5 combination.

Table 5..1.62.4-1: ΔTIB,c

| E-UTRA and NR DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_66\_(n)5 | 5 | 0.3 |
| n5 | 0.3 |
| 66 | 0.3 |

Table 5.1.116.4-2: ΔRIB,c

| E-UTRA and NR DC Configuration | E-UTRA and NR Band | ΔRIB,c [dB] |
| --- | --- | --- |
| DC\_66\_(n)5 | 5 | 0 |
| n5 | 0 |
| 66 | 0 |

5.42.4 REFSENS requirements

No additional REFSENS requirement is needed.

5.43 DC\_12-66\_n5

5.43.1 Operating bands for EN-DC

Table 5.43.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 12-66\_n5 | CA\_12-66 | n5 |  |

### 5.43.2 Configuration for DC

Table 5.43.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_12A-66A\_n5A | DC\_12A\_n5A DC\_66A\_n5A | DC\_12A-66A | n5A |

5.43.3 ∆TIB and ∆RIB values

For DC\_12-66\_n5, the ΔTIB,c and ΔRIB,c values are reused from LTE combination CA\_5-12-66 and are given in the tables below.

**Table 5.43.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_12-66\_n5 | 12 | 0.8 |
| 66 | 0.8 |
| n5 | 0.3 |

**Table 5.43.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_12-66\_n5 | 12 | 0.5 |
| 66 | 0.5 |
| n5 | 0 |

5.43.4 REFSENS requirements

There is IMD4 impact from DC\_66\_n5 UL affecting band 12 DL. MSD derived from DC\_3A-28A\_n5A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_12A-66A\_n5A | 12 | 712 | 5 | 25 | 742 | 9.4 | IMD4 |
| 66 | 1745 | 5 | 25 | 2145 | N/A | N/A |
| n5 | 829 | 5 | 25 | 874 | N/A | N/A |

## 5.44 DC\_7-8\_n28

5.44.1 Operating bands for DC

Table 5.44.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_7-8\_n28 | CA\_7-8 | n28 |

5.44.2 Configuration for DC

Table 5.44.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_7A-8A\_n28A | DC\_7A\_n28A DC\_8A\_n28A | CA\_7-8 | n28 |

5.44.3 Co-existence studies

For UE coexistence study of Band 8 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.44.3-1.

Table 5.44.3-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 880 | 915 | 703 | 748 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1760 | 1830 | 1406 | 1496 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2640 | 2745 | 2109 | 2244 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 3520 | 3660 | 2812 | 2992 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4400 | 4575 | 3515 | 3740 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 212 | 132 | 1583 | 1663 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 1012 | 1127 | 491 | 616 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 2463 | 2578 | 2286 | 2411 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 1892 | 2042 | 1194 | 1364 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 3343 | 3493 | 2989 | 3159 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 264 | 424 | 3166 | 3326 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 2112 | 1897 | 2957 | 2772 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 484 | 279 | 1339 | 1144 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 3692 | 3907 | 4223 | 4408 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 3869 | 4074 | 4046 | 4241 |

For UE coexistence study of Band 7 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.44.3-1.

Table 5.44.3-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 2500 | 2570 | 703 | 748 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 5000 | 5140 | 1406 | 1496 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 7500 | 7710 | 2109 | 2244 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 10000 | 10280 | 2812 | 2992 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 12500 | 12850 | 3515 | 3740 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1867 | 1752 | 3203 | 3318 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 4252 | 4437 | 1164 | 1004 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 5703 | 5888 | 3906 | 4066 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 6752 | 7007 | 461 | 256 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 8203 | 8458 | 4609 | 4814 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 3504 | 3734 | 6406 | 6636 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 492 | 242 | 9577 | 9252 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 2756 | 3031 | 6304 | 6004 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5312 | 5562 | 10703 | 11028 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7109 | 7384 | 8906 | 9206 |

There is no IMD issue for Rx of band 7 with UL DC\_8\_n28.

There is no IMD issue for Rx of band 8 with UL DC\_7\_n28.

5.44.4 ∆TIB and ∆RIB values

Table 5.44.4-1: ΔTIB,c due to EN-DC(three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-8\_n28 | 7 | 0.3 |
| 8 | 0.6 |
| n28 | 0.5 |

**Table 5.44.4-2: ΔRIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-8\_n28 | 7 | 0 |
| 8 | 0.2 |
| n28 | 0.1 |

5.44.5 REFSENS requirements

There is no reference sensitivity exception (MSD) for DC\_7-8\_n28.

## 5.45 DC\_20-28\_n3

5.45.1 Operating bands for DC

Table 5.45.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_20-28\_n3 | CA\_20-28 | n3 |

5.45.2 Configuration for DC

Table 5.45.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_20A-28A\_n3A | DC\_20A\_n3A DC\_28A\_n3A | CA\_20-28 | n3 |

5.45.3 Co-existence studies

For UE coexistence study of Band 20 + Band n3, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.45.3-1.

Table 5.45.3-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 832 | 862 | 1710 | 1785 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1664 | 1724 | 3420 | 3570 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2496 | 2586 | 5130 | 5355 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 3328 | 3448 | 6840 | 7140 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4160 | 4310 | 8550 | 8925 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 848 | 953 | 2542 | 2647 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 121 | 14 | 2558 | 2738 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 3374 | 3509 | 4252 | 4432 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 711 | 876 | 4268 | 4523 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4206 | 4371 | 5962 | 6217 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1906 | 1696 | 5084 | 5294 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6308 | 5978 | 1738 | 1543 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3691 | 3406 | 834 | 1074 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7672 | 8002 | 5038 | 5233 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6794 | 7079 | 5916 | 6156 |

For UE coexistence study of Band 28 + Band n3, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.45.3-1.

Table 5.45.3-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 703 | 748 | 1710 | 1785 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1406 | 1496 | 3420 | 3570 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2109 | 2244 | 5130 | 5355 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2812 | 2992 | 6840 | 7140 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3515 | 3740 | 8550 | 8925 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 962 | 1082 | 2413 | 2533 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 379 | 214 | 2672 | 2867 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 3116 | 3281 | 4123 | 4318 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 324 | 534 | 4382 | 4652 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 3819 | 4029 | 5833 | 6103 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2164 | 1924 | 4826 | 5066 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6437 | 6092 | 1282 | 1027 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3949 | 3634 | 1176 | 1461 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7543 | 7888 | 4522 | 4777 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6536 | 6851 | 5529 | 5814 |

IMD4 may fall into Rx of band 28 with UL DC\_20\_n3.

5.45.4 ∆TIB and ∆RIB values

Table 5.45.4-1: ΔTIB,c due to EN-DC(three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20-28\_n3 | 2 | 0.5 |
| 28 | 0.6 |
| n3 | 0.5 |

**Table 5.45.4-2: ΔRIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20-28\_n3 | 2 | 0.3 |
| 28 | 0.2 |
| n3 | 0.3 |

5.45.5 REFSENS requirements

The reference sensitivity exception (MSD) due to IMD4 for DC\_20-28\_n3 with UL DC\_20\_n3 is specified as below referring to the MSD for DC\_3A-28A\_n5A from 38.101-3.

Table 5.45.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_20A-28A\_n3A | 20 | 845 | 5 | 25 | 804 | N/A | N/A |
| 28 | 730 | 5 | 25 | 785 | 9.4 | IMD4 |
| n3 | 1750 | 5 | 25 | 1845 | N/A | N/A |
|  | | | | | | | |

## 5.46 DC\_28-66\_n66

5.46.1 Operating bands for DC

Table 5.46.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_28-66\_n66 | CA\_28-66 | n66 |

5.46.2 Configuration for DC

Table 5.46.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_28A-66A\_n66A | DC\_28A\_n66A  DC\_66A\_n66A2 | CA\_28-66 | n66 |
| NOTE 2: Only single switched UL is supported | | | |

5.46.3 Co-existence studies

For UE coexistence study of Band 28 + Band n66, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.46.3-1.

Table 5.46.3-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 703 | 748 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1406 | 1496 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2109 | 2244 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2812 | 2992 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3515 | 3740 | 8550 | 8900 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 962 | 1077 | 2413 | 2528 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 374 | 214 | 2672 | 2857 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 3116 | 3276 | 4123 | 4308 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 329 | 534 | 4382 | 4637 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 3819 | 4024 | 5833 | 6088 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2154 | 1924 | 4826 | 5056 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6417 | 6092 | 1282 | 1032 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3934 | 3634 | 1176 | 1451 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7543 | 7868 | 4522 | 4772 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6536 | 6836 | 5529 | 5804 |

For UL DC\_66A\_n66A, there is no need to study the IMD since only single switched UL is supported.

IMD4 may fall into Rx of band 66 with UL DC\_28\_n66.

5.46.4 ∆TIB and ∆RIB values

Table 5.46.4-1: ΔTIB,c due to EN-DC(three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_28-66\_n66 | 28 | 0.6 |
| 66 | 0.3 |
| n66 | 0.3 |

**Table 5.46.4-2: ΔRIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_28-66\_n66 | 28 | 0.2 |
| 66 | 0 |
| n66 | 0 |

5.46.5 REFSENS requirements

The reference sensitivity exception (MSD) due to IMD4 for DC\_28-66\_n66 with UL DC\_28\_n66 is specified as below referring to the MSD for DC\_1A-3A\_n28A from 38.101-3.

Table 5.46.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_28A-66A\_n66A | 28 | 710.5 | 5 | 25 | 765.5 | N/A | N/A |
| 66 | 1729 | 5 | 25 | 2129 | 11.0 | IMD4 |
| n66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
|  | | | | | | | |

## 5.47 DC\_7-28\_n66

5.47.1 Operating bands for DC

Table 5.47.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_7-28\_n66 | CA\_7-28 | n66 |

5.47.2 Configuration for DC

Table 5.47.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_7A-28A\_n66A  DC\_7C-28A\_n66A | DC\_7A\_n66A DC\_28A\_n66A | CA\_7-28 | n66 |

5.47.3 Co-existence studies

For UE coexistence study of Band 28 + Band n66, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.47.3-1.

Table 5.47.3-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 703 | 748 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1406 | 1496 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2109 | 2244 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2812 | 2992 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3515 | 3740 | 8550 | 8900 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 962 | 1077 | 2413 | 2528 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 374 | 214 | 2672 | 2857 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 3116 | 3276 | 4123 | 4308 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 329 | 534 | 4382 | 4637 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 3819 | 4024 | 5833 | 6088 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2154 | 1924 | 4826 | 5056 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6417 | 6092 | 1282 | 1032 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3934 | 3634 | 1176 | 1451 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7543 | 7868 | 4522 | 4772 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6536 | 6836 | 5529 | 5804 |

For UE coexistence study of Band 7 + Band n66, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.47.3-1.

Table 5.47.3-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 2500 | 2570 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 5000 | 5140 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 7500 | 7710 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 10000 | 10280 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 12500 | 12850 | 8550 | 8900 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 860 | 720 | 4210 | 4350 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 3220 | 3430 | 850 | 1060 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 6710 | 6920 | 5920 | 6130 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5720 | 6000 | 2560 | 2840 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 9210 | 9490 | 7630 | 7910 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1440 | 1720 | 8420 | 8700 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 4620 | 4270 | 8570 | 8220 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 340 | 10 | 4290 | 3940 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 9340 | 9690 | 11710 | 12060 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10130 | 10480 | 10920 | 11270 |

IMD3 may fall into Rx of band 7 with UL DC\_28\_n66.

IMD2 may fall into Rx of band 28 with UL DC\_7\_n66.

5.47.4 ∆TIB and ∆RIB values

Table 5.47.4-1: ΔTIB,c due to EN-DC(three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-28\_n66 | 7 | 0.5 |
| 28 | 0.6 |
| n66 | 0.5 |

**Table 5.47.4-2: ΔRIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-28\_n66 | 7 | 0 |
| 28 | 0.2 |
| n66 | 0 |

5.47.5 REFSENS requirements

The reference sensitivity exception (MSD) due to IMD3 for DC\_7-28\_n66 with UL DC\_28\_n66 is specified as below referring to the MSD for DC\_3A-7A\_n28A from 38.101-3.

The reference sensitivity exception (MSD) due to IMD2 for DC\_7-28\_n66 with UL DC\_7\_n66 is specified as below referring to the MSD for DC\_3A\_n7A-n28A from 38.101-3.

Table 5.47.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-28A\_n66A  DC\_7C-28A\_n66A | 7 | 2562 | 10 | 50 | 2682 | 16.9 | IMD3 |
| 28 | 743 | 5 | 25 | 798 | N/A | N/A |
| n66 | 1712.5 | 5 | 25 | 2112.5 | N/A | N/A |
| 7 | 2543 | 5 | 25 | 2663 | N/A | N/A |
| 28 | 741 | 5 | 25 | 796 | 20.0 | IMD2 |
| n66 | 1747 | 5 | 25 | 2147 | N/A | N/A |
|  | | | | | | | |

## 5.48 DC\_2-28\_n66

5.48.1 Operating bands for DC

Table 5.48.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_2-28\_n66 | CA\_2-28 | n66 |

5.48.2 Configuration for DC

Table 5.48.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-28A\_n66A | DC\_2A\_n66A DC\_28A\_n66A | CA\_2-28 | n66 |

5.48.3 Co-existence studies

For UE coexistence study of Band 28 + Band n66, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.48.3-1.

Table 5.48.3-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 703 | 748 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1406 | 1496 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2109 | 2244 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2812 | 2992 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3515 | 3740 | 8550 | 8900 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 962 | 1077 | 2413 | 2528 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 374 | 214 | 2672 | 2857 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 3116 | 3276 | 4123 | 4308 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 329 | 534 | 4382 | 4637 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 3819 | 4024 | 5833 | 6088 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2154 | 1924 | 4826 | 5056 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6417 | 6092 | 1282 | 1032 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3934 | 3634 | 1176 | 1451 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7543 | 7868 | 4522 | 4772 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6536 | 6836 | 5529 | 5804 |

For UE coexistence study of Band 2 + Band n66, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.48.3-1.

Table 5.48.3-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1850 | 1910 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3700 | 3820 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5550 | 5730 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7400 | 7640 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9250 | 9550 | 8550 | 8900 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 200 | 70 | 3560 | 3690 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 1920 | 2110 | 1510 | 1710 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 5410 | 5600 | 5270 | 5470 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 3770 | 4020 | 3220 | 3490 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 7260 | 7510 | 6980 | 7250 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 140 | 400 | 7120 | 7380 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5270 | 4930 | 5930 | 5620 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1640 | 1310 | 2310 | 1990 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8690 | 9030 | 9110 | 9420 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 8830 | 9160 | 8970 | 9290 |

IMD4 may fall into Rx of band 2 with UL DC\_28\_n66.

There is no IMD issue for Rx of band 28 with UL DC\_2\_n66.

5.48.4 ∆TIB and ∆RIB values

Table 5.48.4-1: ΔTIB,c due to EN-DC(three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-28\_n66 | 2 | 0.5 |
| 28 | 0.6 |
| n66 | 0.5 |

**Table 5.48.4-2: ΔRIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-28\_n66 | 2 | 0.3 |
| 28 | 0.2 |
| n66 | 0.3 |

5.48.5 REFSENS requirements

The reference sensitivity exception (MSD) due to IMD4 for DC\_2-28\_n66 with UL DC\_28\_n66 is specified as below referring to the MSD for DC\_1A-3A\_n28A from 38.101-3.

Table 5.48.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-28A\_n66A | 2 | 1900 | 5 | 25 | 1980 | 11 | IMD4 |
| 28 | 730 | 5 | 25 | 785 | N/A | N/A |
| n66 | 1720 | 5 | 25 | 2120 | N/A | N/A |
|  | | | | | | | |

## 5.49 Void

## 5.50 Void

## 5.51 DC\_8-40\_n1

5.51.1 Operating bands for DC

Table 5.51.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_8-40\_n1 | CA\_8-40 | n1 |

5.51.2 Configuration for DC

Table 5.51.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_8A-40A\_n1A  DC\_8A-40C\_n1A | DC\_8A\_n1A DC\_40A\_n1A | CA\_8-40 | n1 |

5.51.3 Co-existence studies

For UE coexistence study of Band 8 + Band n1, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.51.3-1.

Table 5.51.3-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 880 | 915 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 1760 | 1830 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 2640 | 2745 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 3520 | 3660 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 4400 | 4575 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1100 | 1005 | 2800 | 2895 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2925 | 3080 | 220 | 90 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4720 | 4875 | 3680 | 3810 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4845 | 5060 | 660 | 825 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6640 | 6855 | 4560 | 4725 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2010 | 2200 | 5600 | 5790 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1740 | 1540 | 7040 | 6765 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1095 | 1320 | 4180 | 3930 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5440 | 5640 | 8560 | 8835 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6480 | 6705 | 7520 | 7770 |

For UE coexistence study of Band 40 + Band n1, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.51.3-1.

Table 5.51.3-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 2300 | 2400 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 4600 | 4800 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 6900 | 7200 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 9200 | 9600 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 11500 | 12000 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 320 | 480 | 4220 | 4380 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 1440 | 1660 | 2620 | 2880 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 6140 | 6360 | 6520 | 6780 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 3360 | 3640 | 4920 | 5280 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 8060 | 8340 | 8820 | 9180 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 960 | 640 | 8440 | 8760 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 7680 | 7220 | 5620 | 5280 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3360 | 2940 | 1340 | 960 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 11120 | 11580 | 9980 | 10320 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10740 | 11160 | 10360 | 10740 |

IMD4 may fall into Rx of band 8 with UL DC\_40\_n1.

5.51.4 ∆TIB and ∆RIB values

Table 5.51.4-1: ΔTIB,c due to EN-DC(three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8-40\_n1 | 8 | 0.3 |
| 40 | 0.5 |
| n1 | 0.3 |

**Table 5.51.4-2: ΔRIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8-40\_n1 | 8 | 0.2 |
| 40 | 0.5 |
| n1 | 0 |

5.51.5 REFSENS requirements

The reference sensitivity exception (MSD) due to IMD4 for DC\_8-40\_n1 with UL DC\_40\_n1 is specified as below referring to the MSD for DC\_1A\_n8A-n40A from 38.101-3.

Table 5.51.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_8A-40A\_n1A  DC\_8A-40C\_n1A | 8 | 885 | 5 | 25 | 930 | 8.0 | IMD4 |
| 40 | 2395 | 5 | 25 | 2395 | N/A | N/A |
| n1 | 1930 | 5 | 25 | 2120 | N/A | N/A |
|  | | | | | | | |

## 5.52 DC\_1-32\_n3

5.52.1 Operating bands for DC

Table 5.52.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_1-32\_n3 | CA\_1-32 | n3 |

5.52.2 Configuration for DC

Table 5.52.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_1A-32A\_n3A | DC\_1A\_n3A | CA\_1-32 | n3 |

5.52.3 Co-existence studies

For UE coexistence study of Band 1 + Band n3, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.52.3-1.

Table 5.52.3-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 1710 | 1785 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 3420 | 3570 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 5130 | 5355 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 6840 | 7140 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 8550 | 8925 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 270 | 135 | 3630 | 3765 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2055 | 2250 | 1440 | 1650 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 5550 | 5745 | 5340 | 5550 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 3975 | 4230 | 3150 | 3435 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 7470 | 7725 | 7050 | 7335 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 270 | 540 | 7260 | 7530 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5220 | 4860 | 6210 | 5895 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1515 | 1170 | 2520 | 2190 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8760 | 9120 | 9390 | 9705 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 8970 | 9315 | 9180 | 9510 |

IMD3 and IMD5 may fall into Rx of band 32 with UL DC\_1\_n3.

5.52.4 ∆TIB and ∆RIB values

Table 5.52.4-1: ΔTIB,c due to EN-DC(three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-32\_n3 | 1 | 0.5 |
| n3 | 0.5 |

**Table 5.52.4-2: ΔRIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-32\_n3 | 1 | 0 |
| 32 | 0 |
| n3 | 0 |

5.52.5 REFSENS requirements

The reference sensitivity exception (MSD) due to IMD3 for DC\_1-32\_n3 with UL DC\_1\_n3 is specified as below referring to the MSD for DC\_1A-11A\_n3A from 38.101-3.

Table 5.52.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_1A-32A\_n3A | n3 | 1720 | 5 | 25 | 1815 | N/A | N/A |
| 32 | N/A | 5 | 25 | 1480 | 15.2 | IMD34 |
| 1 | 1960 | 5 | 25 | 2150 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. | | | | | | | |

## 5.53 DC\_3-32\_n1

5.53.1 Operating bands for DC

Table 5.53.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_3-32\_n1 | CA\_3-32 | n1 |

5.53.2 Configuration for DC

Table 5.53.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_3A-32A\_n1A | DC\_3A\_n1A | CA\_3-32 | n1 |

5.53.3 Co-existence studies

For UE coexistence study of Band 3 + Band n1, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.53.3-1.

Table 5.53.3-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 1710 | 1785 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 3420 | 3570 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 5130 | 5355 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 6840 | 7140 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 8550 | 8925 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 270 | 135 | 3630 | 3765 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2055 | 2250 | 1440 | 1650 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 5550 | 5745 | 5340 | 5550 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 3975 | 4230 | 3150 | 3435 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 7470 | 7725 | 7050 | 7335 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 270 | 540 | 7260 | 7530 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5220 | 4860 | 6210 | 5895 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1515 | 1170 | 2520 | 2190 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8760 | 9120 | 9390 | 9705 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 8970 | 9315 | 9180 | 9510 |

IMD3 and IMD5 may fall into Rx of band 32 with UL DC\_3\_n1.

5.53.4 ∆TIB and ∆RIB values

Table 5.53.4-1: ΔTIB,c due to EN-DC(three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-32\_n1 | 3 | 0.5 |
| n1 | 0.5 |

**Table 5.53.4-2: ΔRIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-32\_n1 | 3 | 0 |
| 32 | 0 |
| n1 | 0 |

5.53.5 REFSENS requirements

The reference sensitivity exception (MSD) due to IMD3 for DC\_3-32\_n1 with UL DC\_3\_n1 is specified as below referring to the MSD for DC\_1A-11A\_n3A from 38.101-3.

Table 5.53.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_3A-32A\_n1A | 3 | 1720 | 5 | 25 | 1815 | N/A | N/A |
| 32 | N/A | 5 | 25 | 1480 | 15.2 | IMD34 |
| n1 | 1960 | 5 | 25 | 2150 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. | | | | | | | |

## 5.54 DC\_7-32\_n1

### 5.54.1 Configurations for DC

Table 5.54.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-32A\_n1A | DC\_7A\_n1A |

### 5.54.2 Co-existence studies

Table 5.54.2-1 lists the Band 7A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.54.2-1: Band 7 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2500 | 2570 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5000 – 5140 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7500 – 7710 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 520 – 650 | | | 4420 – 4550 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 3020 – 3220 | | | 1270 – 1460 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 6920 – 7120 | | | 6340 – 6530 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2450 – 2620 | | | 1900 – 2000 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5520 – 5790 | | | 3190 – 3440 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1040 – 1300 | | | 8840-9100 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 9420 – 9690 | | | 8260 – 8510 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5110 – 5420 | | | 8020 – 8360 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 620 – 940 | | | 3540 – 3870 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 10180 – 10490 | | | 11920 – 12260 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10760 – 11080 | | | 11340 – 11670 | | |

Based on Table 5.54.2-1,

- 2nd order harmonics may fall into Rx frequencies of band 77

- 3rd order harmonics may fall into Rx frequencies of bands 46 and 47

- 2nd order IMD may fall into Rx frequencies of bands 71 and 79

- 3rd order IMD may fall into Rx frequencies of bands 32, 45, 50, 51, 75, 76, 91, 92, 93 and 94

- 4th order IMD may fall into Rx frequencies of bands 42, 46, 52, 77 and 78

- 5th order IMD may fall into Rx frequencies of bands 5, 6, 8, 12, 13, 14, 17, 18, 19, 20, 22, 26, 27, 28, 29, 42, 43, 44, 46, 48, 49, 67, 68, 71, 77, 78 and 85

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.54.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.54.2-2: 2UL Band 7 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD3 |
| 2400 | - | 2494 | Yes | Asia | IMD3 |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | H3 n1, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | IMD5 |
| 5470 | - | 5725 | Yes | IMD4 |
| 5150 | - | 5825 | Yes | Asia | IMD4, IMD5 |

The requirements for coexistence with protected bands exist for DC\_7A\_n1A in 38101-3.

### 5.54.3 ∆TIB and ∆RIB values

Table 5.54.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n1 | 7 | 0.6 |
| n1 | 0.5 |

**Table 5.54.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n1 | 7 | 0 |
| 32 | 0 |
| n1 | 0 |

### 5.54.4 Reference sensitivity exceptions

**Table 5.54.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_7A-32A\_n1A | n1 | 1977.5 | 5 | 25 | 2167.5 | N/A | N/A |
| 7 | 2502.5 | 5 | 25 | 2622.5 | N/A | N/A |
| 32 | N/A | 5 | N/A | 1454.5 | 15.2 | IMD3 |

## 5.55 DC\_2-66\_n7

5.55.1 Configurations for DC

Table 5.55.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_2A-66A\_n7A  DC\_2A-66A-66A\_n7A | DC\_2A\_n7A  DC\_66A\_n7A |

5.55.2 Co-existence studies

Co-existence studies on DC\_2\_n7 and DC\_66\_n7 show that there is no own Rx impact of the 3rd band from dual UL.

5.55.3 ∆TIB and ∆RIB values

For DC\_2-66\_n7, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_2-7-66, and are given in the tables below.

Table 5.55.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-66-n7 | 2 | 0.5 |
| 66 | 0.5 |
| n7 | 0.5 |

**Table 5.55.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-66-n7 | 2 | 0.3 |
| 66 | 0.5 |
| n7 | 0.5 |

5.55.4 REFSENS requirements

According to the co-existence studies, no additional MSD requirement is needed.

## 5.56 DC\_2-5\_n7

5.56.1 Configurations for DC

Table 5.56.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_2A-5A\_n7A | DC\_2A\_n7A  DC\_5A\_n7A |

5.56.2 Co-existence studies

Co-existence analysis from DC\_2\_n7 and DC\_7\_n5 show that there is no IMD impact from DC\_2\_n7 UL to band 5 DL or from DC\_5\_n7 UL to band 2 DL.

5.56.3 ∆TIB and ∆RIB values

For DC\_2-5\_n7, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_2-5-7, and are given in the tables below.

Table 5.56.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-5-n7 | 2 | 0.5 |
| 5 | 0.3 |
| n7 | 0.5 |

**Table 5.56.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-5-n7 | 2 | 0 |
| 5 | 0 |
| n7 | 0 |

5.56.4 REFSENS requirements

According to the co-existence studies, no additional MSD requirement is needed.

## 5.57 DC\_2-8\_n2

5.57.1 Configurations for DC

Table 5.57.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_2A-8A\_n2A | DC\_2A\_n2A1  DC\_8A\_n2A |
| NOTE1: Only single switched UL is supported | |

5.57.2 Co-existence studies

Co-existence analysis from DC\_8\_n2 show that IMD4 of the dual UL of DC\_8\_n2 may fall into the DL of band 2.

5.57.3 ∆TIB and ∆RIB values

For DC\_2-8\_n2, the ΔTIB,c and ΔRIB,c values are reused from the DC\_8\_n2, and are given in the tables below.

Table 5.57.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-8-n2 | 2 | 0.3 |
| 8 | 0.3 |
| n2 | 0.3 |

**Table 5.57.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-8-n2 | 2 | 0 |
| 8 | 0 |
| n2 | 0 |

5.57.4 REFSENS requirements

Based on the co-existence studies MSD due to IMD4 is required. The MSD values can be reused from DC\_8-n2.

Table 6.1.x.6-1: Reference sensitivity exceptions for PCell due to dual uplink operation for EN-DC in NR FR1 (two bands)

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | Duplex mode | IMD order |
| DC\_2-8\_n2 | 2 | 1860 | 5 | 25 | 1940 | 4 | FDD | IMD4 |
| 8 | 910 | 5 | 25 | 955 | N/A | N/A |
| n2 | 1880 | 5 | 25 | 1960 | N/A | N/A |

## 5.58 DC\_5-66\_n7

5.58.1 Configurations for DC

Table 5.58.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_5A-66A\_n7A  DC\_5A-66A-66A\_n7A | DC\_5A\_n7A  DC\_66A\_n7A |

5.58.2 Co-existence studies

Co-existence studies from lower order DCs show that the IMD3 of the dual UL of DC\_66\_n7 may fall into the DL of band 5 while there is no own Rx impact of the 3rd band from dual UL of DC\_7\_n5.

5.58.3 ∆TIB and ∆RIB values

For DC\_5-66\_n7, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_5-7-66, and are given in the tables below.

Table 5.58.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-66-n7 | 5 | 0.3 |
| 66 | 0.5 |
| n7 | 0.5 |

**Table 5.58.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-66-n7 | 5 | 0 |
| 66 | 0.5 |
| n7 | 0.5 |

5.58.4 REFSENS requirements

The MSD values for own Rx impact of the 3rd band stated in 5.58.2 are shown in the following table.

Table 5.58.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_5A-66A\_n7A  DC\_5A-66A-66A\_n7A | 5 | 835 | 5 | 25 | 880 | 18.0 | FDD | IMD3 |
| 66 | 1720 | 5 | 25 | 2120 | N/A | FDD | N/A |
| n7 | 2560 | 5 | 25 | 2680 | N/A | FDD | N/A |

## 5.59 DC\_20-32\_n1

5.59.1 Configurations for DC

Table 5.59.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_20A-32A\_n1A | DC\_20A\_n1A |

5.59.2 Co-existence studies

Co-existence analysis from DC\_20\_n1 shows that IMD5 of the dual UL may fall into the DL of band 32.

5.59.3 ∆TIB and ∆RIB values

For DC\_20-32\_n1, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_1-20-32, and are given in the tables below.

Table 5.59.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20-32-n1 | 20 | 0.3 |
| n1 | 0.5 |

**Table 5.59.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20-32-n1 | 20 | 0 |
| 32 | 0 |
| n1 | 0 |

5.59.4 REFSENS requirements

**Table 5.59.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_20A-32A\_n1A | n1 | 1950.5 | 5 | 50 | 2140.5 | N/A | N/A |
| 20 | 852.5 | 5 | 25 | 811.5 | N/A | N/A |
| 32 | N/A | 5 | N/A | 1459.5 | 4.0 | IMD5 |

## 5.60 DC\_20-32\_n3

5.60.1 Configurations for DC

Table 5.60.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_20A-32A\_n3A | DC\_20A\_n3A |

5.60.2 Co-existence studies

Co-existence analysis from DC\_20\_n3 shows that no IMD impact on the DL of band 32 from the dual UL.

5.60.3 ∆TIB and ∆RIB values

For DC\_20-32\_n3, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_3-20-32, and are given in the tables below.

Table 5.60.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20-32-n3 | 20 | 0.3 |
| n3 | 0.5 |

**Table 5.60.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20-32-n3 | 20 | 0 |
| 32 | 0 |
| n3 | 0 |

5.60.4 REFSENS requirements

No additional MSD requirement is needed.

## 5.61 DC\_1-3\_n3

### 5.61.1 Configuration for DC

**Table 5.61.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_1A-3A\_n3A | DC\_1A\_n3A  DC\_3A\_n3A2 |
| NOTE 2: Only single switched UL is supported | |

5.61.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fall-back modes. And there is no IMD issue for this DC configuration.

### 5.61.3 ∆TIB and ∆RIB values

For DC\_1-3\_n3, the ΔTIB,c and ΔRIB,c values are given in the tables below. Numbers come from DC\_1\_n3.

Table 5.61.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-3\_n3 | 1 | 0.3 |
| 3 | 0.3 |
| n3 | 0.3 |

Table 5.61.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB,c [dB] |
| --- | --- | --- |
| DC\_1-3\_n3 | 1 | 0 |
| 3 | 0 |
| n3 | 0 |

### 5.61.4 REFSENS requirements

No additional MSD requirements need to be defined.

## 5.62 DC\_1-41\_n3

### 5.62.1 Configuration for DC

**Table 5.62.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_1A-41A\_n3A  DC\_1A-41C\_n3A | DC\_1A\_n3A |

5.62.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fall-back modes. And it can be get:

- IMD5 of band 1 UL and band n3 UL falling to band 41 DL.

The MSD could reuse the value for CA\_1A-3A-41A.

### 5.62.3 ∆TIB and ∆RIB values

For DC\_1-41\_n3, the ΔTIB,c and ΔRIB,c values have been defined in TS 38.101-3..

### 5.62.4 REFSENS requirements

Table 5.62.4-1 shows the required MSD levels for the DC configuration, its value can reuse the value for CA\_1A-3A-41A.

Table 5.62.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| **DC**  **Configuration** | **EUTRA and NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL  CLRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_1A-41A\_n3A  DC\_1A-41C\_n3A | 1 | 1977.5 | 5 | 25 | 2167.5 | N/A | N/A |
| 41 | 2507.5 | 5 | 25 | 2507.5 | 5.0 | IMD5  |3\*fB1-2\*fn3| |
| n3 | 1712.5 | 5 | 25 | 1807.5 | N/A | N/A |

## 5.63 DC\_3-18\_n3

### 5.63.1 Configuration for DC

**Table 5.63.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_3A-18A\_n3A | DC\_3A\_n3A2  DC\_18A\_n3A |
| NOTE 2: Only single switched UL is supported | |

5.63.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fall-back modes. And it can be get:

- IMD4 of band 18 UL and band n3 UL falling to band 3 DL.

The MSD could reuse the value for DC\_18A\_n3A.

### 5.63.3 ∆TIB and ∆RIB values

For DC\_3-18\_n3, the ΔTIB,c and ΔRIB,c values are given in the tables below. Numbers come from DC\_18\_n3.

Table 5.63.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-18\_n3 | 3 | 0.3 |
| 18 | 0.3 |
| n3 | 0.3 |

Table 5.63.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-18\_n3 | 3 | 0 |
| 18 | 0 |
| n3 | 0 |

### 5.63.4 REFSENS requirements

Table 5.63.4-1 shows the required MSD levels for the DC configuration, its value can reuse the value for DC 18A\_n3A.

Table 5.63.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| **DC**  **Configuration** | **EUTRA and NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL  CLRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_3A-18A\_n3A | 3 | 1719 | 5 | 25 | 1814 | 4 | IMD4  |2\*fn3-2\*fB18| |
| 18 | 823 | 5 | 25 | 868 | N/A | N/A |
| n3 | 1730 | 5 | 25 | 1825 | N/A | N/A |

## 5.64 DC\_3-41\_n3

### 5.64.1 Configuration for DC

**Table 5.64.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_3A-41A\_n3A  DC\_3A-41C\_n3A | DC\_3A\_n3A2  DC\_41A\_n3A  DC\_41C\_n3A |
| NOTE 2: Only single switched UL is supported | |

5.64.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fall-back modes. And it can be get:

- IMD4 of band 41 UL and band n3 UL falling to band 3 DL.

The MSD could reuse the value for DC\_41A\_n3A.

### 5.64.3 ∆TIB and ∆RIB values

For DC\_3-41\_n3, the ΔTIB,c and ΔRIB,c values are given in the tables below. Numbers come from DC\_41\_n3.

Table 5.64.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-41\_n3 | 3 | 0.5 |
| 41 | 0.31/0.82 |
| n3 | 0.5 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz. | | |

Table 5.64.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB,c [dB] |
| --- | --- | --- |
| DC\_3-41\_n3 | 3 | 0 |
| 41 | 01/0.52 |
| n3 | 0 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2: Applicable for the frequency range of 2496-2515 MHz. | | |

### 5.64.4 REFSENS requirements

Table 5.64.4-1 shows the required MSD levels for the DC configuration, its value can reuse the value of DC\_3A\_n41A.

Table 5.64.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| **DC**  **Configuration** | **EUTRA and NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL  CLRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_3A-41A\_n3A  DC\_3A-41C\_n3A | 3 | 1770 | 5 | 25 | 1865 | 8.2 | IMD4  |2\*fB41-2\*fn3| |
| 41 | 2657.5 | 5 | 25 | 2657.5 | N/A | N/A |
| n3 | 1725 | 5 | 25 | 1820 | N/A | N/A |

## 5.65 Void

## 5.66 DC\_7-66\_n77 and DC\_7-7-66\_n77

### 5.66.1 Configuration for DC

**Table 5.66.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_7A-66A\_n77A  DC\_7A-7A-66A\_n77A  DC\_7A-7A-66A\_n77(2A)  DC\_7A-66A\_n77(2A)  DC\_7C-66A\_n77A  DC\_7C-66A\_n77(2A) | DC\_7A\_n77A  DC\_66A\_n77A |

5.66.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fall-back modes. And it can be get:

- IMD4 of band 7 UL and band n77 UL falling to band 66 DL.

- IMD5 of band 66 UL and band n77 UL falling to band 7 DL.

The MSD could reuse the value for CA\_3A-7A-26A.

### 5.66.3 ∆TIB and ∆RIB values

For DC\_7-66\_n77 and DC\_7-7-66\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below. Numbers come from LTE CA\_5A-7A-66A.

Table 5.66.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-66\_n77  DC\_7-7-66\_n77 | 7 | 0.5 |
| 66 | 0.6 |
| n77 | 0.8 |

Table 5.66.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-66\_n77  DC\_7-7-66\_n77 | 7 | 0.5 |
| 66 | 0.5 |
| n77 | 0.5 |

### 5.66.4 REFSENS requirements

Table 5.66.4-1 shows the required MSD levels for the DC configuration.

The MSD levels are derived from the text proposal in R4-2014129 and R4-2015711

Table 5.66.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-66A\_n77A  DC\_7C-66A\_n77A  DC\_7A-7A-66A\_n77A  DC\_7A-66A\_n77(2A)  DC\_7C-66A\_n77(2A)  DC\_7A-7A-66A\_n77(2A) | 7 | 2550 | 5 | 25 | 2685 | N/A | N/A |
| 66 | 1750 | 5 | 25 | 2150 | 8.7 | IMD4 |
| n77 | 3625 | 10 | 50 | 3475 | N/A | N/A |
| 66 | 1715 | 5 | 25 | 2115 | N/A | N/A |
| 7 | 2550 | 5 | 25 | 2670 | 5.2 | IMD5 |
| n77 | 4190 | 10 | 50 | 4190 | N/A | N/A |
| 66 | 1720 | 5 | 25 | 2120 | N/A | N/A |
| 7 | 2520 | 5 | 25 | 2640 | 3.4 | IMD5 |
| n77 | 3900 | 10 | 50 | 3900 | N/A | N/A |

## 5.67 DC\_2-5\_n48

### 5.67.1 Configuration for DC

**Table 5.67.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_2A-5A\_n48A  DC\_2A-5A\_n48B | DC\_2A\_n48A  DC\_5A\_n48A |

5.67.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be got:

- The IMD3 of UL configuration on DC\_5\_n48 will impact of the Band 2 DL.

### 5.67.3 ∆TIB and ∆RIB values

For DC\_2-5\_n48, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_2-5-48.

Table 5.67.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-5\_n48 | 2 | 0.6 |
| 5 | 0.3 |
| n48 | 0.8 |

Table 5.67.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-5\_n48 | 2 | 0.2 |
| 5 | 0 |
| n48 | 0.5 |

### 5.67.4 REFSENS requirements

Table 5.67.4-1 shows the required MSD levels for the DC configuration.

Table 5.67.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| **DC**  **Configuration** | **EUTRA and NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL  CLRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-5A\_n48A  DC\_2A-5A\_n48B | 2 | 1882 | 5 | 25 | 1962 | 15.6 | IMD3  | fn48-2\*fB5| |
| 5 | 839 | 5 | 25 | 884 | N/A | N/A |
| n48 | 3640 | 5 | 25 | 3640 | N/A | N/A |

## 5.68 DC\_2-13\_n48

### 5.68.1 Configuration for DC

**Table 5.68.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_2A-13A\_n48A  DC\_2A-13A\_n48B | DC\_2A\_n48A  DC\_13A\_n48A |

5.68.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be got:

- The IMD3 of UL configuration on DC\_13\_n48 will impact of the Band 2 DL.

### 5.68.3 ∆TIB and ∆RIB values

For DC\_2-13\_n48, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_2-13-48.

Table 5.68.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-13\_n48 | 2 | 0.6 |
| 13 | 0.3 |
| n48 | 0.8 |

Table 5.68.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-13\_n48 | 2 | 0.2 |
| 13 | 0 |
| n48 | 0.5 |

### 5.68.4 REFSENS requirements

Table 5.68.4-1 shows the required MSD levels for the DC configuration.

Table 5.68.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| **DC**  **Configuration** | **EUTRA and NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL  CLRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-13A\_n48A  DC\_2A-13A\_n48B | 2 | 1903.5 | 5 | 25 | 1983.5 | 15.6 | IMD3  | fn48-2\*fB13| |
| 13 | 784.5 | 5 | 25 | 753.5 | N/A | N/A |
| n48 | 3552.5 | 5 | 25 | 3552.5 | N/A | N/A |

## 5.69 Void

## 5.70 DC\_5-46\_n66

### 5.70.1 Configuration for DC

**Table 5.70.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_5A-46A\_n66A | DC\_5A\_n66A  DC\_46A\_n66A |

5.70.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be got:

- The IMD4 and IMD5 of UL configuration on DC\_5\_n66 will impact of the Band 46 DL

### 5.70.3 ∆TIB and ∆RIB values

For DC\_5-46\_n66, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for DC\_46-66\_n5.

Table 5.70.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-46\_n66 | 5 | 0.3 |
| 46 | 0 |
| n66 | 0.3 |

Table 5.70.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-46\_n66 | 5 | 0 |
| 46 | 0 |
| n66 | 0 |

### 5.70.4 REFSENS requirements

Table 5.70.4-1 shows the required MSD levels for the DC configuration.

Table 5.70.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| **DC**  **Configuration** | **EUTRA and NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL  CLRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_5A-46A\_n66A | 5 | 847 | 5 | 25 | 892 | N/A | N/A |
| 46 | 5163 | 10 | 50 | 5163 | 9.01 | IMD4  |2\*fB5+2\*fn66| |
| n66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
| NOTE 1: This band is subject to IMD5 also which MSD is not specified | | | | | | | |

## 5.71 DC\_5-66\_n48 and DC\_5-66-66\_n48

### 5.71.1 Configuration for DC

**Table 5.71.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_5A-66A\_n48A  DC\_5A-66A\_n48B  DC\_5A-66A-66A\_n48A  DC\_5A-66A-66A\_n48B | DC\_5A\_n48A  DC\_66A\_n48A |

5.71.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. There is no IMD impact to their own third band RX.

### 5.71.3 ∆TIB and ∆RIB values

For DC\_5-66\_n48, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_5-66-48.

Table 5.71.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-66\_n48  DC\_5-66-66\_n48 | 5 | 0.3 |
| 66 | 0.6 |
| n48 | 0.8 |

Table 5.71.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-66\_n48  DC\_5-66-66\_n48 | 5 | 0 |
| 66 | 0.2 |
| n48 | 0.5 |

### 5.71.4 REFSENS requirements

There is no additional MSD requirement for this band combination.

## 5.72 DC\_5-66\_n77

### 5.72.1 Configuration for DC

**Table 5.72.1-1: Inter-band EN-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_5A-66A\_n77A | DC\_5A\_n77A  DC\_66A\_n77A |

5.72.2 Co-existence study

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be got:

- The IMD3 of UL DC\_5A\_n77A may impact to band 66 Rx.

### 5.72.3 ∆TIB and ∆RIB values

For DC\_5-66\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_5-66\_n78.

Table 5.72.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-66\_n77 | 5 | 0.6 |
| 66 | 0.6 |
| n77 | 0.8 |

Table 5.72.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-66\_n77 | 5 | 0.2 |
| 66 | 0.2 |
| n77 | 0.5 |

### 5.72.4 REFSENS requirements

Table 5.72.4-1 shows the required MSD levels for the DC configuration.

Table 5.72.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **E-UTRA and NR Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| **DC**  **Configuration** | **EUTRA and NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL  CLRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_5A-66A\_n77A | 5 | 826.5 | 5 | 25 | 871.5 | N/A | N/A |
| 66 | 1742 | 5 | 25 | 2142 | 13.2 | IMD3  |fn77-2\*fB5| |
| n77 | 3795 | 10 | 50 | 3795 | N/A | N/A |

## 5.73 DC\_1-42\_n3

5.73.1 Configurations for DC\_1-42\_n3

Table 5.73.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-42A\_n3A | DC\_1A\_n3A  DC\_42A\_n3A |
| DC\_1A-42C\_n3A | DC\_1A\_n3A  DC\_42A\_n3A  DC\_42C\_n3A |

5.73.2 Co-existence studies

When Uplink EN-DC configuration is DC\_1A\_n3A, IMD4 of (B1 - n3) will fall into Rx band of Band 42.

5.73.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.73.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_1-42\_n3 | 1 | 0.3 |
| 42 | 0.8 |
| n3 | 0.6 |

Table 5.73.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_1-42\_n3 | 1 | 0 |
| 42 | 0.5 |
| n3 | 0.2 |

5.73.4 Reference sensitivity exceptions

As mentioned above, IMD4 of B1 and n3 to Band42 Rx needs to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.73.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_1A-42A\_n3A | 1 | 1922.5 | 5 | 25 | 2112.5 | N/A | FDD | N/A |
| n3 | 1782.5 | 5 | 25 | 1877.5 | N/A | FDD | N/A |
| 42 | 3425 | 5 | 25 | 3425 | 13.0 | TDD | IMD4 |

## 5.74 DC\_8-42\_n3

5.74.1 Configurations for DC\_8-42\_n3

Table 5.74.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-42A\_n3A | DC\_8A\_n3A  DC\_42A\_n3A |
| DC\_8A-42C\_n3A | DC\_8A\_n3A  DC\_42A\_n3A  DC\_42C\_n3A |

5.74.2 Co-existence studies

When Uplink EN-DC configuration is DC\_8A\_n3A, IMD3 and IMD5 of (B8 - n3) will fall into Rx band of Band 42.

5.74.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.74.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_8-42\_n3 | 8 | 0.6 |
| 42 | 0.8 |
| n3 | 0.6 |

Table 5.74.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_8-42\_n3 | 8 | 0.2 |
| 42 | 0.5 |
| n3 | 0.2 |

5.74.4 Reference sensitivity exceptions

As mentioned above, IMD3 of B8 and n3 to Band42 Rx needs to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.74.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_8A-42A\_n3A | 8 | 900 | 5 | 25 | 945 | N/A | FDD | N/A |
| n3 | 1740 | 5 | 25 | 1835 | N/A | FDD | N/A |
| 42 | 3540 | 5 | 25 | 3540 | 16.3 | TDD | IMD3 |

## 5.75 DC\_3-18\_n28

### 5.75.1 Configurations for DC

Table 5.75.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-18A\_n28A | DC\_3A\_n28A  DC\_18A\_n28A |

### 5.75.2 Co-existence studies

Based on co-existence studies of DC\_3\_n28 and DC\_18\_n28, there is no the 3rd band issue.

### 5.75.3 ∆TIB and ∆RIB values

For DC\_3-18\_n28, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.75.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-18\_n28 | 3 | 0.3 |
| 18 | 0.5 |
| n28 | 0.3 |

**Table 5.75.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-18\_n28 | 3 | 0 |
| 18 | 0 |
| n28 | 0 |

### 5.75.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.76 DC\_2-66\_n77

5.76.1 Operating bands for DC

Table 5.76.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink configuration |
| --- | --- |
| DC\_2A-66A\_n77A | DC\_2A\_n77A DC\_66A\_n77A |

5.76.2 Co-existence studies

For UE coexistence study of Band 2 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.76.2-1.

Table 5.76.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1850 | 1910 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3700 | 3820 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5550 | 5730 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 7400 | 7640 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9250 | 9550 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1390 | 2350 | 5150 | 6110 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | -500 | 520 | 4690 | 6550 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 7000 | 8020 | 8450 | 10310 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1350 | 2430 | 7990 | 10750 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8850 | 9930 | 11750 | 14510 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | -4700 | -2780 | 10300 | 12220 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | -14950 | -11290 | -4340 | -3200 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 15050 | 18710 | 10700 | 11840 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | -8900 | -6080 | 870 | 2850 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 13600 | 16420 | 12150 | 14130 |

For UE coexistence study of Band 66 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.76.2-2.

Table 5.76.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1780 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3560 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5340 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7120 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8900 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1520 | 2490 | 5010 | 5980 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 780 | 260 | 4820 | 6690 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 6720 | 7760 | 8310 | 10180 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 930 | 2040 | 8120 | 10890 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8430 | 9540 | 11610 | 14380 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 4980 | 3040 | 10020 | 11960 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 15090 | 11420 | 3820 | 2640 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 14910 | 18580 | 10140 | 11320 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 9180 | 6340 | 1260 | 3270 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 13320 | 16160 | 11730 | 13740 |

The Rx impacts can be identified as below,

* 2nd, 4th and 5th order IMD products generated by DC\_2\_n77 uplink may fall into own Rx of band 66
* 2nd, 4th and 5th order IMD products generated by DC\_66\_n77 uplink may fall into own Rx of band 2

5.76.3 ∆TIB and ∆RIB values

Table 5.76.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-66\_n77 | 2 | 0.6 |
| 66 | 0.6 |
| n77 | 0.8 |

**Table 5.76.4-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-66\_n77 | 2 | 0.2 |
| 66 | 0.2 |
| n77 | 0.5 |

### 5.76.4 Reference sensitivity exceptions

As stated in 5.76.2, for MSD requirement caused by IMDs is specified below accordingly.

Table 5.76.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-66A\_n77A | 2 | 1855 | 5 | 25 | 1935 | N/A | N/A |
| 66 | 1765 | 5 | 25 | 2185 | 29.2 | IMD2 |
| n77 | 4040 | 5 | 25 | 4040 | N/A | N/A |
| 2 | 1905 | 5 | 25 | 1985 | M/A | N/A |
| 66 | 1720 | 5 | 25 | 2120 | 10.4 | IMD4 |
| n77 | 3595 | 5 | 25 | 3595 | N/A | N/A |
| 2 | 1885 | 5 | 25 | 1965 | M/A | N/A |
| 66 | 1775 | 5 | 25 | 2195 | 4.0 | IMD5 |
| n77 | 3925 | 5 | 25 | 3925 | N/A | N/A |
| 2 | 1880 | 5 | 25 | 1960 | 32.1 | IMD2 |
| 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |
| n77 | 3700 | 5 | 25 | 3700 | N/A | N/A |
| 2 | 1860 | 5 | 25 | 1940 | 9.1 | IMD4 |
| 66 | 1775 | 5 | 25 | 2195 | N/A | N/A |
| n77 | 3385 | 5 | 25 | 3385 | N/A | N/A |
| 2 | 1900 | 5 | 25 | 1980 | 4.2 | IMD5 |
| 66 | 1770 | 5 | 25 | 2170 | N/A | N/A |
| n77 | 3645 | 5 | 25 | 3645 | N/A | N/A |

## 5.77 DC\_2-48\_n77

5.77.1 Operating bands for DC

Table 5.77.1-1: Inter-band DC configuration (three bands)

| DC  configuration | Uplink  configuration |
| --- | --- |
| DC\_2A-48A\_n77A | DC\_2A\_n77A  DC\_48A\_n77A |

5.77.2 Co-existence studies

For UE coexistence study of Band 2 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.77.2-1.

Table 5.77.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1850 | 1910 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3700 | 3820 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5550 | 5730 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 7400 | 7640 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9250 | 9550 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1390 | 2350 | 5150 | 6110 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 500 | 520 | 4690 | 6550 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 7000 | 8020 | 8450 | 10310 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1350 | 2430 | 7990 | 10750 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8850 | 9930 | 11750 | 14510 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 4700 | 2780 | 10300 | 12220 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 14950 | 11290 | 4340 | 3200 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 15050 | 18710 | 10700 | 11840 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 8900 | 6080 | 870 | 2850 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 13600 | 16420 | 12150 | 14130 |

For UE coexistence study of Band 48 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.77.2-2.

Table 5.77.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 3550 | 3700 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 7100 | 7400 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 10650 | 11100 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 14200 | 14800 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 17750 | 18500 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 400 | 650 | 6850 | 7900 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 2900 | 4100 | 2900 | 4850 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 10400 | 11600 | 10150 | 12100 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 6450 | 7800 | 6200 | 9050 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 13950 | 15300 | 13450 | 16300 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 1300 | 800 | 13700 | 15800 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 13250 | 9500 | 11500 | 10000 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 16750 | 20500 | 17500 | 19000 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 5500 | 2500 | 4500 | 2250 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 17000 | 20000 | 17250 | 19500 |

The Rx impacts can be identified as below,

* There is no IMD issue for Rx of band 2 with UL DC\_48\_n77.
* 5th order harmonics generated by DC\_2\_n77 uplink may fall into own Rx of band 48.
* As the duplex mode for band 48 and n77 is TDD and both bands shall be synchronized to align uplink and downlink timing across and within the two bands for the U.S. C-band (R4-2008118), thus there is no impact to this TDD band 48 with the UL DC\_2\_n77.

5.77.3 ∆TIB and ∆RIB values

Table 5.77.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-48\_n77 | 2 | 0.3 |
| 48 | 0.6 |
| n77 | 0.5 |

**Table 5.77.3-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-48\_n77 | 2 | 0 |
| 48 | 0.2 |
| n77 | 0.1 |

### 5.77.4 Reference sensitivity exceptions

There is no reference sensitivity exception (MSD) for DC\_2-48\_n77 combination.

## 5.78 DC\_2-13\_n77

5.78.1 Operating bands for DC

Table 5.78.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink configuration |
| --- | --- |
| DC\_2A-13A\_n77A | DC\_2A\_n77A DC\_13A\_n77A |

5.78.2 Co-existence studies

For UE coexistence study of Band 2 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.78.2-1.

Table 5.78.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1850 | 1910 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3700 | 3820 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5550 | 5730 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 7400 | 7640 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9250 | 9550 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1390 | 2350 | 5150 | 6110 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 500 | 520 | 4690 | 6550 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 7000 | 8020 | 8450 | 10310 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1350 | 2430 | 7990 | 10750 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8850 | 9930 | 11750 | 14510 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 4700 | 2780 | 10300 | 12220 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 14950 | 11290 | 4340 | 3200 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 15050 | 18710 | 10700 | 11840 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 8900 | 6080 | 870 | 2850 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 13600 | 16420 | 12150 | 14130 |

For UE coexistence study of Band 13 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.78.2-2.

Table 5.78.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 777 | 787 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1554 | 1574 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2331 | 2361 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 3108 | 3148 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3885 | 3935 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 2513 | 3423 | 4077 | 4987 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 2646 | 1726 | 5813 | 7623 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4854 | 5774 | 7377 | 9187 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1869 | 939 | 9113 | 11823 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5631 | 6561 | 10677 | 13387 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 6846 | 5026 | 8154 | 9974 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 16023 | 12413 | 152 | 1092 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 13977 | 17587 | 6408 | 7348 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 11046 | 8326 | 4239 | 6069 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 11454 | 14174 | 8931 | 10761 |

The Rx impacts can be identified as below,

* There is no IMD issue for Rx of band 13 with UL DC\_2\_n77.
* 3rd order IMD products generated by DC\_13\_n77 uplink may fall into own Rx of band 2

5.78.3 ∆TIB and ∆RIB values

Table 5.78.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-13\_n77 | 2 | 0.6 |
| 13 | 0.5 |
| n77 | 0.8 |

**Table 5.78.3-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-13\_n77 | 2 | 0.2 |
| 13 | 0.2 |
| n77 | 0.5 |

### 5.78.4 Reference sensitivity exceptions

As stated in 5.78.2, for MSD requirement caused by IMDs is specified below accordingly.

Table 5.78.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-13A\_n77A | 2 | 1864 | 5 | 25 | 1944 | 16.0 | IMD3 |
| 13 | 783 | 5 | 25 | 752 | N/A | N/A |
| n77 | 3510 | 5 | 25 | 3510 | N/A | N/A |

## 5.79 DC\_2-5\_n77

5.79.1 Operating bands for DC

Table 5.79.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink configuration |
| --- | --- |
| DC\_2A-5A\_n77A | DC\_2A\_n77A DC\_5A\_n77A |

5.79.2 Co-existence studies

For UE coexistence study of Band 2 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.79.2-1.

Table 5.79.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1850 | 1910 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3700 | 3820 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5550 | 5730 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 7400 | 7640 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9250 | 9550 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1390 | 2350 | 5150 | 6110 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 500 | 520 | 4690 | 6550 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 7000 | 8020 | 8450 | 10310 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1350 | 2430 | 7990 | 10750 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8850 | 9930 | 11750 | 14510 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 4700 | 2780 | 10300 | 12220 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 14950 | 11290 | 4340 | 3200 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 15050 | 18710 | 10700 | 11840 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 8900 | 6080 | 870 | 2850 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 13600 | 16420 | 12150 | 14130 |

For UE coexistence study of Band 5 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.79.2-2.

Table 5.79.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 824 | 849 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1648 | 1698 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2472 | 2547 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 3296 | 3396 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4120 | 4245 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 2451 | 3376 | 4124 | 5049 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 2552 | 1602 | 5751 | 7576 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4948 | 5898 | 7424 | 9249 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1728 | 753 | 9051 | 11776 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5772 | 6747 | 10724 | 13449 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 6752 | 4902 | 8248 | 10098 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 15976 | 12351 | 96 | 904 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 14024 | 17649 | 6596 | 7596 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 10952 | 8202 | 4053 | 5928 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 11548 | 14298 | 9072 | 10947 |

The Rx impacts can be identified as below..

* 5th order IMD products generated by DC\_2\_n77 uplink may fall into own Rx of band 5.
* 3rd order IMD products generated by DC\_5\_n77 uplink may fall into own Rx of band 2.

5.79.3 ∆TIB and ∆RIB values

Table 5.79.3-1: ΔTIB,

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-5\_n77 | 2 | 0.6 |
| 5 | 0.6 |
| n77 | 0.8 |

**Table 5.79.3-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-5\_n77 | 2 | 0.2 |
| 5 | 0.2 |
| n77 | 0.5 |

### 5.79.4 Reference sensitivity exceptions

As stated in 5.79.2, for MSD requirement caused by IMDs is specified below accordingly.

Table 5.79.5-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-5A\_n77A | 2 | 1907.5 | 5 | 25 | 1987.5 | N/A | N/A |
| 5 | 842.5 | 5 | 25 | 887.5 | 3.8 | IMD5 |
| n77 | 3305 | 5 | 25 | 3305 | N/A | N/A |
| 2 | 1907 | 5 | 25 | 1987 | 16.5 | IMD3 |
| 5 | 846.5 | 5 | 25 | 891.5 | N/A | N/A |
| n77 | 3680 | 5 | 25 | 3680 | N/A | N/A |

## 5.80 DC\_5-13\_n66

5.80.1 Operating bands for DC

Table 5.80.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_5A-13A\_n66A | DC\_5A\_n66A  DC\_13A\_n66A |

5.80.2 Co-existence studies

For UE coexistence study of Band 5 + Band n66, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.80.2-1.

Table 5.80.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 824 | 849 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1648 | 1698 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2472 | 2547 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 3296 | 3396 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4120 | 4245 | 8550 | 8900 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 861 | 956 | 2534 | 2629 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 132 | 12 | 2571 | 2736 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 3358 | 3478 | 4244 | 4409 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 692 | 837 | 4281 | 4516 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4182 | 4327 | 5954 | 6189 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 1912 | 1722 | 5068 | 5258 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6296 | 5991 | 1686 | 1516 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7664 | 7969 | 5006 | 5176 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 3692 | 3432 | 873 | 1088 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6778 | 7038 | 5892 | 6107 |

For UE coexistence study of Band 13 + Band n66, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.80.2-2.

Table 5.80.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 777 | 787 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1554 | 1574 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2331 | 2361 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 3108 | 3148 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3885 | 3935 | 8550 | 8900 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 923 | 1003 | 2487 | 2567 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 226 | 136 | 2633 | 2783 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 3264 | 3354 | 4197 | 4347 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 551 | 651 | 4343 | 4563 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4041 | 4141 | 5907 | 6127 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 2006 | 1846 | 4974 | 5134 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6343 | 6053 | 1438 | 1328 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7617 | 7907 | 4818 | 4928 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 3786 | 3556 | 1059 | 1229 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6684 | 6914 | 5751 | 5921 |

The Rx impacts can be identified as below..

* 4th order IMD products generated by DC\_5\_n66 uplink may fall into own Rx of band 13.
* There is no IMD issue for Rx of band 5 with UL DC\_13\_n66.

5.80.3 ∆TIB and ∆RIB values

Table 5.80.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-13\_n66 | 5 | 0.3 |
| 13 | 0.3 |
| n66 | 0.3 |

**Table 5.80.4-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-13\_n66 | 5 | 0 |
| 13 | 0 |
| n66 | 0 |

### 5.80.4 Reference sensitivity exceptions

As stated in 5.80.2, the requirement caused by IMDs is specified below accordingly.

Table 5.80.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_5A-13A\_n66A | 5 | 840 | 5 | 25 | 885 | N/A | N/A |
| 13 | 781 | 5 | 25 | 750 | 9.4 | IMD4 |
| n66 | 1770 | 5 | 25 | 2170 | N/A | N/A |

## 5.81 DC\_13-66\_n77

5.81.1 Operating bands for DC

Table 5.81.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink configuration |
| --- | --- |
| DC\_13A-66A\_n77A | DC\_13A\_n77A DC\_66A\_n77A |

5.81.2 Co-existence studies

For UE coexistence study of Band 13 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.81.2-1.

Table 5.81.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 777 | 787 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1554 | 1574 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2331 | 2361 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 3108 | 3148 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3885 | 3935 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 2513 | 3423 | 4077 | 4987 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 2646 | 1726 | 5813 | 7623 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4854 | 5774 | 7377 | 9187 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1869 | 939 | 9113 | 11823 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5631 | 6561 | 10677 | 13387 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 6846 | 5026 | 8154 | 9974 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 16023 | 12413 | 152 | 1092 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 13977 | 17587 | 6408 | 7348 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 11046 | 8326 | 4239 | 6069 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 11454 | 14174 | 8931 | 10761 |

For UE coexistence study of Band 66 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.81.2-2.

Table 5.81.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1780 | 3300 | 4200 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3560 | 6600 | 8400 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5340 | 9900 | 12600 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7120 | 13200 | 16800 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8900 | 16500 | 21000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1520 | 2490 | 5010 | 5980 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 780 | 260 | 4820 | 6690 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 6720 | 7760 | 8310 | 10180 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 930 | 2040 | 8120 | 10890 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8430 | 9540 | 11610 | 14380 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 4980 | 3040 | 10020 | 11960 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 15090 | 11420 | 3820 | 2640 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 14910 | 18580 | 10140 | 11320 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 9180 | 6340 | 1260 | 3270 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 13320 | 16160 | 11730 | 13740 |

The Rx impacts can be identified as below..

* 3rd order IMD products generated by DC\_13\_n77 uplink may fall into own Rx of band 66.
* 3rd order IMD products generated by DC\_66\_n77 uplink may fall into own Rx of band 13

5.81.3 ∆TIB and ∆RIB values

Table 5.81.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_13-66\_n77 | 13 | 0.5 |
| 66 | 0.6 |
| n77 | 0.8 |

**Table 5.81.3-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_13-66\_n77 | 13 | 0.3 |
| 66 | 0.3 |
| n77 | 0.5 |

5.81.4 Reference sensitivity exceptions

As stated in 5.81.2, for MSD requirement caused by IMDs is specified below accordingly.

Table 5.81.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_13A-66A\_n77A | 13 | 777 | 5 | 25 | 746 | N/A | N/A |
| 66 | 1746 | 5 | 25 | 2146 | 17.1 | IMD3 |
| n77 | 3700 | 10 | 50 | 3700 | N/A | N/A |
| 13 | 781 | 5 | 25 | 750 | 15.2 | IMD3 |
| 66 | 1710 | 5 | 25 | 2110 | N/A | N/A |
| n77 | 4170 | 10 | 50 | 4170 | N/A | N/A |

## 5.82 DC\_13-66\_n5

5.82.1 Operating bands for DC

Table 5.82.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_13A-66A\_n5A | DC\_13A\_n5A  DC\_66A\_n5A |

5.82.2 Co-existence studies

For UE coexistence study of Band 13 + Band n5, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.82.2-1.

Table 5.82.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 777 | 787 | 824 | 849 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1554 | 1574 | 1648 | 1698 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2331 | 2361 | 2472 | 2547 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 3108 | 3148 | 3296 | 3396 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3885 | 3935 | 4120 | 4245 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 37 | 72 | 1601 | 1636 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 705 | 750 | 861 | 921 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 2378 | 2423 | 2425 | 2485 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1482 | 1537 | 1685 | 1770 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 3155 | 3210 | 3249 | 3334 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 144 | 74 | 3202 | 3272 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 2619 | 2509 | 2324 | 2259 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4073 | 4183 | 3932 | 3997 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 993 | 898 | 713 | 633 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 4026 | 4121 | 3979 | 4059 |

For UE coexistence study of Band 66 + Band n5, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.82.2-2.

Table 5.82.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1780 | 824 | 849 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3560 | 1648 | 1698 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5340 | 2472 | 2547 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\*fy\_low | 4\*fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7120 | 3296 | 3396 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8900 | 4120 | 4245 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 956 | 861 | 2534 | 2629 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 2571 | 2736 | 132 | 12 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4244 | 4409 | 3358 | 3478 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 4281 | 4516 | 692 | 837 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5954 | 6189 | 4182 | 4327 |
| Two-tone 4th order IMD products | |2\*fx\_low – 2\*fy\_high| | |2\*fx\_high – 2\*fy\_low| | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 1722 | 1912 | 5068 | 5258 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1686 | 1516 | 6296 | 5991 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5006 | 5176 | 7664 | 7969 |
| Two-tone 5th order IMD products | |2\*fx\_low – 3\*fy\_high| | |2\*fx\_high – 3\*fy\_low| | |2\*fy\_low – 3\*fx\_high| | |2\*fy\_high – 3\*fx\_low| |
| IMD frequency limits (MHz) | 873 | 1088 | 3692 | 3432 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5892 | 6107 | 6778 | 7038 |

The Rx impacts can be identified as below..

* There is no IMD issue for Rx of band 66 with UL DC\_13\_n5.
* 4th order IMD products generated by DC\_66\_n77 uplink may fall into own Rx of band 13.

5.82.3 ∆TIB and ∆RIB values

Table 5.82.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_13-66\_n5 | 13 | 0.5 |
| 66 | 0.3 |
| n5 | 0.5 |

**Table 5.82.3-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_13-66\_n5 | 13 | 0 |
| 66 | 0 |
| n5 | 0 |

### 5.82.4 Reference sensitivity exceptions

As stated in 5.82.2, the requirement caused by IMDs is specified below accordingly.

Table 5.82.5-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_13A-66A\_n5A | 13 | 781 | 5 | 25 | 750 | 9.4 | IMD4 |
| 66 | 1770 | 5 | 25 | 2170 | N/A | N/A |
| n5 | 840 | 5 | 25 | 885 | N/A | N/A |

## 5.83 DC\_1-18\_n28

### 5.83.1 Configurations for DC

Table 5.83.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-18A\_n28A | DC\_1A\_n28A  DC\_18A\_n28A |

### 5.83.2 Co-existence studies

Based on co-existence studies of DC\_1\_n28 and DC\_18\_n28, 5th order IMD generated by dual uplink of Band 18 + Band n28 may fall into own Rx of band 1. The MSD value of this configuration can follow CA\_1A-18A-28A with UL CA\_18A-28A case. Since band 18 is only used by KDDI, no additional MSD requirement need to be specified for this configuration considering KDDI spectrum (band n28 UL is limited to 718MHz – 728MHz).

### 5.83.3 ∆TIB and ∆RIB values

For DC\_1-18\_n28, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.83.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-18\_n28 | 1 | 0.3 |
| 18 | 0.5 |
| n28 | 0.5 |

**Table 5.83.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-18\_n28 | 1 | 0 |
| 18 | 0 |
| n28 | 0 |

### 5.83.4 Reference sensitivity exceptions

As stated in 5.83.2, there is no additional MSD requirement for this configuration.

## 5.84 DC\_1-18\_n41

### 5.84.1 Configurations for DC

Table 5.84.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-18A\_n41A | DC\_1A\_n41A  DC\_18A\_n41A |

### 5.84.2 Co-existence studies

Based on co-existence studies of DC\_1\_n41 and DC\_18\_n41, 5th order IMD generated by dual uplink of Band 1 + Band n41 may fall into own Rx of band 18. The MSD value of this configuration can follow CA\_1A-18A-41A with UL CA\_1A-41A case. Since band 18 is only used by KDDI, no additional MSD requirement need to be specified for this configuration considering KDDI spectrum (band n41 is limited to 2595MHz – 2645MHz).

### 5.84.3 ∆TIB and ∆RIB values

For DC\_1-18\_n41, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.84.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-18\_n41 | 1 | 0.5 |
| 18 | 0.3 |
| n41 | 0.5 |

**Table 5.84.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-18\_n41 | 1 | 0 |
| 18 | 0 |
| n41 | 0 |

### 5.84.4 Reference sensitivity exceptions

As stated in 5.84.2, there is no additional MSD requirement for this configuration.

## 5.85 DC\_5-7\_n7

5.85.1 Configurations for DC

Table 5.85.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_5A-7A\_n7A | DC\_5A\_n7A DC\_7A\_n7A2 |
| NOTE 2: Only single switched UL is supported | |

### 5.85.2 Co-existence studies

Co-existence studies have been performed for lower order combinations.

Co-existence analysis for DC\_5\_n7 UL shows that 3rd and 5th IMD may fall in DL band 5.

Co-existence analysis for DC\_7\_n7 UL is not needed since only switched UL is supported.

5.85.3 ∆TIB and ∆RIB values

Table 5.85.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_5-7\_n7 | 5 | 0.5 |
| 7 | 0.3 |
| n7 | 0.3 |

Table 5.85.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_5-7\_n7 | 5 | 0 |
| 7 | 0 |
| n7 | 0 |

5.85.4 Reference sensitivity exceptions

Based on co-existence studies additional MSD is needed defined in Table 7.3B.2.3.5.2-1 of 38.101-3.

Table 6. x.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_5A-7A\_n7A | 5 | 834 | 5 | 25 | 879 | 12 | IMD34 |
| 7 | 2527 | 10 | 50 | 2647 | N/A | N/A |
| n7 | 2547 | 10 | 50 | 2667 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. | | | | | | | |

## 5.86 DC\_2-28\_n7

5.86.1 Configurations for DC

Table 5.86.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_2A-28A\_n7A | DC\_2A\_n7A DC\_28A\_n7A |
|  | |

### 5.86.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. of DC\_2A\_n7A and DC\_28A\_n7A, where:

- No IMD product caused by DC\_2A\_n7A fall into own Rx of band 28.

- No IMD product caused by DC\_28A\_n7A fall into own Rx of band 2.

5.86.3 ∆TIB and ∆RIB values

Table 5.86.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_2-28\_n7 | 2 | 0.5 |
| 28 | 0.3 |
| n7 | 0.5 |

Table 5.86.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_2-28\_n7 | 2 | 0 |
| 28 | 0 |
| n7 | 0 |

5.86.4 Reference sensitivity exceptions

No further REFSENS exceptions needed.

## 5.87 DC\_28-66\_n7

5.87.1 Configurations for DC

Table 5.87.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_28A-66A\_n7A | DC\_28A\_n7A DC\_66A\_n7A |
|  | |

### 5.87.2 Co-existence studies

Co-existence studies have been performed for lower order combinations of DC\_28A\_n7A and DC\_66A\_n7A, where:

- No IMD product caused by DC\_28A\_n7A fall into own Rx of band 66.

- 2nd IMD product caused by DC\_66A\_n7A may fall into own Rx of band 28.

5.87.3 ∆TIB and ∆RIB values

Values are reused from CA including same bands as given in 36.101.

Table 5.87.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_28-66\_n7 | 28 | 0.6 |
| 66 | 0.5 |
| n7 | 0.5 |

Table 5.87.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_28-66\_n7 | 28 | 0.2 |
| 66 | 0.5 |
| n7 | 0.5 |

5.87.4 Reference sensitivity exceptions

Based on co-existence analysis it is found that MSD is needed due to 2nd IMD falling into own Rx band of 28. Therefor additional MSD is needed defined in Table 7.3B.2.3.5.2-1 of 38.101-3.

Table 5. x.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_28A-66A\_n7A | 28 | 735 | 5 | 25 | 790 | 27.6 | IMD2 |
| 66 | 1715 | 5 | 25 | 2115 | N/A | N/A |
| n7 | 2505 | 5 | 50 | 2625 | N/A | N/A |
|  | | | | | | | |

## 5.88 DC\_7-28\_n2

5.88.1 Configurations for DC

Table 5.88.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_7A-28A\_n2A | DC\_7A\_n2A DC\_28A\_n2A |
|  | |

### 5.88.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. of DC\_7A\_n2A and DC\_28A\_n2A, where:

- No IMD product caused by DC\_7A\_n2A fall into own Rx of band 28.

- IMD2 product caused by DC\_28A\_n2A may fall into own Rx of band 7.

5.88.3 ∆TIB and ∆RIB values

Table 5.88.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_7-28\_n2 | 7 | 0.5 |
| 28 | 0.3 |
| n2 | 0.5 |

Table 5.88.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_7-28\_n2 | 7 | 0 |
| 28 | 0 |
| n2 | 0 |

5.88.4 Reference sensitivity exceptions

Based on co-existence studies additional MSD is needed defined in Table 7.3B.2.3.5.2-1 of 38.101-3.

Table 5. x.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_7A-28A\_n2A | 7 | 2510 | 10 | 50 | 2630 | 27.6 | IMD2 |
| 28 | 730 | 5 | 25 | 785 | N/A | N/A |
| n2 | 1900 | 5 | 25 | 1980 | N/A | N/A |
|  | | | | | | | |

## 5.89 DC\_2-7\_n7

5.89.1 Configurations for DC

Table 5.89.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_2A-7A\_n7A | DC\_2A\_n7A DC\_7A\_n7A2 |
| NOTE 2: Only single switched UL is supported | |

### 5.89.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. No further analysis is needed.

5.89.3 ∆TIB and ∆RIB values

Table 5.89.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_2-7\_n7 | 2 | 0.5 |
| 7 | 0.5 |
| n7 | 0.5 |

Table 5.89.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_2-7\_n7 | 2 | 0 |
| 7 | 0 |
| n7 | 0 |

5.89.4 Reference sensitivity exceptions

No further REFSENS exceptions needed.

## 5.90 DC\_2A-71A\_n71A

5.90.1 Configurations for DC

Table 5.90.1-1: Inter-band EN-DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_2A-71A\_n71A | DC\_2A\_n71A |

Note that DC\_71\_n71 is not used as uplink configuration.

### 5.90.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. No further analysis is needed.

5.90.3 ∆TIB and ∆RIB values

Table 5.90.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_2-71\_n71 | 2 | 0.3 |
| 71 | 0.3 |
| n71 |

Table 5.90.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_2-71\_n71 | 2 | 0 |
| 71 | 0 |
| n71 |

5.90.4 Reference sensitivity exceptions

REFSENS exceptions for DC\_2A-71A\_n71A due to band 71 uplink harmonic into band 2 is already specified in Table 7.3B.2.3.1-1 of TS 38.101-3.

Wgap exception have been defined for DC\_71A\_n71A, no further MSD is needed.

## 5.91 DC\_66A-71A\_n71A

5.91.1 Configurations for DC

Table 5.91.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_66A-71A\_n71A | DC\_66A\_n71A |

Note that DC\_71\_n71 is not used as uplink configuration.

### 5.91.2 Co-existence studies

Co-existence studies have been performed for lower order combinations. No further analysis is needed.

5.91.3 ∆TIB and ∆RIB values

Table 5.91.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_66-71\_n71 | 66 | 0.3 |
| 71 | 0.3 |
| n71 |

Table 5.91.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_66-71\_n71 | 66 | 0 |
| 71 | 0 |
| n71 |

5.91.4 Reference sensitivity exceptions

Wgap exception have been defined for DC\_71A\_n71A, no further MSD is needed.

## 5.92 DC\_7-66\_n7/ DC\_7-66-66\_n7

5.92.1 Configurations for DC

Table 5.92.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-66A\_n7A  DC\_7A-66A-66A\_n7A | DC\_7A\_n7A2  DC\_66A\_n7A |
| NOTE 2: Only single switched UL is supported | |

5.92.2 Co-existence studies

For UE coexistence study of Band 66 + Band n7, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.46.3-1.

Table 5.92.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 2500 | 2570 | 1710 | 1780 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 5000 | 5140 | 3420 | 3560 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 7500 | 7710 | 5130 | 5340 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 10000 | 10280 | 6840 | 7120 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 12500 | 12850 | 8550 | 8900 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 860 | 720 | 4210 | 4350 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 3220 | 3430 | 850 | 1060 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 6710 | 6920 | 5920 | 6130 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5720 | 6000 | 2560 | 2840 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 9210 | 9490 | 7630 | 7910 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1440 | 1720 | 8420 | 8700 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 4620 | 4270 | 8570 | 8220 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 340 | 10 | 4290 | 3940 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 9340 | 9690 | 11710 | 12060 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10130 | 10480 | 10920 | 11270 |

For UL DC\_7A\_n7A, there is no need to study the IMD since only single switched UL is supported.

IMD4 may fall into Rx of band 7 with UL DC\_66\_n7.

5.92.3 ∆TIB and ∆RIB values

For DC\_7-66\_n7 and DC\_7-66-66\_n7, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination DC\_66\_n7, and are given in the tables below.

Table 5.92.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-66\_n7  DC\_7-66-66\_n7 | 7 | 0.5 |
| 66 | 0.5 |
| n7 | 0.5 |

**Table 5.92.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-66\_n7  DC\_7-66-66\_n7 | 7 | 0.5 |
| 66 | 0.5 |
| n7 | 0.5 |

5.92.4 Reference sensitivity exceptions

The reference sensitivity exception (MSD) due to IMD4 for DC\_7-66\_n7/ DC\_7-66-66\_n7 with UL DC\_66\_n7 is specified as below referring to the MSD for DC\_66A\_n7A from 38.101-3.

Table 5.92.x.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-66A\_n7A  DC\_7A-66A-66A\_n7A | 7 | 2555 | 10 | 50 | 2675 | 15 | IMD4 |
| 66 | 1730 | 5 | 25 | 2130 | N/A | N/A |
| n7 | 2515 | 10 | 50 | 2635 | N/A | N/A |
|  | | | | | | | |

## 5.93 DC\_2-7\_n77

### 5.93.1 Configurations for DC

Table 5.93.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-7A\_n77A  DC\_2A-7C\_n77A  DC\_2A-7A-7A\_n77A  DC\_2A-7A\_n77(2A)  DC\_2A-7C\_n77(2A)  DC\_2A-7A-7A\_n77(2A) | DC\_2A\_n77A  DC\_7A\_n77A |

### 5.93.2 Co-existence studies

For UE coexistence study of Band 2 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.93.2-1.

**Table 5.93.2-1: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 3300 | 4200 | 1850 | 1910 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 6600 | 8400 | 3700 | 3820 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 9900 | 12600 | 5550 | 5730 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 13200 | 16800 | 7400 | 7640 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 16500 | 21000 | 9250 | 9550 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 2350 | 1390 | 5150 | 6110 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 4690 | 6550 | 500 | 520 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8450 | 10310 | 7000 | 8020 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 7990 | 10750 | 1350 | 2430 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 11750 | 14510 | 8850 | 9030 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 4700 | 2780 | 10300 | 12220 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 11290 | 14950 | 3200 | 4340 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 15050 | 18710 | 10700 | 11840 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 6080 | 8900 | 2850 | 870 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 12150 | 14130 | 13600 | 16420 |

For UE coexistence study of Band 7 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.93.2-2

**Table 5.93.2-2: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 3300 | 4200 | 2500 | 2570 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 6600 | 8400 | 5000 | 5140 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 9900 | 12600 | 7500 | 7710 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 13200 | 16800 | 10000 | 10280 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 16500 | 21000 | 12500 | 12850 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1700 | 730 | 5800 | 6770 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 4030 | 5900 | 800 | 1840 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 9100 | 10970 | 8300 | 9340 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 7330 | 10100 | 3300 | 4410 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 12400 | 15170 | 10800 | 11010 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 3400 | 1460 | 11600 | 13540 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 10630 | 14300 | 5800 | 6980 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 15700 | 19370 | 13300 | 14480 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 4760 | 7600 | 900 | 1110 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 14100 | 16110 | 14900 | 17740 |

Based on co-existence study as presented in the table 5.93.2-1 and 5.93.2-2, own Rx impact of the 3rd band is shown as the followings.

* 4th order IMD generated by dual uplink of Band 7 + Band n77 may also fall into own Rx of band 2
* 5th order IMD generated by dual uplink of Band 2 + Band n77 may also fall into own Rx of band 7

### 5.93.3 ∆TIB and ∆RIB values

Table 5.93.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-7\_n77  DC\_2-7-7\_n77 | 2 | 0.6 |
| 7 | 0.5 |
| n77 | 0.8 |

**Table 5.93.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-7\_n77  DC\_2-7-7\_n77 | 2 | 0.2 |
| 7 | 0.5 |
| n77 | 0.5 |

### 5.93.4 Reference sensitivity exceptions

The MSD requirement due to 4th order IMD for DC\_2-7\_n78 can be reused for DC\_2-7\_n77.

By adjusting the centre frequency of uplink of Band 2 + Band n77, the MSD requirement due to 5th order IMD for DC\_2-7\_n77 can be similar as the requirements of DC\_3-7\_n77 since the source of IMD is the same.

Table 5.93.4-1 lists the MSD required for DC\_2-7\_n77.

**Table 5.93.4-1: MSD for the DC configuration due to IMD issue (three bands)**

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-7A\_n77A  DC\_2A-7C\_n77A  DC\_2A-7A-7A\_n77A  DC\_2A-7A\_n77(2A)  DC\_2A-7C\_n77(2A)  DC\_2A-7A-7A\_n77(2A) | 2 | 1870 | 5 | 25 | 1950 | 8.6 | IMD4 |
| 7 | 2550 | 5 | 25 | 2685 | N/A | N/A |
| n77 | 3525 | 10 | 50 | 3475 | N/A | N/A |
| 2 | 1860 | 5 | 25 | 1940 | N/A | N/A |
| 7 | 2540 | 5 | 25 | 2660 | 3.4 | IMD5 |
| n77 | 4120 | 10 | 50 | 4120 | N/A | N/A |

## 5.94 Void

## 5.95 DC\_20-40\_n78

5.95.1 Operating bands for DC

Table 5.95.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_20-40\_n78 | CA\_20-40 | n78 | No |

5.95.2 Configurations for DC

Table 5.95.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_20A-40A\_n78A | DC\_20A\_n78A  DC\_40A\_n78A | CA\_20A-40A | n78 |

5.95.3 Co-existence studies

Based on co-existence studies of Band 20 + Band n78 captured in 37.863-01-01 there is no IMD interfering band 40

And based on co-existence studies of Band 40 + Band n78 captured in 37.716-11-11, MSD shall be considered since

- 3rd order IMD generated by dual uplink of the two bands may fall into own Rx of band 20.

5.95.4 ∆TIB and ∆RIB values

It is proposed to re-use relaxation values from DC\_8-40-n78 which is very similar.

Table 5.95.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20-40-n78 | 20 | 0.6 |
| 40 | 0.35 |
| n78 | 0.85 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one E-UTRA band and without simultaneous Rx/Tx. | | |

**Table 5.95.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20-40-n78 | 20 | 0.2 |
| 40 | 0.45 |
| n78 | 0.55 |
| NOTE 5: Only applicable for UE supporting inter-band carrier aggregation with uplink in one E-UTRA band and without simultaneous Rx/Tx. | | |

5.95.5 REFSENS requirements

It is proposed to re-use IMD3 MSD value from DC\_8-40-n78 which is very similar.

Table 5.95.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_20A-40A\_n78A | 20 | 856 | 5 | 25 | 815 | 19.8 | IMD3 |
| 40 | 2302.5 | 5 | 25 | 2302.5 | N/A | N/A |
| n78 | 3790 | 10 | 50 | 3790 | N/A | N/A |

## 5.96 DC\_3-18\_n41

### 5.96.1 Configurations for DC

Table 5.96.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-18A\_n41A | DC\_3A\_n41A  DC\_18A\_n41A |

### 5.96.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fall-back modes. And it can be get:

- IMD2 of band 18 UL and band n41 UL falling to band 3 DL.

- IMD2 and IMD3 of band 3 UL and band n41 UL falling to band 18 DL.

### 5.96.3 ∆TIB and ∆RIB values

For DC\_3-18\_n41, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.96.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-18\_n41 | 3 | 0.6 |
| 18 | 0.3 |
| n41 | 0.31 |
| 0.82 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2 Applicable for the frequency range of 2496-2515 MHz. | | |

**Table 5.96.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-18\_n41 | 3 | 0 |
| 18 | 0 |
| n41 | 01 |
| 0.52 |
| NOTE 1: Applicable for the frequency range of 2515-2690 MHz.  NOTE 2 Applicable for the frequency range of 2496-2515 MHz. | | |

### 5.96.4 Reference sensitivity exceptions

Table 5.96.4-1 shows the required MSD:

Table 5.96.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc**  **(MHz)** | **UL/DL BW**  **(MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD**  **(dB)** | **IMD order** |
| DC\_3-18\_n41 | 18 | 820 | 5 | 25 | 865 | 28.9 | IMD2 |
| 3 | 1765 | 5 | 25 | 1860 | N/A | N/A |
| n41 | 2630 | 10 | 50 | 2630 | N/A | N/A |
| 18 | 820 | 5 | 25 | 865 | 19.0 | IMD3 |
| 3 | 1725 | 5 | 25 | 1820 | N/A | N/A |
| n41 | 2585 | 5 | 25 | 2585 | N/A | N/A |
| 3 | 1755 | 5 | 25 | 1850 | 28.8 | IMD2 |
| n41 | 2670 | 10 | 50 | 2670 | N/A | N/A |
| 18 | 820 | 5 | 25 | 865 | MSD | N/A |

## 5.97 DC\_7-25\_n77

5.97.1 Operating bands for DC

Table 5.97.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-25A\_n77A  DC\_7A-7A-25A\_n77A  DC\_7C-25A\_n77A  DC\_7C-25A-25A\_n77A  DC\_7A-25A-25A\_n77A  DC\_7A-7A-25A-25A\_n77A | DC\_7A\_n77A  DC\_25A\_n77A |

### 5.97.2 Co-existence studies

For UE coexistence study of Band 7 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.97.2-1.

**Table 5.97.2-1: Harmonic and IMD analysis for DC\_7\_n77**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 2500 | 2570 | 3300 | 4200 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 5000 | 5140 | 6600 | 8400 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 7500 | 7710 | 9900 | 12600 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 730 | 1700 | 5800 | 6770 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 800 | 1840 | 4030 | 5900 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8300 | 9340 | 9100 | 10970 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 3300 | 4410 | 7330 | 10100 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 10800 | 11910 | 12400 | 15170 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 3400 | 1460 | 11600 | 13540 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 14300 | 10630 | 6980 | 5800 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 15700 | 19370 | 13300 | 14480 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 7600 | 4760 | 1110 | 900 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 14900 | 17740 | 14100 | 16110 |

For UE coexistence study of Band 25 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.97.2-2.

**Table 5.97.2-2: Harmonic and IMD analysis for DC\_25\_n77**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1915 | 3300 | 4200 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3830 | 6600 | 8400 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5745 | 9900 | 12600 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1385 | 2350 | 5150 | 6115 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 500 | 530 | 4685 | 6550 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7000 | 8030 | 8450 | 10315 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1350 | 2445 | 7985 | 10750 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8850 | 9945 | 11750 | 14515 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 4700 | 2770 | 10300 | 12230 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 14950 | 11285 | 4360 | 3200 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 15050 | 18715 | 10700 | 11860 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 8900 | 6070 | 855 | 2850 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 13600 | 16430 | 12150 | 14145 |

Based on co-existence study as presented in the table 5.97.2-1 and 5.97.2-2, own Rx impact is shown in the following.

* The 4th order IMD generated by dual uplink of Band 7 + Band n77 may fall into own Rx of band 25 and n77
* The 2nd harmonic of Band 25 uplink may fall into own Rx of band n77
* The 2nd, 4th and 5th order IMD generated by dual uplink of Band 25 + Band n77 may fall into own Rx of band 25
* The 5th order IMD generated by dual uplink of Band 25 + Band n77 may fall into own Rx of band 7
* The 4th and 5th order IMD generated by dual uplink of Band 25 + Band n77 may fall into own Rx of Band n77

### 5.97.3 ∆TIB and ∆RIB values

The same relaxation values as DC\_2-7\_n77 is used.

Table 5.97.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-25\_n77  DC\_7-7-25\_n77  DC\_7-25-25\_n77  DC\_7-7-25-25\_n77 | 7 | 0.5 |
| 25 | 0.6 |
| n77 | 0.8 |

**Table 5.97.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-25\_n77  DC\_7-7-25\_n77  DC\_7-25-25\_n77  DC\_7-7-25-25\_n77 | 7 | 0.5 |
| 25 | 0.2 |
| n77 | 0.5 |

### 5.97.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the 4th order IMD for 25+n77 falling into band 25 and the 5th order IMD falling into band 7. This issue is similar to DC\_2-7\_n77 and the same MSD is used.

**Table 5.97.4-1: MSD for the DC configuration due to IMD issue (three bands)**

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-25A\_n77A  DC\_7A-7A-25A\_n77A  DC\_7C-25A\_n77A  DC\_7C-25A-25A\_n77A  DC\_7A-25A-25A\_n77A  DC\_7A-7A-25A-25A\_n77A | 7 | 2550 | 5 | 25 | 2670 | N/A | N/A |
| 25 | 1870 | 5 | 25 | 1950 | 8.6 | IMD4 |
| n77 | 3525 | 10 | 50 | 3525 | N/A | N/A |
| 7 | 2540 | 5 | 25 | 2660 | 3.4 | IMD5 |
| 25 | 1860 | 5 | 25 | 1940 | N/A | N/A |
| n77 | 4120 | 10 | 50 | 4120 | N/A | N/A |

## 5.98 DC\_7-25\_n78

5.98.1 Operating bands for DC

Table 5.98.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-25A\_n78A  DC\_7A-7A-25A\_n78A  DC\_7C-25A\_n78A  DC\_7A-25A-25A\_n78A  DC\_7A-7A-25A-25A\_n78A  DC\_7C-25A-25A\_n78A | DC\_7A\_n78A  DC\_25A\_n78A |

### 5.98.2 Co-existence studies

For UE coexistence study of Band 7 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.98.2-1.

**Table 5.98.2-1: Harmonic and IMD analysis for DC\_7\_n78**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 2500 | 2570 | 3300 | 3800 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 5000 | 5140 | 6600 | 7600 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 7500 | 7710 | 9900 | 11400 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 730 | 1300 | 5800 | 6370 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1200 | 1840 | 4030 | 5100 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8300 | 8940 | 9100 | 10170 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 3700 | 4410 | 7330 | 8900 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 10800 | 11510 | 12400 | 13970 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 2600 | 1460 | 11600 | 12740 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 12700 | 10630 | 6980 | 6200 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 15700 | 17770 | 13300 | 14080 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 6400 | 4760 | 1110 | 100 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 14900 | 16540 | 14100 | 15310 |

For UE coexistence study of Band 25 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.98.2-2.

**Table 5.98.2-2: Harmonic and IMD analysis for DC\_25\_n78**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1915 | 3300 | 3800 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3830 | 6600 | 7600 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5745 | 9900 | 11400 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1385 | 1950 | 5150 | 5715 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 100 | 530 | 4685 | 5750 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7000 | 7630 | 8450 | 9515 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1750 | 2445 | 7985 | 9550 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8850 | 9545 | 11750 | 13315 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 3900 | 2770 | 10300 | 11430 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 13350 | 11285 | 4360 | 3600 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 15050 | 17115 | 10700 | 11460 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 7700 | 6070 | 855 | 2050 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 13600 | 15230 | 12150 | 13345 |

Based on co-existence study as presented in the table 5.98.2-1 and 5.98.2-2, own Rx impact is shown in the following.

* The 4th order IMD generated by dual uplink of Band 7 + Band n78 may fall into own Rx of band 25 and n78
* The 2nd harmonic of Band 25 uplink may fall into own Rx of band n78
* The 2nd, 4th and 5th order IMD generated by dual uplink of Band 25 + Band n78 may fall into own Rx of band 25
* The 4th order IMD generated by dual uplink of Band 25 + Band n78 may fall into own Rx of Band n78

### 5.98.3 ∆TIB and ∆RIB values

The same relaxation values as DC\_2-7\_n78 is used.

Table 5.98.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-25\_n78  DC\_7-7-25\_n78  DC\_7-25-25\_n78  DC\_7-7-25-25\_n78 | 7 | 0.5 |
| 25 | 0.6 |
| n78 | 0.8 |

**Table 5.98.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-25\_n78  DC\_7-7-25\_n78  DC\_7-25-25\_n78  DC\_7-7-25-25\_n78 | 7 | 0.5 |
| 25 | 0.2 |
| n78 | 0.5 |

### 5.98.4 Reference sensitivity exceptions

The IMD issue specifc to 3DL/2UL is the 4th order IMD for 25+n78 falling into band 25. This issue is similar to DC\_2-7\_n78 and the same MSD is used.

**Table 5.98.4-1: MSD for the DC configuration due to IMD issue (three bands)**

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-25A\_n78A  DC\_7A-7A-25A\_n78A  DC\_7C-25A\_n78A  DC\_7A-25A-25A\_n78A  DC\_7A-7A-25A-25A\_n78A  DC\_7C-25A-25A\_n78A | 7 | 2550 | 5 | 25 | 2670 | N/A | N/A |
| 25 | 1870 | 5 | 25 | 1950 | 8.6 | IMD4 |
| n78 | 3525 | 10 | 50 | 3525 | N/A | N/A |

## 5.99 DC\_25-66\_n77

5.99.1 Operating bands for DC

Table 5.99.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_25A-66A\_n77A  DC\_25A-25A-66A\_n77A | DC\_25A\_n77A  DC\_66A\_n77A |

### 5.99.2 Co-existence studies

For UE coexistence study of Band 25 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.99.2-1.

**Table 5.99.2-1: Harmonic and IMD analysis for DC\_25\_n77**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1915 | 3300 | 4200 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3830 | 6600 | 8400 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5745 | 9900 | 12600 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1385 | 2350 | 5150 | 6115 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 500 | 530 | 4685 | 6550 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7000 | 8030 | 8450 | 10315 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1350 | 2445 | 7985 | 10750 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8850 | 9945 | 11750 | 14515 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 4700 | 2770 | 10300 | 12230 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 14950 | 11285 | 4360 | 3200 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 15050 | 18715 | 10700 | 11860 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 8900 | 6070 | 855 | 2850 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 13600 | 16430 | 12150 | 14145 |

For UE coexistence study of Band 66 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.99.2-2.

**Table 5.99.2-2: Harmonic and IMD analysis for DC\_66\_n77**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1710 | 1780 | 3300 | 4200 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3420 | 3560 | 6600 | 8400 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5130 | 5340 | 9900 | 12600 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1520 | 2490 | 5010 | 5980 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 780 | 260 | 4820 | 6690 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 6720 | 7760 | 8310 | 10180 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 930 | 2040 | 8120 | 10890 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8430 | 9540 | 11610 | 14380 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | -4980 | -3040 | 10020 | 11960 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 15090 | 11420 | 3820 | 2640 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 14910 | 18580 | 10140 | 11320 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 9180 | 6340 | 1260 | 3270 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 13320 | 16160 | 11730 | 13740 |

Based on co-existence study as presented in the table 5.99.2-1 and 5.99.2-2, own Rx impact is shown in the following.

* The 2nd harmonic of band 25 may fall into own Rx of band n77
* The 2nd, 4th and 5th order IMD generated by dual uplink of 25+n77 may fall into own Rx of band 25 and 66
* The 4th and 5th order IMD generated by dual uplink of 25+n77 may fall into own Rx of n77
* The 2nd harmonic of band 66 may fall into own Rx of band n77
* The 2nd, 4th and 5th order IMD generated by dual uplink of 66+n77 may fall into own Rx of band 25 and 66
* The 4th and 5th order IMD generated by dual uplink of 66+n77 may fall into own Rx of band n77

### 5.99.3 ∆TIB and ∆RIB values

The same relaxation values as DC\_2-66\_n77 is used for DC\_25-66\_n77.

Table 5.99.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_25-66\_n77  DC\_25-25-66\_n77 | 25 | 0.6 |
| 66 | 0.6 |
| n77 | 0.8 |

**Table 5.99.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_25-66\_n77  DC\_25-25-66\_n77 | 25 | 0.2 |
| 66 | 0.2 |
| n77 | 0.5 |

### 5.99.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the IMD2/4/5 for 25+n77 falling into band 66 and for 66+n77 falling into band 25. This issues are similar to DC\_2-66\_n77 and the same MSD is used.

Table 5.99.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_25A-66A\_n77A  DC\_25A-25A-66A\_n77A | 25 | 1855 | 5 | 25 | 1935 | N/A | N/A |
| 66 | 1765 | 5 | 25 | 2165 | 29.2 | IMD2 |
| n77 | 4020 | 10 | 25 | 4020 | N/A | N/A |
| 25 | 1905 | 5 | 25 | 1985 | M/A | N/A |
| 66 | 1720 | 5 | 25 | 2120 | 10.4 | IMD4 |
| n77 | 3595 | 10 | 25 | 3595 | N/A | N/A |
| 25 | 1885 | 5 | 25 | 1965 | M/A | N/A |
| 66 | 1775 | 5 | 25 | 2175 | 4.0 | IMD5 |
| n77 | 3915 | 10 | 25 | 3915 | N/A | N/A |
| 25 | 1880 | 5 | 25 | 1960 | 32.1 | IMD2 |
| 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |
| n77 | 3700 | 10 | 25 | 3700 | N/A | N/A |
| 25 | 1860 | 5 | 25 | 1940 | 9.1 | IMD4 |
| 66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
| n77 | 3385 | 10 | 25 | 3385 | N/A | N/A |
| 25 | 1900 | 5 | 25 | 1980 | 4.2 | IMD5 |
| 66 | 1770 | 5 | 25 | 2170 | N/A | N/A |
| n77 | 3645 | 10 | 25 | 3645 | N/A | N/A |

## 5.100 DC\_25-66\_n78

5.100.1 Operating bands for DC

Table 5.100.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_25A-66A\_n78A  DC\_25A-25A-66A\_n78A | DC\_25A\_n78A  DC\_66A\_n78A |

### 5.100.2 Co-existence studies

For UE coexistence study of Band 25 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.100.2-1.

**Table 5.100.2-1: Harmonic and IMD analysis for DC\_25\_n78**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1915 | 3300 | 3800 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3830 | 6600 | 7600 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5745 | 9900 | 11400 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1385 | 1950 | 5150 | 5715 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 100 | 530 | 4685 | 5750 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7000 | 7630 | 8450 | 9515 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1750 | 2445 | 7985 | 9550 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8850 | 9545 | 11750 | 13315 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 3900 | 2770 | 10300 | 11430 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 13350 | 11285 | 4360 | 3600 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 15050 | 17115 | 10700 | 11460 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 7700 | 6070 | 855 | 2050 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 13600 | 15230 | 12150 | 13345 |

For UE coexistence study of Band 66 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.100.2-2.

**Table 5.100.2-2: Harmonic and IMD analysis for DC\_66\_n78**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1710 | 1780 | 3300 | 3800 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3420 | 3560 | 6600 | 7600 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5130 | 5340 | 9900 | 11400 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1520 | 2090 | 5010 | 5580 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 380 | 260 | 4820 | 5890 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 6720 | 7360 | 8310 | 9380 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1330 | 2040 | 8120 | 9690 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8430 | 9140 | 11610 | 13180 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 4180 | 3040 | 10020 | 11160 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 13490 | 11420 | 3820 | 3040 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 14910 | 16980 | 10140 | 10920 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 980 | 6340 | 1260 | 2470 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 13320 | 14960 | 11730 | 12940 |

Based on co-existence study as presented in the table 5.100.2-1 and 5.100.2-2, own Rx impact is shown in the following.

* The 2nd harmonic of band 25 may fall into own Rx of band n78
* The 2nd, 4th and 5th order IMD generated by dual uplink of 25+n78 may fall into own Rx of band 25
* The 4th order IMD generated by dual uplink of 25+n78 may fall into own Rx of band 66
* The 4th and 5th order IMD generated by dual uplink of 25+n78 may fall into own Rx of n78
* The 2nd harmonic of band 66 may fall into own Rx of band n78
* The 2nd, 4th and 5th order IMD generated by dual uplink of 66+n78 may fall into own Rx of band 25 and 66
* The 4th and 5th order IMD generated by dual uplink of 66+n78 may fall into own Rx of band n78

### 5.100.3 ∆TIB and ∆RIB values

The same relaxation values as DC\_2-66\_n78 is used for DC\_25-66\_n78.

Table 5.100.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_25-66\_n78  DC\_25-25-66\_n78 | 25 | 0.6 |
| 66 | 0.6 |
| n78 | 0.8 |

**Table 5.100.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_25-66\_n78  DC\_25-25-66\_n78 | 25 | 0.2 |
| 66 | 0.2 |
| n78 | 0.5 |

### 5.100.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the IMD4/5 for 25+n78 falling into band 66 and IMD2/4/5 for 66+n78 falling into band 25. This issues are similar to DC\_2-66\_n78 and the same MSD is used.

Table 5.100.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_25A-66A\_n78A  DC\_25A-25A-66A\_n78A | 25 | 1880 | 5 | 25 | 1960 | M/A | N/A |
| 66 | 1760 | 5 | 25 | 2160 | 10.4 | IMD4 |
| n78 | 3480 | 10 | 50 | 3480 | N/A | N/A |
| 25 | 1880 | 5 | 25 | 1960 | 32.1 | IMD2 |
| 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |
| n78 | 3700 | 10 | 50 | 3700 | N/A | N/A |
| 25 | 1880 | 5 | 25 | 1960 | 9.1 | IMD4 |
| 66 | 1770 | 5 | 25 | 2170 | N/A | N/A |
| n78 | 3350 | 10 | 50 | 3350 | N/A | N/A |
| 25 | 1900 | 5 | 25 | 1980 | 4.2 | IMD5 |
| 66 | 1770 | 5 | 25 | 2170 | N/A | N/A |
| n78 | 3645 | 10 | 25 | 3645 | N/A | N/A |

## 5.101 DC\_2-29\_n78

5.101.1 Operating bands for DC

Table 5.101.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_2-29\_n78 | CA\_2-29 | n78 | DC\_2\_n78 |

5.101.2 Configurations for DC

Table 5.101.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_2A-29A\_n78A | DC\_2A\_n78A | CA\_2A-29A | n78 |

5.101.3 Co-existence studies

Based on co-existence studies of DC\_2A-29A\_n78A with 2UL, it can get that:

- no IMD of band 2 UL and band n78 UL falling to band 29 DL

5.101.4 ∆TIB and ∆RIB values

For DC\_2A-29A\_n78A, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_2-13-48, and are given in the tables below.

Table 5.101.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-29-n78 | 2 | 0.6 |
| n78 | 0.8 |

**Table 5.101.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-29-n78 | 2 | 0.2 |
| n78 | 0.5 |

5.101.5 REFSENS requirements

Although DC\_29\_n78 is not defined, 5th order harmonic mixing is from the band n78 UL and DL on band 29 existed and need be considered here. DC\_29\_n78’s MSD can refer to DC\_28-n78 values. Below table can be merged into 38.101-3 Table 7.3B.2.3.2-1 and Table 7.3B.2.3.2-2 respectively:

Table 5.101.5-1: Reference sensitivity exceptions (MSD) due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n78 | 292 | 28 | 25 |  |  |  |  |  |  |  |  |  |
| NOTE 2: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that  with  the DL carrier frequency in the lower band and the UL carrier frequency in the higher band, both in MHz. | | | | | | | | | | | | |

Table 5.101.5-2: Uplink configuration for reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / SCS / Channel bandwidth of the affected DL band / UL RB allocation of the agressor band | | | | | | | | | | | | | |
| UL band | DL band | SCS of UL band  (kHz) | 5 MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n78 | 29 | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |

## 5.102 DC\_29-66\_n78

5.102.1 Operating bands for DC

Table 5.102.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_29-66\_n78 | CA\_29-66 | n78 | DC\_66\_n78 |

5.102.2 Configurations for DC

Table 5.102.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_29A-66A\_n78A | DC\_66A\_n78A | CA\_29A-66A | n78 |

5.102.3 Co-existence studies

Based on co-existence studies of DC\_29A-66A\_n78A with 2UL, it can get that:

- no IMD of band 66 UL and band n78 UL falling to band 29 DL

Although DC\_29\_n78 is not defined, 5th order harmonic mixing is from the band n78 UL and DL on band 29 existed and need be considered here.

5.102.4 ∆TIB and ∆RIB values

For DC\_29A-66A\_n78A, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_13-48-66, and are given in the tables below.

Table 5.102.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_29-66-n78 | 66 | 0.6 |
| n78 | 0.8 |

**Table 5.102.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_29-66-n78 | 66 | 0.2 |
| n78 | 0.5 |

5.102.5 REFSENS requirements

Although DC\_29\_n78 is not defined, 5th order harmonic mixing is from the band n78 UL and DL on band 29 existed and need be considered here. DC\_29\_n78’s MSD can refer to DC\_28-n78 values. Below table can be merged into 38.101-3 Table 7.3B.2.3.2-1 and Table 7.3B.2.3.2-2 respectively:

Table 5.102.5-1: Reference sensitivity exceptions (MSD) due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n78 | 292 | 28 | 25 |  |  |  |  |  |  |  |  |  |
| NOTE 2: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that  with  the DL carrier frequency in the lower band and the UL carrier frequency in the higher band, both in MHz. | | | | | | | | | | | | |

Table 5.102.5-2: Uplink configuration for reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / SCS / Channel bandwidth of the affected DL band / UL RB allocation of the agressor band | | | | | | | | | | | | | |
| UL band | DL band | SCS of UL band  (kHz) | 5 MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n78 | 29 | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |

## 5.103 DC\_1-21\_n28

### 5.103.1 Configurations for DC

The frequency range in band n28 is restricted for this band combination to 728 - 738 MHz for the UL and 783-793 MHz for the DL because only a certain operator uses band 21. This restriction is mentioned in TP for DC\_21\_n28 (R4-2100352).

Table 5.103.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-21A\_n28A | DC\_1A\_n28A  DC\_21A\_n28A |

### 5.103.2 Co-existence studies

Based on co-existence studies of DC\_1\_n28 and DC\_21\_n28, own Rx impact of the 3rd band is the followings.

- 2nd order IMD products generated by DC\_21\_n28 uplink may fall into own Rx of band 1.

- 3rd order IMD products generated by DC\_21\_n28 uplink may fall into own Rx of band 1.

### 5.103.3 ∆TIB and ∆RIB values

For DC\_1-21\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_1-21-28, and are given in the tables below.

Table 5.103.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-21\_n28 | 1 | 0.3 |
| 21 | 0.4 |
| n28 | 0.6 |

**Table 5.103.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-21\_n28 | 1 | 0 |
| 21 | 0 |
| n28 | 0.2 |

### 5.103.4 Reference sensitivity exceptions

- 2nd order IMD products generated by DC\_21\_n28 uplink may fall into own Rx of band 1.

⇒ IMD was calculated based on the frequency range in band n28 that the operator actually owned, which resulted in that IMD2 doesn’t fall into own Rx of band 1. Therefore, we didn’t specify MSD.

- 3rd order IMD products generated by DC\_21\_n28 uplink may fall into own Rx of band 1.

⇒ The MSD values are shown in the following table. These values are the average of the analysis results of the two companies. [1][2]

Table 5.103.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_1A-21A\_n28AX1 | 1 | 1975.3 | 5 | 25 | 2165.3 | 16.1 | IMD3 |
| 21 | 1450.4 | 5 | 25 | 1498.4 | N/A | N/A |
| n28 | 735.5 | 5 | 25 | 790.5 | N/A | N/A |
| NOTE X1: The frequency range in band n28 is restricted for this band combination to 728 - 738 MHz for the UL and 783 - 793 MHz for the DL. This band is subject to IMD2 fall in B1 also which MSD is not specified. | | | | | | | |

## 5.104 DC\_3-21\_n28

### 5.104.1 Configurations for DC

The frequency range in band n28 is restricted for this band combination to 728 - 738 MHz for the UL and 783-793 MHz for the DL because only a certain operator uses band 21. This restriction is mentioned in TP for DC\_21\_n28 (R4-2100352).

Table 5.104.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-21A\_n28A | DC\_3A\_n28A  DC\_21A\_n28A |

### 5.104.2 Co-existence studies

Based on co-existence studies of DC\_3\_n28 and DC\_21\_n28, own Rx impact of the 3rd band is the followings.

- IMD generated by DC\_3\_n28 uplink doesn’t fall into own Rx of band 21.

- IMD generated by DC\_21\_n28 uplink doesn’t fall into own Rx of band 3.

### 5.104.3 ∆TIB and ∆RIB values

For DC\_3-21\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination CA\_3-21-28, and are given in the tables below.

Table 5.104.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-21\_n28 | 3 | 0.8 |
| 21 | 0.9 |
| n28 | 0.3 |

**Table 5.104.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-21\_n28 | 3 | 0.3 |
| 21 | 0.5 |
| n28 | 0 |

### 5.104.4 Reference sensitivity exceptions

Based on co-existence studies of DC\_3-21\_n28, there is no need to have MSD added.

## 5.105 DC\_8-20\_n1

### 5.105.1 Configurations for DC

Table 5.105.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-20A\_n1A | DC\_8A\_n1A  DC\_20A\_n1A |

### 5.105.2 Co-existence studies

Table 5.105.2-1 lists the Band 8A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.105.2-1: Band 8 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 880 | 915 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1760 – 1830 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2640 – 2745 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1005 – 1100 | | | 2800 – 2895 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 90 – 220 | | | 2925 – 3080 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3680 – 3810 | | | 4720 – 4875 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 830 – 965 | | | 1910 – 1990 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 660 – 825 | | | 4845 – 5060 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 2010 – 2200 | | | 5600 – 5790 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4560 – 4725 | | | 6640 – 6855 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6765 – 7040 | | | 1540 – 1740 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3930 – 4180 | | | 1095 – 1320 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8560 – 8835 | | | 5440 – 5640 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7520 – 7770 | | | 6480 – 6705 | | |

Based on Table 5.105.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 7, 41, 77 and 90

- 3rd order harmonics may fall into Rx frequencies of bands 3, 46 and 47

- 3rd order IMD may fall into Rx frequencies of bands 43, 48, 49, 77, 78 and 79

- 4th order IMD may fall into Rx frequencies of bands 1, 4, 10, 12, 13, 14, 17, 20, 23, 28, 29, 34, 44, 46, 65, 66, 67, 68, 70, 79, 79 and 85

- 5th order IMD may fall into Rx frequencies of bands 24, 46 and 77

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.105.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.105.2-2: 2UL Band 8 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD5 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD5 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD5 |
| GPS | 1563 | - | 1587 | Yes |  | IMD5 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 3rd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | No | Europe |  |
| 5470 | - | 5725 | Yes | IMD4, IMD5 |
| 5150 | - | 5825 | Yes | Asia | 3rd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_8\_n1 in 38101-3.

Table 5.105.2-3 lists the Band 20A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.105.2-3: Band 20 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 832 | 862 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1664 – 1724 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2496 – 2586 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1058 – 1148 | | | 2752 – 2842 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 196 – 316 | | | 2978 – 3128 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3584 – 3704 | | | 4672 – 4822 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 782 – 912 | | | 1900 – 2000 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 516 – 666 | | | 4898 – 5108 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 2116 – 2296 | | | 5504 – 5684 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4416 – 4566 | | | 6592 – 6802 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6818 – 7088 | | | 1348 – 1528 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 4036 – 4276 | | | 1254 – 1464 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8512 – 8782 | | | 5248 – 5428 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7424 – 7664 | | | 6336 – 6546 | | |

Based on Table 5.105.2-3,

- 2nd order harmonics may fall into Rx frequencies of bands 38, 41, 69, 77 and 90

- 3rd order harmonics may fall into Rx frequencies of bands 46 and 47

- 3rd order IMD may fall into Rx frequencies of bands 22, 42, 43, 48, 49, 77, 78 and 79

- 4th order IMD may fall into Rx frequencies of bands 1, 4, 10, 23, 46, 65, 66, 71 and 79

- 5th order IMD may fall into Rx frequencies of bands 11, 21, 24, 32, 45, 46, 50, 51, 74, 75, 76, 77, 91, 92, 93 and 94

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.105.2-4 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.105.2-4: 2UL Band 20 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 3rd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | IMD5 |
| 5470 | - | 5725 | Yes | IMD4 |
| 5150 | - | 5825 | Yes | Asia | 3rd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_20\_n1 in 38101-3.

### 5.105.3 ∆TIB and ∆RIB values

Table 5.105.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8A-20A\_n1 | 8 | 0.4 |
| 20 | 0.4 |
| n1 | 0.3 |

**Table 5.105.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8A-20A\_n1 | 8 | 0 |
| 20 | 0 |
| n1 | 0 |

### 5.105.4 Reference sensitivity exceptions

B20 MSD due to IMD4 of 8-n1 is TBD.

## Further study required to agree on achievable performance for LB quadplexer.5.106 DC\_8-20\_n3

### 5.106.1 Configurations for DC

Table 5.106.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-20A\_n3A | DC\_8A\_n3A  DC\_20A\_n3A |

### 5.106.2 Co-existence studies

Table 5.106.2-1 lists the Band 8A + Band n3A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.106.2-1: Band 8 and Band n3 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 880 | 915 | | 1710 | 1785 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1760 – 1830 | | | 3420 – 3570 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2640 – 2745 | | | 5130 – 5355 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 795 – 905 | | | 2590 – 2700 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 25 – 120 | | | 2505 – 2690 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3470 – 3615 | | | 4300 – 4485 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 850 – 945 | | | 1700 – 1795 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 855 – 1035 | | | 4215 – 4475 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1590 – 1810 | | | 5180 – 5400 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4350 – 4530 | | | 6010 – 6270 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5925 – 6260 | | | 1735 – 1950 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3300 – 3595 | | | 675 – 930 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7720 – 8055 | | | 5230 – 5445 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6890 – 7185 | | | 6060 – 6315 | | |

Based on Table 5.106.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 7, 22, 41, 42, 48, 49, 77, 78 and 90

- 3rd order harmonics may fall into Rx frequencies of bands 3 and 46

- 2nd order IMD may fall into Rx frequencies of bands 5, 6, 7, 18, 19, 20, 26, 27, 28, 38, 41, 44, 69 and 90

- 3rd order IMD may fall into Rx frequencies of bands 7, 22, 38, 41, 42, 43, 48, 49, 69, 77, 78, 79 and 90

- 4th order IMD may fall into Rx frequencies of bands 3, 5, 6, 8, 18, 19, 26, 27, 46 and 79

- 5th order IMD may fall into Rx frequencies of bands 2, 3, 5, 6, 8, 9, 12, 13, 14, 17, 18, 19, 20, 22, 25, 26, 27, 28, 29, 33, 35, 36, 37, 39, 42, 44, 46, 48, 49, 52, 67, 68, 77, 78 and 85

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.106.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.106.2-2: 2UL Band 8 + Band n3 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD4 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD4 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD4 |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 3rd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | 3rd Harmonic, IMD4, IMD5 |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 3rd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_8\_n3 in 38101-3.

Table 5.106.2-3 lists the Band 20A + Band n3A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.106.2-3: Band 20 and Band n3 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 832 | 862 | | 1710 | 1785 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1664 – 1724 | | | 3420 – 3570 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2496 – 2586 | | | 5130 – 5355 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 848 – 953 | | | 2542 – 2647 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 14 – 121 | | | 2558 – 2738 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3374 – 3509 | | | 4252 – 4432 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 802 – 892 | | | 1690 – 1805 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 711 – 876 | | | 4268 – 4523 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1696 – 1906 | | | 5084 – 5294 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4206 – 4371 | | | 5962 – 6217 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5978 – 6308 | | | 1543 – 1738 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3406 – 3691 | | | 834 – 1074 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7672 – 8002 | | | 5038 – 5233 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6794 – 7079 | | | 5916 – 6156 | | |

Based on Table 5.106.2-3,

- 2nd order harmonics may fall into Rx frequencies of bands 22, 38, 41, 42, 48, 49, 69, 77, 78 and 90

- 3rd order harmonics may fall into Rx frequencies of band 46

- 2nd order IMD may fall into Rx frequencies of bands 5, 6, 7, 8, 18, 19, 26, 27, 38, 41, 69 and 90

- 3rd order IMD may fall into Rx frequencies of bands 7, 38, 41, 42, 52, 69, 77, 78, 79 and 90

- 4th order IMD may fall into Rx frequencies of bands 3, 5, 6, 9, 12, 13, 14, 17, 18, 19, 20, 26, 27, 28, 29, 33, 35, 39, 44, 46, 67, 68, 79 and 85

- 5th order IMD may fall into Rx frequencies of bands 5, 6, 8, 18, 19, 22, 24, 26, 27, 42, 43, 46, 47, 48, 49, 77 and 78

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.106.2-4 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.106.2-4: 2UL Band 20 + Band n3 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD5 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD5 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD5 |
| GPS | 1563 | - | 1587 | Yes |  | IMD5 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 3rd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | 3rd Harmonic, IMD4, IMD5 |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 3rd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_20\_n3 in 38101-3.

### 5.106.3 ∆TIB and ∆RIB values

Table 5.106.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8A-20A\_n3 | 8 | 0.4 |
| 20 | 0.4 |
| n3 | 0.3 |

**Table 5.106.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8A-20A\_n3 | 8 | 0 |
| 20 | 0 |
| n3 | 0 |

### 5.106.4 Reference sensitivity exceptions

B20 and B8 MSD for IMD2 of 8-n3 and 20-n3 uplinks respectively is TBD.Further study required to agree on achievable performance of LB quadplexer.

## 5.107 DC\_8-32\_n1

### 5.107.1 Configurations for DC

Table 5.107.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-32A\_n1A | DC\_8A\_n1A |

### 5.107.2 Co-existence studies

Table 5.107.2-1 lists the Band 8A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.107.2-1: Band 8 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 880 | 915 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1760 – 1830 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2640 – 2745 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1005 – 1100 | | | 2800 – 2895 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 90 – 220 | | | 2925 – 3080 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3680 – 3810 | | | 4720 – 4875 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 830 – 965 | | | 1910 – 1990 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 660 – 825 | | | 4845 – 5060 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 2010 – 2200 | | | 5600 – 5790 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4560 – 4725 | | | 6640 – 6855 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6765 – 7040 | | | 1540 – 1740 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3930 – 4180 | | | 1095 – 1320 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8560 – 8835 | | | 5440 – 5640 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7520 – 7770 | | | 6480 – 6705 | | |

Based on Table 5.107.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 7, 41, 77 and 90

- 3rd order harmonics may fall into Rx frequencies of bands 3, 46 and 47

- 3rd order IMD may fall into Rx frequencies of bands 43, 48, 49, 77, 78 and 79

- 4th order IMD may fall into Rx frequencies of bands 1, 4, 10, 12, 13, 14, 17, 20, 23, 28, 29, 34, 44, 46, 65, 66, 67, 68, 70, 79, 79 and 85

- 5th order IMD may fall into Rx frequencies of bands 24, 46 and 77

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.107.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.107.2-2: 2UL Band 8 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD5 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD5 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD5 |
| GPS | 1563 | - | 1587 | Yes |  | IMD5 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 3rd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | No | Europe |  |
| 5470 | - | 5725 | Yes | IMD4, IMD5 |
| 5150 | - | 5825 | Yes | Asia | 3rd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_8\_n1 in 38101-3.

### 5.107.3 ∆TIB and ∆RIB values

Table 5.107.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8A-32A\_n1 | 8 | 0.3 |
| 32 | N/A |
| n1 | 0.5 |

**Table 5.107.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8A-32A\_n1 | 8 | 0 |
| 32 | 0 |
| n1 | 0 |

### 5.107.4 Reference sensitivity exceptions

## No additional IMD exceptions required compared to fallbacks.5.108 DC\_12-66\_n41

5.108.1 Operating bands for EN-DC

Table 5.108.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 12-66\_n41 | CA\_12-66 | n41 |  |

### 5.108.2 Configuration for DC

Table 5.108.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_12A-66A\_n41A | DC\_12A\_n41A DC\_66A\_n41A | CA\_12A-66A | n41A |

5.108.3 ∆TIB and ∆RIB values

For DC\_12-66\_n41, the ΔTIB,c and ΔRIB,c values are reused from DC\_66\_n41-n71 and are given in the tables below.

**Table 5.108.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_12-66\_n41 | 12 | 0.6 |
| 66 | 0.5 |
| n41 | 0.81 |
| 1.32 |
| NOTE 1: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 2: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz. | | |

**Table 5.108.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_12-66\_n41 | 12 | 0.5 |
| 66 | 0.5 |
| n41 | 0.51 |
| 12 |
| NOTE 1: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 2: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz. | | |

5.108.4 REFSENS requirements

There is IMD2 impact from UL 66\_n41 affecting DL band 12. The MSD value is derived from DC\_7A-13A\_n66A.

The IMD3 impact from UL 66\_n41 affecting DL band 12 is too close to the band edges to allocate test points and can therefore be disregarded.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_12A-66A\_n41A | 12 | 712 | 5 | 25 | 742 | 31 | IMD2 |
| 66 | 1773 | 5 | 25 | 2173 | N/A | N/A |
| n41 | 2515 | 5 | 25 | 2515 | N/A | N/A |

## 5.109 DC\_2-12\_n41

5.109.1 Operating bands for EN-DC

Table 5.109.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 2-12\_n41 | CA\_2-12 | n41 |  |

### 5.109.2 Configuration for DC

Table 5.109.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-12A\_n41A | DC\_2A\_n41A DC\_12A\_n41A | CA\_2A-12A | n41A |
| DC\_2A-2A-12A\_n41A | DC\_2A\_n41A DC\_12A\_n41A | CA\_2A-2A-12A | n41A |

5.109.3 ∆TIB and ∆RIB values

For DC\_2-12\_n41, the ΔTIB,c and ΔRIB,c values are reused from CA\_2-7-12 and DC\_2\_n41-n71 and are given in the tables below.

**Table 5.109.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-12\_n41 DC\_2-2-12\_n41 | 2 | 0.5 |
| 12 | 0.3 |
| n41 | 0.5 |

**Table 5.109.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-12\_n41  DC\_2-2-12\_n41 | 2 | 0 |
| 12 | 0 |
| n41 | 0 |

5.109.4 REFSENS requirements

There are IMD2 impact from UL 12\_n41 affecting DL band 2. The IMD2 MSD value is derived from DC\_2A-71A\_n38A.

There are IMD2 and IMD5 impact from UL 2\_n41 affecting DL band 12. The IMD2 MSD value is derived from DC\_2A\_n41A-n71A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-12A\_n41A DC\_2A-2A-12A\_n41A | 2 | 1872 | 5 | 25 | 1952 | 26 | IMD2 |
| 12 | 708 | 5 | 50 | 738 | N/A | N/A |
| n41 | 2660 | 10 | 50 | 2660 | N/A | N/A |
| 2 | 1900 | 5 | 25 | 1980 | N/A | N/A |
| 12 | 708 | 5 | 50 | 738 | 28.7 | IMD24 |
| n41 | 2638 | 10 | 50 | 2638 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified | | | | | | | |

## 5.110 DC\_66-71\_n41

5.110.1 Operating bands for EN-DC

Table 5.110.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 66-71\_n41 | CA\_66-71 | n41 |  |

### 5.110.2 Configuration for DC

Table 5.110.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_66A-71A\_n41A | DC\_66A\_n41A DC\_71A\_n41A | CA\_66A-71A | n41A |

5.110.3 ∆TIB and ∆RIB values

For DC\_66-71\_n41, the ΔTIB,c and ΔRIB,c values are reused from DC\_66\_n41-n71 and are given in the tables below.

**Table 5.110.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_66-71\_n41 | 66 | 0.5 |
| 71 | 0.6 |
| n41 | 0.81 |
| 1.32 |
| NOTE 1: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 2: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz. | | |

**Table 5.110.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_66-71\_n41 | 66 | 0.5 |
| 71 | 0.5 |
| n41 | 0.51 |
| 12 |
| NOTE 1: The requirement is applied for UE transmitting on the frequency range of 2545 - 2690 MHz.  NOTE 2: The requirement is applied for UE transmitting on the frequency range of 2496 - 2545 MHz. | | |

5.110.4 REFSENS requirements

There is no need to define MSD.

## 5.111 DC\_2-71\_n41

5.111.1 Operating bands for EN-DC

Table 5.111.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 2-71\_n41 | CA\_2-71 | n41 |  |

### 5.111.2 Configuration for DC

Table 5.111.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-71A\_n41A | DC\_2A\_n41A DC\_71A\_n41A | CA\_2A-71A | n41A |
| DC\_2A-2A-71A\_n41A | DC\_2A\_n41A DC\_71A\_n41A | CA\_2A-2A-71A | n41A |

5.111.3 ∆TIB and ∆RIB values

For DC\_2-71\_n41, the ΔTIB,c and ΔRIB,c values are reused from DC\_2\_n41-n71 and are given in the tables below.

**Table 5.111.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-71\_n41 DC\_2-2-71\_n41 | 2 | 0.5 |
| 71 | 0.3 |
| n41 | 0.5 |

**Table 5.111.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-71\_n41  DC\_2-2-71\_n41 | 2 | 0 |
| 71 | 0 |
| n41 | 0 |

5.111.4 REFSENS requirements

There are IMD2 impact from UL 71\_n41 affecting DL band 2. The IMD2 MSD value is derived from DC\_2A-71A\_n38A.

There are IMD2 and IMD5 impact from UL 2\_n41 affecting DL band 71. The IMD2 MSD value is derived from DC\_2A\_n41A-n71A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-71A\_n41A DC\_2A-2A-71A\_n41A | 2 | 1862 | 5 | 25 | 1942 | 26 | IMD2 |
| 71 | 668 | 5 | 25 | 622 | N/A | N/A |
| n41 | 2610 | 10 | 50 | 2610 | N/A | N/A |
| 2 | 1900 | 5 | 25 | 1980 | N/A | N/A |
| 71 | 676 | 5 | 50 | 630 | 28.7 | IMD24 |
| n41 | 2530 | 10 | 50 | 2530 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified | | | | | | | |

## 5.112 DC\_7-12\_n66

5.112.1 Operating bands for EN-DC

Table 5.112.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 7-12\_n66 | CA\_7-12 | n66 |  |

### 5.112.2 Configuration for DC

Table 5.112.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_7A-12A\_n66A | DC\_7A\_n66A DC\_12A\_n66A | CA\_7A-12A | n66A |

5.112.3 ∆TIB and ∆RIB values

For DC\_7-12\_n66, the ΔTIB,c and ΔRIB,c values are reused from DC\_7-66\_n71 and are given in the tables below.

**Table 5.112.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-12\_n66 | 7 | 0.5 |
| 12 | 0.5 |
| n66 | 0.5 |

**Table 5.112.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-12\_n66 | 7 | 0.5 |
| 12 | 0.1 |
| n66 | 0.5 |

5.112.4 REFSENS requirements

There are IMD2 impact from UL 7\_n66 affecting DL band 12. The IMD2 MSD value is derived from DC\_7A-13A\_n66A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-12A\_n66A | 7 | 2515 | 5 | 25 | 2635 | N/A | N/A |
| 12 | 712 | 5 | 25 | 742 | 31 | IMD2 |
| n66 | 1773 | 5 | 25 | 2173 | N/A | N/A |

## 5.113 DC\_7-71\_n66

5.113.1 Operating bands for EN-DC

Table 5.113.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 7-71\_n66 | CA\_7-71 | n66 |  |

### 5.113.2 Configuration for DC

Table 5.113.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_7A-71A\_n66A | DC\_7A\_n66A DC\_71A\_n66A | CA\_7A-71A | n71A |

5.113.3 ∆TIB and ∆RIB values

For DC\_7-71\_n66, the ΔTIB,c and ΔRIB,c values are reused from DC\_7-66\_n71 and are given in the tables below.

**Table 5.113.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-71\_n66 | 7 | 0.5 |
| 71 | 0.5 |
| n66 | 0.5 |

**Table 5.113.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-71\_n66 | 7 | 0.5 |
| 71 | 0.1 |
| n66 | 0.5 |

5.113.4 REFSENS requirements

There is no need to define MSD.

## 5.114 DC\_7-12\_n78

5.114.1 Operating bands for EN-DC

Table 5.114.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 7-12\_n78 | CA\_7-12 | n78 |  |

### 5.114.2 Configuration for DC

Table 5.114.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_7A-12A\_n78A | DC\_7A\_n78A DC\_12A\_n78A | CA\_7A-12A | n78A |

5.114.3 ∆TIB and ∆RIB values

For DC\_7-12\_n78, the ΔTIB,c and ΔRIB,c values are reused from DC\_12\_n7-n78 and are given in the tables below.

**Table 5.114.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-12\_n78 | 7 | 0.5 |
| 12 | 0.5 |
| n78 | 0.8 |

**Table 5.114.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-12\_n78 | 7 | 0.2 |
| 12 | 0.5 |
| n78 | 0.5 |

5.114.4 REFSENS requirements

There are IMD2 impact from UL 12\_n78 affecting DL band 7. The IMD2 MSD value is derived from DC\_12A\_n7A-n78A.

There are IMD2 and IMD5 impact from UL 7\_n78 affecting DL band 12. The IMD2 MSD value is derived from DC\_28A-41A\_n78A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-12A\_n78A | 7 | 2542 | 5 | 25 | 2662 | 29.6 | IMD2 |
| 12 | 708 | 5 | 25 | 738 | N/A | N/A |
| n78 | 3370 | 10 | 50 | 3370 | N/A | N/A |
| 7 | 2565 | 5 | 25 | 2685 | N/A | N/A |
| 12 | 710 | 5 | 25 | 740 | 30.8 | IMD24 |
| n78 | 3305 | 10 | 50 | 3305 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified | | | | | | | |

## 5.115 DC\_12-66\_n78

5.115.1 Operating bands for EN-DC

Table 5.115.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 12-66\_n78 | CA\_12-66 | n78 |  |

### 5.115.2 Configuration for DC

Table 5.115.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_12A-66A\_n78A | DC\_12A\_n78A DC\_66A\_n78A | CA\_12A-66A | n78A |

5.115.3 ∆TIB and ∆RIB values

For DC\_12-66\_n78, the ΔTIB,c and ΔRIB,c values are reused from DC\_66-71\_n78 and are given in the tables below.

**Table 5.115.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_12-66\_n78 | 12 | 0.6 |
| 66 | 0.6 |
| n78 | 0.8 |

**Table 5.115.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_12-66\_n78 | 12 | 0.2 |
| 66 | 0.2 |
| n78 | 0.5 |

5.115.4 REFSENS requirements

There are IMD3 impact from UL 12\_n78 affecting DL band 66. The IMD3 MSD value is derived from DC\_48A-66A\_n12A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_12A-66A\_n78A | 12 | 710 | 5 | 25 | 740 | N/A | N/A |
| 66 | 1760 | 5 | 25 | 2160 | 17.1 | IMD3 |
| n78 | 3580 | 5 | 25 | 3580 | N/A | N/A |

## 5.116 DC\_2-12\_n78

5.116.1 Operating bands for EN-DC

Table 5.116.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 2-12\_n78 | CA\_2-12 | n78 |  |

### 5.116.2 Configuration for DC

Table 5.116.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-12A\_n78A | DC\_2A\_n78A DC\_12A\_n78A | CA\_2A-12A | n78A |
| DC\_2A-2A-12A\_78A | DC\_2A\_n78A DC\_12A\_n78A | CA\_2A-2A-12A | n78A |
| DC\_2A-12A\_n78(2A) | DC\_2A\_n78A DC\_12A\_n78A | CA\_2A-12A | CA\_n78(2A) |

5.116.3 ∆TIB and ∆RIB values

For DC\_2-12\_n78, the ΔTIB,c and ΔRIB,c values are reused from DC\_2-71\_n78 and are given in the tables below.

**Table 5.116.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-12\_n78 | 2 | 0.6 |
| 12 | 0.6 |
| n78 | 0.8 |

**Table 5.116.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-12\_n78 | 2 | 0.2 |
| 12 | 0.2 |
| n78 | 0.5 |

5.116.4 REFSENS requirements

There are IMD3 impact from UL 12\_n78 affecting DL band 2. The IMD3 MSD value is derived from DC\_2A-71A\_n78A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-12A\_n78A DC\_2A-2A-12A\_n78A  DC\_2A-12A\_n78(2A) | 2 | 1874 | 5 | 25 | 1954 | 16.5 | IMD3 |
| 12 | 708 | 5 | 25 | 738 | N/A | N/A |
| n78 | 3370 | 10 | 50 | 3370 | N/A | N/A |

## 5.117 DC\_7-71\_n78

5.117.1 Operating bands for EN-DC

Table 5.117.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 7-71\_n78 | CA\_7-71 | n78 |  |

### 5.117.2 Configuration for DC

Table 5.117.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_7A-71A\_n78A | DC\_7A\_n78A DC\_71A\_n78A | CA\_7A-71A | n78A |

5.117.3 ∆TIB and ∆RIB values

For DC\_7-71\_n78, the ΔTIB,c and ΔRIB,c values are reused from DC\_12\_n7-n78 and are given in the tables below.

**Table 5.117.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-71\_n78 | 7 | 0.5 |
| 71 | 0.5 |
| n78 | 0.8 |

**Table 5.117.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-71\_n78 | 7 | 0.2 |
| 71 | 0.5 |
| n78 | 0.5 |

5.117.4 REFSENS requirements

There are IMD2 impact from UL 71\_n78 affecting DL band 7. The IMD2 MSD value is derived from DC\_12A\_n7A-n78A.

There are IMD5 impact from UL 7\_n78 affecting DL band 71. The IMD2 MSD value is derived from DC\_28A-41A\_n77A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-71A\_n78A | 7 | 2550 | 5 | 25 | 2670 | 29.6 | IMD2 |
| 71 | 680 | 5 | 25 | 634 | N/A | N/A |
| n78 | 3350 | 10 | 50 | 3350 | N/A | N/A |
| 7 | 2540 | 5 | 25 | 2660 | N/A | N/A |
| 71 | 686 | 5 | 25 | 640 | 3.0 | IMD5 |
| n78 | 3490 | 10 | 50 | 3490 | N/A | N/A |

## 5.118 DC\_20-40\_n1

5.118.1 Operating bands for DC

Table 5.118.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_20-40\_n1 | CA\_20-40 | n1 | No |

5.118.2 Configurations for DC

Table 5.118.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_20A-40A\_n1A  DC\_20A-40C\_n1A | DC\_20A\_n1A  DC\_40A\_n1A | CA\_20A-40A  CA\_20A-40C | n1 |

5.118.3 Co-existence studies

Based on co-existence studies of Band 20 + Band n1 captured in 37.863-01-01 there is no IMD interfering band 40

And based on co-existence studies of Band 40 + Band n1 captured in 37.863-01-01, MSD shall be considered since

- 4th order IMD generated by dual uplink of the two bands may fall into own Rx of band 20.

5.118.4 ∆TIB and ∆RIB values

It is proposed to re-use relaxation values from DC\_1-20\_n38 which is very similar.

Table 5.118.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20-40-n1 | 20 | 0.3 |
| 40 | 0.5 |
| n1 | 0.5 |

**Table 5.118.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20-40-n1 | 20 | 0 |
| 40 | 0 |
| n1 | 0 |

5.118.5 REFSENS requirements

It is proposed to re-use IMD4 MSD value from DC\_1A\_n8A-n40A which is very similar.

Table 5.118.5-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_20A-40A\_n1A  DC\_20A-40C\_n1A | 20 | 841 | 5 | 25 | 800 | 8.0 | IMD4 |
| 40 | 2330 | 5 | 25 | 2330 | N/A | N/A |
| n1 | 1930 | 5 | 25 | 2120 | N/A | N/A |

## 5.119 DC\_5-30\_n2

5.119.1 Operating bands for DC

Table 5.119.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_5-30\_n2 | CA\_5-30 | n2 | No |

5.119.2 Configurations for DC

Table 5.119.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_5A-30A\_n2A | DC\_5A\_n2A  DC\_30A\_n2A | CA\_5A-30A | n2 |

5.119.3 Co-existence studies

Based on co-existence studies of Band 5 + Band n2 captured in 37.716-11-11, no MSD is necessary

Based on co-existence studies of Band 30 + Band n2 captured in 37.716-11-11, MSD shall be considered since

- 4th order IMD generated by dual uplink of the two bands may fall into own Rx of band 5.

5.119.4 ∆TIB and ∆RIB values

Based on E-UTRA CA\_2-5-30 configuration, following relaxations are proposed

Table 5.119.4-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-30\_n2 | 5 | 0.3 |
| 30 | 0.3 |
| n2 | 0.5 |

**Table 5.119.4-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-30\_n2 | 5 | 0 |
| 30 | 0.5 |
| n2 | 0.4 |

5.119.5 REFSENS requirements

As stated in 5.119.3 MSD requirement caused by 4th order IMD is needed and specified below accordingly which is based on similar case of DC\_1A\_n8A-n40A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_5A-30A\_n2A | 5 | 835 | 5 | 25 | 880 | 8 | IMD4 |
| 30 | 2310 | 5 | 25 | 2355 | N/A | N/A |
| n2 | 1870 | 5 | 25 | 1950 | N/A | N/A |

## 5.120 DC\_2-46\_n77

5.120.1 Operating bands for DC

Table 5.120.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-46A\_n77A | DC\_2A\_n77A |

### 5.120.2 Co-existence studies

For UE coexistence study of Band 2 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products are presented in Table 5.120.2-1.

**Table 5.120.2-1: Harmonic and IMD analysis for DC\_2\_n77**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1910 | 3300 | 4200 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3820 | 6600 | 8400 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5730 | 9900 | 12600 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1390 | 2350 | 5150 | 6110 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | -500 | 520 | 4690 | 6550 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7000 | 8020 | 8450 | 10310 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1350 | 2430 | 7990 | 10750 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8850 | 9930 | 11750 | 14510 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 4700 | 2780 | 10300 | 12220 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 14950 | 11290 | 4340 | 3200 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 15050 | 18710 | 10700 | 11840 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 8900 | 6080 | 870 | 2850 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 13600 | 16420 | 12150 | 14130 |

Based on co-existence study as presented in the table 5.120.2-1, own Rx impact is shown in the following.

* The 2nd harmonic of band 2 may fall into own Rx of band n77
* The 3rd harmonic of band 2 may fall into own Rx of band 46
* The 2nd order IMD generated by dual uplink of 2+n77 may fall into own Rx of band 2 and 46
* The 3rd order IMD generated by dual uplink of 2+n77 may fall into own Rx of band 46
* The 4th order IMD generated by dual uplink of 2+n77 may fall into own Rx of band 2 and n77
* The 5th order IMD generated by dual uplink of 2+n77 may fall into own Rx of band 2 and n77

### 5.120.3 ∆TIB and ∆RIB values

The same relaxation values as DC\_2\_n77 is assumed for DC\_2-46\_n77.

Table 5.120.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-46\_n77 | 2 | 0.6 |
| n77 | 0.8 |

**Table 5.120.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-46\_n77 | 2 | 0 |
| 46 | 0 |
| n77 | 0 |

### 5.120.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the IMD2/IMD3 of band 2+n77 falling into band 46. The exclusion zone for IMD to band 46 is applied.

Table 5.120.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-46A\_n77A5 | 2 | N/A | N/A | N/A | N/A | N/A | N/A |
|  | 46 | N/A | N/A | N/A | N/A | N/A | IMD2,  IMD3 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | N/A |
| NOTE 5: When Band 46 have self-interference problems by dual uplink CA/EN-DC, then the requirements do not apply in exclusion zone which is frequency range within (harmonics frequency region + FHD) and IMD frequency region as follow.  IMD frequency range   |  |  |  |  | | --- | --- | --- | --- | | DL\_CA configuration | UL\_CA configuration | Exclusion zone center frequency | Exclusion zone BW | | DC\_2A-46A\_n77A | DC\_2A\_n77A | fc\_2A + fc\_n77A | BW\_2A + BW\_n77A | | DC\_2A-46A\_n77A | DC\_2A\_n77A | -fc\_2A + 2\*fc\_n77A | -BW\_2A + 2\*BW\_n77A | | | | | | | | |

## 5.121 DC\_46-66\_n77

5.121.1 Operating bands for DC

Table 5.121.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_46A-66A\_n77A | DC\_66A\_n77A |

### 5.121.2 Co-existence studies

For UE coexistence study of Band 66 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products are presented in Table 5.121.2-1.

**Table 5.121.2-1: Harmonic and IMD analysis for DC\_66\_n77**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1710 | 1780 | 3300 | 4200 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3420 | 3560 | 6600 | 8400 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5130 | 5340 | 9900 | 12600 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1520 | 2490 | 5010 | 5980 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 780 | 260 | 4820 | 6690 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 6720 | 7760 | 8310 | 10180 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 930 | 2040 | 8120 | 10890 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 8430 | 9540 | 11610 | 14380 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 4980 | 3040 | 10020 | 11960 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 15090 | 11420 | 3820 | 2640 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 14910 | 18580 | 10140 | 11320 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 9180 | 6340 | 1260 | 3270 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 13320 | 16160 | 11730 | 13740 |

Based on co-existence study as presented in the table 5.121.2-1, own Rx impact is shown in the following.

* The 2nd harmonic of band 66 may fall into own Rx of band n77
* The 3rd harmonic of band 66 may fall into own Rx of band 46
* The 2nd order IMD generated by dual uplink of 66+n77 may fall into own Rx of band 46 and 66
* The 3rd order IMD generated by dual uplink of 66+n77 may fall into own Rx of band 46
* The 4th order IMD generated by dual uplink of 66+n77 may fall into own Rx of band n77
* The 5th order IMD generated by dual uplink of 66+n77 may fall into own Rx of band 66 and n77

### 5.121.3 ∆TIB and ∆RIB values

The same relaxation values as DC\_66\_n77 is assumed for DC\_46-66\_n77.

Table 5.121.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_46-66\_n77 | 66 | 0.6 |
| n77 | 0.8 |

**Table 5.121.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_46-66\_n77 | 46 | 0 |
| 66 | 0 |
| n77 | 0 |

### 5.121.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the IMD2/IMD3 of band 66+n77 falling into band 46. The exclusion zone for IMD to band 46 is applied.

Table 5.121.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_46A-66A\_n77A5 | 46 | N/A | N/A | N/A | N/A | N/A | IMD2,  IMD3 |
|  | 66 | N/A | N/A | N/A | N/A | N/A | N/A |
|  | n77 | N/A | N/A | N/A | N/A | N/A | N/A |
| NOTE 5: When Band 46 have self-interference problems by dual uplink CA/EN-DC, then the requirements do not apply in exclusion zone which is frequency range within (harmonics frequency region + FHD) and IMD frequency region as follow.  IMD frequency range   |  |  |  |  | | --- | --- | --- | --- | | DL\_CA configuration | UL\_CA configuration | Exclusion zone center frequency | Exclusion zone BW | | DC\_46A-66A\_n77A | DC\_66A\_n77A | fc\_66A + fc\_n77A | BW\_66A + BW\_n77A | | DC\_46A-66A\_n77A | DC\_66A\_n77A | -fc\_66A + 2\*fc\_n77A | -BW\_66A + 2\*BW\_n77A | | | | | | | | |

## 5.122 DC\_13-46\_n77

5.122.1 Operating bands for DC

Table 5.122.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_13A-46A\_n77A | DC\_13A\_n77A |

### 5.122.2 Co-existence studies

For UE coexistence study of Band 13 + Band n77, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products are presented in Table 5.122.2-1.

**Table 5.122.2-1: Harmonic and IMD analysis for DC\_13\_n77**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 777 | 787 | 3300 | 4200 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 1554 | 1574 | 6600 | 8400 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 2331 | 2361 | 9900 | 12600 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 2513 | 3423 | 4077 | 4987 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 2646 | 1726 | 5813 | 7623 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 4854 | 5774 | 7377 | 9187 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1869 | 939 | 9113 | 11823 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 5631 | 6561 | 10677 | 13387 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 6846 | 5026 | 8154 | 9974 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 16023 | 12413 | 152 | 1092 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 13977 | 17587 | 6408 | 7348 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 11046 | 8326 | 4239 | 6069 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 11454 | 14174 | 8931 | 10761 |

Based on co-existence study as presented in the table 5.122.2-1, own Rx impact is shown in the following.

* The 2nd order IMD generated by dual uplink of 13+n77 may fall into own Rx of band n77
* The 3rd order IMD generated by dual uplink of 13+n77 may fall into own Rx of band 46
* The 3rd and 4th order IMD generated by dual uplink of 13+n77 may fall into own Rx of band 46
* The 5th order IMD generated by dual uplink of 13+n77 may fall into own Rx of band 13, 46 and n77

### 5.122.3 ∆TIB and ∆RIB values

The same relaxation values as DC\_13\_n77 is assumed for DC\_13-46\_n77.

Table 5.122.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_13-46\_n77 | 13 | 0.5 |
| n77 | 0.8 |

**Table 5.122.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_13-46\_n77 | 13 | 0 |
| 46 | 0 |
| n77 | 0 |

### 5.122.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the IMD3/IMD4/IMD5 of band 13+n77 falling into band 46. The exclusion zone for IMD to band 46 is applied.

Table 5.122.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_13A-46A\_n77A5 | 13 | N/A | N/A | N/A | N/A | N/A | N/A |
|  | 46 | N/A | N/A | N/A | N/A | N/A | IMD3,  IMD4,  IMD5 |
|  | n77 | N/A | N/A | N/A | N/A | N/A | N/A |
| NOTE 5: When Band 46 have self-interference problems by dual uplink CA/EN-DC, then the requirements do not apply in exclusion zone which is frequency range within (harmonics frequency region + FHD) and IMD frequency region as follow.  IMD frequency range   |  |  |  |  | | --- | --- | --- | --- | | DL\_CA configuration | UL\_CA configuration | Exclusion zone center frequency | Exclusion zone BW | | DC\_13A-46A\_n77A | DC\_13A\_n77A | 2\*fc\_13A + fc\_n77A | 2\*BW\_13A + BW\_n77A | | DC\_13A-46A\_n77A | DC\_13A\_n77A | 3\*fc\_13A + fc\_n77A | 3\*BW\_13A + BW\_n77A | | DC\_13A-46A\_n77A | DC\_13A\_n77A | -3\*fc\_13A + 2\*fc\_n77A | -3\*BW\_13A + 2\*BW\_n77A | | | | | | | | |

## 5.123 DC\_1-11\_n41

5.123.1 Configurations for DC

**Table 5.123.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_1A-11A\_n41A | DC\_1A\_n41A  DC\_11A\_n41A |

5.123.2 Co-existence studies

Based on co-existence studies of DC\_1A-11A\_n41A with 2UL, it can get that:

- IMD4 by dual uplink DC\_1\_n41 will fall into the own Rx band of Band 11

- IMD4 by dual uplink DC\_11\_n41 will fall into the own Rx band of Band 1

5.123.3 ∆TIB and ∆RIB values

For DC\_1 A-11A\_n41A, the ΔTIB,c and ΔRIB,c values are proposed in the tables below.

**Table 5.123.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-11\_n41 | 1 | 0.5 |
| 11 | 0.3 |
| n41 | 0.5 |

**Table 5.123.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-11\_n41 | 1 | 0 |
| 11 | 0 |
| n41 | 0 |

5.123.4 REFSENS requirements

Based the analysis on 5.123.2 above, MSD values due to IMD are shown below:

Table 5.123.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_1A-11A\_n41A | 11 | 1442 | 5 | 25 | 1490 | N/A | FDD | N/A |
| n41 | 2520 | 10 | 50 | 2520 | N/A | TDD | N/A |
| 1 | 1966 | 5 | 25 | 2156 | 10.2 | FDD | IMD4 |
| DC\_1A-11A\_n41A | 1 | 1940 | 5 | 25 | 2130 | N/A | FDD | N/A |
| n41 | 2685 | 10 | 50 | 2685 | N/A | TDD | N/A |
| 11 | 1442 | 5 | 25 | 1490 | 10.6 | FDD | IMD4 |

5.124 DC\_2-12\_n7

5.124.1 Operating bands for DC

**Table 5.124.1-1: Inter-band DC configurations (three bands)**

| **DC configuration** | **Uplink configuration** |
| --- | --- |
| DC\_2A-12A\_n7A  DC\_2A-12A\_n7(2A) | DC\_2A\_n7A  DC\_12A\_n7A |

5.124.2 Co-existence studies

For UE coexistence study of Band 2 + Band n7, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.124.2-1.

**Table 5.124.2-1: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1850 | 1910 | 2500 | 2570 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3700 | 3820 | 5000 | 5140 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5550 | 5730 | 7500 | 7710 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7400 | 7640 | 10000 | 10280 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9250 | 9550 | 12500 | 12850 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 590 | 720 | 4350 | 4480 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | -1130 | -1320 | 3090 | 3290 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 6200 | 6390 | 6850 | 7050 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | -2980 | -3230 | 5590 | 5860 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8050 | 8300 | 9350 | 9560 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 1180 | 1440 | 8700 | 8960 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 4830 | 5140 | 8090 | 8430 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 9900 | 10210 | 11850 | 12190 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 410 | 730 | 3680 | 4010 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 11200 | 11530 | 10550 | 10870 |

For UE coexistence study of Band 12 + Band n7, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.124.2-2.

**Table 5.124.2-2: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 699 | 716 | 2500 | 2570 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1398 | 1432 | 5000 | 5140 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2097 | 2148 | 7500 | 7710 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2796 | 2864 | 10000 | 10280 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3495 | 3580 | 12500 | 12850 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1784 | 1871 | 3199 | 3286 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1172 | 1068 | 4284 | 4441 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 3898 | 4002 | 5699 | 5856 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 473 | 352 | 6784 | 7011 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4597 | 4718 | 8199 | 8409 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 3568 | 3742 | 6398 | 6572 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 226 | 364 | 9284 | 9581 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5296 | 5434 | 10699 | 10996 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 3043 | 2852 | 6068 | 6312 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 8898 | 9142 | 7097 | 7288 |

The Rx impacts can be identified as below.

* 5th order IMD products generated by DC\_2\_n7 uplink may fall into own Rx of band 12.

5.124.3 ∆TIB and ∆RIB values

**Table 5.124.3-1: ΔTIB,**

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔTIB,c [dB]** |
| --- | --- | --- |
| DC\_2-12\_n7 | 2 | 0.5 |
| 12 | 0.3 |
| n7 | 0.5 |

**Table 5.124.3-2: ΔRIB,c**

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔRIB [dB]** |
| --- | --- | --- |
| DC\_2-12\_n7 | 2 | 0 |
| 12 | 0 |
| n7 | 0 |

5.124.4 Reference sensitivity exceptions

As stated in 5.124.2, for MSD requirement caused by IMDs is specified below accordingly, which is derived from DC\_2A-5A\_n77A.

**Table 5.124.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)**

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-12A\_n7A  DC\_2A-12A\_n7(2A) | 2 | 1907.5 | 5 | 25 | 1987.5 | N/A | N/A |
| 12 | 701.5 | 5 | 25 | 731.5 | 4.5 | IMD5 |
| n7 | 2502.5 | 5 | 25 | 2622.5 | N/A | N/A |

5.125 DC\_2-5\_n78

5.125.1 Operating bands for DC

**Table 5.125.1-1: Inter-band DC configurations (three bands)**

| **DC configuration** | **Uplink configuration** |
| --- | --- |
| DC\_2A-5A\_n78A  DC\_2A-5A\_n78(2A) | DC\_2A\_n78A  DC\_5A\_n78A |

5.125.2 Co-existence studies

For UE coexistence study of Band 2 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.125.2-1.

**Table 5.125.2-1: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1850 | 1910 | 3300 | 3800 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3700 | 3820 | 6600 | 7600 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5550 | 5730 | 9900 | 11400 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7400 | 7640 | 13200 | 15200 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9250 | 9550 | 16500 | 19000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 1390 | 1950 | 5150 | 5710 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 100 | 520 | 4690 | 5750 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 7000 | 7620 | 8450 | 9510 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1750 | 2430 | 7990 | 9550 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8850 | 9530 | 11750 | 13250 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 2780 | 3900 | 10300 | 11420 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 3600 | 4340 | 11290 | 13350 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 10700 | 11440 | 15050 | 17110 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 2050 | 870 | 6080 | 7700 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 13600 | 15220 | 12150 | 13330 |

For UE coexistence study of Band 5 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.125.2-2.

**Table 5.125.2-2: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 824 | 849 | 3300 | 3800 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1648 | 1698 | 6600 | 7600 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2472 | 2547 | 9900 | 11400 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 3296 | 3396 | 13200 | 15200 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4120 | 4245 | 16500 | 19000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 2451 | 2976 | 4124 | 4649 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 2152 | 1602 | 5751 | 6776 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 4948 | 5498 | 7424 | 8449 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 1328 | 753 | 9051 | 10576 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 5772 | 6347 | 10724 | 12224 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 4902 | 5952 | 8248 | 9298 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 504 | 96 | 12351 | 14376 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 6596 | 7196 | 14024 | 16049 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 5128 | 4053 | 8202 | 9752 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 11548 | 13098 | 9072 | 10147 |

The Rx impacts can be identified as below.

* 5th order IMD products generated by DC\_2\_n78 uplink may fall into own Rx of band 5.
* 3rd order IMD products generated by DC\_5\_n78 uplink may fall into own Rx of band 2.

5.125.3 ∆TIB and ∆RIB values

**Table 5.125.3-1: ΔTIB,**

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔTIB,c [dB]** |
| --- | --- | --- |
| DC\_2-5\_n78 | 2 | 0.6 |
| 5 | 0.6 |
| n78 | 0.8 |

**Table 5.125.3-2: ΔRIB,c**

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔRIB [dB]** |
| --- | --- | --- |
| DC\_2-5\_n78 | 2 | 0.2 |
| 5 | 0.2 |
| n78 | 0.5 |

5.125.4 Reference sensitivity exceptions

As stated in 5.125.2, for MSD requirement caused by IMDs is specified below accordingly, which is reused from DC\_2A-5A\_n77A.

**Table 5.125.5-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)**

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-5A\_n78A  DC\_2A-5A\_n78(2A) | 2 | 1907.5 | 5 | 25 | 1987.5 | N/A | N/A |
| 5 | 842.5 | 5 | 25 | 887.5 | 3.8 | IMD5 |
| n78 | 3305 | 5 | 25 | 3305 | N/A | N/A |
| 2 | 1907 | 5 | 25 | 1987 | 16.5 | IMD3 |
| 5 | 846.5 | 5 | 25 | 891.5 | N/A | N/A |
| n78 | 3680 | 5 | 25 | 3680 | N/A | N/A |

5.126 DC\_7-29\_n78

5.126.1 Operating bands for DC

**Table 5.126.1-1: Inter-band DC configurations (three bands)**

| **DC configuration** | **Uplink configuration** |
| --- | --- |
| DC\_7A-29A\_n78A  DC\_7C-29A\_n78A  DC\_7A-7A-29A\_n78A | DC\_7A\_n78A |

5.126.2 Co-existence studies

For UE coexistence study of Band 7 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.126.2-1.

**Table 5.126.2-1: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 2500 | 2570 | 3300 | 3800 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 5000 | 5140 | 6600 | 7600 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 7500 | 7710 | 9900 | 11400 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 10000 | 10280 | 13200 | 15200 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 12500 | 12850 | 16500 | 19000 |
| Two tone 2nd order IMD products | fy\_low – fx\_high | fy\_high – fx\_low | fx\_low + fy\_low | fx\_high + fy\_high |
| IMD frequency limits (MHz) | 730 | 1300 | 5800 | 6370 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | 2\*fy\_low – fx\_high | 2\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | -1200 | -1840 | 4030 | 5100 |
| Two-tone 3rd order IMD products | 2\*fx\_low + fy\_low | 2\*fx\_high + fy\_high | 2\*fy\_low + fx\_low | 2\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 8300 | 8940 | 9100 | 10170 |
| Two-tone 4th order IMD products | |3\*fx\_low – fy\_high| | |3\*fx\_high – fy\_low| | 3\*fy\_low – fx\_high | 3\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 3700 | 4410 | 7330 | 8900 |
| Two-tone 4th order IMD products | 3\*fx\_low + fy\_low | 3\*fx\_high + fy\_high | 3\*fy\_low + fx\_low | 3\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 10800 | 11510 | 12400 | 13900 |
| Two-tone 4th order IMD products | 2\*fy\_low – 2\*fx\_high | 2\*fy\_high – 2\*fx\_low | 2\*fx\_low + 2\*fy\_low | 2\*fx\_high + 2\*fy\_high |
| IMD frequency limits (MHz) | 1460 | 2600 | 11600 | 12740 |
| Two-tone 5th order IMD products | |4\*fx\_low – fy\_high| | |4\*fx\_high – fy\_low| | 4\*fy\_low – fx\_high | 4\*fy\_high – fx\_low |
| IMD frequency limits (MHz) | 6200 | 6980 | 10630 | 12700 |
| Two-tone 5th order IMD products | 4\*fx\_low + fy\_low | 4\*fx\_high + fy\_high | 4\*fy\_low + fx\_low | 4\*fy\_high + fx\_high |
| IMD frequency limits (MHz) | 13300 | 14080 | 15700 | 17770 |
| Two-tone 5th order IMD products | |3\*fx\_low – 2\*fy\_high| | |3\*fx\_high – 2\*fy\_low| | 3\*fy\_low – 2\*fx\_high | 3\*fy\_high – 2\*fx\_low |
| IMD frequency limits (MHz) | 100 | 1110 | 4760 | 6400 |
| Two-tone 5th order IMD products | 2\*fx\_low + 3\*fy\_low | 2\*fx\_high + 3\*fy\_high | 2\*fy\_low + 3\*fx\_low | 2\*fy\_high + 3\*fx\_high |
| IMD frequency limits (MHz) | 14900 | 16540 | 14100 | 15310 |

The Rx impacts can be identified as below.

* 5th order IMD products generated by DC\_7\_n78 uplink may fall into own Rx of band 29.

5.126.3 ∆TIB and ∆RIB values

**Table 5.126.3-1: ΔTIB,**

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔTIB,c [dB]** |
| --- | --- | --- |
| DC\_7-29\_n78 | 7 | 0.5 |
| n78 | 0.8 |

**Table 5.126.3-2: ΔRIB,c**

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔRIB [dB]** |
| --- | --- | --- |
| DC\_7-29\_n78 | n78 | 0.5 |

5.126.4 Reference sensitivity exceptions

As stated in 5.126.2, for MSD requirement caused by IMDs is specified below accordingly, which is derived from DC\_7A-28A\_n78A.

**Table 5.126.5-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)**

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-29A\_n78A  DC\_7C-29A\_n78A  DC\_7A-7A-29A\_n78A | 7 | 2540 | 5 | 25 | 2660 | N/A | N/A |
| 29 | N/A | N/A | N/A | 720 | 3.0 | IMD5 |
| n78 | 3450 | 10 | 50 | 3450 | N/A | N/A |

## 5.127 DC\_1-38\_n28

5.127.1 Configurations for DC

Table 5.127.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-38A\_n28A | DC\_1A\_n28A  DC\_38A\_n28A |
|  | |

5.127.2 Co-existence studies

For UE coexistence study of Band 1 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.127.2-1.

Table 5.127.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 703 | 748 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 1406 | 1496 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 2109 | 2244 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 2812 | 2992 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 3515 | 3740 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1277 | 1172 | 2623 | 2728 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 3092 | 3257 | 574 | 424 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4543 | 4708 | 3326 | 3476 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5012 | 5237 | 129 | 324 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6463 | 6688 | 4029 | 4224 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2344 | 2554 | 5246 | 5456 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1072 | 832 | 7217 | 6932 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1596 | 1851 | 4534 | 4264 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4732 | 4972 | 8383 | 8668 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5949 | 6204 | 7166 | 7436 |

For UE coexistence study of Band 38 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.127.2-2.

Table 5.127.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 703 | 748 | 2570 | 2620 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1406 | 1496 | 5140 | 5240 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2109 | 2244 | 7710 | 7860 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2812 | 2992 | 10280 | 10480 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3515 | 3740 | 12850 | 13100 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1822 | 1917 | 3273 | 3368 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 1214 | 1074 | 4392 | 4537 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 3976 | 4116 | 5843 | 5988 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 511 | 326 | 6962 | 7157 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4679 | 4864 | 8413 | 8608 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 3834 | 3644 | 6546 | 6736 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 9777 | 9532 | 422 | 192 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 6454 | 6214 | 2896 | 3131 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 10983 | 11228 | 5382 | 5612 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 9116 | 9356 | 7249 | 7484 |

There is no IMD interference for this band combination.

5.127.3 ∆TIB and ∆RIB values

For DC\_1-38\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination DC\_66\_n7, and are given in the tables below.

Table 5.127.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-38\_n28 | 1 | 0.5 |
| 38 | 0.5 |
| n28 | 0.6 |

**Table 5.127.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-38\_n28 | 1 | 0 |
| 38 | 0 |
| n28 | 0.2 |

5.127.4 Reference sensitivity exceptions

There is no MSD issue for this band combination.

## 5.128 DC\_3-38\_n28

5.128.1 Configurations for DC

Table 5.128.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-38A\_n28A  DC\_3C-38A\_n28A | DC\_3A\_n28A  DC\_38A\_n28A |
|  | |

5.128.2 Co-existence studies

For UE coexistence study of Band 38 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.128.2-1.

Table 5.128.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 703 | 748 | 2570 | 2620 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1406 | 1496 | 5140 | 5240 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2109 | 2244 | 7710 | 7860 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2812 | 2992 | 10280 | 10480 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3515 | 3740 | 12850 | 13100 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1822 | 1917 | 3273 | 3368 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 1214 | 1074 | 4392 | 4537 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 3976 | 4116 | 5843 | 5988 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 511 | 326 | 6962 | 7157 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4679 | 4864 | 8413 | 8608 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 3834 | 3644 | 6546 | 6736 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 9777 | 9532 | 422 | 192 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 6454 | 6214 | 2896 | 3131 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 10983 | 11228 | 5382 | 5612 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 9116 | 9356 | 7249 | 7484 |

For UE coexistence study of Band 3 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.128.2-2.

Table 5.128.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1785 | 703 | 748 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3570 | 1406 | 1496 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5355 | 2109 | 2244 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7140 | 2812 | 2992 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8925 | 3515 | 3740 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1082 | 962 | 2413 | 2533 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2672 | 2867 | 379 | 214 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4123 | 4318 | 3116 | 3281 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4382 | 4652 | 324 | 534 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 5833 | 6103 | 3819 | 4029 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1924 | 2164 | 4826 | 5066 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1282 | 1027 | 6437 | 6092 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1176 | 1461 | 3949 | 3634 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4522 | 4777 | 7543 | 7888 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5529 | 5814 | 6536 | 6851 |

IMD2 may fall into Rx of band 3 when band 38 and n28 transmit.

5.128.3 ∆TIB and ∆RIB values

For DC\_3-38\_n28, the ΔTIB,c and ΔRIB,c values are reused from the LTE combination DC\_66\_n7, and are given in the tables below.

Table 5.128.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-38\_n28 | 3 | 0.5 |
| 38 | 0.5 |
| n28 | 0.6 |

**Table 5.128.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-38\_n28 | 3 | 0 |
| 38 | 0 |
| n28 | 0.2 |

5.128.4 Reference sensitivity exceptions

The MSD requirements due to IMD2 from DC\_3A-41A\_n28A can be reused for DC\_3-38\_n28. Thus, the requirements can be specified as below.

Table 5.128.4-1 MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_3A-38A\_n28A  DC\_3C-38A\_n28A | 38 | 2575 | 5 | 25 | 2575 | N/A | N/A |
|  | n28 | 725 | 5 | 25 | 780 | N/A | N/A |
|  | 3 | 1755 | 5 | 25 | 1850 | 26 | IMD2 |

## 5.129 DC\_14-30\_n66

5.129.1 Operating bands for EN-DC

Table 5.129.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 14-30\_n66 | CA\_14-30 | n66 |  |

### 5.129.2 Configuration for DC

Table 5.129.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_14A-30A\_n66A | DC\_14A\_n66A DC\_30A\_n66A | CA\_14A-30A | n66A |

5.129.3 ∆TIB and ∆RIB values

For DC\_14-30\_n66, the ΔTIB,c and ΔRIB,c values are reused from CA\_14-30-66 and are given in the tables below.

**Table 5.129.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_14-30\_n66 | 14 | 0.3 |
| 30 | 0.3 |
| n66 | 0.5 |

**Table 5.129.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_14-30\_n66 | 14 | 0 |
| 30 | 0.5 |
| n66 | 0.4 |

5.129.4 REFSENS requirements

There are no IMD impact from UL 14\_n66 affecting DL band 30, and there are no IMD impact from UL 30\_n66 affecting DL band 14. Therefore, MSD is not needed to be defined.

5.130 DC\_14-30\_n2

5.130.1 Operating bands for EN-DC

Table 5.130.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 14-30\_n2 | CA\_14-30 | n2 |  |

### 5.130.2 Configuration for DC

Table 5.130.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_14A-30A\_n2A | DC\_14A\_n2A DC\_30A\_n2A | CA\_14A-30A | n2A |

5.130.3 ∆TIB and ∆RIB values

For DC\_14-30\_n2, the ΔTIB,c and ΔRIB,c values are reused from DC\_12-30\_n2 and are given in the tables below.

**Table 5.130.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_14-30\_n2 | 14 | 0.3 |
| 30 | 0.3 |
| n2 | 0.5 |

**Table 5.130.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_14-30\_n2 | 14 | 0 |
| 30 | 0.5 |
| n2 | 0.4 |

5.130.4 REFSENS requirements

There are no IMD impact from UL 14\_n2 affecting DL band 30, and there are no IMD impact from UL 30\_n2 affecting DL band 14. Therefore, MSD is not needed to be defined.

5.131 DC\_2-(n)5

5.131.1 Operating bands for EN-DC

Table 5.131.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_2-(n)5 | CA\_2-5 | n5 |  |

### 5.131.2 Configuration for DC

Table 5.131.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-(n)5AA | DC\_2A\_n5A  DC\_(n)5AA1 | CA\_2A-5A | n5A |
| NOTE1: Only single switched UL is supported | | | |

5.131.3 ∆TIB and ∆RIB values

For DC\_2-(n)5, the ΔTIB,c and ΔRIB,c values are reused from DC\_2\_n5 and are given in the tables below.

**Table 5.131.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-(n)5 | 2 | 0.3 |
| 5 | 0.3 |
| n5 | 0.3 |

**Table 5.131.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-(n)5 | 2 | 0 |
| 5 | 0 |
| n5 | 0 |

5.131.4 REFSENS requirements

No additional MSD requirements need to be defined.

5.132 DC\_30-(n)5

5.132.1 Operating bands for EN-DC

Table 5.132.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_30-(n)5 | CA\_30-5 | n5 |  |

### 5.132.2 Configuration for DC

Table 5.132.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_30A-(n)5AA | DC\_30A\_n5A  DC\_(n)5AA1 | CA\_30A-5A | n5A |
| NOTE1: Only single switched UL is supported | | | |

5.132.3 ∆TIB and ∆RIB values

For DC\_30-(n)5, the ΔTIB,c and ΔRIB,c values are reused from DC\_30\_n5 and are given in the tables below.

**Table 5.132.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_30-(n)5 | 30 | 0.3 |
| 5 | 0.3 |
| n5 | 0.3 |

**Table 5.132.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_30-(n)5 | 30 | 0 |
| 5 | 0 |
| n5 | 0 |

5.132.4 REFSENS requirements

No additional MSD requirements need to be defined.

5.133 DC\_28-40\_n78

5.133.1 Operating bands for EN-DC

Table 5.133.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 28-40\_n78 | CA\_28-40 | n78 |  |

### 5.133.2 Configuration for DC

Table 5.133.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_28A-40A\_n78A | DC\_28A\_n78A DC\_40A\_n78A | CA\_28A-40A | n78A |
| DC\_28A-40C\_n78A | DC\_28A\_n78A DC\_40A\_n78A | CA\_28A-40C | n78A |

5.133.3 ∆TIB and ∆RIB values

For DC\_28-40\_n78, the ΔTIB,c and ΔRIB,c values are reused from DC\_28\_n40-n78 and are given in the tables below.

**Table 5.133.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_28-40\_n78 | 28 | 0.5 |
| 40 | 0.3 |
| n78 | 0.8 |

**Table 5.133.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_28-40\_n78 | 28 | 0.2 |
| 40 | 0.4 |
| n78 | 0.5 |

5.133.4 REFSENS requirements

UL 28\_n78 might cause IMD3 into 40 DL. MSD value for 40 is chosen as in DC\_28A\_n1A-n78A.

UL 40\_n78 might cause IMD3 into the sidelobe of 28 DL. MSD value for 28 is chosen as in DC\_20A-40A\_n78A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_28A-40A\_n78A DC\_28A-40C\_n78A | 28 | N/A | 5 | 25 | 800.5 | 11 | IMD3 |
| 40 | 2302.5 | 5 | 25 | 2302.5 | N/A | N/A |
| n78 | 3795 | 10 | 50 | 3795 | N/A | N/A |
| 28 | 715 | 5 | 25 | 770 | N/A | N/A |
| 40 | 2320 | 5 | 25 | 2320 | 15.7 | IMD3 |
| n78 | 3750 | 10 | 50 | 3750 | N/A | N/A |

5.134 DC\_7-13\_n25

5.134.1 Operating bands for EN-DC

Table 5.134.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 7-13\_n25 | CA\_7-13 | n25 |  |

### 5.134.2 Configuration for DC

Table 5.134.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_7A-13A\_n25A | DC\_7A\_n25A DC\_13A\_n25A | CA\_7A-13A | n25A |
| DC\_7A-7A-13A\_n25A | DC\_7A\_n25A DC\_13A\_n25A | CA\_7A-7A-13A | n25A |
| DC\_7C-13A\_n25A | DC\_7A\_n25A DC\_13A\_n25A | CA\_7C-13A | n25A |

5.134.3 ∆TIB and ∆RIB values

For DC\_7-13\_n25, the ΔTIB,c and ΔRIB,c values are reused from DC\_7-28\_n2 and are given in the tables below.

**Table 5.134.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-13\_n25  DC\_7-7-13\_n25 | 7 | 0.5 |
| 13 | 0.3 |
| n25 | 0.5 |

**Table 5.134.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-13\_n25  DC\_7-7-13\_n25 | 7 | 0 |
| 13 | 0 |
| n25 | 0 |

5.134.4 REFSENS requirements

There are no IMD impact from UL 7\_n25 affecting DL band 13.

There are IMD2 impact from UL 13\_n25 affecting DL band 7. The MSD value is derived from DC\_7A-28A\_n2A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_7A-13A\_n25A  DC\_7A-7A-13A\_n25A  DC\_7C-13A\_n25A | 7 | 2542 | 10 | 50 | 2662 | 27.6 | IMD2 |
| 13 | 782 | 5 | 25 | 751 | N/A | N/A |
| n25 | 1880 | 5 | 25 | 1960 | N/A | N/A |

5.135 DC\_7-66\_n25

5.135.1 Operating bands for EN-DC

Table 5.135.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 7-66\_n25 | CA\_7-66 | n25 |  |

### 5.135.2 Configuration for DC

Table 5.135.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_7A-66A\_n25A | DC\_7A\_n25A DC\_66A\_n25A | CA\_7A-66A | n25A |
| DC\_7A-7A-66A\_n25A | DC\_7A\_n25A DC\_66A\_n25A | CA\_7A-7A-66A | n25A |
| DC\_7C-66A\_n25A | DC\_7A\_n25A DC\_66A\_n25A | CA\_7C-66A | n25A |

5.135.3 ∆TIB and ∆RIB values

For DC\_7-66\_n25, the ΔTIB,c and ΔRIB,c values are reused from DC\_2-7\_n66 and are given in the tables below.

**Table 5.135.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-66\_n25  DC\_7-7-66\_n25 | 7 | 0.5 |
| 66 | 0.5 |
| n25 | 0.5 |

**Table 5.135.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-66\_n25  DC\_7-7-66\_n25 | 7 | 0.3 |
| 66 | 0.5 |
| n25 | 0.5 |

5.135.4 REFSENS requirements

There are no IMD impact from UL 7\_n25 affecting DL band 66.

There are no IMD impact from UL 66\_n25 affecting DL band 7.

5.136 DC\_3-7\_n3

5.136.1 Operating bands for EN-DC

Table 5.136.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 3-7\_n3 | CA\_3-7 | n3 |  |

### 5.136.2 Configuration for DC

Table 5.136.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_3A-7A\_n3A | DC\_3A\_n3A1  DC\_7A\_n3A | CA\_3A-7A | n3A |
| DC\_3A-7C\_n3A | DC\_3A\_n3A1  DC\_7A\_n3A  DC\_7C\_n3A | CA\_3A-7C | n3A |
| NOTE 1: Only single switched UL is supported | | | |

5.136.3 ∆TIB and ∆RIB values

For DC\_3-7\_n3, the ΔTIB,c and ΔRIB,c values are reused from DC\_7\_n3 and are given in the tables below.

**Table 5.136.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-7\_n3 | 3 | 0.5 |
| 7 | 0.5 |
| n3 | 0.5 |

**Table 5.136.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-7\_n3 | 3 | 0 |
| 7 | 0 |
| n3 | 0 |

5.136.4 REFSENS requirements

No additional MSD requirements need to be defined.

5.137 DC\_3-28\_n3

5.137.1 Operating bands for EN-DC

Table 5.137.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 3-28\_n3 | CA\_3-28 | n3 |  |

### 5.137.2 Configuration for DC

Table 5.137.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_3A-28A\_n3A | DC\_3A\_n3A1  DC\_28A\_n3A | CA\_3A-28A | n3A |
| NOTE 1: Only single switched UL is supported | | | |

5.137.3 ∆TIB and ∆RIB values

For DC\_3-28\_n3, the ΔTIB,c and ΔRIB,c values are reused from DC\_28\_n3 and are given in the tables below.

**Table 5.137.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-28\_n3 | 3 | 0.3 |
| 28 | 0.3 |
| n3 | 0.3 |

**Table 5.137.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-28\_n3 | 3 | 0 |
| 28 | 0 |
| n3 | 0 |

5.137.4 REFSENS requirements

No additional MSD requirements need to be defined.

5.138 DC\_3-3-7\_n8, DC\_3-7-7\_n8, DC\_3-3-7-7\_n8

5.138.1 Configuration for DC

**Table 5.138.1-1: Inter-band DC configurations (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration |
| --- | --- |
| DC\_3A-3A-7A\_n8A  DC\_3A-7A-7A\_n8A  DC\_3A-3A-7A-7A\_n8A | DC\_3A\_n8A  DC\_7A\_n8A |

5.138.2 Co-existence studies

The co-existence studies can be covered by the fallback combination, DC\_3-7\_n8, which was specified in Rel.16. Based on the studies in TR 37.716-21-11 section 5.1.124, the IMD2 and IMD3 for Tx band 3 + band n8 may fall into Rx of band 7.

5.138.3 ∆TIB and ∆RIB values

For DC\_3-3\_n8, the ΔTIB,c and ΔRIB,c values are given in the tables below.

**Table 5.138.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-3-7\_n8  DC\_3-7-7\_n8  DC\_3-3-7-7\_n8 | 3 | 0.5 |
| 7 | 0.5 |
| n8 | 0.6 |

**Table 5.138.3-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB,c [dB] |
| --- | --- | --- |
| DC\_3-3-7\_n8  DC\_3-7-7\_n8  DC\_3-3-7-7\_n8 | 3 | 0 |
| 7 | 0 |
| n8 | 0.2 |

5.138.4 Reference sensitivity exceptions

The needed exceptions can be covered by the fallback combination, DC\_3-7\_n8, which was specified in Rel.16. No additional exception is foreseen.

## 5.139 DC\_13-46\_n66

5.139.1 Configurations for DC

Table 5.139.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_13A-46A\_n66A3 | DC\_13A\_n66A |
| NOTE 3: Restricted to E-UTRA operation when inter-band carrier aggregation is configured. The downlink operating band for Band 46 is paired with the uplink operating band (external E-UTRA band) of the carrier aggregation configuration that is supporting the configured Pcell. | |

### 5.139.2 Co-existence studies

Co-existence studies have been performed for lower order combinations of DC\_13A\_n66, where:

- 4th and 5th IMD product caused by DC\_13A\_n66A may fall into own Rx of band 46.

5.139.3 ∆TIB and ∆RIB values

Values are reused from CA including same bands, CA\_13-46-66, as given in 36.101.

Table 5.139.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_13-46\_n66 | 13 | 0.3 |
| 46 | 0 |
| n66 | 0.3 |

Table 5.139.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_13-46\_n66 | 13 | 0 |
| 46 | 0 |
| n66 | 0 |

5.139.4 Reference sensitivity exceptions

Based on co-existence analysis it is found that MSD is needed due to 4th and 5th IMD falling into own Rx band of 46. Therefor additional MSD is needed defined in Table 7.3B.2.3.5.2-1 of 38.101-3.

Table 5. x.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_13A-46A\_n66A5 | 13 | N/A | N/A | N/A | N/A | N/A | N/A |
| 46 | N/A | N/A | N/A | N/A | N/A | IMD4,  IMD5 |
| n66 | N/A | N/A | N/A | N/A | N/A | N/A |
| NOTE 5: When Band 46 have self-interference problems by dual uplink CA/EN-DC, then the requirements do not apply in exclusion zone which is frequency range within (harmonics frequency region + FHD) and IMD frequency region as follow.  IMD frequency range   |  |  |  |  | | --- | --- | --- | --- | | DL\_CA configuration | UL\_CA configuration | Exclusion zone center frequency | Exclusion zone BW | | DC\_2A-46A\_n66A | DC\_2A\_n66A | 2\*fc\_2A + fc\_n66A | 2\*BW\_2A + BW\_n66A | | DC\_2A-46A\_n66A | DC\_2A\_n66A | fc\_2A + 2\*fc\_n66A | BW\_2A + 2\*BW\_n66A | | DC\_13A-46A\_n66A | DC\_13A\_n66A | 3\*fc\_13A + fc\_n66A | BW\_13A + 2\*BW\_n66A | | DC\_13A-46A\_n66A | DC\_13A\_n66A | 2\*fc\_13A + 3\*fc\_n66A | BW\_13A + 2\*BW\_n66A | | | | | | | | |

## 5.140 DC\_46-48\_n66

5.140.1 Configurations for DC

Table 5.140.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_46A-48A\_n66A3  DC\_46C-48A\_n66A3  DC\_46D-48A\_n66A3  DC\_46E-48A\_n66A3 | DC\_48A\_n66A |
| NOTE 3: Restricted to E-UTRA operation when inter-band carrier aggregation is configured. The downlink operating band for Band 46 is paired with the uplink operating band (external E-UTRA band) of the carrier aggregation configuration that is supporting the configured Pcell. | |

### 5.140.2 Co-existence studies

Co-existence studies have been performed for lower order combinations of DC\_48A\_n66, where:

- 2nd and 3rd IMD product caused by DC\_48A\_n66A may fall into own Rx of band 46.

5.140.3 ∆TIB and ∆RIB values

Values are reused from CA including same bands, CA\_46-48-66, as given in 36.101.

Table 5.140.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_46-48\_n66 | 46 | 0 |
| 48 | 0.8 |
| 66 | 0.6 |

Table 5.140.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_46-48\_n66 | 46 | 0 |
| 48 | 0.5 |
| 66 | 0.3 |

5.140.4 Reference sensitivity exceptions

Based on co-existence analysis it is found that MSD is needed due to 2nd and 3rd IMD falling into own Rx band of 46. Therefor additional MSD is needed defined in Table 7.3B.2.3.5.2-1 of 38.101-3.

Table 5. x.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_46A-48A\_n66A5  DC\_46C-48A\_n66A5  DC\_46D-48A\_n66A5  DC\_46E-48A\_n66A5 | 46 | N/A | N/A | N/A | N/A | N/A | IMD2,  IMD3 |
| 48 | N/A | N/A | N/A | N/A | N/A | N/A |
| n66 | N/A | N/A | N/A | N/A | N/A | N/A |
| NOTE 5: When Band 46 have self-interference problems by dual uplink CA/EN-DC, then the requirements do not apply in exclusion zone which is frequency range within (harmonics frequency region + FHD) and IMD frequency region as follow.  IMD frequency range   |  |  |  |  | | --- | --- | --- | --- | | DL\_CA configuration | UL\_CA configuration | Exclusion zone center frequency | Exclusion zone BW | | DC\_2A-46A\_n66A | DC\_2A\_n66A | 2\*fc\_2A + fc\_n66A | 2\*BW\_2A + BW\_n66A | | DC\_2A-46A\_n66A | DC\_2A\_n66A | fc\_2A + 2\*fc\_n66A | BW\_2A + 2\*BW\_n66A | | DC\_46-48A\_n66A | DC\_48A\_n66A | fc\_48A + fc\_n66A | BW\_48A + 2\*BW\_n66A | | DC\_46-48A\_n66A | DC\_48A\_n66A | 2\*fc\_48A + fc\_n66A | 2\*BW\_48A + BW\_n66A | | | | | | | | |

## 5.141 DC\_2-46\_n5

5.141.1 Configurations for DC

Table 5.141.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_2A-46A\_n5A3  DC\_2A-46C\_n5A3  DC\_2A-46D\_n5A3  DC\_2A-46E\_n5A3 | DC\_2A\_n5A |
| NOTE 3: Restricted to E-UTRA operation when inter-band carrier aggregation is configured. The downlink operating band for Band 46 is paired with the uplink operating band (external E-UTRA band) of the carrier aggregation configuration that is supporting the configured Pcell. | |

### 5.141.2 Co-existence studies

Co-existence studies have been performed for lower order combinations of DC\_2A\_n5, where:

- 4th and 5th IMD product caused by DC\_2A\_n5A may fall into own Rx of band 46.

5.141.3 ∆TIB and ∆RIB values

Values are reused from CA including same bands, CA\_2-5-46, as given in 36.101.

Table 5.141.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_2-46\_n5 | 2 | 0.3 |
| 46 | 0 |
| n5 | 0.3 |

Table 5.141.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_2-46\_n5 | 2 | 0 |
| 46 | 0 |
| n5 | 0 |

5.141.4 Reference sensitivity exceptions

Based on co-existence analysis it is found that MSD is needed due to 4th and 5th IMD falling into own Rx band of 46. Therefor additional MSD is needed defined in Table 7.3B.2.3.5.2-1 of 38.101-3.

Table 5. x.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-46A\_n5A5  DC\_2A-46C\_n5A5  DC\_2A-46D\_n5A5  DC\_2A-46E\_n5A5 | 2 | N/A | N/A | N/A | N/A | N/A | N/A |
| 46 | N/A | N/A | N/A | N/A | N/A | IMD4,  IMD5 |
| n5 | N/A | N/A | N/A | N/A | N/A | N/A |
| NOTE 5: When Band 46 have self-interference problems by dual uplink CA/EN-DC, then the requirements do not apply in exclusion zone which is frequency range within (harmonics frequency region + FHD) and IMD frequency region as follow.  IMD frequency range   |  |  |  |  | | --- | --- | --- | --- | | DL\_CA configuration | UL\_CA configuration | Exclusion zone center frequency | Exclusion zone BW | | DC\_2A-46A\_n66A | DC\_2A\_n66A | 2\*fc\_2A + fc\_n66A | 2\*BW\_2A + BW\_n66A | | DC\_2A-46A\_n66A | DC\_2A\_n66A | fc\_2A + 2\*fc\_n66A | BW\_2A + 2\*BW\_n66A | | DC\_2A-46\_n5A | DC\_2A\_n5A | 2\*fc\_2A + 2\*fc\_n5A | BW\_2A + 2\*BW\_n5A | | DC\_2A-46\_n5A | DC\_2A\_n5A | fc\_2A + 4\*fc\_n5A | BW\_2\*2A + BW\_n5A | | | | | | | | |

## 5.142 DC\_46-48\_n5

5.142.1 Configurations for DC

Table 5.142.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_46A-48A\_n5A3  DC\_46C-48A\_n5A3  DC\_46D-48A\_n5A3  DC\_46E-48A\_n5A3 | DC\_48A\_n5A |
| NOTE 3: Restricted to E-UTRA operation when inter-band carrier aggregation is configured. The downlink operating band for Band 46 is paired with the uplink operating band (external E-UTRA band) of the carrier aggregation configuration that is supporting the configured Pcell. | |

### 5.142.2 Co-existence studies

Co-existence studies have been performed for lower order combinations of DC\_48A\_n5, where:

- 3rd and 4th IMD product caused by DC\_48A\_n5A may fall into own Rx of band 46.

5.142.3 ∆TIB and ∆RIB values

Values are reused from CA including same bands as given in 36.101.

Table 5.142.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_46-48\_n5 | 46 | 0 |
| 48 | 0.8 |
| n5 | 0.3 |

Table 5.142.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_46-48\_n5 | 46 | 0 |
| 48 | 0.5 |
| n5 | 0 |

5.142.4 Reference sensitivity exceptions

Based on co-existence analysis it is found that MSD is needed due to 3rd and 4th IMD falling into own Rx band of 46. Therefor additional MSD is needed defined in Table 7.3B.2.3.5.2-1 of 38.101-3.

Table 5.142.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_46A-48A\_n5A5  DC\_46C-48A\_n5A5  DC\_46D-48A\_n5A5  DC\_46E-48A\_n5A5 | 46 | N/A | N/A | N/A | N/A | N/A | IMD2,  IMD3 |
| 48 | N/A | N/A | N/A | N/A | N/A | N/A |
| n5 | N/A | N/A | N/A | N/A | N/A | N/A |
| NOTE 5: When Band 46 have self-interference problems by dual uplink CA/EN-DC, then the requirements do not apply in exclusion zone which is frequency range within (harmonics frequency region + FHD) and IMD frequency region as follow.  IMD frequency range   |  |  |  |  | | --- | --- | --- | --- | | DL\_CA configuration | UL\_CA configuration | Exclusion zone center frequency | Exclusion zone BW | | DC\_2A-46A\_n66A | DC\_2A\_n66A | 2\*fc\_2A + fc\_n66A | 2\*BW\_2A + BW\_n66A | | DC\_2A-46A\_n66A | DC\_2A\_n66A | fc\_2A + 2\*fc\_n66A | BW\_2A + 2\*BW\_n66A | | DC\_46-48A\_n5A | DC\_48A\_n5A | 2\*fc\_48A + fc\_n5A | BW\_48A + 2\*BW\_n5A | | DC\_46-48A\_n5A | DC\_48A\_n5A | 2\*fc\_48A + 2\*fc\_n5A | BW\_2\*48A + BW\_n5A | | | | | | | | |

## 5.143 DC\_20-28\_n1

5.143.1 Configurations for DC

Table 5.143.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_20A-28A\_n1A | DC\_20A\_n1A  DC\_28A\_n1A |

5.143.2 Co-existence studies

For UE coexistence study of Band 28 + Band n1, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.143.2-1.

Table 5.143.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 703 | 748 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 1406 | 1496 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 2109 | 2244 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 2812 | 2992 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 3515 | 3740 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1277 | 1172 | 2623 | 2728 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 3092 | 3257 | 574 | 424 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4543 | 4708 | 3326 | 3476 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5012 | 5237 | 129 | 324 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6463 | 6688 | 4029 | 4224 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2344 | 2554 | 5246 | 5456 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1072 | 832 | 7217 | 6932 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1596 | 1851 | 4534 | 4264 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4732 | 4972 | 8383 | 8668 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5949 | 6204 | 7166 | 7436 |

For UE coexistence study of Band 20 + Band n1, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.143.2-2.

Table 5.143.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 832 | 862 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 1664 | 1724 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 2496 | 2586 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 3328 | 3448 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 4160 | 4310 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1148 | 1058 | 2752 | 2842 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2978 | 3128 | 316 | 196 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4672 | 4822 | 3584 | 3704 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4898 | 5108 | 516 | 666 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6592 | 6802 | 4416 | 4566 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2116 | 2296 | 5504 | 5684 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1528 | 1348 | 7088 | 6818 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1254 | 1464 | 4276 | 4036 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5248 | 5428 | 8512 | 8782 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6336 | 6546 | 7424 | 7664 |

5.143.3 ∆TIB and ∆RIB values

For DC\_20-28\_n1, the ΔTIB,c and ΔRIB,c values are reused from DC\_1-20\_n8, and are given in the tables below.

Table 5.143.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20-28\_n1 | n1 | 0.5 |
| 20 | 0.6 |
| 28 | 0.6 |

**Table 5.143.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20-28\_n1 | n1 | 0 |
| 20 | 0.2 |
| 28 | 0.2 |

5.143.4 Reference sensitivity exceptions

There is no MSD requirements for this band combination.

## 5.144 DC\_8-20\_n1

5.144.1 Configurations for DC

Table 5.144.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-20A\_n1A | DC\_8A\_n1A  DC\_20A\_n1A |
|  | |

5.144.2 Co-existence studies

For UE coexistence study of Band 8 + Band n1, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.144.2-1.

Table 5.144.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 880 | 915 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 1760 | 1830 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 2640 | 2745 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 3520 | 3660 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 4400 | 4575 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1100 | 1005 | 2800 | 2895 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2925 | 3080 | 220 | 90 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4720 | 4875 | 3680 | 3810 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4845 | 5060 | 660 | 825 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6640 | 6855 | 4560 | 4725 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2010 | 2200 | 5600 | 5790 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1740 | 1540 | 7040 | 6765 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1095 | 1320 | 4180 | 3930 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5440 | 5640 | 8560 | 8835 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6480 | 6705 | 7520 | 7770 |

For UE coexistence study of Band 20 + Band n1, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.144.2-2.

Table 5.144.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 832 | 862 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 1664 | 1724 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 2496 | 2586 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 3328 | 3448 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 4160 | 4310 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1148 | 1058 | 2752 | 2842 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2978 | 3128 | 316 | 196 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4672 | 4822 | 3584 | 3704 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4898 | 5108 | 516 | 666 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6592 | 6802 | 4416 | 4566 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2116 | 2296 | 5504 | 5684 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1528 | 1348 | 7088 | 6818 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1254 | 1464 | 4276 | 4036 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5248 | 5428 | 8512 | 8782 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6336 | 6546 | 7424 | 7664 |

IMD4 of Tx band 8 + band n1 may fall into Rx of band 20.

5.144.3 ∆TIB and ∆RIB values

For DC\_8-20\_n1, the ΔTIB,c and ΔRIB,c values are reused from DC\_1-20\_n8, and are given in the tables below.

Table 5.144.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8-20\_n1 | n1 | 0.3 |
| 8 | 0.4 |
| 20 | 0.4 |

**Table 5.144.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8-20\_n1 | n1 | 0 |
| 8 | 0 |
| 20 | 0 |

5.144.4 Reference sensitivity exceptions

MSD due to IMD4 for DC\_1-20\_n8 can be reused for this combination, referring to approved R4-2001051.

Table 5.144.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_8-20\_n1 | n1 | 1925 | 5 | 25 | 2115 | N/A | N/A |
| 8 | 910 | 5 | 25 | 955 | N/A | N/A |
| 20 | 846 | 5 | 25 | 805 | 11.5 | IMD4 |

## 5.145 DC\_8-20\_n3

5.145.1 Configurations for DC

Table 5.145.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-20A\_n3A | DC\_8A\_n3A  DC\_20A\_n3A |
|  | |

5.145.2 Co-existence studies

For UE coexistence study of Band 8 + Band n3, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.145.2-1.

Table 5.145.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1785 | 880 | 915 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3570 | 1760 | 1830 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5355 | 2640 | 2745 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7140 | 3520 | 3660 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8925 | 4400 | 4575 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 905 | 795 | 2590 | 2700 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2505 | 2690 | 25 | 120 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4300 | 4485 | 3470 | 3615 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4215 | 4475 | 855 | 1035 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6010 | 6270 | 4350 | 4530 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1590 | 1810 | 5180 | 5400 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1950 | 1735 | 6260 | 5925 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 675 | 930 | 3595 | 3300 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5230 | 5445 | 7720 | 8055 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6060 | 6315 | 6890 | 7185 |

For UE coexistence study of Band 20 + Band n3, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.145.2-2.

Table 5.145.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1785 | 832 | 862 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3570 | 1664 | 1724 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5355 | 2496 | 2586 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7140 | 3328 | 3448 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8925 | 4160 | 4310 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 953 | 848 | 2542 | 2647 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2558 | 2738 | 121 | 14 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4252 | 4432 | 3374 | 3509 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4268 | 4523 | 711 | 876 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 5962 | 6217 | 4206 | 4371 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1696 | 1906 | 5084 | 5294 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1738 | 1543 | 6308 | 5978 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 834 | 1074 | 3691 | 3406 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5038 | 5233 | 7672 | 8002 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5916 | 6156 | 6794 | 7079 |

IMD2 and IMD5 of Tx band 8 + band n3 may fall into Rx of band 20.

IMD2 and IMD5 of Tx band 20 + band n3 may fall into Rx of band 8.

5.145.3 ∆TIB and ∆RIB values

For DC\_8-20\_n3, the ΔTIB,c and ΔRIB,c values are reused from DC\_3-20\_n8, and are given in the tables below.

Table 5.145.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8-20\_n3 | n3 | 0.3 |
| 8 | 0.4 |
| 20 | 0.4 |

**Table 5.145.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8-20\_n3 | n3 | 0 |
| 8 | 0 |
| 20 | 0 |

5.145.4 Reference sensitivity exceptions

The MSD due to IMD2 for DC\_3-20\_n8 can be reused for this combination, referring to approved R4-2001053.

Table 5.145.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_8-20\_n3 | n3 | 1720 | 5 | 25 | 1815 | N/A | N/A |
| 8 | 910 | 5 | 25 | 955 | N/A | N/A |
| 20 | 851 | 5 | 25 | 810 | 27 | IMD24  |fn8-fB3| |
| DC\_8-20\_n3 | n3 | 1770 | 5 | 25 | 1865 | N/A | N/A |
| 8 | 890 | 5 | 25 | 930 | 27 | IMD24  |fn20-fB3| |
| 20 | 840 | 5 | 25 | 799 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. | | | | | | | |

5.146 DC\_2-13\_n25

5.146.1 Operating bands for EN-DC

Table 5.146.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 2-13\_n25 | CA\_2-13 | n25 |  |

### 5.146.2 Configuration for DC

Table 5.146.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-13A\_n25A13,14 | DC\_13A\_n25A | CA\_2A-13A | n25A |
| NOTE 13: For UEs not indicating *interBandMRDC-WithOverlapDL-Bands-r16*, the minimum requirements for intra-band contiguous or non-contiguous EN-DC apply for the Band 42 and Band n77/n78 combinations and for the Band 2 and Band n25 combinations.  NOTE 14: For UEs not indicating *interBandMRDC-WithOverlapDL-Bands-r16*, the minimum requirements for inter-band EN-DC apply when the maximum power spectral density imbalance between downlink carriers contained in overlapping or partially overlapping DL bands is within 6 dB. | | | |

5.146.3 ∆TIB and ∆RIB values

For DC\_2-13\_n25, the ΔTIB,c and ΔRIB,c values are reused from DC\_13\_n2 and are given in the tables below.

**Table 5.146.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-13\_n25 | 2 | 0.3 |
| 13 | 0.3 |
| n25 | 0.3 |

**Table 5.146.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-13\_n25 | 2 | 0 |
| 13 | 0 |
| n25 | 0 |

5.146.4 REFSENS requirements

There are no IMD impact from UL 13\_n25 affecting DL band 2.

5.147 DC\_2-66\_n25

5.147.1 Operating bands for EN-DC

Table 5.147.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band | Single UL allowed |
| --- | --- | --- | --- |
| 2-66\_n25 | CA\_2-66 | n25 | DC\_66\_n25 |

### 5.147.2 Configuration for DC

Table 5.147.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-66A\_n25A13,14 | DC\_66A\_n25A | CA\_2A-66A | n25A |
| NOTE 13: For UEs not indicating *interBandMRDC-WithOverlapDL-Bands-r16*, the minimum requirements for intra-band contiguous or non-contiguous EN-DC apply for the Band 42 and Band n77/n78 combinations and for the Band 2 and Band n25 combinations.  NOTE 14: For UEs not indicating *interBandMRDC-WithOverlapDL-Bands-r16*, the minimum requirements for inter-band EN-DC apply when the maximum power spectral density imbalance between downlink carriers contained in overlapping or partially overlapping DL bands is within 6 dB. | | | |

5.147.3 ∆TIB and ∆RIB values

For DC\_2-66\_n25, the ΔTIB,c and ΔRIB,c values are reused from DC\_66\_n2 and are given in the tables below.

**Table 5.147.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-66\_n25 | 2 | 0.5 |
| 66 | 0.5 |
| n25 | 0.5 |

**Table 5.147.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-66\_n25 | 2 | 0.3 |
| 66 | 0.3 |
| n25 | 0.3 |

5.147.4 REFSENS requirements

There is IMD3 impact from UL 66\_n25 affecting DL band 2. The MSD value is derived from DC\_66A\_n25A.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-66A\_n25A | 2 | 1895 | 5 | 25 | 1975 | 20 | IMD3 |
| 66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
| n25 | 1875 | 5 | 25 | 1955 | N/A | N/A |

## 5.148 DC\_2-12\_n77

### 5.148.1 Configurations for DC

Table 5.148.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_2A-12A\_n77A | DC\_2A\_n77A  DC\_12A\_n77A |

### 5.148.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- There are no IMD products produced by Band 2 and n77 that might fall in Rx of band 12.

- IMD3 and IMD4 products are produced by Band 12 and n77 that might fall in Rx of band 2.

### 5.148.3 ∆TIB and ∆RIB values

For DC\_2-12\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n2-n12-n77.

Table 5.148.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-12\_n77 | 2 | 0.6 |
| 12 | 0.3 |
| n77 | 0.8 |

Table 5.148.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-12\_n77 | 2 | 0.2 |
| 12 | 0.2 |
| n77 | 0.5 |

### 5.148.4 Reference sensitivity exceptions

Table 5.148.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n2A-n12A-n77A.

Table 5.148.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-12A\_n77A | 2 | 1880 | 5 | 25 | 1960 | 16.5 | IMD39,11 |
| 12 | 707.5 | 5 | 25 | 737.5 | N/A | N/A |
| n77 | 3375 | 10 | 50 | 3375 | N/A | N/A |
| NOTE 9: This band is subject to IMD4 also which MSD is not specified.  NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | |

## 5.149 DC\_2-14\_n77

### 5.149.1 Configurations for DC

Table 5.149.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_2A-14A\_n77A | DC\_2A\_n77A  DC\_14A\_n77A |

### 5.149.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- There are no IMD products produced by Band 2 and n77 that might fall in Rx of band 14.

- IMD3 products are produced by Band 14 and n77 that might fall in Rx of band 2.

### 5.149.3 ∆TIB and ∆RIB values

For DC\_2-14\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n2-n14-n77.

Table 5.149.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-14\_n77 | 2 | 0.5 |
| 14 | 0.3 |
| n77 | 0.8 |

Table 5.149.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-14\_n77 | 2 | 0.2 |
| 14 | 0.2 |
| n77 | 0.5 |

### 5.149.4 Reference sensitivity exceptions

Table 5.149.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n2A-n14A-n77A.

Table 5.149.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-14A\_n77A | 2 | 1874 | 5 | 25 | 1954 | 16.5 | IMD3 |
| 14 | 793 | 5 | 25 | 763 | N/A | N/A |
| n77 | 3540 | 10 | 50 | 3540 | N/A | N/A |

## 5.150 DC\_2-29\_n77

### 5.150.1 Configurations for DC

Table 5.150.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_2A-29A\_n77A | DC\_2A\_n77A |

### 5.150.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback mode, DC\_2A\_n77A. It can be seen that:

- There are no IMD products produced by Band 2 and n77 that might fall in Rx of band 29.

Although DC\_29\_n77 is not defined, 5th order harmonic mixing is produced from band n77 UL that might fall in Rx of band 29.

### 5.150.3 ∆TIB and ∆RIB values

For DC\_2-29\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below. The values are proposed to be reused from the values for CA\_n2-n12-n77 with the exception that ΔTIB,c would not be applicable for band 29.

Table 5.150.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-29\_n77 | 2 | 0.6 |
| n77 | 0.8 |

Table 5.150.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-29\_n77 | 2 | 0.2 |
| 29 | 0.2 |
| n77 | 0.5 |

### 5.150.4 Reference sensitivity exceptions

DC\_2-29\_n77 5th order harmonic mixing impact to band 29 can be derived from DC\_12-n77 values.

Table 5.150.4-1: Reference sensitivity exceptions (MSD) due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n77zz | 292 | 31 | 28 |  |  |  |  |  |  |  |  |  |
| NOTE 2: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that  with  the DL carrier frequency in the lower band and the UL carrier frequency in the higher band, both in MHz.  NOTE ZZ: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | | | | | | |

Table 5.150.4-2: Uplink configuration for reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / SCS / Channel bandwidth of the affected DL band / UL RB allocation of the aggressor band | | | | | | | | | | | | | |
| UL band | DL band | SCS of UL band  (kHz) | 5 MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n77 | 29 | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |

## 5.151 DC\_2-30\_n77

### 5.151.1 Configurations for DC

Table 5.151.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_2A-30A\_n77A | DC\_2A\_n77A  DC\_30A\_n77A |

### 5.151.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD4 and IMD5 products are produced by Band 2 and n77 that might fall in Rx of band 30.

- IMD4 products are produced by Band 30 and n77 that might fall in Rx of band 2.

### 5.151.3 ∆TIB and ∆RIB values

For DC\_2-30\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n2-n30-n77.

Table 5.151.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-30\_n77 | 2 | 0.6 |
| 30 | 0.3 |
| n77 | 0.8 |

Table 5.151.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-30\_n77 | 2 | 0.2 |
| 30 | 0 |
| n77 | 0.5 |

### 5.151.4 Reference sensitivity exceptions

Table 5.151.4-1 shows the required MSD levels for the DC configuration. The required MSD values for IMD4 are derived from CA-n2A-n30A-n77A. The required MSD value for IMD5 is derived from DC\_2A-7A\_n77A.

Table 5.151.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-30A\_n77A | 2 | 1906 | 5 | 25 | 1986 | 8.6 | IMD411 |
| 30 | 2312 | 5 | 25 | 2357 | N/A | N/A |
| n77 | 3305 | 10 | 50 | 3305 | N/A | N/A |
| 2 | 1905 | 5 | 25 | 1985 | N/A | N/A |
| 30 | 2309 | 5 | 25 | 2354 | 10.6 | IMD411 |
| n77 | 3361 | 10 | 50 | 3361 | N/A | N/A |
| 2 | 1860 | 5 | 25 | 1940 | N/A | N/A |
| 30 | 2309 | 5 | 25 | 2354 | 3.4 | IMD5 |
| n77 | 3967 | 10 | 50 | 3967 | N/A | N/A |
| NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | |

## 5.152 DC\_5-30\_n77

### 5.152.1 Configurations for DC

Table 5.152.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_5A-30A\_n77A | DC\_5A\_n77A  DC\_30A\_n77A |

### 5.152.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD3 products are produced by Band 5 and n77 that might fall in Rx of band 30.

- IMD3 and IMD5 products are produced by Band 30 and n77 that might fall in Rx of band 5.

### 5.152.3 ∆TIB and ∆RIB values

For DC\_5-30\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n5-n30-n77.

Table 5.152.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-30\_n77 | 5 | 0.6 |
| 30 | 0.3 |
| n77 | 0.8 |

Table 5.152.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-30\_n77 | 5 | 0.2 |
| 30 | 0 |
| n77 | 0.5 |

### 5.152.4 Reference sensitivity exceptions

Table 5.152.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n5A-n30A-n77A.

Table 5.152.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_5A-30A\_n77A | 5 | 835 | 5 | 25 | 880 | 15.2 | IMD34 |
| 30 | 2310 | 5 | 25 | 2355 | N/A | N/A |
| n77 | 3740 | 10 | 50 | 3740 | N/A | N/A |
| 5 | 835 | 5 | 25 | 880 | N/A | N/A |
| 30 | 2310 | 5 | 25 | 2355 | 13.2 | IMD311 |
| n77 | 4025 | 10 | 50 | 4025 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified.  NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | |

## 5.153 DC\_12-30\_n77

### 5.153.1 Configurations for DC

Table 5.153.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_12A-30A\_n77A | DC\_12A\_n77A  DC\_30A\_n77A |

### 5.153.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD3 products are produced by Band 12 and n77 that might fall in Rx of band 30.

- IMD3 and IMD5 products are produced by Band 30 and n77 might fall in Rx of band 12.

### 5.153.3 ∆TIB and ∆RIB values

For DC\_12-30\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n12-n30-n77.

Table 5.153.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_12-30\_n77 | 12 | 0.5 |
| 30 | 0.3 |
| n77 | 0.5 |

Table 5.153.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_12-30\_n77 | 12 | 0.2 |
| 30 | 0 |
| n77 | 0.5 |

### 5.153.4 Reference sensitivity exceptions

Table 5.153.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n12A-n30A-n77A.

Table 5.153.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_12A-30A\_n77A | 12 | 710 | 5 | 25 | 740 | 15.2 | IMD34 |
| 30 | 2310 | 5 | 25 | 2355 | N/A | N/A |
| n77 | 3880 | 10 | 50 | 3880 | N/A | N/A |
| 12 | 707.5 | 5 | 25 | 737.5 | N/A | N/A |
| 30 | 2310 | 5 | 25 | 2355 | 13.2 | IMD3 |
| n77 | 3770 | 10 | 50 | 3770 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. | | | | | | | |

## 5.154 DC\_12-66\_n77

### 5.154.1 Configurations for DC

Table 5.154.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_12A-66A\_n77A | DC\_12A\_n77A  DC\_66A\_n77A |

### 5.154.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD3 products are produced by Band 12 and n77 that might fall in Rx of band 66.

- IMD3 products are produced by Band 66 and n77 that might fall in Rx of band 12.

### 5.154.3 ∆TIB and ∆RIB values

For DC\_12-66\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n12-n66-n77.

Table 5.154.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_12-66\_n77 | 12 | 0.8 |
| 66 | 0.6 |
| n77 | 0.8 |

Table 5.154.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_12-66\_n77 | 12 | 0.5 |
| 66 | 0.5 |
| n77 | 0.5 |

### 5.154.4 Reference sensitivity exceptions

Table 5.154.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n12A-n66A-n77A.

Table 5.154.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_12A-66A\_n77A | 12 | 710 | 5 | 25 | 740 | 15.2 | IMD311 |
| 66 | 1720 | 5 | 25 | 2120 | N/A | N/A |
| n77 | 4180 | 10 | 50 | 4180 | N/A | N/A |
| 12 | 707 | 5 | 25 | 737 | N/A | N/A |
| 66 | 1726 | 5 | 25 | 2126 | 13.2 | IMD3 |
| n77 | 3540 | 10 | 50 | 3540 | N/A | N/A |
| NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | |

## 5.155 DC\_14-30\_n77

### 5.155.1 Configurations for DC

Table 5.155.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_14A-30A\_n77A | DC\_14A\_n77A  DC\_30A\_n77A |

### 5.155.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD3 products are produced by Band 14 and n77 that might fall in Rx of band 30.

- IMD3 and IMD5 products are produced by Band 30 and n77 that might fall in Rx of band 14.

### 5.155.3 ∆TIB and ∆RIB values

For DC\_14-30\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n14-n30-n77.

Table 5.155.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_14-30\_n77 | 14 | 0.5 |
| 30 | 0.3 |
| n77 | 0.8 |

Table 5.155.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_14-30\_n77 | 14 | 0.2 |
| 30 | 0 |
| n77 | 0.5 |

### 5.155.4 Reference sensitivity exceptions

Table 5.155.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n14A-n30A-n77A.

Table 5.155.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_14A-30A\_n77A | 14 | 793 | 5 | 25 | 763 | 15.2 | IMD34 |
| 30 | 2310 | 5 | 25 | 2355 | N/A | N/A |
| n77 | 3857 | 10 | 50 | 3857 | N/A | N/A |
| 14 | 793 | 5 | 25 | 763 | N/A | N/A |
| 30 | 2310 | 5 | 25 | 2355 | 13.2 | IMD3 |
| n77 | 3941 | 10 | 50 | 3941 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. | | | | | | | |

## 5.156 DC\_14-66\_n77

### 5.156.1 Configurations for DC

Table 5.156.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_14A-66A\_n77A | DC\_14A\_n77A  DC\_66A\_n77A |

### 5.156.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD3 products are produced by Band 14 and n77 that might fall in Rx of band 66.

- IMD3 products are produced by Band 66 and n77 that might fall in Rx of band 14.

### 5.156.3 ∆TIB and ∆RIB values

For DC\_14-66\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n14-n66-n77.

Table 5.156.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_14-66\_n77 | 14 | 0.6 |
| 66 | 0.6 |
| n77 | 0.8 |

Table 5.156.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_14-66\_n77 | 14 | 0.2 |
| 66 | 0.5 |
| n77 | 0.5 |

### 5.156.4 Reference sensitivity exceptions

Table 5.156.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n14A-n66A-n77A.

Table 5.156.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_14A-66A\_n77A | 14 | 793 | 5 | 25 | 763 | 15.2 | IMD311 |
| 66 | 1712.5 | 5 | 25 | 2112.5 | N/A | N/A |
| n77 | 4188 | 10 | 50 | 4188 | N/A | N/A |
| 14 | 793 | 5 | 25 | 763 | N/A | N/A |
| 66 | 1755 | 5 | 25 | 2155 | 13.2 | IMD3 |
| n77 | 3741 | 10 | 50 | 3741 | N/A | N/A |
| NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | |

## 5.157 DC\_29-30\_n77

### 5.157.1 Configurations for DC

Table 5.157.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_29A-30A\_n77A | DC\_30A\_n77A |

### 5.157.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD3 and IMD5 products are produced by Band 30 and n77 that might fall in Rx of band 29.

Although DC\_29\_n77 is not defined, 5th order harmonic mixing is produced from band n77 UL that might fall in Rx of band 29.

### 5.157.3 ∆TIB and ∆RIB values

For DC\_29-30\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below. The values are proposed to be reused from the values for CA\_n12-n30-n77 with the exception that ΔTIB,c would not be applicable for band 29.

Table 5.157.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_29-30\_n77 | 30 | 0.3 |
| n77 | 0.5 |

Table 5.157.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_29-30\_n77 | 29 | 0.2 |
| 30 | 0 |
| n77 | 0.5 |

### 5.157.4 Reference sensitivity exceptions

Table 5.157.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n12A-n30A-n77A.

Table 5.157.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_29A-30A\_n77A | 29 | N/A | 5 | N/A | 722 | 15.2 | IMD34 |
| 30 | 2310 | 5 | 25 | 2355 | N/A | N/A |
| n77 | 3898 | 10 | 50 | 3898 | N/A | N/A |
| NOTE 4: This band is subject to IMD5 also which MSD is not specified. | | | | | | | |

DC\_29-30\_n77 5th order harmonic mixing impact to band 29 can be derived from DC\_12-n77 values.

Table 5.157.4-2: Reference sensitivity exceptions (MSD) due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n77ZZ | 292 | 31 | 28 |  |  |  |  |  |  |  |  |  |
| NOTE 2: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that  with  the DL carrier frequency in the lower band and the UL carrier frequency in the higher band, both in MHz.  NOTE ZZ: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | | | | | | |

Table 5.157.4-3: Uplink configuration for reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / SCS / Channel bandwidth of the affected DL band / UL RB allocation of the aggressor band | | | | | | | | | | | | | |
| UL band | DL band | SCS of UL band  (kHz) | 5 MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n77 | 29 | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |

## 5.158 DC\_29-66\_n77

### 5.158.1 Configurations for DC

Table 5.158.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_29A-66A\_n77A | DC\_66A\_n77A |

### 5.158.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD3 products are produced by Band 66 and n77 that might fall in Rx of band 29.

Although DC\_29\_n77 is not defined, 5th order harmonic mixing is produced from band n77 UL that might fall in Rx of band 29.

### 5.158.3 ∆TIB and ∆RIB values

For DC\_29-66\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below. The values are proposed to be reused from the values for CA\_n12-n66-n77 with the exception that ΔTIB,c would not be applicable for band 29.

Table 5.158.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_29-66\_n77 | 66 | 0.6 |
| n77 | 0.8 |

Table 5.158.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_29-66\_n77 | 29 | 0.5 |
| 66 | 0.5 |
| n77 | 0.5 |

### 5.158.4 Reference sensitivity exceptions

Table 5.158.4-1 shows the required MSD levels for the DC configuration. The required MSD values are derived from CA-n12A-n66A-n77A.

Table 5.158.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_29A-66A\_n77A | 29 | N/A | 5 | N/A | 722 | 15.2 | IMD311 |
| 66 | 1734 | 5 | 25 | 2134 | N/A | N/A |
| n77 | 4190 | 10 | 50 | 4190 | N/A | N/A |
| NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | |

DC\_29-66\_n77 5th order harmonic mixing impact to band 29 can be derived from DC\_12-n77 values.

Table 5.158.4-2: Reference sensitivity exceptions (MSD) due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | |
| UL band | DL band | 5  MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n77ZZ | 292 | 31 | 28 |  |  |  |  |  |  |  |  |  |
| NOTE 2: The requirements should be verified for DL EARFCN of the victim (lower) band (superscript LB) such that  with  the DL carrier frequency in the lower band and the UL carrier frequency in the higher band, both in MHz.  NOTE ZZ: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | | | | | | |

Table 5.158.4-3: Uplink configuration for reference sensitivity exceptions due to receiver harmonic mixing for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / SCS / Channel bandwidth of the affected DL band / UL RB allocation of the aggressor band | | | | | | | | | | | | | |
| UL band | DL band | SCS of UL band  (kHz) | 5 MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n77 | 29 | 15 | 25 | 50 |  |  |  |  |  |  |  |  |  |

## 5.159 DC\_30-66\_n77

### 5.159.1 Configurations for DC

Table 5.159.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_30A-66A\_n77A | DC\_30A\_n77A  DC\_66A\_n77A |

### 5.159.2 Co-existence studies

Co-existence studies of this 3DL/2UL DC configuration are already covered in the constituent fallback modes. It can be seen that:

- IMD4 products are produced by Band 30 and n77 that might fall in Rx of band 66.

- IMD2 and IMD5 products are produced by Band 66 and n77 that might fall in Rx of band 30.

### 5.159.3 ∆TIB and ∆RIB values

For DC\_30-66\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below that reused the values for CA\_n30-n66-n77.

Table 5.159.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_30-66\_n77 | 30 | 0.3 |
| 66 | 0.6 |
| n77 | 0.8 |

Table 5.159.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_30-66\_n77 | 30 | 0.5 |
| 66 | 0.4 |
| n77 | 0.5 |

### 5.159.4 Reference sensitivity exceptions

Table 5.159.4-1 shows the required MSD levels for the DC configuration. The required MSD values for IMD2 and IMD4 are derived from CA-n30A-n66A-n77A. The required MSD value for IMD5 is derived from DC\_2A-7A\_n77A

Table 5.159.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA and NR Band / Channel bandwidth / NRB / MSD | | | | | | | |
| EN-DC  Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_30A-66A\_n77A | 30 | 2310 | 5 | 25 | 2355 | 29.2 | IMD211 |
| 66 | 1745 | 5 | 25 | 2145 | N/A | N/A |
| n77 | 4100 | 10 | 50 | 4100 | N/A | N/A |
| 30 | 2310 | 5 | 25 | 2355 | 3.4 | IMD5 |
| 66 | 1735 | 5 | 25 | 2135 | N/A | N/A |
| n77 | 3780 | 10 | 50 | 3780 | N/A | N/A |
| 30 | 2310 | 5 | 25 | 2355 | N/A | N/A |
| 66 | 1760 | 5 | 25 | 2160 | 8.7 | IMD411 |
| n77 | 3390 | 10 | 50 | 3390 | N/A | N/A |
| NOTE 11: The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | |

## 5.160 DC\_2-5\_n30

5.160.1 Operating bands for DC

Table 5.160.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-5A\_n30A  DC\_2A-2A-5A\_n30A | DC\_2A\_n30A  DC\_5A\_n30A |

### 5.160.2 Co-existence studies

For UE coexistence study of Band 2 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.160.2-1.

**Table 5.160.2-1: Harmonic and IMD analysis for DC\_2\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1910 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3820 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5730 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 395 | 465 | 4155 | 4225 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1385 | 1515 | 2700 | 2780 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 6005 | 6135 | 6460 | 6540 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 3235 | 3425 | 5005 | 5095 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7855 | 8045 | 8765 | 8855 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 930 | 790 | 8310 | 8450 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7410 | 7310 | 5335 | 5085 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 11070 | 11170 | 9705 | 9955 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3245 | 3095 | 1120 | 920 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10615 | 10765 | 10160 | 10360 |

For UE coexistence study of Band 5 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.160.2-2.

**Table 5.160.2-2: Harmonic and IMD analysis for DC\_5\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 824 | 849 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 1648 | 1698 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 2472 | 2547 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1456 | 1491 | 3129 | 3164 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 667 | 607 | 3761 | 3806 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 3953 | 4013 | 5434 | 5479 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 157 | 242 | 6066 | 6121 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 4777 | 4862 | 7739 | 7794 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 2982 | 2912 | 6258 | 6328 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 8436 | 8371 | 1091 | 981 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10044 | 10109 | 5601 | 5711 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 5297 | 5217 | 2063 | 2158 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 8563 | 8643 | 7082 | 7177 |

Based on co-existence study as presented in the table 5.160.2-1 and 5.160.2-2, the 4th order IMD of dual uplink 2+n30 may falls into the own Rx band of n5.

### 5.160.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_2-5-30.

Table 5.160.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-5\_n30  DC\_2-2-5\_n30 | 2 | 0.5 |
| 5 | 0.3 |
| n30 | 0.3 |

**Table 5.160.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-5\_n30  DC\_2-2-5\_n30 | 2 | 0.4 |
| 5 | 0 |
| n30 | 0.5 |

### 5.160.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the IMD4 for 2+n30 falling into band 5. This issue is similar to CA\_n2-n5-n30 and the same MSD is reused.

Table 5.160.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-5A\_n30A | 2 | 1870 | 5 | 25 | 1959 | N/A | N/A |
| 5 | 835 | 5 | 25 | 880 | 9.7 | IMD4 |
| n30 | 2310 | 10 | 50 | 2355 | N/A | N/A |

## 5.161 DC\_2-12\_n30

5.161.1 Operating bands for DC

Table 5.161.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-12A\_n30A  DC\_2A-2A-12A\_n30A | DC\_2A\_n30A  DC\_12A\_n30A |

### 5.161.2 Co-existence studies

For UE coexistence study of Band 2 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.161.2-1.

**Table 5.161.2-1: Harmonic and IMD analysis for DC\_2\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1910 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3820 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5730 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 395 | 465 | 4155 | 4225 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1385 | 1515 | 2700 | 2780 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 6005 | 6135 | 6460 | 6540 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 3235 | 3425 | 5005 | 5095 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7855 | 8045 | 8765 | 8855 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 930 | 790 | 8310 | 8450 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7410 | 7310 | 5335 | 5085 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 11070 | 11170 | 9705 | 9955 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3245 | 3095 | 1120 | 920 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10615 | 10765 | 10160 | 10360 |

For UE coexistence study of Band 12 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.161.2-2.

**Table 5.161.2-2: Harmonic and IMD analysis for DC\_12\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 699 | 716 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 1398 | 1432 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 2097 | 2148 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1589 | 1616 | 3004 | 3031 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 917 | 873 | 3894 | 3931 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 3703 | 3747 | 5309 | 5346 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 218 | 157 | 6199 | 6246 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 4402 | 4463 | 7614 | 7661 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 3232 | 3178 | 6008 | 6062 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 8561 | 8504 | 559 | 481 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 9919 | 9976 | 5101 | 5179 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 5547 | 5483 | 2462 | 2533 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 8313 | 8377 | 6707 | 6778 |

Based on co-existence study as presented in the table 5.161.2-1 and 5.161.2-2, no harmonic or IMD issue is identified.

### 5.161.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_2-12-30.

Table 5.161.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-12\_n30  DC\_2-2-12\_n30 | 2 | 0.5 |
| 12 | 0.3 |
| n30 | 0.3 |

**Table 5.161.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-12\_n30  DC\_2-2-12\_n30 | 2 | 0.4 |
| 12 | 0 |
| n30 | 0.5 |

### 5.161.4 Reference sensitivity exceptions

No Refsens exception is identified.

## 5.162 DC\_2-14\_n30

5.162.1 Operating bands for DC

Table 5.162.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-14A\_n30A  DC\_2A-2A-14A\_n30A | DC\_2A\_n30A  DC\_14A\_n30A |

### 5.162.2 Co-existence studies

For UE coexistence study of Band 2 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.162.2-1.

**Table 5.162.2-1: Harmonic and IMD analysis for DC\_2\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1910 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3820 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5730 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 395 | 465 | 4155 | 4225 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1385 | 1515 | 2700 | 2780 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 6005 | 6135 | 6460 | 6540 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 3235 | 3425 | 5005 | 5095 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7855 | 8045 | 8765 | 8855 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 930 | 790 | 8310 | 8450 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7410 | 7310 | 5335 | 5085 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 11070 | 11170 | 9705 | 9955 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3245 | 3095 | 1120 | 920 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10615 | 10765 | 10160 | 10360 |

For UE coexistence study of Band 14 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.162.2-2.

**Table 5.162.2-2: Harmonic and IMD analysis for DC\_14\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 788 | 798 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 1576 | 1596 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 2364 | 2394 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1507 | 1527 | 3093 | 3113 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 739 | 709 | 3812 | 3842 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 3881 | 3911 | 5398 | 5428 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 49 | 89 | 6117 | 6157 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 4669 | 4709 | 7703 | 7743 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 3054 | 3014 | 6186 | 6226 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 8472 | 8422 | 887 | 837 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10008 | 10058 | 5457 | 5507 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 5369 | 5319 | 2216 | 2266 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 8491 | 8541 | 6974 | 7024 |

Based on co-existence study as presented in the table 5.162.2-1 and 5.162.2-2, own Rx impact is not identified.

### 5.162.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_2-14-30.

Table 5.162.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-14\_n30  DC\_2-2-14\_n30 | 2 | 0.5 |
| 14 | 0.3 |
| n30 | 0.5 |

**Table 5.162.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-14\_n30  DC\_2-2-14\_n30 | 2 | 0.3 |
| 14 | 0 |
| n30 | 0.3 |

### 5.162.4 Reference sensitivity exceptions

There is no exception due to no harmonic or IMD issue.

## 5.163 DC\_2-29\_n30

5.163.1 Operating bands for DC

Table 5.163.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-29A\_n30A  DC\_2A-2A-29A\_n30A | DC\_2A\_n30A |

### 5.163.2 Co-existence studies

For UE coexistence study of Band 2 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.163.2-1.

**Table 5.163.2-1: Harmonic and IMD analysis for DC\_2\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1910 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3820 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5730 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 395 | 465 | 4155 | 4225 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1385 | 1515 | 2700 | 2780 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 6005 | 6135 | 6460 | 6540 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 3235 | 3425 | 5005 | 5095 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7855 | 8045 | 8765 | 8855 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 930 | 790 | 8310 | 8450 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7410 | 7310 | 5335 | 5085 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 11070 | 11170 | 9705 | 9955 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3245 | 3095 | 1120 | 920 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10615 | 10765 | 10160 | 10360 |

Based on co-existence study as presented in the table 5.163.2-1 and 5.163.2-2, own Rx impact is not identified.

### 5.163.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_2-29-30.

Table 5.163.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-29\_n30  DC\_2-2-29\_n30 | 2 | 0.5 |
| n30 | 0.3 |

**Table 5.163.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-29\_n30  DC\_2-2-29\_n30 | 2 | 0.3 |
| 29 | 0 |
| n30 | 0.3 |

### 5.163.4 Reference sensitivity exceptions

There is no exception due to no harmonic or IMD issue.

## 5.164 DC\_2-66\_n30

5.164.1 Operating bands for DC

Table 5.164.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_2A-66A\_n30A  DC\_2A-2A-66A\_n30A  DC\_2A-66A-66A\_n30A  DC\_2A-2A-66A-66A\_n30A | DC\_2A\_n30A  DC\_66A\_n30A |

### 5.164.2 Co-existence studies

For UE coexistence study of Band 2 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.164.2-1.

**Table 5.164.2-1: Harmonic and IMD analysis for DC\_2\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1850 | 1910 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3700 | 3820 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5550 | 5730 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 395 | 465 | 4155 | 4225 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1385 | 1515 | 2700 | 2780 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 6005 | 6135 | 6460 | 6540 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 3235 | 3425 | 5005 | 5095 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7855 | 8045 | 8765 | 8855 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 930 | 790 | 8310 | 8450 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7410 | 7310 | 5335 | 5085 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 11070 | 11170 | 9705 | 9955 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3245 | 3095 | 1120 | 920 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10615 | 10765 | 10160 | 10360 |

For UE coexistence study of Band 66 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.164.2-2.

**Table 5.164.2-2: Harmonic and IMD analysis for DC\_66\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1710 | 1780 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3420 | 3560 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5130 | 5340 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 525 | 605 | 4015 | 4095 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1105 | 1255 | 2830 | 2920 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 5725 | 5875 | 6320 | 6410 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 2815 | 3035 | 5135 | 5235 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7435 | 7655 | 8625 | 8725 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 1210 | 1050 | 8030 | 8190 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7550 | 7440 | 4815 | 4525 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10930 | 11040 | 9145 | 9435 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3525 | 3355 | 730 | 500 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10335 | 10505 | 9740 | 9970 |

Based on co-existence study as presented in the table 5.164.2-1 and 5.164.2-2, own Rx impact is not identified.

### 5.164.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_2-30-66.

Table 5.164.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-66\_n30  DC\_2-2-66\_n30  DC\_2-66-66\_n30  DC\_2-2-66-66\_n30 | 2 | 0.5 |
| 66 | 0.5 |
| n30 | 0.3 |

**Table 5.164.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-66\_n30  DC\_2-2-66\_n30  DC\_2-66-66\_n30  DC\_2-2-66-66\_n30 | 2 | 0.4 |
| 66 | 0.4 |
| n30 | 0.5 |

### 5.164.4 Reference sensitivity exceptions

There is no exception due to no harmonic or IMD issue.

## 5.165 DC\_5-66\_n30

5.165.1 Operating bands for DC

Table 5.165.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_5A-66A\_n30A  DC\_5A-66A-66A\_n30A | DC\_5A\_n30A  DC\_66A\_n30A |

### 5.165.2 Co-existence studies

For UE coexistence study of Band 5 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.165.2-1.

**Table 5.165.2-1: Harmonic and IMD analysis for DC\_5\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 824 | 849 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 1648 | 1698 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 2472 | 2547 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1456 | 1491 | 3129 | 3164 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 667 | 607 | 3761 | 3806 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 3953 | 4013 | 5434 | 5479 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 157 | 242 | 6066 | 6121 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 4777 | 4862 | 7739 | 7794 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 2982 | 2912 | 6258 | 6328 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 8436 | 8371 | 1091 | 981 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10044 | 10109 | 5601 | 5711 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 5297 | 5217 | 2063 | 2158 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 8563 | 8643 | 7082 | 7177 |

For UE coexistence study of Band 66 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.165.2-2.

**Table 5.165.2-2: Harmonic and IMD analysis for DC\_66\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1710 | 1780 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3420 | 3560 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5130 | 5340 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 525 | 605 | 4015 | 4095 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1105 | 1255 | 2830 | 2920 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 5725 | 5875 | 6320 | 6410 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 2815 | 3035 | 5135 | 5235 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7435 | 7655 | 8625 | 8725 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 1210 | 1050 | 8030 | 8190 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7550 | 7440 | 4815 | 4525 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10930 | 11040 | 9145 | 9435 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3525 | 3355 | 730 | 500 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10335 | 10505 | 9740 | 9970 |

Based on co-existence study as presented in the table 5.165.2-1 and 5.165.2-2, the 5th order IMD of dual uplink 5+n30 may fall into own Rx of band 66.

### 5.165.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_5-30-66.

Table 5.165.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-66\_n30  DC\_5-66-66\_n30 | 5 | 0.3 |
| 66 | 0.5 |
| n30 | 0.3 |

**Table 5.165.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-66\_n30  DC\_5-66-66\_n30 | 5 | 0 |
| 66 | 0.4 |
| n30 | 0.5 |

### 5.165.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the IMD5 for 5+n30 falling into band 66. This issue is similar to CA\_n5-n30-n66 and the same MSD is reused.

Table 5.165.4-1: MSD test points due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_5A-66A\_n30A | 5 | 830 | 5 | 25 | 875 | N/A | N/A |
| 66 | 1725 | 5 | 25 | 2125 | 4 | IMD5 |
| n30 | 2307.5 | 5 | 50 | 2352.5 | N/A | N/A |

## 5.166 DC\_12-66\_n30

5.166.1 Operating bands for DC

Table 5.166.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_12A-66A\_n30A  DC\_12A-66A-66A\_n30A | DC\_12A\_n30A  DC\_66A\_n30A |

### 5.166.2 Co-existence studies

For UE coexistence study of Band 12 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.166.2-1.

**Table 5.166.2-1: Harmonic and IMD analysis for DC\_12\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 699 | 716 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 1398 | 1432 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 2097 | 2148 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1589 | 1616 | 3004 | 3031 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 917 | 873 | 3894 | 3931 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 3703 | 3747 | 5309 | 5346 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 218 | 157 | 6199 | 6246 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 4402 | 4463 | 7614 | 7661 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 3232 | 3178 | 6008 | 6062 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 8561 | 8504 | 559 | 481 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 9919 | 9976 | 5101 | 5179 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 5547 | 5483 | 2462 | 2533 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 8313 | 8377 | 6707 | 6778 |

For UE coexistence study of Band 66 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.166.2-2.

**Table 5.166.2-2: Harmonic and IMD analysis for DC\_66\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1710 | 1780 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3420 | 3560 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5130 | 5340 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 525 | 605 | 4015 | 4095 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1105 | 1255 | 2830 | 2920 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 5725 | 5875 | 6320 | 6410 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 2815 | 3035 | 5135 | 5235 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7435 | 7655 | 8625 | 8725 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 1210 | 1050 | 8030 | 8190 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7550 | 7440 | 4815 | 4525 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10930 | 11040 | 9145 | 9435 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3525 | 3355 | 730 | 500 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10335 | 10505 | 9740 | 9970 |

Based on co-existence study as presented in the table 5.166.2-1 and 5.166.2-2, the third order harmonic may fall into own Rx band 66.

### 5.166.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_12-30-66.

Table 5.166.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_12-66\_n30  DC\_12-66-66\_n30 | 12 | 0.8 |
| 66 | 0.5 |
| n30 | 0.3 |

**Table 5.166.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_12-66\_n30  DC\_12-66-66\_n30 | 12 | 0.5 |
| 66 | 0.4 |
| n30 | 0.5 |

### 5.166.4 Reference sensitivity exceptions

The MSD due to the harmonic issue is specified in 2DL/1UL CA/DC.

## 5.167 DC\_14-66\_n30

5.167.1 Operating bands for DC

Table 5.167.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_14A-66A\_n30A  DC\_14A-66A-66A\_n30A | DC\_14A\_n30A  DC\_66A\_n30A |

### 5.167.2 Co-existence studies

For UE coexistence study of Band 14 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.167.2-1.

**Table 5.167.2-1: Harmonic and IMD analysis for DC\_14\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 788 | 798 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 1576 | 1596 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 2364 | 2394 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 1507 | 1527 | 3093 | 3113 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 739 | 709 | 3812 | 3842 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 3881 | 3911 | 5398 | 5428 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 49 | 89 | 6117 | 6157 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 4669 | 4709 | 7703 | 7743 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 3054 | 3014 | 6186 | 6226 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 8472 | 8422 | 887 | 837 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10008 | 10058 | 5457 | 5507 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 5369 | 5319 | 2216 | 2266 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 8491 | 8541 | 6974 | 7024 |

For UE coexistence study of Band 66 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.167.2-2.

**Table 5.167.2-2: Harmonic and IMD analysis for DC\_66\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1710 | 1780 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3420 | 3560 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5130 | 5340 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 525 | 605 | 4015 | 4095 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1105 | 1255 | 2830 | 2920 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 5725 | 5875 | 6320 | 6410 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 2815 | 3035 | 5135 | 5235 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7435 | 7655 | 8625 | 8725 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 1210 | 1050 | 8030 | 8190 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7550 | 7440 | 4815 | 4525 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10930 | 11040 | 9145 | 9435 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3525 | 3355 | 730 | 500 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10335 | 10505 | 9740 | 9970 |

Based on co-existence study as presented in the table 5.167.2-1 and 5.167.2-2, no harmonic or IMD issue is identified.

### 5.167.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_14-30-66.

Table 5.167.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_14-66\_n30  DC\_14-66-66\_n30 | 14 | 0.3 |
| 66 | 0.5 |
| n30 | 0.3 |

**Table 5.167.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_14-66\_n30  DC\_14-66-66\_n30 | 14 | 0 |
| 66 | 0.4 |
| n30 | 0.5 |

### 5.167.4 Reference sensitivity exceptions

The MSD due to the harmonic issue is specified in 2DL/1UL CA/DC.

## 5.168 DC\_29-66\_n30

5.168.1 Operating bands for DC

Table 5.168.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_29A-66A\_n30A  DC\_29A-66A-66A\_n30A | DC\_66A\_n30A |

### 5.168.2 Co-existence studies

For UE coexistence study of Band 66 + Band n30, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.168.2-1.

**Table 5.168.2-1: Harmonic and IMD analysis for DC\_66\_n30**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| UE UL carriers | f1\_low | f1\_high | f2\_low | f2\_high |
| UL frequencies (MHz) | 1710 | 1780 | 2305 | 2315 |
| 2nd harmonic | 2\* f1\_low | 2\*f1\_high | 2\*f2\_low | 2\*f2\_high |
| harmonic frequency limit (MHz) | 3420 | 3560 | 4610 | 4630 |
| 3rd harmonic | 3\* f1\_low | 3\*f1\_high | 3\*f2\_low | 3\*f2\_high |
| harmonic frequency limit (MHz) | 5130 | 5340 | 6915 | 6945 |
| 2nd order IMD products | f2\_low – f1\_high | f2\_high – f1\_low | f2\_low + f1\_low | f2\_high + f1\_high |
| IMD frequency limit (MHz) | 525 | 605 | 4015 | 4095 |
| 3rd order IMD products | 2\*f1\_low – f2\_high | 2\*f1\_high – f2\_low | 2\*f2\_low – f1\_high | 2\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 1105 | 1255 | 2830 | 2920 |
| 3rd order IMD products | 2\*f1\_low + f2\_low | 2\*f1\_high + f2\_high | 2\*f2\_low + f1\_low | 2\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 5725 | 5875 | 6320 | 6410 |
| 4th order IMD products | 3\*f1\_low – f2\_high | 3\*f1\_high – f2\_low | 3\*f2\_low – f1\_high | 3\*f2\_high – f1\_low |
| IMD frequency limit (MHz) | 2815 | 3035 | 5135 | 5235 |
| 4th order IMD products | 3\*f1\_low + f2\_low | 3\*f1\_high + f2\_high | 3\*f2\_low + f1\_low | 3\*f2\_high + f1\_high |
| IMD frequency limit (MHz) | 7435 | 7655 | 8625 | 8725 |
| 4th order IMD products | 2\*f1\_low – 2\*f2\_high | 2\*f1\_high – 2\*f2\_low | 2\*f1\_low + 2\*f2\_low | 2\*f1\_high + 2\*f2\_high |
| IMD frequency limit (MHz) | 1210 | 1050 | 8030 | 8190 |
| 5th order IMD products | f1\_low – 4\*f2\_high | f1\_high – 4\*f2\_low | f2\_low – 4\*f1\_high | f2\_high – 4\*f1\_low |
| IMD frequency limit (MHz) | 7550 | 7440 | 4815 | 4525 |
| 5th order IMD products | f1\_low + 4\*f2\_low | f1\_high + 4\*f2\_high | f2\_low + 4\*f1\_low | f2\_high + 4\*f1\_high |
| IMD frequency limit (MHz) | 10930 | 11040 | 9145 | 9435 |
| 5th order IMD products | 2\*f1\_low – 3\*f2\_high | 2\*f1\_high - 3\*f2\_low | 2\*f2\_low – 3\*f1\_high | 2\*f2\_high – 3\*f1\_low |
| IMD frequency limit (MHz) | 3525 | 3355 | 730 | 500 |
| 5th order IMD products | 2\*f1\_low + 3\*f2\_low | 2\*f1\_high + 3\*f2\_high | 2\*f2\_low + 3\*f1\_low | 2\*f2\_high + 3\*f1\_high |
| IMD frequency limit (MHz) | 10335 | 10505 | 9740 | 9970 |

Based on co-existence study as presented in the table 5.168.2-1 and 5.168.2-2, the 5th order IMD of dual uplink 66+n30 may fall into own Rx band 29.

### 5.168.3 ∆TIB and ∆RIB values

The same relaxation values is reused from E-UTRA CA\_29-30-66.

Table 5.168.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_29-66\_n30  DC\_29-66-66\_n30 | 66 | 0.5 |
| n30 | 0.3 |

**Table 5.168.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_29-66\_n30  DC\_29-66-66\_n30 | 29 | 0 |
| 66 | 0.4 |
| n30 | 0.5 |

### 5.168.4 Reference sensitivity exceptions

The IMD issues specifc to 3DL/2UL is the IMD5 for 66+n30 falling into band 29. However, there is only a partial hit of IMD5 for this band combination. The MSDs due to IMD5 of two high bands into a low victim band are generally small (such as 1 dB for band 1+5+7, 3.5dB for band 1+7+26) so we propose that MSD is not specified for this band combination.

## 5.169 DC\_2-46\_n2

5.169.1 Configurations for DC

**Table 5.169.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_2A-46A\_n2A3  DC\_2A-46C\_n2A3  DC\_2A-46D\_n2A3  DC\_2A-46E\_n2A3 | DC\_2A\_n2A2 |
| NOTE 2: Only single switched UL is supported  NOTE 3: Restricted to E-UTRA operation when inter-band carrier aggregation is configured. The downlink operating band for Band 46 is paired with the uplink operating band (external E-UTRA band) of the carrier aggregation configuration that is supporting the configured Pcell. | |

5.169.2 Co-existence studies

For UL DC\_2A\_n2A, there is no need to study IMD for only single switch UL is supported.

3rd harmonic of n2 UL falls into b46 DL.

5.169.3 ∆TIB and ∆RIB values

For DC\_2-46\_n2, the ΔTIB,c and ΔRIB,c values are reused from CA\_2-46 shown below.

**Table 5.169.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-46\_n2 | 2 | 0 |
| 46 | 0 |
| n2 | 0 |

**Table 5.169.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-46\_n2 | 2 | 0 |
| 46 | 0 |
| n2 | 0 |

5.169.4 REFSENS requirements

Based on 5.169.2 discussion above, REFSENS exceptions are specified below.(A new table below is introduced and could be number as **Table 7.3B.2.3.1-6** in TS38.101-3 )

**Table 5.169.4-1: Reference sensitivity QPSK PREFSENS (EN-DC with b46)**

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD** | | | | | | | | | | | | |
| **UL band** | **DL band** | **5**  **MHz**  **(dB)** | **10 MHz**  **(dB)** | **15 MHz**  **(dB)** | **20 MHz**  **(dB)** | **25 MHz**  **(dB)** | **40 MHz**  **(dB)** | **50 MHz**  **(dB)** | **60 MHz**  **(dB)** | **80 MHz**  **(dB)** | **90 MHz**  **(dB)** | **100 MHz**  **(dB)** |
| n2 | 461 |  | N/A |  | N/A |  |  |  |  |  |  |  |
| NOTE 1: These requirements apply when there is at least one individual RE within the downlink (victim) transmission bandwidth which falls into the reference sensitivity exclusion region overlapping with UL harmonic zones | | | | | | | | | | | | |

## 5.170 DC\_2-48\_n2

5.170.1 Configurations for DC

**Table 5.170.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_2A-48A\_n2A  DC\_2A-48C\_n2A  DC\_2A-48D\_n2A  DC\_2A-48E\_n2A | DC\_2A\_n2A2 |
| NOTE 2: Only single switched UL is supported | |

5.170.2 Co-existence studies

For UL DC\_2A\_n2A, there is no need to study IMD for only single switch UL is supported.

5.170.3 ∆TIB and ∆RIB values

For DC\_2-48\_n2, the ΔTIB,c and ΔRIB,c values are reused from CA\_2-48 shown below.

**Table 5.170.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-48\_n2 | 2 | 0.6 |
| 48 | 0.8 |
| n2 | 0.6 |

**Table 5.170.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-48\_n2 | 2 | 0.2 |
| 48 | 0.5 |
| n2 | 0.2 |

5.170.4 REFSENS requirements

Based on 5.170.2 discussion above, REFSENS exceptions are not specified.

## 5.171 DC\_13-46\_n2

5.171.1 Configurations for DC

**Table 5.171.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_13A-46A\_n2A3 | DC\_13A\_n2A |
| NOTE 3: Restricted to E-UTRA operation when inter-band carrier aggregation is configured. The downlink operating band for Band 46 is paired with the uplink operating band (external E-UTRA band) of the carrier aggregation configuration that is supporting the configured Pcell. | |

5.171.2 Co-existence studies

Based on co-existence study of UL DC\_13A\_n2A, IMD4 of band 13 UL and n2 UL falls into own RX of band46.

3rd harmonic of n2 UL falls into b46 DL.

5.171.3 ∆TIB and ∆RIB values

For DC\_13-46\_n2, the ΔTIB,c and ΔRIB,c values reused from CA\_2-13-46 shown below.

**Table 5.171.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_13-46\_n2 | 13 | 0.3 |
| 46 | 0 |
| n2 | 0.3 |

**Table 5.171.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_13-46\_n2 | 13 | 0 |
| 46 | 0 |
| n2 | 0 |

5.171.4 REFSENS requirements

Based on 5.171.2 discussion above, REFSENS exceptions due to IMD are specified below, REFSENS exceptions due to harmonic are specified in R4-2112446 TP for DC\_2-46\_n2.

Table 5.171.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_13A-46A\_n2A5 | 13 | N/A | N/A | N/A | N/A | N/A | N/A |
| 46 | N/A | N/A | N/A | N/A | N/A | IMD4 |
| n2 | N/A | N/A | N/A | N/A | N/A | N/A |
| NOTE 5: When Band 46 have self-interference problems by dual uplink CA/EN-DC, then the requirements do not apply in exclusion zone which is frequency range within (harmonics frequency region + FHD) and IMD frequency region as follow.  IMD frequency range   |  |  |  |  | | --- | --- | --- | --- | | DL\_CA configuration | UL\_CA configuration | Exclusion zone center frequency | Exclusion zone BW | | DC\_2A-46A\_n66A | DC\_2A\_n66A | 2\*fc\_2A + fc\_n66A | 2\*BW\_2A + BW\_n66A | | DC\_2A-46A\_n66A | DC\_2A\_n66A | fc\_2A + 2\*fc\_n66A | BW\_2A + 2\*BW\_n66A | | DC\_2A-46A\_n77A | DC\_2A\_n77A | fc\_2A + fc\_n77A | BW\_2A + BW\_n77A | | DC\_2A-46A\_n77A | DC\_2A\_n77A | -fc\_2A + 2\*fc\_n77A | -BW\_2A + 2\*BW\_n77A | | DC\_13A-46A\_n2A | DC\_13A\_n2A | 2\*fc\_n2A + 2\*fc\_13A | 2\*BW\_n2A+2\*BW\_13A | | DC\_13A-46A\_n77A | DC\_13A\_n77A | 2\*fc\_13A + fc\_n77A | 2\*BW\_13A + BW\_n77A | | DC\_13A-46A\_n77A | DC\_13A\_n77A | 3\*fc\_13A + fc\_n77A | 3\*BW\_13A + BW\_n77A | | DC\_13A-46A\_n77A | DC\_13A\_n77A | -3\*fc\_13A + 2\*fc\_n77A | -3\*BW\_13A + 2\*BW\_n77A | | DC\_46A-66A\_n77A | DC\_66A\_n77A | fc\_66A + fc\_n77A | BW\_66A + BW\_n77A | | DC\_46A-66A\_n77A | DC\_66A\_n77A | -fc\_66A + 2\*fc\_n77A | -BW\_66A + 2\*BW\_n77A | | DC\_13A-46A\_n66A | DC\_13A\_n66A | 3\*fc\_13A + fc\_n66A | BW\_13A + 2\*BW\_n66A | | DC\_13A-46A\_n66A | DC\_13A\_n66A | 2\*fc\_13A + 3\*fc\_n66A | BW\_13A + 2\*BW\_n66A | | DC\_46-48A\_n66A | DC\_48A\_n66A | fc\_48A + fc\_n66A | BW\_48A + 2\*BW\_n66A | | DC\_46-48A\_n66A | DC\_48A\_n66A | 2\*fc\_48A + fc\_n66A | 2\*BW\_48A + BW\_n66A | | DC\_2A-46\_n5A | DC\_2A\_n5A | 2\*fc\_2A + 2\*fc\_n5A | BW\_2A + 2\*BW\_n5A | | DC\_2A-46\_n5A | DC\_2A\_n5A | fc\_2A + 4\*fc\_n5A | BW\_2\*2A + BW\_n5A | | DC\_46-48A\_n5A | DC\_48A\_n5A | 2\*fc\_48A + fc\_n5A | BW\_48A + 2\*BW\_n5A | | DC\_46-48A\_n5A | DC\_48A\_n5A | 2\*fc\_48A + 2\*fc\_n5A | BW\_2\*48A + BW\_n5A | | | | | | | | |

## 5.172 DC\_13-48\_n77

5.172.1 Configurations for DC

**Table 5.172.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_13A-48A\_n77A  DC\_13A-48A-48A\_n77A | DC\_13A\_n77A |

5.172.2 Co-existence studies

DC\_48\_n77 is not used alone, and no uplink inter-band EN-DC is specified for the configuration since the minimum requirements apply only when there is non-simultaneous Tx/Rx operation between E-UTRA B48 and NR n77 carriers (please refer to [Rev 2 of R4-2112654](https://urldefense.proofpoint.com/v2/url?u=https-3A__www.3gpp.org_ftp_tsg-5Fran_WG4-5FRadio_TSGR4-5F100-2De_Inbox_Drafts_-255B100-2De-255D-255B113-255D-2520NR-5FBaskets-5FPart-5F2_Round-25201_Rev-25202-2520R4-2D2112654-2520PC3-2520TP-2520for-2520TR-252037.717-2D11-2D11-2520for-2520DL-2520DC-5F48-5Fn77.docx&d=DwMGaQ&c=VYRDWu-sKuQrybEAJ2u-dYX_FK6X1lTrDf-PKXUa2P4&r=rpQpwfeegXayI5SMT1DB47efAybt3sLDy0PvL0L8ZLw&m=htocqblOkHAmpVEeLp_5lX3aNFI_SlxGCLP1fiGcktM&s=tlmRoCcKk1674gJCn4E95xlTL7X_kKeo6cCrjMEe548&e=)for DC\_48\_n77 this meeting). Thus no co-existence study is needed for TDD Band 48.

5.172.3 ∆TIB and ∆RIB values

For DC\_13-48\_n77, the ΔTIB,c and ΔRIB,c values are specified in the tables below, reusing DC\_13\_n77 values.

**Table 5.172.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_13-48\_n77 | 13 | 0.5 |
| 48 | 0.8 |
| n77 | 0.8 |

**Table 5.172.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_13-48\_n77 | 13 | 0.2 |
| 48 | 0.5 |
| n77 | 0.5 |

5.172.4 REFSENS requirements

Based on 5.172.2 discussion above, REFSENS exceptions are not expected.

## 5.173 DC\_48-66\_n2

5.173.1 Configurations for DC

**Table 5.173.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_48A-66A\_n2A  DC\_48C-66A\_n2A  DC\_48D-66A\_n2A  DC\_48E-66A\_n2A | DC\_66A\_n2A |

5.173.2 Co-existence studies

Based on the co-existence study of UL DC\_66A\_n2A, IMD2 of b66 UL and n2 UL falls into band 48 RX.

5.173.3 ∆TIB and ∆RIB values

For DC\_48-66\_n2, the ΔTIB,c and ΔRIB,c values are reused from DC\_2-48\_n66 shown below:

**Table 5.173.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_48-66\_n2 | 48 | 0.8 |
| 66 | 0.6 |
| n2 | 0.6 |

**Table 5.173.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_48-66\_n2 | 48 | 0.5 |
| 66 | 0.3 |
| n2 | 0.3 |

5.173.4 REFSENS requirements

Based on 5.173.2 discussion above, MSD values due to IMD are reused from DC\_2-48\_n66 shown below:

Table 5.173.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_48A-66A\_n2A  DC\_48C-66A\_n2A  DC\_48D-66A\_n2A  DC\_48E-66A\_n2A | n2 | 1880 | 5 | 25 | 1960 | N/A | N/A |
|  | 48 | 3620 | 10 | 50 | 3620 | 29.4 | IMD2 |
|  | 66 | 1740 | 5 | 25 | 2140 | N/A | N/A |

## 5.174 DC\_48-66\_n66

5.174.1 Configurations for DC

**Table 5.174.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_48A-66A\_n66A  DC\_48C-66A\_n66A  DC\_48D-66A\_n66A  DC\_48E-66A\_n66A | DC\_66A\_n66A2  DC\_48A\_n66A |
| NOTE 2: Only single switched UL is supported | |

5.174.2 Co-existence studies

For UL DC\_66A\_n66A, there is no need to study IMD for only single switch UL is supported.

For UL DC\_48A\_n66A, IMD5 of the 2UL falls into band 66 Rx.

5.174.3 ∆TIB and ∆RIB values

For DC\_48-66\_n66, the ΔTIB,c and ΔRIB,c values are specified in the tables below.

**Table 5.174.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_48-66\_n66 | 48 | 0.8 |
| 66 | 0.6 |
| n66 | 0.6 |

**Table 5.174.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_48-66\_n66 | 48 | 0.5 |
| 66 | 0.2 |
| n66 | 0.2 |

5.174.4 REFSENS requirements

Based on discussion on 5.174.2, Reference exception specifies below:

Table 5.174.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_48A-66A\_n66A  DC\_48C-66A\_n66A  DC\_48D-66A\_n66A  DC\_48E-66A\_n66A | 48 | 3660 | 20 | 100 | 3660 | N/A | N/A |
|  | 66 | 1775 | 5 | 25 | 2175 | 4.0 | IMD5 |
|  | n66 | 1715 | 5 | 25 | 2115 | N/A | N/A |

## 5.175 DC\_48-66\_n77

5.175.1 Configurations for DC

**Table 5.175.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_48A-66A\_n77A  DC\_48A-48A-66A\_n77A  DC\_48C-66A\_n77A  DC\_48D-66A\_n77A  DC\_48E-66A\_n77A | DC\_66A\_n77A |

5.175.2 Co-existence studiesDC\_48\_n77 is not used alone, and no uplink inter-band EN-DC is specified for the configuration since the minimum requirements apply only when there is non-simultaneous Tx/Rx operation between E-UTRA B48 and NR n77 carriers (please refer to [Rev 2 of R4-2112654](https://urldefense.proofpoint.com/v2/url?u=https-3A__www.3gpp.org_ftp_tsg-5Fran_WG4-5FRadio_TSGR4-5F100-2De_Inbox_Drafts_-255B100-2De-255D-255B113-255D-2520NR-5FBaskets-5FPart-5F2_Round-25201_Rev-25202-2520R4-2D2112654-2520PC3-2520TP-2520for-2520TR-252037.717-2D11-2D11-2520for-2520DL-2520DC-5F48-5Fn77.docx&d=DwMGaQ&c=VYRDWu-sKuQrybEAJ2u-dYX_FK6X1lTrDf-PKXUa2P4&r=rpQpwfeegXayI5SMT1DB47efAybt3sLDy0PvL0L8ZLw&m=htocqblOkHAmpVEeLp_5lX3aNFI_SlxGCLP1fiGcktM&s=tlmRoCcKk1674gJCn4E95xlTL7X_kKeo6cCrjMEe548&e=)for DC\_48\_n77 this meeting). Thus no co-existence study is needed for TDD Band 48.

5.175.3 ∆TIB and ∆RIB values

For DC\_48-66\_n77, the ΔTIB,c and ΔRIB,c values are specified in the tables below, reusing DC\_66\_n77 values.

**Table 5.175.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_48-66\_n77 | 48 | 0.8 |
| 66 | 0.6 |
| n77 | 0.8 |

**Table 5.175.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_48-66\_n77 | 48 | 0.5 |
| 66 | 0.2 |
| n77 | 0.5 |

5.175.4 REFSENS requirements

Based on 5.175.2 discussion above, REFSENS exceptions are not expected.

## 5.176 DC\_1-5\_n77

### 5.176.1 Configurations for DC

Table 5.176.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-5A\_n77A | DC\_1A\_n77A  DC\_5A\_n77A |
| DC\_1A-5A\_n77(2A) | DC\_1A\_n77A  DC\_5A\_n77A |

### 5.176.2 Co-existence studies

Based on co-existence studies of DC\_1\_n77 and DC\_5\_n77, own Rx impact of the 3rd band is the followings.

- 5th order IMD products generated by DC\_1\_n77 uplink may fall into own Rx of Band 5.

- 3rd order IMD products generated by DC\_5\_n77 uplink may fall into own Rx of Band 1.

- There was no additional IMD problem for non- contiguous DL CA operation by dual uplink transmission.

### 5.176.3 ∆TIB and ∆RIB values

For DC\_1-5\_n77, the ΔTIB,c and ΔRIB,c values are reused from DC\_1-5\_n78, and are given in the tables below.

Table 5.176.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-5\_n77 | B1 | 0.3 |
| B5 | 0.6 |
| n77 | 0.8 |

**Table 5.176.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-5\_n77 | B1 | 0.2 |
| B5 | 0.2 |
| n77 | 0.5 |

### 5.176.4 Reference sensitivity exceptions

For the DC\_1A-5A\_n77A and DC\_1A-5A\_n77(2A), RAN4 can reuse the MSD results of the DC\_1A-5A\_n78A. Hence, the proposed MSD test configuration and MSD requirements as follow.

**Table 5.176.4-1: MSD requirements**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_1A-5A\_n77A  DC\_1A-5A\_n77(2A) | 1 | 1932 | 5 | 25 | 2122 | 18.1 | IMD3 |
| 5 | 829 | 5 | 25 | 874 | N/A | N/A |
| n77 | 3780 | 10 | 50 | 3780 | N/A | N/A |
| 1 | 1975 | 5 | 25 | 2165 | N/A | N/A |
| 5 | 840 | 5 | 25 | 885 | 3.1 | IMD5 |
| n77 | 3405 | 10 | 50 | 3405 | N/A | N/A |

## 5.177 DC\_1-7\_n77

### 5.177.1 Configurations for DC

Table 5.177.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-7A\_n77A | DC\_1A\_n77A  DC\_7A\_n77A |
| DC\_1A-7A\_n77(2A) | DC\_1A\_n77A  DC\_7A\_n77A |
| DC\_1A-7A-7A-n77A | DC\_1A\_n77A  DC\_7A\_n77A |
| DC\_1A-7A-7A-n77(2A) | DC\_1A\_n77A  DC\_7A\_n77A |

### 5.177.2 Co-existence studies

Based on co-existence studies of DC\_1\_n77 and DC\_7\_n77, own Rx impact of the 3rd band is the followings.

- 4th & 5th order IMD products generated by DC\_1\_n77 uplink may fall into own Rx of Band 7.

- 4th order IMD products generated by DC\_7\_n77 uplink may fall into own Rx of Band 1.

- There was no additional IMD problem for non- contiguous DL CA operation by dual uplink transmission.

### 5.177.3 ∆TIB and ∆RIB values

For DC\_1-7\_n77, the ΔTIB,c and ΔRIB,c values are reused from DC\_1-7\_n78, and are given in the tables below.

Table 5.177.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-7\_n77 | B1 | 0.6 |
| B7 | 0.6 |
| n77 | 0.8 |

**Table 5.177.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-7\_n77 | B1 | 0.2 |
| B7 | 0.2 |
| n77 | 0.5 |

### 5.177.4 Reference sensitivity exceptions

For the DC\_1A-7A\_n77A, DC\_1A-7A\_n77(2A), DC\_1A-7A-7A\_n77A and DC\_1A-7A-7A\_n77(2A), RAN4 can reuse the MSD results of the DC\_1A-7A\_n78A. Hence, the proposed MSD test configuration and MSD requirements as follow.

**Table 5.177.4-1: MSD requirements**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_1A-7A\_n77A  DC\_1A-7A\_n77(2A)  DC\_1A-7A-7A\_n77A  DC\_1A-7A-7A\_n77(2A) | 1 | 1977.5 | 5 | 25 | 2167.5 | N/A | N/A |
| 7 | 2507.5 | 5 | 25 | 2627.5 | 9.1 | IMD41 |
| n77 | 3305 | 10 | 50 | 3305 | N/A | N/A |
| 1 | 1950 | 5 | 25 | 2140 | 8.7 | IMD4 |
| 7 | 2510 | 10 | 50 | 2630 | N/A | N/A |
| n77 | 3580 | 10 | 50 | 3580 | N/A | N/A |
| Note 1. The DC combinations is subject to IMD5 also which MSD is not specified. | | | | | | | |

## 5.178 DC\_3-5\_n77

### 5.178.1 Configurations for DC

Table 5.178.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-5A\_n77A | DC\_3A\_n77A  DC\_5A\_n77A |
| DC\_3A-5A\_n77(2A) | DC\_3A\_n77A  DC\_5A\_n77A |

### 5.178.2 Co-existence studies

Based on co-existence studies of DC\_3\_n77 and DC\_5\_n77, own Rx impact of the 3rd band is the followings.

- No IMD problems by DC\_3\_n77 uplink in the own Rx of Band 5.

- 3rd order IMD products generated by DC\_5\_n77 uplink may fall into own Rx of Band 3.

- There was no additional IMD problem for non- contiguous DL CA operation by dual uplink transmission.

### 5.178.3 ∆TIB and ∆RIB values

For DC\_3-5\_n77, the ΔTIB,c and ΔRIB,c values are reused from DC\_3-5\_n78, and are given in the tables below.

Table 5.178.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-5\_n77 | B3 | 0.6 |
| B5 | 0.6 |
| n77 | 0.8 |

**Table 5.178.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-5\_n77 | B3 | 0.2 |
| B5 | 0.2 |
| n77 | 0.5 |

### 5.178.4 Reference sensitivity exceptions

For the DC\_3A-5A\_n77A and DC\_3A-5A\_n77(2A), RAN4 can reuse the MSD results of the DC\_3A-20A\_n78A. Hence, the proposed MSD test configuration and MSD requirements as follow.

**Table 5.178.4-1: MSD requirements**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_3A-5A\_n77A  DC\_3A-5A\_n77(2A) | 3 | 1725 | 5 | 25 | 1820 | 17.3 | IMD3 |
| 5 | 845 | 5 | 25 | 804 | N/A | N/A |
| n77 | 3510 | 10 | 50 | 3510 | N/A | N/A |

## 5.179 DC\_3-7\_n77

### 5.179.1 Configurations for DC

Table 5.179.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-7A\_n77(2A) | DC\_3A\_n77A  DC\_7A\_n77A |
| DC\_3A-7A-7A\_n77(2A) | DC\_3A\_n77A  DC\_7A\_n77A |

### 5.179.2 Co-existence studies

Based on co-existence studies of DC\_3\_n77 and DC\_7\_n77, own Rx impact of the 3rd band is the followings.

- 5th order IMD products generaged by DC\_3\_n77 uplink may fall into own Rx of Band 7.

- 3rd & 4th order IMD products generated by DC\_7\_n77 uplink may fall into own Rx of Band 3.

- There was no additional IMD problem for non- contiguous DL CA operation by dual uplink transmission.

### 5.179.3 ∆TIB and ∆RIB values

For DC\_3-7\_n77, the ΔTIB,c and ΔRIB,c values are already specified in TS38.101-3 as follow.

Table 5.179.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-7\_n77 | B3 | 0.6 |
| B7 | 0.6 |
| n77 | 0.8 |

**Table 5.179.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-7\_n77 | B3 | 0.2 |
| B7 | 0.2 |
| n77 | 0.5 |

### 5.179.4 Reference sensitivity exceptions

For the DC\_3A-7A\_n77(2A) and DC\_3A-7A-7A\_n77(2A), RAN4 can reuse the MSD results of the DC\_3A-7A\_n77A. Hence, the proposed MSD test configuration and MSD requirements as follow.

**Table 5.179.4-1: MSD requirements**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order | |
| DC\_3A-7A\_n77(2A)  DC\_3A-7A-7A\_n77(2A) | 3 | 1725 | 5 | 25 | 1820 | 17.6 | IMD3 |
| 7 | 2565 | 5 | 25 | 2685 | N/A | N/A |
| n77 | 3310 | 10 | 50 | 3310 | N/A | N/A |
| 3 | 1725 | 5 | 25 | 1820 | 8.6 | IMD4 |
| 7 | 2565 | 5 | 25 | 2685 | N/A | N/A |
| n77 | 3475 | 10 | 50 | 3475 | N/A | N/A |
| 3 | 1715 | 5 | 25 | 1810 | N/A | N/A |
| 7 | 2550 | 5 | 25 | 2670 | 5.2 | IMD5 |
| n77 | 4190 | 10 | 50 | 4190 | N/A | N/A |
| 3 | 1720 | 5 | 25 | 1815 | N/A | N/A |
| 7 | 2520 | 5 | 25 | 2640 | 3.4 | IMD5 |
| n77 | 3900 | 10 | 50 | 3900 | N/A | N/A |

## 5.180 DC\_5-7\_n77

### 5.180.1 Configurations for DC

Table 5.180.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_5A-7A\_n77A | DC\_5A\_n77A  DC\_7A\_n77A |
| DC\_5A-7A\_n77(2A) | DC\_5A\_n77A  DC\_7A\_n77A |
| DC\_5A-7A-7A-n77A | DC\_5A\_n77A  DC\_7A\_n77A |
| DC\_5A-7A-7A-n77(2A) | DC\_5A\_n77A  DC\_7A\_n77A |

### 5.180.2 Co-existence studies

Based on co-existence studies of DC\_5\_n77 and DC\_7\_n77, own Rx impact of the 3rd band is the followings.

- 2nd order IMD products generated by DC\_5\_n77 uplink may fall into own Rx of Band 7.

- 2nd & 3rd order IMD products generated by DC\_7\_n77 uplink may fall into own Rx of Band 5.

- There was no additional IMD problem for non- contiguous DL CA operation by dual uplink transmission.

### 5.180.3 ∆TIB and ∆RIB values

For DC\_5-7\_n77, the ΔTIB,c and ΔRIB,c values are reused from DC\_5-7\_n78, and are given in the tables below.

Table 5.180.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-7\_n77 | B5 | 0.6 |
| B7 | 0.6 |
| n77 | 0.8 |

**Table 5.180.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-7\_n77 | B5 | 0.2 |
| B7 | 0.2 |
| n77 | 0.5 |

### 5.180.4 Reference sensitivity exceptions

For the DC\_5A-7A\_n77A, DC\_5A-7A\_n77(2A), DC\_5A-7A-7A\_n77A and DC\_5A-7A-7A\_n77(2A), RAN4 can reuse the MSD results of the DC\_5A-7A\_n78A. Hence, the proposed MSD test configuration and MSD requirements as follow.

**Table 5.180.4-1: MSD requirements**

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_5A-7A\_n77A  DC\_5A-7A\_n77(2A)  DC\_5A-7A-7A\_n77A  DC\_5A-7A-7A\_n77(2A) | 5 | 844 | 5 | 25 | 889 | N/A | N/A |
| 7 | 2525 | 5 | 25 | 2645 | 30.1 | IMD2 |
| n77 | 3489 | 10 | 50 | 3489 | N/A | N/A |
| 5 | 834 | 5 | 25 | 879 | 30.2 | IMD21 |
| 7 | 2550 | 5 | 25 | 2670 | N/A | N/A |
| n77 | 3429 | 10 | 50 | 3429 | N/A | N/A |
| Note 1. The DC combinations is subject to IMD3 also which MSD is not specified. | | | | | | | |

5.181 DC\_2\_(n)66

5.181.1 Operating bands for EN-DC

Table 5.181.1-1: Band combinations EN-DC (three bands)

| EN-DC band | E-UTRA CA band | NR band |
| --- | --- | --- |
| DC\_2-(n)66 | CA\_2-66 | n66 |

### 5.181.2 Configuration for DC

Table 5.181.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-(n)66AA | DC\_2A\_n66A | CA\_2A-66A | n66A |
| NOTE1: Only single switched UL is supported | | | |

5.181.3 Co-existence studies

Based on co-existence studies of CA\_n2-n66, the followings are concluded: .

- IMD3 generated by UL n66 might affect DL band 2.

- IMD5 generated by UL band 2 might affect DL n66.

5.181.4 ∆TIB and ∆RIB values

For DC\_2\_(n)66 the ΔTIB,c and ΔRIB,c values are derived from CA\_n2-n66 combination.

Table 5.181.4-1: ΔTIB,c

| E-UTRA and NR DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2\_(n)66 | 2 | 0.5 |
| 66 | 0.5 |
| n66 | 0.5 |

Table 5.181.4-2: ΔRIB,c

| E-UTRA and NR DC Configuration | E-UTRA and NR Band | ΔRIB,c [dB] |
| --- | --- | --- |
| DC\_2\_(n)66 | 2 | 0.3 |
| 66 | 0.3 |
| n66 | 0.3 |

5.181.5 REFSENS requirements

For DC\_2\_(n)66, REFSENS are reused from the CA\_n2-n66 and are given in the table below.

Table 5.3.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_2A-(n)66AA | 2 | 1855 | 5 | 25 | 1935 | 20 | IMD3 |
| n66 | 1775 | 5 | 25 | 2175 | N/A | N/A |
| 2 | 1883.3 | 5 | 25 | 1963.3 | N/A | N/A |
| n66 | 1750 | 5 | 25 | 2150 | 4 | IMD5 |

## 5.182 DC\_1-7\_n3

### 5.182.1 Configurations for DC

Table 5.182.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-7A\_n3A | DC\_1A\_n3A |

### 5.182.2 Co-existence studies

The co-existence studies of DC\_1\_n3 have already been captured in TR 37.716-11-11, where:

- No IMD produce caused by DC\_1\_n3 uplink may fall into own Rx of band 7.

### 5.182.3 ∆TIB and ∆RIB values

For DC\_1A-7A\_n3A, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.182.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-7\_n3 | 1 | 0.3 |
| 7 | 0.5 |
| n3 | 0.5 |

**Table 5.182.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-7\_n3 | 1 | 0 |
| 7 | 0 |
| n3 | 0 |

### 5.182.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.183 DC\_1-38\_n3

### 5.183.1 Configurations for DC

Table 5.183.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-38A\_n3A | DC\_1A\_n3A |

### 5.183.2 Co-existence studies

The co-existence studies of DC\_1\_n3 have already been captured in TR 37.716-11-11, where:

- No IMD produce caused by DC\_1\_n3 uplink may fall into own Rx of band 38.

### 5.183.3 ∆TIB and ∆RIB values

For DC\_1A-38A\_n3A, same ΔTIB,c and ΔRIB,c values as DC\_1A-3A\_n38A are reused, and are given in the tables below.

Table 5.183.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-38\_n3 | 1 | 0.5 |
| 38 | 0.5 |
| n3 | 0.5 |

**Table 5.183.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-38\_n3 | 1 | 0 |
| 38 | 0 |
| n3 | 0 |

### 5.183.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.184 DC\_7-38\_n3

### 5.184.1 Configurations for DC

Table 5.184.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink configuration |
| --- | --- |
| DC\_7A-38A\_n3Ax,y | N/A |
| NOTE x: The combination is not used alone as fall back mode of other band combinations.  NOTE y: Power imbalance between downlink carriers on Band 7 and Band 38 is assumed to be within 6dB. The power spectral density imbalance condition also applies for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration. | |

### 5.184.2 Co-existence studies

No need to analysis the co-existence studies for this configuration.

### 5.184.3 ∆TIB and ∆RIB values

For DC\_7-38\_n3, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.184.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-38\_n3 | 7 | 0.5 |
| 38 | 0.5 |
| n3 | 0.5 |

**Table 5.184.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-38\_n3 | 7 | 0 |
| 38 | 0 |
| n3 | 0 |

### 5.184.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.185 DC\_20-38\_n3

### 5.185.1 Configurations for DC

Table 5.185.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_20A-38A\_n3A | DC\_20A\_n3A |

### 5.185.2 Co-existence studies

The co-existence studies of DC\_20\_n3 have already been captured in TR 37.716-11-11, where:

- IMD2, IMD3 produce caused by DC\_20\_n3 uplink may fall into own Rx of band 38.

### 5.185.3 ∆TIB and ∆RIB values

For DC\_20A-38A\_n3A, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.185.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20-38\_n3 | 20 | 0.3 |
| 38 | 0.5 |
| n3 | 0.5 |

**Table 5.185.3-2: ΔRIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB,c [dB] |
| --- | --- | --- |
| DC\_20-38\_n3 | 20 | 0 |
| 38 | 0 |
| n3 | 0 |

### 5.185.4 Reference sensitivity exceptions

According to co-existence studies, both IMD2 and IMD3 may fall into the Rx of band 38. Here we only define MSD caused by IMD2 for this band combination in table 5.185.4-1. For MSD caused by IMD3, noteX in the table is specfied.

Table 5.185.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_20A-38A\_n3A | 20 | 850 | 5 | 25 | 809 | N/A | N/A |
|  | 38 | 2610 | 5 | 25 | 2610 | 28.4 | IMD2X |
|  | n3 | 1760 | 5 | 25 | 1855 | N/A | N/A |
| NOTE X: This band is subject to IMD3 also which MSD is not specified. | | | | | | | |

## 5.186 DC\_1-32\_n8

### 5.186.1 Configurations for DC

Table 5.186.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-32A\_n8A | DC\_1A\_n8A |

### 5.186.2 Co-existence studies

Table 5.186.2-1 lists the Band 1A + Band n8A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.186.2-1: Band 1 and Band n8 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 1920 | 1980 | | 880 | 915 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 3840 – 3960 | | | 1760 – 1830 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 5760 – 5940 | | | 2640 – 2745 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1005 – 1100 | | | 2800 – 2895 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 2925 – 3080 | | | 90 – 220 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 4720 – 4875 | | | 3680 – 3810 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 1900 – 2000 | | | 860 – 935 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4845 – 5060 | | | 660 – 825 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 2010 – 2200 | | | 5600 – 5790 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6640 – 6855 | | | 4560 – 4725 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1540 – 1740 | | | 6765 – 7040 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1095 – 1320 | | | 3930 – 4180 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5440 – 5640 | | | 8560 – 8835 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6480 – 6705 | | | 7520 – 7770 | | |

Based on Table 5.186.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 3, 46 and 47

- 3rd order harmonics may fall into Rx frequencies of bands 7, 41, 77 and 90

- 3rd order IMD may fall into Rx frequencies of bands 43, 48, 49, 77, 78 and 79

- 4th order IMD may fall into Rx frequencies of bands 1, 4, 10, 12, 13, 14, 17, 20, 23, 28, 29, 34, 44, 46, 65, 66, 67, 68, 70, 79 and 85

- 5th order IMD may fall into Rx frequencies of bands 24, 46 and 77

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.186.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.186.2-2: 2UL Band 1 + Band n8 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD5 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD5 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD5 |
| GPS | 1563 | - | 1587 | Yes |  | IMD5 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | No | Europe |  |
| 5470 | - | 5725 | Yes | IMD4, IMD5 |
| 5150 | - | 5825 | Yes | Asia | 2nd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_1\_n8 in 38101-3.

### 5.186.3 ∆TIB and ∆RIB values

Table 5.186.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1A-32A\_n8 | 1 | 0.5 |
| n8 | 0.3 |

**Table 5.186.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1A-32A\_n8 | 1 | 0 |
| 32 | 0 |
| n8 | 0 |

### 5.186.4 Reference sensitivity exceptions

## No additional MSD compared to fallbacks.5.187 DC\_1-38\_n8

### 5.187.1 Configurations for DC

Table 5.187.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-38A\_n8A | DC\_1A\_n8A  DC\_38A\_n8A |

### 5.187.2 Co-existence studies

Table 5.187.2-1 lists the Band 1A + Band n8A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.187.2-1: Band 1 and Band n8 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 1920 | 1980 | | 880 | 915 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 3840 – 3960 | | | 1760 – 1830 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 5760 – 5940 | | | 2640 – 2745 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1005 – 1100 | | | 2800 – 2895 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 2925 – 3080 | | | 90 – 220 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 4720 – 4875 | | | 3680 – 3810 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 1900 – 2000 | | | 860 – 935 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4845 – 5060 | | | 660 – 825 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 2010 – 2200 | | | 5600 – 5790 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6640 – 6855 | | | 4560 – 4725 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1540 – 1740 | | | 6765 – 7040 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1095 – 1320 | | | 3930 – 4180 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 5440 – 5640 | | | 8560 – 8835 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6480 – 6705 | | | 7520 – 7770 | | |

Based on Table 5.187.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 3, 46 and 47

- 3rd order harmonics may fall into Rx frequencies of bands 7, 41, 77 and 90

- 3rd order IMD may fall into Rx frequencies of bands 43, 48, 49, 77, 78 and 79

- 4th order IMD may fall into Rx frequencies of bands 1, 4, 10, 12, 13, 14, 17, 20, 23, 28, 29, 34, 44, 46, 65, 66, 67, 68, 70, 79 and 85

- 5th order IMD may fall into Rx frequencies of bands 24, 46 and 77

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.187.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.187.2-2: 2UL Band 1 + Band n8 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD5 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD5 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD5 |
| GPS | 1563 | - | 1587 | Yes |  | IMD5 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe | IMD5 |
| 2400 | - | 2494 | No | Asia | IMD5 |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | No | Europe |  |
| 5470 | - | 5725 | Yes | IMD4, IMD5 |
| 5150 | - | 5825 | Yes | Asia | 2nd harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_1\_n8 in 38101-3.

Table 5.187.2-3 lists the Band 38A + Band n8A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.187.2-3: Band 38 and Band n8 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2570 | 2620 | | 880 | 915 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5140 – 5240 | | | 1760 – 1830 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7710 – 7860 | | | 2640 – 2745 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1655 – 1740 | | | 3450 – 3535 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 4225 – 4360 | | | 740 – 860 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 6020 – 6155 | | | 4330 – 4450 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2550 – 2640 | | | 860 – 935 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 6795 – 6980 | | | 20 – 175 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 3310 – 3480 | | | 6900 – 7070 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 8590 – 8775 | | | 5210 – 5365 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 900 – 1090 | | | 9365 – 9600 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 2395 – 2600 | | | 5880 – 6100 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 6090 – 6280 | | | 11160 – 11395 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7780 – 7985 | | | 9470 – 9690 | | |

Based on Table 5.187.2-3,

- 2nd order harmonics may fall into Rx frequencies of bands 7, 41, 46 and 90

- 3rd order harmonics may fall into Rx frequencies of band 3

- 2nd order IMD may fall into Rx frequencies of bands 22, 42, 77 and 78

- 3rd order IMD may fall into Rx frequencies of bands 12, 13, 14, 17, 20, 26, 27, 28, 44, 67, 68, 79 and 85

- 4th order IMD may fall into Rx frequencies of bands 42, 46, 52, 77 and 78

- 5th order IMD may fall into Rx frequencies of bands 8, 38, 40, 41, 46, 47, 53, 69 and 90

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.187.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.187.2-4: 2UL Band 38 + Band n8 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD5 |
| 2400 | - | 2494 | Yes | Asia | IMD5 |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | 2nd harmonic, IMD4 |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 2nd harmonic, IMD4 |

The requirements for spurious emission band UE coexistence are proposed in a parallel TP for fallback DC\_38\_n8.

### 5.187.3 ∆TIB and ∆RIB values

Table 5.187.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1A-38A\_n8 | 1 | 0.5 |
| 38 | 0.5 |
| n8 | 0.3 |

**Table 5.187.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1A-38A\_n8 | 1 | 0 |
| 38 | 0 |
| n8 | 0 |

### 5.187.4 Reference sensitivity exceptions

No additional MSD required based on fallbacks.

## 5.188 DC\_7-32\_n3

### 5.188.1 Configurations for DC

Table 5.188.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-32A\_n3A | DC\_7A\_n3A |

### 5.188.2 Co-existence studies

Table 5.188.2-1 lists the Band 7A + Band n3A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.188.2-1: Band 7 and Band n3 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2500 | 2570 | | 1710 | 1785 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5000 – 5140 | | | 3420 – 3570 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7500 – 7710 | | | 5130 – 5355 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 715 – 860 | | | 4210 – 4355 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 3215 – 3430 | | | 850 – 1070 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 6710 – 6925 | | | 5920 – 6140 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2470 – 2600 | | | 1690 – 1805 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5715 – 6000 | | | 2560 – 2855 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1430 – 1720 | | | 8420 – 8710 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 9210 – 9495 | | | 7630 – 7925 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 4270 – 4640 | | | 8215 – 8570 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 10 – 355 | | | 3930 – 4290 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 9340 – 9710 | | | 11710 – 12065 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10130 – 10495 | | | 10920 – 11280 | | |

Based on Table 5.188.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 22, 42, 48, 49, 77 and 78

- 3rd order harmonics may fall into Rx frequencies of band 46

- 2nd order IMD may fall into Rx frequencies of bands 12, 13, 14, 17, 20, 26, 27, 28, 29, 44, 67, 68 and 85

- 3rd order IMD may fall into Rx frequencies of bands 5, 6, 8, 18, 19, 26, 27, 42, 46, 47, 52, 77 and 78

- 4th order IMD may fall into Rx frequencies of bands 7, 11, 21, 24, 32, 38, 41, 45, 46, 47, 50, 51, 69, 74, 75, 76, 90, 91, 92, 93 and 94

- 5th order IMD may fall into Rx frequencies of bands 77 and 79

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.188.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.188.2-2: 2UL Band 7 + Band n3 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD4 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD4 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD4 |
| GPS | 1563 | - | 1587 | Yes |  | IMD4 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 3rd Harmonic, IMD3, IMD4 |
| 5150 | - | 5350 | Yes | Europe | 3rd Harmonic |
| 5470 | - | 5725 | Yes | IMD4 |
| 5150 | - | 5825 | Yes | Asia | 3rd Harmonic, IMD4 |

The requirements for spurious emission band UE coexistence exist for DC\_7\_n3 in 38101-3.

### 5.188.3 ∆TIB and ∆RIB values

Table 5.188.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n3 | 7 | 0.7 |
| n3 | 0.7 |

**Table 5.188.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n3 | 7 | 0 |
| 32 | 0 |
| n3 | 0 |

### 5.188.4 Reference sensitivity exceptions

Table 5.188.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_7A-32A\_n3A | 7 | 1775 | 5 | 25 | 1870 | N/A | N/A |
| n3 | 2510 | 10 | 50 | 2630 | N/A | N/A |
| 32 | - | - | - | 1470 | 10.5 | IMD4 |

## 5.189 DC\_3-32\_n28

### 5.189.1 Configurations for DC

Table 5.189.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_3A-32A\_n28A  DC\_3C-32A\_n28A | DC\_3A\_n28A  DC\_3C\_n28A |
|  | |

### 5.189.2 Co-existence studies

For UE coexistence study of Band 3 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.189.2-1.

Table 5.189.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1785 | 703 | 748 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3570 | 1406 | 1496 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5355 | 2109 | 2244 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7140 | 2812 | 2992 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8925 | 3515 | 3740 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1082 | 962 | 2413 | 2533 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2672 | 2867 | 379 | 214 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4123 | 4318 | 3116 | 3281 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4382 | 4652 | 324 | 534 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 5833 | 6103 | 3819 | 4029 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1924 | 2164 | 4826 | 5066 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1282 | 1027 | 6437 | 6092 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1176 | 1461 | 3949 | 3634 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4522 | 4777 | 7543 | 7888 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5529 | 5814 | 6536 | 6851 |

The second harmonic interference of band n28 may fall into band 32.

IMD5 may fall into Rx of band 32 when band 3 and n28 transmit.

### 5.189.3 ∆TIB and ∆RIB values

For DC\_3-32\_n28, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.189.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-32\_n28 | 3 | 0.3 |
| n28 | 0.3 |

**Table 5.189.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-32\_n28 | 3 | 0.5 |
| 32 | 0 |
| n28 | 0.5 |

### 5.189.4 Reference sensitivity exceptions

The band 32 MSD requirements due to 2nd order harmonic from band n28 can be specified as below by reusing the MSD requirements for DC\_28\_n50.

Table 5.189.4-1: Reference sensitivity exceptions (MSD) due to UL harmonic for EN-DC in NR FR1

| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| UL band | DL band | 5 MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 30 MHz (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 70 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n28 | 322,13 | 27.8 | 24.6 | 22.8 | 21.6 |  |  |  |  |  |  |  |  |  |
|  | 323 | 1.9 | 1.4 | 0.9 | 0.4 |  |  |  |  |  |  |  |  |  |
| NOTE 2: The requirements should be verified for UL EARFCN or NR ARFCN of the aggressor (lower) band (superscript LB) such that in MHz and  with carrier frequency in the victim (higher) band in MHz and the channel bandwidth configured in the lower band.  NOTE 3: The requirements are only applicable to channel bandwidths no larger than 20 MHz and with a carrier frequency at  MHz offset from  in the victim (higher band) with , whereandare the channel bandwidths configured in the aggressor (lower) and victim (higher) bands in MHz, respectively.  NOTE 13: These requirements apply when there is at least one individual RE within the uplink transmission bandwidth of the aggressor (lower) band for which the 2nd transmitter harmonic is within the downlink transmission bandwidth of a victim (higher) band and a range ∆FHD above and below the edge of this downlink transmission bandwidth. The value ∆FHD depends on the EN-DC band combination: ∆FHD = 10 MHz for DC\_1\_n77, DC\_2\_n48, DC\_2\_n77, DC\_42\_n3, DC\_48\_n25, DC\_48\_n66, DC\_66\_n48, DC\_66\_n77, DC\_3\_n77, DC\_3\_n78, DC\_11\_n28 and DC\_28\_n50, DC\_28\_n51, DC\_66\_n78, DC\_25\_n77, DC\_25\_n78. | | | | | | | | | | | | | | |

Table 5.189.4-2: Uplink configuration for reference sensitivity exceptions due to UL harmonic interference for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / UL RB allocation of the agressor band | | | | | | | | | | | | | | | |
| UL band | DL band | SCS of UL band  (kHz) | 5  MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 30 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 70 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n28 | 32 | 15 | 12 | 25 | 25 | 25 |  |  |  |  |  |  |  |  |  |

The MSD requirements due to IMD5 from DC\_3A-32A\_n28A don’t need to be specified, since a test case that the interference hits the victim channel directly can’t be found.

## 5.190 DC\_28-32\_n1

### 5.190.1 Configurations for DC

Table 5.190.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_28A-32A\_n1A | DC\_28A\_n1A |
|  | |

### 5.190.2 Co-existence studies

For UE coexistence study of Band n1 + Band 28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.190.2-1.

Table 5.190.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1920 | 1980 | 703 | 748 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3840 | 3960 | 1406 | 1496 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5760 | 5940 | 2109 | 2244 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 7680 | 7920 | 2812 | 2992 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 9600 | 9900 | 3515 | 3740 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1277 | 1172 | 2623 | 2728 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 3092 | 3257 | 574 | 424 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4543 | 4708 | 3326 | 3476 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5012 | 5237 | 129 | 324 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6463 | 6688 | 4029 | 4224 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2344 | 2554 | 5246 | 5456 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1072 | 832 | 7217 | 6932 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1596 | 1851 | 4534 | 4264 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4732 | 4972 | 8383 | 8668 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5949 | 6204 | 7166 | 7436 |

There is no IMD issue for this band combination.

### 5.190.3 ∆TIB and ∆RIB values

For DC\_28-32\_n1, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.190.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_28-32\_n1 | n1 | 0.5 |
| 28 | 0.6 |

**Table 5.190.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_28-32\_n1 | n1 | 0 |
| 32 | 0 |
| 28 | 0.2 |

### 5.190.4 Reference sensitivity exceptions

No need to specify the REFSENS exception for this band combination. The REFSENS exception due to harmonic interference between band 28 and 32 can refer to the MSD definition in Table 7.3.1A-0a from TS 36.101.

## 5.191 DC\_28-32\_n3

### 5.191.1 Configurations for DC

Table 5.191.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_28A-32A\_n3A | DC\_28A\_n3A |
|  | |

### 5.191.2 Co-existence studies

For UE coexistence study of Band n3 + Band 28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.191.2-1.

Table 5.191.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1785 | 703 | 748 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3570 | 1406 | 1496 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5355 | 2109 | 2244 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7140 | 2812 | 2992 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8925 | 3515 | 3740 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1082 | 962 | 2413 | 2533 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2672 | 2867 | 379 | 214 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4123 | 4318 | 3116 | 3281 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 4382 | 4652 | 324 | 534 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 5833 | 6103 | 3819 | 4029 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1924 | 2164 | 4826 | 5066 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 1282 | 1027 | 6437 | 6092 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1176 | 1461 | 3949 | 3634 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4522 | 4777 | 7543 | 7888 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 5529 | 5814 | 6536 | 6851 |

IMD5 may fall into Rx of band 32 when band n3 and 28 transmit.

### 5.191.3 ∆TIB and ∆RIB values

For DC\_28-32\_n3, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.191.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_28-32\_n3 | n3 | 0.3 |
| 28 | 0.3 |

**Table 5.191.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_28-32\_n3 | n3 | 0 |
| 32 | 0 |
| 28 | 0 |

### 5.191.4 Reference sensitivity exceptions

The REFSENS exception due to harmonic interference between band 28 and 32 can refer to the MSD definition in Table 7.3.1A-0a from TS 36.101.

The MSD requirements due to IMD5 from DC\_28A-32A\_n3A don’t need to be specified, since a test case that the interference hits the victim channel directly can’t be found.

## 5.192 DC\_7-32\_n8

### 5.192.1 Configurations for DC

Table 5.192.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_7A-32A\_n8A | DC\_7A\_n8A |

### 5.192.2 Co-existence studies

Table 5.192.2-1 lists the Band 7A + Band n8A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.192.2-1: Band 7 and Band n8 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2500 | 2570 | | 880 | 915 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5000 – 5140 | | | 1760 – 1830 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7500 – 7710 | | | 2640 – 2745 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1585 – 1690 | | | 3380 – 3485 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 4085 – 4260 | | | 670 – 810 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 5880 – 6055 | | | 4260 – 4400 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2480 – 2590 | | | 860 – 935 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 6585 – 6830 | | | 70 – 245 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 3170 – 3380 | | | 6760 – 6970 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 8380 – 8625 | | | 5140 – 5315 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 950 – 1160 | | | 9085 – 9400 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 2255 – 2500 | | | 5670 – 5950 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 6020 – 6230 | | | 10880 – 11195 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7640 – 7885 | | | 9260 – 9540 | | |

Based on Table 5.192.2-1,

- 2nd order harmonics may fall into Rx frequencies of band 3

- 3rd order harmonics may fall into Rx frequencies of bands 7, 41 and 90

- 2nd order IMD may fall into Rx frequencies of bands 42, 52, 77 and 78

- 3rd order IMD may fall into Rx frequencies of bands 12, 13, 14, 17, 20, 28, 29, 44, 46, 47, 67, 68, 77 and 85

- 4th order IMD may fall into Rx frequencies of bands 46, 52, 77 and 78

- 5th order IMD may fall into Rx frequencies of bands 8, 30, 40, 41, 46, 47, 53 and 90

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.192.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.192.2-2: 2UL Band 7 + Band n8 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD2 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD2 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD2 |
| GPS | 1563 | - | 1587 | Yes |  | IMD2 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD5 |
| 2400 | - | 2494 | Yes | Asia | IMD5 |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | IMD3, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | IMD4 |
| 5470 | - | 5725 | Yes | IMD5 |
| 5150 | - | 5825 | Yes | Asia | IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_7\_n8 in 38101-3.

### 5.192.3 ∆TIB and ∆RIB values

Table 5.192.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n8 | 7 | 0.7 |
| n8 | 0.6 |

**Table 5.192.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7A-32A\_n8 | 7 | 0 |
| 32 | 0 |
| n8 | 0.2 |

### 5.192.4 Reference sensitivity exceptions

## No additional MSD compared to fallbacks.5.193 DC\_20-32\_n8

### 5.193.1 Configurations for DC

Table 5.193.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_20A-32A\_n8A | DC\_20A\_n8A |

### 5.193.2 Co-existence studies

Table 5.193.2-1 lists the Band 20A + Band n8A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.193.2-1: Band 20 and Band n8 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 832 | 862 | | 880 | 915 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1664 – 1724 | | | 1760 – 1830 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2496 – 2586 | | | 2640 – 2745 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 18 – 83 | | | 1712 – 1777 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 749 – 844 | | | 898 – 998 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 2544 – 2639 | | | 2592 – 2692 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 812 – 882 | | | 860 – 935 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 1581 – 1706 | | | 1778 – 1913 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 36 – 166 | | | 3424 – 3554 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 3376 – 3501 | | | 3472 – 3607 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 2658 – 2828 | | | 2413 – 2568 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 916 – 1081 | | | 666 – 826 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4352 – 4522 | | | 4208 – 4363 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 4304 – 4469 | | | 4256 – 4416 | | |

Based on Table 5.193.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 3, 38, 41, 69 and 90

- 3rd order harmonics may fall into Rx frequencies of bands 7, 41 and 90

- 3rd order IMD may fall into Rx frequencies of bands 7, 8, 13, 14, 20, 28, 38, 41, 44, 67, 68, 69 and 90

- 4th order IMD may fall into Rx frequencies of bands 3, 9, 22, 33, 35, 37, 39, 42, 43, 48, 49, 52, 77 and 78

- 5th order IMD may fall into Rx frequencies of bands 7, 8, 12, 13, 14, 17, 20, 28, 29, 41, 44, 53, 67, 68, 79, 85 and 90

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.193.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.193.2-2: 2UL Band 20 + Band n8 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD4 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD4 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD4 |
| GPS | 1563 | - | 1587 | Yes |  | IMD4 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD5 |
| 2400 | - | 2494 | Yes | Asia | IMD5 |
| ISM band  (5GHz) | 5150 | - | 5925 | No | US |  |
| 5150 | - | 5350 | No | Europe |  |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | No | Asia |  |

The requirements for spurious emission band UE coexistence exist for DC\_20\_n8 in 38101-3.

### 5.193.3 ∆TIB and ∆RIB values

Table 5.193.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20A-32A\_n8 | 20 | 0.4 |
| n8 | 0.4 |

**Table 5.193.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20A-32A\_n8 | 20 | 0 |
| 32 | 0 |
| n8 | 0 |

### 5.193.4 Reference sensitivity exceptions

## No additional MSD compared to fallbacks.5.194 DC\_20-38\_n1

### 5.194.1 Configurations for DC

Table 5.194.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_20A-38A\_n1A | DC\_20A\_n1A  DC\_38A\_n1A |

### 5.194.2 Co-existence studies

Table 5.194.2-1 lists the Band 20A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.194.2-1: Band 20 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 832 | 862 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1664 – 1724 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2496 – 2586 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1058 – 1148 | | | 2752 – 2842 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 196 – 316 | | | 2978 – 3128 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3584 – 3704 | | | 4672 – 4822 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 782 – 912 | | | 1900 – 2000 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 516 – 666 | | | 4898 – 5108 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 2116 – 2296 | | | 5504 – 5684 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4416 – 4566 | | | 6592 – 6802 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6818 – 7088 | | | 1348 – 1528 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 4036 – 4276 | | | 1254 – 1464 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8512 – 8782 | | | 5248 – 5428 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7424 – 7664 | | | 6336 – 6546 | | |

Based on Table 5.194.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 46 and 47

- 3rd order harmonics may fall into Rx frequencies of bands 38, 41, 69, 77 and 90

- 3rd order IMD may fall into Rx frequencies of bands 22, 42, 43, 48, 49, 77, 78 and 79

- 4th order IMD may fall into Rx frequencies of bands 1, 4, 10, 23, 46, 65, 66, 71 and 79

- 5th order IMD may fall into Rx frequencies of bands 11, 21, 24, 32, 45, 46, 50, 51, 74, 75, 76, 77, 91, 92, 93 and 94

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.194.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.194.2-2: 2UL Band 20 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | IMD5 |
| 5470 | - | 5725 | Yes | IMD4 |
| 5150 | - | 5825 | Yes | Asia | 2nd harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_20\_n1 in 38101-3.

Table 5.194.2-3 lists the Band 38A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.194.2-3: Band 38 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2570 | 2620 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5140 – 5240 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7710 – 7860 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 590 – 700 | | | 4490 – 4600 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 3160 – 3320 | | | 1220 – 1390 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 7060 – 7220 | | | 6410 – 6580 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2520 – 2670 | | | 1900 – 2000 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5730 – 5940 | | | 3140 – 3370 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1180 – 1400 | | | 8980 – 9200 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 9630 – 9840 | | | 8330 – 8560 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5060 – 5350 | | | 8300 – 8560 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 520 – 800 | | | 3750 – 4020 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 10250 – 10540 | | | 12200 – 12460 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10900 – 11180 | | | 11550 – 11820 | | |

Based on Table 5.194.2-3,

- 2nd order harmonics may fall into Rx frequencies of bands 46 and 47

- 3rd order harmonics may fall into Rx frequencies of band 77

- 2nd order IMD may fall into Rx frequencies of bands 71 and 79

- 3rd order IMD may fall into Rx frequencies of bands 52, 77 and 78

- 4th order IMD may fall into Rx frequencies of bands 46, 47, 52, 77 and 78

- 5th order IMD may fall into Rx frequencies of bands 12, 13, 14, 17, 20, 28, 29, 43, 44, 46, 67, 68, 71, 77, 78 and 85

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.194.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.194.2-4: 2UL Band 38 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | 2nd harmonic, IMD5 |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 2nd harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence are proposed in a parallel TP for fallback DC\_38\_n1 mirroring the values used for DC\_1\_n38.

### 5.194.3 ∆TIB and ∆RIB values

Table 5.194.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_20A-38A\_n1 | 20 | 0.5 |
| 38 | 0.3 |
| n1 | 0.5 |

**Table 5.194.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_20A-38A\_n1 | 20 | 0.2 |
| 38 | 0 |
| n1 | 0 |

### 5.194.4 Reference sensitivity exceptions

No additional MSD required for band 20 3rd harmonic hit in band 38 compared to CA\_1A-20A-38A in 36101.

The following can be re-used from DC\_1A-20A\_n38A to cover the DC\_38A\_n1A IMD5 hit in band 20:

Table 5.194.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | | EUTRA / NR band | | UL Fc  (MHz) | | UL/DL BW  (MHz) | | UL  LCRB | | DL Fc (MHz) | | MSD  (dB) | | IMD order | |
| DC\_20A-38A\_n1A | | n1 | | N/A | | N/A | | N/A | | N/A | | N/A | | N/A | |
|  | | 20 | | N/A | | N/A | | N/A | | N/A | | N/A | | IMD5 | |
|  | | 38 | | N/A | | N/A | | N/A | | N/A | | N/A | | N/A | |

## 5.195 DC\_32-38\_n1

### 5.195.1 Configurations for DC

Table 5.195.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_32A-38A\_n1A | DC\_38A\_n1A |

### 5.195.2 Co-existence studies

Table 5.195.2-1 lists the Band 38A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.195.2-1: Band 38 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2570 | 2620 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5140 – 5240 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7710 – 7860 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 590 – 700 | | | 4490 – 4600 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 3160 – 3320 | | | 1220 – 1390 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 7060 – 7220 | | | 6410 – 6580 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2520 – 2670 | | | 1900 – 2000 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5730 – 5940 | | | 3140 – 3370 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1180 – 1400 | | | 8980 – 9200 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 9630 – 9840 | | | 8330 – 8560 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5060 – 5350 | | | 8300 – 8560 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 520 – 800 | | | 3750 – 4020 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 10250 – 10540 | | | 12200 – 12460 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10900 – 11180 | | | 11550 – 11820 | | |

Based on Table 5.195.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 46 and 47

- 3rd order harmonics may fall into Rx frequencies of band 77

- 2nd order IMD may fall into Rx frequencies of bands 71 and 79

- 3rd order IMD may fall into Rx frequencies of bands 52, 77 and 78

- 4th order IMD may fall into Rx frequencies of bands 46, 47, 52, 77 and 78

- 5th order IMD may fall into Rx frequencies of bands 12, 13, 14, 17, 20, 28, 29, 43, 44, 46, 67, 68, 71, 77, 78 and 85

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.195.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.195.2-2: 2UL Band 38 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | 2nd harmonic, IMD5 |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 2nd harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence are proposed in a parallel TP for fallback DC\_38\_n1 mirroring the values used for DC\_1\_n38.

### 5.195.3 ∆TIB and ∆RIB values

Table 5.195.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_32A-38A\_n1 | 38 | 0.5 |
| n1 | 0.5 |

**Table 5.195.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_32A-38A\_n1 | 32 | 0 |
| 38 | 0 |
| n1 | 0 |

### 5.195.4 Reference sensitivity exceptions

No additional MSD exceptions required.

## 5.196 DC\_7-7-28\_n1

5.196.1 Configurations for DC

Table 5.196.1-1: Inter-band DC configurations (three bands)

| DC  Configuration | Uplink DC  configuration |
| --- | --- |
| DC\_7A-7A-28A\_n1A | DC\_28A\_n1A DC\_7A\_n1A |

### 5.196.2 Co-existence studies

Co-existence studies have been performed for DC\_7-28\_n1 as well as for lower order combinations.

5.196.3 ∆TIB and ∆RIB values

Table 5.196.3-1: ΔTIB,c

| Inter-band DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_7-7-28\_n1 | 7 | 0.6 |
| 28 | 0.6 |
| n1 | 0.5 |

Table 5.196.3-2: ΔRIB

| Inter-band DC configuration | E-UTRA or NR Band | ΔRIB,c (dB) |
| --- | --- | --- |
| DC\_7-7-28\_n1 | 7 | 0 |
| 28 | 0.2 |
| n1 | 0 |

5.196.4 Reference sensitivity exceptions

The MSD requirements can reuse the same requirements for DC\_7A-28A\_n1A.

## 5.197 DC\_8-20\_n28

### 5.197.1 Configurations for DC

Table 5.197.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-20A\_n28A6,X | DC\_8A\_n28A  DC\_20A\_n28A |
| NOTE 6: The frequency range in band n28 is restricted for this band combination to 703-733 MHz for the UL and 758 – 788 MHz for the DL.  NOTE X: The implementation with 3 low-band antennas is targeted for FWA form factor for this band combination in Release 17. | |

### 5.197.2 Co-existence studies

For UE coexistence study of Band 8 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.197.2-1.

Table 5.197.2-1: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 703 | 748 | 880 | 915 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1406 | 1496 | 1760 | 1830 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2109 | 2244 | 2640 | 2745 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2812 | 2992 | 3520 | 3660 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3515 | 3740 | 4400 | 4575 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 132 | 212 | 1583 | 1663 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 491 | 616 | 1012 | 1127 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 2286 | 2411 | 2463 | 2578 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 1194 | 1364 | 1892 | 2042 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 2989 | 3159 | 3343 | 3493 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 424 | 264 | 3166 | 3326 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 2957 | 2772 | 2112 | 1897 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1339 | 1144 | 484 | 279 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4223 | 4408 | 3692 | 3907 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 4046 | 4241 | 3869 | 4074 |

For UE coexistence study of Band 20 + Band n28, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.197.2-2.

Table 5.197.2-2: Harmonic and IMD analysis

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 703 | 748 | 832 | 862 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1406 | 1496 | 1664 | 1724 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2109 | 2244 | 2496 | 2586 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 2812 | 2992 | 3328 | 3448 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 3515 | 3740 | 4160 | 4310 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 84 | 159 | 1535 | 1610 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 544 | 664 | 916 | 1021 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 2238 | 2358 | 2367 | 2472 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 1247 | 1412 | 1748 | 1883 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 2941 | 3106 | 3199 | 3334 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 318 | 168 | 3070 | 3220 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 2745 | 2580 | 2160 | 1950 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1180 | 1000 | 580 | 385 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 4031 | 4196 | 3644 | 3854 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 3902 | 4082 | 3773 | 3968 |

IMD3 of Tx band 20 + band n28 may fall into Rx of band 8.

### 5.197.3 ∆TIB and ∆RIB values

For DC\_8-20\_n28, the ΔTIB,c and ΔRIB,c values are reused from DC\_20\_n28 and DC\_8\_n28, and are given in the tables below.

Table 5.197.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8-20\_n28 | 8 | 0.6 |
| 20 | 0.5 |
| n28 | 0.5 |

**Table 5.197.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8-20\_n28 | 8 | 0.2 |
| 20 | 0 |
| n28 | 0.1 |

### 5.197.4 Reference sensitivity exceptions

MSD due to IMD3 of Tx band 20 + band n28 can be specified as below. Currently, the RF architecture with three antennas for low band are assumed. The implementation with three antennas for low band need a larger form factor than implementation with two antennas.

Table 5.197.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| DC\_8A-20A\_n28A | 8 | 901 | 5 | 25 | 946 | [23.5] | IMD3 |
| 20 | 837 | 5 | 25 | 796 | N/A | N/A |
| n28 | 728 | 5 | 25 | 773 | N/A | N/A |

## 5.198 DC\_8\_(n)3

5.198.1 Operating bands for EN-DC

Table 5.198.1.1-1: Band combinations EN-DC (three bands)

| EN-DC Band | E-UTRA Band | NR Band | Single UL allowed |
| --- | --- | --- | --- |
| DC\_8\_(n)3 | CA\_8-3 | n3 | DC\_(n)3AA1 |
| NOTE 1: Only single switched UL is supported | | | |

5.198.2 Configurations for EN-DC

Table 5.198.1.2-1: Inter-band EN-DC configurations (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA configuration | NR configuration |
| --- | --- | --- | --- |
| DC\_8A\_(n)3AA | DC\_(n)3AA  DC\_8A\_n3A | CA\_8A-3A | n3A |

5.198.3 ∆TIB and ∆RIB values

∆TIB, ∆RIB values for DC\_8\_n3 are specified as follows:

Table 5.198.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8\_(n)3 | 8 | 0.3 |
| 3 | 0.3 |
| n3 | 0.3 |

Table 5.198.3-2: ΔRIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8\_(n)3 | 8 | 0 |
| 3 | 0 |
| n3 | 0 |

5.198.4 MSD Analysis and requirements

For DC\_8A\_n3A the harmonics and intermodulation product intervals are calculated as below:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 880 | 915 | 1710 | 1785 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 1760 | 1830 | 3420 | 3570 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 2640 | 2745 | 5130 | 5355 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 3520 | 3660 | 6840 | 7140 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 4400 | 4575 | 8550 | 8925 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 795 | 905 | 2590 | 2700 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 25 | 120 | 2505 | 2690 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 3470 | 3615 | 4300 | 4485 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 855 | 1035 | 4215 | 4475 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4350 | 4530 | 6010 | 6270 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 1810 | 1590 | 5180 | 5400 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6260 | 5925 | 1950 | 1735 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3595 | 3300 | 675 | 930 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7720 | 8055 | 5230 | 5445 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6890 | 7185 | 6060 | 6315 |

- 2nd order harmonic of band 8 could fall on n3 DL frequency range.

- IMD4 and IMD5 could fall on n3 DL frequency range.

The MSD values are similar to DC\_3\_n8, which can be found on Table 7.3B.2.3.5.1-1 in TS 38.101-3.

For DC\_(n)3AA the harmonics and intermodulation product intervals are calculated as below:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | **fy\_low** | **fy\_high** |
| UL frequency (MHz) | 1710 | 1785 | 1710 | 1785 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 3420 | 3570 | 3420 | 3570 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 5130 | 5355 | 5130 | 5355 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 6840 | 7140 | 6840 | 7140 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 8550 | 8925 | 8550 | 8925 |
| 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 75 | 75 | 3420 | 3570 |
| Two-tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 1635 | 1860 | 1635 | 1860 |
| Two-tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 5130 | 5355 | 5130 | 5355 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 3345 | 3645 | 3345 | 3645 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 6840 | 7140 | 6840 | 7140 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 150 | 150 | 6840 | 7140 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5430 | 5055 | 5430 | 5055 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 1935 | 1560 | 1935 | 1560 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8550 | 8925 | 8550 | 8925 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 8550 | 8925 | 8550 | 8925 |

No harmonic or intermodulation product of DC\_(n)3AA interfers with the band 8 DL frequency range.

For MSD values for n3 DL, refer to DC\_(n)3AA configuration in TR 37.717-11-11

## 5.199 DC\_1-11\_n79

5.199.1 Configurations for DC\_1-11\_n79

Table 5.199.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_1A-11A\_n79A5 | DC\_1A\_n79A  DC\_11A\_n79A |
| NOTE 5: Applicable for UE supporting inter-band EN-DC with mandatory simultaneous Rx/Tx capability | |

5.199.2 Co-existence studies

When Uplink EN-DC configuration is DC\_1A\_n79A, (1) 4th IMD of (B1 - n79) will fall into Rx band of Band 11. When Uplink EN-DC configuration is DC\_11A\_n79A, (2) 3rd IMD of (B11 - n79) will fall into Rx band of Band 1.

5.199.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.199.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_1-11\_n79 | 1 | 0.3 |
| 11 | 0.3 |
| n79 | 0 |

Table 5.199.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_1-11\_n79 | 1 | 0 |
| 11 | 0 |
| n79 | 0 |

5.199.4 Reference sensitivity exceptions

As mentioned above, IMD4 of B1 and n79 to Band11 Rx and IMD3 of B11 and n79 to Band1 Rx need to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.199.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_1A-11A\_n79A | 1 | 1970 | 5 | 25 | 2160 | N/A | FDD | N/A |
| n79 | 4427 | 40 | 216 | 4427 | N/A | TDD | N/A |
| 11 | 1435 | 5 | 25 | 1483 | 10.2 | FDD | IMD4 |
| DC\_1A-11A\_n79A | 11 | 1431 | 5 | 25 | 1479 | N/A | FDD | N/A |
| n79 | 4980 | 40 | 216 | 4980 | N/A | TDD | N/A |
| 1 | 1928 | 5 | 25 | 2118 | 15.6 | FDD | IMD3 |

## 5.200 DC\_8-11\_n79

5.200.1 Configurations for DC\_8-11\_n79

Table 5.200.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-11A\_n79A5 | DC\_8A\_n79A  DC\_11A\_n79A |
| NOTE 5: Applicable for UE supporting inter-band EN-DC with mandatory simultaneous Rx/Tx capability | |

5.200.2 Co-existence studies

When Uplink EN-DC configuration is DC\_8A\_n79A, (1) IMD5 of (B8 - n79) will fall into Rx band of Band 11. When Uplink EN-DC configuration is DC\_11A\_n79A, (2) IMD5 of (B11 - n79) will fall into Rx band of Band 8. 5.200.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.200.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_8-11\_n79 | 8 | 0.3 |
| 11 | 0.4 |
| n79 | 0 |

Table 5.200.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_8-11\_n79 | 8 | 0 |
| 11 | 0 |
| n79 | 0 |

5.200.4 Reference sensitivity exceptions

As mentioned above, IMD5 of B8 and n79 to Band11 Rx and IMD5 of B11 and n79 to Band8 Rx need to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.200.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_8A-11A\_n79A | 8 | 882.5 | 5 | 25 | 927.5 | N/A | FDD | N/A |
| n79 | 4980 | 40 | 216 | 4980 | N/A | TDD | N/A |
| 11 | 1430.4 | 5 | 25 | 1478.4 | 1.2 | FDD | IMD5 |
| DC\_8A-11A\_n79A | 11 | 1435 | 5 | 25 | 1483 | N/A | FDD | N/A |
| n79 | 4810 | 40 | 216 | 4810 | N/A | TDD | N/A |
| 8 | 885 | 5 | 25 | 930 | 2.8 | FDD | IMD5 |

## 5.201 DC\_8-41\_n3

5.201.1 Configurations for DC\_8-41\_n3

Table 5.201.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-41A\_n3A5  DC\_8A-41C\_n3A5 | DC\_8A\_n3A  DC\_41A\_n3A  DC\_41C\_n3A |
| NOTE 5: Applicable for UE supporting inter-band EN-DC with mandatory simultaneous Rx/Tx capability | |

5.201.2 Co-existence studies

When Uplink EN-DC configuration is DC\_8A\_n3A, (1) IMD2/3 of (B8 - n3) will fall into Rx band of Band 41. When Uplink EN-DC configuration is DC\_41A\_n3A, (2) IMD2/3 of (B41 - n3) will fall into Rx band of Band 8. 5.201.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.201.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_8-41\_n3 | 8 | 0.3 |
| 41 | 0.33/0.84 |
| n3 | 0.5 |
| NOTE 3: Applicable for the frequency range of 2515 - 2690 MHz.  NOTE 4: Applicable for the frequency range of 2496 - 2515 MHz. | | |

Table 5.201.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_8-41\_n3 | 8 | 0 |
| 41 | 03/0.54 |
| n3 | 0 |
| NOTE 3: Applicable for the frequency range of 2515 - 2690 MHz.  NOTE 4: Applicable for the frequency range of 2496 - 2515 MHz. | | |

5.201.4 Reference sensitivity exceptions

As mentioned above, IMD2/3 of B8 and n3 to Band41 Rx and IMD2/3 of B41 and n3 to Band8 Rx need to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.201.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_8A-41A\_n3A  DC\_8A-41C\_n3A | 8 | 885 | 5 | 25 | 930 | N/A | FDD | N/A |
| n3 | 1780 | 5 | 25 | 1875 | N/A | FDD | N/A |
| 41 | 2665 | 5 | 25 | 2665 | 27.4 | TDD | IMD21 |
| DC\_8A-41A\_n3A  DC\_8A-41C\_n3A | 41 | 2665 | 5 | 25 | 2665 | N/A | TDD | N/A |
| n3 | 1715 | 5 | 25 | 1810 | N/A | FDD | N/A |
| 8 | 905 | 5 | 25 | 950 | 28.9 | FDD | IMD21 |
| NOTE 1: This band is subject to IMD3 also which MSD is not specified. | | | | | | | | |

## 5.202 DC\_8-42\_n1

5.202.1 Configurations for DC\_8-42\_n1

Table 5.202.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-42A\_n1A5  DC\_8A-42C\_n1A5 | DC\_8A\_n1A  DC\_42A\_n1A  DC\_42C\_n1A |
| NOTE 5: Applicable for UE supporting inter-band EN-DC with mandatory simultaneous Rx/Tx capability | |

5.202.2 Co-existence studies

When Uplink EN-DC configuration is DC\_42A\_n1A, (2) IMD5 of (B42 - n1) will fall into Rx band of Band 8. 5.202.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.202.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_8-42\_n1 | 8 | 0.6 |
| 42 | 0.8 |
| n1 | 0.3 |

Table 5.202.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_8-42\_n1 | 8 | 0.2 |
| 42 | 0.5 |
| n1 | 0 |

5.202.4 Reference sensitivity exceptions

As mentioned above, IMD5 of B42 and n1 to Band8 Rx need to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.202.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_8A-42A\_n1A  DC\_8A-42C\_n1A | 42 | 3405 | 10 | 50 | 3405 | N/A | FDD | N/A |
| n1 | 1955 | 5 | 25 | 2145 | N/A | TDD | N/A |
| 8 | 900 | 5 | 25 | 945 | 3.3 | FDD | IMD5 |

## 5.203 DC\_8-41\_n77

5.203.1 Configurations for DC\_8-41\_n77

Table 5.203.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-41A\_n77A  DC\_8A-41C\_n77A | DC\_8A\_n77A  DC\_41A\_n77A  DC\_41C\_n77A |

5.203.2 Co-existence studies

When Uplink EN-DC configuration is DC\_8A\_n77A, (1) IMD2 of (B8 - n77) will fall into Rx band of Band 41. When Uplink EN-DC configuration is DC\_41A\_n77A, (2) IMD2/3/5 of (B41 - n77) will fall into Rx band of Band 8. But the synchronous operation is considered to DC\_41A\_n77A, (1) do not need to be considered. 5.203.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.203.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_8-41\_n77 | 8 | 0.6 |
| 41 | 0.3 |
| n77 | 0.8 |

Table 5.203.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_8-41\_n77 | 8 | 0.2 |
| 41 | 0 |
| n77 | 0.5 |

5.203.4 Reference sensitivity exceptions

As mentioned above, IMD2/3/5 of B41 and n77 to Band8 Rx and IMD2 of B8 and n77 to Band41 need to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.203.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA/NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **Duplex mode** | **IMD order** |
| DC\_8A-41A\_n77A  DC\_8A-41C\_n77A | 41 | 2630 | 10 | 50 | 2630 | N/A | FDD | N/A |
| n77 | 3580 | 10 | 50 | 3580 | N/A | TDD | N/A |
| 8 | 905 | 5 | 25 | 950 | 29.1 | FDD | IMD21, 4 |
| DC\_8A-41A\_n77A  DC\_8A-41C\_n77A | 8 | 895 | 5 | 25 | 940 | N/A | FDD | N/A |
| n77 | 3545 | 10 | 50 | 3545 | N/A | TDD | N/A |
| 41 | 2650 | 5 | 25 | 2650 | 28.0 | TDD | IMD2 |
| NOTE 1: This band is subject to IMD3 also which MSD is not specified.  NOTE 4: This band is subject to IMD5 also which MSD is not specified. | | | | | | | | |

## 5.204 DC\_5-13\_n77

### 5.204.1 Configuration for DC

Table 5.204.1-1: Inter-band EN-DC configurations within FR1 (three bands)

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_5A-13A\_n77A  DC\_5A-13A\_n77C | DC\_5A\_ n77A  DC\_13A\_ n77A |

### 5.204.2 Co-existence studies

According to the studies in 37.717-11-11, the Rx impacts are identified as below,

* For UL DC\_5A\_n77A, IMD5 of the 2UL may fall into band n13 Rx (For IMD4, although in calculation there is 3MHz overlap with n13 Rx, but considering there is no way to allocate a minimum channel bandwidth on either transmitter side, IMD4 shall not be pursued)
* For UL DC\_13A\_n77A, IMD5 of the 2UL may fall into band n5 Rx

Thus additional MSD should be considered to mitigate the impact of the interference for DC\_5A-13A\_n77A combination.

### 5.204.3 ∆TIB and ∆RIB values

For DC\_5-13\_n77, the ΔTIB,c and ΔRIB,c values are given in the tables below, reused from DC\_13\_n5-n77.

**Table 5.204.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-13\_n77 | 5 | 0.6 |
| 13 | 0.5 |
| n77 | 0.8 |

Table 5.204.3-2 ΔRIB,c due to EN-DC (three bands)

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-13\_n77 | 5 | 0.2 |
| 13 | 0.2 |
| n77 | 0.5 |

### 5.204.4 REFSENS requirements

Based on Table 5.3-1 in TR 37.717-11-21, there is IMD5 produced by Band 13 and NR band n77 that impact the reference sensitivity of NR band n5.

The required MSD level and test configuration are specified in Table 5.204.4-1 for this dual connectivity configuration.

Table 5.204.4-1: Reference sensitivity exceptions for Scell due to dual uplink operation for DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_5A-13A\_n77A11  DC\_5A-13A\_n77C11 | 5 | 840 | 5 | 25 | 885 | N/A | N/A |
|  | n77 | 4110 | 10 | 50 | 4110 | N/A | N/A |
|  | 13 | 781 | 5 | 20 | 750 | 4.4 | IMD5 |
|  | 13 | 782 | 5 | 20 | 751 | N/A | N/A |
|  | n77 | 4013 | 10 | 50 | 4013 | N/A | N/A |
|  | 5 | 840 | 5 | 25 | 885 | 4.5 | IMD5 |
| NOTE 11:The MSD test points cannot be verified for the band combination in US due to the Band n77 frequency range restriction. | | | | | | | |

## 5.205 DC\_5-48\_n77

5.205.1 Configurations for DC

**Table 5.205.1-1: Inter-band EN-DC configurations within FR1 (three bands)**

| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| --- | --- |
| DC\_5A-48A\_n77A  DC\_5A-48C\_n77A  DC\_5A-48D\_n77A  DC\_5A-48A\_n77C  DC\_5A-48C\_n77C  DC\_5A-48D\_n77C | DC\_5A\_n77A |

5.205.2 Co-existence studies

DC\_48\_n77 is fully limited for downlink only, and there is no simultaneous Tx/Rx operation between E-UTRA B48 and NR n77 carriers. Thus there is no additional co-existence study is needed for TDD Band 48.

5.205.3 ∆TIB and ∆RIB values

For DC\_5-48\_n77, the ΔTIB,c and ΔRIB,c values are specified in the tables below, reusing DC\_5\_n77 values.

**Table 5.205.3-1: ΔTIB,c due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_5-48\_n77 | 5 | 0.6 |
| 48 | 0.8 |
| n77 | 0.8 |

**Table 5.205.3-2: ΔRIB due to EN-DC (three bands)**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_5-48\_n77 | 5 | 0.2 |
| 48 | 0.5 |
| n77 | 0.5 |

5.205.4 REFSENS requirements

Based on 5.205.2 discussion above, REFSENS exceptions are not expected.

## 5.206 DC\_1-7\_n38

### 5.206.1 Configurations for DC

Table 5.206.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink EN-DC configuration | Uplink E-UTRA configuration | Uplink NR configuration |
| --- | --- | --- | --- |
| DC\_1A-7A\_n38A17,18 | N/A | 1A | N/A |
| NOTE 17: The combination is not used alone as fall back mode of other band combinations.  NOTE 18: Power imbalance between downlink carriers on Band 7 and Band 38 or band n38 is assumed to be within 6dB. The power spectral density imbalance condition also applies for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration. | | | |

To avoid duplicated NOTEs in the TS38.101-3 specification, it is proposed to add ‘or band n38’ on top of the existing NOTE 18 in table 5.5B.4.2 in the TS38.101-3, shown as above.

### 5.206.2 Co-existence studies

No need to analysis the co-existence studies for this configuration.

### 5.206.3 ∆TIB and ∆RIB values

For DC\_1-7\_n38, same ΔTIB,c and ΔRIB,c values of LTE CA 1-7-38 are reused which are given in the tables below.

Table 5.206.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_1-7\_n38 | 1 | 0.5 |

**Table 5.206.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_1-7\_n38 | 1 | 0 |
| 7 | 0 |
| n38 | 0.2 |

### 5.206.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.207 DC\_3-7\_n38

### 5.207.1 Configurations for DC

Table 5.207.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink EN-DC configuration | Uplink E-UTRA configuration | Uplink NR configuration |
| --- | --- | --- | --- |
| DC\_3A-7A\_n38A17,18 | N/A | 3A | N/A |
| NOTE 17: The combination is not used alone as fall back mode of other band combinations.  NOTE 18: Power imbalance between downlink carriers on Band 7 and Band 38 or band n38 is assumed to be within 6dB. The power spectral density imbalance condition also applies for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration. | | | |

To avoid duplicated NOTEs in the TS38.101-3 specification, it is proposed to add ‘or band n38’ on top of the existing NOTE 18 in table 5.5B.4.2 in the TS38.101-3, shown as above.

### 5.207.2 Co-existence studies

No need to analysis the co-existence studies for this configuration.

### 5.207.3 ∆TIB and ∆RIB values

For DC\_3-7\_n38, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.207.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_3-7\_n38 | 3 | 0.5 |

**Table 5.207.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_3-7\_n38 | 3 | 0 |
| 7 | 0 |
| n38 | 0.2 |

### 5.207.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.208 DC\_7-20\_n38

### 5.208.1 Configurations for DC

Table 5.208.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink EN-DC configuration | Uplink E-UTRA configuration | Uplink NR configuration |
| --- | --- | --- | --- |
| DC\_7A-20A\_n38A17,18 | N/A | 20A | N/A |
| NOTE 17: The combination is not used alone as fall back mode of other band combinations.  NOTE 18: Power imbalance between downlink carriers on Band 7 and Band 38 or band n38 is assumed to be within 6dB. The power spectral density imbalance condition also applies for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration. | | | |

To avoid duplicated NOTEs in the TS38.101-3 specification, it is proposed to add ‘or band n38’ on top of the existing NOTE 18 in table 5.5B.4.2 in the TS38.101-3, shown as above.

### 5.208.2 Co-existence studies

No need to analysis the co-existence studies for this configuration.

### 5.208.3 ∆TIB and ∆RIB values

For DC\_7-20\_n38, the ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.208.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_7-20\_n38 | 20 | 0.3 |

**Table 5.208.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_7-20\_n38 | 7 | 0 |
| 20 | 0 |
| n38 | 0.2 |

### 5.208.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

## 5.209 DC\_8-41\_n1

### 5.209.1 Configurations for DC\_8-41\_n1

Table 5.209.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-41A\_n1A  DC\_8A-41C\_n1A | DC\_8A\_n1A  DC\_41A\_n1A |

### 5.209.2 Co-existence studies

When Uplink EN-DC configuration is DC\_41A\_n1A, IMD5 of (B41 - n1) will fall into Rx band of Band 8. Thus, it is proposed to evaluate.

### 5.209.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.209.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_8-41\_n1 | 8 | 0.3 |
| 41 | 0.3 |
| n1 | 0.3 |

Table 5.209.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_8-41\_n1 | 8 | 0 |
| 41 | 0 |
| n1 | 0 |

### 5.209.4 Reference sensitivity exceptions

As mentioned above, IMD of B8 and n1 to Band41 Rx and IMD of B41 and n1 to Band8 Rx need to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.209.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA/NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | Duplex mode | IMD order |
| DC\_8A-41A\_n1A  DC\_8A-41C\_n1A | 41 | 2500 | 5 | 25 | 2500 | N/A | TDD | N/A |
| n1 | 1977 | 5 | 25 | 2167 | N/A | FDD | N/A |
| 8 | 886 | 5 | 25 | 931 | 4.5 | FDD | IMD5 |

## 5.210 DC\_n3\_1-8

### 5.210.1 Configuration for DC

**Table 5.210.1-1: Inter-band NE-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_n3A\_1A-8A | DC\_n3A\_1A  DC\_n3A-8A |

5.210.2 Co-existence study

Similar to DC\_1A-8A\_n3A, which can be found in TR 37.716-21-11 section 5.1.59.3

### 5.210.3 ∆TIB and ∆RIB values

Similar to DC\_1A-8A\_n3A, which can be found in TR 37.716-21-11 section 5.1.59.4

### 5.210.4 REFSENS requirements

Similar to DC\_1A-8A\_n3A, which can be found in TR 37.716-21-11 section 5.1.59.4

## 5.211 DC\_n77\_1-8

### 5.211.1 Configuration for DC

**Table 5.211.1-1: Inter-band NE-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_n77A\_1A-8A  DC\_n77(2A)\_1A-8A | DC\_n77A\_1A  DC\_n77A\_8A |

5.211.2 Co-existence study

Similar to DC\_1A-8A\_n77A, which can be found in TR 37.716-21-11 section 5.1.15.3

### 5.211.3 ∆TIB and ∆RIB values

Similar to DC\_1A-8A\_n77A, which can be found in TR 37.716-21-11 section 5.1.15.4

### 5.211.4 REFSENS requirements

Similar to DC\_1A-8A\_n77A, which can be found in TR 37.716-21-11 section 5.1.15.5

## 5.212 DC\_n77\_3-1

### 5.212.1 Configuration for DC

**Table 5.212.1-1: Inter-band NE-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_n77A\_3A-1A | DC\_n77A\_1A DC\_n77A\_3A |

5.212.2 Co-existence study

Similar to DC\_1A\_n3A-n77A. Which can be found in TR 37.717-01-21 section 6.13.3

### 5.212.3 ∆TIB and ∆RIB values

Similar to DC\_1A\_n3A-n77A. Which can be found in TR 37.717-01-21 section 6.13.4

### 5.212.4 REFSENS requirements

Similar to DC\_1A\_n3A-n77A. Which can be found in TR 37.717-01-21 section 6.13.5

## 5.213 DC\_n77\_3-8

### 5.213.1 Configuration for DC

**Table 5.213.1-1: Inter-band NE-DC configurations (three bands)**

| DC configuration | Uplink configuration  (NOTE 1) |
| --- | --- |
| DC\_n77A\_3A-8A  DC\_n77(2A)\_3A-8A | DC\_n77A\_3A  DC\_n77A\_8A |

5.213.2 Co-existence study

Similar to DC\_3A-8A\_n77A, which can be found in TR 37.716-21-11 section 5.1.10.3

### 5.213.3 ∆TIB and ∆RIB values

Similar to DC\_3A-8A\_n77A, which can be found in TR 37.716-21-11 section 5.1.10.4

### 5.213.4 REFSENS requirements

Similar to DC\_3A-8A\_n77A, which can be found in TR 37.716-21-11 section 5.1.1.4

## 5.214 DC\_1-38\_n78

### 5.214.1 Configurations for DC

Table 5.214.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink EN-DC configuration | Uplink E-UTRA configuration | Uplink NR configuration |
| --- | --- | --- | --- |
| DC\_1A-38A\_n78A | DC\_1A\_n78A | CA\_1A-38A | n78A |

### 5.214.2 Co-existence studies

Co-existence analysis for DC\_1\_n78 UL in TR 37.863-01-01 shows IMD4 produce may fall into LTE Band 38 DL.

### 5.214.3 ∆TIB and ∆RIB values

For DC\_1-38\_n78, same ΔTIB,c and ΔRIB,c values of DC\_1\_n38-n78 are reused which are given in the tables below.

Table 5.214.3-1: ΔTIB,c

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔTIB,c [dB]** |
| --- | --- | --- |
| DC\_1-38\_n78 | 1 | 0.5 |
| 38 | 0.5 |
| n78 | 0.8 |

**Table 5.214.3-2: ΔRIB,c**

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔRIB,c [dB]** |
| --- | --- | --- |
| DC\_1-38\_n78 | 1 | 0 |
| 38 | 0 |
| n78 | 0.5 |

### 5.214.4 Reference sensitivity exceptions

Based on co-existence studies additional MSD is needed to be defined. The MSD value is given in table 6.x.5-1, where same MSD values as DC\_1\_n38-n78 with UL configuration of DC\_1\_n78 are reused .

Table 6.x.5-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC  Configuration | EUTRA or NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_1A-38A\_n78A | 1 | 1970 | 5 | 25 | 2160 | N/A | N/A |
|  | 38 | 2590 | 5 | 25 | 2590 | 12.7 | IMD4 |
|  | n78 | 3320 | 10 | 50 | 3320 | N/A | N/A |

## 5.215 DC\_7-38\_n78

### 5.215.1 Configurations for DC

Table 5.215.1-1: Inter-band DC configurations (three bands)

| DC configuration | Uplink EN-DC configuration | Uplink E-UTRA configuration | Uplink NR configuration |
| --- | --- | --- | --- |
| DC\_7A-38A\_n78A17,18 | N/A | N/A | n78A |
| NOTE 17: The combination is not used alone as fall back mode of other band combinations.  NOTE 18: Power imbalance between downlink carriers on Band 7 and Band 38 is assumed to be within 6dB. The power spectral density imbalance condition also applies for these carriers when applicable EN-DC configuration is a subset of a higher order EN-DC configuration. | | | |

### 5.215.2 Co-existence studies

No need to analysis the co-existence studies for this configuration.

### 5.215.3 ∆TIB and ∆RIB values

For DC\_7-38\_n78, same ΔTIB,c and ΔRIB,c values are given in the tables below.

Table 5.215.3-1: ΔTIB,c

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔTIB,c [dB]** |
| --- | --- | --- |
| DC\_7-38\_n78 | n78 | 0.8 |

**Table 5.215.3-2: ΔRIB,c**

| **Inter-band DC Configuration** | **E-UTRA and NR Band** | **ΔRIB,c [dB]** |
| --- | --- | --- |
| DC\_7-38\_n78 | 7 | 0 |
| 38 | 0 |
| n78 | 0.5 |

### 5.215.4 Reference sensitivity exceptions

There is no additional MSD requirement for this configuration.

5.216 DC\_2-38\_n78

### 5.216.1 Configuration for DC

Table 5.216.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-38A\_n78A | DC\_2A\_n78A  DC\_38A\_n78A | CA\_2A-38A | n78A |

5.216.2 Co-existence studies

For UE coexistence study of Band 2 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.216.2-1.

**Table 5.216.2-1: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Fx low | Fx high | Fy low | Fy high |
| UL Frequency [MHz] | 1850 | 1910 | 3300 | 3800 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 10300 | 11850 | 6600 | 7600 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 15450 | 17775 | 9900 | 11400 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 20600 | 23700 | 13200 | 15200 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 25750 | 29625 | 16500 | 19000 |
| Two tone 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1390 | 1950 | 5150 | 5710 |
| Two tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 100 | 520 | 4690 | 5750 |
| Two tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 7000 | 7620 | 8450 | 9510 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 1750 | 2430 | 7990 | 9550 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 3900 | 2780 | 10300 | 11420 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 8850 | 9530 | 11750 | 13310 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 13350 | 11290 | 4340 | 3600 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 7700 | 6080 | 870 | 2050 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 15050 | 17110 | 10700 | 11440 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 13600 | 15220 | 12150 | 13330 |

For UE coexistence study of Band 38 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.216.2-2.

**Table 5.216.2-2: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Fx low | Fx high | Fy low | Fy high |
| UL Frequency [MHz] | 2570 | 2620 | 3300 | 3800 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 10300 | 11850 | 6600 | 7600 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 15450 | 17775 | 9900 | 11400 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 20600 | 23700 | 13200 | 15200 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 25750 | 29625 | 16500 | 19000 |
| Two tone 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 680 | 1230 | 5870 | 6420 |
| Two tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 1340 | 1940 | 3980 | 5030 |
| Two tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 8440 | 9040 | 9170 | 10220 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 3910 | 4560 | 7280 | 8830 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 2460 | 1360 | 11740 | 12840 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 11010 | 11660 | 12470 | 14020 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 12630 | 10580 | 7180 | 6480 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 6260 | 4660 | 1260 | 110 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 15770 | 17820 | 13580 | 14280 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 15040 | 16640 | 14310 | 15460 |

The Rx impacts can be identified as below.

* No IMD products generated by DC\_2\_n78 uplink fall into own Rx of band 38.
* 3rd and 4th order IMD products generated by DC\_38\_n78 uplink may fall into own Rx of band 2.

5.216.3 ∆TIB and ∆RIB values

For DC\_2A-38A\_n78A, the ΔTIB,c and ΔRIB,c values are reused from DC\_2\_n38-n78 and are given in the tables below.

**Table 5.216.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-38\_n78 | 2 | 0.6 |
| 38 | 0.9 |
| n78 | 0.8 |

**Table 5.216.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-38\_n78 | 2 | 0.5 |
| 38 | 0.5 |
| n78 | 0.5 |

5.216.4 Reference sensitivity exceptions

UL band 38\_n78 might cause IMD3 and IMD4 into band 2 DL. MSD value is derived from similar combination.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-38A\_n78A | 2 | 1852.5 | 5 | 25 | 1932.5 | 16 | IMD39 |
| 38 | 2617.5 | 5 | 25 | 2617.5 | N/A | N/A |
| n78 | 3305 | 10 | 50 | 3305 | N/A | N/A |
| NOTE 9: This band is subject to IMD4 also which MSD is not specified. | | | | | | | |

5.217 DC\_2-28\_n78

### 5.217.1 Configuration for DC

Table 5.217.1-1: Inter-band EN-DC configurations (three bands)

| EN-DC  Configuration | Uplink EN-DC  configuration  (NOTE 1) | E-UTRA CA configuration | NR band |
| --- | --- | --- | --- |
| DC\_2A-28A\_n78A | DC\_2A\_n78A  DC\_28A\_n78A | CA\_2A-28A | n78A |

5.217.2 Co-existence studies

For UE coexistence study of Band 2 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.217.2-1.

**Table 5.217.2-1: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Fx low | Fx high | Fy low | Fy high |
| UL Frequency [MHz] | 1850 | 1910 | 3300 | 3800 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 10300 | 11850 | 6600 | 7600 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 15450 | 17775 | 9900 | 11400 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 20600 | 23700 | 13200 | 15200 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 25750 | 29625 | 16500 | 19000 |
| Two tone 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 1390 | 1950 | 5150 | 5710 |
| Two tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 100 | 520 | 4690 | 5750 |
| Two tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 7000 | 7620 | 8450 | 9510 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 1750 | 2430 | 7990 | 9550 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 3900 | 2780 | 10300 | 11420 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 8850 | 9530 | 11750 | 13310 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 13350 | 11290 | 4340 | 3600 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 7700 | 6080 | 870 | 2050 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 15050 | 17110 | 10700 | 11440 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 13600 | 15220 | 12150 | 13330 |

For UE coexistence study of Band 28 + Band n78, the 2nd, 3rd, 4th and 5th order harmonics and 2nd, 3rd, 4th and 5th order intermodulation products were calculated and presented in Table 5.217.2-2.

**Table 5.217.2-2: Harmonic and IMD analysis**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Fx low | Fx high | Fy low | Fy high |
| UL Frequency [MHz] | 703 | 748 | 3300 | 3800 |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | 2\* fy\_low | 2\* fy\_high |
| 2nd harmonics frequency limits (MHz) | 10300 | 11850 | 6600 | 7600 |
| 3rd harmonics frequency limits | 3\*fx\_low | 3\*fx\_high | 3\* fy\_low | 3\* fy\_high |
| 3rd harmonics frequency limits (MHz) | 15450 | 17775 | 9900 | 11400 |
| 4th harmonics frequency limits | 4\*fx\_low | 4\*fx\_high | 4\* fy\_low | 4\* fy\_high |
| 4th harmonics frequency limits (MHz) | 20600 | 23700 | 13200 | 15200 |
| 5th harmonics frequency limits | 5\*fx\_low | 5\*fx\_high | 5\* fy\_low | 5\* fy\_high |
| 5th harmonics frequency limits (MHz) | 25750 | 29625 | 16500 | 19000 |
| Two tone 2nd order IMD products | |fy\_low – fx\_high| | |fy\_high – fx\_low| | |fy\_low + fx\_low| | |fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 2552 | 3097 | 4003 | 4548 |
| Two tone 3rd order IMD products | |2\*fx\_low – fy\_high| | |2\*fx\_high – fy\_low| | |2\*fy\_low – fx\_high| | |2\*fy\_high – fx\_low| |
| IMD frequency limits (MHz) | 2394 | 703 | 5852 | 6897 |
| Two tone 3rd order IMD products | |2\*fx\_low + fy\_low| | |2\*fx\_high + fy\_high| | |2\*fy\_low + fx\_low| | |2\*fy\_high + fx\_high| |
| IMD frequency limits (MHz) | 4706 | 5296 | 7303 | 8348 |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fy\_high| | |3\*fx\_high – 1\*fy\_low| | |3\*fy\_low – 1\*fx\_high| | |3\*fy\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 1691 | 1056 | 9152 | 10697 |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fy\_high| | |2\*fx\_high –2\* fy\_low| | |2\*fx\_low +2\* fy\_low| | |2\*fx\_high +2\* fy\_high| |
| IMD frequency limits (MHz) | 6194 | 5104 | 8006 | 9096 |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fy\_low| | |3\*fx\_high + 1\*fy\_high| | |3\*fy\_low + 1\*fx\_low| | |3\*fy\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 5409 | 6044 | 10603 | 12148 |
| Two-tone 5th order IMD products | |fx\_low – 4\*fy\_high| | |fx\_high – 4\*fy\_low| | |fy\_low – 4\*fx\_high| | |fy\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 14497 | 12452 | 308 | 988 |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fy\_high| | |2\*fx\_high - 3\*fy\_low| | |2\*fy\_low - 3\*fx\_high| | |2\*fy\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 9994 | 8404 | 4356 | 5491 |
| Two-tone 5th order IMD products | |fx\_low + 4\*fy\_low| | |fx\_high + 4\*fy\_high| | |fy\_low + 4\*fx\_low| | |fy\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 13903 | 15948 | 6112 | 6792 |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fy\_low| | |2\*fx\_high + 3\*fy\_high| | |2\*fy\_low + 3\*fx\_low| | |2\*fy\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 11306 | 12896 | 8709 | 9844 |

The Rx impacts can be identified as below.

* No IMD products generated by DC\_2\_n78 uplink fall into own Rx of band 28.
* 3rd order IMD products generated by DC\_28\_n78 uplink may fall into own Rx of band 2.

5.217.3 ∆TIB and ∆RIB values

For DC\_2A-28A\_n78A, the ΔTIB,c and ΔRIB,c values are reused from DC\_28\_n78 and DC\_2\_n78 and are given in the tables below.

**Table 5.217.3-1: ΔTIB,c**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_2-28\_n78 | 2 | 0.6 |
| 28 | 0.5 |
| n78 | 0.8 |

**Table 5.217.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_2-28\_n78 | 2 | 0.2 |
| 28 | 0.2 |
| n78 | 0.5 |

5.217.4 Reference sensitivity exceptions

UL band 28\_n78 might cause IMD3 into band 2 DL. MSD value is derived from similar combination.

Table 7.3B.2.3.5.2-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| **NR or E-UTRA Band / Channel bandwidth / NRB / MSD** | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **EN-DC Configuration** | **EUTRA / NR band** | **UL Fc  (MHz)** | **UL/DL BW  (MHz)** | **UL**  **LCRB** | **DL Fc (MHz)** | **MSD  (dB)** | **IMD order** |
| DC\_2A-28A\_n78A | 2 | 1904 | 5 | 25 | 1984 | 16.5 | IMD3 |
| 28 | 708 | 5 | 25 | 763 | N/A | N/A |
| n78 | 3400 | 10 | 50 | 3400 | N/A | N/A |

## 5.218 DC\_8-32\_n3

### 5.218.1 Configurations for DC

Table 5.218.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-32A\_n3A | DC\_8A\_n3A |

### 5.218.2 Co-existence studies

Table 5.218.2-1 lists the Band 8A + Band n3A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.218.2-1: Band 8 and Band n3 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 880 | 915 | | 1710 | 1785 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1760 – 1830 | | | 3420 – 3570 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2640 – 2745 | | | 5130 – 5355 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 795 – 905 | | | 2590 – 2700 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 25 – 120 | | | 2505 – 2690 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3470 – 3615 | | | 4300 – 4485 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 850 – 945 | | | 1700 – 1795 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 855 – 1035 | | | 4215 – 4475 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1590 – 1810 | | | 5180 – 5400 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4350 – 4530 | | | 6010 – 6270 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5925 – 6260 | | | 1735 – 1950 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3300 – 3595 | | | 675 – 930 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 7720 – 8055 | | | 5230 – 5445 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 6890 – 7185 | | | 6060 – 6315 | | |

Based on Table 5.218.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 3 and 46.

- 3rd order harmonics may fall into Rx frequencies of band 7, 22, 41, 42, 48, 49, 77, 78 and 90

- 2nd order IMD may fall into Rx frequencies of bands 5, 6, 7, 18, 19, 20, 26, 27, 28, 38, 41, 44, 69 and 90

- 3rd order IMD may fall into Rx frequencies of bands 7, 22, 38, 41, 42, 43, 48, 49, 69, 77, 78, 79 and 90

- 4th order IMD may fall into Rx frequencies of bands 3, 5, 6, 8, 18, 19, 26, 27, 46 and 79

- 5th order IMD may fall into Rx frequencies of bands 2, 3, 5, 6, 8, 9, 12, 13, 14, 17, 18, 19, 20, 22, 25, 26, 27, 28, 29, 33, 35, 36, 37, 39, 42, 44, 46, 48, 49, 52, 67, 68, 77, 78 and 85

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.218.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.218.2-2: 2UL Band 8 + Band n3 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD4 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD4 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD4 |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | 2nd Harmonic |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 2nd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_8\_n3 in 38.101-3.

### 5.218.3 ∆TIB and ∆RIB values

Table 5.218.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8A-32A\_n3 | 8 | 0.3 |
| n3 | 0.8 |

**Table 5.218.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8A-32A\_n3 | 8 | 0 |
| 32 | 0.5 |
| n3 | 0.3 |

### 5.218.4 Reference sensitivity exceptions

The following MSD (obtained from values used for n8 and 3 in 38.101-3) is proposed for the band 8 2nd harmonic hit in band 3:

Table 5.218.4-1: Reference sensitivity exceptions (MSD) due to UL harmonic for EN-DC in NR FR1

| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| UL band | DL band | 5 MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 30 MHz (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 70 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| 8 | n314 | N/A | N/A | N/A | N/A |  |  |  |  |  |  |  |  |  |
| NOTE 14: No requirements apply when there is at least one individual RE within the uplink transmission bandwidth of the low band for which the 2nd transmitter harmonic is within the downlink transmission bandwidth of the high band. The reference sensitivity for all active downlink component carriers is only verified when this is not the case (the requirements specified in clause 7.3.1 from TS 36.101-1 apply unless otherwise specified). | | | | | | | | | | | | | | |

## 5.219 DC\_8-38\_n1

### 5.219.1 Configurations for DC

Table 5.219.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-38A\_n1A | DC\_8A\_n1A  DC\_38A\_n1A |

### 5.219.2 Co-existence studies

Table 5.219.2-1 lists the Band 8A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.219.2-1: Band 8 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 880 | 915 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1760 – 1830 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2640 – 2745 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1005 – 1100 | | | 2800 – 2895 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 90 – 220 | | | 2925 – 3080 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3680 – 3810 | | | 4720 – 4875 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 830 – 965 | | | 1910 – 1990 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 660 – 825 | | | 4845 – 5060 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 2010 – 2200 | | | 5600 – 5790 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4560 – 4725 | | | 6640 – 6855 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6765 – 7040 | | | 1540 – 1740 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 3930 – 4180 | | | 1095 – 1320 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8560 – 8835 | | | 5440 – 5640 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7520 – 7770 | | | 6480 – 6705 | | |

Based on Table 5.219.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 3, 46 and 47.

- 3rd order harmonics may fall into Rx frequencies of band 7, 41, 77 and 90.

- 3rd order IMD may fall into Rx frequencies of bands 43, 48, 49, 77, 78 and 79.

- 4th order IMD may fall into Rx frequencies of bands 1, 4, 10, 12, 13, 14, 17, 20, 23, 28, 29, 34, 44, 46, 65, 66, 67, 68, 70, 79 and 85.

- 5th order IMD may fall into Rx frequencies of bands 24, 46 and 77.

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.219.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.219.2-2: 2UL Band 8 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | Yes |  | IMD5 |
| Galileo | 1559 | - | 1591 | Yes |  | IMD5 |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD5 |
| GPS | 1563 | - | 1587 | Yes |  | IMD5 |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | No | Europe |  |
| 5470 | - | 5725 | Yes | IMD4, IMD5 |
| 5150 | - | 5825 | Yes | Asia | 2nd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_8\_n1 in 38.101-3.

Table 5.219.2-3 lists the Band 38A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.219.2-3: Band 38 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2570 | 2620 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5140 – 5240 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7710 – 7860 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 590 – 700 | | | 4490 – 4600 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 3160 – 3320 | | | 1220 – 1390 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 7060 – 7220 | | | 6410 – 6580 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2520 – 2670 | | | 1900 – 2000 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5730 – 5940 | | | 3140 – 3370 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1180 – 1400 | | | 8980 – 9200 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 9630 – 9840 | | | 8330 – 8560 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5060 – 5350 | | | 8300 – 8560 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 520 – 800 | | | 3750 – 4020 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 10250 – 10540 | | | 12200 – 12460 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10900 – 11180 | | | 11550 – 11820 | | |

Based on Table 5.219.2-3,

- 2nd order harmonics may fall into Rx frequencies of bands 46 and 47.

- 3rd order harmonics may fall into Rx frequencies of band 77.

- 2nd order IMD may fall into Rx frequencies of bands 71 and 79.

- 3rd order IMD may fall into Rx frequencies of bands 52, 77 and 78.

- 4th order IMD may fall into Rx frequencies of bands 46, 47, 52, 77 and 78.

- 5th order IMD may fall into Rx frequencies of bands 12, 13, 14, 17, 20, 28, 29, 43, 44, 46, 67, 68, 71, 77, 78 and 85

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.219.2-4 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.219.2-4: 2UL Band 38 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | 2nd Harmonic, IMD5 |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 2nd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_38\_n1 in 38.101-3.

### 5.219.3 ∆TIB and ∆RIB values

Table 5.219.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_8A-38A\_n1 | 8 | 0.3 |
| 38 | 0.5 |
| n1 | 0.5 |

**Table 5.219.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_8A-38A\_n1 | 8 | 0 |
| 38 | 0 |
| n1 | 0 |

### 5.219.4 Reference sensitivity exceptions

## No additional exceptions compared to fallbacks.5.220 DC\_28-38\_n1

### 5.220.1 Configurations for DC

Table 5.220.1-1: Inter-band DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_28A-38A\_n1A | DC\_28A\_n1A  DC\_38A\_n1A |

### 5.220.2 Co-existence studies

Table 5.220.2-1 lists the Band 28A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.220.2-1: Band 28 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 703 | 748 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 1406 – 1496 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 2109 – 2244 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 1172 – 1277 | | | 2623 – 2728 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 424 – 574 | | | 3092 – 3257 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 3326 – 3476 | | | 4543 – 4708 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 653 – 798 | | | 1900 – 2000 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 129 – 324 | | | 5012 – 5237 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 2344 – 2554 | | | 5246 – 5456 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 4029 – 4224 | | | 6463 – 6688 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 6932 – 7217 | | | 832 – 1072 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 4264 – 4534 | | | 1596 – 1851 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 8383 – 8668 | | | 4732 – 4972 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 7166 – 7436 | | | 5949 – 6204 | | |

Based on Table 5.220.2-1,

- 2nd order harmonics may fall into Rx frequencies of bands 11, 21, 32, 45, 46, 47, 50, 51, 74, 75, 76, 91, 92, 93 and 94.

- 3rd order harmonics may fall into Rx frequencies of band 1, 4, 10, 23, 65, 66 and 77.

- 2nd order IMD may fall into Rx frequencies of bands 7, 41 and 90

- 3rd order IMD may fall into Rx frequencies of bands 31, 42, 52, 72, 73, 77, 78, 79, 87 and 88.

- 4th order IMD may fall into Rx frequencies of bands 30, 40, 41, 46, 53, 77 and 90.

- 5th order IMD may fall into Rx frequencies of bands 3, 5, 6, 8, 9, 18, 19, 26, 27, 35 and 79.

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.220.2-2 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.220.2-2: 2UL Band 28 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | Yes |  | IMD5 |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | Yes | US/Europe | IMD4 |
| 2400 | - | 2494 | Yes | Asia | IMD4 |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd Harmonic, IMD4 |
| 5150 | - | 5350 | Yes | Europe | IMD4 |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 2nd Harmonic, IMD4 |

The requirements for spurious emission band UE coexistence exist for DC\_28\_n1 in 38.101-3.

Table 5.220.2-3 lists the Band 38A + Band n1A 2UL DC 2nd and 3rd order harmonics and 2nd, 3rd, 4th and 5th order IMD for the UE-to-UE coexistence analysis.

Table 5.220.2-3: Band 38 and Band n1 UL harmonics and IMD products

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **UE UL carriers** | **fx\_low** | **fx\_high** | | **fn\_low** | **fn\_high** | |
| UL frequency (MHz) | 2570 | 2620 | | 1920 | 1980 | |
| 2nd harmonics frequency limits | 2\*fx\_low | 2\*fx\_high | | 2\* fn\_low | 2\* fn\_high | |
| 2nd harmonics frequency limits (MHz) | 5140 – 5240 | | | 3840 – 3960 | | |
| 3rd harmonics frequency limits | 3\*fx\_low | | 3\*fx\_high | 3\* fn\_low | | 3\* fn\_high |
| 3rd harmonics frequency limits (MHz) | 7710 – 7860 | | | 5760 – 5940 | | |
| 2nd order IMD products | |fn\_low – fx\_high| | |fn\_high – fx\_low| | | |fn\_low + fx\_low| | |fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 590 – 700 | | | 4490 – 4600 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low – fn\_high| | |2\*fx\_high – fn\_low| | | |2\*fn\_low – fx\_high| | |2\*fn\_high – fx\_low| | |
| IMD frequency limits (MHz) | 3160 – 3320 | | | 1220 – 1390 | | |
| Two-tone 3rd order IMD products | |2\*fx\_low + fn\_low| | |2\*fx\_high + fn\_high| | | |2\*fn\_low + fx\_low| | |2\*fn\_high + fx\_high| | |
| IMD frequency limits (MHz) | 7060 – 7220 | | | 6410 – 6580 | | |
| Two-tone 3rd order IMD products | (fx\_low – max BW fn) | | (fx\_high + max BW fn) | (fn\_low – max BW fx) | | (fn\_high + max BW fx) |
| IMD frequency limits (MHz) | 2520 – 2670 | | | 1900 – 2000 | | |
| Two-tone 4th order IMD products | |3\*fx\_low –1\* fn\_high| | | |3\*fx\_high – 1\*fn\_low| | |3\*fn\_low – 1\*fx\_high| | | |3\*fn\_high – 1\*fx\_low| |
| IMD frequency limits (MHz) | 5730 – 5940 | | | 3140 – 3370 | | |
| Two-tone 4th order IMD products | |2\*fx\_low –2\* fn\_high| | | |2\*fx\_high –2\* fn\_low| | |2\*fx\_low +2\* fn\_low| | | |2\*fx\_high +2\* fn\_high| |
| IMD frequency limits (MHz) | 1180 – 1400 | | | 8980 – 9200 | | |
| Two-tone 4th order IMD products | |3\*fx\_low +1\* fn\_low| | | |3\*fx\_high + 1\*fn\_high| | |3\*fn\_low + 1\*fx\_low| | | |3\*fn\_high + 1\*fx\_high| |
| IMD frequency limits (MHz) | 9630 – 9840 | | | 8330 – 8560 | | |
| Two-tone 5th order IMD products | |fx\_low – 4\*fn\_high| | | |fx\_high – 4\*fn\_low| | |fn\_low – 4\*fx\_high| | | |fn\_high – 4\*fx\_low| |
| IMD frequency limits (MHz) | 5060 – 5350 | | | 8300 – 8560 | | |
| Two-tone 5th order IMD products | |2\*fx\_low - 3\*fn\_high| | | |2\*fx\_high - 3\*fn\_low| | |2\*fn\_low - 3\*fx\_high| | | |2\*fn\_high -3\*fx\_low| |
| IMD frequency limits (MHz) | 520 – 800 | | | 3750 – 4020 | | |
| Two-tone 5th order IMD products | |fx\_low + 4\*fn\_low| | | |fx\_high + 4\*fn\_high| | |fn\_low + 4\*fx\_low| | | |fn\_high + 4\*fx\_high| |
| IMD frequency limits (MHz) | 10250 – 10540 | | | 12200 – 12460 | | |
| Two-tone 5th order IMD products | |2\*fx\_low + 3\*fn\_low| | | |2\*fx\_high + 3\*fn\_high| | |2\*fn\_low + 3\*fx\_low| | | |2\*fn\_high + 3\*fx\_high| |
| IMD frequency limits (MHz) | 10900 – 11180 | | | 11550 – 11820 | | |

Based on Table 5.220.2-3,

- 2nd order harmonics may fall into Rx frequencies of bands 46 and 47.

- 3rd order harmonics may fall into Rx frequencies of band 77.

- 2nd order IMD may fall into Rx frequencies of bands 71 and 79.

- 3rd order IMD may fall into Rx frequencies of bands 52, 77 and 78.

- 4th order IMD may fall into Rx frequencies of bands 46, 47, 52, 77 and 78.

- 5th order IMD may fall into Rx frequencies of bands 12, 13, 14, 17, 20, 28, 29, 43, 44, 46, 67, 68, 71, 77, 78 and 85

When a 2UL inter-band DC UE is operating with other systems such as Wi-Fi, Bluetooth and GNSS, the harmonics and intermodulation products can have an impact on these systems. Table 5.220.2-4 lists if up to 3rd order harmonics and IMD up to 5th order falls into one of these receiving bands.

Table 5.220.2-4: 2UL Band 38 + Band n1 harmonic and IMD for ISM and GNSS bands

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Victim Systems** | **Frequency range [MHz]** | | | **Impact** | **Regions** | **Comments** |
| COMPASS  (Beidou) | 1559 | - | 1591 | No |  |  |
| Galileo | 1559 | - | 1591 | No |  |  |
| GLONASS | 1591 | - | 1610 | No |  |  |
| GPS | 1563 | - | 1587 | No |  |  |
| ISM band  (2.4GHz) | 2400 | - | 2483.5 | No | US/Europe |  |
| 2400 | - | 2494 | No | Asia |  |
| ISM band  (5GHz) | 5150 | - | 5925 | Yes | US | 2nd Harmonic, IMD4, IMD5 |
| 5150 | - | 5350 | Yes | Europe | 2nd Harmonic, IMD5 |
| 5470 | - | 5725 | No |  |
| 5150 | - | 5825 | Yes | Asia | 2nd Harmonic, IMD4, IMD5 |

The requirements for spurious emission band UE coexistence exist for DC\_38\_n1 in 38.101-3.

### 5.220.3 ∆TIB and ∆RIB values

Table 5.220.3-1: ΔTIB,c

| Inter-band DC Configuration | E-UTRA and NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| DC\_28A-38A\_n1 | 28 | 0.6 |
| 38 | 0.5 |
| n1 | 0.5 |

**Table 5.220.3-2: ΔRIB**

| Inter-band DC Configuration | E-UTRA and NR Band | ΔRIB [dB] |
| --- | --- | --- |
| DC\_28A-38A\_n1 | 28 | 0.2 |
| 38 | 0 |
| n1 | 0 |

### 5.220.4 Reference sensitivity exceptions

The following MSD test point (based on DC\_1A\_n28A-n41A) is proposed for the band 20 IMD5 hit from 38A\_n1A uplink:Table 5.220.4-1: MSD test points for Scell due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA / NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | IMD order |
| DC\_28A-38A\_n1A | n1 | 1975 | 5 | 25 | 2165 | N/A | N/A |
|  | 28 | 720 | 5 | 25 | 775 | 4.5 | IMD5 |
|  | 38 | 2575 | 5 | 25 | 2575 | N/A | N/A |

## 5.221 DC\_8-11\_n1

### 5.221.1 Configurations for DC\_8-11\_n1

Table 5.221.1-1: Inter-band EN-DC configurations (three bands)

| DC  configuration | Uplink configuration |
| --- | --- |
| DC\_8A-11A\_n1A | DC\_8A\_n1A  DC\_11A\_n1A |

### 5.221.2 Co-existence studies

### 5.221.3 ∆TIB and ∆RIB values

The following relaxation values are proposed:

Table 5.221.3-1: ΔTIB,c

| Inter-band EN-DC configuration | E-UTRA or NR Band | ΔTIB,c (dB) |
| --- | --- | --- |
| DC\_8-11\_n1 | 8 | 0.3 |
| 11 | 0.4 |
| n1 | 0.3 |

Table 5.221.3-2: ΔRIB

|  |  |  |
| --- | --- | --- |
| Inter-band EN-DC configuration | NR Band | ΔRIB,c (dB) |
| DC\_8-11\_n1 | 8 | 0 |
| 11 | 0 |
| n1 | 0 |

### 5.221.4 Reference sensitivity exceptions

As mentioned above, IMD of B11 and n1 to Band8 Rx need to be addressed for REFSENS relaxation. The following values are proposed:

Table 5.221.4-1: Reference sensitivity exceptions due to dual uplink operation for EN-DC in NR FR1 (three bands)

| NR or E-UTRA Band / Channel bandwidth / NRB / MSD | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| EN-DC Configuration | EUTRA/NR band | UL Fc  (MHz) | UL/DL BW  (MHz) | UL  LCRB | DL Fc (MHz) | MSD  (dB) | Duplex mode | IMD order |
| DC\_8A-11A\_n1A | 11 | 1435 | 5 | 25 | 1483 | N/A | FDD | N/A |
| n1 | 1940 | 5 | 25 | 2130 | N/A | FDD | N/A |
| 8 | 885 | 5 | 25 | 930 | 16.6 | FDD | IMD35 |
| NOTE 5: This band is subject to IMD4 also which MSD is not specified. | | | | | | | | |

Annex A (informative):  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Change history** | | | | | | | |
| **Date** | **Meeting** | **TDoc** | **CR** | **Rev** | **Cat** | **Subject/Comment** | **New version** |
| 2020-8 | 3GPP RAN4#96-e |  |  |  |  | TR skeleton | 0.0.1 |
| 2020-8 | 3GPP RAN4#96-e | R4-2011889 |  |  |  | The following approved TPs at RAN4#96-e have been implemented:  R4-2011584 TP for TR 37.717-21-11: DC\_1-32\_n28  R4-2011585 TP for TR 37.717-21-11: DC\_7-32\_n28  R4-2009716 TP for TR 37.717-21-11: DC\_7-32\_n78  R4-2011586 TP for TR 37.717-21-11: DC\_20-32\_n28  R4-2010232 TP for TR 37.717.21-11: DC\_2A-48A\_n5A  R4-2010233 TP for TR 37.717.21-11: DC\_5A-48A\_n12A  R4-2010234 TP for TR 37.717.21-11: DC\_5A-48A\_n71A  R4-2010235 TP for TR 37.717.21-11: DC\_12A-48A\_n5A  R4-2010245 TP for TR 37.717-21-11 DC\_3A\_(n)41AA  R4-2011605 TP for 37.717-21-11 to introduce DC\_2A-48A\_n48A  R4-2011607 TP for 37.717-21-11 to introduce DC\_48-66A\_n25A  R4-2010410 TP for 37.717-21-11 to introduce DC\_48A-66A\_n48A  R4-2011608 TP for 37.717-21-11 to introduce DC\_3A-8A\_n40A  R4-2011609 TP for 37.717-21-11 to introduce DC\_3A-28A\_n1A  R4-2010421 TP for 37.717-21-11 to introduce DC\_7A-8A\_n40A  R4-2011610 TP for 37.717-21-11 to introduce DC\_7A-28A\_n1A  R4-2010439 TP for DC\_3-19\_n1 for TR 37.717-21-11  R4-2011612 TP for DC\_3-21\_n1 for TR 37.717-21-11  R4-2010453 TP for DC\_3-42\_n1 for TR 37.717-21-11  R4-2010454 TP for DC\_19-21\_n1 for TR 37.717-21-11  R4-2011613 TP for DC\_19-42\_n1 for TR 37.717-21-11  R4-2011614 TP for DC\_21-42\_n1 for TR 37.717-21-11  R4-2011616 TP for TR 37.717-21-11: DC\_7-66\_n5  R4-2010513 TP for TR 37.717-21-11: DC\_2-7\_n5  R4-2010556 TP to TR 37.717-21-11 DC\_1A-40A\_n78A  R4-2010557 TP to TR 37.717-21-11 DC\_3A-40A\_n78A  R4-2010558 TP to TR 37.717-21-11 DC\_7A-40A\_n78A  R4-2011618 TP to TR 37.717-21-11 DC\_8A-40A\_n78A  R4-2011620 TP for TR 37.717-21-11 to include DC\_2A-12A\_n5A  R4-2011621 TP for TR 37.717-21-11 to include DC\_2A-5A\_n12A  R4-2010699 TP for TR 37.717-21-11 to include DC\_5A-66A\_n12A  R4-2010700 TP for TR 37.717-21-11 to include DC\_66A\_(n)5AA  R4-2010701 TP for TR 37.717-21-11 to include DC\_12A-66A\_n5A  R4-2010883 TP for TR 37.717-21-11: DC\_7A-8A\_n28A  R4-2010884 TP for TR 37.717-21-11: DC\_20A-28A\_n3A  R4-2010885 TP for TR 37.717-21-11: DC\_28A-66A\_n66A  R4-2010886 TP for TR 37.717-21-11: DC\_7A-28A\_n66A / DC\_7C-28A\_n66A  R4-2010887 TP for TR 37.717-21-11: DC\_2A-28A\_n66A  R4-2010888 TP for TR 37.717-21-11: DC\_3A-28A\_n1A  R4-2010889 TP for TR 37.717-21-11: DC\_7A-28A\_n1A  R4-2010890 TP for TR 37.717-21-11: DC\_8A-40A\_n1A / DC\_8A-40C\_n1A  R4-2010894 TP for TR 37.717-21-11: DC\_1A-32A\_n3A  R4-2010895 TP for TR 37.717-21-11: DC\_3A-32A\_n1A  R4-2009924 TP for TR 37.717-21-11 for DC\_2A-4A\_n28A  R4-2009925 TP for TR 37.717-21-11 for DC\_2A-7A\_n28A  R4-2009926 TP for TR 37.717-21-11 for DC\_2A-66A\_n28A  R4-2009927 TP for TR 37.717-21-11 for DC\_4A-7A\_n28A  R4-2009928 TP for TR 37.717-21-11 for DC\_5-7\_n66  R4-2009929 TP for TR 37.717-21-11 for DC\_7A-66A\_n28A  R4-2009992 TP for TR 37.717-21-11: EN-DC\_1-11\_n28  R4-2009993 TP for TR 37.716-21-11: EN-DC\_3-11\_n28  R4-2009994 TP for TR 37.717-21-11: EN-DC\_8-11\_n28  R4-2011593 TP for TR 37.717-21-11: EN-DC\_3-11\_n77 | 0.1.0 |
| 2020-11 | 3GPP RAN4#97-e | R4-2015704 |  |  |  | The following approved TPs at RAN4#97-e have been implemented:  R4-2014056 TP for TR 37.717-21-11: DC\_7-32\_n78  R4-2014057 TP for TR 37.717-21-11: DC\_7-32\_n1  R4-2014031 TP for 37.717-21-11 for DC\_2-66\_n7  R4-2014032 TP for 37.717-21-11 for DC\_2-5\_n7  R4-2014033 TP for 37.717-21-11 for DC\_2-8\_n2  R4-2014034 TP for 37.717-21-11 for DC\_5-66\_n7  R4-2016656 TP for 37.717-21-11 for DC\_20-32\_n1  R4-2014036 TP for 37.717-21-11 for DC\_20-32\_n3  R4-2014103 TP for TR 37.717-21-11 DC\_1-3\_n3  R4-2014104 TP for TR 37.717-21-11 DC\_1-41\_n3  R4-2014105 TP for TR 37.717-21-11 DC\_3-18\_n3  R4-2014106 TP for TR 37.717-21-11 DC\_3-41\_n3  R4-2014128 TP for TR 37.717-21-11 DC\_5A-7A\_n66A  R4-2014129 TP for TR 37.717-21-11 DC\_7-66\_n77  R4-2014132 TP for TR 37.717-21-11 DC\_2-5\_n48  R4-2014133 TP for TR 37.717-21-11 DC\_2-13\_n48  R4-2014135 TP for TR 37.717-21-11 DC\_2-48\_n5  R4-2014136 TP for TR 37.717-21-11 DC\_5-46\_n66  R4-2014137 TP for TR 37.717-21-11 DC\_5-66\_n48  R4-2014138 TP for TR 37.717-21-11 DC\_5-66\_n77  R4-2014612 TP for TR 37.717-21-11: EN-DC\_1-42\_n3  R4-2014613 TP for TR 37.717-21-11: EN-DC\_8-42\_n3  R4-2016662 TP update for TR 37.717-21-11: EN-DC\_1-11\_n28  R4-2014811 TP for DC\_3-18\_n28  R4-2014852 TP for TR 37.717-21-11: CA\_2-66\_n77  R4-2014854 TP for TR 37.717-21-11: CA\_2-48\_n77  R4-2014856 TP for TR 37.717-21-11: CA\_2-13\_n77  R4-2014857 TP for TR 37.717-21-11: CA\_2-5\_n77  R4-2014858 TP for TR 37.717-21-11: CA\_5-13\_n66  R4-2014860 TP for TR 37.717-21-11: CA\_13-66\_n77  R4-2014862 TP for TR 37.717-21-11: CA\_13-66\_n5  R4-2016664 TP for DC\_1-18\_n28  R4-2016665 TP for DC\_1-18\_n41  R4-2014982 TP for DC\_3-42\_n1 for TR 37.717-21-11  R4-2016668 TP for 37.717-21-11 to introduce DC\_5A-7A\_n7A  R4-2015226 TP for 37.717-21-11 to introduce DC\_2A-28A\_n7A  R4-2016669 TP for 37.717-21-11 to introduce DC\_28A-66A\_n7A  R4-2015228 TP for 37.717-21-11 to introduce DC\_7A-28A\_n2A  R4-2015229 TP for 37.717-21-11 to introduce DC\_2A-7A\_n7A  R4-2015246 TP for 37.717-21-11 to introduce DC\_2A-71A\_n71A and DC\_66A-71A\_n71A  R4-2015268 TP to TR 37.717-21-11 DC\_1A-40C\_n78A  R4-2015269 TP to TR 37.717-21-11 DC\_3A-40C\_n78A  R4-2015270 TP to TR 37.717-21-11 DC\_7A-40C\_n78A  R4-2015271 TP to TR 37.717-21-11 DC\_8A-40C\_n78A  R4-2015404 TP for TR 37.717-21-11: DC\_7A-66A\_n7A/DC\_7A-66A-66A\_n7A  R4-2015710 TP for TR 37.717-21-11: DC\_2-7\_n77  R4-2015711 TP for TR 37.717-21-11: DC\_7-66\_n77 | 0.2.0 |
| 2021-02 | 3GPP RAN4#98-e | R4-2101508 |  |  |  | The following approved TPs at RAN4#98-e have been implemented:  R4-2103006 TP to TR 37.717-21-11: DC\_20-40\_n78  R4-2103010 TP for TR 37.717-21-11: DC\_3-18\_n41  R4-2103011 TP update for TR 37.717-21-11: EN-DC\_1-11\_n28  R4-2103014 TP to TR 37.717-21-11 DC\_7-25\_n77  R4-2103015 TP to TR 37.717-21-11 DC\_7-25\_n78  R4-2103016 TP to TR 37.717-21-11 DC\_25-66\_n77  R4-2103017 TP to TR 37.717-21-11 DC\_25-66\_n78  R4-2103018 TP for TR 37.717-21-11: DC\_2-29\_n78  R4-2103019 TP for TR 37.717-21-11: DC\_29-66\_n78  R4-2103022 TP for DC\_1-21\_n28 for TR 37.717-21-11  R4-2101231 TP for DC\_3-21\_n28 for TR 37.717-21-11  R4-2101511 TP for 37.717-21-11: correction of duplicated TPS for some combinations  R4-2103023 TP for TR 37.717-21-11: DC\_8-20\_n1  R4-2103024 TP for TR 37.717-21-11: DC\_8-20\_n3  R4-2101548 TP for TR 37.717-21-11: DC\_8-32\_n1  R4-2101913 TP for TR 37.717-21-11 to include 12A-66A\_n41A  R4-2101914 TP for TR 37.717-21-11 to include 2A-12A\_n41A, 2A-2A-12A\_n41A  R4-2101915 TP for TR 37.717-21-11 to include 66A-71A\_n41A  R4-2101916 TP for TR 37.717-21-11 to include 2A-71A\_n41A, 2A-2A-71A\_n41A  R4-2101917 TP for TR 37.717-21-11 to include 7A-12A\_n66A  R4-2101918 TP for TR 37.717-21-11 to include 7A-71A\_n66A  R4-2101919 TP for TR 37.717-21-11 to include 7A-12A\_n78A  R4-2101920 TP for TR 37.717-21-11 to include 12A-66A\_n78A  R4-2101921 TP for TR 37.717-21-11 to include 2A-12A\_78A, 2A-2A-12A\_78A  R4-2102050 TP for TR 37.717-21-11 to include 7A-71A\_n78A | 0.3.0 |
| 2021-04 | 3GPP RAN4#98-bis-e | R4-2106490 |  |  |  | The following approved TPs at RAN4#98-bis-e have been implemented:  R4-2104406 TP to TR 37.717-21-11: DC\_20-40\_n1  R4-2104411 TP to TR 37.717-21-11: DC\_5A-30A\_n2A  R4-2105293 TP to TR 37.717-21-11 DC\_2-46\_n77  R4-2105294 TP to TR 37.717-21-11 DC\_13-46\_n77  R4-2105295 TP to TR 37.717-21-11 DC\_46-66\_n77  R4-2105327 TP for TR 37.717-21-22: DC\_1-11\_n41  R4-2105306 TP for TR 37.717-21-11: DC\_2-12\_n7  R4-2106499 TP for TR 37.717-21-11: DC\_5A-7A-7A\_n66a  R4-2106500 TP for TR 37.717-21-11: DC\_2-5\_n78  R4-2106501 TP for TR 37.717-21-11: DC\_2A-12A\_n78(2A)  R4-2106502 TP for TR 37.717-21-11: DC\_7-29\_n78  R4-2106641 TP for TR 37.717-21-11: DC\_1A-38A\_n28A  R4-2106642 TP for TR 37.717-21-11: DC\_3A-38A\_n28A/ DC\_3C-38A\_n28A  R4-2105312 TP for TR 37.717-21-11 to include 14-30\_n66  R4-2106712 TP for TR 37.717-21-11 to include 14-30\_n2  R4-2106713 TP for TR 37.717-21-11 to include 2-(n)5  R4-2106714 TP for TR 37.717-21-11 to include 30-(n)5  R4-2105315 TP for TR 37.717-21-11 to include 28-40\_n78  R4-2106739 TP for TR 37.717-21-11 to include DC\_7-13\_n25  R4-2106740 TP for TR 37.717-21-11 to include DC\_7-66\_n25  R4-2106761 TP for TR 37.717-21-11 to include 3-7\_n3  R4-2106762 TP for TR 37.717-21-11 to include 3-28\_n3  R4-2106925 TP for TR 37.717-21-11: support of DC\_3-3-7\_n8, DC\_3-7-7\_n8, DC\_3-3-7-7\_n8  R4-2105319 TP to TR 37.717-21-11 Addition of DC\_13-46\_n66  R4-2105321 TP to TR 37.717-21-11 Addition of DC\_2-46\_n5  R4-2105322 TP to TR 37.717-21-11 Addition of DC\_46-48\_n5 | 0.4.0 |
| 2021-04 | 3GPP RAN4#99-e | R4-2110665 |  |  |  | The following approved TPs at RAN4#99-e have been implemented:  R4-2109463 TP update for TR 37.717-21-11: EN-DC\_1-11\_n41  R4-2110240 TP for TR 37.717-21-11: DC\_20A-28A\_n1A  R4-2110241 TP for TR 37.717-21-11: DC\_8A-20A\_n1A  R4-2107688 TP for TR 37.717-21-11: DC\_8A-20A\_n3A  The following approved TPs at RAN4#98-bis-e which are missing in v 0.4.0 have been implemented:  R4-2106737 TP for TR 37.717-21-11 to include 2-13\_n25  R4-2106738 TP for TR 37.717-21-11 to include 2-66\_n25 | 0.5.0 |
| 2021-08 | 3GPP RAN4#100-e | R4-2113051 |  |  |  | R4-2114794 TP for TR 37.717-21-11 Addition of DC\_2-12\_n77  R4-2114795 TP for TR 37.717-21-11 Addition of DC\_2-14\_n77  R4-2114796 TP for TR 37.717-21-11 Addition of DC\_2-29\_n77  R4-2114797 TP for TR 37.717-21-11 Addition of DC\_2-30\_n77  R4-2114798 TP for TR 37.717-21-11 Addition of DC\_5-30\_n77  R4-2111755 TP for TR 37.717-21-11 Addition of DC\_12-30\_n77  R4-2114799 TP for TR 37.717-21-11 Addition of DC\_12-66\_n77  R4-2114800 TP for TR 37.717-21-11 Addition of DC\_14-30\_n77  R4-2114801 TP for TR 37.717-21-11 Addition of DC\_14-66\_n77  R4-2114802 TP for TR 37.717-21-11 Addition of DC\_29-30\_n77  R4-2114803 TP for TR 37.717-21-11 Addition of DC\_29-66\_n77  R4-2114804 TP for TR 37.717-21-11 Addition of DC\_30-66\_n77  R4-2111784 TP to TR 37.717-21-11 DC\_2-5\_n30  R4-2111785 TP to TR 37.717-21-11 DC\_2-12\_n30  R4-2111786 TP to TR 37.717-21-11 DC\_2-14\_n30  R4-2111787 TP to TR 37.717-21-11 DC\_2-29\_n30  R4-2111788 TP to TR 37.717-21-11 DC\_2-66\_n30  R4-2111789 TP to TR 37.717-21-11 DC\_5-66\_n30  R4-2111790 TP to TR 37.717-21-11 DC\_12-66\_n30  R4-2111791 TP to TR 37.717-21-11 DC\_14-66\_n30  R4-2111792 TP to TR 37.717-21-11 DC\_29-66\_n30  R4-2114806 TP for TR 37.717-21-11 DC\_2-46\_n2  R4-2112447 TP for TR 37.717-21-11 DC\_2-48\_n2  R4-2114807 TP for TR 37.717-21-11 DC\_13-46\_n2  R4-2114808 TP for TR 37.717-21-11 DC\_13-48\_n77  R4-2112450 TP for TR 37.717-21-11 DC\_48-66\_n2  R4-2112451 TP for TR 37.717-21-11 DC\_48-66\_n66  R4-2114809 TP for TR 37.717-21-11 DC\_48-66\_n77  R4-2114811 TP for TR 37.717-21-11 DC\_1-5\_n77, DC\_1-7\_n77, DC\_3-5\_n77, DC\_3-7\_n77 and DC\_5-7\_n77  R4-2112929 TP for TR 37.717-21-11\_DC\_1A-7A\_n3A  R4-2112759 TP for TR 37.717-21-11 to include DC\_2-(n)66  R4-2112930 TP for TR 37.717-21-11\_DC\_1A-38A\_n3A  R4-2112931 TP for TR 37.717-21-11\_DC\_7A-38A\_n3A  R4-2112932 TP for TR 37.717-21-11\_DC\_20A-38A\_n3A  R4-2113347 TP for TR 37.717-21-11: DC\_1-32\_n8  R4-2113348 TP for TR 37.717-21-11: DC\_1-38\_n8  R4-2113371 TP for TR 37.717-21-11: DC\_7-32\_n3  R4-2114820 TP for TR 37.717-21-11: DC\_3A-32A\_n28A and DC\_3C-32A\_n28A  R4-2114821 TP for TR 37.717-21-11: DC\_28A-32A\_n1A  R4-2114822 TP for TR 37.717-21-11: DC\_28A-32A\_n3A  R4-2113393 TP for TR 37.717-21-11: DC\_7-32\_n8  R4-2113395 TP for TR 37.717-21-11: DC\_20-32\_n8  R4-2113396 TP for TR 37.717-21-11: DC\_20-38\_n1  R4-2113482 TP for TR 37.717-21-11: DC\_32-38\_n1  R4-2114151 TP to TR 37.717-21-11 for DC\_7-7-28-n1  R4-2114901 TP for TR 37.717-21-11: DC\_8A-20A\_n28A |  |
| 2021-08 | 3GPP RAN4#101-e | R4-2117897 |  |  |  | The following approved TPs at RAN4#101-e have been implemented:  R4-2119807 TP for TR 37.717-21-11: DC\_8A\_(n)3AA  R4-2117654 TP for TR 37.717-21-11: EN-DC\_1-11\_n79  R4-2117657 TP for TR 37.717-21-11: EN-DC\_8-11\_n79  R4-2119812 TP for TR 37.717-21-11: EN-DC\_8-41\_n3  R4-2119813 TP for TR 37.717-21-11: EN-DC\_8-42\_n1  R4-2119816 TP for TR 37.717-21-11: EN-DC\_8-41\_n77  R4-2117917 PC3 TP for TR 37.717-21-11 DC\_5-13\_n77  R4-2117918 PC3 TP for TR 37.717-21-11 DC\_5-48\_n77  R4-2118195 TP for TR 37.717-21-11: DC\_1A-7A\_n38A  R4-2118196 TP for TR 37.717-21-11: DC\_3A-7A\_n38A  R4-2118197 TP for TR 37.717-21-11: DC\_7A-20A\_n38A | 0.7.0 |
| 2022-03 | 3GPP RAN4#102-e | R4-2205165 |  |  |  | The following approved TPs at RAN4#101bis-e have been implemented:  R4-2200367 TP for TR 37.717-21-11 DC\_n3A\_1A-8A  R4-2200368 TP for TR 37.717-21-11: DC\_n77A\_1A-8A and DC\_n77(2A)\_1A-8A  R4-2200369 TP for TR 37.717-21-11 DC\_n77A\_3A\_1A  R4-2200370 TP for TR 37.717-21-11 DC\_n77A\_3A-8A and DC\_n77(2A)\_3A-8A  R4-2201356 TP for TR 37.717-21-11\_DC\_1A-38A\_n78A  R4-2201357 TP for TR 37.717-21-11\_DC\_7A-38A\_n78A  R4-2202005 TP update for TR 37.717-21-11: EN-DC\_1-11\_n79  R4-2202007 TP update for TR 37.717-21-11: EN-DC\_8-11\_n79  R4-2202166 TP for TR 37.717-21-11: EN-DC\_8-41\_n1  R4-2202168 TP to TR 37.717-21-11 Addition of DC\_2A-38A\_n78A  R4-2202169 TP to TR 37.717-21-11 Addition of DC\_2A-28A\_n78A  The following approved TPs at RAN4#102-e have been implemented:  R4-2203628 TP for TR 37.717-21-11: DC\_8-32\_n3  R4-2203629 TP for TR 37.717-21-11: DC\_8-38\_n1  R4-2206261 TP for TR 37.717-21-11: DC\_28-38\_n1  R4-2204554 TP for TR 37.717-21-11: EN-DC\_8-11\_n1  R4-2206269 Updated TP for TR 37.717-21-11: add MSD due to harmonic interference between band n28 and 32 | 0.8.0 |