**3GPP TSG-RAN WG4 Meeting #104-e R4-22xxxxx**

**Electronic Meeting, August 15th – 26th, 2022**

**Title:** WF on system parameters for 5G broadcast

**Agenda Item:** x.x.x

**Source: Qualcomm Incorporated**

**Document for:** Approval

# System parameters for 5G broadcast

**<Way forward/Agreement>**:

1. A new band type is needed for Standalone Downlink Only (SDO). No impact to RAN1 and RAN2 specifications is expected.
2. For BS, define new channel bandwidths 6, 7 and 8 MHz. FFS for the UE.
3. Maintain the 100 kHz channel raster.
4. 30, 35, and 40 RB’s is the maximum transmission bandwidth configuration for 15 kHz SCS in 6, 7, and 8 MHz channel bandwidths.