{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cover","Parameters","PUSCH requirement 4Rx","PUSCH requirement 8Rx"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":7,"n_cols":10,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #116bis",null,null,null,null,null,null,null,"R4-251xxxx"]
[null,"Prague, Czech Republic, 13th-17th, Nov, 2025"]
[]
[null,"Source: Ericsson"]
[null,"Title: Simulation results summary for 3Tx  BS demodulation requirement"]
[null,"Agenda: 6.12.3"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[6,2,6,4],[7,2,7,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PUSCH requirement 4Rx","index":2,"n_rows":61,"n_cols":21,"rows_kept":61,"cut":false,"hidden":false,"merged":[[59,1,60,1],[59,2,60,2],[59,3,60,3],[59,4,60,4],[59,6,60,6],[59,7,60,7],[59,8,60,8],[52,1,53,1],[52,2,53,2],[52,3,53,3],[52,4,53,4],[52,6,53,6],[52,7,53,7],[52,8,53,8],[55,1,56,1],[55,2,56,2],[55,3,56,3],[55,4,56,4],[55,6,56,6],[55,7,56,7],[55,8,56,8],[45,1,46,1],[45,2,46,2],[45,3,46,3],[45,4,46,4],[45,6,46,6],[45,7,46,7],[45,8,46,8],[49,1,50,1],[49,2,50,2],[49,3,50,3],[49,4,50,4],[49,6,50,6],[49,7,50,7],[49,8,50,8],[24,1,25,1],[24,2,25,2],[24,3,25,3],[24,4,25,4],[24,6,25,6],[24,7,25,7],[24,8,25,8],[28,1,29,1],[28,2,29,2],[28,3,29,3],[28,4,29,4],[28,6,29,6],[28,7,29,7],[28,8,29,8],[42,8,43,8],[39,8,40,8],[36,8,37,8],[33,8,34,8],[14,8,15,8],[11,8,12,8],[5,8,6,8],[2,8,3,8],[8,8,9,8],[18,8,19,8],[21,8,22,8],[0,17,0,18],[0,19,0,20],[31,11,31,12],[31,13,31,14],[31,15,31,16],[31,17,31,18],[31,19,31,20],[0,11,0,12],[0,13,0,14],[0,15,0,16],[2,1,3,1],[5,1,6,1],[11,1,12,1],[14,1,15,1],[33,1,34,1],[36,1,37,1],[39,1,40,1],[42,1,43,1],[2,2,3,2],[5,2,6,2],[11,2,12,2],[14,2,15,2],[33,2,34,2],[36,2,37,2],[39,2,40,2],[42,2,43,2],[8,1,9,1],[8,2,9,2],[18,1,19,1],[18,2,19,2],[21,1,22,1],[21,2,22,2],[2,3,3,3],[5,3,6,3],[11,3,12,3],[14,3,15,3],[33,3,34,3],[36,3,37,3],[39,3,40,3],[42,3,43,3],[2,4,3,4],[5,4,6,4],[11,4,12,4],[14,4,15,4],[33,4,34,4],[36,4,37,4],[39,4,40,4],[42,4,43,4],[8,3,9,3],[8,4,9,4],[18,3,19,3],[18,4,19,4],[21,3,22,3],[21,4,22,4],[18,6,19,6],[21,6,22,6],[21,7,22,7],[2,6,3,6],[5,6,6,6],[11,6,12,6],[14,6,15,6],[33,6,34,6],[36,6,37,6],[39,6,40,6],[42,6,43,6],[8,6,9,6],[2,7,3,7],[5,7,6,7],[11,7,12,7],[14,7,15,7],[33,7,34,7],[36,7,37,7],[39,7,40,7],[42,7,43,7],[8,7,9,7],[18,7,19,7]]}
["case ","Tx","SCS","Waveform","BW","Mapping Type","Propagation condition ","MCS","Additional DM-RS position","38.104 req","38.141-1/2 req","Samsung",null,"Nokia",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,3,"15kHz","CP-OFDM","5MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L3:Q3)","v":{"$error":"#NAME?"}},{"$f":"IF(J3>-100,J3+0.6,J3)","v":{"$error":"#NAME?"}},-1.4319999999999999,null,-2.78,null,-2.71,null,{"$f":"MAX(L3,N3,P3)-MIN(L3,N3,P3)","v":1.3479999999999999},{"$f":"MAX(M34,O34,Q34)","v":0},{"$f":"AVERAGE(L3,N3,P3)","v":-2.3073333333333332},{"$f":"AVERAGE(M3,O3,Q3)","v":{"$error":"#DIV/0!"}}]
[2,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L4:Q4)","v":{"$error":"#NAME?"}},{"$f":"IF(J4>-100,J4+0.6,J4)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,{"$f":"MAX(L4,N4,P4)-MIN(L4,N4,P4)","v":0},{"$f":"MAX(M35,O35,Q35)","v":0},{"$f":"AVERAGE(L4,N4,P4)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(M4,O4,Q4)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[3,3,"15kHz","CP-OFDM","5MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L6:Q6)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},13.593999999999999,null,8.76,null,12.76,null,4.8339999999999996,0,11.704666666666666,{"$error":"#DIV/0!"}]
[4,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L7:Q7)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[5,3,"15kHz","CP-OFDM","5MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L9:Q9)","v":{"$error":"#NAME?"}},{"$f":"IF(J9>-100,J9+0.6,J9)","v":{"$error":"#NAME?"}},15.016,null,11.43,null,14.29,null,3.5860000000000003,0,13.578666666666665,{"$error":"#DIV/0!"}]
[6,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L10:Q10)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[7,3,"15kHz","CP-OFDM","20MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L12:Q12)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},-1.413,null,-4.74,null,-2.72,null,3.327,0,-2.9576666666666669,{"$error":"#DIV/0!"}]
[8,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L13:Q13)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[9,3,"15kHz","CP-OFDM","20MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L15:Q15)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},13.835000000000001,null,6.41,null,12.75,null,7.4250000000000007,0,10.998333333333335,{"$error":"#DIV/0!"}]
[10,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L16:Q16)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L18:Q18)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[11,3,"15kHz","CP-OFDM","20MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L19:Q19)","v":{"$error":"#NAME?"}},{"$f":"IF(J19>-100,J19+0.6,J19)","v":{"$error":"#NAME?"}},15.679,null,10.61,null,14.28,null,5.0690000000000008,0,13.523000000000001,{"$error":"#DIV/0!"}]
[12,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L20:Q20)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[13,3,"15kHz","CP-OFDM","50MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L22:Q22)","v":{"$error":"#NAME?"}},{"$f":"IF(J22>-100,J22+0.6,J22)","v":{"$error":"#NAME?"}},-1.5209999999999999,null,-5.19,null,-2.7,null,3.6690000000000005,0,-3.1370000000000005,{"$error":"#DIV/0!"}]
[14,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L23:Q23)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[15,3,"15kHz","CP-OFDM","50MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L25:Q25)","v":{"$error":"#NAME?"}},{"$f":"IF(J25>-100,J25+0.6,J25)","v":{"$error":"#NAME?"}},14.7,null,6.06,null,12.75,null,8.64,0,11.17,{"$error":"#DIV/0!"}]
[16,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L26:Q26)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L28:Q28)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[17,3,"15kHz","CP-OFDM","50MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L29:Q29)","v":{"$error":"#NAME?"}},{"$f":"IF(J29>-100,J29+0.6,J29)","v":{"$error":"#NAME?"}},17.251999999999999,null,10.86,null,14.29,null,6.3919999999999995,0,14.134,{"$error":"#DIV/0!"}]
[18,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L30:Q30)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
["case ","Tx","SCS","Waveform","BW","Mapping Type","Propagation condition ","MCS","Additional DM-RS position","38.104 req","38.141-1/2 req","Samsung",null,"Nokia",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,3,"30kHz","CP-OFDM","10MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L34:Q34)","v":{"$error":"#NAME?"}},{"$f":"IF(J34>-100,J34+0.6,J34)","v":{"$error":"#NAME?"}},-1.669,null,null,null,null,null,{"$f":"MAX(L34,N34,P34)-MIN(L34,N34,P34)","v":0},{"$f":"MAX(M65,O65,Q65)","v":0},{"$f":"AVERAGE(L34,N34,P34)","v":-1.669},{"$f":"AVERAGE(M34,O34,Q34)","v":{"$error":"#DIV/0!"}}]
[2,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L35:Q35)","v":{"$error":"#NAME?"}},{"$f":"IF(J35>-100,J35+0.6,J35)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,{"$f":"MAX(L35,N35,P35)-MIN(L35,N35,P35)","v":0},{"$f":"MAX(M66,O66,Q66)","v":0},{"$f":"AVERAGE(L35,N35,P35)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(M35,O35,Q35)","v":{"$error":"#DIV/0!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[3,3,"30kHz","CP-OFDM","10MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L37:Q37)","v":{"$error":"#NAME?"}},{"$f":"IF(J37>-100,J37+0.6,J37)","v":{"$error":"#NAME?"}},13.712,null,null,null,null,null,0,0,13.712,{"$error":"#DIV/0!"}]
[4,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L38:Q38)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[5,3,"30kHz","CP-OFDM","10MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L40:Q40)","v":{"$error":"#NAME?"}},{"$f":"IF(J40>-100,J40+0.6,J40)","v":{"$error":"#NAME?"}},15.09,null,null,null,null,null,0,0,15.09,{"$error":"#DIV/0!"}]
[6,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L41:Q41)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[7,3,"30kHz","CP-OFDM","40MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L43:Q43)","v":{"$error":"#NAME?"}},{"$f":"IF(J43>-100,J43+0.6,J43)","v":{"$error":"#NAME?"}},-1.645,null,null,null,null,null,0,0,-1.645,{"$error":"#DIV/0!"}]
[8,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L44:Q44)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[9,3,"30kHz","CP-OFDM","40MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L46:Q46)","v":{"$error":"#NAME?"}},{"$f":"IF(J46>-100,J46+0.6,J46)","v":{"$error":"#NAME?"}},13.773,null,null,null,null,null,0,0,13.773,{"$error":"#DIV/0!"}]
[10,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L47:Q47)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L49:Q49)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[11,3,"30kHz","CP-OFDM","40MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L50:Q50)","v":{"$error":"#NAME?"}},{"$f":"IF(J50>-100,J50+0.6,J50)","v":{"$error":"#NAME?"}},15.82,null,null,null,null,null,0,0,15.82,{"$error":"#DIV/0!"}]
[12,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L51:Q51)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[13,3,"30kHz","CP-OFDM","100MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L53:Q53)","v":{"$error":"#NAME?"}},{"$f":"IF(J53>-100,J53+0.6,J53)","v":{"$error":"#NAME?"}},-1.724,null,null,null,null,null,0,0,-1.724,{"$error":"#DIV/0!"}]
[14,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L54:Q54)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[15,3,"30kHz","CP-OFDM","100MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L56:Q56)","v":{"$error":"#NAME?"}},{"$f":"IF(J56>-100,J56+0.6,J56)","v":{"$error":"#NAME?"}},14.371,null,null,null,null,null,0,0,14.371,{"$error":"#DIV/0!"}]
[16,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L57:Q57)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L59:Q59)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[17,3,"30kHz","CP-OFDM","100MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L60:Q60)","v":{"$error":"#NAME?"}},{"$f":"IF(J60>-100,J60+0.6,J60)","v":{"$error":"#NAME?"}},16.899999999999999,null,null,null,null,null,0,0,16.899999999999999,{"$error":"#DIV/0!"}]
[18,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L61:Q61)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]

{"sheet":"PUSCH requirement 8Rx","index":3,"n_rows":61,"n_cols":21,"rows_kept":61,"cut":false,"hidden":false,"merged":[[59,8,60,8],[59,1,60,1],[59,2,60,2],[59,3,60,3],[59,4,60,4],[59,6,60,6],[59,7,60,7],[52,8,53,8],[55,1,56,1],[55,2,56,2],[55,3,56,3],[55,4,56,4],[55,6,56,6],[55,7,56,7],[55,8,56,8],[52,1,53,1],[52,2,53,2],[52,3,53,3],[52,4,53,4],[52,6,53,6],[52,7,53,7],[45,8,46,8],[49,1,50,1],[49,2,50,2],[49,3,50,3],[49,4,50,4],[49,6,50,6],[49,7,50,7],[49,8,50,8],[45,1,46,1],[45,2,46,2],[45,3,46,3],[45,4,46,4],[45,6,46,6],[45,7,46,7],[39,8,40,8],[42,1,43,1],[42,2,43,2],[42,3,43,3],[42,4,43,4],[42,6,43,6],[42,7,43,7],[42,8,43,8],[39,1,40,1],[39,2,40,2],[39,3,40,3],[39,4,40,4],[39,6,40,6],[39,7,40,7],[33,8,34,8],[36,1,37,1],[36,2,37,2],[36,3,37,3],[36,4,37,4],[36,6,37,6],[36,7,37,7],[36,8,37,8],[33,1,34,1],[33,2,34,2],[33,3,34,3],[33,4,34,4],[33,6,34,6],[33,7,34,7],[28,8,29,8],[31,11,31,12],[31,13,31,14],[31,15,31,16],[31,17,31,18],[31,19,31,20],[28,1,29,1],[28,2,29,2],[28,3,29,3],[28,4,29,4],[28,6,29,6],[28,7,29,7],[21,8,22,8],[24,1,25,1],[24,2,25,2],[24,3,25,3],[24,4,25,4],[24,6,25,6],[24,7,25,7],[24,8,25,8],[21,1,22,1],[21,2,22,2],[21,3,22,3],[21,4,22,4],[21,6,22,6],[21,7,22,7],[14,8,15,8],[18,1,19,1],[18,2,19,2],[18,3,19,3],[18,4,19,4],[18,6,19,6],[18,7,19,7],[18,8,19,8],[14,1,15,1],[14,2,15,2],[14,3,15,3],[14,4,15,4],[14,6,15,6],[14,7,15,7],[8,8,9,8],[11,1,12,1],[11,2,12,2],[11,3,12,3],[11,4,12,4],[11,6,12,6],[11,7,12,7],[11,8,12,8],[8,1,9,1],[8,2,9,2],[8,3,9,3],[8,4,9,4],[8,6,9,6],[8,7,9,7],[2,7,3,7],[2,8,3,8],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,6,6,6],[5,7,6,7],[5,8,6,8],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,19,0,20],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,6,3,6]]}
["case ","Tx","SCS","Waveform","BW","Mapping Type","Propagation condition ","MCS","Additional DM-RS position","38.104 req","38.141-1/2 req","Samsung",null,"Nokia",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,3,"15kHz","CP-OFDM","5MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L3:Q3)","v":{"$error":"#NAME?"}},{"$f":"IF(J3>-100,J3+0.6,J3)","v":{"$error":"#NAME?"}},null,null,-4.74,null,-5.99,null,{"$f":"MAX(L3,N3,P3)-MIN(L3,N3,P3)","v":1.25},{"$f":"MAX(M34,O34,Q34)","v":0},{"$f":"AVERAGE(L3,N3,P3)","v":-5.3650000000000002},{"$f":"AVERAGE(M3,O3,Q3)","v":{"$error":"#DIV/0!"}}]
[2,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L4:Q4)","v":{"$error":"#NAME?"}},{"$f":"IF(J4>-100,J4+0.6,J4)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,{"$f":"MAX(L4,N4,P4)-MIN(L4,N4,P4)","v":0},{"$f":"MAX(M35,O35,Q35)","v":0},{"$f":"AVERAGE(L4,N4,P4)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[3,3,"15kHz","CP-OFDM","5MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L6:Q6)","v":{"$error":"#NAME?"}},{"$f":"IF(J6>-100,J6+0.6,J6)","v":{"$error":"#NAME?"}},null,null,3.92,null,7.13,null,3.21,0,5.5250000000000004,{"$error":"#DIV/0!"}]
[4,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L7:Q7)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[5,3,"15kHz","CP-OFDM","5MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L9:Q9)","v":{"$error":"#NAME?"}},{"$f":"IF(J9>-100,J9+0.6,J9)","v":{"$error":"#NAME?"}},null,null,5.53,null,9.08,null,3.55,0,7.3049999999999997,{"$error":"#DIV/0!"}]
[6,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L10:Q10)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[7,3,"15kHz","CP-OFDM","20MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L12:Q12)","v":{"$error":"#NAME?"}},{"$f":"IF(J12>-100,J12+0.6,J12)","v":{"$error":"#NAME?"}},null,null,-7.21,null,-5.98,null,1.2299999999999995,0,-6.5950000000000006,{"$error":"#DIV/0!"}]
[8,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L13:Q13)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[9,3,"15kHz","CP-OFDM","20MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L15:Q15)","v":{"$error":"#NAME?"}},{"$f":"IF(J15>-100,J15+0.6,J15)","v":{"$error":"#NAME?"}},null,null,6.16,null,7.12,null,0.96,0,6.6400000000000006,{"$error":"#DIV/0!"}]
[10,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L16:Q16)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L18:Q18)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[11,3,"15kHz","CP-OFDM","20MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L19:Q19)","v":{"$error":"#NAME?"}},{"$f":"IF(J19>-100,J19+0.6,J19)","v":{"$error":"#NAME?"}},null,null,4.33,null,9.0500000000000007,null,4.7200000000000006,0,6.69,{"$error":"#DIV/0!"}]
[12,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L20:Q20)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[13,3,"15kHz","CP-OFDM","50MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L22:Q22)","v":{"$error":"#NAME?"}},{"$f":"IF(J22>-100,J22+0.6,J22)","v":{"$error":"#NAME?"}},null,null,-7.19,null,-5.99,null,1.2000000000000002,0,-6.59,{"$error":"#DIV/0!"}]
[14,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L23:Q23)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[15,3,"15kHz","CP-OFDM","50MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L25:Q25)","v":{"$error":"#NAME?"}},{"$f":"IF(J25>-100,J25+0.6,J25)","v":{"$error":"#NAME?"}},null,null,2.68,null,7.1,null,4.42,0,4.8899999999999997,{"$error":"#DIV/0!"}]
[16,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L26:Q26)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L28:Q28)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[17,3,"15kHz","CP-OFDM","50MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L29:Q29)","v":{"$error":"#NAME?"}},{"$f":"IF(J29>-100,J29+0.6,J29)","v":{"$error":"#NAME?"}},null,null,4.6100000000000003,null,9.11,null,4.4999999999999991,0,6.8599999999999994,{"$error":"#DIV/0!"}]
[18,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L30:Q30)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[]
["case ","Tx","SCS","Waveform","BW","Mapping Type","Propagation condition ","MCS","Additional DM-RS position","38.104 req","38.141-1/2 req","Samsung",null,"Nokia",null,"Ericsson",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,null,"ideal","Impairment","ideal","Impairment","ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
[1,3,"30kHz","CP-OFDM","10MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L34:Q34)","v":{"$error":"#NAME?"}},{"$f":"IF(J34>-100,J34+0.6,J34)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,{"$f":"MAX(L34,N34,P34)-MIN(L34,N34,P34)","v":0},{"$f":"MAX(M65,O65,Q65)","v":0},{"$f":"AVERAGE(L34,N34,P34)","v":{"$error":"#DIV/0!"}},{"$f":"AVERAGE(M34,O34,Q34)","v":{"$error":"#DIV/0!"}}]
[2,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L35:Q35)","v":{"$error":"#NAME?"}},{"$f":"IF(J35>-100,J35+0.6,J35)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,{"$f":"MAX(L35,N35,P35)-MIN(L35,N35,P35)","v":0},{"$f":"MAX(M66,O66,Q66)","v":0},{"$f":"AVERAGE(L35,N35,P35)","v":{"$error":"#DIV/0!"}},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[3,3,"30kHz","CP-OFDM","10MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L37:Q37)","v":{"$error":"#NAME?"}},{"$f":"IF(J37>-100,J37+0.6,J37)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[4,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L38:Q38)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[5,3,"30kHz","CP-OFDM","10MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L40:Q40)","v":{"$error":"#NAME?"}},{"$f":"IF(J40>-100,J40+0.6,J40)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[6,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L41:Q41)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[7,3,"30kHz","CP-OFDM","40MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L43:Q43)","v":{"$error":"#NAME?"}},{"$f":"IF(J43>-100,J43+0.6,J43)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[8,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L44:Q44)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[9,3,"30kHz","CP-OFDM","40MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L46:Q46)","v":{"$error":"#NAME?"}},{"$f":"IF(J46>-100,J46+0.6,J46)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[10,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L47:Q47)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L49:Q49)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[11,3,"30kHz","CP-OFDM","40MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L50:Q50)","v":{"$error":"#NAME?"}},{"$f":"IF(J50>-100,J50+0.6,J50)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[12,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L51:Q51)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[13,3,"30kHz","CP-OFDM","100MHz","A","TDLB100-400",2,"pos1",{"$f":"DerivingPerfReq(L53:Q53)","v":{"$error":"#NAME?"}},{"$f":"IF(J53>-100,J53+0.6,J53)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[14,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L54:Q54)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[15,3,"30kHz","CP-OFDM","100MHz","A","TDLC300-100",16,"pos1",{"$f":"DerivingPerfReq(L56:Q56)","v":{"$error":"#NAME?"}},{"$f":"IF(J56>-100,J56+0.6,J56)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[16,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L57:Q57)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[32,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L59:Q59)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[17,3,"30kHz","CP-OFDM","100MHz","A","TDLA30-10",20,"pos1",{"$f":"DerivingPerfReq(L60:Q60)","v":{"$error":"#NAME?"}},{"$f":"IF(J60>-100,J60+0.6,J60)","v":{"$error":"#NAME?"}},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]
[18,null,null,null,null,"B",null,null,null,{"$f":"DerivingPerfReq(L61:Q61)","v":{"$error":"#NAME?"}},{"$error":"#NAME?"},null,null,null,null,null,null,0,0,{"$error":"#DIV/0!"},{"$error":"#DIV/0!"}]