3GPP TSG-RAN WG4 Meeting #94-e R4-2002849

Electronic Meeting, 24th February – 6th March, 2020

|  |
| --- |
| *CR-Form-v11.4* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-1** | **CR** | **0249** | **rev** | **1** | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for 38.101-1: to introduce UE RF requirements for adding wider channel bandwidth in band n28 |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_n28\_BW-Core |  | ***Date:*** | 2020-01-15 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Introduction of adding wider channel bandwidth for n28 into the specifications. |
| ***Summary of change:*** | MPR, AMPR, spurious emissions for UE co-existence and REFSENS are specified for 30MHz band n28. |
| ***Consequences if not approved:*** | New channel bandwidth for band n28 are not usable. |
|  |  |
| ***Clauses affected:*** | 3.2, 5.3.5, 6.2.2, 6.2.3.1, 6.2.3.13, 6.5.3.2, 6.5A.3.2.3, 6.5.3.3.3, 7.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.521-1 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

## **<Start of Changes>**

## 3.2 Symbols

For the purposes of the present document, the following symbols apply:

ΔFGlobal Granularity of the global frequency raster

ΔFRaster Band dependent channel raster granularity

ΔfOOB Δ Frequency of Out Of Band emission

ΔFTX-RX Δ Frequency of default TX-RX separation of the FDD *operating band*

∆MPRc Allowed Maximum Power Reduction relaxation for serving cell *c*

ΔPPowerClass Adjustment to maximum output power for a given power class

RB The starting frequency offset between the allocated RB and the measured non-allocated RBΔRIB,c Allowed reference sensitivity relaxation due to support for inter-band CA operation, for serving cell *c*

ΔRIB,4R Reference sensitivity adjustment due to support for 4 antenna ports

ΔShift Channel raster offset

TC Allowed operating band edge transmission power relaxation

TC,*c*Allowed operating band edge transmission power relaxation for serving cell *c*

ΔTIB,c Allowed maximum configured output power relaxation due to support for inter-band CA operation and due to support for SUL operations, for serving cell *c*

BWChannel Channel bandwidth

BWChannel,block Sub-block bandwidth, expressed in MHz. BWChannel,block= Fedge,block,high- Fedge,block,low

BWChannel\_CA Aggregated channel bandwidth, expressed in MHz

BWChannel,max Maximum channel bandwidth supported among all bands in a release

BWGB max( BWGB,Channel(*k*) )

BWGB,Channel(k) Minimum guard band defined in clause 5.3A.1 of carrier *k*

BWDL Channel bandwidth for DL

BWUL Channel bandwidth for UL

BWinterferer Bandwidth of the interferer

Ceil(x) Rounding upwards; ceil(x) is the smallest integer such that ceil(x) ≥ x

Floor(x) Rounding downwards; floor(x) is the greatest integer such that floor(x) ≤ x

FC *RF reference frequency* on the channel raster, given in table 5.4.2.2-1

FC,block, high Fc of the highest transmitted/received carrier in a *sub-block*

FC,block, low Fc of the lowest transmitted/received carrier in a *sub-block*

FC,low The Fc of the lowest carrier, expressed in MHz

FC,high The Fc of the highest carrier, expressed in MHz

FDL\_low The lowest frequency of the downlink *operating band*

FDL\_high The highest frequency of the downlink *operating band*

FUL\_low The lowest frequency of the uplink *operating band*

FUL\_high The highest frequency of the uplink *operating band*

Fedge,block,low The lower *sub-block* edge, where Fedge,block,low = FC,block,low - Foffset, low.

Fedge,block,high The upper *sub-block* edge, where Fedge,block,high = FC,block,high + Foffset, high.

Fedge , low The *lower edge* of *aggregated channel bandwidth*, expressed in MHz. Fedge,low = FC,low - Foffset,low.

Fedge, high The *higher edge* of *aggregated channel bandwidth*, expressed in MHz. Fedge,high = FC,high + Foffset,high.

FInterferer (offset) Frequency offset of the interferer (between the center frequency of the interferer and the carrier frequency of the carrier measured)

FInterferer Frequency of the interferer

FIoffset Frequency offset of the interferer (between the center frequency of the interferer and the closest edge of the carrier measured)

Foffset Frequency offset from FC\_high to the *higher edge* or FC\_low to the *lower edge.*

Foffset,high Frequency offset from FC,high to the upper *UE RF Bandwidth edge*, or from FC,block, high to the upper sub-block edge

Foffset,low Frequency offset from FC,low to the lower *UE RF Bandwidth edge*, or from FC,block, low to the lower sub-block edge

FOOB The boundary between the NR out of band emission and spurious emission domains

FREF RF reference frequency

FREF-Offs Offset used for calculating FREF

FREF,Shift RF reference frequency for Supplementary Uplink (SUL) bands and for the uplink for all FDD bands

Fuw (offset) The frequency separation of the center frequency of the carrier closest to the interferer and the center frequency of the interferer

GBChannel Minimum guard band defined in clause 5.3.3

LCRB Transmission bandwidth which represents the length of a contiguous resource block allocation

expressed in units of resources blocks

Max() The largest of given numbers

Min() The smallest of given numbers

 Physical resource block number

NRACLR NR ACLR

NRB Transmission bandwidth configuration, expressed in units of resource blocks

NRB\_agg The number of the aggregated RBs within the fully allocated aggregated channel bandwidth

NRB,c The transmission bandwidth configuration of component carrier c, expressed in units of resource blocks

NRB,largest BW The largest transmission bandwidth configuration of the component carriers in the bandwidth combination, expressed in units of resource blocks

NRB,low The transmission bandwidth configurations according to Table 5.3.2-1 for the lowest assigned component carrier in clause 5.3A.1

NRB,high The transmission bandwidth configurations according to Table 5.3.2-1 for the highest assigned component carrier in clause 5.3A.1

NREF NR Absolute Radio Frequency Channel Number (NR-ARFCN)

NREF-Offs Offset used for calculating NREF

PCMAX The configured maximum UE output power

PCMAX, *c* The configured maximum UE output power for serving cell *c*

PCMAX, *f*, *c* The configured maximum UE output power for carrier *f* of serving cell *c* in each slot

PEMAX Maximum allowed UE output power signalled by higher layers

PEMAX, *c* Maximum allowed UE output power signalled by higher layers for serving cell *c*

PInterferer Modulated mean power of the interferer

Plargest BW Power of the largest transmission bandwidth configuration of the component carriers in the bandwidth combination

PPowerClass PPowerClass is the nominal UE power (i.e., no tolerance)

P-MPR*c* Maximum allowed UE output power reduction for serving cell *c*

PRB The transmitted power per allocated RB, measured in dBm

PUMAX The measured configured maximum UE output power

Puw Power of an unwanted DL signal

Pw Power of a wanted DL signal

RBstart Indicates the lowest RB index of transmitted resource blocks

SCSc SCS for the component carrier c

SCSlargest BW SCS for the largest transmission bandwidth configuration of the component carriers in the bandwidth combination

SCSlow SCS for the lowest assigned component carrier in clause 5.3A.1

SCShigh SCS for the highest assigned component carrier in clause 5.3A.1

T(PCMAX, *f*, *c*) Tolerance for applicable values of PCMAX, *f*, *c* for configured maximum UE output power for carrier *f* of serving cell *c*

TL,c Absolute value of the lower tolerance for the applicable *operating band* as specified in clause 6.2.1

SSREF SS block reference frequency position

UTRAACLR UTRA ACLR

## **<Next of Changes>**

### 5.3.5 UE channel bandwidth per operating band

The requirements in this specification apply to the combination of channel bandwidths, SCS and operating bands shown in Table 5.3.5-1. The transmission bandwidth configuration in Table 5.3.2-1 shall be supported for each of the specified channel bandwidths. The channel bandwidths are specified for both the TX and RX path.

Table 5.3.5-1 Channel bandwidths for each NR band

|  |  | NR band / SCS / UE Channel bandwidth |
| --- | --- | --- |
| NR Band | SCSkHz | 5 MHz | 101,2 MHz | 152 MHz | 202 MHz | 252 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 70 MHz | 80 MHz | 90 MHz | 100 MHz |
| n1 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n2 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n3 | 15 | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| n5 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n7 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n8 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n20 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n25 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n28 | 15 | Yes | Yes | Yes | Yes7 |  | Yes7 |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes7 |  | Yes7 |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n29 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | 15 | Yes | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| n38 | 15 | Yes | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| n39 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n40 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  | Yes |  |  |
| n41 | 15 |  | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| n48 | 15 | Yes5 | Yes | Yes | Yes |  |  | Yes | Yes6 |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  | Yes | Yes6 | Yes6 |  | Yes6 | Yes6,4 | Yes6 |
| 60 |  | Yes | Yes | Yes |  |  | Yes | Yes6 | Yes6 |  | Yes6 | Yes6,4 | Yes6 |
| n50 | 15 | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes3 |  |  |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes3 |  |  |
| n51 | 15 | Yes |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n65 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n66 | 15 | Yes | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| n70 | 15 | Yes | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |
| n71 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n74 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n75 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| n76 | 15 | Yes |  |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n77 | 15 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes4 | Yes |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes4 | Yes |
| n78 | 15 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes4 | Yes | Yes | Yes |
| n79 | 15 |  |  |  |  |  |  | Yes | Yes |  |  |  |  |  |
| 30 |  |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
| 60 |  |  |  |  |  |  | Yes | Yes | Yes |  | Yes |  | Yes |
| n80 | 15 | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |
| n81 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n82 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n83 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n84 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| n86 | 15 | Yes | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes |  |  | Yes |  |  |  |  |  |  |
| n89 | 15 | Yes | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n90 | 15 |  | Yes | Yes | Yes |  | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| 60 |  | Yes | Yes | Yes |  | Yes | Yes | Yes | Yes |  | Yes | Yes | Yes |
| n91 | 15 | Yes | Yes8 |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n92 | 15 | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | 15 | Yes | Yes8 |  |  |  |  |  |  |  |  |  |  |  |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n94 | 15 | Yes | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes3 | Yes3 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n95 | 15 | Yes | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 30 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| 60 |  | Yes | Yes |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: 90% spectrum utilization may not be achieved for 30kHz SCS.NOTE 2: 90% spectrum utilization may not be achieved for 60kHz SCS.NOTE 3: This UE channel bandwidth is applicable only to downlink.NOTE 4: This UE channel bandwidth is optional in this release of the specification.NOTE 5: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an SCell part of DC or CA configuration.NOTE 6: For this bandwidth, the minimum requirements are restricted to operation when carrier is configured as an downlink SCell part of CA configuration.NOTE 7: For the 20 MHz bandwidth, the minimum requirements are specified for NR UL carrier frequencies confined to either 713-723 MHz or 728-738 MHz. For the 30MHz bandwidth, the minimum requirements are specified for NR UL transmission bandwidth configuration confined to either 703-733 or 718-748 MHz.NOTE 8: This UE channel bandwidth is applicable only to uplink. |

## **<Next of Changes>**

### 6.2.2 UE maximum output power reduction

UE is allowed to reduce the maximum output power due to higher order modulations and transmit bandwidth configurations. For UE power class 2 and 3, the allowed maximum power reduction (MPR) is defined in Table 6.2.2-2 and Table 6.2.2-1, respectively for channel bandwidths that meets both following criteria:

Channel bandwidth ≤ 100 MHz.

Relative channel bandwidth ≤ 4 % for TDD bands and ≤ 3 % for FDD bands. Unless otherwise stated, the ∆MPR is set to zero.

If the relative channel bandwidth is larger than 4% for TDD bands or 3% for FDD bands, the ∆MPR is defined in Table 6.2.2-3.

Where relative channel bandwith = 2\*BWChannel / (FUL\_low + FUL\_high)

The allowed MPR for SRS, PUCCH formats 0, 1, 3 and 4, and PRACH shall be as specified for QPSK modulated DFT-s-OFDM of equivalent RB allocation. The allowed MPR for PUCCH format 2 shall be as specified for QPSK modulated CP-OFDM of equivalent RB allocation.

Table 6.2.2-1 Maximum power reduction (MPR) for power class 3

|  |  |
| --- | --- |
| Modulation | MPR (dB) |
| Edge RB allocations | Outer RB allocations | Inner RB allocations |
| DFT-s-OFDM  | Pi/2 BPSK | ≤ 3.51 | ≤ 1.21 | ≤ 0.21 |
| ≤ 0.52 | ≤ 0.52 | 02 |
| QPSK | ≤ 1 | 0 |
| 16 QAM | ≤ 2 | ≤ 1 |
| 64 QAM | ≤ 2.5 |
| 256 QAM | ≤ 4.5 |
| CP-OFDM  | QPSK | ≤ 3 | ≤ 1.5 |
| 16 QAM | ≤ 3 | ≤ 2 |
| 64 QAM | ≤ 3.5 |
| 256 QAM | ≤ 6.5 |
| NOTE 1: Applicable for UE operating in TDD mode with Pi/2 BPSK modulation and UE indicates support for UE capability *powerBoosting-pi2BPSK* and if the IE *powerBoostPi2BPSK* is set to 1 and 40 % or less slots in radio frame are used for UL transmission for bands n40, n41, n77, n78 and n79. The reference power of 0 dB MPR is 26 dBm.NOTE 2: Applicable for UE operating in FDD mode, or in TDD mode in bands other than n40, n41, n77, n78 and n79 with Pi/2 BPSK modulation and if the IE *powerBoostPi2BPSK* is set to 0 and if more than 40 % of slots in radio frame are used for UL transmission for bands n40, n41, n77, n78 and n79.  |

Table 6.2.2-2 Maximum power reduction (MPR) for power class 2

|  |  |
| --- | --- |
| Modulation | MPR (dB) |
| Edge RB allocations | Outer RB allocations | Inner RB allocations |
| DFT-s-OFDM  | Pi/2 BPSK | ≤ 3.5 | ≤ 0.5 | 0 |
| QPSK | ≤ 3.5 | ≤ 1 | 0 |
| 16 QAM | ≤ 3.5 | ≤ 2 | ≤ 1 |
| 64 QAM | ≤ 3.5 | ≤ 2.5 |
| 256 QAM | ≤ 4.5 |
| CP-OFDM  | QPSK | ≤ 3.5 | ≤ 3 | ≤ 1.5 |
| 16 QAM | ≤ 3.5 | ≤ 3 | ≤ 2 |
| 64 QAM | ≤ 3.5 |
| 256 QAM | ≤ 6.5 |

Table 6.2.2-3: ∆MPR

|  |  |  |  |
| --- | --- | --- | --- |
| NR Band | Power class | Channel bandwidth | ∆MPR (dB) |
| n28 | Power class 3 | 30 MHz | [1] |

Where the following parameters are defined to specify valid RB allocation ranges for Outer and Inner RB allocations:

NRB is the maximum number of RBs for a given Channel bandwidth and sub-carrier spacing defined in Table 5.3.2-1. RBStart,Low = max(1, floor(LCRB/2))

where max() indicates the largest value of all arguments and floor(x) is the greatest integer less than or equal to x.

RBStart,High = NRB – RBStart,Low – LCRB

The RB allocation is an Inner RB allocation if the following conditions are met

RBStart,Low ≤ RBStart ≤ RBStart,High,and

LCRB ≤ ceil(NRB/2)

where ceil(x) is the smallest integer greater than or equal to x.

An Edge RB allocation is the one for which the RB(s) is (are) allocated at the lowermost or uppermost edge of the channel with LCRB ≤ 2 RBs.

The RB allocation is an Outer RB allocation for all other allocations which are not an Inner RB allocation or Edge RB allocation.

If CP-OFDM allocation satisfies following conditions, it is considered as almost contiguous allocation

NRB\_gap / (NRB\_alloc + NRB\_gap ) ≤ 0.25

and NRB\_alloc + NRB\_gap is larger than 106, 51 or 24 RBs for 15 kHz, 30 kHz or 60 kHz respectively where NRB\_gap is the total number of unallocated RBs between allocated RBs and NRB\_alloc is the total number of allocated RBs. The size and location of allocated and unallocated RBs are restricted by RBG parameters specified in clause 6.1.2.2 of TS 38.214 [10]. For these almost contiguous signals in power class 2 and 3, the allowed maximum power reduction defined in Table 6.2.2-1 is increased by

CEIL{ 10 log10(1 + NRB\_gap / NRB\_alloc), 0.5 } dB,

where CEIL{x,0.5} means x rounding upwards to closest 0.5dB. The parameters of RBStart,Low and RBStart,High to specify valid RB allocation ranges for Outer and Inner RB allocations are defined as following:

RBStart,Low = max(1, floor((NRB\_alloc + NRB\_gap)/2))

RBStart,High = NRB – RBStart,Low – NRB\_alloc –NRB\_gap

For the UE maximum output power modified by MPR, the power limits specified in clause 6.2.4 apply.

### 6.2.3 UE additional maximum output power reduction

#### 6.2.3.1 General

Additional emission requirements can be signalled by the network. Each additional emission requirement is associated with a unique network signalling (NS) value indicated in RRC signalling by an NR frequency band number of the applicable operating band and an associated value in the field *additionalSpectrumEmission.* Throughout this specification, the notion of indication or signalling of an NS value refers to the corresponding indication of an NR frequency band number of the applicable operating band, the IE field *freqBandIndicatorNR* and an associated value of *additionalSpectrumEmission* in the relevant RRC information elements [7]*.*

To meet the additional requirements, additional maximum power reduction (A-MPR) is allowed for the maximum output power as specified in Table 6.2.1-1. Unless stated otherwise, the total reduction to UE maximum output power is max(MPR, A-MPR) where MPR is defined in clause 6.2.2. Outer and inner allocation notation used in clause 6.2.3 is defined in clause 6.2.2 In absense of modulation and waveform types the A-MPR applies to all modulation and waveform types.

Table 6.2.3.1-1 specifies the additional requirements with their associated network signalling values and the allowed A-MPR and applicable operating band(s) for each NS value. In case of a power class 3 UE, when IE *powerBoostPi2BPSK* is set to 1, power class 2 A-MPR values apply. The mapping of NR frequency band numbers and values of the *additionalSpectrumEmission* to network signalling labels is specified in Table 6.2.3.1-1A.

For almost contiguous allocations in CP-OFDM waveforms in power class 3, the allowed A-MPR defined in clause 6.2.3 is increased by CEIL{ 10 log10(1 + NRB\_gap / NRB\_alloc), 0.5 } dB, where NRB\_gap is the total number of unallocated RBs between allocated RBs and NRB\_alloc is the total number of allocated RBs, and the parameter LCRB is replaced by NRB\_alloc + NRB\_gap in specifying the RB allocation regions.

Table 6.2.3.1-1: Additional maximum power reduction (A-MPR)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Network signalling label | Requirements (clause) | NR Band | Channel bandwidth (MHz) | Resources blocks (*N*RB) | A-MPR (dB) |
| NS\_01 |  | Table 5.2-1 | 5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 90, 100 | Table 5.3.2-1 | N/A |
| NS\_03 | 6.5.2.3.3 | n2, n25, n66,n70, n86 |  |  | Clause 6.2.3.7 |
| NS\_03U | 6.5.2.3.3, 6.5.2.4.2 | n2, n25, n66, n86 |  |  | Clause 6.2.3.7 |
| NS\_04 | 6.5.2.3.2, 6.5.3.3.1 | n41 | 10, 15, 20, 30, 40, 50, 60 80, 90, 100 |  | Clause 6.2.3.2 |
| NS\_05 | 6.5.3.3.4 | n1, n84 | 5, 10, 15, 20(NOTE 2) |  | Clause 6.2.3.4 |
| NS\_05U | 6.5.3.3.4, 6.5.2.4.2 | n1, n84 | 5, 10, 15, 20 |  | Clause 6.2.3.4 |
| NS\_06 | 6.5.2.3.4 | n12 | 5, 10, 15 |  | N/A |
| n14 | 5,10 |
| NS\_10 |  | n20 | 15, 20 | Table 6.2.3.3-1 | Table6.2.3.3-1 |
| NS\_17 | 6.5.3.3.2 | n28, n83 | 5,10 | Table 5.3.2-1 | N/A |
| NS\_18 | 6.5.3.3.3 | n28, n83 | 5 |  | Table 6.2.3.13-1, A1 |
| 10, 15, 20 |  | Table 6.2.3.13-1, A2 |
| 30 |  | Table 6.2.3.13-1, A3, A4, A5 |
| NS\_21 | 6.5.3.3.12 | n30 | 5, 10 |  | Clause 6.2.3.14 |
| NS\_24 | 6.5.3.3.13 | n65 (NOTE 4) | 5, 10, 15, 20 | Table 6.2.3.15-1 | Clause 6.2.3.15 |
| NS\_27 | 6.5.2.3.86.5.3.3.14 | n48 | 5, 10, 15, 20, 40 | Table 6.2.3.16-1 | Table 6.2.3.16-2 |
| NS\_35 | 6.5.2.3.1 | n71 | 5, 10, 15, 20 | Table 5.3.2-1 | N/A |
| NS\_37 | 6.5.3.3.6 | n74(NOTE 3) | 10, 15 | Table 6.2.3.8-1 | Table6.2.3.8-1 |
| NS\_38 | 6.5.3.3.7 | n74 | 5, 10, 15, 20 | Table 6.2.3.9-1 | Table6.2.3.9-1 |
| NS\_39 | 6.5.3.3.8 | n74 | 10, 15, 20 | Table 6.2.3.10-1 | Table 6.2.3.10-1 |
| NS\_40 | 6.5.3.3.9 | n51 | 5 |  | Table6.2.3.5-1 |
| NS\_41 | 6.5.3.3.10 | n50 | 5, 10, 15, 20, 30, 40, 50, 60 |  | Table 6.2.3.11-1 |
| NS\_42 | 6.5.3.3.11 | n50 | 5, 10, 15, 20, 30, 40, 50, 60 |  | Table 6.2.3.12-1 |
| NS\_43 | 6.5.3.3.5 | n8, n81 | 5, 10, 15 |  | Clause 6.2.3.6 |
| NS\_43U | 6.5.3.3.5, 6.5.2.4.2 | n8, n81 | 5, 10, 15 |  | Clause 6.2.3.6 |
| NS\_44 | 6.5.3.2 | n38 | 40 | Table 6.2.3.20-1 | Table 6.2.3.20-1 |
| NS\_45 | 6.5.3.3.16 | n39 | 25, 30, 40 |  | Clause 6.2.3.19 |
| NS\_46 | 6.5.3.2 | n7 | 25, 30, 40, 50 | Table 6.2.3.17-1 | Table 6.2.3.17-2 |
| NS\_47 | 6.5.3.3.15 | n41 (Note 5) | 30 | Table 6.2.3.18-1 | Table 6.2.3.18-2 |
| NS\_100 | 6.5.2.4.2 | n1, n2, n3, n5, n8, n18, n25, n65, n66, n80, n81, n84, n86, n89(NOTE 1) |  |  | Table6.2.3.1-2 |
| NOTE 1: This NS can be signalled for NR bands that have UTRA services deployedNOTE 2: No A-MPR is applied for 5 MHz CBW where the lower channel edge is ≥ 1930 MHz,10 MHz CBW where the lower channel edge is ≥ 1950 MHz and 15 MHz CBW where the lower channel edge is ≥ 1955 MHz.NOTE 3: Applicable when the NR carrier is within 1447.9 – 1462.9 MHzNOTE 4: Applicable when the upper edge of the channel bandwidth frequency is greater than 1980 MHz.NOTE 5: Applicable when the NR carrier is within 2545 – 2575 MHz |

[The NS\_01 label with the field *additionalPmax* [7] absent is default for all NR bands.]

Table 6.2.3.1-1A: Mapping of network signaling label

|  |  |
| --- | --- |
| NR band | Value of additionalSpectrumEmission |
| **0** | **1** | **2** | **3** | **4** | **5** | **6** | **7** |
| n1 | NS\_01 | NS\_100 | NS\_05 | NS\_05U |  |  |  |  |
| n2 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n3 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n5 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n7 | NS\_01 | NS\_46 |  |  |  |  |  |  |
| n8 | NS\_01 | NS\_100 | NS\_43 | NS\_43U |  |  |  |  |
| n12 | NS\_01 | NS\_06 |  |  |  |  |  |  |
| n14 | NS\_01 | NS\_06 |  |  |  |  |  |  |
| n18 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n20 | NS\_01 | Void | NS\_10 |  |  |  |  |  |
| n25 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n28 | NS\_01 | NS\_17 | NS\_18 |  |  |  |  |  |
| n30 | NS\_01 | NS\_21 |  |  |  |  |  |  |
| n34 | NS\_01 |  |  |  |  |  |  |  |
| n38 | NS\_01 | NS\_44 |  |  |  |  |  |  |
| n39 | NS\_01 | NS\_45 |  |  |  |  |  |  |
| n40 | NS\_01 |  |  |  |  |  |  |  |
| n41 | NS\_01 | NS\_04 | NS\_47 |  |  |  |  |  |
| n48 | NS\_01 | NS\_27 |  |  |  |  |  |  |
| n50 | NS\_01 | NS\_41 | NS\_42 |  |  |  |  |  |
| n51 | NS\_01 | NS\_40 |  |  |  |  |  |  |
| n65 | NS\_01 | NS\_24 | NS\_100 |  |  |  |  |  |
| n66 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n70 | NS\_01 | NS\_03 |  |  |  |  |  |  |
| n71 | NS\_01 | NS\_35 |  |  |  |  |  |  |
| n74 | NS\_01 | NS\_37 | NS\_38 | NS\_39 |  |  |  |  |
| n77 | NS\_01 |  |  |  |  |  |  |  |
| n78 | NS\_01 |  |  |  |  |  |  |  |
| n79 | NS\_01 |  |  |  |  |  |  |  |
| n80 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n81 | NS\_01 | NS\_100 | NS\_43 | NS\_43U |  |  |  |  |
| n82 | NS\_01 | Void |  |  |  |  |  |  |
| n83 | NS\_01 | NS\_17 | NS\_18 |  |  |  |  |  |
| n84 | NS\_01 | NS\_100 | NS\_05 | NS\_05U |  |  |  |  |
| n86 | NS\_01 | NS\_100 | NS\_03 | NS\_03U |  |  |  |  |
| n89 | NS\_01 | NS\_100 |  |  |  |  |  |  |
| n95 | NS\_01 |  |  |  |  |  |  |  |
| NOTE: *additionalSpectrumEmission* corresponds to an information element of the same name defined in clause 6.3.2 of TS 38.331 [7]. |

Table 6.2.3.1-2: A-MPR for NS\_100 (UTRA protection)

|  |  |
| --- | --- |
| Modulation/Waveform | Outer (dB) |
| DFT-s-OFDM | Pi/2 BPSK | ≤ 2 |
| QPSK | ≤ 2 |
| 16 QAM | ≤ 2.5 |
| 64 QAM | ≤ 3 |
| 256 QAM | ≤ 4.5 |
| CP-OFDM | QPSK | ≤ 4 |
| 16 QAM | ≤ 4 |
| 64 QAM | ≤ 4 |
| 256 QAM | ≤ 6.5 |
| NOTE 1: VoidNOTE 2: Void |

## **<Next of Changes>**

### 6.2.4 Configured transmitted power

The UE is allowed to set its configured maximum output power PCMAX,f,c for carrier f of serving cell c in each slot. The configured maximum output power PCMAX,f,c is set within the following bounds:

PCMAX\_L,f,c ≤ PCMAX,f,c ≤ PCMAX\_H,f,c with

 PCMAX\_L,f,c = MIN {PEMAX,c– ∆TC,c, (PPowerClass – ΔPPowerClass) – MAX(MAX(MPRc+∆MPRc, A-MPRc)+ ΔTIB,c + ∆TC,c +∆TRxSRS, P-MPRc) }

PCMAX\_H,f,c = MIN {PEMAX,c, PPowerClass – ΔPPowerClass }

where

PEMAX,c is the value given by either the *p-Max* IE or the field *additionalPmax* of the *NR-NS-PmaxList IE*, whichever is applicable according to TS 38.331[7];

PPowerClass is the maximum UE power specified in Table 6.2.1-1 without taking into account the tolerance specified in the Table 6.2.1-1;

When the IE *powerBoostPi2BPSK* is set to 1, PEMAX,c is increased by +3 dB for a power class 3 capable UE operating in TDD bands n40, n41, n77, n78, and n79 with PI/2 BPSK modulation and UE indicates support for UE capability *powerBoosting-pi2BPSK* and 40% or less symbols in certain evaluation period are used for UL transmission when PEMAX,c ≥ 20 dBm (The exact evaluation period is no less than one radio frame).

When the IE *powerBoostPi2BPSK* is set to 1, ΔPPowerClass = -3 dB for a power class 3 capable UE operating in TDD bands n40, n41, n77, n78, and n79 with Pi/2 BPSK modulation and UE indicates support for UE capability *powerBoosting-pi2BPSK* and 40% or less slots in radio frame are used for UL transmission.

ΔPPowerClass = 3 dB for a power class 2 capable UE when P-max of 23 dBm or lower is indicated; or when the field of UE capability *maxUplinkDutyCycle* is absent and the percentage of uplink symbols transmitted in a certain evalutation period is larger than 50%; or when the field of UE capability *maxUplinkDutyCycle* is not absent and the percentage of uplink symbols transmitted in a certain evaluation period is larger than *maxUplinkDutyCycle* as defined in TS 38.331 (The exact evaluation period is no less than one radio frame); otherwise ΔPPowerClass = 0 dB;

∆TIB,c is the additional tolerance for serving cell c as specified in TS 38.101-3 clause 6.2A.4.2 and 6.2B.4.2; ∆TIB,c = 0 dB otherwise;

∆TC,c = 1.5dB when NOTE 3 in Table 6.2.1-1 in 38.101-1 applies for a serving cell c, otherwise ∆TC,c = 0 dB ;

MPRc and A-MPRc for serving cell c are specified in clause 6.2.2 and clause 6.2.3, respectively;

∆MPRc for serving cell c is specified in clause 6.2.2.

∆TRxSRS is applied when UE transmits SRS to other than first SRS port when the *SRS-TxSwitch* capability is indicated as '1T2R', '1T4R' or, '1T4R/2T4R' with UE configured with 4 SRS resources in the SRS resource set, and when UE transmits SRS to other than first or second SRS port when the *SRS-TxSwitch* capabilityis indicated as '2T4R' or '1T4R/2T4R' with the UE configured with 2 SRS resources in the SRS resource set. The value of ∆TRxSRS is 4.5dB for n79 and 3 dB for bands whose FUL\_high is lower than the FUL\_low of n79.

For other SRS transmissions ∆TRxSRS is zero;

P-MPRc is the allowed maximum output power reduction for

a) ensuring compliance with applicable electromagnetic energy absorption requirements and addressing unwanted emissions / self desense requirements in case of simultaneous transmissions on multiple RAT(s) for scenarios not in scope of 3GPP RAN specifications;

b) ensuring compliance with applicable electromagnetic energy absorption requirements in case of proximity detection is used to address such requirements that require a lower maximum output power.

The UE shall apply P-MPRc for serving cell c only for the above cases. For UE conducted conformance testing P-MPRc shall be 0 dB

NOTE 1: P-MPRc was introduced in the PCMAX,f,c equation such that the UE can report to the gNB the available maximum output transmit power. This information can be used by the gNB for scheduling decisions.

NOTE 2: P-MPRc may impact the maximum uplink performance for the selected UL transmission path.

TREF and Teval are specified in Table 6.2.4-1. For each TREF, the PCMAX,L,c for serving cell c are evaluated per Teval and given by the minimum value taken over the transmission(s) within the Teval; the minimum PCMAX\_L,f,c over one or more Teval is then applied for the entire TREF

Table 6.2.4-1: Evaluation and reference periods for Pcmax

|  |  |  |
| --- | --- | --- |
| TREF | Teval | Teval with frequency hopping |
| Physical channel length | Physical channel length | Min(*Tno\_hopping*, Physical Channel Length) |

The measured configured maximum output power PUMAX,f,c shall be within the following bounds:

 PCMAX\_L,f,c – MAX{TL,c, T(PCMAX\_L,f,c)} ≤ PUMAX,f,c ≤ PCMAX\_H,f,c + T(PCMAX\_H,f,c).

where the tolerance T(PCMAX,f,c) for applicable values of PCMAX,f,c is specified in Table 6.2.4-1. The tolerance TL,c is the absolute value of the lower tolerance for the applicable operating band as specified in Table 6.2.1-1.

Table 6.2.4-1: PCMAX tolerance

|  |  |
| --- | --- |
| PCMAX,f,c (dBm) | Tolerance T(PCMAX,f,c) (dB) |
| 23 < PCMAX,c ≤ 33 | 2.0 |
| 21 ≤ PCMAX,c ≤ 23 | 2.0 |
| 20 ≤ PCMAX,c < 21 | 2.5 |
| 19 ≤ PCMAX,c < 20 | 3.5 |
| 18 ≤ PCMAX,c < 19 | 4.0 |
| 13 ≤ PCMAX,c < 18 | 5.0 |
| 8 ≤ PCMAX,c < 13 | 6.0 |
| -40 ≤ PCMAX,c < 8 | 7.0 |

## **<Next of Changes>**

#### 6.2.3.13 A-MPR for NS\_18

Table 6.2.3.13-0: Band n28 30MHz A-MPR regions for NS\_18

|  |  |  |  |
| --- | --- | --- | --- |
| Channel Bandwidth, MHz | Frequency range of UL transmission bandwidth configuration, MHz | Regions | A-MPR |
| RBstart\*12\*SCSMHz | LCRB\*12\*SCSMHz |
| 30 | 703~733 | >(LCRB\*12\*SCS)/2+5.22 | ≥Max(0, 12\*SCS\*NRB – 1.8 – RBstart\*12\*SCS) | A3 |
| ≤(LCRB\*12\*SCS)/2+5.22 | ≥5.4 | A4 |
| ≤7.92 | <5.4 | A5 |

Table 6.2.3.13-1: A-MPR for NS\_18

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Modulation/Waveform** | **A1 (dB)** | **A2 (dB)** | A3 | A4 | A5 |
| **Outer** | **Inner** | **Inner/Outer** | Outer/Inner | Outer/Inner | Outer/Inner |
| DFT-s-OFDM  |  Pi/2 BPSK | ≤ 2 | N/A | ≤ 5 | [3] | [8] | [3] |
| QPSK | ≤ 2 | ≤ 5 | [3] | [8] | [3] |
| 16 QAM | ≤ 3 | ≤ 6 | [3] | [8] | [3] |
| 64 QAM | ≤ 4 | ≤ 7 | [3] | [8] | [4.5] |
| 256 QAM | ≤ 6 | ≤ 9 | [3] | [8] | [5.5] |
| CP-OFDM | QPSK | ≤ 5 | ≤ 6.5 | [4.5] | [9.5] | [5] |
| 16 QAM | ≤ 5 | ≤ 7 | [4.5] | [9.5] | [5] |
| 64 QAM | ≤ 5.5 | ≤ 8.5 | [4.5] | [9.5] | [5.5] |
| 256 QAM | ≤ 8.5 | ≤ 11.5 | [4.5] | [9.5] | [7.5] |
| NOTE 1: VoidNOTE 2: Void |

## **<Next of Changes>**

#### 6.5.3.2 Spurious emissions for UE co-existence

This clause specifies the requirements for NR bands for coexistence with protected bands.

Table 6.5.3.2-1: Requirements for spurious emissions for UE co-existence

| NR Band | Spurious emission for UE co-existence |
| --- | --- |
| Protected band | Frequency range (MHz) | Maximum Level (dBm) | MBW (MHz) | NOTE |
| n1, n84 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 22, 26, 27, 28, 31, 32, 38, 40, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 73, 74, 75, 76,NR Band n78, n79 | FDL\_low  | - | FDL\_high  | -50 | 1 |  |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 15, 27 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 15, 26, 27 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 15, 26, 27 |
| n2 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 42, 48, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low  | - | FDL\_high  | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low  | - | FDL\_high  | -50 | 1 | 15 |
| E-UTRA Band 43 | FDL\_low  | - | FDL\_high  | -50 | 1 | 2 |
| n3, n80 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 38, 39, 40, 41, 43, 44, 45, 50, 51, 65, 67, 68, 69, 72, 73,74, 75, 76.NR Band n79 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 11, 18, 19, 21 | FDL\_low | - |  FDL\_high | -50 | 1 | 13 |
| E-UTRA Band 22, 42, 52, NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 13 |
| n5, n89 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 18, 19, 24, 25, 26, 28, 29, 30, 31, 34, 38, 40, 42, 43, 45, 48, 50, 51, 53, 65, 66, 70, 71, 73, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 39 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8,39 |
| n7 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 20, 22, 26, 27, 28, 29, 30, 31, 32, 33, 34, 40, 42, 43, 50, 51, 52, 65, 66, 67, 68, 72, 74, 75, 76, 85,NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570  | - | 2575 | +1.6 | 5 | 15, 21, 26 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 15, 21, 26 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 15, 21 |
| n8, n81 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 22, 41, 42, 43, 52,NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA 8 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n12 | E-UTRA Band 2, 5, 13, 14, 17, 24, 25, 26, 27, 30, 41, 48, 50, 51, 53, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| n14 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 23, 24, 25, 26, 27, 29, 30, 41, 48, 53, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 769 | - | 775 | -35 | 0.00625 | 12, 15 |
| Frequency range | 799 | - | 805 | -35 | 0.00625 | 11, 12, 15 |
| n18 | E-UTRA Band 1, 3, 11, 21, 34, 42, 65NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 |  |
| Frequency range | 860 | - | 890 | -40 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| n20, n82 | E-UTRA Band 1, 3, 7, 8, 22, 31, 32, 33, 34, 40, 42, 43, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 38, 42, 69,NR Band n77, n78 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| n25 | E-UTRA Band 4, 5, 10,12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 42, 48, 53, 66, 70, 71, 85 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2 | FDL\_low  | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 25 | FDL\_low  | - | FDL\_high | -50 | 1 | 15 |
| E-UTRA Band 43 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| n28, n83 | E-UTRA Band 1, 4, 10, 22, 32, 42, 43, 50, 51, 52, 65, 66, 73, 74, 75, 76,NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 19, 25 |
| E-UTRA Band 2, 3, 5, 7, 8, 18, 19, 20, 25, 26, 27, 31, 34, 38, 39, 40, 41, 66, 72,NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 19, 24 |
| Frequency range | 470 | - | 694 | -42 | 8 | 15, 35 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 34 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 15 |
| Frequency range | 758 | - | 773 | -32 | 1 | 15 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8, 19 |
| n30 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 24, 25, 26, 27, 29, 30, 38, 41, 48, 53, 66, 70, 71, 85 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| n34 | E-UTRA Band 1, 3, 7, 8, 11, 18, 19, 20, 21, 22, 26, 28, 31, 32, 33, 38,39, 40, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 69, 72, 74, 75, 76,NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n38 | E-UTRA Band 1, 2, 3, 4, 5, 8, 10, 12, 13, 14, 17, 20, 22, 27, 28, 29, 30, 31, 32, 33, 34, 40, 42, 43, 50, 51, 52, 65, 66, 67, 68, 72, 74, 75, 76, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2620 | - | 2645 | -15.5 | 5 | 15, 22, 26 |
| Frequency range | 2645 | - | 2690 | -40 | 1 | 15, 22 |
| n39 | E-UTRA Band 1, 8, 22, 26, 28, 34, 40, 41, 42, 44, 45, 50, 51, 52, 74,NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 33 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 15, 26, 33 |
| n40 | E-UTRA Band 1, 3, 5, 7, 8, 20, 22, 26, 27, 28, 31, 32, 33, 34, 38, 39, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 74, 75, 76,NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| n41 | E-UTRA Band 1, 2, 3, 4, 5, 8, 10, 12, 13, 14, 17, 24, 25, 26, 27, 28, 29, 30, 34, 39, 42, 44, 45, 48, 50, 51, 52, 65, 66, 70, 71, 73, 74, 85, NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 9, 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 30 |
| Frequency range | 1884.5 |  | 1915.7 | -41 | 0.3 | 8, 30 |
| n48 | E-UTRA Band 2, 4, 5, 12, 13, 14, 17, 24, 25, 26, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85  | FDL\_low | - | FDL\_high | -50 | 1 |  |
| n50 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 12, 13, 17, 20, 26, 28, 29, 31, 34, 38, 39, 40, 41, 42, 43, 48, 65, 66, 67, 68 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| n51 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 12, 13, 17, 20, 26, 28, 29, 31, 34, 38, 39, 40, 41, 42, 43, 48, 52, 65, 66, 67, 68, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| n65 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 22, 26, 27, 28, 31, 32, 38, 40, 41, 42, 43, 50, 51, 65, 68, 69, 72, 74, 75, 76,NR Band n78, n79 | FDL\_low  | - | FDL\_high  | -50 | 1 |  |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 34 | FDL\_low | - | FDL\_high | -50 | 1 | 15 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| Frequency range | 1900 | - | 1915 | -15.5 | 5 | 15, 26, 27 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 15, 26, 27 |
| n66, n86 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 25, 26, 27, 28, 29, 30, 38, 41, 43, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| n70 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 24, 25, 26, 29, 30, 41, 48, 66, 70, 71, 85 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| n71 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 30, 48, 53, 66, 85 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 29 | FDL\_low | - | FDL\_high | -38 | 1 | 15 |
| E-UTRA Band 71 | FDL\_low  | - | FDL\_high | -50 | 1 | 15 |
| n74 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 12, 13, 17, 18, 19, 20, 26, 28, 29, 31, 34, 38, 39, 40, 41, 42, 43, 48, 52, 65, 66, 67, 68, 85 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| Frequency range | 1400 | - | 1427 | -32 | 27 | 15, 41 |
| Frequency range | 1475 | - | 1488 | -50 | 1 | 42 |
| Frequency range | 1488 | - | 1518 | -50 | 1 | 15 |
| n77, n78 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n79 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 28, 34, 39, 40, 41, 42, 65 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| n95 | E-UTRA Band 1, 3 , 5, 8, 28, 39, 40, 41,NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| NR Band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 8 |
| NOTE 1: FDL\_low and FDL\_high refer to each frequency band specified in Table 5.2-1 in TS 38.101-1 or Table 5.5-1 in TS 36.101NOTE 2: As exceptions, measurements with a level up to the applicable requirements defined in Table 6.5.3.1-2 are permitted for each assigned NR carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. Due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2 MHz + N x LCRB x RBsize kHz), where N is 2, 3, 4, 5 for the 2nd, 3rd, 4th or 5th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.NOTE 3: 15 kHz SCS is assumed when RB is mentioned in the note when channel bandwidth is less than or equal to 50 MHz, lowest SCS is assumed when channel bandwidth is larger than 50 MHz. The transmission bandwidth in terms of RB position and range is not limited to 15 kHz SCS and shall scale with SCS accordingly.NOTE 4: VoidNOTE 5: For non-synchronised TDD operation to meet these requirements some restriction will be needed for either the operating band or protected bandNOTE 6: N/ANOTE 7: VoidNOTE 8: Applicable when co-existence with PHS system operating in 1884.5 - 1915.7 MHz.NOTE 9: VoidNOTE 10: VoidNOTE 11: VoidNOTE 12: The emissions measurement shall be sufficiently power averaged to ensure a standard deviation < 0.5 dBNOTE 13: This requirement applies for 5, 10, 15 and 20 MHz NR channel bandwidth allocated within 1744.9 MHz and 1784.9 MHz.NOTE 14: VoidNOTE 15: These requirements also apply for the frequency ranges that are less than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth.NOTE 16: VoidNOTE 17: VoidNOTE 18: VoidNOTE 19: Applicable when the assigned NR carrier is confined within 718 MHz and 748 MHz and when the channel bandwidth used is 5 or 10 MHz.NOTE 20: VoidNOTE 21: This requirement is applicable for any channel bandwidths within the range 2500 - 2570 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 2560.5 - 2562.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 2552 - 2560 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.NOTE 22: This requirement is applicable for power class 3 UE for any channel bandwidths within the range 2570 - 2615 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 2605.5 - 2607.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 2597 - 2605 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB. For power class 2 UE for any channel bandwidths within the range 2570 - 2615 MHz, NS\_44 shall apply. For power class 2 or 3 UE for carriers with channel bandwidth overlapping the frequency range 2615 - 2620 MHz the requirement applies with the maximum output power configured to +19 dBm in the IE P-Max.NOTE 23: VoidNOTE 24: As exceptions, measurements with a level up to the applicable requirement of -38 dBm/MHz is permitted for each assigned NR carrier used in the measurement due to 2nd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.3.1-1) for which the 2nd harmonic totally or partially overlaps the measurement bandwidth (MBW).NOTE 25: As exceptions, measurements with a level up to the applicable requirement of -36 dBm/MHz is permitted for each assigned NR carrier used in the measurement due to 3rd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.3.1-1) for which the 3rd harmonic totally or partially overlaps the measurement bandwidth (MBW).NOTE 26: For these adjacent bands, the emission limit could imply risk of harmful interference to UE(s) operating in the protected operating band.NOTE 27: This requirement is applicable for any channel bandwidths within the range 1920 - 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 1930 - 1938 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.NOTE 28: VoidNOTE 29: VoidNOTE 30: This requirement applies when the NR carrier is confined within 2545 – 2575 MHz or 2595 – 2645 MHz and the channel bandwidth is 10 or 20 MHzNOTE 31: VoidNOTE 32: VoidNOTE 33: This requirement is only applicable for carriers with bandwidth confined within 1885-1920 MHz (requirement for carriers with at least 1RB confined within 1880 - 1885 MHz is not specified). This requirement applies for an uplink transmission bandwidth less than or equal to 54 RB for carriers of 15 MHz bandwidth when carrier center frequency is within the range 1892.5 - 1894.5 MHz and for carriers of 20 MHz bandwidth when carrier center frequency is within the range 1895 - 1903 MHz. For 25 MHz, 30 MHz, and 40 MHz channel bandwidths, NS\_45 shall apply.NOTE 34: This requirement is applicable for 5 and 10 MHz NR channel bandwidth allocated within 718-728 MHz. For carriers of 10 MHz bandwidth, this requirement applies for an uplink transmission bandwidth less than or equal to 30 RB with RBstart > 1 and RBstart < 48.NOTE 35: This requirement is applicable in the case of a 10 MHz NR carrier confined within 703 MHz and 733 MHz, otherwise the requirement of -25 dBm with a measurement bandwidth of 8 MHz applies.NOTE 36: VoidNOTE 37: VoidNOTE 38: VoidNOTE 39: VoidNOTE 40: VoidNOTE 41: Applicable for cases and when the lower edge of the assigned NR UL channel bandwidth frequency is greater than or equal to 1427 MHz + the channel BW assigned for 5 and 10 MHz bandwidth, and when the lower edge of the assigned NR UL channel bandwidth frequency is greater than or equal to 1440 MHz for 15 and 20 MHz bandwidth.NOTE 42: Applicable for 5 MHz bandwidth, and when the upper edge of the assigned NR UL channel bandwidth frequency is less than or equal to 1467 MHz assigned for 10 MHz bandwidth, and when the upper edge of the assigned NR UL channel bandwidth frequency is less than or equal to 1463.8 MHz for 15 MHz bandwidth, and when the upper edge of the assigned NR UL channel bandwidth frequency is less than or equal to 1460.8 MHz for 20 MHz bandwidth. |

NOTE: To simplify Table 6.5.3.2-1, E-UTRA band numbers are listed for bands which are specified only for E-UTRA operation or both E-UTRA and NR operation. NR band numbers are listed for bands which are specified only for NR operation.

## **<Next of Changes>**

##### 6.5A.3.2.3 Spurious emissions for UE co-existence for Inter-band CA

For inter-band carrier aggregation with the uplink assigned to two NR bands, the requirements in Table 6.5A.3.2.3-1 apply on each component carrier with all component carriers are active.

NOTE: For inter-band carrier aggregation with uplink assigned to two NR bands the requirements in Table 6.5A.3.2.3-1 could be verified by measuring spurious emissions at the specific frequencies where second and third order intermodulation products generated by the two transmitted carriers can occur; in that case, the requirements for remaining applicable frequencies in Table 6.5A.3.2.3-1 would be considered to be verified by the measurements verifying the one uplink inter-band CA UE to UE co-existence requirements.

Table 6.5A.3.2.3-1: Requirements for uplink inter-band carrier aggregation (two bands)

|  |  |
| --- | --- |
| NR CA combination | Spurious emission |
| Protected Band | Frequency range (MHz) | Maximum Level (dBm) | MBW (MHz) | NOTE |
| CA\_n1-n3 | E-UTRA Band 1, 5, 7, 8, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 38, 40, 41, 43, 44, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |   |
| E-UTRA band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| E-UTRA band 22, 42, 52NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 17 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 4,6 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 4, 6, 7 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 4, 6, 7 |
| CA\_n1-n7 | E-UTRA Band 1, 5, 7, 8, 20, 22, 26, 27, 28, 31,32, 40, 42, 43, 50, 51, 52, 65, 67, 68, 72, 74, 75, 76NR Band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| band n77 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 4, 6 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 4. 7, 6 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 4. 7, 6 |
| Frequency range | 2570  | -  | 2575 | +1.6 | 5 | 4, 7, 18 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 4, 7, 18 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 4, 18 |
| CA\_n1-n8 | E-UTRA Band 20, 28, 31, 32, 38, 40, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 22, 41, 42, 43NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1, 8, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 4, 6 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 4, 6, 7 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 4, 6, 7 |
| CA\_n1-n28 | E-UTRA Band 5, 7, 8, 18, 19, 20, 26, 27, 31, 32, 38, 40, 41, 50, 51, 72, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 43, 75, 76NR band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 11, 15 |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 11, 12 |
| Frequency range | 470 | - | 694 | -42 | 8 | 4, 14 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 15 |
| Frequency range | 758 | - | 773 | -30 | 1 | 4 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 4 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 4, 6 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 4, 6, 7 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 4, 6, 7 |
| Frequency range | 1839.9 | - | 1879.9 | -50 | 1 | 4 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 11, 17 |
| CA\_n1-n41 | E-UTRA Band 1, 3, 5, 8, 26, 27, 28, 42, 44, 45, 50, 51, 52, 65, 73, 74NR Band n78 | FDL\_low | - | FDL\_high | -50 | 1 |   |
| E-UTRA band 34 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| NR Band n77, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 10 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 10 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 4,6 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 4, 6, 7 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 4, 6, 7 |
| CA\_n1-n78 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 4, 6 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 4, 6, 7 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 4, 6, 7 |
| CA\_n1-n79 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 21, 26, 28, 34, 40, 41, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 4, 6 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 4, 6, 7 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 4, 6, 7 |
| CA\_n2-n5 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 25, 26, 28, 29, 30, 42, 48, 50, 51, 53, 66, 70, 71, 74, 85,  | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, 43 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| CA\_n2-n48 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 25, 26, 29, 30, 41, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| CA\_n3-n8 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 44, 50, 51, 65, 67, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 8 | FDL\_low | - | FDL\_high | -50 | 1 | 2, 4 |
| E-UTRA band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 7, 22, 41, 42, 43, 52NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 860 | - | 890 | -40 | 1 | 4, 5 |
| CA\_n3-n28 | E-UTRA Band 5, 7, 8, 18, 19, 20, 26, 27, 31, 32, 38, 40, 41, 50, 51, 72, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42, 43, 75, 76NR band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 11, 15 |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 11, 12 |
| Frequency range | 470 | - | 694 | -42 | 8 | 4, 14 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 15 |
| Frequency range | 758 | - | 773 | -30 | 1 | 4 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 4 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 4, 6 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 4, 6, 7 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 4, 6, 7 |
| Frequency range | 1839.9 | - | 1879.9 | -50 | 1 | 4 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 11, 17 |
| CA\_n3-n40 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 38, 39, 41, 43, 44. 45, 50, 51, 65, 67, 68, 69, 72, 73, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| UTRA Band 22, 42, 52NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 13 |
| CA\_n3-n41 | E-UTRA Band 1, 5, 8, 20, 26, 27, 28, 34, 39, 40, 44, 45, 50, 51, 65, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| E-UTRA Band 11, 18, 19, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| E-UTRA Band 42,NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| CA\_n3-n77 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| CA\_n3-n78 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| CA\_n3-n79 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| CA\_n5-n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 24, 25, 28, 29, 30, 31, 34, 38, 40, 42, 43, 45, 48, 65, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 7 |
| CA\_n5-n79 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 24, 25, 28, 29, 30, 31, 34, 38, 40, 42, 43, 45, 48, 50, 51, 65, 66, 70, 71, 73, 74, 85 | FDL\_low | - | FDL\_high |  |  |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| CA\_n7-n28 | E-UTRA Band 2, 3, 5, 7, 8, 20, 26, 27, 31, 34, 40 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 4, 10, 42, 43, 50, 51, 65, 66, 74, 75, 76NR band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band n1 | FDL\_low | - | FDL\_high | -50 | 1 | 11, 12 |
| Frequency range | 758 | - | 773 | -32 | 1 | 4 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 2570  | -  | 2575 | +1.6 | 5 | 4, 7, 18 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 4, 7, 18 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 4, 18 |
| CA\_n7-n66 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 26, 27, 28, 29, 30, 43, 66, 71, , 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 4, 7, 18 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 4, 7, 18 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 4, 18 |
| CA\_n7-n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 33, 34, 40, 50, 51, 65, 66, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570 | - | 2575 | +1.6 | 5 | 4, 7, 18 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 4, 7, 18 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 4, 18 |
| CA\_n8-n39 | E-UTRA Band 1, 28, 34, 40, 50, 51, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 22, 41, 42NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA 8 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| CA\_n8-n40 | E-UTRA Bands 1, 20, 28, 31, 32, 33, 34, 38, 39, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| UTRA Bands 3, 7, 22, 41, 42, 43, 52NR Bands n77, n78, n79 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| Band 8 | FDL\_low  | - | FDL\_high | -50 | 1 | 4 |
| Frequency range | 860 | - | 890 | -40 | 1 | 4, 5 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 5 |
| CA\_n8-n41 | E-UTRA Band 1, 28, 34, 39, 40, 45, 50, 51, 65, 73,74, NR band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| CA\_n8-n78 | E-UTRA Band 1, 8, 20, 28, 34, 39, 40, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 860 | - | 890 | -40 | 1 | 4,5 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| CA\_n8-n79 | E-UTRA Band 1, 8, 28, 34, 39, 40, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 41, 42  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 860 | - | 890 | -40 | 1 | 4, 5 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| CA\_n20-n28 | E-UTRA Band 1, 3, 7, 22, 28, 31, 32, 34, 38, 42, 43, 65, 75, 76NR Band n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| CA\_n20-n78 | E-UTRA Band 1, 3, 7, 8, 34, 40, 65 | FDL\_low | - | FDL\_high | -50 | 1 |   |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| E-UTRA Band 38, 69 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| CA\_n25-n41 | E-UTRA Band 4, 5, 10, 12, 13 , 14, 17, 24, 26, 27, 28, 29, 30, 42, 48, 66, 70, 71,85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 4 |
| CA\_n28-n41 | E-UTRA Band 2, 3, 5, 8, 25, 26, 27, 34 | FDL\_low | - | FDL\_high | -50 | 1 |   |
| E-UTRA Band 4, 10, 42, 50, 51, 52, 65, 66, 73, 74NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 18, 19 | FDL\_low | - | FDL\_high | -50 | 1 | 10 |
| Frequency range | 470 | - | 694 | -42 | 8 | 4, 14 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 13 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 4 |
| Frequency range | 758 | - | 773 | -32 | 1 | 4 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 10, 11 |
| CA\_n28-n50 | E-UTRA Band 2, 3, 5, 7, 8, 18, 19, 25, 26, 27, 29, 31, 34, 38, 39, 40, 41, 48, 52, 67, 72, 85NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 12, 13, 17, 22, 42, 43, 52, 65, 66, 73NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 10, 11 |
| Frequency range | 470 | - | 694 | -42 | 8 | 4, 14 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 13 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 4 |
| Frequency range | 758 | - | 773 | -32 | 1 | 4 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 11 |
| CA\_n28-n77 | E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 34, 39, 40, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 11 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 11 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range |  1884.5 | - | 1915.7 | -41 | 0.3 | 3, 11 |
| CA\_n28-n78 | E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 34, 39, 40, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 11 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 11 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range |  1884.5 | - | 1915.7 | -41 | 0.3 | 3, 11 |
| CA\_n39-n40 | E-UTRA Band 1, 8, 22, 26, 28, 34, 41, 42, 44, 45, 50, 51, 52, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78, n79 | FDL\_low  | -  | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1805 |  | 1855 | -40 | 1 | 8 |
| Frequency range | 1855 |  | 1880 | -15.5 | 5 | 4, 7, 8 |
| CA\_n39-n41 | E-UTRA Band 1, 8, 26, 28, 34, 40, 42, 44, 45, 50, 51, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 4 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 4, 7, 8 |
| CA\_n39-n79 | E-UTRA Band 1, 8, 28, 34, 40, 41, 44, 45NR Band n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 4, 8 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 4, 7, 8 |
| CA\_n40-n41 | E-UTRA Band 1, 3, 5, 8, 26, 27, 28, 34, 39, 42, 44, 45, 50, 51, 65, 73, 74,NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 10 |
| CA\_n40-n79 | E-UTRA Band 1, 3, 5, 8, 28, 34, 39, 41, 42, 65, | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 10 |
| CA\_n41-n50 | E-UTRA Band 1, 2, 3, 4, 5, 8, 10, 12, 13 , 14, 17, 20, 24, 25, 26, 27, 28, 29, 30, 31, 34, 38, 39, 40, 42, 43, 44, 45, 48, 52, 65, 66, 67, 68, 70, 71, 73, 85NR Band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| CA\_n41-n79 | E-UTRA Band 1, 3, 5, 8, 9, 11, 18, 19, 21, 28, 34, 40, 42, 44, 45, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| CA\_n48-n66 | E-UTRA Band 2, 4, 5, 7, 10, 12, 13, 14, 17, 24, 25, 26, 27, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| CA\_n50-n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 17, 20, 25, 26, 27, 28, 29, 31, 33, 34, 38, 39, 40, 41, 44, 48, 65, 66, 67, 68, 69, 72, 73, 85NR Band n79 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| CA\_n66-n78 | E-UTRA Band 2, 4, 5, 7, 12, 13, 14, 17, 29, 26, 28, 41, 66, 71 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| NOTE 1: FDL\_low and FDL\_high refer to each frequency band specified in Table 5.2-1 in TS 38.101-1 or Table 5.5-1 in TS 36.101NOTE 2: As exceptions, measurements with a level up to the applicable requirements defined in Table 6.5.3.1-2 are permitted for each assigned NR carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. Due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2 MHz + N x LCRB x 180kHz), where N is 2, 3, 4, 5 for the 2nd, 3rd, 4th or 5th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.NOTE 3: Applicable when co-existence with PHS system operating in 1884.5 -1915.7 MHzNOTE 4: These requirements also apply for the frequency ranges that are less than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth.NOTE 5: This requirement is applicable only for the following cases: A: for carriers of 5 MHz channel bandwidth when carrier centre frequency (Fc) is within the range 902.5 MHz ≤ Fc < 907.5 MHz with an uplink transmission bandwidth less than or equal to 20 RB; B: for carriers of 5 MHz channel bandwidth when carrier centre frequency (Fc) is within the range 907.5 MHz ≤ Fc ≤ 912.5 MHz without any restriction on uplink transmission bandwidth; D: for carriers of 10 MHz channel bandwidth when carrier centre frequency (Fc) is Fc = 910 MHz with an uplink transmission bandwidth less than or equal to 32 RB with RBstart > 3.NOTE 6: This requirement is applicable for any channel bandwidths within the range 1920 – 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 1930 – 1938 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.NOTE 7: For these adjacent bands, the emission limit could imply risk of harmful interference to UE(s) operating in the protected operating band.NOTE 8: This requirement is only applicable for carriers with bandwidth confined within 1885-1920 MHz (requirement for carriers with at least 1RB confined within 1880 - 1885 MHz is not specified). This requirement applies for an uplink transmission bandwidth less than or equal to 54 RB for carriers of 15 MHz bandwidth when carrier center frequency is within the range 1892.5 - 1894.5 MHz and for carriers of 20 MHz bandwidth when carrier center frequency is within the range 1895 - 1903 MHz.NOTE 9: This requirement applies for 5, 10, 15 and 20 MHz NR channel bandwidth allocated within 1744.9 MHz and 1784.9 MHz.NOTE 10: This requirement applies when the NR carrier is confined within 2545 - 2575 MHz or 2595 – 2645vMHz and the channel bandwidth is 10 or 20 MHz.NOTE 11:Applicable when the assigned NR carrier is confined within 718 MHz and 748 MHz and when the channel bandwidth used is 5 or 10 MHz.NOTE 12: As exceptions, measurements with a level up to the applicable requirement of -36 dBm/MHz is permitted for each assigned NR carrier used in the measurement due to 3rd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.3.1-1) for which the 3rd harmonic totally or partially overlaps the measurement bandwidth (MBW).NOTE 13: This requirement is applicable for 5 and 10 MHz NR channel bandwidth allocated within 718 - 728 MHz. For carriers of 10 MHz bandwidth, this requirement applies for an uplink transmission bandwidth less than or equal to 30 RB with RBstart > 1 and Rbstart < 48.NOTE 14: This requirement is applicable in the case of a 10 MHz NR carrier confined within 703 MHz and 733 MHz, otherwise the requirement of -25 dBm with a measurement bandwidth of 8 MHz applies.NOTE 15: As exceptions, measurements with a level up to the applicable requirement of -38 dBm/MHz is permitted for each assigned E-UTRA carrier used in the measurement due to 3rd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.6-1) for which the 3rd harmonic totally or partially overlaps the measurement bandwidth (MBW).NOTE 17: Applicable when NS\_05 in clause 6.6.3.3.1 is signalled by the network.NOTE 18: This requirement is applicable for any channel bandwidths within the range 2500 – 2570 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 2560.5 - 2562.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 2552 – 2560 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB. |

NOTE: To simplify Table 6.5A.3.2.3-1, E-UTRA band numbers are listed for bands which are specified only for E-UTRA operation or both E-UTRA and NR operation. NR band numbers are listed for bands which are specified only for NR operation.

## **<Next of Changes>**

##### 6.5.3.3.3 Requirement for network signalled value "NS\_18"

When "NS\_18" is indicated in the cell, the power of any UE emission shall not exceed the levels specified in Table 6.5.3.3. 3-1. This requirement also applies for the frequency ranges that are less than FOOB (MHz) in Table 6.5.3.1-1 from the edge of the channel bandwidth.

Table 6.5.3.3.3-1: Additional requirements for "NS\_18"

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency range(MHz) | Channel bandwidth / Spectrum emission limit (dBm) | Measurement bandwidth  |  |
| 5, 10, 15, 20, 30 MHz |
| 692-698 | -26.2 | 6 MHz |  |

## **<Next of Changes>**

### 7.3.2 Reference sensitivity power level

The throughput shall be ≥ 95 % of the maximum throughput of the reference measurement channels as specified in Annexes A.2.2.2, A.2.3.2, A3.2 and A.3.3 (with one sided dynamic OCNG Pattern OP.1 FDD/TDD for the DL-signal as described in Annex A.5.1.1/A.5.2.1) with parameters specified in Table 7.3.2-1 and Table 7.3.2-2.

Table 7.3.2-1: Two antenna port reference sensitivity QPSK PREFSENS

|  | Operating band / SCS / Channel bandwidth / Duplex-mode |
| --- | --- |
| Operating Band | SCS kHz | 5MHz(dBm) | 10MHz(dBm) | 15MHz(dBm) | 20MHz(dBm) | 25MHz(dBm) | 30 MHz (dBm) | 40MHz(dBm) | 50MHz(dBm) | 60MHz(dBm) | 70MHz(dBm) | 80MHz(dBm) | 90MHz(dBm) | 100 MHz(dBm) | Duplex Mode |
| n1 | 15 | -100.0 | -96.8 | -95.0 | -93.8 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -97.1 | -95.1 | -94.0 |  |  |  |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 |  |  |  |  |  |  |  |  |  |
| n2 | 15 | -98.0 | -94.8 | -93.0 | -91.8 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -95.1 | -93.1 | -92.0 |  |  |  |  |  |  |  |  |  |
| 60 |  | -95.5 | -93.4 | -92.2 |  |  |  |  |  |  |  |  |  |
| n3 | 15 | -97.0 | -93.8 | -92.0 | -90.8 | -89.7 | -88.9 |  |  |  |  |  |  |  | FDD |
| 30 |  | -94.1 | -92.1 | -91.0 | -89.8 | -89.0 |  |  |  |  |  |  |  |
| 60 |  | -94.5 | -92.4 | -91.2 | -90.0 | -89.1 |  |  |  |  |  |  |  |
| n5 | 15 | -98.0 | -94.8 | -93.0 | -86.8 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -95.1 | -93.1 | -88.6 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n71 | 15 | -98.0 | -94.8 | -93.0 | -91.8 | -90.7 | -89.9 | -88.6 | -81.5 |  |  |  |  |  | FDD |
| 30 |  | -95.1 | -93.1 | -92.0 | -90.8 | -90.0 | -88.7 | -81.5 |  |  |  |  |  |
| 60 |  | -95.5 | -93.4 | -92.2 | -91.0 | -90.1 | -88.9 | -81.5 |  |  |  |  |  |
| n8 | 15 | -97.0 | -93.8 | -91.4 | -85.8 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -94.1 | -91.7 | -87.2 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | 15 | -97.0 | -93.8 | -84.0 |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -94.1 | -84.1 |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | 15 | -97.0 | -93.8 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -94.1 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | 15 | -100.0 | -96.8 | -95.0 |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -97.1 | -95.1 |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n20 | 15 | -97.0 | -93.8 | -91.0 | -89.8 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -94.1 | -91.1 | -90.0 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n25 | 15 | -96.5 | -93.3 | -91.5 | -90.3 | -89.3 | -82.2 | -79.5 |  |  |  |  |  |  | FDD |
| 30 |  | -93.6 | -91.6 | -90.5 | -89.4 | -82.3 | -79.6 |  |  |  |  |  |  |
| 60 |  | -94.0 | -91.9 | -90.7 | -89.6 | -82.4 | -79.7 |  |  |  |  |  |  |
| n28 | 15 | -98.5 | -95.5 | -93.5 | -90.8 |  | [-78.5] |  |  |  |  |  |  |  | FDD |
| 30 |  | -95.6 | -93.6 | -91.0 |  | [-78.6] |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | 15 | -99.0 | -95.8 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -96.1 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | 15 | -100.0 | -96.8 | -95.0 |  |  |  |  |  |  |  |  |  |  | TDD |
| 30 |  | -97.1 | -95.1 |  |  |  |  |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 |  |  |  |  |  |  |  |  |  |  |
| n381 | 15 | -100.0 | -96.8 | -95.0 | -93.8 |  |  | -90.6 |  |  |  |  |  |  | TDD |
| 30 |  | -97.1 | -95.1 | -94.0 |  |  | -90.7 |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 |  |  | -90.9 |  |  |  |  |  |  |
| n39 | 15 | -100.0 | -96.8 | -95.0 | -93.8 | -92.7 | -91.9 | -90.6 |  |  |  |  |  |  | TDD |
| 30 |  | -97.1 | -95.1 | -94.0 | -92.8 | -92.0 | -90.7 |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 | -93.0 | -92.1 | -90.9 |  |  |  |  |  |  |
| n40 | 15 | -100.0 | -96.8 | -95.0 | -93.8 | -92.7 | -91.9 | -90.6 | -89.6 |  |  |  |  |  | TDD |
| 30 |  | -97.1 | -95.1 | -94.0 | -92.8 | -92.0 | -90.7 | -89.7 | -88.9 |  | -87.6 |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 | -93.0 | -92.1 | -90.9 | -89.8 | -89.1 |  | -87.6 |  |  |
| n411 | 15 |  | -94.8 | -93.0 | -91.8 |  | -89.9 | -88.6 | -87.6 |  |  |  |  |  | TDD |
| 30 |  | -95.1 | -93.1 | -92.0 |  | -90.0 | -88.7 | -87.7 | -86.9 |  | -85.6 | -85.1 | -84.7 |
| 60 |  | -95.5 | -93.4 | -92.2 |  | -90.1 | -88.9 | -87.8 | -87.1 |  | -85.6 | -85.1 | -84.7 |
| n481 | 15 | -99 | -95.8 | -94.0 | -92.7 |  |  | -89.6 | -88.65 |  |  |  |  |  | TDD |
| 30 |  | -96.1 | -94.1 | -92.9 |  |  | -89.7 | -88.75 | -87.95 |  | -86.65 | -86.15 | -85.65 |
| 60 |  | -96.5 | -94.4 | -93.1 |  |  | -89.9 | -88.85 | -88.05 |  | -86.75 | -86.25 | -85.75 |
| n50 | 15 | -100.0 | -96.8 | -95.0 | -93.8 |  | -91.9 | -90.6 | -89.6 |  |  |  |  |  | TDD |
| 30 |  | -97.1 | -95.1 | -94.0 |  | -92.0 | -90.7 | -89.7 | -88.9 |  | -87.6 |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 |  | -92.1 | -90.9 | -89.8 | -89.1 |  | -87.6 |  |  |
| n51 | 15 | -100.0 |  |  |  |  |  |  |  |  |  |  |  |  | TDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n65 | 15 | -99.5 | -96.3 | -94.5 | -93.3 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -96.6 | -94.6 | -93.5 |  |  |  |  |  |  |  |  |  |
| 60 |  | -97.0 | -94.9 | -93.7 |  |  |  |  |  |  |  |  |  |
| n66 | 15 | -99.5 | -96.3 | -94.5 | -93.3 |  |  | -90.1 |  |  |  |  |  |  | FDD |
| 30 |  | -96.6 | -94.6 | -93.5 |  |  | -90.2 |  |  |  |  |  |  |
| 60 |  | -97.0 | -94.9 | -93.7 |  |  | -90.4 |  |  |  |  |  |  |
| n70 | 15 | -100.0 | -96.8 | -95.0 | -93.8 | -92.7 |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -97.1 | -95.1 | -94.0 | -92.8 |  |  |  |  |  |  |  |  |
| 60 |  | -97.5 | -95.4 | -94.2 | -93.0 |  |  |  |  |  |  |  |  |
| n71 | 15 | -97.2 | -94.0 | -91.6 | -86.0 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -94.3 | -91.9 | -87.4 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n74 | 15 | -99.53 | -96.33 | -94.53 | -89.33 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -96.63 | -94.63 | -89.53 |  |  |  |  |  |  |  |  |  |
| 60 |  | -97.03 | -94.93 | -89.63 |  |  |  |  |  |  |  |  |  |
| n771,4 | 15 |  | -95.3 | -93.5 | -92.2 | -91.2 | -90.4 | -89.1 | -88.1 |  |  |  |  |  | TDD |
| 30 |  | -95.6 | -93.6 | -92.4 | -91.3 | -90.5 | -89.2 | -88.2 | -87.4 | -86.7 | -86.1 | -85.6 | -85.1 |
| 60 |  | -96.0 | -93.9 | -92.6 | -91.5 | -90.6 | -89.4 | -88.3 | -87.5 | -86.8 | -86.2 | -85.7 | -85.2 |
| n781 | 15 |  | -95.8 | -94.0 | -92.7 | -91.7 | -90.9 | -89.6 | -88.6 |  |  |  |  |  | TDD |
| 30 |  | -96.1 | -94.1 | -92.9 | -91.8 | -91 | -89.7 | -88.7 | -87.9 | -87.2 | -86.6 | -86.1 | -85.6 |
| 60 |  | -96.5 | -94.4 | -93.1 | -92 | -91.1 | -89.9 | -88.8 | -88.0 | -87.3 | -86.7 | -86.2 | -85.7 |
| n791 | 15 |  |  |  |  |  |  | -89.6 | -88.6 |  |  |  |  |  | TDD |
| 30 |  |  |  |  |  |  | -89.7 | -88.7 | -87.9 |  | -86.6 |  | -85.6 |
| 60 |  |  |  |  |  |  | -89.9 | -88.8 | -88.0 |  | -86.7 |  | -85.7 |
| n91 | 15 | -100 |  |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n92 | 15 | -100 | -96.8 | -95.0 | -93.8 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -97.1 | -95.1 | -94.0 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | 15 | -100 |  |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n94 | 15 | -100 | -96.8 | -95.0 | -93.8 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | -97.1 | -95.1 | -94.0 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: Four Rx antenna ports shall be the baseline for this operating band except for two Rx vehicular UE.NOTE 2: The transmitter shall be set to PUMAX as defined in clause 6.2.4NOTE 3: The requirement is modified by -0.5 dB when the assigned NR channel bandwidth is confined within 1475.9 - 1510.9 MHz.NOTE 4: The requirement is modified by -0.5 dB when the assigned UE channel bandwidth is confined within 3300 - 3800 MHz.NOTE 5: For these bandwidths, the minimum requirements are restricted to operation when carrier is configured as a downlink carrier part of CA configuration |

For UE(s) equipped with 4 Rx antenna ports, reference sensitivity for 2Rx antenna ports in Table 7.3.2-1 shall be modified by the amount given in ΔRIB,4R in Table 7.3.2-2 for the applicable operating bands.

Table 7.3.2-2: Four antenna port reference sensitivity allowance ΔRIB,4R

|  |  |
| --- | --- |
| Operating band | ΔRIB,4R (dB) |
| n28, n71 | -2.71 |
| n1, n2, n3, n40, n7, n34, n38, n39, n41, n66, n70 | -2.7 |
| n48, n77, n78, n79 | -2.2 |
| NOTE 1: 4 Rx operation is targeted for FWA form factor |

The reference receive sensitivity (REFSENS) requirement specified in Table 7.3.2-1 and Table 7.3.2-2 shall be met with uplink transmission bandwidth less than or equal to that specified in Table 7.3.2-3.

Table 7.3.2-3: Uplink configuration for reference sensitivity

|  | Operating band / SCS / Channel bandwidth / Duplex mode |
| --- | --- |
| Operating Band | SCS kHz | 5MHz | 10MHz | 15MHz | 20MHz | 25 MHz | 30 MHz | 40MHz | 50MHz | 60MHz | 70MHz | 80MHz | 90MHz | 100 MHz | Duplex Mode |
| n1 | 15 | 25 | 501 | 751 | 1001 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | 501 |  |  |  |  |  |  |  |  |  |
| 60 |  | 101 | 18 | 24 |  |  |  |  |  |  |  |  |  |
| n2 | 15 | 25 | 501 | 501 | 501 |  |  |  |  |  |  |  |  |  | FDD |
| 30 | 101 | 24 | 241 | 241 |  |  |  |  |  |  |  |  |  |
| 60 |  | 101 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| n3 | 15 | 25 | 501 | 501 | 501 | 501 | 501  |  |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 241 | 241 | 241 | 241 |  |  |  |  |  |  |  |
| 60 |  | 101 | 101 | 101 | 101 | 101 |  |  |  |  |  |  |  |
| n5 | 15 | 25 | 251 | 201 | 201 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | 101 | 101  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n7 | 15 | 25 | 501 | 751 | 751 | 721 | 641 | 451 | 451 |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | 361 | 361 | 321 | 201 | 201 |  |  |  |  |  |
| 60 |  | 101 | 18 | 181 | 181 | 161 | 101 | 101 |  |  |  |  |  |
| n8 | 15 | 25 | 251 | 201 | 201 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n12 | 15 | 201 | 201 | 201 |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n14 | 15 | 201 | 201 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n18 | 15 | 25 | 251 | 251 |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n20 | 15 | 25 | 201 | 202 | 202 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 102 | 102 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n25 | 15 | 25 | 501 | 501 | 501 | 501 | 481 | 401 |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 241 | 241 | 241 | 241 | 201 |  |  |  |  |  |  |
| 60 |  | 101 | 101 | 101 | 101 | 101 | 101 |  |  |  |  |  |  |
| n28 | 15 | 25 | 251 | 251 | 251 |  | 251 |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 | 101 |  | 101 |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n30 | 15 | 201 | 201 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n34 | 15 | 25 | 50 | 75 |  |  |  |  |  |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 |  |  |  |  |  |  |  |  |  |  |
| 60 |  | 10 | 18 |  |  |  |  |  |  |  |  |  |  |
| n38 | 15 | 25 | 50 | 75 | 100 |  |  | 216 |  |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 |  |  | 100 |  |  |  |  |  |  |
| 60 |  | 10 | 18 | 24 |  |  | 50 |  |  |  |  |  |  |
| n39 | 15 | 25 | 50 | 75 | 100 | 128 | 160 | 216 |  |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 |  |  |  |  |  |  |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 |  |  |  |  |  |  |
| n40 | 15 | 25 | 50 | 75 | 100 | 128 | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 | 128 | 162 |  | 216 |  |  |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 | 64 | 75 |  | 100 |  |  |
| n41 | 15 |  | 50 | 75 | 100 |  | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 |  | 75 | 100 | 128 | 162 |  | 216 | 243 | 270 |
| 60 |  | 10 | 18 | 24 |  | 36 | 50 | 64 | 75 |  | 100 | 120 | 135 |
| n48 | 15 | 25 | 50 | 75 | 100 |  |  | 216 |  |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 |  |  | 100 |  |  |  |  |  |  |
| 60 |  | 10 | 18 | 24 |  |  | 50 |  |  |  |  |  |  |
| n50 | 15 | 25 | 50 | 75 | 100 |  | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 |  | 75 | 100 | 128 | 162 |  | NOTE 3 |  |  |
| 60 |  | 10 | 18 | 24 |  | 36 | 50 | 64 | 75 |  | NOTE 3 |  |  |
| n51 | 15 | 25 |  |  |  |  |  |  |  |  |  |  |  |  | TDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n65 | 15 | 25 | 501 | 751 | 1001 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | 501 |  |  |  |  |  |  |  |  |  |
| 60 |  | 101 | 18 | 24 |  |  |  |  |  |  |  |  |  |
| n66 | 15 | 25 | 501 | 751 | 1001 |  |  | 216 |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | 501 |  |  | 1001 |  |  |  |  |  |  |
| 60 |  | 101 | 18 | 24 |  |  | 501 |  |  |  |  |  |  |
| n70 | 15 | 25 | 501 | 751 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 24 | 361 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  |
| 60 |  | 101 | 18 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  |
| n71 | 15 | 25 | 251 | 201 | 201 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n74 | 15 | 25 | 251 | 251 | 251 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | 101 | 101 |  |  |  |  |  |  |  |  |  |
| 60 |  | 51 | 51 | 51 |  |  |  |  |  |  |  |  |  |
| n77 | 15 |  | 50 | 75 | 100 | 128 | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 | 128 | 162 | 180 | 216 | 243 | 270 |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 | 64 | 75 | 90 | 100 | 120 | 135 |
| n78 | 15 |  | 50 | 75 | 100 | 128 | 160 | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  | 24 | 36 | 50 | 64 | 75 | 100 | 128 | 162 | 180 | 216 | 243 | 270 |
| 60 |  | 10 | 18 | 24 | 30 | 36 | 50 | 64 | 75 | 90 | 100 | 120 | 135 |
| n79 | 15 |  |  |  |  |  |  | 216 | 270 |  |  |  |  |  | TDD |
| 30 |  |  |  |  |  |  | 100 | 128 | 162 |  | 216 |  | 270 |
| 60 |  |  |  |  |  |  | 50 | 64 | 75 |  | 100 |  | 135 |
| n91 | 15 | 254 | 201,4 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n92 | 15 | 25 | 201 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 101 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n93 | 15 | 254 | 251,4 |  |  |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| n94 | 15 | 25 | 251 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  |  | FDD |
| 30 |  | 121 | NOTE 3 | NOTE 3 |  |  |  |  |  |  |  |  |  |
| 60 |  |  |  |  |  |  |  |  |  |  |  |  |  |
| NOTE 1: UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission bandwidth configuration for the channel bandwidth (Table 5.3.2-1).NOTE 2: For Band 20; for 15 kHz SCS, in the case of 15 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 11 and in the case of 20 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 16; for 30 kHz SCS, in the case of 15 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 6 and in the case of 20 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 8; for 60 kHz SCS, in the case of 15 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 3 and in the case of 20 MHz channel bandwidth, the UL resource blocks shall be located at RBstart 4;NOTE 3: For DL channel bandwidths that do not have symmetric UL channel bandwidth, highest valid UL configuration with lowest TX-RX separation (Table 5.4.4-1) shall be used.NOTE 4: For band n91 and n93, largest supported UL bandwidth configuration shall be used. |

Unless given by Table 7.3.2-4, the minimum requirements specified in Tables 7.3.2-1 and 7.3.2-2 shall be verified with the network signalling value NS\_01 (Table 6.2.3-1) configured.

Table 7.3.2-4: Network signaling value for reference sensitivity

|  |  |
| --- | --- |
| Operating band | Network Signalling value |
| n2 | NS\_03 |
| n12 | NS\_06 |
| n14 | NS\_06 |
| n25 | NS\_03 |
| n30 | NS\_21 |
| n48 | NS\_27 |
| n66 | NS\_03 |
| n70 | NS\_03 |
| n71 | NS\_35 |

## **<End of Changes>**