**3GPP TSG-RAN WG4 Meeting #96 *R4-200XXXX***

**Online, 17th Aug - 28th Aug 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-1** | **CR** |  | **rev** | **2** | **Current version:** | **15.9.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | VODAFONE Group Plc | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core | | | | |  | ***Date:*** | | | 2020-09-03 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12) Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Make it known in the Rel-15 spec that a 7.5 kHz uplink shift is required for spectrum sharing solutions in Band 38/n38 as specified in TS38.307 and Rel-16 onwards. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Clause 5.4.2.1: 7.5 kHz uplink shift applicable for Band [n38] | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Potential for two tracks of implementation with not all n38 devices supporting DSS. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.4.2.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **x** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

|  |  |
| --- | --- |
|  |  |

*< start of changes >*

### 5.4.2 Channel raster

#### 5.4.2.1 NR-ARFCN and channel raster

The global frequency channel raster defines a set of RF reference frequencies FREF. The RF reference frequency is used in signalling to identify the position of RF channels, SS blocks and other elements.

The global frequency raster is defined for all frequencies from 0 to 100 GHz. The granularity of the global frequency raster is ΔFGlobal.

RF reference frequencies are designated by an NR Absolute Radio Frequency Channel Number (NR-ARFCN) in the range (0…2016666) on the global frequency raster. The relation between the NR-ARFCN and the RF reference frequency FREF in MHz is given by the following equation, where FREF-Offs and NRef-Offs are given in table 5.4.2.1-1 and NREF is the NR-ARFCN.

FREF = FREF-Offs + ΔFGlobal (NREF – NREF-Offs)

Table 5.4.2.1-1: NR-ARFCN parameters for the global frequency raster

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Frequency range (MHz) | ΔFGlobal (kHz) | FREF-Offs (MHz) | NREF-Offs | Range of NREF |
| 0 – 3000 | 5 | 0 | 0 | 0 – 599999 |
| 3000 – 24250 | 15 | 3000 | 600000 | 600000 – 2016666 |

The channel raster defines a subset of RF reference frequencies that can be used to identify the RF channel position in the uplink and downlink. The RF reference frequency for an RF channel maps to a resource element on the carrier. For each operating band, a subset of frequencies from the global frequency raster are applicable for that band and forms a channel raster with a granularity ΔFRaster, which may be equal to or larger than ΔFGlobal.

For SUL bands and for the uplink of all FDD bands defined in Table 5.2-1.

FREF, shift = FREF + Δshift, Δshift = 0 kHz or 7.5 kHz.

where Δshift is signalled by the network in higher layer parameter *frequencyShift7p5khz* [7].

NOTE: The FREF.shift requirement is introduced in a Release-independent manner to UEs operating n38 uplink transmissions with a 15kHz SCS, as specified in TS38.307 in later release specifications. A Release 15 UE not supporting this requirement will not be able to access a network operating n38 with ∆shift configured to 7.5kHz.

The mapping between the channel raster and corresponding resource element is given in Clause 5.4.2.2. The applicable entries for each operating band are defined in Clause 5.4.2.3

*< end of changes >*