**3GPP TSG-RAN4 Meeting #97-e *R4-2016496***

**Electronic Meeting, 2nd - 13th November, 2020**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-3** | **CR** | **0423** | **rev** | **1** | **Current version:** | **15.11.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for TS 38.101-3: correction of spurious emission band UE co-existence (R15) |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2020-10-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-15 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | For Rel-15 EN-DC combos listed in summary of change, the requirements for spurious emission band UE co-existence are incorrect. |
|  |  |
| ***Summary of change:*** | For DC\_2\_n5, DC\_8\_n78, DC\_12\_n66, DC\_30\_n5, some errors are corrected by the following changes:1. Adding new protected bands to aligh with the latest 36.101 and 38.101.
2. Correcting those wrong Notes.
3. Deleting those repeated protected bands.
 |
|  |  |
| ***Consequences if not approved:*** | The requirements for spurious emission UE co-existence remain incorrect for the above Rel-15 EN-DC combos. |
|  |  |
| ***Clauses affected:*** | 6.5B.3.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-3 CR ... |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

### <Start of Changes>

##### 6.5B.3.3.2 Spurious emission band UE co-existence

This clause specifies the requirements for the specified EN-DC, for coexistence with protected bands. The requirements in Table 6.5B.3.3.2-1 apply on each component carrier with all component carriers are active.

NOTE: For inter-band EN-DC with uplink assigned to one LTE band and one NR band the requirements in Table 6.5B.3.3.2-1 could be verified by measuring spurious emissions at the specific frequencies where second and third order intermodulation products generated by the two transmitted carriers can occur;

Table 6.5B.3.3.2-1: Requirements

| EN-DC Configuration | Spurious emission  |
| --- | --- |
| Protected band | Frequency range (MHz) | Maximum Level (dBm) | MBW (MHz) | NOTE |
| DC\_1\_n28 | E-UTRA Band 5, 7, 8, 18, 19, 20, 26, 27, 31, 38, 40, 41, 72, 73NR band n79 | FDL\_low  | -  | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 22, 32, 42, 43, 50, 51, 52, 65, 74, 75, 76NR band n77, n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 3, 34 | FDL\_low  | -  | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5,16 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 16 |
| DC\_1\_n40 | Band 1, 5, 7, 8, 20, 22, 26, 27, 28, 31, 32, 38, 41, 42, 43, 44, 45, 50, 51, 52, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| Band 3, 34 | FDL\_low  | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 1880 |  | 1895 | -40 | 1 | 5, 17 |
| Frequency range | 1895 |  | 1915 | -15.5 | 5 | 5, 7, 17 |
| Frequency range | 1915 |  | 1920 | +1.6 | 5 | 5, 7, 17 |
| DC\_1\_n51 | E-UTRA Band 7, 12, 13, 17, 20, 22, 27, 28, 29, 31, 38, 44, 48, 67, 68, 69, 72, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 34 | FDL\_low | - | FDL\_high | -50 | 1 | 5, 2 |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 16 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 16 |
| E-UTRA Band 5, 6, 8, 26, 30, 40, 41, 42, 43, 46NR Band n77, n78, n79,  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_1\_n77 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_1\_n78DC\_1\_n84\_ULSUP-TDM\_n78 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_1\_n79 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 21, 26, 28, 34, 40, 41, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1880 | - | 1895 | -40 | 1 | 5, 8 |
| Frequency range | 1895 | - | 1915 | -15.5 | 5 | 5, 7, 8 |
| Frequency range | 1915 | - | 1920 | +1.6 | 5 | 5, 7, 8 |
| DC\_2\_n5 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 28, 29, 30, 42, 48, 50, 51, 53, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 41, 43 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_2\_n66 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low  | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 42, 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_2\_n71 | E-UTRA Band 4, 5, 12, 13, 14, 17, 24, 26, 29, 30, 48, 66 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_2\_n78 | E-UTRA Band 4, 5, 10, 12, 13, 14, 17, 24, 26, 27, 28, 29, 30, 41, 50, 51, 66, 70, 71, 74, 85 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n7 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 40, 43, 44, 50, 51, 65, 67, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA band 22, 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 2570  | -  | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_3\_n28 | E-UTRA Band 1, 42, 43, 50, 51, 65, 74, 75, 76NR band n77, n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 5, 7, 8, 18, 19, 20, 26, 27, 31, 34, 38, 40, 41, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 11, 21 | FDL\_low  | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 13 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 9 |
| DC\_3\_n40 | E-UTRA Band 1, 5, 7, 8, 20, 26, 27, 28, 31, 32, 33, 34, 38, 39, 41, 43, 44. 45, 50, 51, 65, 67, 68, 69, 72, 73, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 22, 42, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n51 | E-UTRA Band 7, 8, 12, 13, 17, 20, 27, 28, 31, 33, 38, 48, 67, 68, 69, 72, 73 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 1, 5, 6, 22, 26, 30, 34, 36, 40, 41, 42, 43, 44, 46, 65, 71 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_3\_n77 | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_3\_n78DC\_3\_n80\_ULSUP-TDM\_n78, | E-UTRA Band 1, 3, 5, 7, 8, 11, 18, 19, 20, 21, 26, 28, 34, 39, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_3\_n79 DC\_3\_n80\_ULSUP-TDM\_n79, | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 28, 34, 39, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| DC\_3\_n82 | E-UTRA Band 1, 3 7, 8, 20，22, 31, 32, 33, 34, 38, 40, 43, 50, 51, 65, 67, 68, 69, 72,74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 42 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_5\_n40 | E-UTRA Band 1, 3, 5, 7, 8, 28, 31, 34, 38, 42, 43, 45, 65, 73 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41, 52 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_5\_n66 | E-UTRA Band 1, 2, 3, 4, 5, 6, 7, 8, 10, 12, 13, 14, 17, 24, 25, 28, 29, 30, 34, 38, 40, 43, 45, 50, 51, 65, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41, 42, 48, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_5\_n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 12, 13, 14, 17, 24, 25, 28, 29, 30, 31, 34, 38, 40, 45, 65, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 26 | 859 | - | 869 | -27 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 7 |
| DC\_7\_n28 | E-UTRA Band 2, 3, 5, 7, 8, 20, 26, 27, 31, 34, 40, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 4, 10, 42, 43, 50, 65, 66, 74, 75, 76NR band n78 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 2570  | -  | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_7\_n51 | E-UTRA Band 2, 3, 5, 8, 26, 30, 31, 32, 33, 34, 40, 48, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570  | - | 2575 | +1.6 | 5 | 5, 7, 16 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 7, 16 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5 |
| E-UTRA Band 1, 4, 10, 12, 13, 14, 17, 20, 22, 23, 27, 28, 29, 42, 43, 44, 46, 65, 66, 67, 68NR Band n77, n78, n79,  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_7\_n78 | E-UTRA Band 1, 2, 3, 4, 5, 7, 8, 10, 11, 18, 19, 20, 21, 26, 27, 28, 31, 32, 33, 34, 40, 50, 51, 65, 66, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 2570  | - | 2575 | +1.6 | 5 | 5, 6, 7 |
| Frequency range | 2575 | - | 2595 | -15.5 | 5 | 5, 6, 7 |
| Frequency range | 2595 | - | 2620 | -40 | 1 | 5, 6 |
| DC\_8\_n40 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39,, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 22, 41, 42, 43, 52 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low  | - | FDL\_high | -50 | 1 | 5 |
| DC\_8\_n77 | E-UTRA Band 1, 20, 28, 31, 32, 33, 34, 38, 39, 40, 44, 45, 50, 51, 65, 67, 68, 69, 72, 73, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA band 3, 7, 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 12 |
| DC\_8\_n78DC\_8\_n81\_ULSUP-TDM\_n78, | E-UTRA Band 1, 20, 28, 34, 39, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3, 7, 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 8 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3, 12 |
| DC\_8\_n79DC\_8\_n81\_ULSUP-TDM\_n79, | E-UTRA Band 1, 8, 28, 34, 39, 40, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 3,41,42  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 12 |
| Frequency range | 860 | - | 890 | -40 | 1 | 5, 12 |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_11\_n77 | E-UTRA Band 1, 3, 18, 19, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_11\_n78 | E-UTRA Band 1, 3, 18, 19, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_11\_n79 | E-UTRA Band 1, 3, 18, 19, 28, 34, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_12\_n5 | E-UTRA Band 2, 5, 13, 14, 17, 24, 25, 26, 30, 42, 43 50, 51, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Bands 4, 10, 41, 48, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_12\_n66 | E-UTRA Band 2, 5, 13, 14, 17, 25, 26, 27, 30, 41, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 48, 50, 51, 66, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 12, 85 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
|  |  |  |  |  |  |  |  |
| DC\_18\_n77 | E-UTRA Band 1, 3, 11, 21, 28, 34, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_18\_n78 | E-UTRA Band 1, 3, 11, 21, 28, 34, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_18\_n79 | E-UTRA Band 1, 3, 11, 21, 28, 34, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n77 | E-UTRA Band 1, 3, 11, 21, 28, 34, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n78 | E-UTRA Band 1, 3, 11, 21, 28, 34, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_19\_n79 | E-UTRA Band 1, 3, 11, 21, 28, 34, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_20\_n8 | E-UTRA Band 1, 3, 7, 22, 28, 31, 32, 34, 38, 42, 43, 65, 75, 76NR bandn78 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_20\_n28DC\_20\_n83 | E-UTRA Band 1, 3, 7, 8, 22, 31, 32, 34, 38, 42, 43, 65, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| DC\_20\_n51 | E-UTRA Band 1, 3, 4, 8, 17, 22, 28, 29, 31, 40, 43, 48, 65, 66, 68, 72 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| Frequency range | 758 | - | 788 | -50 | 1 |  |
| E-UTRA Band 2, 7, 25, 32, 33, 34, 35, 36, 37, 38, 39, 41, 42, 46, 69, 70NR Band n77, n78, n79,  | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n77 | E-UTRA Band 1, 3, 7, 8, 31, 32, 33, 34, 40, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 38, 69 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_20\_n78,DC\_20\_n82\_ULSUP-TDM\_n78, | E-UTRA Band 1, 3, 7, 8, 31, 32, 33, 34, 40, 50, 51, 65, 67, 68, 72, 74, 75, 76 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 20 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| E-UTRA Band 38, 69 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_21\_n77 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_21\_n78 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_21\_n79 | E-UTRA Band 1, 3, 18, 19, 21, 28, 34, 42, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_25\_n41 | E-UTRA Band 4, 5, 10, 12, 13 , 14, 17, 24, 26, 27, 28, 29, 30, 42, 45, 48, 66, 70, 71 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA/NR Band 2, 25 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_26\_n41 | E-UTRA Band 1, 2, 3, 4, 5, 10, 11, 12, 13 , 14, 17, 18, 19, 21, 24, 25, 26, 29, 30, 31, 34, 39, 42, 43, 48, 50, 51, 65, 66, 70, 71, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 |  | 1915.7 | -41 | 0.3 | 3 |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| DC\_26\_n77 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 41, , 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_26\_n78 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 41, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_26\_n79 | E-UTRA Band 1, 3, 5, 11, 18, 19, 21, 26, 34, 39, 40, 41, 42, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 703 | - | 799 | -50 | 1 |  |
| Frequency range | 799 | - | 803 | -40 | 1 | 5 |
| Frequency range | 945 | - | 960 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3 |
| Frequency range | 2545 | - | 2575 | -50 | 1 |  |
| Frequency range | 2595 | - | 2645 | -50 | 1 |  |
| DC\_28\_n51 | E-UTRA Band 2, 3, 5, 7, 8, 25, 26, 31, 34, 38, 40, 41, 72 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 4, 10, 20, 22, 24, 32, 42, 43, 45, 46, 65, 66, 71, 73NR band n78, n79 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 2, 9, 10 |
| Frequency range | 470 | - | 694 | -42 | 8 | 5, 17 |
| Frequency range | 470 | - | 710 | -26.2 | 6 | 14 |
| Frequency range | 662 | - | 694 | -26.2 | 6 | 5 |
| Frequency range | 758 | - | 773 | -32 | 1 | 5 |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| DC\_28\_n77 | E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 34, 39, 40, 41, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 65 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3, 9 |
| DC\_28\_n78DC\_28\_n83\_ULSUP-TDM\_n78, | E-UTRA Band 3, 5, 7, 8, 18, 19, 20, 26, 34, 39, 40, 41 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3, 9 |
| DC\_28\_n79 | E-UTRA Band 3, 5, 8, 18, 19, 34, 39, 40, 41, 42 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 1 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 11 |
| E-UTRA Band 11, 21 | FDL\_low | - | FDL\_high | -50 | 1 | 9, 10 |
| Frequency range | 758 | - | 773 | -32 | 1 |  |
| Frequency range | 773 | - | 803 | -50 | 1 |  |
| Frequency range | 1884.5  | -  | 1915.7  | -41 | 0.3 | 3, 9 |
| DC\_30\_n5 | E-UTRA Band 2, 4, 5, 7, 12, 13, 14, 17, 24, 25, 26, 29, 30, 38, 48, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| DC\_30\_n66 | E-UTRA Band 2, 4, 5, 10, 12, 13, 14, 17, 24, 25, 26, 27, 29, 30, 38, 41, 66, 70, 71 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Band 48 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_38\_n78 | N/A |
| DC\_39\_n78 | E-UTRA Band 1, 8, 34, 40, 41, 44, 45 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 18 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 18 |
| DC\_39\_n79 | E-UTRA Band 1, 8, 34, 40, 41, 44, 45  | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1805 | - | 1855 | -40 | 1 | 18 |
| Frequency range | 1855 | - | 1880 | -15.5 | 5 | 18 |
| DC\_40\_n77 | N/A |
| DC\_41\_n77 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 26, 28, 33, 34, 39, 40, 44, 45, 73, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 |  | 1915.7 | -41 | 0.3 | 3 |
| DC\_41\_n78 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 26, 28, 34, 39, 40, 44, 45, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_41\_n79 | E-UTRA Band 1, 3, 5, 8, 11, 18, 19, 21, 26, 28, 34, 40, 42, 44, 45, 65, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| Frequency range | 1884.5 | - | 1915.7 | -41 | 0.3 | 3 |
| DC\_42\_n51 | E-UTRA Band 3, 8, 20, 25, 30, 31, 34, 39, 41, 73 | FDL\_low  | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 1, 2, 4, 5, 6, 7, 10, 12, 13, 14, 17, 23, 24, 26, 27, 28, 29, 32, 38, 40, 44, 46, 65, 66, 67, 68, 70, 71 | FDL\_low  | - | FDL\_high | -50 | 1 | 2 |
| DC\_42\_n77 | N/A |
| DC\_42\_n78 | N/A |
| DC\_42\_n79 | N/A |
| DC\_66\_n5 | E-UTRA Band 1, 2, 3, 4, 5, 6, 7, 8, 10, 12, 13, 14, 17, 24, 25, 26, 28, 29, 30, 34, 38, 40, 43, 45, 50, 51, 65, 66, 70, 71, 85 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 41, 42, 48, 52 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| DC\_66\_n71 | E-UTRA Band 4, 5, 7,10, 13, 14, 17, 22, 24, 26, 27, 29, 30, 43,50, 51, 66, 74 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| E-UTRA Band 2, 25, 41, 42, 48, 70 | FDL\_low | - | FDL\_high | -50 | 1 | 2 |
| E-UTRA Band 71 | FDL\_low | - | FDL\_high | -50 | 1 | 5 |
| DC\_66\_n78,DC\_66\_n86\_ULSUP-TDM\_n78, | E-UTRA Band 1, 3, 5, 7, 8, 20, 26, 28, 34, 39, 40, 41, 65 | FDL\_low | - | FDL\_high | -50 | 1 |  |
| NOTE 1: FDL\_low and FDL\_high refer to each E-UTRA frequency band specified in Table 5.5-1 in TS 36.101 [4].NOTE 2: As exceptions, measurements with a level up to the applicable requirements defined in Table 6.6.3.1-2 are permitted for each assigned E-UTRA carrier used in the measurement due to 2nd, 3rd, 4th or 5th harmonic spurious emissions. Due to spreading of the harmonic emission the exception is also allowed for the first 1 MHz frequency range immediately outside the harmonic emission on both sides of the harmonic emission. This results in an overall exception interval centred at the harmonic emission of (2 MHz + N x LCRB x 180 kHz), where N is 2, 3, 4, 5 for the 2nd, 3rd, 4th or 5th harmonic respectively. The exception is allowed if the measurement bandwidth (MBW) totally or partially overlaps the overall exception interval.NOTE 3: Applicable when co-existence with PHS system operating in 1884.5 - 1915.7 MHzNOTE 4: VoidNOTE 5: These requirements also apply for the frequency ranges that are less than FOOB (MHz) in Table 6.6.3.1-1 and Table 6.6.3.1A-1 from the edge of the channel bandwidth.NOTE 6: This requirement is applicable for any channel bandwidths within the range 2500 - 2570 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 2560.5 - 2562.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 2552 - 2560 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.NOTE 7: For these adjacent bands, the emission limit could imply risk of harmful interference to UE(s) operating in the protected operating band.NOTE 8: This requirement is applicable for any channel bandwidths within the range 1920 - 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 1930 - 1938 MHz the requirement is applicable only for an uplinkNOTE 9: Applicable when the assigned E-UTRA carrier is confined within 718 MHz and 748 MHz and when the channel bandwidth used is 5 or 10 MHz.NOTE 10: As exceptions, measurements with a level up to the applicable requirement of -38 dBm/MHz is permitted for each assigned E-UTRA carrier used in the measurement due to 2nd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.6-1) for which the 2nd harmonic totally or partially overlaps the measurement bandwidth (MBW).NOTE 11: As exceptions, measurements with a level up to the applicable requirement of -38 dBm/MHz is permitted for each assigned E-UTRA carrier used in the measurement due to 3rd harmonic spurious emissions. An exception is allowed if there is at least one individual RB within the transmission bandwidth (see Figure 5.6-1) for which the 3rd harmonic totally or partially overlaps the measurement bandwidth (MBW).NOTE 12: This requirement is applicable only for the following cases: A: for carriers of 5 MHz channel bandwidth when carrier centre frequency (Fc) is within the range 902.5 MHz ≤ Fc < 907.5 MHz with an uplink transmission bandwidth less than or equal to 20 RB; B: for carriers of 5 MHz channel bandwidth when carrier centre frequency (Fc) is within the range 907.5 MHz ≤ Fc ≤ 912.5 MHz without any restriction on uplink transmission bandwidth; C: for carriers of 10 MHz channel bandwidth when carrier centre frequency (Fc) is Fc = 910 MHz with an uplink transmission bandwidth less than or equal to 32 RB with RBstart > 3.NOTE 13: VoidNOTE 14: This requirement is applicable for 5 and 10 MHz E-UTRA channel bandwidth allocated within 718-728MHz. For carriers of 10 MHz bandwidth, this requirement applies for an uplink transmission bandwidth less than or equal to 30 RB with RBstart > 1 and RBstart < 48.NOTE 15: VoidNOTE 16: This requirement is applicable for any channel bandwidths within the range 1920 - 1980 MHz with the following restriction: for carriers of 15 MHz bandwidth when carrier centre frequency is within the range 1927.5 - 1929.5 MHz and for carriers of 20 MHz bandwidth when carrier centre frequency is within the range 1930 - 1938 MHz the requirement is applicable only for an uplink transmission bandwidth less than or equal to 54 RB.NOTE 17: This requirement is applicable in the case of a 10 MHz E-UTRA carrier confined within 703 MHz and 733 MHz, otherwise the requirement of -25 dBm with a measurement bandwidth of 8 MHz applies.NOTE 18: This requirement is only applicable for E-UTRA carriers with bandwidth confined within 1885 - 1920 MHz (requirement for carriers with at least 1RB confined within 1880 - 1885 MHz is not specified). This requirement applies for an uplink transmission bandwidth less than or equal to 54 RB for E-UTRA carriers of 15 MHz bandwidth when carrier center frequency is within the range 1892.5 - 1894.5 MHz and for E-UTRA carriers of 20 MHz bandwidth when carrier center frequency is within the range 1895 - 1903 MHz.NOTE 19: Void |

NOTE: To simplify the above Table, E-UTRA band numbers are listed for bands which are specified only for E-UTRA operation or both E-UTRA and NR operation. NR band numbers are listed for bands which are specified only for NR operation.

### <End of Changes >