3GPP TSG-RAN WG4 Meeting # 97-e R4-201xxxx

Electronic Meeting, 2nd – 13th November, 2020

**Source:** Huawei, HiSilicon

**Title:** TP to TR 38.717.02-01 for CA\_n3A-n7A

**Agenda item:** 10.2.2

**Document for:** Approval

# Background

This contribution provides text proposal on the NR CA band combination CA\_n3A-n7A as defined in New WID on NR Inter-band Carrier Aggregation/Dual Connectivity for 2 bands DL with x bands UL (x=1,2) RP-201539 [1].

# Text Proposal

##### ---Start of changes---

## 6.X CA\_n3-n7

### 6.X.1 Common for 1 band UL and 2 bands UL CA

#### 6.X.1.1 Operating bands for CA

Table 6.X.1.1-1: CA band combination CA\_n3A-n7A

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **NR CA Band Combination** | **NR Band** | **Uplink (UL) band** | | | **Downlink (DL) band** | | | **Duplex**  **mode** |
| **BS receive / UE transmit** | | | **BS transmit / UE receive** | | |
| **FUL\_low – FUL\_high** | | | **FDL\_low – FDL\_high** | | |
| CA\_n3-n7 | n3 | 1710 MHz | – | 1785 MHz | 1805 MHz | – | 1880 MHz | FDD |
| n7 | 2500 MHz | – | 2570 MHz | 2620 MHz | – | 2690 MHz | FDD |

#### 6.X.1.2 Channel bandwidths per operating band for CA

Table 6.X.1.2-1: Supported bandwidths per CA band combination CA\_n3A-n7A

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **CA operating / channel bandwidth [MHz]** | | | | | | | | | | | | | | | | | |
| **NR CA Configuration** | | **UL Configuration** | **NR Band** | **SCS [kHz]** | **5** | **10** | **15** | **20** | **25** | **30** | **40** | **50** | **60** | **70** | **80** | **90** | **100** | **Bandwidth combination set** |
| CA\_n3A-n7A | | - | n3 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  | 0 |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |  |
| n7 | 15 | Yes | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 30 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |
| 60 |  | Yes | Yes | Yes | Yes | Yes | Yes | Yes |  |  |  |  |  |

#### 6.X.1.3 UE Co-existence studies

Table 6.X.1.3-1/2 summarizes frequency ranges where harmonics and/or harmonics mixing occur for CA\_n3-n7.

**Table 6.X.1.3-1: Impact of UL/DL Harmonic**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  | **2nd Harmonic** | | **3rd Harmonic** | | **4th Harmonic** | |
| **Band** | **UL Low Band Edge** | UL High Band Edge | DL Low Band Edge | DL High Band Edge | UL Low Band Edge | UL High Band Edge | UL Low Band Edge | UL High Band Edge | UL Low Band Edge | UL High Band Edge |
| n3 | 1710 | 1785 | 1805 | 1880 | 3420 | 3570 | 5130 | 5355 | 6840 | 7140 |
| n7 | 2500 | 2570 | 2620 | 2690 | 5000 | 5140 | 7500 | 7710 | 10000 | 10280 |

Based on above table, there is no harmonic interference.

**Table 6.X.1.3-2: Impact of UL/DL Harmonic mixing**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  | **2nd Harmonic** | | **3rd Harmonic** | | **4th Harmonic** | |
| **Band** | **UL Low Band Edge** | UL High Band Edge | DL Low Band Edge | DL High Band Edge | DL Low Band Edge | DL High Band Edge | DL Low Band Edge | DL High Band Edge | DL Low Band Edge | DL High Band Edge |
| n3 | 1710 | 1785 | 1805 | 1880 | 3610 | 3760 | 5415 | 5640 | 7220 | 7520 |
| n7 | 2500 | 2570 | 2620 | 2690 | 5240 | 5380 | 7860 | 8070 | 10480 | 10760 |

Based on above table, there is no harmonic mixing issue.

#### 6.X.1.4 ∆TIB and ∆RIB values

For CA\_n3A-n7A, the ΔTIB,c and ΔRIB are given in the tables below reusing the values of DC\_3\_n7.

Table 6.X.1.4-1: ΔTIB,c

| Inter-band CA Configuration | NR Band | ΔTIB,c [dB] |
| --- | --- | --- |
| CA\_n3-n7 | n3 | 0.5 |
| n7 | 0.5 |
|  | | |

Table 6.X.1.4-2: ΔRIB

| Inter-band CA Configuration | NR Band | ΔRIB [dB] |
| --- | --- | --- |
| CA\_n3-n7 | n3 | 0 |
| n7 | 0 |
|  | | |

#### 6.X.1.5 REFSENs requirements

The MSD due to cross band isolation for CA\_n3-n7 is shown below, referring to DC\_3\_n41.

Table 6.X.1.5-1: Reference sensitivity exceptions (MSD) due to cross band isolation for PC3 EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / Channel bandwidth of the affected DL band / MSD | | | | | | | | | | | | | | |
| UL band | DL band | 5 MHz  (dB) | 10 MHz  (dB) | 15 MHz  (dB) | 20 MHz  (dB) | 25 MHz  (dB) | 30 MHz  (dB) | 40 MHz  (dB) | 50 MHz  (dB) | 60 MHz  (dB) | 70 MHz  (dB) | 80 MHz  (dB) | 90 MHz  (dB) | 100 MHz  (dB) |
| n7 | n3 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |

Table 6.X.1.5-2: Uplink configuration for reference sensitivity exceptions due to cross band isolation for EN-DC in NR FR1

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| E-UTRA or NR Band / SCS / Channel bandwidth of the affected DL band / UL RB allocation of the agressor band | | | | | | | | | | | | | | | |
| UL band | DL band | SCS of UL band (kHz) | 5 MHz  (LCRB) | 10 MHz  (LCRB) | 15 MHz  (LCRB) | 20 MHz  (LCRB) | 25 MHz  (LCRB) | 30 MHz  (LCRB) | 40 MHz  (LCRB) | 50 MHz  (LCRB) | 60 MHz  (LCRB) | 70 MHz  (LCRB) | 80 MHz  (LCRB) | 90 MHz  (LCRB) | 100 MHz  (LCRB) |
| n7 | n3 | 15 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |

#### 6.X.1.6 OOB blocking exception requirements

There is no OOB blocking exception requirement for CA\_n3-n7.

##### ---End of changes---

# Reference

[1] RP-201539, “Rel-17 NR Inter-band Carrier Aggregation/Dual Connectivity for 2 bands DL with x bands UL (x=1,2)”, ZTE Corporation