**3GPP TSG-RAN WG4 Meeting #97-e *R4-2017131***

**Electronic Meeting, Nov 2 – 13, 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.133** | **CR** | **1275** | **rev** | **1** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction CR to Rel-16 UE power saving requirements |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_UE\_pow\_sav-Core |  | ***Date:*** | 2020-11-09 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | 1. Correct some mistakes;
2. Made some clarifications
 |
|  |  |
| ***Summary of change:*** | 1. The condition of requirements application is not clear. For example, the condition of the requirements in section 4.2.2.9.2 is satisfied is that UE is configured with lowMobilityEvalutation criterion and UE has fulfuled.
2. Correct some mistakes in section 4.2.2.10.3 and 4.2.2.10.4.
 |
|  |  |
| ***Consequences if not approved:*** | The specification is not correct. |
|  |  |
| ***Clauses affected:*** |  4.2.2.9, 4.2.2.10, 4.2.2.11 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

----------------------------------------------------- Beginning of Change 1 ------------------------------------------------------------

#### 4.2.2.9 Measurements of intra-frequency NR cells for UE configured with relaxed measurement criterion

##### 4.2.2.9.1 Introduction

This section contains the requirements for measurements on intra-frequency NR cells when Srxlev ≤ SIntraSearchP or Squal ≤ SIntraSearchQ and when the UE is configured any of the following relaxed measurement critera:

- Relaxed measurement criterion for UE with low mobility defined in clause 5.2.4.9.1 in [1],

- Relaxed measurement criterion for UE not-at-cell edge defined in clause 5.2.4.9.2 in [1],

- Both low mobility criterion and not-at-cell edge criterion as defined in clauses 5.2.4.9.1 and 5.2.4.9.2 in [1] respectively.

##### 4.2.2.9.2 Measurements for UE fulfilling low mobility criterion

This clause contains requirements for measurements on intra-frequency NR cells provided that:

- T331 timer is not running for EMR measurements on intra-frequency NR carrier and

- UE is configured with *lowMobilityEvalutation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured or configured but set to FALSE, and UE has fulfilled only the *lowMobilityEvalutation* [2] criterion.

The requirements defined in clause 4.2.2.3 apply for this section except that:

- Tdetect,NR\_Intraas specified in Table 4.2.2.9.1-1.

- Tmeasure,NR\_Intra as specified in Table 4.2.2.9.1-1.

- Tevaluate,NR\_Intra as specified in Table 4.2.2.9.1-1.

Table 4.2.2.9.1-1: Tdetect,NR\_Intra, Tmeasure,NR\_Intra and Tevaluate,NR\_Intra

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DRX cycle length [s] | Scaling Factor (N1) | Tdetect,NR\_Intra [s] (number of DRX cycles) | Tmeasure,NR\_Intra [s] (number of DRX cycles) | Tevaluate,NR\_Intra[s] (number of DRX cycles) |
| **FR1** | **FR2Note1** |
| 0.32 | 1 | 8 | 11.52 x N1 x M2 x K1 (36 x N1 x M2 x K1) | 1.28 x N1 x M2 x K1 (4 x N1 x M2 x K1) | 5.12 x N1 x M2 x K1 (16 x N1 x M2 x K1) |
| 0.64 | 5 | 17.92 x N1 x K1 (28 x N1 x K1) | 1.28 x N1 x K1 (2 x N1 x K1) | 5.12 x N1 x K1 (8 x N1 x K1) |
| 1.28 | 4 | 32 x N1 x K1 (25 x N1 x K1) | 1.28 x N1 x K1 (1 x N1 x K1) | 6.4 x N1 x K1 (5 x N1 x K1) |
| 2.56 | 3 | 58.88 x N1 x K1 (23 x N1 x K1) | 2.56 x N1 x K1 (1 x N1 x K1) | 7.68 x N1 x K1 (3 x N1 x K1) |
| Note 1: Applies for UE supporting power class 2&3&4. For UE supporting power class 1, N1 = 8 for all DRX cycle length.Note 2: M2 = 1.5 if SMTC periodicity of measured intra-frequency cell > 20 ms; otherwise M2=1.Note 3: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *lowMobilityEvalutation* [2] criterion. |

##### 4.2.2.9.3 Measurements for UE fulfilling not-at-cell edge criterion

This clause contains requirements for measurements on intra-frequency NR cells provided that:

- T331 timer is not running for EMR measurements on intra-frequency NR carrier and

- UE is configured with *cellEdgeEvaluation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criteria and *combineRelaxedMeasCondition* [2] not configured or is configured but set to FALSE, and UE has fulfilled only the *cellEdgeEvaluation* [2] criterion.

The requirements defined in clause 4.2.2.3 apply for this section except that:

- Tdetect,NR\_Intraas specified in Table 4.2.2.9.3-1.

- Tmeasure,NR\_Intra as specified in Table 4.2.2.9.3-1.

- Tevaluate,NR\_Intra as specified in Table 4.2.2.9.3-1.

Table 4.2.2.9.3-1: Tdetect,NR\_Intra, Tmeasure,NR\_Intra and Tevaluate,NR\_Intra

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DRX cycle length [s] | Scaling Factor (N1) | Tdetect,NR\_Intra [s] (number of DRX cycles) | Tmeasure,NR\_Intra [s] (number of DRX cycles) | Tevaluate,NR\_Intra[s] (number of DRX cycles) |
| FR1 | FR2Note1 |
| 0.32 | 1 | 8 | 11.52 x N1 x M2 x K1 (36 x N1 x M2 x K1) | 1.28 x N1 x M2 x K1 (4 x N1 x M2 x K1) | 5.12 x N1 x M2 x K1 (16 x N1 x M2 x K1) |
| 0.64 | 5 | 17.92 x N1 x K1 (28 x N1 x K1) | 1.28 x N1 x K1 (2 x N1 x K1) | 5.12 x N1 x K1 (8 x N1 x K1) |
| 1.28 | 4 | 32 x N1 x K1 (25 x N1 x K1) | 1.28 x N1 x K1 (1 x N1 x K1) | 6.4 x N1 x K1 (5 x N1 x K1) |
| 2.56 | 3 | 58.88 x N1 x K1 (23 x N1 x K1) | 2.56 x N1 x K1 (1 x N1 x K1) | 7.68 x N1 x K1 (3 x N1 x K1) |
| Note 1: Applies for UE supporting power class 2&3&4. For UE supporting power class 1, N1 = 8 for all DRX cycle length.Note 2: M2 = 1.5 if SMTC periodicity of measured intra-frequency cell > 20 ms; otherwise M2=1.Note 3: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *cellEdgeEvaluation* [2] criterion. |

##### 4.2.2.9.4 Measurements for UE fulfilling low mobility and not-at-cell edge criteria

This clause contains requirements for measurements on intra-frequency NR cells provided that:

- T331 timer is not running for EMR measurements on intra-frequency NR carrier, and

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion, and

- has also fulfilled both criteria, and

* less than 1 hour have passed since measurements for cell reselection were last performed

In this case the UE is not required to meet Tdetect,NR\_Intra, Tmeasure,NR\_Intra and Tevaluate,NR\_Intra as defined in Table 4.2.2.3-1.

#### 4.2.2.10 Measurements of inter-frequency NR cells for UE configured with relaxed measurement criterion

##### 4.2.2.10.1 Introduction

This section contains the requirements for measurements on inter-frequency NR cells when the UE is configured with any of following relaxed measurement criteria:

* Relaxed measurement criterion for UE with low mobility defined in clause 5.2.4.9.1 in [1],
* Relaxed measurement criterion for UE not-at-cell edge defined in clause 5.2.4.9.2 in [1],
* Both low mobility criterion and not-at-cell edge criterion as defined in clauses 5.2.4.9.1 and 5.2.4.9.2 in [1] respectively.

##### 4.2.2.10.2 Measurements for UE fulfilling low mobility criterion

This clause contains requirements for measurements on inter-frequency NR cells provided that:

* T331 timer is not running for EMR measurements on inter-frequency NR carrier, and
* UE is configured with *lowMobilityEvalutation* [2] criterion and UE has fulfilled, or
* UE is configured with both *lowMobilityEvalutation* [2] and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured or configured but set to FALSE, and
* UE has fulfilled only the *lowMobilityEvalutation* [2] criterion.

When Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ then the requirements defined in clause 4.2.2.4 apply for this section except that:

- Tdetect,NR\_Interas specified in Table 4.2.2.10.2-1.

- Tmeasure,NR\_Inter as specified in Table 4.2.2.10.2-1.

- Tevaluate,NR\_Inter as specified in Table 4.2.2.10.2-1.

When Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ and the UE is configured with *highPriorityMeasRelax* [2] then the UE shall search for inter-frequency layers of higher priority at least every K2\*Thigher\_priority\_search seconds where Thigher\_priority\_search is described in clause 4.2.2.7 and, K2 = 60. Otherwise if the UE is not configured with *highPriorityMeasRelax* [2] then the UE shall search for inter-frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2.2.7.

Table 4.2.2.10.2-1: Tdetect,NR\_Inter, Tmeasure,NR\_Inter and Tevaluate,NR\_Inter

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **DRX cycle length [s]** | **Scaling Factor (N1)** | **Tdetect,NR\_Inter [s] (number of DRX cycles)** | **Tmeasure,NR\_Inter [s] (number of DRX cycles)** | **Tevaluate,NR\_Inter [s] (number of DRX cycles)** |
| **FR1** | **FR2Note1** |
| 0.32 | 1 | 8 | 11.52 x N1 x 1.5 x K1 (36 x N1 x 1.5 x K1) | 1.28 x N1 x 1.5 x K1 (4 x N1 x 1.5 x K1) | 5.12 x N1 x 1.5 x K1 (16 x N1 x 1.5 x K1) |
| 0.64 | 5 | 17.92x N1 x K1 (28 x N1 x K1) | 1.28 x N1 x K1 (2 x N1 x K1) | 5.12 x N1 x K1 (8 x N1 x K1) |
| 1.28 | 4 | 32 x N1 x K1 (25 x N1 x K1) | 1.28 x N1 x K1 (1 x N1 x K1) | 6.4 x N1 x K1 (5 x N1 x K1) |
| 2.56 | 3 | 58.88 x N1 x K1 (23 x N1 x K1) | 2.56 x N1 x K1 (1 x N1 x K1) | 7.68 x N1 x K1 (3 x N1 x K1) |
| Note 1: Applies for UE supporting power class 2&3&4. For UE supporting power class 1, N1 = 8 for all DRX cycle length.Note 2: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *lowMobilityEvalutation* [2] criterion. |

##### 4.2.2.10.3 Measurements for UE fulfilling not-at-cell edge criterion

This clause contains requirements for measurements on inter-frequency NR cells provided that:

- T331 timer is not running for EMR measurements on inter-frequency NR carrier, and

- UE is configured with *cellEdgeEvaluation* [2] criterion, and UE has fulfilled or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured or configured but set to FALSE, and

- UE has fulfilled only the *cellEdgeEvaluation* [2] criterion.

When Srxlev ≤ SnonIntraSearchP or Squal ≤ SnonIntraSearchQ then the requirements defined in clause 4.2.2.4 apply for this section except that:

- Tdetect,NR\_Interas specified in Table 4.2.2.10.3-1.

- Tmeasure,NR\_Inter as specified in Table 4.2.2.10.3-1.

- Tevaluate,NR\_Inter as specified in Table 4.2.2.10.3-1.

When Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ and regardless of whether the UE is configured with *highPriorityMeasRelax* [2] or not, the UE shall search for inter-frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2.2.7

Table 4.2.2.10.3-1: Tdetect,NR\_Inter, Tmeasure,NR\_Inter and Tevaluate,NR\_Inter

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DRX cycle length [s] | Scaling Factor (N1) | Tdetect,NR\_Inter [s] (number of DRX cycles) | Tmeasure,NR\_Inter [s] (number of DRX cycles) | Tevaluate,NR\_Inter [s] (number of DRX cycles) |
| FR1 | FR2Note1 |
| 0.32 | 1 | 8 | 11.52 x N1 x 1.5 x K1 (36 x N1 x 1.5 x K1) | 1.28 x N1 x 1.5 x K1 (4 x N1 x 1.5 x K1) | 5.12 x N1 x 1.5 x K1 (16 x N1 x 1.5 x K1) |
| 0.64 | 5 | 17.92x N1 x K1 (28 x N1 x K1) | 1.28 x N1 x K1 (2 x N1 x K1) | 5.12 x N1 x K1 (8 x N1 x K1) |
| 1.28 | 4 | 32 x N1 x K1 (25 x N1 x K1) | 1.28 x N1 x K1 (1 x N1 x K1) | 6.4 x N1 x K1 (5 x N1 x K1) |
| 2.56 | 3 | 58.88 x N1 x K1 (23 x N1 x K1) | 2.56 x N1 x K1 (1 x N1 x K1) | 7.68 x N1 x K1 (3 x N1 x K1) |
| Note 1: Applies for UE supporting power class 2&3&4. For UE supporting power class 1, N1 = 8 for all DRX cycle length.Note 2: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *cellEdgeEvaluation* [2] criterion. |

##### 4.2.2.10.4 Measurements for UE fulfilling low mobility and not-at-cell edge criterion

This clause contains requirements for measurements on inter-frequency NR cells provided that:

- T331 timer is not running for EMR measurements on inter-frequency NR carrier, and

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion, and

- Has also fulfilled both criteria, and

- less than 1 hour have passed since measurements for cell reselection were last performed

In this case the UE is not required to meet Tdetect,NR\_Inter, Tmeasure,NR\_Inter and Tevaluate,NR\_Inter as defined in Table 4.2.2.4-1.

##### 4.2.2.11 Measurements of inter-RAT E-UTRAN cells for UE configured with relaxed measurement criterion

4.2.2.11.1 Introduction

This section contains the requirements for measurements on inter-RAT E-UTRAN cells when the UE is configured with any of following relaxed measurement critera:

- Relaxed measurement criterion for UE with low mobility defined in clause 5.2.4.9.1 in [1],

- Relaxed measurement criterion for UE not-at-cell edge defined in clause 5.2.4.9.2 in [1],

- Both low mobility criterion and not-at-cell edge criterion as defined in clauses 5.2.4.9.1 and 5.2.4.9.2 in [1] respectively.

##### 4.2.2.11.2 Measurements for UE fulfilling low mobility criterion

This clause contains requirements for measurements on inter-RAT E-UTRAN cells provided that:

- T331 timer is not running for EMR measurements on inter-RAT E-UTRAN, and

- UE is configured with *lowMobilityEvalutation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured or configured but set to FALSE, and

- UE has fulfilled only the *lowMobilityEvalutation* [2] criterion.

When Srxlev ≤ SnonIntraSearchP and Squal ≤ SnonIntraSearchQ then The requirements defined in clause 4.2.2.5 apply for this section except that:

- Tdetect,EUTRANas specified in Table 4.2.2.11.2-1.

- Tmeasure,EUTRAN as specified in Table 4.2.2.11.2-1.

- Tevaluate,EUTRAN as specified in Table 4.2.2.11.2-1.

When Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ and the UE is configured with *highPriorityMeasRelax* [2] then the UE shall search for E-UTRA inter-RAT frequency layers of higher priority at least every K2\*Thigher\_priority\_search seconds where Thigher\_priority\_search is described in clause 4.2.2.7 and, K2 = 60. Otherwise if the UE is not configured with *highPriorityMeasRelax* [2] then the UE shall search for E-UTRA inter-RAT frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2.2.7.

Table 4.2.2.11.2-1: Tdetect,EUTRAN, Tmeasure,EUTRAN, and Tevaluate,EUTRAN

|  |  |  |  |
| --- | --- | --- | --- |
| DRX cycle length [s] | Tdetect,EUTRAN [s] (number of DRX cycles) | Tmeasure,EUTRAN [s] (number of DRX cycles) | Tevaluate,EUTRAN[s] (number of DRX cycles) |
| 0.32 | 11.52 x K1 (36 x K1) | 1.28 x K1 (4 x K1) | 5.12 x K1 (16 x K1) |
| 0.64 | 17.92 x K1 (28 x K1) | 1.28 x K1 (2 x K1) | 5.12 x K1 (8 x K1) |
| 1.28 | 32 x K1 (25 x K1) | 1.28 x K1 (1 x K1) | 6.4 x K1 (5 x K1) |
| 2.56 | 58.88 x K1 (23 x K1) | 2.56 (1 x K1) | 7.68 x K1 (3 x K1) |
| Note 1: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *lowMobilityEvalutation* [2] criterion. |

##### 4.2.2.11.3 Measurements for UE fulfilling with not-at-cell edge criterion

This clause contains requirements for measurements on inter-RAT E-UTRAN cells provided that:

- T331 timer is not running for EMR measurements on inter-RAT E-UTRAN, and

- UE is configured with *cellEdgeEvaluation* [2] criterion and UE has fulfilled, or

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion and *combineRelaxedMeasCondition* [2] not configured or configured but set to FALSE, and

- UE has fulfilled only the *cellEdgeEvaluation* [2] criterion.

When Srxlev ≤ SnonIntraSearchP and Squal ≤ SnonIntraSearchQ then the requirements defined in clause 4.2.2.5 apply for this section except that:

- Tdetect,EUTRANas specified in Table 4.2.2.11.3-1.

- Tmeasure,EUTRAN as specified in Table 4.2.2.11.3-1.

- Tevaluate,EUTRAN as specified in Table 4.2.2.11.3-1.

When Srxlev > SnonIntraSearchP and Squal > SnonIntraSearchQ and regardless of whether the UE is configured with *highPriorityMeasRelax* [2] or not, the UE shall search for inter-RAT E-UTRAN frequency layers of higher priority at least every Thigher\_priority\_search where Thigher\_priority\_search is described in clause 4.2.2.7

Table 4.2.2.11.3-1: Tdetect,EUTRAN, Tmeasure,EUTRAN, and Tevaluate,EUTRAN

|  |  |  |  |
| --- | --- | --- | --- |
| DRX cycle length [s] | Tdetect,EUTRAN [s] (number of DRX cycles) | Tmeasure,EUTRAN [s] (number of DRX cycles) | Tevaluate,EUTRAN[s] (number of DRX cycles) |
| 0.32 | 11.52 x K1 (36 x K1) | 1.28 x K1 (4 x K1) | 5.12 x K1 (16 x K1) |
| 0.64 | 17.92 x K1 (28 x K1) | 1.28 x K1 (2 x K1) | 5.12 x K1 (8 x K1) |
| 1.28 | 32 x K1 (25 x K1) | 1.28 x K1 (1 x K1) | 6.4 x K1 (5 x K1) |
| 2.56 | 58.88 x K1 (23 x K1) | 2.56 x K1 (1 x K1) | 7.68 x K1 (3 x K1) |
| Note 1: K1 = 3 is the measurement relaxation factor applicable for UE fulfilling the *lowMobilityEvalutation* [2] criterion. |

##### 4.2.2.11.4 Measurements for UE fulfilling low mobility and not-at-cell edge criterion

This clause contains requirements for measurements on inter-RAT E-UTRAN cells provided that:

- T331 timer is not running for EMR measurements on inter-RAT E-UTRAN, and

- UE is configured with both *lowMobilityEvalutation* [2] criterion and *cellEdgeEvaluation* [2] criterion, and

- has also fulfilled both criteria, and

* less than 1 hour have passed since measurements for cell reselection were last performed,

In this case the UE is not required to meet Tdetect,EUTRAN , Tmeasure,EUTRAN and Tevaluate,EUTRAN as defined in Table 4.2.2.5-1.

------------------------------------------------------------- End of change 1 ------------------------------------------------------------